{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["20170"],"read":"whole","date_system":"1900"}

{"sheet":"20170","index":0,"n_rows":6101,"n_cols":8,"rows_kept":6101}
["ITEM NO",{"$nulls":4},"QUANTITY","RATE","AMOUNT"]
[]
[null,null,"SECTION 1"]
[]
[null,null,"BILL NO. 1"]
[]
[null,null,"PRELIMINARIES"]
[]
[null,null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,null,"The JBCC Principal Building Agreement (Edition 6.2 - May 2018) prepared by the Joint Building Contracts Committee shall be the applicable building agreement, amended as hereinafter described"]
[]
[null,null,"The JBCC Principal Building Agreement contract data form an integral part of this agreement"]
[]
[null,null,"The JBCC General Preliminaries (May 2018) published by the Joint Building Contracts Committee for use with the JBCC Principal Building Agreement (Edition 6.2 - May 2018) shall be deemed to be incorporated in these bills of quantities, amended as hereinafter described"]
[]
[null,null,"The contractor is deemed to have referred to the above mentioned documents for the full intent and meaning of each clause"]
[]
[null,null,"The clauses in the above mentioned documents are hereinafter referred to by clause number and heading only"]
[]
[null,null,"Where any item is not relevant to this agreement such item is marked N/A signifying \"not applicable\""]
[]
[null,null,"Where standard clauses or alternatives are not entirely applicable to this agreement such amendments, modifications, corrections or supplements as will apply are given under each relevant clause heading and such amendments, modifications, corrections or supplements shall take precedence notwithstanding anything to the contrary contained in the above mentioned documents"]
[]
[null,null,"PREAMBLES FOR TRADES"]
[]
[null,null,"The General Preambles for Trades 2017 published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of items fully described in the said General Preambles will be entertained"]
[]
[null,null,"Supplementary preambles and/or specifications are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles and/or specifications shall take precedence over the provisions of the General Preambles"]
[]
[null,null,"The contractor's prices for all items throughout these bills of quantities shall take account of and include where applicable for all of the obligations, requirements and specifications given in the General Preambles and in any supplementary preambles and/or specifications"]
[]
[null,null,"STRUCTURE OF THIS PRELIMINARIES BILL"]
[]
[null,null,"Section A :  A recital of the headings of the individual clauses in the aforementioned JBCC Principal Building Agreement"]
[]
[null,null,"Section B :  A recital of the headings of the individual clauses in the aforementioned JBCC General Preliminaries"]
[]
[null,null,"Section C : Any special clauses to meet the particular circumstances of the project"]
[]
[null,null,"PRICING OF PRELIMINARIES"]
[]
[null,null,"Should the contractor select Option A in the contract data for the adjustment of preliminaries, the amounts entered against the relevant items in these preliminaries are to be divided into one or more of the three categories provided namely fixed (F), value related (V) and time related (T)"]
[]
[null,null,"SECTION A: PRINCIPAL BUILDING AGREEMENT"]
[]
[null,null,"Interpretation (A1-A7)"]
[]
[{"v":1,"d":"1 "},null,"Clause 1.0 - Definitions and interpretation",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Pricing of bills of quantities",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor is to allow opposite each item for all costs in connection therewith. All prices to include, unless otherwise stated, for all materials, fabrication, conveyance and delivery, unloading, storing, unpacking, hoisting, labour, setting, fitting and fixing in position, cutting and waste (except where to be measured in accordance with the standard system of measurement), patterns, models and templates, plant, temporary works, returning of packaging, duties, taxes (other than Value Added Tax), imposts, establishment charges, overheads, profit and all other obligations arising out of this agreement. Value Added Tax (VAT) is to be separately stated on the summary page of these bills of quantities",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Items left unpriced will be deemed to be covered in prices against other items throughout these bills of quantities and no claim for any extras arising out of the contractor's omission to price any item will be entertained",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Prices for all construction equipment, temporary works, services and other items shall include for the supply, maintenance, operating cost and subsequent removal and making good as necessary",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Abbreviated descriptions",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The items in these bills of quantities utilise abbreviated descriptions. It is the intention that the abbreviated descriptions be fully described when read with the applicable measuring system and the relevant preambles and/or specifications. However, should the full intent and meaning of any description not be clear, the contractor shall, before submission of his tender, call for a written directive from the principal agent, failing which it shall be assumed that the contractor has allowed in his pricing for materials and workmanship in terms of international best practice",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Legal status of contractor",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"If the contractor constitutes a joint venture, consortium or other unincorporated grouping of two or more persons then:",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.   These persons are deemed to be jointly and severally liable to the employer for the performance of this agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2.   These persons shall notify the employer of their leader who has assigned authority to bind the contractor and each of these persons",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.  The contractor shall not alter its composition or legal status without the prior written consent of the employer",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":2,"d":"2 "},null,"Clause 2.0 - Law, regulations and notices",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":3,"d":"3 "},null,"Clause 3.0 - Offer and acceptance  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":4,"d":"4 "},null,"Clause 4.0 - Cession and assignment  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":5,"d":"5 "},null,"Clause 5.0 - Documents",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Value Added Tax",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Provision is made in the summary page of these bills of quantities for the inclusion of Value Added Tax (VAT)",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Electronic issue of drawings  All drawings for this project will be issued electronically and the contractor shall be deemed to have received such drawings on the date that such drawings have been dispatched electronically [5.6]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":6,"d":"6 "},null,"Clause 6.0 - Employer's agents",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Delegated authority",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The authority of the principal agent to issue contract instructions [17.1] and perform duties for specific aspects of the works is delegated to agents as follows [6.2]. This does not preclude the principal agent from issuing such contract instructions:",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1. Architect",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.1 Duties [6.2] :  The architect is responsible for the architectural design, functional design and quality inspection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.1     Rectification of discrepancies, errors in description or quantity or                  omission of items in the agreement other than in the JBCC Principal Building Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.2     Alteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.3     The site [13.0]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.4     Compliance with the law, regulations and bylaws [2.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.5     Provision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.6     Opening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.7     Removal or re-execution of work",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.8     Removal or substitution of any materials and goods",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.9     Protection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.10   Making good physical loss and repairing damage to the works [23.2.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.11   Rectification of defects [21.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.12    A list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.13\t Work by direct contractors [16.0]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.2.14   On suspension or termination, protection of the works, removal of construction equipment and surplus materials and goods [29.0]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2. Quantity surveyor",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2.1 Duties [6.2] :  The quantity surveyor is responsible for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2.2.1 No contract instructions delegated to the quantity surveyor",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3. Structural engineer",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.1 Duties [6.2] :  The structural engineer is responsible for all aspects of structural engineering design and quality inspection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.1\tRectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.2\tAlteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.3\tThe site [13.0]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.4\tCompliance with the law, regulations and bylaws [2.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.5\tProvision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.6\tOpening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.7\tRemoval or re-execution of work",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.8\tRemoval or substitution of any materials and goods",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.9\tProtection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.10\tMaking good physical loss and repairing damage to the works [23.2.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.11\tRectification of defects [21.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.2.12\tA list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4. Mechanical engineer",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.1 Duties [6.2] :  The mechanical engineer is responsible for all aspects of mechanical engineering design and quality inspection of the works and, where appointed by the employer for quantity surveying services in respect of the mechanical installations, for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.1\tRectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.2\tAlteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.3\tCompliance with the law, regulations and bylaws [2.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.4\tProvision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.5\tOpening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.6\tRemoval or re-execution of work",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.7\tRemoval or substitution of any materials and goods",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.8\tProtection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.9\tMaking good physical loss and repairing damage to the works [23.2.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.10\tRectification of defects [21.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.11\tA list for practical completion specifying outstanding or defective work to be  rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.2.12\tExpenditure of budgetary allowances, prime cost amounts and provisional sums",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5. Electrical engineer",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.1 Duties [6.2] :  The electrical engineer is responsible for all aspects of electrical engineering design and quality inspection of the works and, where appointed by the employer for quantity surveying services in respect of the electrical installations, for all measurements, valuations, financial assessments and all other quantity surveying and cost control functions",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.1\tRectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.2\tAlteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.3\tCompliance with the law, regulations and bylaws [2.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.4\tProvision and testing of samples of materials and goods and/or of finishes and assemblies of elements of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.5\tOpening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.6\tRemoval or re-execution of work",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.7\tRemoval or substitution of any materials and goods",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.8\tProtection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.9\tMaking good physical loss and repairing damage to the works [23.2.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.10\tRectification of defects [21.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.11\tA list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"5.2.12\tExpenditure of budgetary allowances, prime cost amounts and provisional sums",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6. Fire consultant",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.1 Duties [6.2] :  The fire consultant is responsible for all aspects of rational fire design and quality inspection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2 Contract instructions [6.2; 17.1] :",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.1\tRectification of discrepancies, errors in description or quantity or omission of items in the agreement other than in the JBCC Principal Building Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.2\tAlteration to design, standards or quantity of the works provided that such contract instructions shall not substantially change the scope of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.3\tCompliance with the law, regulations and bylaws [2.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.4\tProvision and testing of samples of materials and goods  and/or of finishes and assemblies of elements of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.5\tOpening up of work for inspection, removal or re-execution [23.2.4; 26.4.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.6\tRemoval or re-execution of work",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.7\tRemoval or substitution of any materials and goods",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.8\tProtection of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.9\tMaking good physical loss and repairing damage to the works [23.2.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.10\tRectification of defects [21.2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"6.2.11\tA list for practical completion specifying outstanding or defective work to be rectified to achieve practical completion, a list for completion and a list for final completion specifying outstanding or defective work to be rectified to achieve final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7. Health and safety consultant",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1 Duties [6.2] :  The health and safety consultant is responsible for all aspects of health and safety of the works. Without derogating from the generality thereof, the health and safety consultant will perform the following specific functions and duties in respect of the health and safety aspects of the works. He shall:",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1.1\tAct as the employer's agent in terms of the Construction Regulations issued in terms of the Occupational Health and Safety Act, 1993 as amended",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1.2\tPrepare and update the health and safety specification for the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1.3\tAgree with the contractor the health and safety plan for the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1.4\tCarry out regular audits to ensure adherence to the safety plan and compliance with the act and regulations",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"7.1.5\tStop the execution of the works where the agreed specification or plan is not adhered to",null,"CONT",{"v":0,"d":"0 "}]
[]
[{"v":7,"d":"7 "},null,"Clause 7.0 - Design responsibility  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Insurances and securities (A8-A11)"]
[]
[{"v":8,"d":"8 "},null,"Clause 8.0 - Works risk  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":9,"d":"9 "},null,"Clause 9.0 - Indemnities  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":10,"d":"10 "},null,"Clause 10.0 - Insurances  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":11,"d":"11 "},null,"Clause 11.0 - Securities",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor shall waive his lien or right of continuing possession of the works [11.10]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Extension of waiver of lien",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor shall ensure that a waiver of lien is included in all subcontracts and that the works executed on the site are kept free of all liens and other encumbrances at all times [11.10]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Execution (A12 - A17)"]
[]
[{"v":12,"d":"12 "},null,"Clause 12.0 - Obligations of the parties",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Office accommodation  The contractor shall provide, maintain and remove on practical completion air conditioned office accommodation with suitable tables and chairs for meetings to be held on the site. Such offices shall be kept clean and fit for use at all times [12.2.18]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Notice board  The contractor shall erect in a position approved by the principal agent, maintain and remove on practical completion a notice board recommended by the South African Institute of Architects and as approved by the principal agent listing the names and logos of the employer, the contractor and the professional consultants. No subcontractor or supplier notice boards may be erected unless permission is granted by the principal agent for such notice boards to be erected [12.2.18]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Statutory and other notices",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor shall submit and/or comply with all statutory and other notices that may be required by any local or other authority in order not to cause any delay to the commencement of the works by the contractor. The contractor shall pay all deposits or fees in this regard",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"It is, however, specifically recorded that the employer shall be responsible for the timeous approval of building plans by any local or other authorities and the payment of any fees or charges related thereto",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":13,"d":"13 "},null,"Clause 13.0 - Setting out  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":14,"d":"14 "},null,"Clause 14.0 - Nominated subcontractors",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":15,"d":"15 "},null,"Clause 15.0 - Selected subcontractors",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":16,"d":"16 "},null,"Clause 16.0 - Direct contractors  Attendance on direct contractors  In respect of direct contractors the contractor shall:",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"1.   Designate an area for the direct contractor to establish a temporary office and workshop and storage of equipment and materials",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"2.\tAllow the use of personnel welfare facilities, where provided",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"3.   Provide water, lighting and single phase electric power to a position within 50m of the place where the direct contract work is to be carried out, other than fuel or power for commissioning of any installation",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"4.   Permit the direct contractor to use erected scaffolding, hoisting facilities, etc provided by the contractor, in common with others having the like right, while it remains erected on the site [16.1]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":17,"d":"17 "},null,"Clause 17.0 - Contract instructions  Site instructions  Instructions issued on site are to be recorded in a site instruction book which is to be supplied and maintained on site by the contractor",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Completion (A18 - A24)"]
[]
[{"v":18,"d":"18 "},null,"Clause 18.0 - Interim completion",null,"N/A",{"v":0,"d":"0 "}]
[]
[{"v":19,"d":"19 "},null,"Clause 19.0 - Practical completion  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":20,"d":"20 "},null,"Clause 20.0 - Completion in sections",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":21,"d":"21 "},null,"Clause 21.0 - Defects liability period and final completion",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":22,"d":"22 "},null,"Clause 22.0 - Latent defects liability period F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":23,"d":"23 "},null,"Clause 23.0 - Revision of the date for practical completion  Substitution of materials and goods  The removal or substitution of any materials and goods which do not conform to the specification or the contract drawings shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value [17.1.8; 23.1 & 2]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":24,"d":"24 "},null,"Clause 24.0 - Penalty for late or non-completion  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Payment (A25 - A27)"]
[]
[{"v":25,"d":"25 "},null,"Clause 25.0 - Payment",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Prices submitted  Where prices are submitted by the contractor or subcontractor during the progress of the works in respect of contract instructions or in regard to a claim under the terms of this agreement and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the principal agent wish to accept any such prices prior to the issue of the certificate of final completion, it shall be in writing",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":26,"d":"26 "},null,"Clause 26.0 - Adjustment of the contract value and final account",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Fluctuations in costs  All fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor [26.9.5]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Cost of claims  All costs incurred by the contractor in the preparation of claims shall be borne by the contractor. This provision shall not preclude an adjudicator or an arbitrator appointed in terms of this agreement [30.6 & 7] from making a determination on costs",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Claims from subcontractors The contractor shall review, assess and adjudicate any claims received by him from any subcontractor and thereafter submit same to the principal agent with a recommendation in order to assist the principal agent in adjudicating the claim [26.6]",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":27,"d":"27 "},null,"Clause 27.0 - Recovery of expense and/or loss  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Suspension and termination (A28 - A29)"]
[]
[{"v":28,"d":"28 "},null,"Clause 28.0 - Suspension by the contractor",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":29,"d":"29 "},null,"Clause 29.0 - Termination",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Dispute resolution (A30)"]
[]
[{"v":30,"d":"30 "},null,"Clause 30.0 - Dispute resolution  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":31,"d":"31 "},null,"Agreement",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The required information of the parties and the amount of the contract sum shall be inserted in the agreement for signature of the agreement by the parties  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":32,"d":"32 "},null,"Contract data",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Tenderer's selections",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Before submission of his tender the contractor is to complete the tenderer's selections in the contract data",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"SECTION B:  GENERAL PRELIMINARIES"]
[]
[null,null,"Definitions and interpretation (B1)"]
[]
[{"v":33,"d":"33 "},null,"Clause 1.1 - Definitions  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":34,"d":"34 "},null,"Clause 1.2 - Interpretation  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Documents (B2)"]
[]
[{"v":35,"d":"35 "},null,"Clause 2.1 - Checking of documents  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":36,"d":"36 "},null,"Clause 2.2 - Provisional bills of quantities",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Multiple procurement  These bills of quantities are in multiple procurement format i.e all trades are provisionally measured and the subsequent trades ire ironmongery, joinery fittings, plumbing and drainage, signage and specialist waterproofing are budgetary allowances and/or provisional sums  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":37,"d":"37 "},null,"Clause 2.3 - Availability of construction information",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":38,"d":"38 "},null,"Clause 2.4 - Ordering of materials and goods  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Previous work and adjoining properties (B3)"]
[]
[{"v":39,"d":"39 "},null,"Clause 3.1 - Previous work - dimensional accuracy  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":40,"d":"40 "},null,"Clause 3.2 - Previous work - defects  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":41,"d":"41 "},null,"Clause 3.3 - Inspection of adjoining properties  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"The site (B4)"]
[]
[{"v":42,"d":"42 "},null,"Clause 4.1 - Handover of site in stages  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":43,"d":"43 "},null,"Clause 4.2 - Enclosure of the works",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"F:............................. V:............................ T:............................",null,"CONT",{"v":0,"d":"0 "}]
[]
[{"v":44,"d":"44 "},null,"Clause 4.3 - Geotechnical and other investigations  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":45,"d":"45 "},null,"Clause 4.4 - Encroachments  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":46,"d":"46 "},null,"Clause 4.5 - Existing premises occupied  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":47,"d":"47 "},null,"Clause 4.6 - Services - known  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Management of contract (B5)"]
[]
[{"v":48,"d":"48 "},null,"Clause 5.1 - Management of the works  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":49,"d":"49 "},null,"Clause 5.2 - Progress meetings  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":50,"d":"50 "},null,"Clause 5.3 - Technical meetings  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Samples, shop drawings and manufacturer's instructions (B6)"]
[]
[{"v":51,"d":"51 "},null,"Clause 6.1 - Samples of materials  F:............................. V:............................ T:...........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":52,"d":"52 "},null,"Clause 6.2 - Workmanship samples  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":53,"d":"53 "},null,"Clause 6.3 - Shop drawings  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":54,"d":"54 "},null,"Clause 6.4 - Compliance with manufacturer's instructions  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Deposits and fees (B7)"]
[]
[{"v":55,"d":"55 "},null,"Clause 7.1 - Deposits and fees  F:.......................... V:........................... T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Temporary services (B8)"]
[]
[{"v":56,"d":"56 "},null,"Clause 8.1 - Water  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":57,"d":"57 "},null,"Clause 8.2 - Electricity  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":58,"d":"58 "},null,"Clause 8.3 - Ablution and welfare facilities  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":59,"d":"59 "},null,"Clause 8.4 - Communication facilities  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Prime cost amounts (B9)"]
[]
[{"v":60,"d":"60 "},null,"Clause 9.1 - Responsibility for prime cost amounts",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null," F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Attendance on subcontractors (B10)"]
[]
[{"v":61,"d":"61 "},null,"Clause 10.1 - General attendance  User note  General attendance is defined as being the duties of the contractor in terms of clause 12.2 of the JBCC n/s subcontract agreement  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":62,"d":"62 "},null,"Clause 10.2 - Special attendance",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null," F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"General (B11)"]
[]
[{"v":63,"d":"63 "},null,"Clause 11.1 - Protection of the works  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":64,"d":"64 "},null,"Clause 11.2 - Protection/isolation of existing works and works occupied in sections F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":65,"d":"65 "},null,"Clause 11.3 - Security of the works  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":66,"d":"66 "},null,"Clause 11.4 - Notice before covering work  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":67,"d":"67 "},null,"Clause 11.5 - Disturbance",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Disturbance All work is to be carried out in such a manner as to cause no unacceptable or unreasonable dust, noise, vibrations, nuisance, inconvenience, annoyance and the like to the public, others, other properties and traffic in so far as they exceed the permissible limitations set by government legislation or by the local authority. Any delays, stoppages and the like arising from or in order to comply with the above will not constitute grounds for an adjustment to the construction period or contract value whatsoeverF:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":68,"d":"68 "},null,"Clause 11.6 - Environmental disturbance",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"Controlling all forms of pollution  The contractor shall be responsible for and take all precautions in controlling by whatever means necessary all forms of pollution emanating from the site during the construction period due inter alia to noise, artificial light, wind-blown sand, dust, deposits of mud, etc",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor is to ensure that all roads which border the site and are used by the contractor during the execution of the works are kept clean and free of any dirt or debris caused by the execution of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[{"v":69,"d":"69 "},null,"Clause 11.7 - Works cleaning and clearing  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":70,"d":"70 "},null,"Clause 11.8 - Vermin  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":71,"d":"71 "},null,"Clause 11.9 - Overhand work  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":72,"d":"72 "},null,"Clause 11.10 - Tenant installations  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":73,"d":"73 "},null,"Clause 11.11 - Advertising  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"SECTION  C: SPECIFIC PRELIMINARIES"]
[]
[{"v":74,"d":"74 "},null,"Warranties for materials and workmanship  Where warranties for materials and/or workmanship are called for, the contractor shall obtain a written warranty, addressed to the employer, from the entity supplying the materials and/or executing the work and shall deliver same to the principal agent on final completion of the contract",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The warranty shall state that workmanship, materials and installation are warranted for a specific period from the date of practical completion and that any defects that may arise during the specified period shall be made good at the expense of the entity supplying the materials and/or doing the work, upon written notice to do so",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The warranty will not be enforced if the work is damaged by defects in the execution of the works, in which case the responsibility for replacement shall rest entirely with the contractor  F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":75,"d":"75 "},null,"Overtime  Should overtime be required to be worked for any reason whatsoever, the cost of such overtime is to be borne by the contractor unless the principal agent has specifically authorised, prior to execution thereof, that costs for such overtime are to be borne by the employer  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":76,"d":"76 "},null,"Cooperation of the contractor for cost management  It is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management. The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the contract value does not exceed the budget  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":77,"d":"77 "},null,"Overloading  The contractor shall take all necessary steps to ensure that no damage occurs due to overloading of any portion of the works or temporary works e.g scaffolding, etc. The contractor shall submit details of his proposed loading, storage, plant erection, etc to the principal agent for approval prior to proceeding with such loading, storing or erecting and shall comply with and pay for the principal agent's requirements in connection with the provision of temporary support work, etc. Any damage caused to the works by overloading shall be made good by the contractor at his sole expense  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":78,"d":"78 "},null,"Propping of floors below  The contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc. The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":79,"d":"79 "},null,"Testing of flat roof waterproofing for watertightness  Flat roof waterproof areas shall be flooded and kept \"ponded\" for at least forty eight (48) hours as a test to ensure the watertightness of the waterproofing and before any further construction work is carried out above the waterproofing  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"Health and safety  Without limiting the generality of the provisions of clause 2.0, the contractor's attention is drawn to the provisions of the Construction Regulations issued in terms of the Occupational Health and Safety Act, 1993 as amended. It is specifically stated that the employer shall prepare a documented health and safety specification for the works (refer to Part 5 for a copy of the relevant specification) and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works. The contractor shall price opposite this item for compliance with the act and the regulations and the provisions of the aforementioned health and safety specification [2.1]"]
[]
[null,null,"The contractor shall:  1.   Comply with the health and safety specification for the works  2.   Prepare and agree with the health and safety consultant the health and  safety plan for the works  3.   Cooperate with the health and safety consultant in all respects  4.   Manage the compliance of all subcontractors with the regulations and with the health and safety plan and specification  5.   Conform to the conditions contained in the employer's health and safety specification"]
[]
[null,null,"F:............................. V:............................ T:............................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":80,"d":"80 "},null,"Broad based black economic empowerment (BBBEE)  Tenders submitted will be evaluated taking into account their empowerment rating  The employer will be monitoring the broad based black economic empowerment (BBBEE) status of the contractor throughout the execution of the works",null,"CONT",{"v":0,"d":"0 "}]
[]
[null,null,"The contractor is to submit to the principal agent on an annual basis a schedule of spend, split into vendors engaged as subcontractors and suppliers indicating their BBBEE rating including proof of the said rating  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":81,"d":"81 "},null,"Advertising rights  The employer may elect to contract with advertising agencies for the erection of advertising hoardings, banners, wraps or the like for the duration of the contract. The contractor shall not prevent such an arrangement and will assist in the facilitation of same. The position and type of advertising structure to be agreed with the principal agent so as not to hinder the contractor in meeting his obligations under this agreement  F:........................ V:.........................T:.........................",null,"N/A",{"v":0,"d":"0 "}]
[]
[{"v":82,"d":"82 "},null,"Confidentiality  The contractor undertakes to maintain in confidence any and all information regarding this project and shall obtain appropriate similar undertakings from all subcontractors and suppliers. Such information shall not be used in any way except in connection with the execution of the works  No information regarding this project shall be published or disclosed without the prior written consent of the employer  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":83,"d":"83 "},null,"Media releases  All rights of publication of articles in the media, together with any advertising relating thereto or in any way connected with this project, shall vest with the employer  The contractor together with his subcontractors shall not, without the prior written consent of the employer, cause any statement or advertisement connected with this project to be printed, screened or aired by the media  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":84,"d":"84 "},null,"Allow for the relocation of the Contractors camp from phase 1 (block A scope of work) to phase 2 (block B scope of work). Should phase 2 not form part of this contract this amount will be omitted from the final contract value  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[{"v":85,"d":"85 "},null,"Provide an amount as \"caretaker preliminaries\" for one month between phases 1 and 2 of the contract. Should phase 2 not form part of this contract this amount will be omitted from the final contract value  F:........................ V:.........................T:.........................",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"SUMMARY OF CATEGORIES"]
[]
[null,null,"Category : Fixed   R........................................  Category : Value   R........................................  Category : Time    R........................................"]
[]
[null,null,"SECTION 2"]
[]
[null,null,"BILL NO. 1"]
[]
[null,null,"ALTERATIONS"]
[]
[null,null,"View site"]
[]
[null,null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials salvageable from the alterations.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,null,"Explosives"]
[]
[null,null,"No explosives whatsoever may be used for alteration purposes unless otherwise stated"]
[]
[null,null,"General"]
[]
[null,null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent"]
[]
[null,null,"With regard to building up of openings in existing walls, cement screeds and pavings, granolithic, tops of walls, etc, shall be levelled and prepared for raising of brickwork"]
[]
[null,null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[null,null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc)"]
[]
[null,null,"Removal or demolition of existing work comprising or containing asbestos products"]
[]
[null,null,"Where existing works comprising or containing asbestos products are removed or demolished, the Contractor shall ensure that such work is conducted in accordance with the provisions of the Asbestos Regulations promulgated by Government Notice No. R155 of 10 February 2002, as amended, as provided for in clause 14 (9) of the Construction Regulations.  Such works shall be carried out by a company registered with the Department of Labour as an Asbestos Contractor.  Prior to the commencement of such works, a plan of work approved by an approved Asbestos Inspection Authority shall be submitted to the Provincial Director/Provincial Executive Manager."]
[]
[null,null,"REMOVAL OF EXISTING WORK"]
[]
[null,null,"Breaking up and removing brick paving"]
[]
[{"v":1,"d":"1 "},null,"85mm Thick brick paving with mortar joints and sand bedding",null,"m²",{"v":26,"d":"26 "}]
[]
[{"v":2,"d":"2 "},null,"Precast concrete grass blocks",null,"m²",{"v":83,"d":"83 "}]
[]
[{"v":3,"d":"3 "},null,"Precast kerbs",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement"]
[]
[{"v":4,"d":"4 "},null,"Saw cut through approximately 75mm thick tarmac surfaces including breaking up and removing",null,"m²",{"v":33,"d":"33 "}]
[]
[{"v":5,"d":"5 "},null,"200mm Thick shower plinth",null,"m³",{"v":0.2,"d":"0 "}]
[]
[{"v":6,"d":"6 "},null,"Screed on floors",null,"m²",{"v":1,"d":"1 "}]
[]
[null,null,"Breaking down and removing brickwork etc"]
[]
[{"v":7,"d":"7 "},null,"One brick walls",null,"m²",{"v":42,"d":"42 "}]
[]
[{"v":8,"d":"8 "},null,"280mm thick brick walls including glass block windows exceeding 2.5m\"² and not exceeding not exceeding 5m\"²",null,"m²",{"v":3,"d":"3 "}]
[]
[{"v":9,"d":"9 "},null,"Loffelstein retaining wall",null,"m²",{"v":32,"d":"32 "}]
[]
[null,null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[]
[{"v":10,"d":"10 "},null,"Existing shade cloth canopy from steel structure",null,"m²",{"v":85,"d":"85 "}]
[]
[{"v":11,"d":"11 "},null,"Entire existing shade cloth and metal structure including foundation",null,"m²",{"v":17,"d":"17 "}]
[]
[{"v":12,"d":"12 "},null,"Acoustic tile suspended ceilings tiles",null,"m²",{"v":817,"d":"817 "}]
[]
[{"v":13,"d":"13 "},null,"Acoustic tile suspended ceilings, including suspension grid, hangers, cornices, etc.",null,"m²",{"v":278,"d":"278 "}]
[]
[{"v":14,"d":"14 "},null,"Drywall partitions 3m high, including doors, glazed, borrowed lights, etc",null,"m",{"v":223,"d":"223 "}]
[]
[{"v":15,"d":"15 "},null,"Drywall partitions 1.5m high, including doors, glazed, borrowed lights, etc",null,"m",{"v":8,"d":"8 "}]
[]
[{"v":16,"d":"16 "},null,"Protruding 1800 x 1800mm ceiling system, suspended from existing ceiling system",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":17,"d":"17 "},null,"Cut back approximately 400mm rafters back in with gutters exceeding 10m but not exceeding 11.5m",null,"No",{"v":86,"d":"86 "}]
[]
[null,null,"Taking out and removing sundry joinery work, fittings, etc"]
[]
[{"v":18,"d":"18 "},null,"Power skirting fixed to walls",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":19,"d":"19 "},null,"Tile skirtings 100mm high",null,"m",{"v":108,"d":"108 "}]
[]
[{"v":20,"d":"20 "},null,"Timber skirtings 100mm high",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":21,"d":"21 "},null,"Cover strip",null,"m",{"v":1,"d":"1 "}]
[]
[null,null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings"]
[]
[{"v":22,"d":"22 "},null,"Carpet tile floor covering and glue",null,"m²",{"v":1170,"d":"1,170 "}]
[]
[{"v":23,"d":"23 "},null,"Vinyl floor covering",null,"m²",{"v":50,"d":"50 "}]
[]
[null,null,"Taking down and removing steel fencing and gates"]
[]
[{"v":24,"d":"24 "},null,"Take down and remove existing 1000mm high stainless steel balustrades as well as fixings on the concrete floor",null,"m",{"v":26,"d":"26 "}]
[]
[{"v":25,"d":"25 "},null,"Palisade fencing including posts",null,"m",{"v":21,"d":"21 "}]
[]
[{"v":26,"d":"26 "},null,"Take down and remove existing welded metal mesh panel with steel tube sub frame bolted onto concrete and brickwork 2600mm high",null,"m",{"v":7,"d":"7 "}]
[]
[{"v":27,"d":"27 "},null,"Take down and remove existing welded metal mesh panel double gate with steel tube sub frame bolted onto concrete and brickwork 2600mm high",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc"]
[]
[{"v":28,"d":"28 "},null,"Internal plaster from walls and columns",null,"m²",{"v":214,"d":"214 "}]
[]
[{"v":29,"d":"29 "},null,"External plaster from walls and columns",null,"m²",{"v":195,"d":"195 "}]
[]
[null,null,"Hacking up/off and removing waterproofing on surfaces and prepare for new waterproofing"]
[]
[{"v":30,"d":"30 "},null,"Bituminous waterproofing on parapet walls",null,"m²",{"v":12,"d":"12 "}]
[]
[{"v":31,"d":"31 "},null,"Bituminous waterproofing on concrete roofs to falls",null,"m²",{"v":231,"d":"231 "}]
[]
[{"v":32,"d":"32 "},null,"Polyurethane sealant in floors",null,"m",{"v":7,"d":"7 "}]
[]
[{"v":33,"d":"33 "},null,"Polyurethane sealant around air grids",null,"m",{"v":99,"d":"99 "}]
[]
[{"v":34,"d":"34 "},null,"Polyurethane sealant around sanitary fittings",null,"m",{"v":13,"d":"13 "}]
[]
[null,null,"Hacking up/off and removing ceramic tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc"]
[]
[{"v":35,"d":"35 "},null,"300 x 300mm Tiles to bathroom walls",null,"m²",{"v":193,"d":"193 "}]
[]
[{"v":36,"d":"36 "},null,"Tiles to shower floors",null,"m²",{"v":1,"d":"1 "}]
[]
[{"v":37,"d":"37 "},null,"Tiles to floors",null,"m²",{"v":180,"d":"180 "}]
[]
[null,null,"Hacking up/off and removing slate tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc. Set tiles aside for later use."]
[]
[{"v":38,"d":"38 "},null,"Tiles to floors",null,"m²",{"v":159,"d":"159 "}]
[]
[null,null,"Taking out and removing doors, windows, etc, including thresholds, sills, etc (building up openings and making good finishes elsewhere)"]
[]
[{"v":39,"d":"39 "},null,"Timber single door and frame in half brick wall not exceeding 2,5m\"²",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":40,"d":"40 "},null,"Timber single door and frame in 90mm drywall not exceeding 2,5m\"²",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":41,"d":"41 "},null,"Timber double door and frame in half brick wall not exceeding 2,5m\"²",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":42,"d":"42 "},null,"Timber double door and frame in 90mm drywall exceeding 2,5m\"² not exceeding 5m\"²",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":43,"d":"43 "},null,"Glazed aluminium window in 280mm brick wall not exceeding 2,5m\"²",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":44,"d":"44 "},null,"Glazed aluminium window exceeding 7.5m\"² and not exceeding 10m\"² in 280mm brick wall",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Taking out and removing piping, including cutting off as necessary, holder bats and making good floor and wall finishes (making good tiling and paintwork elsewhere)"]
[]
[{"v":45,"d":"45 "},null,"Rainwater down pipe from wall",null,"m",{"v":19,"d":"19 "}]
[]
[{"v":46,"d":"46 "},null,"PVC piping not exceeding 50mm external diameter",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":47,"d":"47 "},null,"Existing rainwater downpipe outlet",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":48,"d":"48 "},null,"Flanged side outlets on concrete slabs",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":49,"d":"49 "},null,"600 x 600mm Catch pit",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good wall and floor finishes (measured elsewhere)"]
[]
[{"v":50,"d":"50 "},null,"Vitreous china wash hand basin",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":51,"d":"51 "},null,"Stainless steel double sink including disconnecting waste pipe",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":52,"d":"52 "},null,"Stainless steel single sink including disconnecting waste pipe",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":53,"d":"53 "},null,"Shower mixer and rose",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":54,"d":"54 "},null,"Shower trap and plumbing fittings",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":55,"d":"55 "},null,"Toilet seat",null,"No",{"v":10,"d":"10 "}]
[]
[{"v":56,"d":"56 "},null,"Hydro boil fixed to wall including disconnecting pipes",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":57,"d":"57 "},null,"900 x 900mm high mirror from wall",null,"No",{"v":6,"d":"6 "}]
[]
[null,null,"Taking out and removing sundry joinery work, fittings, etc"]
[]
[{"v":58,"d":"58 "},null,"600mm wide x 900mm high floor mounted cupboard including countertop",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":59,"d":"59 "},null,"400mm wide x 800mm high wall mounted cupboard",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":60,"d":"60 "},null,"5000 x 600 x 2400mm high built in cupboard",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":61,"d":"61 "},null,"3150 x 600 x 1100mm high built in cupboard",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":62,"d":"62 "},null,"2200 x 3700mm L shaped reception counter",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":63,"d":"63 "},null,"2200 x 600 x 900mm high kitchen unit",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":64,"d":"64 "},null,"600mm x 3000mm x 900mm high floor mounted cupboard",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":65,"d":"65 "},null,"500 x 1200 x 900mm high kitchen built in cupboard",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"MAINTENANCE OF EXISTING WORK"]
[]
[null,null,"Refit and reposition existing doors, ironmongery, etc"]
[]
[{"v":66,"d":"66 "},null,"Service existing single door to securely close and refix hinges where required",null,"No",{"v":21,"d":"21 "}]
[]
[null,null,"Cleaning and servicing"]
[]
[{"v":67,"d":"67 "},null,"Clean and service existing gullies",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Taking out and removing window dressings"]
[]
[{"v":68,"d":"68 "},null,"Remove 1200mm high blinds from brick walls",null,"m",{"v":43,"d":"43 "}]
[]
[{"v":69,"d":"69 "},null,"Remove 1900mm high blinds from brick walls",null,"m",{"v":27,"d":"27 "}]
[]
[{"v":70,"d":"70 "},null,"Remove 2100mm high blinds from brick walls",null,"m",{"v":54,"d":"54 "}]
[]
[null,null,"MAKING GOOD OF FINISHES ETC"]
[]
[null,null,"Making good face brickwork"]
[]
[{"v":71,"d":"71 "},null,"Remove stains and glue from external face brick walls",null,"m²",{"v":4,"d":"4 "}]
[]
[{"v":72,"d":"72 "},null,"Wash and remove water damage  from face brick wall",null,"m²",{"v":16,"d":"16 "}]
[]
[{"v":73,"d":"73 "},null,"Making good brick walls where 230mm wall was removed",null,"m²",{"v":0.2,"d":"0 "}]
[]
[null,null,"Making good internal plastered brickwork"]
[]
[{"v":74,"d":"74 "},null,"Fill in drill hole in walls and make even surfaces",null,"m²",{"v":8,"d":"8 "}]
[]
[{"v":75,"d":"75 "},null,"Repair hairline cracks in walls and make good to receive paint (paint measured elsewhere)",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"Making good cement screeds"]
[]
[{"v":76,"d":"76 "},null,"Making good floors where 230mm wall were removed",null,"m²",{"v":1,"d":"1 "}]
[]
[{"v":77,"d":"77 "},null,"70mm Thick on floors to falls to receive waterproofing",null,"m²",{"v":210,"d":"210 "}]
[]
[null,null,"Making good timber surfaces"]
[]
[{"v":78,"d":"78 "},null,"Sand down, make even timber handrails and prepare for new paintwork (paintwork elsewhere measured)",null,"m",{"v":14,"d":"14 "}]
[]
[null,null,"Making good lift doors"]
[]
[{"v":79,"d":"79 "},null,"Remove stains, paint and make good 1800 x 2100mm high lift bi-parting doors",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Remove existing airconditioning ducts along external building fa×§ade and build up opening (building up elsewhere)"]
[]
[{"v":80,"d":"80 "},null,"1000 x 650mm high air conditioning louvres not exceeding 2.5m above natural ground level",null,"No",{"v":17,"d":"17 "}]
[]
[{"v":81,"d":"81 "},null,"1000 x 650mm high air conditioning louvres exceeding 5m and not exceeding 7.5m above natural ground level",null,"No",{"v":27,"d":"27 "}]
[]
[{"v":82,"d":"82 "},null,"1000 x 650mm high air conditioning louvres exceeding 7.5m and not exceeding 10m above natural ground level",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"Remove sealant and reseal with neutral-cure silicon sealant"]
[]
[{"v":83,"d":"83 "},null,"Around 1600 x 650mm high air conditioning louvres on both sides",null,"No",{"v":11,"d":"11 "}]
[]
[null,null,"OPENINGS THROUGH EXISTING WALLS ETC"]
[]
[null,null,"Altering openings"]
[]
[{"v":84,"d":"84 "},null,"Altering opening in one brick wall where 1500 x 1200m high aluminium window removed to form opening for new double door and frame 1800 x 2100m high overall by breaking out brickwork on both sides and bottom, including prestressed concrete lintels, making good cement plaster on one side and into reveals and face brickwork on other side and into reveals and with 20 MPa concrete threshold with steel trowelled finish (new door and frame  and making good paintwork elsewhere)",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":85,"d":"85 "},null,"Altering opening in one brick wall where 1500 x 1200m high aluminium window removed to form opening 1800 x 2100m high overall by breaking out brickwork on both sides and bottom, including prestressed concrete lintels, making good cement plaster on one side and into reveals and face brickwork on other side and into reveals and with 20 MPa concrete threshold with steel trowelled finish",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":86,"d":"86 "},null,"Altering opening in one brick wall where 900 x 600m high aluminium window removed to form opening 1800 x 2100m high overall by breaking out brickwork on both sides and bottom, including prestressed concrete lintels, making good cement plaster on one side and into reveals and face brickwork on other side and into reveals and with 20 MPa concrete threshold with steel trowelled finish",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Breaking out for and forming plain openings through brick walls, including prestressed concrete lintels, making good cement plaster on both sides and into reveals and with 20 MPa concrete thresholds with steel trowelled finish (making good paintwork elsewhere)"]
[]
[{"v":87,"d":"87 "},null,"Opening 1500 x 600mm high through one brick wall",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Breaking out for and forming openings through brick walls for new louvres, including precast lintels, making good cement plaster on both sides and into reveals (new louvres and making good paintwork elsewhere)"]
[]
[{"v":88,"d":"88 "},null,"Opening for weather louvre 250 x 200m high through 280mm brick wall",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":89,"d":"89 "},null,"Opening for weather louvre 300 x 250m high through 280mm brick wall",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":90,"d":"90 "},null,"Opening for weather louvre 300 x 300m high through 280mm brick wall",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":91,"d":"91 "},null,"Opening for weather louvre 300 x 350m high through 280mm brick wall",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BUILDING UP OPENINGS"]
[]
[null,null,"Brickwork in NFX bricks in class II mortar in building up openings"]
[]
[{"v":92,"d":"92 "},null,"280mm brick walls including brick reinforcement",null,"m²",{"v":52,"d":"52 "}]
[]
[null,null,"Sundries"]
[]
[{"v":93,"d":"93 "},null,"Cutting toothing and bonding new brickwork to existing",null,"m²",{"v":19,"d":"19 "}]
[]
[null,null,"BUILDERS WORK"]
[]
[{"v":94,"d":"94 "},null,"Budgetary allowance of R 10 000.00 for general builders work",null,"Item",{"v":1,"d":"1 "}]
[]
[null,null,"HOLES ETC"]
[]
[null,null,"Core drilling hole exceeding 50mm and not exceeding 100mm diameter"]
[]
[{"v":95,"d":"95 "},null,"280mm Thick reinforced concrete slab, beam, wall, etc",null,"No",{"v":23,"d":"23 "}]
[]
[{"v":96,"d":"96 "},null,"Deduct:\tAllowance of credit for materials salvaged from the works",null,"Item",{"v":0,"d":"0 "}]
[]
[null,null,"BILL NO. 2"]
[]
[null,null,"EARTHWORKS"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SITE CLEARANCE"]
[]
[null,null,"Site clearance"]
[]
[{"v":97,"d":"97 "},null,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth",null,"m²",{"v":12,"d":"12 "}]
[]
[null,null,"REMOVAL OF TREES ETC"]
[]
[null,null,"Taking out and removing, grubbing up roots, filling in holes and compacting to 95% Mod AASHTO density"]
[]
[{"v":98,"d":"98 "},null,"Tree stump exceeding 1m high, not exceeding 200mm girth",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"EXCAVATION, FILLING, ETC"]
[]
[null,null,"Excavation in earth not exceeding 2m deep"]
[]
[{"v":99,"d":"99 "},null,"Reduce levels under floors",null,"m³",{"v":7,"d":"7 "}]
[]
[{"v":100,"d":"100 "},null,"Trenches",null,"m³",{"v":108,"d":"108 "}]
[]
[{"v":101,"d":"101 "},null,"Holes",null,"m³",{"v":5,"d":"5 "}]
[]
[null,null,"WORKING SPACE EXCAVATIONS"]
[]
[null,null,"Back excavation of vertical sides of excavation in earth exceeding 500mm and not exceeding 1,5m deep for working space, including backfilling compacted to 93% Mod AASHTO density"]
[]
[{"v":102,"d":"102 "},null,"For placing and removing formwork to footings, bases, walls etc against excavated face",null,"m²",{"v":223,"d":"223 "}]
[]
[null,null,"SUNDRIES"]
[]
[null,null,"Extra over all excavations for carting away"]
[]
[{"v":103,"d":"103 "},null,"Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor",null,"m³",{"v":1306,"d":"1,306 "}]
[]
[null,null,"Risk of collapse of excavations"]
[]
[{"v":104,"d":"104 "},null,"Sides of trench and hole excavations not exceeding 1,5m deep",null,"m²",{"v":246,"d":"246 "}]
[]
[null,null,"Keeping excavations free of water"]
[]
[{"v":105,"d":"105 "},null,"Keeping excavations free of water",null,"Item",{"v":2,"d":"2 "}]
[]
[null,null,"FILLING ETC"]
[]
[null,null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 100% Mod AASHTO density"]
[]
[{"v":106,"d":"106 "},null,"Backfilling to trenches, holes, etc",null,"m³",{"v":35,"d":"35 "}]
[]
[null,null,"Selected G5 filling supplied by the contractor, compacted to 95% Mod AASHTO density in layers of 100mm"]
[]
[{"v":107,"d":"107 "},null,"Under floors, steps, pavings, etc",null,"m³",{"v":1456,"d":"1,456 "}]
[]
[null,null,"Selected G7 filling supplied by the contractor, compacted to 95% Mod AASHTO density in layers of 100mm"]
[]
[{"v":108,"d":"108 "},null,"Under floors, steps, paving",null,"m³",{"v":47,"d":"47 "}]
[]
[null,null,"Sand filling supplied by the contractor, compacted to 100% Mod AASHTO density"]
[]
[{"v":109,"d":"109 "},null,"Under floors, steps, pavings, etc",null,"m³",{"v":8,"d":"8 "}]
[]
[null,null,"Compaction of surfaces"]
[]
[{"v":110,"d":"110 "},null,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density",null,"m²",{"v":315,"d":"315 "}]
[]
[null,null,"Prescribed density tests on filling"]
[]
[{"v":111,"d":"111 "},null,"\"Modified AASHTO Density\" test",null,"No",{"v":25,"d":"25 "}]
[]
[null,null,"SOIL POISONING"]
[]
[null,null,"Soil insecticide"]
[]
[{"v":112,"d":"112 "},null,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming",null,"m²",{"v":292,"d":"292 "}]
[]
[{"v":113,"d":"113 "},null,"To bottoms and sides of trenches etc",null,"m²",{"v":293,"d":"293 "}]
[]
[null,null,"BILL NO. 3"]
[]
[null,null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Cost of tests"]
[]
[null,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the architect.  The testing shall be undertaken by an independent firm or institution nominated by the contractor and to the approval of the architect.  (Test cubes are measured separately)"]
[]
[null,null,"Formwork"]
[]
[null,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[null,null,"The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself"]
[]
[null,null,"Formwork to soffits of solid slabs, etc shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described"]
[]
[null,null,"Formwork to soffits of slabs, beams, etc shall be deemed to be propped up exceeding 1,5m and not exceeding 3,5m high unless otherwise described"]
[]
[null,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons. Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[null,null,"Smooth Formwork"]
[]
[null,null,"Formwork described as smooth formwork (degree of accuracy 1) shall be formwork to dense well compacted concrete showing the slight grain marks of planed boards or smooth plywood with well fitted joints and sound arises, with a surface within degree of accuracy 1 complying with SANS 20001 (Part CC1)  Shuttering panel and tie-rod layout shall be to the approval of the Engineer.  Formwork ties permanently cast in are subject to the approval of the Engineer. Wire ties are not permitted.  Preparation of a sample panel is provided for in these bills of quantities"]
[]
[null,null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES"]
[]
[null,null,"15MPa/20mm concrete"]
[]
[{"v":114,"d":"114 "},null,"Surface blinding under footings and bases",null,"m³",{"v":12,"d":"12 "}]
[]
[null,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES"]
[]
[null,null,"25MPa/20mm concrete"]
[]
[{"v":115,"d":"115 "},null,"Strip footings",null,"m³",{"v":26,"d":"26 "}]
[]
[null,null,"30MPa/19mm concrete"]
[]
[{"v":116,"d":"116 "},null,"Bases",null,"m³",{"v":2,"d":"2 "}]
[]
[{"v":117,"d":"117 "},null,"Surface beds on waterproofing",null,"m³",{"v":20,"d":"20 "}]
[]
[null,null,"REINFORCED CONCRETE"]
[]
[null,null,"30MPa/19mm concrete"]
[]
[{"v":118,"d":"118 "},null,"Cavity infill to brick cavity walls",null,"m³",{"v":2,"d":"2 "}]
[]
[{"v":119,"d":"119 "},null,"Cavity infill to brick piers",null,"m³",{"v":2,"d":"2 "}]
[]
[{"v":120,"d":"120 "},null,"Stairs, including landings, beams and inverted beams",null,"m³",{"v":3,"d":"3 "}]
[]
[null,null,"TEST CUBES"]
[]
[{"v":121,"d":"121 "},null,"Making and testing a set of three 150 x 150 x 150mm concrete strength test cubes",null,"No",{"v":8,"d":"8 "}]
[]
[null,null,"CONCRETE SUNDRIES"]
[]
[null,null,"\"Full-flow\" cast iron outlets"]
[]
[{"v":122,"d":"122 "},null,"100mm 45 Degree side outlet and connecting to existing piping",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"35MPa non-shrink structural grout"]
[]
[{"v":123,"d":"123 "},null,"Bedding approximately 25mm thick under300 x 300mm base plate",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"MOVEMENT JOINTS ETC"]
[]
[null,null,"Two layers of 375 micron \"Consol Plastic Brickgrip DPC\" in slip joints between horizontal concrete and brick surfaces, including cement mortar bed"]
[]
[{"v":124,"d":"124 "},null,"Not exceeding 300mm wide",null,"m",{"v":49,"d":"49 "}]
[]
[null,null,"Expansion joints with bitumen impregnated  softboard between vertical concrete surfaces"]
[]
[{"v":125,"d":"125 "},null,"10mm Joints not exceeding 300mm high along edges of surface beds",null,"m",{"v":9,"d":"9 "}]
[]
[null,null,"Expansion joints with bitumen impregnated softboard between vertical concrete surfaces, including necessary formwork"]
[]
[{"v":126,"d":"126 "},null,"Not exceeding 300mm wide between brick piers",null,"m",{"v":34,"d":"34 "}]
[]
[null,null,"Saw cut joints"]
[]
[{"v":127,"d":"127 "},null,"30 x 3mm Saw cut joints in top of concrete",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"ROUGH FORMWORK"]
[]
[null,null,"Rough formwork to sides"]
[]
[{"v":128,"d":"128 "},null,"Strip footings",null,"m²",{"v":61,"d":"61 "}]
[]
[{"v":129,"d":"129 "},null,"Bases",null,"m²",{"v":9,"d":"9 "}]
[]
[{"v":130,"d":"130 "},null,"Edges, risers, ends and reveals not exceeding 300mm high or wide",null,"m",{"v":55,"d":"55 "}]
[]
[{"v":131,"d":"131 "},null,"Sloping and stepped outer edges of stairs not exceeding 400mm high extreme",null,"m",{"v":16,"d":"16 "}]
[]
[null,null,"Rough formwork to soffits"]
[]
[{"v":132,"d":"132 "},null,"Raking soffits of stairs",null,"m²",{"v":9,"d":"9 "}]
[]
[null,null,"REINFORCEMENT"]
[]
[null,null,"Mild steel reinforcement"]
[]
[{"v":133,"d":"133 "},null,"Various diameter bars",null,"t",0.36]
[]
[null,null,"High tensile steel reinforcement"]
[]
[{"v":134,"d":"134 "},null,"Various diameter bars",null,"t",1.98]
[]
[{"v":135,"d":"135 "},null,"Y20 dowels in brick piers",null,"m",{"v":17,"d":"17 "}]
[]
[null,null,"Fabric reinforcement"]
[]
[{"v":136,"d":"136 "},null,"Type 245 reinforcement in surface beds, slabs, etc",null,"m²",{"v":134,"d":"134 "}]
[]
[null,null,"BILL NO. 4"]
[]
[null,null,"MASONRY"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"FOUNDATIONS"]
[]
[null,null,"14 MPa Brickwork of NFX bricks in class II mortar"]
[]
[{"v":137,"d":"137 "},null,"Rectangular shaped piers",null,"m³",{"v":1,"d":"1 "}]
[]
[{"v":138,"d":"138 "},null,"One brick walls in foundations",null,"m²",{"v":23,"d":"23 "}]
[]
[{"v":139,"d":"139 "},null,"280mm hollow brick walls of two half brick skins including wire ties with 50mm cavity filled solid foundation wall (concrete filling elsewhere measured)",null,"m²",{"v":46,"d":"46 "}]
[]
[null,null,"SUPERSTRUCTURE"]
[]
[null,null,"14 MPa Brickwork of NFX bricks in class II mortar"]
[]
[{"v":140,"d":"140 "},null,"Rectangular shaped piers",null,"m³",{"v":4,"d":"4 "}]
[]
[{"v":141,"d":"141 "},null,"One brick walls",null,"m²",{"v":50,"d":"50 "}]
[]
[{"v":142,"d":"142 "},null,"280mm hollow walls of two half brick skin including wire ties",null,"m²",{"v":119,"d":"119 "}]
[]
[null,null,"FACE BRICKWORK"]
[]
[null,null,"\"Buff Travertine FBS\" or similar and approved face bricks pointed with flush horizontal and vertical joints"]
[]
[{"v":143,"d":"143 "},null,"Extra over brickwork for face brickwork",null,"m²",{"v":250,"d":"250 "}]
[]
[{"v":144,"d":"144 "},null,"Fair raking cutting",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":145,"d":"145 "},null,"Extra over brickwork for brick-on-edge stretcher course bands one course high",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"BRICKWORK SUNDRIES"]
[]
[null,null,"Miscellaneous"]
[]
[{"v":146,"d":"146 "},null,"Splayed mortar fillet one course high in 50mm cavity",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":147,"d":"147 "},null,"Closing 50mm cavity of hollow wall vertically with brickwork half brick wide",null,"m",{"v":29,"d":"29 "}]
[]
[{"v":148,"d":"148 "},null,"Closing 50mm cavity of hollow wall horizontally with one course of brickwork",null,"m",{"v":9,"d":"9 "}]
[]
[{"v":149,"d":"149 "},null,"Vertical chasing into existing brickwork not deeper than one third of the wall/leaf thickness or 30mm and solidly filled with mortar once conduits are in place",null,"m",{"v":142,"d":"142 "}]
[]
[{"v":150,"d":"150 "},null,"Horizontal chasing into existing brickwork not deeper than one sixth of the wall/leaf thickness and not exceeding 1250mm in length and solidly filled with mortar once conduits are in place",null,"m",{"v":142,"d":"142 "}]
[]
[null,null,"Brickwork reinforcement"]
[]
[{"v":151,"d":"151 "},null,"75mm Wide reinforcement built in horizontally in foundations (Provisional)",null,"m",{"v":1075,"d":"1,075 "}]
[]
[{"v":152,"d":"152 "},null,"75mm Wide reinforcement built in horizontally",null,"m",{"v":747,"d":"747 "}]
[]
[{"v":153,"d":"153 "},null,"150mm Wide reinforcement built in horizontally in foundations (Provisional)",null,"m",{"v":272,"d":"272 "}]
[]
[{"v":154,"d":"154 "},null,"150mm Wide reinforcement built in horizontally",null,"m",{"v":254,"d":"254 "}]
[]
[null,null,"Pre-stressed fabricated lintels"]
[]
[{"v":155,"d":"155 "},null,"90 x 90mm Lintels in lengths not exceeding 3m",null,"m",{"v":12,"d":"12 "}]
[]
[null,null,"Copings, sills, etc to the architect's approval, including facing and pointing on all exposed faces"]
[]
[{"v":156,"d":"156 "},null,"600 x 480mm paving coping on brick piers",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Galvanised hoop iron cramps, ties, etc"]
[]
[{"v":157,"d":"157 "},null,"300 x 40 x 1,6mm  wall tie strips shot pinned to existing brickwork and with ties bent out and built into new brickwork",null,"m",{"v":89,"d":"89 "}]
[]
[null,null,"BLOCKWORK"]
[]
[null,null,"SUPERSTRUCTURE"]
[]
[null,null,"Blockwork in class ll mortar"]
[]
[{"v":158,"d":"158 "},null,"90mm block walls",null,"m²",{"v":20,"d":"20 "}]
[]
[null,null,"BLOCKWORK SUNDRIES"]
[]
[null,null,"Cement wash of 1:3 liquid cement and sand mixture applied with a brush"]
[]
[{"v":159,"d":"159 "},null,"On brick walls, piers, etc",null,"m²",{"v":20,"d":"20 "}]
[]
[null,null,"PAVING"]
[]
[null,null,"New 73mm De Hoop Red paving bricks with butt joints on 10mm thick river sand bed with sand and cements mixture swept into joints and hosed down, including preparation of ground or filling"]
[]
[{"v":160,"d":"160 "},null,"Paving in herring bond to fall",null,"m²",{"v":158,"d":"158 "}]
[]
[null,null,"BILL NO. 5"]
[]
[null,null,"WATERPROOFING"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"DAMP PROOFING OF WALLS AND FLOORS"]
[]
[null,null,"One layer of 250\"µm damp proof course in conforming to SANS 952-1:2011 laid with minimum 150mm overlaps. bearing SABS 952 -1: Type B with minimum 150mm overlaps at joints and intersections and bedded and joined in cement mortar."]
[]
[{"v":161,"d":"161 "},null,"In walls",null,"m²",{"v":55,"d":"55 "}]
[]
[null,null,"Gunplas USB Green 3 LAYER 170\"® damp proof sheeting bearing SABS 952 - 1: 2010 shall be laid in the widest practical widths to minimize joints and shall be turned down, dressed to ground beams. DPC may be lapped according to manufacturer\"€™s specifications. DPC conforming to SANS 952-1:2011 laid with minimum 150mm overlaps and sealed with Gunplas pressure sensitive tape"]
[]
[{"v":162,"d":"162 "},null,"Under surface beds",null,"m²",{"v":136,"d":"136 "}]
[]
[null,null,"JOINT SEALANTS ETC"]
[]
[null,null,"Mastic sealing compound including backing cord, bond breaker, primer, etc as per architect specifications"]
[]
[{"v":163,"d":"163 "},null,"25 x 20mm in joints between frames and walls",null,"m",{"v":1397,"d":"1,397 "}]
[]
[{"v":164,"d":"164 "},null,"25 x 20mm in joints between sanitary fittings and walls",null,"m",{"v":13,"d":"13 "}]
[]
[null,null,"ABE Construction Chemicals Durakol G LM manganese cured, low modulus polysulphide sealant applied, including the use of epidermix 391 and epidermix 326 primers where required, all in accordance with the manufacturer's instructions"]
[]
[{"v":165,"d":"165 "},null,"12 x 10mm In expansion joints in floors",null,"m",{"v":16,"d":"16 "}]
[]
[{"v":166,"d":"166 "},null,"30 x 3mm In saw cut joints in floors",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"BILL NO. 6"]
[]
[null,null,"ROOF COVERINGS, ETC."]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"PROFILED METAL SHEETING AND ACCESSORIES"]
[]
[null,null,"Youngman Roofing Springlok concealed fix profile 0.47mm TCT Clean COLORBOND\"„¢ steel - Ultra, metallic coating AZ200 (minimum 200g/m\"² coating mass), G300 (minimum yield strength 300 MPa), super polyester paint system, 25um on topside and 10um on reverse side, as per manufacturer's instructions Top colour: White Underside: Light Grey"]
[]
[{"v":167,"d":"167 "},null,"Roof coverings with pitches not exceeding 25 degrees",null,"m²",{"v":22,"d":"22 "}]
[]
[{"v":168,"d":"168 "},null,"230 x 77mm Side wall flashing overlapping two ribs - prepainted",null,"m",{"v":6,"d":"6 "}]
[]
[{"v":169,"d":"169 "},null,"230 x 150mm Head wall flashing overlapping two ribs - prepainted",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":170,"d":"170 "},null,"30 x 112mm Counter flashing overlapping, cut and sealed into wall minimum 50mm deep - prepainted",null,"m",{"v":22,"d":"22 "}]
[]
[{"v":171,"d":"171 "},null,"\"Sika Boom\" expandable polyurethane foam sealant or equal and approved roof sealant",null,"m",{"v":11,"d":"11 "}]
[]
[null,null,"ROOF AND WALL INSULATION"]
[]
[null,null,"\"Sisalation FR 405\" insulation membrane or proven equivalent laid taut directly over trusses with support wires, leaving an air gap between the roof sheet and insulation all in accordance with manufacturer\"€™s recommendations and specifications. R-value 1.2\"² K/W"]
[]
[{"v":172,"d":"172 "},null,"Insulation sheeting fixed to underside of rafters with 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required",null,"m²",{"v":22,"d":"22 "}]
[]
[null,null,"RAINWATER DISPOSAL"]
[]
[null,null,"Aluminium or other approved"]
[]
[{"v":173,"d":"173 "},null,"85 x 125 x 0.9mm Aluminium seamless gutter (square profile), coated internally and externally with \"ColourTech G4\" Colour: match the colour of the roof sheeting",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":174,"d":"174 "},null,"80mm diameter uPVC (painted to match the colour of the gutter it is fixed to) downpipe, screwed to steel columns/walls with PVC brackets, including sealing joints.",null,"m",{"v":36,"d":"36 "}]
[]
[{"v":175,"d":"175 "},null,"Extra over for angle",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":176,"d":"176 "},null,"Extra for stopped end",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":177,"d":"177 "},null,"Extra over 80mm diameter pipe for shoe",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":178,"d":"178 "},null,"Reposition existing rainwater downpipe to new gulley point",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO. 7"]
[]
[null,null,"CARPENTRY AND JOINERY"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Joinery"]
[]
[null,null,"Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc"]
[]
[null,null,"Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes"]
[]
[null,null,"Fixing"]
[]
[null,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete"]
[]
[null,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[null,null,"Decorative thermosetting plastic laminate covering"]
[]
[null,null,"Laminate finish shall be glued under pressure.  Edge strips shall be butt jointed at junctions with adjacent similar finish"]
[]
[null,null,"STRUCTURAL TIMBERWORK ETC"]
[]
[null,null,"Sawn softwood grade 7PAR"]
[]
[{"v":179,"d":"179 "},null,"38 x 114mm Wall plate",null,"m",{"v":19,"d":"19 "}]
[]
[{"v":180,"d":"180 "},null,"38 x 114mm Rafters in lengths not exceeding 2,4m bolted to brick work or concrete beams",null,"m",{"v":30,"d":"30 "}]
[]
[{"v":181,"d":"181 "},null,"38 x 76mm Purlins bolted to timber rafters",null,"m",{"v":17,"d":"17 "}]
[]
[null,null,"Sundries"]
[]
[{"v":182,"d":"182 "},null,"Two coats creosote on sawn timbers",null,"m²",{"v":13,"d":"13 "}]
[]
[null,null,"EAVES, VERGES, ETC"]
[]
[null,null,"Fibre-cement medium density plain ungrooved fascia boards -  fixed to 38 x 38mm tilter batten and 38 x 38mm support battens between rafters, twice screwed with 12 x 40mm countersunk brass screws at 900mm centres to support battens."]
[]
[{"v":183,"d":"183 "},null,"Fascia Type F1: 12 x 225mm Fascias and barge boards",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"SKIRTINGS"]
[]
[null,null,"Meranti with mitred internal and external corners, screwed to walls"]
[]
[{"v":184,"d":"184 "},null,"20 x 100mm Skirtings",null,"m",{"v":699,"d":"699 "}]
[]
[null,null,"DOORS, ETC"]
[]
[null,null,"Supply and installation"]
[]
[null,null,"Solid flush doors, hung to steel frames"]
[]
[{"v":185,"d":"185 "},null,"813 x 2032mm high doors",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":186,"d":"186 "},null,"1200 x 2032mm high door",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Class A fire doors with veneer suitable for painting"]
[]
[{"v":187,"d":"187 "},null,"1613 x 2032mm high double fire door including pressed steel frame for 90mm block wall and preparing frame for door closer and lock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Class B fire doors with veneer suitable for painting"]
[]
[{"v":188,"d":"188 "},null,"824 x 2125mm high single fire door including pressed steel frame for 230mm block wall and preparing frame for door closer and lock",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":189,"d":"189 "},null,"1613 x 2125mm high double fire door including pressed steel frame for 280mm block wall and preparing frame for door closer and lock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"FITTINGS"]
[]
[null,null,"CUPBOARDS & COUNTERTOPS TO KITCHENS"]
[]
[null,null,"The following cupboard fittings are given as complete units i.e. the components of the units have not been given separately. Descriptions of such units shall, therefore, be deemed to include all components, assembling, housing, notching, glueing, blocking, planting-on and screwing with countersunk screws, edge strips, thermosetting plastic laminate, glass, ironmongery, metalwork, paint or varnish finishes, etc  Prices are to include for all necessary filler pieces against walls etc"]
[]
[null,null,"Supply and installation"]
[]
[null,null,"Handles, hinges, drawer slides  to cupboard doors by shopfitter, refer to architects specification.  Standard colour melamine refer to architects specification approval."]
[]
[null,null,"Floor cupboard with  shelves, drawers, doors etc. comprising of 16mm thick white faced melamine (Melawood) moisture resistant  particle boards to all visible surfaces colour super white peen finish, with 16mm thick MDF back panel, 40 x 40mm MDF Battern, plinths to be adjustable PVC feet with clip on skirting with 2mm aluminium lining. Doors to have 2mm impact edging, carcass to have 1mm white ABS high impact edging. Drawer runners to be commercial grade soft close ball bearing runners. Cupboard door hinges to be slide on hinge with mounting plate 110 degree metal hinge. Handle to be 100mm brushed nickel, cupboard lockset Hafele square body lock #232.26.600 , drawer lockset 19 X 22mm Roco rvlc173NP all complete as per Architect's specification"]
[]
[{"v":190,"d":"190 "},null,"Floor unit 4800 x 600 x 900mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_411 Elevation 100-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":191,"d":"191 "},null,"Floor unit 3800 x 600 x 900mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_412 Elevation 158-D",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":192,"d":"192 "},null,"Floor unit 1800 x 600 x 900mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_412 Elevation 158-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":193,"d":"193 "},null,"Floor unit 2100 x 600 x 900mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_413 Elevation 168-D",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"High level cupboard with  shelves, drawers, doors etc. comprising of 16mm thick white faced melamine (Melawood) moisture resistant  particle boards to all visible surfaces colour super white peen finish, with 16mm thick MDF back panel. Doors to have 2mm impact edging, carcass to have 1mm white ABS high impact edging. Drawer runners to be commercial grade soft close ball bearing runners. Cupboard door hinges to be slide on hinge with mounting plate 110 degree metal hinge. Handle to be 100mm brushed nickel, cupboard lockset Hafele square body lock #232.26.600 , drawer lockset 19 X 22mm Roco rvlc173NP all complete as per Architect's specification"]
[]
[{"v":194,"d":"194 "},null,"Wall unit 4800 x 350 x 600mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_411 Elevation 100-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":195,"d":"195 "},null,"Wall unit 3800 x 350 x 600mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_412 Elevation 158-D",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":196,"d":"196 "},null,"Wall unit 1800 x 350 x 600mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_412 Elevation 158-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":197,"d":"197 "},null,"Wall unit 2100 x 350 x 600mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_413 Elevation 168-D",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Tall  cupboard with  shelves, drawers, doors etc. comprising of 16mm thick white faced melamine (Melawood) moisture resistant  particle boards to all visible surfaces colour super white peen finish, with 16mm thick MDF back panel and plinths to be adjustable PVC feet with clip on skirting with 2mm aluminium lining. Doors to have 2mm impact edging, carcass to have 1mm white ABS high impact edging. Drawer runners to be commercial grade soft close ball bearing runners. Cupboard door hinges to be slide on hinge with mounting plate 110 degree metal hinge. Handle to be 100mm brushed nickel, cupboard lockset Hafele square body lock #232.26.600 , drawer lockset 19 X 22mm Roco rvlc173NP all complete as per Architect's specification"]
[]
[{"v":198,"d":"198 "},null,"Wall unit 800 x 580 x 2100mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_412 Elevation 158-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":199,"d":"199 "},null,"Wall unit  800 x 580 x 2100mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_411 Elevation 100-B",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":200,"d":"200 "},null,"Wall unit 400 x 580 x 2100mm high cupboard complete as per drawing WCGRB 024525 A_W3-01_413 Elevation 168-D",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"32 mm Post formed Formica LifeSeal Worktop with 3mm radius on exposed edge supported by steel leg 1100mm high,  60mm diameter, matt chrome finish all  as per Architect's specification"]
[]
[{"v":201,"d":"201 "},null,"450mm Wide bar counter",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"32 mm Post formed Formica LifeSeal Worktop with 3mm radius on exposed edge fixed on cupboard all  as per Architect's specification"]
[]
[{"v":202,"d":"202 "},null,"600mm Wide countertop",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":203,"d":"203 "},null,"E.O. for Cut out to 32mm thick formica worktop for sink  opening",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Take delivery of fittings, assemble and place"]
[]
[{"v":204,"d":"204 "},null,"Take delivery, assemble and placing of 1800 x 800 x 740mm high desk",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":205,"d":"205 "},null,"Take delivery, assemble and placing of 2000 x 800 x 740mm high desk",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":206,"d":"206 "},null,"Take delivery, assemble and placing of 600 x 400 x 600mm mobile pedestal FLEXUS",null,"No",{"v":68,"d":"68 "}]
[]
[{"v":207,"d":"207 "},null,"Take delivery, assemble and placing of 800 x 450 x 740mm high roller door credenza",null,"No",{"v":10,"d":"10 "}]
[]
[{"v":208,"d":"208 "},null,"Take delivery, assemble and placing of 800 x 350 x 760mm high file box",null,"No",{"v":40,"d":"40 "}]
[]
[{"v":209,"d":"209 "},null,"Take delivery, assemble and placing of 800 x 450 x 1500mm high swing door cupboard",null,"No",{"v":27,"d":"27 "}]
[]
[{"v":210,"d":"210 "},null,"Take delivery, assemble and placing of 800 x 350 x 1800mm high bookcase",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":211,"d":"211 "},null,"Take delivery, assemble and placing of 1800 x 450 x 950mm high server unit",null,"No",{"v":20,"d":"20 "}]
[]
[{"v":212,"d":"212 "},null,"Take delivery, assemble and placing of 1800 x 350 x 850mm high server unit add-on (Wall Unit)",null,"No",{"v":20,"d":"20 "}]
[]
[{"v":213,"d":"213 "},null,"Take delivery, assemble and placing of 1600 x 24 x 1500mm high double floor based screen",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":214,"d":"214 "},null,"Take delivery, assemble and placing of 800 x 24 x 1500mm high single floor based screen",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":215,"d":"215 "},null,"Take delivery, assemble and placing of 1600 x 1600mm L-shape desk",null,"No",{"v":40,"d":"40 "}]
[]
[{"v":216,"d":"216 "},null,"Take delivery, assemble and placing of 1800 x 1600mm L-shape desk",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"BILL NO. 8"]
[]
[null,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"CEILING TIMBERS, BEADS, INSULATION, ETC"]
[]
[null,null,"135mm Aerolite insulation (Non-combustible and Class 1 fire index rating) or proven equivalent laid on top of the ceiling, ensuring that it fits tightly between the tie beams. Aerolite should be cut 50mm more than distance between the tie beams. Cut Aerolite out around down lights. To be read in conjunction with Glass wool handling Instructions in the Installation methodology. 135mm R-value 3.38\"² K/W"]
[]
[{"v":217,"d":"217 "},null,"135mm Insulation in blanket form lapped not less than 50mm along all edges and laid on top of brandering between roof timbers etc",null,"m²",{"v":16,"d":"16 "}]
[]
[null,null,"SUSPENDED CEILINGS"]
[]
[null,null,"OWAcoustic Constellation Premium biologically absorbable mineral wool ceiling tiles, NRC - 0.80, CAC - 33dB, Fire classification A2-s1, d0, weight - 4.5 kg/m\"², size 1200 x 600 x 15mm or 1200x600mm with Square-edge and white painted finish, laid on fire rated OWAconstruct S3 exposed demountable Butt-cut T24 suspension system, comprising galvanised main tees and cross tees with main tees suspended by means of galvanised hangers at centres not exceeding 1200mm, and all installed to manufacturer's instructions"]
[]
[{"v":218,"d":"218 "},null,"Horizontal ceilings not exceeding 1m below concrete soffits",null,"m²",{"v":318,"d":"318 "}]
[]
[{"v":219,"d":"219 "},null,"Replace broken and/or damaged ceiling lay-in boards only",null,"m²",{"v":835,"d":"835 "}]
[]
[{"v":220,"d":"220 "},null,"Replace aluminium tees and crosses",null,"m",{"v":417,"d":"417 "}]
[]
[{"v":221,"d":"221 "},null,"20 x 20mm Aluminium shadow line cornices",null,"m",{"v":545,"d":"545 "}]
[]
[null,null,"NAILED UP CEILINGS"]
[]
[null,null,"1x RhinoBoard\"® 9 mm (locally manufactured, ISO 9001 & 14001 certification, recycled paper content, Greentag Level B) fixed to Gypframe\"® UltraSTEEL\"® Brandering spaced at 400 mm centres clipped onto Gyproc Suspension Brackets and fixed to tie beam/joist using one line of 2 Gyproc Grabber Screw 32 mm. Maximum joist/tie beam spacing is 1200 mm. Branders are joined using brander joiners. Fixed using Gyproc Sharp-point Screws 25 mm at maximum 150 mm centres. Gypframe\"® UltraSTEEL\"® Brandering suspended using Gyproc Suspension Bracket at 1200 mm centres. Apply Gyproc RhinoTape\"® to all joints and internal corners. Install Gypframe\"® Corner Bead to all external corners. Cover Gyproc RhinoTape\"® with 1 layer of Gyproc RhinoLite\"® Multipurpose/ RhinoLite\"® Natural Plus\"®/ RhinoLite\"® CreteStone\"® (locally manufactured, Greentag Level B)."]
[]
[{"v":222,"d":"222 "},null,"Ceilings",null,"m²",{"v":32,"d":"32 "}]
[]
[{"v":223,"d":"223 "},null,"Rectangular bulkheads against wall 600mm wide x 200mm high suspended not exceeding 300mm below concrete soffits",null,"m",{"v":37,"d":"37 "}]
[]
[{"v":224,"d":"224 "},null,"Rectangular bulkheads against wall 900mm wide x 200mm high suspended not exceeding 300mm below concrete soffits",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":225,"d":"225 "},null,"Rectangular bulkheads against wall 1000mm wide x 200mm high suspended not exceeding 300mm below concrete soffits",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":226,"d":"226 "},null,"Rectangular bulkheads against wall 1350mm wide x 200mm high suspended not exceeding 300mm below concrete soffits",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":227,"d":"227 "},null,"Extra over for opening in ceiling for downlight",null,"No",{"v":71,"d":"71 "}]
[]
[null,null,"Fix Gyproc Rhino Cove Cornice\"„¢ 75 mm as per manufacturers detail and specification"]
[]
[{"v":228,"d":"228 "},null,"Coved cornice",null,"m",{"v":64,"d":"64 "}]
[]
[null,null,"PARTITIONS ETC"]
[]
[null,null,"12mm Gypsum plasterboard screwed to 63.5mm galvanised steel studs at 400mm centre to centre and tracks framework, screwed to floors and underside of ceiling grids as per the architect's specifications"]
[]
[{"v":229,"d":"229 "},null,"Partitions 2600mm high with bottom track plugged and top track fixed to suspended ceiling tees/soffit",null,"m",{"v":350,"d":"350 "}]
[]
[{"v":230,"d":"230 "},null,"Extra over partition 2600mm high for corner",null,"No",{"v":44,"d":"44 "}]
[]
[{"v":231,"d":"231 "},null,"Extra over partition 2600m high for T-intersection",null,"No",{"v":38,"d":"38 "}]
[]
[{"v":232,"d":"232 "},null,"Extra over partition 2600mm high for fair ends",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":233,"d":"233 "},null,"Extra over partition 2600mm high for irregular T-intersection",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":234,"d":"234 "},null,"Extra over partition 2600mm high for irregular corners",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":235,"d":"235 "},null,"Extra over partition 2600m high for ends",null,"No",{"v":67,"d":"67 "}]
[]
[null,null,"Extra over for breaking out for and forming openings through 90mm drywalls for new ducting, including making good on both sides"]
[]
[{"v":236,"d":"236 "},null,"Opening for ducting 100 x 100mm high",null,"No",{"v":26,"d":"26 "}]
[]
[{"v":237,"d":"237 "},null,"Opening for ducting 100mm high diameter",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":238,"d":"238 "},null,"Opening for ducting 125mm high diameter",null,"No",{"v":36,"d":"36 "}]
[]
[{"v":239,"d":"239 "},null,"Opening for ducting 150mm high diameter",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":240,"d":"240 "},null,"Opening for ducting 200mm high diameter",null,"No",{"v":17,"d":"17 "}]
[]
[null,null,"Extra over partitions for 44mm Pre-primed MDF (Medium-Density Fiberboard) or HDF (High-Density Fiberboard) skins for a smooth finish with veneer on both sides and lipped hardwood edge strips to vertical edges, hung to and including 90mm drywall natural anodised aluminium door frame with one and a half pairs of 100mm steel hinges to each hanging stile, including additional studding, trimming, etc. to partitions"]
[]
[{"v":241,"d":"241 "},null,"DA: 817 x 2125mm high hinged door including aluminium frame",null,"No",{"v":28,"d":"28 "}]
[]
[{"v":242,"d":"242 "},null,"DG: 1520 x 2125mm high double timber door including metal frame",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Extra over partitions for aluminium powder coated shopfront consisting of 44mm Pre-primed MDF (Medium-Density Fiberboard) or HDF (High-Density Fiberboard) skins for a smooth finish with veneer on both sides and lipped hardwood edge strips to vertical edges, hung to and including 90mm drywall natural anodised aluminium door frame with one and a half pairs of 100mm steel hinges to each hanging stile, including additional studding, trimming, etc. to partitions with connected sidelight as per architect's specifications"]
[]
[{"v":243,"d":"243 "},null,"DD: 1500 x 2125mm high aluminium shop front comprising of 800 x 2075mm high hinged timber door connected to  600mm wide sidelight consisting of 550 x 1200mm high fixed panel and 550 x 665mm high solid aluminium panel in drywall",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":244,"d":"244 "},null,"DF: 1500 x 2125mm high aluminium shop front comprising of 800 x 2075mm high hinged timber door connected to  600mm wide sidelight consisting of 550 x 1915mm high fixed panel in drywall",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Extra over partitions for Class A fire doors"]
[]
[{"v":245,"d":"245 "},null,"DH: 824 x 2125mm high single fire door including metal frame for 90mm drywall and preparing frame for door closer and lock",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Extra over partitions for Class B fire doors"]
[]
[{"v":246,"d":"246 "},null,"1613 x 2125mm high double fire door including metal frame for 90mm drywall and preparing frame for door closer and lock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO. 9"]
[]
[null,null,"FLOOR FINISHES"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"CARPETS"]
[]
[null,null,"10mm thick Belgotex Baltimore Heavy Commercial SDN, Tufted Broadloom Eco SDX (Solution Dyed Nylon), with FussionBac backing in 4m wide roll Colour to be confirmed"]
[]
[{"v":247,"d":"247 "},null,"On screeded floors",null,"m²",{"v":102,"d":"102 "}]
[]
[null,null,"5,5 x 500 x 500mm Heavy Commercial Belgotex \"€˜Accelerate Boost\"€™ manufactured from robust SDN Tufted Loop Pile Bitumen Tile - SS flooring; with NexBac SX Colour to be confirmed"]
[]
[{"v":248,"d":"248 "},null,"On screeded floors",null,"m²",{"v":1035,"d":"1,035 "}]
[]
[{"v":249,"d":"249 "},null,"Self levelling screed",null,"m²",{"v":1034,"d":"1,034 "}]
[]
[null,null,"BILL NO. 10"]
[]
[null,null,"METALWORK"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Descriptions Descriptions of bolts shall be deemed to include nuts and washers Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete Metalwork described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described"]
[]
[null,null,"Aluminium windows and doors"]
[]
[null,null,"Descriptions of aluminium windows and doors shall be deemed to include all necessary temporary protection measures and fittings as well as timber or other subframes, templates, etc which are required in terms of the approved design.  Descriptions of aluminium windows and doors shall be deemed to include sealing with approved silicone sealing compound along edges as necessary.  Descriptions of aluminium windows and doors shall be deemed to include preparation for fitting of ironmongery.  The sized stated in the descriptions of aluminium units are indicative only, not prescriptive and may have to be adjusted to suit circumstances.  Testing of windows for watertightness:  Each window shall be tested for watertightness with water sprayed on using adequate pressure.  If, in the opinion of the Principal Agent, the pressure proves to be inadequate then the pressure shall be boosted by means of compressed air or other means.  Ironmongery to be included in tendered rates"]
[]
[null,null,"The following certificates shall be provided prior to commencement of site work:1\tA copy of the relevant AAAMSA Performance Test Certificate from the manufacturer/contractor supplying the architectural aluminium product 2\tA Certificate of Conformance confirming that anodising or powder coating has been processed in accordance with SANS 999 and SANS 1796 respectively"]
[]
[null,null,"3\tA powder guarantee of not less than 15 years issued by the powder manufacturer.  The specific conditions contained in this guarantee shall form part of the powder coating process 4\tA Certificate of Conformance confirming that glazing has been installed in accordance with SANS 10137, ensuring that safety glazing materials have been installed in the mandatory areas and that each individual pane of safety glazing materials has been permanently marked5\tA warranty from the manufacturer of the laminated safety glass and/or hermetically sealed glazing units guaranteeing the products against delamination and colour degredation for a period of not less than five years"]
[]
[null,null,"STAINLESS STEEL HANDRAILS, BALUSTRADES, ETC."]
[]
[null,null,"Stainless steel balustrading"]
[]
[{"v":250,"d":"250 "},null,"60mm diameter handrails welded to 10mm round stainless steel bars with square bend and chemically anchored to walls. Allow 60mm gap between wall face and inner handrail",null,"m",{"v":79,"d":"79 "}]
[]
[{"v":251,"d":"251 "},null,"Galvanised mild steel hollow tubing to be bent twice on each landing to welded to existing handrails to create continuous handrail",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":252,"d":"252 "},null,"40 x 40mm galvanised mild steel angle section bent twice to be welded to existing handrail to create continuous handrail",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"GALVANISED STEEL STAIRS"]
[]
[{"v":253,"d":"253 "},null,"3mm galvanised mild steel diamond checker plate panels welded onto existing 1170 x 2500mm landings",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":254,"d":"254 "},null,"3mm galvanised mild steel diamond checker plate panels welded onto existing 250 x 1050mm wide treads",null,"No",{"v":54,"d":"54 "}]
[]
[{"v":255,"d":"255 "},null,"3mm galvanised mild steel diamond checker plate panels welded onto existing 178 x 1050mm wide risers",null,"No",{"v":54,"d":"54 "}]
[]
[null,null,"GALVANISED PRESSED STEEL DOOR FRAMES"]
[]
[null,null,"1,2mm Rebated frames suitable for half brick walls"]
[]
[{"v":256,"d":"256 "},null,"Frame for door 813 x 2032mm high",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":257,"d":"257 "},null,"Frame for door 1200 x 2032mm high",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"WINDOWS"]
[]
[null,null,"Powder coated aluminium windows with 4mm floated glass complete with subframes, ironmongery to architect approval, waterproofing sealant to internal and external perimeter of aluminium frame, etc plugged to brickwork or concrete designed in accordance to AAAMSA guidelines Colour to be confirmed by architect"]
[]
[{"v":258,"d":"258 "},null,"W1: 1500 x 600mm high window",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Powder coated aluminium windows with 6.4mm safety glass complete with subframes, ironmongery to architect approval, waterproofing sealant to internal and external perimeter of aluminium frame, etc plugged to brickwork or concrete designed in accordance to AAAMSA guidelines Colour to be confirmed by architect"]
[]
[{"v":259,"d":"259 "},null,"W2: 1500 x 1860mm high aluminium window",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":260,"d":"260 "},null,"W3: 900 x 2125mm high aluminium window",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":261,"d":"261 "},null,"W4: 1500 x 2125mm high aluminium window",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DOORS"]
[]
[null,null,"Powder coated aluminium doors with 6.4mm safety glass complete with subframes, ironmongery to architect approval, waterproofing sealant to internal and external perimeter of aluminium frame, etc plugged to brickwork or concrete designed in accordance to AAAMSA guidelines Colour to be confirmed by architect"]
[]
[{"v":262,"d":"262 "},null,"DB: 900 x 2125mm high aluminium single door and frame",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":263,"d":"263 "},null,"DE: 1500 x 2125mm high aluminium double door and frame",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"SUNDRIES"]
[]
[{"v":264,"d":"264 "},null,"60 x 60 x 2mm GMS angle corner protector to brick walls",null,"m",{"v":3,"d":"3 "}]
[]
[null,null,"BILL NO 11"]
[]
[null,null,"IRONMONGERY"]
[]
[null,null,"SUPPLY AND INSTALL"]
[]
[null,null,"User note"]
[]
[null,null,"Proprietary items"]
[]
[null,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the products/articles specified or alternative product equal to in performance and same in appearance."]
[]
[null,null,"HINGES, BOLTS, ETC"]
[]
[null,null,"Manufactured by \"Dormakaba\""]
[]
[{"v":265,"d":"265 "},null,"102 x 75 x 3mm, EN1935 Grade 13, two ball bearing butt hinge (Pair)",null,"No",{"v":12,"d":"12 "}]
[]
[{"v":266,"d":"266 "},null,"100 x 76 x 2mm, EN1935 Grade 201 SS sinkless ball bearing hinge with satin stainless steel (Pair)",null,"No",{"v":24,"d":"24 "}]
[]
[{"v":267,"d":"267 "},null,"\"DFB-SS-027\" 160mm Manual flush bolt",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":268,"d":"268 "},null,"\"DFB-SS-028\" 300mm Manual flush bolt",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":269,"d":"269 "},null,"\"DPS-SS-028\" Dust proof strike",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":270,"d":"270 "},null,"\"DDS-SS-017\" Floor mounted door stop",null,"No",{"v":58,"d":"58 "}]
[]
[{"v":271,"d":"271 "},null,"\"CH 150\" 150mm Cabin hook",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"LOCKS"]
[]
[null,null,"Keys"]
[]
[null,null,"Unless otherwise described locks shall have three keys each"]
[]
[null,null,"Manufactured by \"Dormakaba\""]
[]
[{"v":272,"d":"272 "},null," \"D02835 SS\" Narrow stile roller dead lock with european profile cylinder, case 174 x 52mm forend 238 x 22mm, back set 35mm and throw 20mm",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":273,"d":"273 "},null,"\"D036S SS\" Cylinder sash lock , case 117 x 78mm forend 168 x 22mm, back set 57mm and centre 61mm",null,"No",{"v":54,"d":"54 "}]
[]
[{"v":274,"d":"274 "},null,"\"D037D SS\" Cylinder dead lock , case 117 x 78mm forend 168 x 22mm and back set 57mm",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":275,"d":"275 "},null,"\"DDC206301GMK\" 63mm Europrofile E-SP 5 pin double cylinder grand master keyed satin nickel finish",null,"No",{"v":41,"d":"41 "}]
[]
[{"v":276,"d":"276 "},null,"\"DKC206301GMK\" 63mm Europrofile E-SP 5 pin knob cylinder grand master keyed satin nickel finish",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":277,"d":"277 "},null,"\"DKC204101GMK\" 40.5mm Europrofile E-SP 5 pin single cylinder grand master keyed satin nickel finish",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":278,"d":"278 "},null,"\"D038R NP\" Rebate conversion kit for euro profile locks, nickel plated finish",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":279,"d":"279 "},null,"\"PHA1 S SD\" One point locking panicking bar for single door 1000mm wide (set)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":280,"d":"280 "},null,"\"PHA 3 S DD\" Three point locking panicking bar for double door (set)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":281,"d":"281 "},null,"\"PHT3901\" Exterior access lock with lever handle (each)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":282,"d":"282 "},null,"Grand master key",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"HANDLES"]
[]
[null,null,"Manufactured by \"Dormakaba\""]
[]
[{"v":283,"d":"283 "},null,"\"DPH206 BTB\" 400 x 30mm offset tubular pull handle BTB fixing sets included BS 8424 pull handle. grade 3 - heavy duty stainless steel (Pair)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":284,"d":"284 "},null,"\"DPH301C BT\" 149 x 19mm Straight tubular pull handle BT (Each)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":285,"d":"285 "},null,"\"TH132\" Latch S.S. lever handle on rose (Pair)",null,"No",{"v":54,"d":"54 "}]
[]
[null,null,"DOOR CLOSERS"]
[]
[null,null,"Manufactured by \"Dormakaba\""]
[]
[{"v":286,"d":"286 "},null,"\"SR 392\" Size 1 door co-ordinator for door leaf widths more than 800mm",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":287,"d":"287 "},null,"\"SR 392\" Size 2 door co-ordinator for door leaf widths less than 800mm",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":288,"d":"288 "},null,"\"TS71-SL\" EN 3/4  rack & pinion door closer with standard non hold open scissor arm, EN1154  hydraulic speed control, standard pull side fixing, transom push side fixing EN4 suitable for door width 950-1100mm fire rated.",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":289,"d":"289 "},null,"\"TS71 PA-SL\" EN 3/4  rack & pinion door closer with standard non hold open scissor arm and parallel arm bracket, EN1154  hydraulic speed control, standard pull side fixing, transom push side fixing EN4 suitable for door width 950-1100mm fire rated.",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":290,"d":"290 "},null,"\"TS90 SL\" EN 3/4  cam action door closer with standard non hold slide channel armt, EN1154  hydraulic speed control, standard pull side fixing, transom push side fixing EN4 suitable for door width 950-1100mm fire rated.",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"PUSH PLATES AND KICK PLATES"]
[]
[null,null,"1.2mm Thick 304 brushed stainless steel plates countersunk screwed along edges at not exceeding 200mm centres"]
[]
[{"v":291,"d":"291 "},null,"200 x 200mm Push plate",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":292,"d":"292 "},null,"800 x 400mm Kick plate",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"BILL NO 12"]
[]
[null,null,"STRUCTURAL STEELWORK"]
[]
[null,null,"User note"]
[]
[null,null,"Insert preambles/specifications as may be required or in order to supplement any applicable preambles, specifications or bills of quantities descriptions Take note that these Model Bills of Quantities utilise abbreviated descriptions The Model Preambles for Trades 2008 published by the Association of South African Quantity Surveyors is designed to support and extend the abbreviated bills of quantities descriptions by inter alia referring to SANS construction standards. Where such model preambles are not applicable (eg where BS or Euro construction standards are applicable or the design consultants provide other preambles/specifications for insertion), users are to ensure that the abbreviated descriptions when read in conjunction with the applicable measuring system, represents the full description by extending the abbreviated bills of quantities descriptions and/or by inserting appropriate preambles or specifications Consider inserting the preambles hereunder when using the abovementioned Model Preambles for Trades 2008"]
[]
[null,null,"Consideration is to be given in specific applications (e.g. where \"heavy\" steel structures such as in industrial plants, towers for mine shafts, etc are dominant) to implement the principles laid down by the \"Measurement for Structural Steelwork\" as prepared and recommended by the South African Institute of Steel Construction or any other appropriate principles  This bill is, however, based on the building work measuring  system"]
[]
[null,null,"Finishing-off painting is to be included in this trade only when the structural steel contractor is required to execute the work"]
[]
[null,null,"Descriptions"]
[]
[null,null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[null,null,"Descriptions of L-shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete"]
[]
[null,null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[]
[null,null,"GALVANISED STEEL COLUMNS AND BEAMS"]
[]
[null,null,"User note"]
[]
[null,null,"In the event of there being only a limited number of different heights or lengths of columns or beams, the specific heights or lengths may be given separately or may be suitably grouped together"]
[]
[null,null,"Welded columns in single lengths with flat base, cap, bearer and connection plates, bolted to concrete"]
[]
[{"v":293,"d":"293 "},null,"100 x 100 x 3mm x 8.9kg/m  SHS  (Square) columns",null,"t",0.55]
[]
[null,null,"Welded beams in single lengths with flat bearer and connection plates, bolted to steel"]
[]
[{"v":294,"d":"294 "},null,"100 x 50 x 2mm x 3.6kg/m CFLC beams",null,"t",0.45]
[]
[null,null,"BOLTS, FASTENERS, ETC"]
[]
[{"v":295,"d":"295 "},null,"M16 bolts grade 8.8 anchored minimum 120mm into concrete with Sikafix S",null,"No",{"v":32,"d":"32 "}]
[]
[{"v":296,"d":"296 "},null,"M16 bolts grade 8.8 embedded minimum 120mm into brickwork with Sikafix S",null,"No",{"v":144,"d":"144 "}]
[]
[null,null,"BILL NO. 13"]
[]
[null,null,"PLASTERING"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SCREEDS"]
[]
[null,null,"Screeds on concrete"]
[]
[{"v":297,"d":"297 "},null,"On floors",null,"m²",{"v":16,"d":"16 "}]
[]
[{"v":298,"d":"298 "},null,"Average 80mm Thick on roofs to falls",null,"m²",{"v":180,"d":"180 "}]
[]
[null,null,"INTERNAL PLASTER"]
[]
[null,null,"10mm Smooth steel trowelled plaster on brickwork with a maximum tolerance of 1mm"]
[]
[{"v":299,"d":"299 "},null,"On walls",null,"m²",{"v":395,"d":"395 "}]
[]
[{"v":300,"d":"300 "},null,"On raking soffits of stairs",null,"m²",{"v":5,"d":"5 "}]
[]
[{"v":301,"d":"301 "},null,"On narrow widths",null,"m²",{"v":8,"d":"8 "}]
[]
[null,null,"EXTERNAL PLASTER"]
[]
[null,null,"12-15mm Smooth cement plaster on brickwork with a maximum tolerance of 2mm"]
[]
[{"v":302,"d":"302 "},null,"On walls",null,"m²",{"v":314,"d":"314 "}]
[]
[{"v":303,"d":"303 "},null,"On narrow widths",null,"m²",{"v":18,"d":"18 "}]
[]
[null,null,"BILL NO. 14"]
[]
[null,null,"PLUMBING AND DRAINAGE"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Stainless steel basins, sinks, wash troughs, urinals, etc"]
[]
[null,null,"Stainless steel for economy basins, domestic sinks and worktops shall be Type 430 (17/0)  Stainless steel for urinals, basins, quality sinks, wash troughs, institutional equipment, etc shall be Type 304 (18/8)  Stainless steel for laboratory sinks, photographic equipment, etc shall be Type 316 (18/8)  Units shall have standard aprons on all exposed edges and tiling keys against walls where applicable"]
[]
[null,null,"Sealing of edges"]
[]
[null,null,"Outer edges of sinks, basins, baths, urinals, etc are to be sealed against adjacent surfaces with approved silicone"]
[]
[null,null,"uPVC pipes and fittings"]
[]
[null,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed"]
[]
[null,null,"uPVC pressure pipes and fittings"]
[]
[null,null,"Pipes of 50mm diameter and smaller shall be plain ended with solvent welded uPVC loose sockets and fittings  Pipes of 63mm diameter and greater shall have sockets and spigots with push-in type integral rubber ring joints.  Bends shall be uPVC and all other fittings shall be cast iron, all with similar push-in type joints"]
[]
[null,null,"Copper pipes"]
[]
[null,null,"Pipes shall be hard drawn and half-hard \"Maksal\" pipes of the class described.  Class 0 (thin walled hard drawn) pipes shall not be bent.  Class 1 (thin walled half-hard), Class 2 (half-hard) and Class 3 (heavy walled half-hard) pipes shall only be bent with benders with inner and outer formers.  Fittings to copper waste, vent and anti-syphon pipes, capillary solder fittings and compression fittings shall be \"Cobra Watertech\" type.  Capillary solder fittings shall comply with ISO 2016"]
[]
[null,null,"Copper pipes are to be installed in accordance with the latest revision of the Code of Practice for Copper Plumbing soldering techniques.  Flux, solder, etc to be strictly in accordance with the manufacturer's requirements with special attention to copper flux composition"]
[]
[null,null,"Reducing fittings"]
[]
[null,null,"Where fittings have reducing ends or branches they are described as \"reducing\" and only the largest end or branch size is given. Should the contractor wish to use other fittings and bushes or reducers he may do so on the understanding that no claim in this regard will be entertained"]
[]
[null,null,"Fixing of pipes"]
[]
[null,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[null,null,"Laying, backfilling, bedding, etc of pipes"]
[]
[null,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled"]
[]
[null,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with Clauses 5.1 and 5.2 of each of the following: SABS 1200L\t: Medium-pressure pipelines SABS 1200LD\t: Sewers SABS 1200LE\t: Stormwater drainage Pipe trenches, etc shall be backfilled in accordance with Clauses 3, 5.5, 5.6, 5.7 and 7 of SABS 1200DB : Earthworks (Pipe trenches)Pipes shall be bedded in accordance with Clauses 3.1 to 3.4.1, 5.1 to 5.3 and 7 of SABS 1200LB : Bedding (Pipes)Unless otherwise described bedding of rigid pipes shall be Class B bedding"]
[]
[null,null,"WATER SUPPLY AND SANITARY PLUMBING"]
[]
[null,null,"Internal reticulation"]
[]
[null,null,"Design and supply an internal water reticulation system and testing of complete internal sanitary plumbing system for complete office building, comprising Class 1 Copper piping and fittings, including connecting to underground and existing water supply."]
[]
[null,null,"The contractor shall be responsible for the design of the internal plumbing reticulation. The contractor will submit shop drawings for approval to the Principal Agent for approval by the architect within two weeks after successful appointment. Appointment of the successful tenderer will be subject of the internal plumbing reticulation design. The contractor shall commence manufacturing only after written approval of shop drawings from the architect.  Stormwater drainage, soil drainage, sanitary drainage and water supplies need to be taken into consideration in the design and pricing of the internal reticulation."]
[]
[null,null,"Class 2 copper pipes"]
[]
[{"v":304,"d":"304 "},null,"15mm Pipes chased into brick walls",null,"m",{"v":75,"d":"75 "}]
[]
[{"v":305,"d":"305 "},null,"22mm Pipes chased in and including chasing in brickwork",null,"m",{"v":75,"d":"75 "}]
[]
[null,null,"Extra over class 2 copper pipes for capillary fittings"]
[]
[{"v":306,"d":"306 "},null,"15mm Fittings",null,"No",{"v":45,"d":"45 "}]
[]
[{"v":307,"d":"307 "},null,"22mm Fittings",null,"No",{"v":45,"d":"45 "}]
[]
[null,null,"STORMWATER DRAINAGE"]
[]
[null,null,"Excavations in all materials including backfill, compact and dispose of surplus material"]
[]
[{"v":308,"d":"308 "},null,"Excavations exceeding 2m and not exceeding 3m deep for pipe trenches (Labour Intensive)",null,"m³",{"v":2,"d":"2 "}]
[]
[null,null,"Class 100D concrete pipes with interlocking joints"]
[]
[{"v":309,"d":"309 "},null,"100mm Diameter pipes",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":310,"d":"310 "},null,"Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"SOIL DRAINAGE"]
[]
[null,null,"uPVC pipes"]
[]
[{"v":311,"d":"311 "},null,"50mm S&V pipes in concrete",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":312,"d":"312 "},null,"110mm S&V pipes in concrete",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"Extra over uPVC pipes for fittings"]
[]
[{"v":313,"d":"313 "},null,"50mm S&V bend 90\"°",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":314,"d":"314 "},null,"110mm S&V bend 90\"°",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":315,"d":"315 "},null,"50mm S&V access bend",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":316,"d":"316 "},null,"110mm S&V access bend",null,"No",{"v":15,"d":"15 "}]
[]
[null,null,"Catch pits and gulleys as per architect's specifications"]
[]
[{"v":317,"d":"317 "},null,"600 x 600mm Mild steel gulley cover only",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":318,"d":"318 "},null,"600 x 600mm Grated mild steel catch pit cover",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Sumps, catchpits, inspection chambers, etc including concrete kerbs or precast concrete cover slabs and excavating (gratings and covers elsewhere)"]
[]
[{"v":319,"d":"319 "},null,"600 x 600mm Brick catchpit 800mm deep internally",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"HOLES ETC"]
[]
[null,null,"Core drilling hole exceeding 50mm and not exceeding 100mm diameter"]
[]
[{"v":320,"d":"320 "},null,"200mm Thick reinforced concrete slab, beam, wall, etc",null,"No",{"v":19,"d":"19 "}]
[]
[null,null,"Sundries"]
[]
[{"v":321,"d":"321 "},null,"Cutting into existing 40mm drain pipe for and forming junction with 40mm pipe",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":322,"d":"322 "},null,"Cutting into existing 110mm drain pipe for and forming junction with 110mm pipe",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":323,"d":"323 "},null,"Allow for testing the whole of the Sanitary Plumbing, Water Supplies and Fire Services to the satisfaction of the Principal Agent and Local Authorities.",null,"Item",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO. 15"]
[]
[null,null,"SANITARY FITTINGS AND SUNDRIES SUPPLY & INSTALLATION"]
[]
[null,null,"Water Closet"]
[]
[{"v":324,"d":"324 "},null,"Toilet pan wall hung Code: 439550WH",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":325,"d":"325 "},null,"Toilet seat",null,"No",{"v":12,"d":"12 "}]
[]
[{"v":326,"d":"326 "},null,"Element for WC with EPS housing Code: G-38643001",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":327,"d":"327 "},null,"Pneumatic actuation plate Code: G-37059000",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Basin"]
[]
[{"v":328,"d":"328 "},null,"Basin Wall Hung 400x321x170 Code: 709000WH",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":329,"d":"329 "},null,"Pillartap heavy patt blue 15mm CP Code: 505-21B/HP",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":330,"d":"330 "},null,"Bottle trap universal Code: 340/N",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":331,"d":"331 "},null,"Basin clicker waist slotted Code: 303/N",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":332,"d":"332 "},null,"Angle valve Code: 232-10/NV",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":333,"d":"333 "},null,"Flexi Connector Code: C-15/350",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"Sinks"]
[]
[{"v":334,"d":"334 "},null,"1160mm long o/a x 460mm wide double end bowl drop in sink Code: 1990002",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":335,"d":"335 "},null,"Space saving plumbing kit FSA Code: 1120009",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":336,"d":"336 "},null,"800mm long o/a x 460mm wide double end bowl drop in sink Code: 1990001",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":337,"d":"337 "},null,"Space saving plumbing kit FSA Code: 1120008",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ELECTRIC WATER HEATERS"]
[]
[null,null,"Hot water heaters etc (Supply and Install)"]
[]
[{"v":338,"d":"338 "},null,"5 litre SS Zip Hydroboil, 318 x 150 x 460mm zip, 25 - 30 cups boiling water FSA Code: 2610009",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":339,"d":"339 "},null,"Single-lever sink mixer 1/2 Code: G-31180000",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":340,"d":"340 "},null,"Angle valve Code: 232-10/NV",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":341,"d":"341 "},null,"Angle valve adaptor Code: C-AV/ADAP1/2F-3/8M",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":342,"d":"342 "},null,"Drip tray to suit 5 litre hot water cylinder",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Supply & Installation of Sanitary Fitting Sundries"]
[]
[{"v":343,"d":"343 "},null,"Double toilet roll holder with spindel system for wall mounting, stainless steel surface satin finish, folded front cover, cylinder lock with Franke standard key. 144 x 138 x 301 FSA Code: 2120101",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":344,"d":"344 "},null,"Soap dispenser for wall mounting, stainless steel surface satin finish, folded front cover, cylinder lock with Franke standard key, suitable for liquid soaps, 0.8 litre soap tank, pull lever supplied, 321 x 116 x 140 FSA CodeL 2120254",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":345,"d":"345 "},null,"Paper towel dispenser for wall mounting. Manufacture from Grade 304 0.9mm Stainless Steel with satin finish, folded front cover, cylinder lock with Franke standard key, inspection windows on the front, loading capacity 500 - 800 pieces pf paper depending on convolution. Includes Stainless Steel screws and dowels. FSA Code: 2120241",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":346,"d":"346 "},null,"Waste Bin for wall mounting. manufactured from Grade 304 0.9mm Stainless Steel, surface satin finished. Approximately 23 litre capacity, mounting either with mounting bracket or directly onto the wall, includes Stainless Steel crews and dowles. 355mm x 168mm x 460mm FSA Code: 2120248",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":347,"d":"347 "},null,"Grab rail manufactured from 18/10 Stainless Steel , satin finish to prevent slipping, with diameter 31,8mm. Certified products, Includes screws and dowels FSA Code: 2510012",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":348,"d":"348 "},null,"Grab rail manufactured from 18/10 Stainless Steel , satin finish to prevent slipping, with diameter 31,8mm. Certified products, Includes screws and dowels FSA Code: 2510006",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":349,"d":"349 "},null,"6mm silvered float glass, copper backed with bevelled edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete.",null,"No",{"v":12,"d":"12 "}]
[]
[null,null,"BILL NO. 16"]
[]
[null,null,"PAINTWORK"]
[]
[null,null,"Tenderers are advised to study the Model Preambles for Trades before pricing this bill"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Paint specifications"]
[]
[null,null,"All surface preparation and painting shall be done in accordance with the specifications from  \"Plascon Paints\" attached to these Bills of Quantities unless otherwise described"]
[]
[null,null,"Colours"]
[]
[null,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[null,null,"PAINTWORK, ETC TO NEW WORK ON"]
[]
[null,null,"FLOATED PLASTER SURFACES WITH"]
[]
[null,null,"One coat Professional Gypsum & Plaster Primer (PP700) and two coats Double Velvet (VEL/TDV)"]
[]
[{"v":350,"d":"350 "},null,"Internal walls",null,"m²",{"v":178,"d":"178 "}]
[]
[{"v":351,"d":"351 "},null,"Bagged internal walls",null,"m²",{"v":20,"d":"20 "}]
[]
[null,null,"One coat Professional Bridging Compound (PWC520), one coat Professional Gypsum & Plaster Primer (PP700) and two coats Wall & All (WAA/TWA) for interior and exterior use"]
[]
[{"v":352,"d":"352 "},null,"External walls",null,"m²",{"v":134,"d":"134 "}]
[]
[{"v":353,"d":"353 "},null,"Extra over for paintwork on external walls in the \"Pastel\" colour group for paintwork in the \"Deep\" colour group",null,"m²",{"v":134,"d":"134 "}]
[]
[null,null,"PLASTER BOARD SURFACES WITH"]
[]
[null,null,"One coat Professional Gypsum & Plaster Primer (PP700) and two coats Double Velvet (VEL/TDV)"]
[]
[{"v":354,"d":"354 "},null,"Partitions",null,"m²",{"v":1960,"d":"1,960 "}]
[]
[null,null,"One coat Professional Gypsum & Plaster Primer (PP700) and two coats Professional All Purpose Matt (PEM800/TDA)"]
[]
[{"v":355,"d":"355 "},null,"Ceilings, bulkheads and cornices",null,"m²",{"v":69,"d":"69 "}]
[]
[null,null,"ON FIBRE-CEMENT BOARD SURFACES"]
[]
[null,null,"One coat Professional Bridging Compound (PWC520), one coat Professional Gypsum & Plaster Primer (PP700) and two coats Wall & All (WAA/TWA) for interior and exterior use"]
[]
[{"v":356,"d":"356 "},null,"Fascias and barge boards not exceeding 300mm girth, including priming metal jointing strips",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":357,"d":"357 "},null,"On roof eaves soffit at heights exceeding 10m but not exceeding 11.5m high",null,"m²",{"v":83,"d":"83 "}]
[]
[null,null,"METAL SURFACES WITH"]
[]
[null,null,"Sand down and clean to bare steel, thereafter apply one coat Professional All Purpose Undercoat (PU800) and two coats Velvaglo Water Based (VLW/TVW)/ Steel Tect 1300WB (EMS18)"]
[]
[{"v":358,"d":"358 "},null,"Door frame",null,"m²",{"v":19,"d":"19 "}]
[]
[{"v":359,"d":"359 "},null,"Rails, bars, pipes, etc. not exceeding 300mm girth",null,"m",{"v":79,"d":"79 "}]
[]
[null,null,"WOOD SURFACES WITH"]
[]
[null,null,"Prepare and apply one coat Wood Primer (UC2) and two coats Velvaglo Water Based (VLW/TVW)"]
[]
[{"v":360,"d":"360 "},null,"Doors",null,"m²",{"v":300,"d":"300 "}]
[]
[{"v":361,"d":"361 "},null,"Skirtings, rails, etc. not exceeding 300mm girth",null,"m",{"v":699,"d":"699 "}]
[]
[null,null,"SIGNWRITING"]
[]
[null,null,"Two coats reflective road marking paint on tarmacadam"]
[]
[{"v":362,"d":"362 "},null,"Line 100mm wide",null,"m",{"v":128,"d":"128 "}]
[]
[{"v":363,"d":"363 "},null,"Paraplegic parking motif 2000 x 1800mmm extreme",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"PAINTWORK, ETC TO PREVIOUSLY PAINTED WORK"]
[]
[null,null,"FLOATED PLASTER SURFACES WITH"]
[]
[null,null,"Prepare surface and apply one coat Professional Gypsum & Plaster Primer (PP700) and two coats of Professional Superior Low Sheen (PEM 1000/TLS)"]
[]
[{"v":364,"d":"364 "},null,"Internal walls",null,"m²",{"v":912,"d":"912 "}]
[]
[{"v":365,"d":"365 "},null,"Bagged internal walls",null,"m²",{"v":396,"d":"396 "}]
[]
[{"v":366,"d":"366 "},null,"On raking soffits of stairs",null,"m²",{"v":5,"d":"5 "}]
[]
[{"v":367,"d":"367 "},null,"Extra over for paintwork on internal walls in the \"Pastel\" colour group for paintwork in the \"Deep\" colour group",null,"m²",{"v":5,"d":"5 "}]
[]
[null,null,"Prepare surface and apply one coat Professional Gypsum & Plaster Primer (PP700) and two coats of Professional Superior Low Sheen (PEM 1000/TLS)"]
[]
[{"v":368,"d":"368 "},null,"External walls",null,"m²",{"v":727,"d":"727 "}]
[]
[{"v":369,"d":"369 "},null,"Extra over for paintwork on external walls in the \"Pastel\" colour group for paintwork in the \"Deep\" colour group",null,"m²",{"v":725,"d":"725 "}]
[]
[null,null,"PLASTER BOARD SURFACES WITH"]
[]
[null,null,"Prepare surface and apply two coats of White Liquid Rubber and two coats Weatherseal exterior matt paint"]
[]
[{"v":370,"d":"370 "},null,"Drywalls",null,"m²",{"v":86,"d":"86 "}]
[]
[null,null,"One coat Professional Gypsum & Plaster Primer (PP700) and two coats Kitchens & Bathrooms (KBM/TKM)"]
[]
[{"v":371,"d":"371 "},null,"Ceilings and beams (\"White\" colour group)",null,"m²",{"v":32,"d":"32 "}]
[]
[null,null,"ON SMOOTH CONCRETE SURFACES"]
[]
[null,null,"One coat Professional Gypsum Plaster Primer (PP700) and two coats Professional All Purpose Matt (PEM800/TDA), including stopping blowholes"]
[]
[{"v":372,"d":"372 "},null,"Ceilings and beams (\"White\" colour group)",null,"m²",{"v":12,"d":"12 "}]
[]
[null,null,"Spot primer bare and apply one coat Professional Water Based Gypsum Seal (PGS1) and two coats Professional Superior Low Sheen (PEM 1000/TLS), including stopping blow holes"]
[]
[{"v":373,"d":"373 "},null,"Walls and columns",null,"m²",{"v":351,"d":"351 "}]
[]
[null,null,"METAL SURFACES WITH"]
[]
[null,null,"Sand down and clean to bare steel, thereafter apply one coat Professional All Purpose Undercoat (PU800) and two coats Velvaglo Water Based (VLW/TVW)/ Steel Tect 1300WB (EMS18)"]
[]
[{"v":374,"d":"374 "},null,"Door frames",null,"m²",{"v":4,"d":"4 "}]
[]
[{"v":375,"d":"375 "},null,"On steel staircase  (both sides measured over the full flat area)",null,"m²",{"v":69,"d":"69 "}]
[]
[{"v":376,"d":"376 "},null,"On steel handrails 1000mm high not exceeding 300mm girth",null,"m",{"v":42,"d":"42 "}]
[]
[null,null,"WOOD SURFACES WITH"]
[]
[null,null,"Sand down to a smooth, even surface and apply three coats Woodcare Water Based Interior Varnish (Gloss: X45-50 range/WUT 3000 tint base Suede X51/WUB 3000 tint base)"]
[]
[{"v":377,"d":"377 "},null,"Doors",null,"m²",{"v":113,"d":"113 "}]
[]
[{"v":378,"d":"378 "},null,"Skirtings, rails, etc not exceeding 300mm girth",null,"m",{"v":14,"d":"14 "}]
[]
[{"v":1,"d":"1 "},null,"ALTERATIONS",null,"Page",{"v":44,"d":"44 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"EARTHWORKS",null,"Page",{"v":48,"d":"48 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"CONCRETE, FORMWORK AND REINFORCEMENT",null,"Page",{"v":54,"d":"54 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"MASONRY",null,"Page",{"v":58,"d":"58 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"WATERPROOFING",null,"Page",{"v":61,"d":"61 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"ROOF COVERINGS",null,"Page",{"v":64,"d":"64 "},{"v":0,"d":"0.00"}]
[]
[{"v":7,"d":"7 "},null,"CARPENTRY AND JOINERY",null,"Page",{"v":72,"d":"72 "},{"v":0,"d":"0.00"}]
[]
[{"v":8,"d":"8 "},null,"CEILINGS, PARTITIONS AND ACCESS FLOORING",null,"Page",{"v":78,"d":"78 "},{"v":0,"d":"0.00"}]
[]
[{"v":9,"d":"9 "},null,"FLOOR COVERINGS",null,"Page",{"v":79,"d":"79 "},{"v":0,"d":"0.00"}]
[]
[{"v":10,"d":"10 "},null,"METALWORK",null,"Page",{"v":85,"d":"85 "},{"v":0,"d":"0.00"}]
[]
[{"v":11,"d":"11 "},null,"IRONMONGERY",null,"Page",{"v":90,"d":"90 "},{"v":0,"d":"0.00"}]
[]
[{"v":12,"d":"12 "},null,"STRUCTURAL STEELWORK",null,"Page",{"v":93,"d":"93 "},{"v":0,"d":"0.00"}]
[]
[{"v":13,"d":"13 "},null,"PLASTERING",null,"Page",{"v":96,"d":"96 "},{"v":0,"d":"0.00"}]
[]
[{"v":14,"d":"14 "},null,"PLUMBING AND DRAINAGE (PROVISIONAL)",null,"Page",{"v":103,"d":"103 "},{"v":0,"d":"0.00"}]
[]
[{"v":15,"d":"15 "},null,"SANITARY FITTINGS",null,"Page",{"v":107,"d":"107 "},{"v":0,"d":"0.00"}]
[]
[{"v":16,"d":"16 "},null,"PAINTWORK",null,"Page",{"v":113,"d":"113 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SECTION 3 ELECTRICAL INSTALLATION"]
[]
[null,null,"BILL NO.1"]
[]
[null,null,"PRELIMINARY & GENERAL"]
[]
[{"v":1,"d":"1 "},null,"Allow for preliminary and general costs: (Site establishment and overheads)",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":2,"d":"2 "},null,"Safety plan and measures",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"OTHER : To be specified by the Tenderer"]
[]
[{"v":3,"d":"3 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":4,"d":"4 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":5,"d":"5 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":6,"d":"6 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.2"]
[]
[null,null,"LV ELECTRICITY SUPPLY"]
[]
[null,null,"DISTRIBUTION BOARDS"]
[]
[null,null,"Neatening, additional circuits as required, re-labelling and new panel doors including COC for each existing DB / DB Zone"]
[]
[null,null,"MDB"]
[]
[{"v":7,"d":"7 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":8,"d":"8 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DB BM"]
[]
[{"v":9,"d":"9 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":10,"d":"10 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DB GF"]
[]
[{"v":11,"d":"11 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":12,"d":"12 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DB 1F"]
[]
[{"v":13,"d":"13 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":14,"d":"14 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DB 2F"]
[]
[{"v":15,"d":"15 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":16,"d":"16 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"TESTING"]
[]
[{"v":17,"d":"17 "},null,"Testing and commission the installation included in this bill",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":18,"d":"18 "},null,"Provide CoC for the section in DB BM",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":19,"d":"19 "},null,"Provide CoC for the section in DB GF",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":20,"d":"20 "},null,"Provide CoC for the section in DB 1F",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":21,"d":"21 "},null,"Provide CoC for the section in DB 2F",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ATTENDANCE:"]
[]
[{"v":22,"d":"22 "},null,"Attendance on PABX / Access Control / CCTV installation by client & specialist equipment installation",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":23,"d":"23 "},null,"Attendance on I.T. cable installation by Client and Specialists",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":24,"d":"24 "},null,"Attendance on Making & Sealing of holes in Walls for cable tray & trunkings entering IT room.",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.3"]
[]
[null,null,"BASEMENT LIGHTING"]
[]
[null,null,"ELECTRICAL INSTALLATIONS : LIGHTING"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits in ceiling space/on surface"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":25,"d":"25 "},null,"MATERIAL :",null,"m",{"v":230,"d":"230 "}]
[]
[{"v":26,"d":"26 "},null,"LABOUR :",null,"m",{"v":230,"d":"230 "}]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":27,"d":"27 "},null,"MATERIAL:",null,"m",{"v":140,"d":"140 "}]
[]
[{"v":28,"d":"28 "},null,"LABOUR:",null,"m",{"v":140,"d":"140 "}]
[]
[null,null,"Conduits recessed in brickwork"]
[]
[null,null,"20mm diam  PVC"]
[]
[{"v":29,"d":"29 "},null,"MATERIAL :",null,"m",{"v":21,"d":"21 "}]
[]
[{"v":30,"d":"30 "},null,"LABOUR :",null,"m",{"v":21,"d":"21 "}]
[]
[null,null,"CONDUIT BOXES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x50x50 deep PVC onto brick, concrete surface or in roof space"]
[]
[{"v":31,"d":"31 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":32,"d":"32 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"50mm diam  x 25 PVC with lid deep onto brick, concrete surface or in roof space"]
[]
[{"v":33,"d":"33 "},null,"MATERIAL :",null,"No",{"v":18,"d":"18 "}]
[]
[{"v":34,"d":"34 "},null,"LABOUR :",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or in cable tray"]
[]
[null,null,"2.5mm2"]
[]
[{"v":35,"d":"35 "},null,"MATERIAL :",null,"m",{"v":740,"d":"740 "}]
[]
[{"v":36,"d":"36 "},null,"LABOUR :",null,"m",{"v":740,"d":"740 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or in cable tray"]
[]
[null,null,"2.5mm2"]
[]
[{"v":37,"d":"37 "},null,"MATERIAL",null,"m",{"v":360,"d":"360 "}]
[]
[{"v":38,"d":"38 "},null,"LABOUR",null,"m",{"v":360,"d":"360 "}]
[]
[null,null,"LUMINAIRES (including Tubes & Lamps)"]
[]
[null,null,"Supply & Install Luminaries"]
[]
[null,null,"Type F1"]
[]
[{"v":39,"d":"39 "},null,"MATERIAL :",null,"No",{"v":21,"d":"21 "}]
[]
[{"v":40,"d":"40 "},null,"LABOUR :",null,"No",{"v":21,"d":"21 "}]
[]
[null,null,"Type F2"]
[]
[{"v":41,"d":"41 "},null,"MATERIAL :",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":42,"d":"42 "},null,"LABOUR :",null,"No",{"v":6,"d":"6 "}]
[]
[null,null,"Type F4"]
[]
[{"v":43,"d":"43 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":44,"d":"44 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Type B1"]
[]
[{"v":45,"d":"45 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":46,"d":"46 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"Surface-mounted switch units(s) with cover plate(s) (boxes measured elsewhere)"]
[]
[null,null,"16A single lever, one-way light switch"]
[]
[{"v":47,"d":"47 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":48,"d":"48 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Ultrasound presence detector"]
[]
[{"v":49,"d":"49 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":50,"d":"50 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"16 Amp LED Dimmer Switch"]
[]
[{"v":51,"d":"51 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":52,"d":"52 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"TESTING"]
[]
[{"v":53,"d":"53 "},null,"Testing and commission the installation included in this bill",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.4"]
[]
[null,null,"BASEMENT POWER"]
[]
[null,null,"LV ELECTRICAL INSTALLATIONS : POWER AND IT"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits fixed on ceiling & surface & drywall"]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":54,"d":"54 "},null,"MATERIAL :",null,"m",{"v":55,"d":"55 "}]
[]
[{"v":55,"d":"55 "},null,"LABOUR :",null,"m",{"v":55,"d":"55 "}]
[]
[null,null,"Conduits fixed on ceiling & surface"]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":56,"d":"56 "},null,"MATERIAL:",null,"m",{"v":103,"d":"103 "}]
[]
[{"v":57,"d":"57 "},null,"LABOUR:",null,"m",{"v":103,"d":"103 "}]
[]
[null,null,"CONDUIT BOXES AND ACCESSORIES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x100x50 deep PVC in brick or concrete"]
[]
[{"v":58,"d":"58 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":59,"d":"59 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"100x100x50 deep PVC surface onto brick, concrete surface or in roof space"]
[]
[{"v":60,"d":"60 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":61,"d":"61 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"50mm diam x 25 surface PVC onto brick, concrete surface or in roof space"]
[]
[{"v":62,"d":"62 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":63,"d":"63 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"50mm diam PVC lids"]
[]
[{"v":64,"d":"64 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":65,"d":"65 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"100x100x50 deep Bosal surface onto brick, concrete surface or in roof space"]
[]
[{"v":66,"d":"66 "},null,"MATERIAL :",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":67,"d":"67 "},null,"LABOUR :",null,"No",{"v":8,"d":"8 "}]
[]
[null,null,"50mm diam x 25 surface Bosal onto brick, concrete surface or in roof space"]
[]
[{"v":68,"d":"68 "},null,"MATERIAL :",null,"No",{"v":19,"d":"19 "}]
[]
[{"v":69,"d":"69 "},null,"LABOUR :",null,"No",{"v":19,"d":"19 "}]
[]
[null,null,"50mm diam Bosal lids"]
[]
[{"v":70,"d":"70 "},null,"MATERIAL :",null,"No",{"v":20,"d":"20 "}]
[]
[{"v":71,"d":"71 "},null,"LABOUR :",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or trunking"]
[]
[null,null,"4mm2"]
[]
[{"v":72,"d":"72 "},null,"MATERIAL :",null,"m",{"v":475,"d":"475 "}]
[]
[{"v":73,"d":"73 "},null,"LABOUR :",null,"m",{"v":475,"d":"475 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or trunking"]
[]
[null,null,"2,5mm2"]
[]
[{"v":74,"d":"74 "},null,"MATERIAL",null,"m",{"v":240,"d":"240 "}]
[]
[{"v":75,"d":"75 "},null,"LABOUR",null,"m",{"v":240,"d":"240 "}]
[]
[null,null,"Drawwire"]
[]
[{"v":76,"d":"76 "},null,"MATERIAL",null,"m",{"v":90,"d":"90 "}]
[]
[{"v":77,"d":"77 "},null,"LABOUR",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"16A single phase isolator (surface indoor)"]
[]
[{"v":78,"d":"78 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":79,"d":"79 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Normal  Euro 16 Amp SSO"]
[]
[{"v":80,"d":"80 "},null,"MATERIAL :",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":81,"d":"81 "},null,"LABOUR :",null,"No",{"v":8,"d":"8 "}]
[]
[null,null,"BILL NO.5"]
[]
[null,null,"GROUND FLOOR LIGHTING"]
[]
[null,null,"ELECTRICAL INSTALLATIONS : LIGHTING"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits in ceiling space/on surface"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":82,"d":"82 "},null,"MATERIAL :",null,"m",{"v":350,"d":"350 "}]
[]
[{"v":83,"d":"83 "},null,"LABOUR :",null,"m",{"v":350,"d":"350 "}]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":84,"d":"84 "},null,"MATERIAL:",null,"m",{"v":65,"d":"65 "}]
[]
[{"v":85,"d":"85 "},null,"LABOUR:",null,"m",{"v":65,"d":"65 "}]
[]
[null,null,"Conduits recessed in brickwork"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":86,"d":"86 "},null,"MATERIAL :",null,"m",{"v":80,"d":"80 "}]
[]
[{"v":87,"d":"87 "},null,"LABOUR :",null,"m",{"v":80,"d":"80 "}]
[]
[null,null,"CONDUIT BOXES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x50x50 deep PVC onto brick, concrete surface or in roof space"]
[]
[{"v":88,"d":"88 "},null,"MATERIAL :",null,"No",{"v":25,"d":"25 "}]
[]
[{"v":89,"d":"89 "},null,"LABOUR :",null,"No",{"v":25,"d":"25 "}]
[]
[null,null,"50mm diam x 25 PVC with lid deep onto brick, concrete surface or in roof space"]
[]
[{"v":90,"d":"90 "},null,"MATERIAL :",null,"No",{"v":85,"d":"85 "}]
[]
[{"v":91,"d":"91 "},null,"LABOUR :",null,"No",{"v":85,"d":"85 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or in cable tray"]
[]
[null,null,"2.5mm2"]
[]
[{"v":92,"d":"92 "},null,"MATERIAL :",null,"m",{"v":840,"d":"840 "}]
[]
[{"v":93,"d":"93 "},null,"LABOUR :",null,"m",{"v":840,"d":"840 "}]
[]
[null,null,"4mm2"]
[]
[{"v":94,"d":"94 "},null,"MATERIAL :",null,"m",{"v":90,"d":"90 "}]
[]
[{"v":95,"d":"95 "},null,"LABOUR :",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or in cable tray"]
[]
[null,null,"2,5mm2"]
[]
[{"v":96,"d":"96 "},null,"MATERIAL",null,"m",{"v":450,"d":"450 "}]
[]
[{"v":97,"d":"97 "},null,"LABOUR",null,"m",{"v":450,"d":"450 "}]
[]
[null,null,"LUMINAIRES (including Tubes & Lamps)"]
[]
[null,null,"Supply & Install Luminiares"]
[]
[null,null,"Type F2"]
[]
[{"v":98,"d":"98 "},null,"MATERIAL :",null,"No",{"v":29,"d":"29 "}]
[]
[{"v":99,"d":"99 "},null,"LABOUR :",null,"No",{"v":29,"d":"29 "}]
[]
[null,null,"Type F3"]
[]
[{"v":100,"d":"100 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":101,"d":"101 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Type F4"]
[]
[{"v":102,"d":"102 "},null,"MATERIAL :",null,"No",{"v":28,"d":"28 "}]
[]
[{"v":103,"d":"103 "},null,"LABOUR :",null,"No",{"v":28,"d":"28 "}]
[]
[null,null,"Type F4/E"]
[]
[{"v":104,"d":"104 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":105,"d":"105 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"Type D1"]
[]
[{"v":106,"d":"106 "},null,"MATERIAL :",null,"No",{"v":13,"d":"13 "}]
[]
[{"v":107,"d":"107 "},null,"LABOUR :",null,"No",{"v":13,"d":"13 "}]
[]
[null,null,"Type D2"]
[]
[{"v":108,"d":"108 "},null,"MATERIAL :",null,"No",{"v":24,"d":"24 "}]
[]
[{"v":109,"d":"109 "},null,"LABOUR :",null,"No",{"v":24,"d":"24 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"Surface-mounted switch units(s) with coverplate(s) (boxes measured elsewhere)"]
[]
[null,null,"16A single lever, one-way light switch"]
[]
[{"v":110,"d":"110 "},null,"MATERIAL :",null,"No",{"v":24,"d":"24 "}]
[]
[{"v":111,"d":"111 "},null,"LABOUR :",null,"No",{"v":24,"d":"24 "}]
[]
[null,null,"16 Amp LED Dimmer Switch"]
[]
[{"v":112,"d":"112 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":113,"d":"113 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"TESTING"]
[]
[{"v":114,"d":"114 "},null,"Testing and commission the installation included in this bill",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.6"]
[]
[null,null,"GROUND FLOOR POWER"]
[]
[null,null,"LV ELECTRICAL INSTALLATIONS : POWER AND IT"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits fixed on ceiling & surface & drywall"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":115,"d":"115 "},null,"MATERIAL :",null,"m",{"v":60,"d":"60 "}]
[]
[{"v":116,"d":"116 "},null,"LABOUR :",null,"m",{"v":60,"d":"60 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":117,"d":"117 "},null,"MATERIAL :",null,"m",{"v":731,"d":"731 "}]
[]
[{"v":118,"d":"118 "},null,"LABOUR :",null,"m",{"v":731,"d":"731 "}]
[]
[null,null,"Conduits in slab / chased into brickwork"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":119,"d":"119 "},null,"MATERIAL :",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":120,"d":"120 "},null,"LABOUR :",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":121,"d":"121 "},null,"MATERIAL :",null,"m",{"v":75,"d":"75 "}]
[]
[{"v":122,"d":"122 "},null,"LABOUR :",null,"m",{"v":75,"d":"75 "}]
[]
[null,null,"Conduits fixed on ceiling & surface"]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":123,"d":"123 "},null,"MATERIAL:",null,"m",{"v":35,"d":"35 "}]
[]
[{"v":124,"d":"124 "},null,"LABOUR:",null,"m",{"v":35,"d":"35 "}]
[]
[null,null,"CONDUIT BOXES AND ACCESSORIES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x100x50 deep PVC in brick or concrete"]
[]
[{"v":125,"d":"125 "},null,"MATERIAL :",null,"No",{"v":33,"d":"33 "}]
[]
[{"v":126,"d":"126 "},null,"LABOUR :",null,"No",{"v":33,"d":"33 "}]
[]
[null,null,"100x50x50 deep PVC under desk"]
[]
[{"v":127,"d":"127 "},null,"MATERIAL :",null,"No",{"v":72,"d":"72 "}]
[]
[{"v":128,"d":"128 "},null,"LABOUR :",null,"No",{"v":72,"d":"72 "}]
[]
[null,null,"100x100x50 deep PVC surface onto brick, concrete surface or in roof space"]
[]
[{"v":129,"d":"129 "},null,"MATERIAL :",null,"No",{"v":9,"d":"9 "}]
[]
[{"v":130,"d":"130 "},null,"LABOUR :",null,"No",{"v":9,"d":"9 "}]
[]
[null,null,"50mm diam x 25 surface PVC onto brick, concrete surface or in roof space"]
[]
[{"v":131,"d":"131 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":132,"d":"132 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"50mm diam PVC lids"]
[]
[{"v":133,"d":"133 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":134,"d":"134 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"100x100x50 deep Bosal surface onto brick, concrete surface or in roof space"]
[]
[{"v":135,"d":"135 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":136,"d":"136 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"50mm diam x 25 surface Bosal onto brick, concrete surface or in roof space"]
[]
[{"v":137,"d":"137 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":138,"d":"138 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"50mm diam Bosal lids"]
[]
[{"v":139,"d":"139 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":140,"d":"140 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Powerskirting & Recessed Floor Outlets"]
[]
[null,null,"PVC Powerskiting complete with covers fixing outlets as indicated"]
[]
[null,null,"3 compartment 2 cover powerskirting"]
[]
[{"v":141,"d":"141 "},null,"MATERIAL :",null,"m",{"v":109,"d":"109 "}]
[]
[{"v":142,"d":"142 "},null,"LABOUR :",null,"m",{"v":109,"d":"109 "}]
[]
[null,null,"Corner piece"]
[]
[{"v":143,"d":"143 "},null,"MATERIAL :",null,"No",{"v":10,"d":"10 "}]
[]
[{"v":144,"d":"144 "},null,"LABOUR :",null,"No",{"v":10,"d":"10 "}]
[]
[null,null,"End Caps"]
[]
[{"v":145,"d":"145 "},null,"MATERIAL :",null,"No",{"v":20,"d":"20 "}]
[]
[{"v":146,"d":"146 "},null,"LABOUR :",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"Back box for powerskirting"]
[]
[{"v":147,"d":"147 "},null,"MATERIAL :",null,"No",{"v":28,"d":"28 "}]
[]
[{"v":148,"d":"148 "},null,"LABOUR :",null,"No",{"v":28,"d":"28 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or trunking"]
[]
[null,null,"6mm2"]
[]
[{"v":149,"d":"149 "},null,"MATERIAL :",null,"m",{"v":340,"d":"340 "}]
[]
[{"v":150,"d":"150 "},null,"LABOUR :",null,"m",{"v":340,"d":"340 "}]
[]
[null,null,"4mm2"]
[]
[{"v":151,"d":"151 "},null,"MATERIAL :",null,"m",{"v":4280,"d":"4,280 "}]
[]
[{"v":152,"d":"152 "},null,"LABOUR :",null,"m",{"v":4280,"d":"4,280 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or trunking"]
[]
[null,null,"4mm2"]
[]
[{"v":153,"d":"153 "},null,"MATERIAL",null,"m",{"v":130,"d":"130 "}]
[]
[{"v":154,"d":"154 "},null,"LABOUR",null,"m",{"v":130,"d":"130 "}]
[]
[null,null,"2,5mm2"]
[]
[{"v":155,"d":"155 "},null,"MATERIAL",null,"m",{"v":2140,"d":"2,140 "}]
[]
[{"v":156,"d":"156 "},null,"LABOUR",null,"m",{"v":2140,"d":"2,140 "}]
[]
[null,null,"Drawwire"]
[]
[{"v":157,"d":"157 "},null,"MATERIAL",null,"m",{"v":840,"d":"840 "}]
[]
[{"v":158,"d":"158 "},null,"LABOUR",null,"m",{"v":840,"d":"840 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"16 Amp 1x SA and 1x Euro SSO for powerskirting"]
[]
[{"v":159,"d":"159 "},null,"MATERIAL :",null,"No",{"v":45,"d":"45 "}]
[]
[{"v":160,"d":"160 "},null,"LABOUR :",null,"No",{"v":45,"d":"45 "}]
[]
[null,null,"16 Amp Double D-pin SSO for powerskirting"]
[]
[{"v":161,"d":"161 "},null,"MATERIAL :",null,"No",{"v":39,"d":"39 "}]
[]
[{"v":162,"d":"162 "},null,"LABOUR :",null,"No",{"v":39,"d":"39 "}]
[]
[null,null,"IT Cover Plate for powerskirting"]
[]
[{"v":163,"d":"163 "},null,"MATERIAL :",null,"No",{"v":70,"d":"70 "}]
[]
[{"v":164,"d":"164 "},null,"LABOUR :",null,"No",{"v":70,"d":"70 "}]
[]
[null,null,"16A single phase isolator (surface indoor)"]
[]
[{"v":165,"d":"165 "},null,"MATERIAL :",null,"No",{"v":13,"d":"13 "}]
[]
[{"v":166,"d":"166 "},null,"LABOUR :",null,"No",{"v":13,"d":"13 "}]
[]
[null,null,"16A single phase isolator (surface weatherproof)"]
[]
[{"v":167,"d":"167 "},null,"MATERIAL :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":168,"d":"168 "},null,"LABOUR :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"32A single phase isolator (surface weatherproof)"]
[]
[{"v":169,"d":"169 "},null,"MATERIAL :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":170,"d":"170 "},null,"LABOUR :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"32A three-phase isolator (surface weatherproof)"]
[]
[{"v":171,"d":"171 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":172,"d":"172 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Outlets in wall / drywall"]
[]
[null,null,"Normal  Euro 16 Amp SSO"]
[]
[{"v":173,"d":"173 "},null,"MATERIAL :",null,"No",{"v":17,"d":"17 "}]
[]
[{"v":174,"d":"174 "},null,"LABOUR :",null,"No",{"v":17,"d":"17 "}]
[]
[null,null,"Double 16 Amp D-pin SSO"]
[]
[{"v":175,"d":"175 "},null,"MATERIAL :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":176,"d":"176 "},null,"LABOUR :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":177,"d":"177 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":178,"d":"178 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"HDMI outlet"]
[]
[{"v":179,"d":"179 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":180,"d":"180 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Floor box outlet complete with SSO's (recessed 2xSA & 2xEuro with 2xIT/Data outlets)"]
[]
[{"v":181,"d":"181 "},null,"MATERIAL :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":182,"d":"182 "},null,"LABOUR :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Outlets in boxes mounted surface under desks"]
[]
[null,null,"Normal  Euro 16 Amp SSO complete with flyleads"]
[]
[{"v":183,"d":"183 "},null,"MATERIAL :",null,"No",{"v":36,"d":"36 "}]
[]
[{"v":184,"d":"184 "},null,"LABOUR :",null,"No",{"v":36,"d":"36 "}]
[]
[null,null,"Double 16 Amp D-pin SSO complete with flyleads"]
[]
[{"v":185,"d":"185 "},null,"MATERIAL :",null,"No",{"v":36,"d":"36 "}]
[]
[{"v":186,"d":"186 "},null,"LABOUR :",null,"No",{"v":36,"d":"36 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":187,"d":"187 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":188,"d":"188 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"CABLE TRAYS"]
[]
[null,null,"200mm wide heavy-duty wire mesh cable tray"]
[]
[{"v":189,"d":"189 "},null,"MATERIAL :",null,"m",{"v":60,"d":"60 "}]
[]
[{"v":190,"d":"190 "},null,"LABOUR :",null,"m",{"v":60,"d":"60 "}]
[]
[null,null,"200mm wide wire mesh cable tray 90 deg bend"]
[]
[{"v":191,"d":"191 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":192,"d":"192 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"200mm wide wire mesh cable tray T-piece"]
[]
[{"v":193,"d":"193 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":194,"d":"194 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"100mm wire mesh cable tray fixed under desks"]
[]
[{"v":195,"d":"195 "},null,"MATERIAL :",null,"m",{"v":50,"d":"50 "}]
[]
[{"v":196,"d":"196 "},null,"LABOUR :",null,"m",{"v":50,"d":"50 "}]
[]
[null,null,"P9000 Trunking in ceiling space"]
[]
[{"v":197,"d":"197 "},null,"MATERIAL :",null,"m",{"v":60,"d":"60 "}]
[]
[{"v":198,"d":"198 "},null,"LABOUR :",null,"m",{"v":60,"d":"60 "}]
[]
[null,null,"BILL NO.7"]
[]
[null,null,"FIRST FLOOR LIGHTING"]
[]
[null,null,"ELECTRICAL INSTALLATIONS : LIGHTING"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits in ceiling space/on surface"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":199,"d":"199 "},null,"MATERIAL :",null,"m",{"v":280,"d":"280 "}]
[]
[{"v":200,"d":"200 "},null,"LABOUR :",null,"m",{"v":280,"d":"280 "}]
[]
[null,null,"Conduits recessed in brickwork"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":201,"d":"201 "},null,"MATERIAL :",null,"m",{"v":90,"d":"90 "}]
[]
[{"v":202,"d":"202 "},null,"LABOUR :",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"CONDUIT BOXES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x50x50 deep PVC onto brick, concrete surface or in roof space"]
[]
[{"v":203,"d":"203 "},null,"MATERIAL :",null,"No",{"v":29,"d":"29 "}]
[]
[{"v":204,"d":"204 "},null,"LABOUR :",null,"No",{"v":29,"d":"29 "}]
[]
[null,null,"50mm diam x 25 PVC with lid deep onto brick, concrete surface or in roof space"]
[]
[{"v":205,"d":"205 "},null,"MATERIAL :",null,"No",{"v":110,"d":"110 "}]
[]
[{"v":206,"d":"206 "},null,"LABOUR :",null,"No",{"v":110,"d":"110 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or in cable tray"]
[]
[null,null,"2.5mm2"]
[]
[{"v":207,"d":"207 "},null,"MATERIAL :",null,"m",{"v":1200,"d":"1,200 "}]
[]
[{"v":208,"d":"208 "},null,"LABOUR :",null,"m",{"v":1200,"d":"1,200 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or in cable tray"]
[]
[null,null,"2,5mm2"]
[]
[{"v":209,"d":"209 "},null,"MATERIAL",null,"m",{"v":450,"d":"450 "}]
[]
[{"v":210,"d":"210 "},null,"LABOUR",null,"m",{"v":450,"d":"450 "}]
[]
[null,null,"LUMINAIRES (including Tubes & Lamps)"]
[]
[null,null,"Supply & Install Luminiares"]
[]
[null,null,"Type F4"]
[]
[{"v":211,"d":"211 "},null,"MATERIAL :",null,"No",{"v":64,"d":"64 "}]
[]
[{"v":212,"d":"212 "},null,"LABOUR :",null,"No",{"v":64,"d":"64 "}]
[]
[null,null,"Type F4/E"]
[]
[{"v":213,"d":"213 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":214,"d":"214 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Type D1"]
[]
[{"v":215,"d":"215 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":216,"d":"216 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"Type D2"]
[]
[{"v":217,"d":"217 "},null,"MATERIAL :",null,"No",{"v":22,"d":"22 "}]
[]
[{"v":218,"d":"218 "},null,"LABOUR :",null,"No",{"v":22,"d":"22 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"Surface-mounted switch units(s) with coverplate(s) (boxes measured elsewhere)"]
[]
[null,null,"16A single lever, one-way light switch"]
[]
[{"v":219,"d":"219 "},null,"MATERIAL :",null,"No",{"v":27,"d":"27 "}]
[]
[{"v":220,"d":"220 "},null,"LABOUR :",null,"No",{"v":27,"d":"27 "}]
[]
[null,null,"16 Amp LED Dimmer Switch"]
[]
[{"v":221,"d":"221 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":222,"d":"222 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"TESTING"]
[]
[{"v":223,"d":"223 "},null,"Testing and commission the installation included in this bill",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.8"]
[]
[null,null,"FIRST FLOOR POWER"]
[]
[null,null,"LV ELECTRICAL INSTALLATIONS : POWER AND IT"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits fixed on ceiling & surface & drywall"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":224,"d":"224 "},null,"MATERIAL :",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":225,"d":"225 "},null,"LABOUR :",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":226,"d":"226 "},null,"MATERIAL :",null,"m",{"v":440,"d":"440 "}]
[]
[{"v":227,"d":"227 "},null,"LABOUR :",null,"m",{"v":440,"d":"440 "}]
[]
[null,null,"Conduits in slab / chased into brickwork"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":228,"d":"228 "},null,"MATERIAL :",null,"m",{"v":30,"d":"30 "}]
[]
[{"v":229,"d":"229 "},null,"LABOUR :",null,"m",{"v":30,"d":"30 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":230,"d":"230 "},null,"MATERIAL :",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":231,"d":"231 "},null,"LABOUR :",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"Conduits fixed on ceiling & surface"]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":232,"d":"232 "},null,"MATERIAL:",null,"m",{"v":80,"d":"80 "}]
[]
[{"v":233,"d":"233 "},null,"LABOUR:",null,"m",{"v":80,"d":"80 "}]
[]
[null,null,"CONDUIT BOXES AND ACCESSORIES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x100x50 deep PVC in brick or concrete"]
[]
[{"v":234,"d":"234 "},null,"MATERIAL :",null,"No",{"v":32,"d":"32 "}]
[]
[{"v":235,"d":"235 "},null,"LABOUR :",null,"No",{"v":32,"d":"32 "}]
[]
[null,null,"100x50x50 deep PVC under desk"]
[]
[{"v":236,"d":"236 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":237,"d":"237 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"100x100x50 deep PVC surface onto brick, concrete surface or in roof space"]
[]
[{"v":238,"d":"238 "},null,"MATERIAL :",null,"No",{"v":15,"d":"15 "}]
[]
[{"v":239,"d":"239 "},null,"LABOUR :",null,"No",{"v":15,"d":"15 "}]
[]
[null,null,"50mm diam x 25 surface PVC onto brick, concrete surface or in roof space"]
[]
[{"v":240,"d":"240 "},null,"MATERIAL :",null,"No",{"v":22,"d":"22 "}]
[]
[{"v":241,"d":"241 "},null,"LABOUR :",null,"No",{"v":22,"d":"22 "}]
[]
[null,null,"50mm diam PVC lids"]
[]
[{"v":242,"d":"242 "},null,"MATERIAL :",null,"No",{"v":22,"d":"22 "}]
[]
[{"v":243,"d":"243 "},null,"LABOUR :",null,"No",{"v":22,"d":"22 "}]
[]
[null,null,"100x100x50 deep Bosal surface onto brick, concrete surface or in roof space"]
[]
[{"v":244,"d":"244 "},null,"MATERIAL :",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":245,"d":"245 "},null,"LABOUR :",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"50mm diam x 25 surface Bosal onto brick, concrete surface or in roof space"]
[]
[{"v":246,"d":"246 "},null,"MATERIAL :",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":247,"d":"247 "},null,"LABOUR :",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"50mm diam Bosal lids"]
[]
[{"v":248,"d":"248 "},null,"MATERIAL :",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":249,"d":"249 "},null,"LABOUR :",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"Powerskirting & Recessed Floor Outlets"]
[]
[null,null,"PVC Powerskiting complete with covers fixing outlets as indicated"]
[]
[null,null,"3 compartment 2 cover powerskirting"]
[]
[{"v":250,"d":"250 "},null,"MATERIAL :",null,"m",{"v":115,"d":"115 "}]
[]
[{"v":251,"d":"251 "},null,"LABOUR :",null,"m",{"v":115,"d":"115 "}]
[]
[null,null,"Corner piece"]
[]
[{"v":252,"d":"252 "},null,"MATERIAL :",null,"No",{"v":19,"d":"19 "}]
[]
[{"v":253,"d":"253 "},null,"LABOUR :",null,"No",{"v":19,"d":"19 "}]
[]
[null,null,"End Caps"]
[]
[{"v":254,"d":"254 "},null,"MATERIAL :",null,"No",{"v":26,"d":"26 "}]
[]
[{"v":255,"d":"255 "},null,"LABOUR :",null,"No",{"v":26,"d":"26 "}]
[]
[null,null,"Back box for powerskirting"]
[]
[{"v":256,"d":"256 "},null,"MATERIAL :",null,"No",{"v":18,"d":"18 "}]
[]
[{"v":257,"d":"257 "},null,"LABOUR :",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or trunking"]
[]
[null,null,"6mm2"]
[]
[{"v":258,"d":"258 "},null,"MATERIAL :",null,"m",{"v":350,"d":"350 "}]
[]
[{"v":259,"d":"259 "},null,"LABOUR :",null,"m",{"v":350,"d":"350 "}]
[]
[null,null,"4mm2"]
[]
[{"v":260,"d":"260 "},null,"MATERIAL :",null,"m",{"v":4120,"d":"4,120 "}]
[]
[{"v":261,"d":"261 "},null,"LABOUR :",null,"m",{"v":4120,"d":"4,120 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or trunking"]
[]
[null,null,"4mm2"]
[]
[{"v":262,"d":"262 "},null,"MATERIAL",null,"m",{"v":110,"d":"110 "}]
[]
[{"v":263,"d":"263 "},null,"LABOUR",null,"m",{"v":110,"d":"110 "}]
[]
[null,null,"2,5mm2"]
[]
[{"v":264,"d":"264 "},null,"MATERIAL",null,"m",{"v":2050,"d":"2,050 "}]
[]
[{"v":265,"d":"265 "},null,"LABOUR",null,"m",{"v":2050,"d":"2,050 "}]
[]
[null,null,"Drawwire"]
[]
[{"v":266,"d":"266 "},null,"MATERIAL",null,"m",{"v":485,"d":"485 "}]
[]
[{"v":267,"d":"267 "},null,"LABOUR",null,"m",{"v":485,"d":"485 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"16 Amp 1x SA and 1x Euro SSO for powerskirting"]
[]
[{"v":268,"d":"268 "},null,"MATERIAL :",null,"No",{"v":38,"d":"38 "}]
[]
[{"v":269,"d":"269 "},null,"LABOUR :",null,"No",{"v":38,"d":"38 "}]
[]
[null,null,"16 Amp Double D-pin SSO for powerskirting"]
[]
[{"v":270,"d":"270 "},null,"MATERIAL :",null,"No",{"v":27,"d":"27 "}]
[]
[{"v":271,"d":"271 "},null,"LABOUR :",null,"No",{"v":27,"d":"27 "}]
[]
[null,null,"IT Cover Plate for powerskirting"]
[]
[{"v":272,"d":"272 "},null,"MATERIAL :",null,"No",{"v":34,"d":"34 "}]
[]
[{"v":273,"d":"273 "},null,"LABOUR :",null,"No",{"v":34,"d":"34 "}]
[]
[null,null,"16A single phase isolator (surface indoor)"]
[]
[{"v":274,"d":"274 "},null,"MATERIAL :",null,"No",{"v":13,"d":"13 "}]
[]
[{"v":275,"d":"275 "},null,"LABOUR :",null,"No",{"v":13,"d":"13 "}]
[]
[null,null,"16A single phase isolator (surface weatherproof)"]
[]
[{"v":276,"d":"276 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":277,"d":"277 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"32A single phase isolator (surface weatherproof)"]
[]
[{"v":278,"d":"278 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":279,"d":"279 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"32A three-phase isolator (surface weatherproof)"]
[]
[{"v":280,"d":"280 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":281,"d":"281 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Outlets in wall / drywall"]
[]
[null,null,"Normal  Euro 16 Amp SSO"]
[]
[{"v":282,"d":"282 "},null,"MATERIAL :",null,"No",{"v":22,"d":"22 "}]
[]
[{"v":283,"d":"283 "},null,"LABOUR :",null,"No",{"v":22,"d":"22 "}]
[]
[null,null,"Double 16 Amp D-pin SSO"]
[]
[{"v":284,"d":"284 "},null,"MATERIAL :",null,"No",{"v":7,"d":"7 "}]
[]
[{"v":285,"d":"285 "},null,"LABOUR :",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":286,"d":"286 "},null,"MATERIAL :",null,"No",{"v":9,"d":"9 "}]
[]
[{"v":287,"d":"287 "},null,"LABOUR :",null,"No",{"v":9,"d":"9 "}]
[]
[null,null,"HDMI outlet"]
[]
[{"v":288,"d":"288 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":289,"d":"289 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Floor box outlet complete with SSO's (recessed 2xSA & 2xEuro with 2xIT/Data outlets)"]
[]
[{"v":290,"d":"290 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":291,"d":"291 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Outlets in boxes mounted surface under desks"]
[]
[null,null,"Normal  Euro 16 Amp SSO complete with flyleads"]
[]
[{"v":292,"d":"292 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":293,"d":"293 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Double 16 Amp D-pin SSO complete with flyleads"]
[]
[{"v":294,"d":"294 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":295,"d":"295 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":296,"d":"296 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":297,"d":"297 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"CABLE TRAYS"]
[]
[null,null,"200mm wide heavy-duty wire mesh cable tray"]
[]
[{"v":298,"d":"298 "},null,"MATERIAL :",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":299,"d":"299 "},null,"LABOUR :",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"200mm wide wire mesh cable tray 90 deg bend"]
[]
[{"v":300,"d":"300 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":301,"d":"301 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"200mm wide wire mesh cable tray T-piece"]
[]
[{"v":302,"d":"302 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":303,"d":"303 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"100mm wire mesh cable tray fixed under desks"]
[]
[{"v":304,"d":"304 "},null,"MATERIAL :",null,"m",{"v":50,"d":"50 "}]
[]
[{"v":305,"d":"305 "},null,"LABOUR :",null,"m",{"v":50,"d":"50 "}]
[]
[null,null,"P9000 Trunking in ceiling space"]
[]
[{"v":306,"d":"306 "},null,"MATERIAL :",null,"m",{"v":60,"d":"60 "}]
[]
[{"v":307,"d":"307 "},null,"LABOUR :",null,"m",{"v":60,"d":"60 "}]
[]
[null,null,"BILL NO.9"]
[]
[null,null,"SECOND FLOOR LIGHTING"]
[]
[null,null,"ELECTRICAL INSTALLATIONS : LIGHTING"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits in ceiling space/on surface"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":308,"d":"308 "},null,"MATERIAL :",null,"m",{"v":170,"d":"170 "}]
[]
[{"v":309,"d":"309 "},null,"LABOUR :",null,"m",{"v":170,"d":"170 "}]
[]
[null,null,"Conduits recessed in brickwork"]
[]
[null,null,"20mm diam PVC"]
[]
[{"v":310,"d":"310 "},null,"MATERIAL :",null,"m",{"v":70,"d":"70 "}]
[]
[{"v":311,"d":"311 "},null,"LABOUR :",null,"m",{"v":70,"d":"70 "}]
[]
[null,null,"CONDUIT BOXES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x50x50 deep PVC onto brick, concrete surface or in roof space"]
[]
[{"v":312,"d":"312 "},null,"MATERIAL :",null,"No",{"v":22,"d":"22 "}]
[]
[{"v":313,"d":"313 "},null,"LABOUR :",null,"No",{"v":22,"d":"22 "}]
[]
[null,null,"50mm diam x 25 PVC with lid deep onto brick, concrete surface or in roof space"]
[]
[{"v":314,"d":"314 "},null,"MATERIAL :",null,"No",{"v":102,"d":"102 "}]
[]
[{"v":315,"d":"315 "},null,"LABOUR :",null,"No",{"v":102,"d":"102 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or in cable tray"]
[]
[null,null,"2.5mm2"]
[]
[{"v":316,"d":"316 "},null,"MATERIAL :",null,"m",{"v":780,"d":"780 "}]
[]
[{"v":317,"d":"317 "},null,"LABOUR :",null,"m",{"v":780,"d":"780 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or in cable tray"]
[]
[null,null,"2,5mm2"]
[]
[{"v":318,"d":"318 "},null,"MATERIAL",null,"m",{"v":350,"d":"350 "}]
[]
[{"v":319,"d":"319 "},null,"LABOUR",null,"m",{"v":350,"d":"350 "}]
[]
[null,null,"LUMINAIRES (including Tubes & Lamps)"]
[]
[null,null,"Supply & Install Luminiares"]
[]
[null,null,"Type F2"]
[]
[{"v":320,"d":"320 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":321,"d":"321 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Type F4"]
[]
[{"v":322,"d":"322 "},null,"MATERIAL :",null,"No",{"v":44,"d":"44 "}]
[]
[{"v":323,"d":"323 "},null,"LABOUR :",null,"No",{"v":44,"d":"44 "}]
[]
[null,null,"Type F4/E"]
[]
[{"v":324,"d":"324 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":325,"d":"325 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Type D1"]
[]
[{"v":326,"d":"326 "},null,"MATERIAL :",null,"No",{"v":8,"d":"8 "}]
[]
[{"v":327,"d":"327 "},null,"LABOUR :",null,"No",{"v":8,"d":"8 "}]
[]
[null,null,"Type D2"]
[]
[{"v":328,"d":"328 "},null,"MATERIAL :",null,"No",{"v":18,"d":"18 "}]
[]
[{"v":329,"d":"329 "},null,"LABOUR :",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"Surface-mounted switch units(s) with coverplate(s) (boxes measured elsewhere)"]
[]
[null,null,"16A single lever, one-way light switch"]
[]
[{"v":330,"d":"330 "},null,"MATERIAL :",null,"No",{"v":21,"d":"21 "}]
[]
[{"v":331,"d":"331 "},null,"LABOUR :",null,"No",{"v":21,"d":"21 "}]
[]
[null,null,"16 Amp LED Dimmer Switch"]
[]
[{"v":332,"d":"332 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":333,"d":"333 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"TESTING"]
[]
[{"v":334,"d":"334 "},null,"Testing and commission the installation included in this bill",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.10"]
[]
[null,null,"SECOND FLOOR POWER"]
[]
[null,null,"LV ELECTRICAL INSTALLATIONS : POWER AND IT"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits fixed on ceiling & surface & drywall"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":335,"d":"335 "},null,"MATERIAL :",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":336,"d":"336 "},null,"LABOUR :",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":337,"d":"337 "},null,"MATERIAL :",null,"m",{"v":605,"d":"605 "}]
[]
[{"v":338,"d":"338 "},null,"LABOUR :",null,"m",{"v":605,"d":"605 "}]
[]
[null,null,"Conduits in slab / chased into brickwork"]
[]
[null,null,"32mm diam PVC"]
[]
[{"v":339,"d":"339 "},null,"MATERIAL :",null,"m",{"v":45,"d":"45 "}]
[]
[{"v":340,"d":"340 "},null,"LABOUR :",null,"m",{"v":45,"d":"45 "}]
[]
[null,null,"25mm diam PVC"]
[]
[{"v":341,"d":"341 "},null,"MATERIAL :",null,"m",{"v":80,"d":"80 "}]
[]
[{"v":342,"d":"342 "},null,"LABOUR :",null,"m",{"v":80,"d":"80 "}]
[]
[null,null,"Conduits fixed on ceiling & surface"]
[]
[null,null,"25mm diam  Bosal"]
[]
[{"v":343,"d":"343 "},null,"MATERIAL:",null,"m",{"v":25,"d":"25 "}]
[]
[{"v":344,"d":"344 "},null,"LABOUR:",null,"m",{"v":25,"d":"25 "}]
[]
[null,null,"CONDUIT BOXES AND ACCESSORIES"]
[]
[null,null,"Outlet boxes without covers"]
[]
[null,null,"100x100x50 deep PVC in brick or concrete"]
[]
[{"v":345,"d":"345 "},null,"MATERIAL :",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":346,"d":"346 "},null,"LABOUR :",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"100x50x50 deep PVC under desk"]
[]
[{"v":347,"d":"347 "},null,"MATERIAL :",null,"No",{"v":42,"d":"42 "}]
[]
[{"v":348,"d":"348 "},null,"LABOUR :",null,"No",{"v":42,"d":"42 "}]
[]
[null,null,"100x100x50 deep PVC surface onto brick, concrete surface or in roof space"]
[]
[{"v":349,"d":"349 "},null,"MATERIAL :",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":350,"d":"350 "},null,"LABOUR :",null,"No",{"v":6,"d":"6 "}]
[]
[null,null,"50mm diam x 25 surface PVC onto brick, concrete surface or in roof space"]
[]
[{"v":351,"d":"351 "},null,"MATERIAL :",null,"No",{"v":95,"d":"95 "}]
[]
[{"v":352,"d":"352 "},null,"LABOUR :",null,"No",{"v":95,"d":"95 "}]
[]
[null,null,"50mm diam PVC lids"]
[]
[{"v":353,"d":"353 "},null,"MATERIAL :",null,"No",{"v":95,"d":"95 "}]
[]
[{"v":354,"d":"354 "},null,"LABOUR :",null,"No",{"v":95,"d":"95 "}]
[]
[null,null,"100x100x50 deep Bosal surface onto brick, concrete surface or in roof space"]
[]
[{"v":355,"d":"355 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":356,"d":"356 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"50mm diam x 25 surface Bosal onto brick, concrete surface or in roof space"]
[]
[{"v":357,"d":"357 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":358,"d":"358 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"50mm diam Bosal lids"]
[]
[{"v":359,"d":"359 "},null,"MATERIAL :",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":360,"d":"360 "},null,"LABOUR :",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"Powerskirting & Recessed Floor Outlets"]
[]
[null,null,"PVC Powerskiting complete with covers fixing outlets as indicated"]
[]
[null,null,"3 compartment 2 cover powerskirting"]
[]
[{"v":361,"d":"361 "},null,"MATERIAL :",null,"m",{"v":90,"d":"90 "}]
[]
[{"v":362,"d":"362 "},null,"LABOUR :",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"Corner piece"]
[]
[{"v":363,"d":"363 "},null,"MATERIAL :",null,"No",{"v":18,"d":"18 "}]
[]
[{"v":364,"d":"364 "},null,"LABOUR :",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"End Caps"]
[]
[{"v":365,"d":"365 "},null,"MATERIAL :",null,"No",{"v":26,"d":"26 "}]
[]
[{"v":366,"d":"366 "},null,"LABOUR :",null,"No",{"v":26,"d":"26 "}]
[]
[null,null,"Back box for powerskirting"]
[]
[{"v":367,"d":"367 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":368,"d":"368 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"CONDUCTORS"]
[]
[null,null,"PVC insulated copper conductors drawn into conduit or trunking"]
[]
[null,null,"6mm2"]
[]
[{"v":369,"d":"369 "},null,"MATERIAL :",null,"m",{"v":130,"d":"130 "}]
[]
[{"v":370,"d":"370 "},null,"LABOUR :",null,"m",{"v":130,"d":"130 "}]
[]
[null,null,"4mm2"]
[]
[{"v":371,"d":"371 "},null,"MATERIAL :",null,"m",{"v":3141,"d":"3,141 "}]
[]
[{"v":372,"d":"372 "},null,"LABOUR :",null,"m",{"v":3141,"d":"3,141 "}]
[]
[null,null,"PVC insulated copper earth conductors drawn into conduit or trunking"]
[]
[null,null,"4mm2"]
[]
[{"v":373,"d":"373 "},null,"MATERIAL",null,"m",{"v":50,"d":"50 "}]
[]
[{"v":374,"d":"374 "},null,"LABOUR",null,"m",{"v":50,"d":"50 "}]
[]
[null,null,"2,5mm2"]
[]
[{"v":375,"d":"375 "},null,"MATERIAL",null,"m",{"v":1623,"d":"1,623 "}]
[]
[{"v":376,"d":"376 "},null,"LABOUR",null,"m",{"v":1623,"d":"1,623 "}]
[]
[null,null,"Drawwire"]
[]
[{"v":377,"d":"377 "},null,"MATERIAL",null,"m",{"v":770,"d":"770 "}]
[]
[{"v":378,"d":"378 "},null,"LABOUR",null,"m",{"v":770,"d":"770 "}]
[]
[null,null,"FITTINGS AND ACCESSORIES"]
[]
[null,null,"16 Amp 1x SA and 1x Euro SSO for powerskirting"]
[]
[{"v":379,"d":"379 "},null,"MATERIAL :",null,"No",{"v":27,"d":"27 "}]
[]
[{"v":380,"d":"380 "},null,"LABOUR :",null,"No",{"v":27,"d":"27 "}]
[]
[null,null,"16 Amp Double D-pin SSO for powerskirting"]
[]
[{"v":381,"d":"381 "},null,"MATERIAL :",null,"No",{"v":18,"d":"18 "}]
[]
[{"v":382,"d":"382 "},null,"LABOUR :",null,"No",{"v":18,"d":"18 "}]
[]
[null,null,"IT Cover Plate for powerskirting"]
[]
[{"v":383,"d":"383 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":384,"d":"384 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"16A single phase isolator (surface indoor)"]
[]
[{"v":385,"d":"385 "},null,"MATERIAL :",null,"No",{"v":26,"d":"26 "}]
[]
[{"v":386,"d":"386 "},null,"LABOUR :",null,"No",{"v":26,"d":"26 "}]
[]
[null,null,"16A single phase isolator (surface weatherproof)"]
[]
[{"v":387,"d":"387 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":388,"d":"388 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"32A single phase isolator (surface weatherproof)"]
[]
[{"v":389,"d":"389 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":390,"d":"390 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"32A three-phase isolator (surface weatherproof)"]
[]
[{"v":391,"d":"391 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":392,"d":"392 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Outlets in wall / drywall"]
[]
[null,null,"Normal  Euro 16 Amp SSO"]
[]
[{"v":393,"d":"393 "},null,"MATERIAL :",null,"No",{"v":30,"d":"30 "}]
[]
[{"v":394,"d":"394 "},null,"LABOUR :",null,"No",{"v":30,"d":"30 "}]
[]
[null,null,"Double 16 Amp D-pin SSO"]
[]
[{"v":395,"d":"395 "},null,"MATERIAL :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":396,"d":"396 "},null,"LABOUR :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":397,"d":"397 "},null,"MATERIAL :",null,"No",{"v":16,"d":"16 "}]
[]
[{"v":398,"d":"398 "},null,"LABOUR :",null,"No",{"v":16,"d":"16 "}]
[]
[null,null,"HDMI outlet"]
[]
[{"v":399,"d":"399 "},null,"MATERIAL :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":400,"d":"400 "},null,"LABOUR :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Floor box outlet complete with SSO's (recessed 2xSA & 2xEuro with 2xIT/Data outlets)"]
[]
[{"v":401,"d":"401 "},null,"MATERIAL :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":402,"d":"402 "},null,"LABOUR :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Outlets in boxes mounted surface under desks"]
[]
[null,null,"Normal  Euro 16 Amp SSO complete with flyleads"]
[]
[{"v":403,"d":"403 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":404,"d":"404 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"Double 16 Amp D-pin SSO complete with flyleads"]
[]
[{"v":405,"d":"405 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":406,"d":"406 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"IT Cover Plate"]
[]
[{"v":407,"d":"407 "},null,"MATERIAL :",null,"No",{"v":14,"d":"14 "}]
[]
[{"v":408,"d":"408 "},null,"LABOUR :",null,"No",{"v":14,"d":"14 "}]
[]
[null,null,"CABLE TRAYS"]
[]
[null,null,"200mm wide heavy-duty wire mesh cable tray"]
[]
[{"v":409,"d":"409 "},null,"MATERIAL :",null,"m",{"v":50,"d":"50 "}]
[]
[{"v":410,"d":"410 "},null,"LABOUR :",null,"m",{"v":50,"d":"50 "}]
[]
[null,null,"200mm wide wire mesh cable tray 90 deg bend"]
[]
[{"v":411,"d":"411 "},null,"MATERIAL :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":412,"d":"412 "},null,"LABOUR :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"200mm wide wire mesh cable tray T-piece"]
[]
[{"v":413,"d":"413 "},null,"MATERIAL :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":414,"d":"414 "},null,"LABOUR :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"100mm wire mesh cable tray fixed under desks"]
[]
[{"v":415,"d":"415 "},null,"MATERIAL :",null,"m",{"v":40,"d":"40 "}]
[]
[{"v":416,"d":"416 "},null,"LABOUR :",null,"m",{"v":40,"d":"40 "}]
[]
[null,null,"P9000 Trunking in ceiling space"]
[]
[{"v":417,"d":"417 "},null,"MATERIAL :",null,"m",{"v":40,"d":"40 "}]
[]
[{"v":418,"d":"418 "},null,"LABOUR :",null,"m",{"v":40,"d":"40 "}]
[]
[null,null,"BILL NO.11"]
[]
[null,null,"REMOVE AND MAKE SAFE"]
[]
[{"v":419,"d":"419 "},null,"Survey and mark up drawing of existing electrical installation in ceiling spaces",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":420,"d":"420 "},null,"Remove and make safe all electrical installations as specified.",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":421,"d":"421 "},null,"Existing IT installation cameras, time and attendance, Wifi, etc. to be protected and remain unchanged",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.11"]
[]
[null,null,"REMOVE AND MAKE SAFE"]
[]
[{"v":422,"d":"422 "},null,"Provisional Additional earthing should it be required to get the correct earth reading at the MDB.",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":423,"d":"423 "},null,"Provisional sum for additional requirements by the IT department for wireways.",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":424,"d":"424 "},null,"Provisional Sum for Contingency",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":425,"d":"425 "},null,"Testing of existing Generator and Solar PV installations",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":426,"d":"426 "},null,"Reuse existing cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":427,"d":"427 "},null,"Reuse existing cable trunking",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"BILL NO.13"]
[]
[null,null,"PROVISIONAL DAYWORKS"]
[]
[null,null,"(Provisional : as allowance only) (Exclusive of VAT) Provisional dayworks allowed for : Making safe of and work on and alterations to the existing installations not already included in the specification Work sall only be carried out on Dayworks where specifically agreed to or instructed by the Employer/ Architect/Engineer in advance. Generally the cost of additions and omissions shall be based on the scheduled rates in Part 5"]
[]
[null,null,"Labour The rates for labour in Dayworks are to be applied to the hours worked and they are to include for the cost of labour, supervision, overheads, transport, profit, all lefies, bonuses, leave pay, etc. not already covered by the P&G in the contract sum."]
[]
[{"v":428,"d":"428 "},null,"Electrician",null,"Hrs",{"v":20,"d":"20 "}]
[]
[{"v":429,"d":"429 "},null,"Operator (semi-skilled)",null,"Hrs",{"v":20,"d":"20 "}]
[]
[{"v":430,"d":"430 "},null,"Labourer",null,"Hrs",{"v":20,"d":"20 "}]
[]
[null,null,"Time sheets specifying the workers involved, the time spent daily upon the work and the materials imployed in Dayworks shall be deliveded to the Employer/Architect/Engineer or his representative weekly"]
[]
[null,null,"Materials the cost of materials in Dayworks ahall be based on the net cost and shall be substantiated with invoices and, where no rates exist in the Schedules for such material, shall be based on the net cost and shall be substantiated with invoices"]
[]
[{"v":431,"d":"431 "},null,"Provisional Sum for materials in Dayworks.",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":432,"d":"432 "},null,"Add for supervision, insurances, profit, transport, establishment changes, etc. not already covered by the P&G in the contract sum.",null,"%"]
[]
[null,null,"Plant, etc. The cost of mechanically operated plant and transport, etc. in Dayworks are to be based on the net costs and shall be substantiated with invoices and/or audited statements."]
[]
[{"v":433,"d":"433 "},null,"Provisional sum for hire of mechanical plant, etc. in Dayworks.",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":434,"d":"434 "},null,"Add for supervision, insurances, profit, transport, establishment changes, etc. not already covered by the P&G.",null,"%"]
[]
[{"v":1,"d":"1 "},null,"PRELIMINARIES",null,"Page",{"v":115,"d":"115 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"LV ELECTRICITY SUPPLY",null,"Page",{"v":118,"d":"118 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"BASEMENT LIGHTING",null,"Page",{"v":122,"d":"122 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"BASEMENT POWER",null,"Page",{"v":126,"d":"126 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"GROUND FLOOR LIGHTING",null,"Page",{"v":131,"d":"131 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"GROUND FLOOR POWER",null,"Page",{"v":140,"d":"140 "},{"v":0,"d":"0.00"}]
[]
[{"v":7,"d":"7 "},null,"FIRST FLOOR LIGHTING",null,"Page",{"v":144,"d":"144 "},{"v":0,"d":"0.00"}]
[]
[{"v":8,"d":"8 "},null,"FIRST FLOOR POWER",null,"Page",{"v":153,"d":"153 "},{"v":0,"d":"0.00"}]
[]
[{"v":9,"d":"9 "},null,"SECOND FLOOR LIGHTING",null,"Page",{"v":157,"d":"157 "},{"v":0,"d":"0.00"}]
[]
[{"v":10,"d":"10 "},null,"SECOND FLOOR POWER",null,"Page",{"v":166,"d":"166 "},{"v":0,"d":"0.00"}]
[]
[{"v":11,"d":"11 "},null,"REMOVE & MAKE SAFE",null,"Page",{"v":167,"d":"167 "},{"v":0,"d":"0.00"}]
[]
[{"v":12,"d":"12 "},null,"GENERAL",null,"Page",{"v":168,"d":"168 "},{"v":0,"d":"0.00"}]
[]
[{"v":13,"d":"13 "},null,"PROVISIONAL DAYWORKS",null,"Page",{"v":171,"d":"171 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SECTION 4 FIRE DETECTION INSTALLATION"]
[]
[null,null,"BILL\" NO.1"]
[]
[null,null,"PRELIMINARY\" &\" GENERAL"]
[]
[{"v":1,"d":"1 "},null,"Allow for preliminary and general costs: (Site establishment and overheads)",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":2,"d":"2 "},null,"Safety plan and measures",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"OTHER : To be specified by the Tenderer"]
[]
[{"v":3,"d":"3 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":0,"d":"0 "}]
[]
[{"v":4,"d":"4 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":0,"d":"0 "}]
[]
[{"v":5,"d":"5 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":0,"d":"0 "}]
[]
[{"v":6,"d":"6 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":0,"d":"0 "}]
[]
[null,null,"BILL\" NO.2\" "]
[]
[null,null,"FIRE\" DETECTION\" INSTALLATION"]
[]
[null,null,"BASEMENT"]
[]
[null,null,"CONDUITS"]
[]
[null,null,"Conduits\" PVC\" surface\" /\" in\" ceiling\" space\" on galvanized\" steel\" spacer\" bar\" saddles"]
[]
[null,null,"25mm×˜ PVC"]
[]
[{"v":7,"d":"7 "},null,"MATERIAL",null,"m",{"v":75,"d":"75 "}]
[]
[{"v":8,"d":"8 "},null,"LABOUR",null,"m",{"v":75,"d":"75 "}]
[]
[null,null,"FITTINGS\" AND\" ACCESSORIES"]
[]
[null,null,"Smoke detectors with sounder & strobe"]
[]
[{"v":9,"d":"9 "},null,"MATERIAL",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":10,"d":"10 "},null,"LABOUR",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"Relay in 100x100 box with lid"]
[]
[{"v":11,"d":"11 "},null,"MATERIAL",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":12,"d":"12 "},null,"LABOUR",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Relay units with enclosure for access control doors"]
[]
[{"v":13,"d":"13 "},null,"MATERIAL",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":14,"d":"14 "},null,"LABOUR",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Line Isolators"]
[]
[{"v":15,"d":"15 "},null,"MATERIAL",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":16,"d":"16 "},null,"LABOUR",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Breakglass Units (Manual Call Point)"]
[]
[{"v":17,"d":"17 "},null,"MATERIAL",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":18,"d":"18 "},null,"LABOUR",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Breakglass Units (Door Release)"]
[]
[{"v":19,"d":"19 "},null,"MATERIAL",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":20,"d":"20 "},null,"LABOUR",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Sounder / Strobe"]
[]
[{"v":21,"d":"21 "},null,"MATERIAL",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":22,"d":"22 "},null,"LABOUR",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":23,"d":"23 "},null,"Labelling of system devices",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"GENERAL\" FOR\" FIRE\" DETECTION"]
[]
[{"v":24,"d":"24 "},null,"PH30 Fire Cable layed wire mesh tray or in steel conduit",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL\" NO.3"]
[]
[null,null,"FIRE\" DETECTION\" INSTALLATION"]
[]
[null,null,"GROUND\" FLOOR CONDUITS"]
[]
[null,null,"Conduits\" PVC\" surface\" /\" in\" ceiling\" space\" on galvanized\" steel\" spacer\" bar\" saddles"]
[]
[null,null,"25mm×˜ PVC"]
[]
[{"v":25,"d":"25 "},null," MATERIAL   :",null,"m",{"v":90,"d":"90 "}]
[]
[{"v":26,"d":"26 "},null,"LABOUR      :",null,"m",{"v":90,"d":"90 "}]
[]
[null,null,"FITTINGS\" AND\" ACCESSORIES"]
[]
[null,null,"Smoke detectors with sounder & strobe"]
[]
[{"v":27,"d":"27 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":28,"d":"28 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Relay in 100x100 box with lid"]
[]
[{"v":29,"d":"29 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":30,"d":"30 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Relay units with enclosure for access control doors"]
[]
[{"v":31,"d":"31 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":32,"d":"32 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Line Isolators"]
[]
[{"v":33,"d":"33 "},null,"MATERIAL   :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":34,"d":"34 "},null,"LABOUR      :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Breakglass Units (Manual Call Point)"]
[]
[{"v":35,"d":"35 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":36,"d":"36 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Breakglass Units (Door Release)"]
[]
[{"v":37,"d":"37 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":38,"d":"38 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Sounder / Strobe"]
[]
[{"v":39,"d":"39 "},null,"MATERIAL   :",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":40,"d":"40 "},null,"LABOUR      :",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":41,"d":"41 "},null,"Labelling of system devices",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"GENERAL\" FOR\" FIRE\" DETECTION"]
[]
[{"v":42,"d":"42 "},null,"PH30 Fire Cable layed wire mesh tray or in steel conduit",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"Fire Panel"]
[]
[{"v":43,"d":"43 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":44,"d":"44 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL\" NO.4"]
[]
[null,null,"FIRE\" DETECTION\" INSTALLATION"]
[]
[null,null,"FIRST\" FLOOR CONDUITS"]
[]
[null,null,"Conduits\" PVC\" surface\" /\" in\" ceiling\" space\" on galvanized\" steel\" spacer\" bar\" saddles"]
[]
[null,null,"25mm×˜ PVC"]
[]
[{"v":45,"d":"45 "},null,"MATERIAL   :",null,"m",{"v":75,"d":"75 "}]
[]
[{"v":46,"d":"46 "},null,"LABOUR      :",null,"m",{"v":75,"d":"75 "}]
[]
[null,null,"FITTINGS\" AND\" ACCESSORIES"]
[]
[null,null,"Smoke detectors with sounder & strobe"]
[]
[{"v":47,"d":"47 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":48,"d":"48 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Relay in 100x100 box with lid"]
[]
[{"v":49,"d":"49 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":50,"d":"50 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Relay units with enclosure for access control doors"]
[]
[{"v":51,"d":"51 "},null,"MATERIAL   :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":52,"d":"52 "},null,"LABOUR      :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"Line Isolators"]
[]
[{"v":53,"d":"53 "},null,"MATERIAL   :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":54,"d":"54 "},null,"LABOUR      :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Breakglass Units (Manual Call Point)"]
[]
[{"v":55,"d":"55 "},null,"MATERIAL   :",null,"No",{"v":0,"d":"0 "}]
[]
[{"v":56,"d":"56 "},null,"LABOUR      :",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"Breakglass Units (Door Release)"]
[]
[{"v":57,"d":"57 "},null,"MATERIAL   :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":58,"d":"58 "},null,"LABOUR      :",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"Sounder / Strobe"]
[]
[{"v":59,"d":"59 "},null,"MATERIAL   :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":60,"d":"60 "},null,"LABOUR      :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":61,"d":"61 "},null,"Labelling of system devices",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"GENERAL FOR FIRE DETECTION"]
[]
[{"v":62,"d":"62 "},null,"PH30 Fire cable laid wire mesh tray and in steel conduit",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL\" NO.5"]
[]
[null,null,"FIRE\" DETECTION\" INSTALLATION"]
[]
[null,null,"SECOND\" FLOOR CONDUITS"]
[]
[null,null,"Conduits\" PVC\" surface\" /\" in\" ceiling\" space\" on galvanized\" steel\" spacer\" bar\" saddles"]
[]
[null,null,"25mm×˜ PVC"]
[]
[{"v":63,"d":"63 "},null,"MATERIAL   :",null,"m",{"v":75,"d":"75 "}]
[]
[{"v":64,"d":"64 "},null,"LABOUR      :",null,"m",{"v":75,"d":"75 "}]
[]
[null,null,"FITTINGS\" AND\" ACCESSORIES"]
[]
[null,null,"Smoke detectors with sounder & strobe"]
[]
[{"v":65,"d":"65 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":66,"d":"66 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Relay in 100x100 box with lid"]
[]
[{"v":67,"d":"67 "},null,"MATERIAL   :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":68,"d":"68 "},null,"LABOUR      :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Relay units with enclosure for access control doors"]
[]
[{"v":69,"d":"69 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":70,"d":"70 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Line Isolators"]
[]
[{"v":71,"d":"71 "},null,"MATERIAL   :",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":72,"d":"72 "},null,"LABOUR      :",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"Breakglass Units (Manual Call Point)"]
[]
[{"v":73,"d":"73 "},null,"MATERIAL   :",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":74,"d":"74 "},null,"LABOUR      :",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"Breakglass Units (Door Release)"]
[]
[{"v":75,"d":"75 "},null,"MATERIAL   :",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":76,"d":"76 "},null,"LABOUR      :",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"Sounder / Strobe"]
[]
[{"v":77,"d":"77 "},null,"MATERIAL   :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":78,"d":"78 "},null,"LABOUR      :",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":79,"d":"79 "},null,"Labelling of system devices",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"GENERAL FOR FIRE DETECTION"]
[]
[{"v":80,"d":"80 "},null,"PH30 Fire cable laid wire mesh tray and in steel conduit",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL\" NO.6"]
[]
[null,null,"GENERAL"]
[]
[{"v":81,"d":"81 "},null,"Provisional sum for additional Fire Detection requirements",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":82,"d":"82 "},null,"Training",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":83,"d":"83 "},null,"Test & Commision installations",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":84,"d":"84 "},null,"Guarantee & maintenance for 1 year",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":85,"d":"85 "},null,"Attendance and liaison with the Main Contractor",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":86,"d":"86 "},null,"Attendance and liaison with the Electrical Subcontractor",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":87,"d":"87 "},null,"As builts / record drawings / manuals",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":88,"d":"88 "},null,"Hand over",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":1,"d":"1 "},null,"PRELIMINARY & GENERAL",null,"Page",{"v":173,"d":"173 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"FIRE DETECTION BASEMENT",null,"Page",{"v":176,"d":"176 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"FIRE DETECTION GROUND FLOOR",null,"Page",{"v":179,"d":"179 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"FIRE DETECTION FIRST FLOOR",null,"Page",{"v":182,"d":"182 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"FIRE DETECTION SECOND FLOOR",null,"Page",{"v":185,"d":"185 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"GENERAL",null,"Page",{"v":186,"d":"186 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SECTION 5 FIRE PROTECTION SERVICES"]
[]
[null,null,"BILL NO.1"]
[]
[null,null,"PRELIMINARY & GENERAL"]
[]
[{"v":1,"d":"1 "},null,"Allow for preliminaries and general costs: (Site establishment and overheads)",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":2,"d":"2 "},null,"Safety plan and measures",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"OTHER : To be specified by the Tenderer"]
[]
[{"v":3,"d":"3 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":4,"d":"4 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":5,"d":"5 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":6,"d":"6 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.2"]
[]
[null,null,"Equipment (Drawing CM-0769-Y40)"]
[]
[null,null,"Including supply, installation, consumables, hangers, painting, electrical controls, wiring, etc and all associated costs for completion of works as per specification:"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for supply, delivery, fittings, connections, bends, joints,  junctions and hanging materials, etc to be included."]
[]
[null,null,"WATER CONNECTION"]
[]
[{"v":7,"d":"7 "},null,"×¸100mm Water connection (below ground)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":8,"d":"8 "},null,"×¸100mm Non-return Valve (below ground)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":9,"d":"9 "},null,"Remove existing steel piping",null,"No",{"v":25,"d":"25 "}]
[]
[null,null,"FIRE RETICULATION"]
[]
[{"v":10,"d":"10 "},null,"×˜100mm uPVC (incl. all fittings, albows & Tees)",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":11,"d":"11 "},null,"×˜100mm steel (incl. all fittings, albows & Tees)",null,"m",{"v":25,"d":"25 "}]
[]
[null,null,"PHOTOLUMINESCENT (190 x 190)"]
[]
[{"v":12,"d":"12 "},null,"Exit signage",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.3"]
[]
[null,null,"Equipment (Drawing CM-0769-Y10)"]
[]
[null,null,"Including supply, installation, consumables, hangers,painting, electrical controls, wiring, etc and all associated costs for completion of works as per specification:"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for supply, delivery, fittings, connections, bends, joints,  junctions and hanging materials, etc to be included."]
[]
[null,null,"FIRE HYDRANT"]
[]
[{"v":13,"d":"13 "},null,"Fire Hydrant including landing valve, brass 100mm, incl cap and chain",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":14,"d":"14 "},null,"Pressure gauge, 100mm diameter glycerine filled 1000kPA, incl. stopcock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"FIRE PIPING"]
[]
[{"v":15,"d":"15 "},null,"×¸100mm Steel Pipe (incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"PHOTOLUMINESCENT (190 X 190)"]
[]
[{"v":16,"d":"16 "},null,"Running man",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":17,"d":"17 "},null,"Arrow",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":18,"d":"18 "},null,"Fire Extinguisher Signage",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":19,"d":"19 "},null,"Fire Hydrant Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":20,"d":"20 "},null,"Relocate signage",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"BILL NO.4"]
[]
[null,null,"Equipment (Drawing CM-0769-Y20)"]
[]
[null,null,"Including supply, installation, consumables, hangers, painting, electrical controls, wiring, etc and all associated costs for completion of works as per specification:"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for supply, delivery, fittings, connections, bends, joints,  junctions and hanging materials, etc to be included."]
[]
[null,null,"FIRE HYDRANT"]
[]
[{"v":21,"d":"21 "},null,"Fire Hydrant including landing valve, brass 100mm, incl cap and chain",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":22,"d":"22 "},null,"Pressure gauge, 100mm diameter glycerine filled 1000kPA, incl. stopcock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"FIRE PIPING"]
[]
[{"v":23,"d":"23 "},null,"×¸100mm Steel Pipe (incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"PORTABLE FIRE EXTINGUISHER"]
[]
[null,null,"All extinguisher as per SABS approved standards. Extinguishes to be provided each with 25mm thick meranti backing board min. size 150 x 700mm, plugged and screwed to brickwork and all exposed edges bevelled, incl. 1 x coat primer and 2 x coats Signal Red enamel paint. Mounting brackets to be approved in accordance with SABS 810."]
[]
[{"v":24,"d":"24 "},null,"Extinguisher 4,5kg DCP",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"PHOTOLUMINESCENT (190 X 190)"]
[]
[{"v":25,"d":"25 "},null,"Running man",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":26,"d":"26 "},null,"Arrow",null,"No",{"v":9,"d":"9 "}]
[]
[{"v":27,"d":"27 "},null,"Fire Extinguisher Signage",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":28,"d":"28 "},null,"Fire Hose reel  Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":29,"d":"29 "},null,"Fire Hydrant  Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":30,"d":"30 "},null,"Relocate signage",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"BILL NO.5"]
[]
[null,null,"Equipment (Drawing CM-0769-Y30)"]
[]
[null,null,"Including supply, installation, consumables, hangers, painting, electrical controls, wiring, etc and all associated costs for completion of works as per specification:"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for supply, delivery, fittings, connections, bends, joints,  junctions and hanging materials, etc to be included."]
[]
[null,null,"FIRE HYDRANT"]
[]
[{"v":31,"d":"31 "},null,"Fire Hydrant including landing valve, brass 100mm, incl cap and chain",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":32,"d":"32 "},null,"Pressure gauge, 100mm diameter glycerine filled 1000kPA, incl. stopcock",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"FIRE PIPING"]
[]
[{"v":33,"d":"33 "},null,"×¸100mm Steel Pipe (incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"PHOTOLUMINESCENT (190 x 190)"]
[]
[{"v":34,"d":"34 "},null,"Running man",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":35,"d":"35 "},null,"Arrow",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":36,"d":"36 "},null,"Fire Extinguisher Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":37,"d":"37 "},null,"Fire Hose reel  Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":38,"d":"38 "},null,"Fire Hydrant  Signage",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":39,"d":"39 "},null,"Relocate signage",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO.6"]
[]
[null,null,"GENERAL"]
[]
[{"v":40,"d":"40 "},null,"Test & commission the installation as per SABS",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":41,"d":"41 "},null,"Painting, labeling and identification as per SABS",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":42,"d":"42 "},null,"Fire stopping",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":43,"d":"43 "},null,"Workshop Drawings",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":44,"d":"44 "},null,"Samples",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":45,"d":"45 "},null,"Liason with local Authority",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":46,"d":"46 "},null,"Painting of pipework",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":47,"d":"47 "},null,"Works test with Engineer",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":48,"d":"48 "},null,"Attendance of final inspection with Fire Chief",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":49,"d":"49 "},null,"Manuals & Instructions",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":50,"d":"50 "},null,"Operator Training",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":51,"d":"51 "},null,"Maintenance Contract and Guarantee",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":1,"d":"1 "},null,"PRELIMINARIES",null,"Page",{"v":188,"d":"188 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"BASEMENT",null,"Page",{"v":189,"d":"189 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"GROUND FLOOR",null,"Page",{"v":190,"d":"190 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"FIRST FLOOR",null,"Page",{"v":193,"d":"193 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"SECOND FLOOR",null,"Page",{"v":194,"d":"194 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"GENERAL",null,"Page",{"v":195,"d":"195 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SECTION 6 VENTILATION AND AIR CONDITIONING INSTALLATION"]
[]
[null,null,"BILL NO.1"]
[]
[null,null,"PRELIMINARY & GENERAL"]
[]
[{"v":1,"d":"1 "},null,"Allow for preliminaries and general costs: (Site establishment and overheads)",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":2,"d":"2 "},null,"Safety plan and measures",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"OTHER : To be specified by the Tenderer"]
[]
[{"v":3,"d":"3 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":4,"d":"4 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":5,"d":"5 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":6,"d":"6 "},null,"...........................................................................\"€¦..",null,"SUM",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.2"]
[]
[null,null,"FAF B.1 (See Drawing CM0769-Y4)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN B.1"]
[]
[{"v":7,"d":"7 "},null,"AMS TD500/150 SILENT SERIES c/w ON/OFF switch rate of 100L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":8,"d":"8 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":9,"d":"9 "},null,"250x200 Washable slide out filter  sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":10,"d":"10 "},null,"×¸200",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":11,"d":"11 "},null,"×¸100",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"TRANSFORMATIONS"]
[]
[{"v":12,"d":"12 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":13,"d":"13 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":14,"d":"14 "},null,"×¸200 - ×¸100",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":15,"d":"15 "},null,"×¸150 90\"° BEND",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":16,"d":"16 "},null,"100x100 GRILLE  OBD",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":17,"d":"17 "},null,"×˜100 Flex ducting",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":18,"d":"18 "},null,"×¸200 Flex ducting",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":19,"d":"19 "},null,"×¸100 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":20,"d":"20 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":21,"d":"21 "},null,"×¸200 balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":22,"d":"22 "},null,"Removal of existing Fan and ducting as per drawing (CM0769Y4)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.3"]
[]
[null,null,"FAF G.1 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN G.1"]
[]
[{"v":23,"d":"23 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 190L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":24,"d":"24 "},null,"Weather louvre, natural anodised 300x300, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":25,"d":"25 "},null,"300x300 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":26,"d":"26 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":27,"d":"27 "},null,"×¸250",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":28,"d":"28 "},null,"×¸200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":29,"d":"29 "},null,"×¸150",null,"m",{"v":6,"d":"6 "}]
[]
[{"v":30,"d":"30 "},null,"×¸125",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":31,"d":"31 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":32,"d":"32 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":33,"d":"33 "},null,"×¸250 - ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":34,"d":"34 "},null,"×¸200 - ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":35,"d":"35 "},null,"×¸250 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":36,"d":"36 "},null,"×¸200 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":37,"d":"37 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":38,"d":"38 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":39,"d":"39 "},null,"×¸125 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":40,"d":"40 "},null,"×¸200 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":41,"d":"41 "},null,"×¸150 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":42,"d":"42 "},null,"×¸125 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":43,"d":"43 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":44,"d":"44 "},null,"Trox Z_LVS ×¸200 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":45,"d":"45 "},null,"Trox Z_LVS ×¸125 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.4"]
[]
[null,null,"FAF G.2 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN G.2"]
[]
[{"v":46,"d":"46 "},null,"TD 1000/200 SILENT SERIES c/w ON/OFF switchrate of 230L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":47,"d":"47 "},null,"Weather louvre, natural anodised 350x300, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":48,"d":"48 "},null,"350x300 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":49,"d":"49 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":50,"d":"50 "},null,"AMS Sound Attenuator SN020-090 900mm Long",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":51,"d":"51 "},null,"×¸250",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":52,"d":"52 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":53,"d":"53 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":54,"d":"54 "},null,"duct to grille transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":55,"d":"55 "},null,"×¸250 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":56,"d":"56 "},null,"×¸250 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":57,"d":"57 "},null,"250x200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":58,"d":"58 "},null,"250x200 Grille  OBD",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO.5"]
[]
[null,null,"FAF G.3 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN G.3"]
[]
[{"v":59,"d":"59 "},null,"TD 500/150 SILENT SERIES c/w ON/OFF switch rate of 100L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":60,"d":"60 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":61,"d":"61 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":62,"d":"62 "},null,"AMS Sound Attenuator SN015-030 300mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":63,"d":"63 "},null,"×¸200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":64,"d":"64 "},null,"×¸150",null,"m",{"v":8,"d":"8 "}]
[]
[{"v":65,"d":"65 "},null,"×¸125",null,"m",{"v":4,"d":"4 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":66,"d":"66 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":67,"d":"67 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":68,"d":"68 "},null,"×¸200 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":69,"d":"69 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":70,"d":"70 "},null,"×¸125 45\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":71,"d":"71 "},null,"×˜150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":72,"d":"72 "},null,"×˜150 Balancing damper",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":73,"d":"73 "},null,"Trox Z_LVS ×¸150 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":74,"d":"74 "},null,"Trox Z_LVS ×¸125 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO.6"]
[]
[null,null,"FAF G.4 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN G.4"]
[]
[{"v":75,"d":"75 "},null,"TD 1000/200 SILENT SERIES c/w ON/OFF switch rate of 190L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":76,"d":"76 "},null,"Weather louvre, natural anodised 350x300, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":77,"d":"77 "},null,"350x300 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":78,"d":"78 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":79,"d":"79 "},null,"AMS Sound Attenuator SN020-090 900mm Long",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":80,"d":"80 "},null,"×¸250",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":81,"d":"81 "},null,"×¸200",null,"m",{"v":6,"d":"6 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":82,"d":"82 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":83,"d":"83 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":84,"d":"84 "},null,"×¸250 - ×¸200",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":85,"d":"85 "},null,"×¸250 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":86,"d":"86 "},null,"×¸200 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":87,"d":"87 "},null,"200x150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":88,"d":"88 "},null,"200x150 Grille  OBD",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":89,"d":"89 "},null,"×¸250 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.7"]
[]
[null,null,"FAF G.4 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN G.5"]
[]
[{"v":90,"d":"90 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 140L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":91,"d":"91 "},null,"Weather louvre, natural anodised 300x250, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":92,"d":"92 "},null,"300x250 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":93,"d":"93 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":94,"d":"94 "},null,"×¸200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":95,"d":"95 "},null,"×¸150",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":96,"d":"96 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":97,"d":"97 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":98,"d":"98 "},null,"Duct to grille transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":99,"d":"99 "},null,"×¸200 - ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":100,"d":"100 "},null,"×¸200 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":101,"d":"101 "},null,"×¸150 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":102,"d":"102 "},null,"×¸200 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":103,"d":"103 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":104,"d":"104 "},null,"×˜150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":105,"d":"105 "},null,"200x200 Grille  OBD",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":106,"d":"106 "},null,"×¸250 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":107,"d":"107 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"REMOVAL"]
[]
[{"v":108,"d":"108 "},null,"Ceiling fan",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"BILL NO.8"]
[]
[null,null,"FAF 1,1 (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 1,1"]
[]
[{"v":109,"d":"109 "},null,"TD 500/150 SILENT SERIES c/w ON/OFF switch rate of 100L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":110,"d":"110 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":111,"d":"111 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":112,"d":"112 "},null,"AMS Sound Attenuator SN015-030 300mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":113,"d":"113 "},null,"×¸200",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":114,"d":"114 "},null,"Filter to fan tranformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":115,"d":"115 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":116,"d":"116 "},null,"×¸200 90\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":117,"d":"117 "},null,"×¸200 45\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":118,"d":"118 "},null,"Rickard CCD 200  flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.9"]
[]
[null,null,"FAF 1,2 (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 1,2"]
[]
[{"v":119,"d":"119 "},null,"TD 500/150 SILENT SERIES c/w ON/OFF switch rate of 100L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":120,"d":"120 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":121,"d":"121 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":122,"d":"122 "},null,"AMS Sound Attenuator SN015-030 300mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":123,"d":"123 "},null,"×¸200",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":124,"d":"124 "},null,"×¸150",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":125,"d":"125 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":126,"d":"126 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":127,"d":"127 "},null,"×¸200 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":128,"d":"128 "},null,"×¸150 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":129,"d":"129 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":130,"d":"130 "},null,"×¸150 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":131,"d":"131 "},null,"×¸150 Balancing damper",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":132,"d":"132 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"BILL NO.10"]
[]
[null,null,"FAF 1,3 (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 1,3"]
[]
[{"v":133,"d":"133 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 140L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":134,"d":"134 "},null,"Weather louvre, natural anodised 300x250, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":135,"d":"135 "},null,"300x250 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":136,"d":"136 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":137,"d":"137 "},null,"×¸250",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":138,"d":"138 "},null,"×¸150",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":139,"d":"139 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":140,"d":"140 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":141,"d":"141 "},null,"×¸250 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":142,"d":"142 "},null,"×¸150 90\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":143,"d":"143 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":144,"d":"144 "},null,"×¸150 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":145,"d":"145 "},null,"×¸150 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":146,"d":"146 "},null,"×¸150 Balancing damper",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":147,"d":"147 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"BILL NO.11"]
[]
[null,null,"FAF 1,4 (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 1,4"]
[]
[{"v":148,"d":"148 "},null,"TD 1000/200 SILENT SERIES c/w ON/OFF switch rate of 190L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":149,"d":"149 "},null,"Weather louvre, natural anodised 350x300, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":150,"d":"150 "},null,"350x300 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":151,"d":"151 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":152,"d":"152 "},null,"AMS Sound Attenuator SN020-090 900mm Long",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":153,"d":"153 "},null,"×¸250",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":154,"d":"154 "},null,"×¸200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":155,"d":"155 "},null,"×¸150",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":156,"d":"156 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":157,"d":"157 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":158,"d":"158 "},null,"×¸250 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":159,"d":"159 "},null,"×¸200 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":160,"d":"160 "},null,"×¸150 45\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":161,"d":"161 "},null,"×¸250 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":162,"d":"162 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":163,"d":"163 "},null,"×¸150 Spigot",null,"No",{"v":6,"d":"6 "}]
[]
[{"v":164,"d":"164 "},null,"×¸250 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":165,"d":"165 "},null,"×¸150 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":166,"d":"166 "},null,"×¸150 Balancing damper",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":167,"d":"167 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":7,"d":"7 "}]
[]
[null,null,"BILL NO.12"]
[]
[null,null,"FAF 1,5 (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 1,5"]
[]
[{"v":168,"d":"168 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 140L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":169,"d":"169 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":170,"d":"170 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":171,"d":"171 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":172,"d":"172 "},null,"×¸200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":173,"d":"173 "},null,"×¸150",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":174,"d":"174 "},null,"×¸125",null,"m",{"v":3,"d":"3 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":175,"d":"175 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":176,"d":"176 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":177,"d":"177 "},null,"×¸200 -  ×¸150",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":178,"d":"178 "},null,"×¸150 90\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":179,"d":"179 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":180,"d":"180 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":181,"d":"181 "},null,"×¸150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":182,"d":"182 "},null,"×¸125 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":183,"d":"183 "},null,"×¸150 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":184,"d":"184 "},null,"×¸150 Balancing damper",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":185,"d":"185 "},null,"×¸125 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":186,"d":"186 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":187,"d":"187 "},null,"Trox Z_LVS ×¸125 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO.13"]
[]
[null,null,"FAF 2,1 (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 2,1"]
[]
[{"v":188,"d":"188 "},null,"TD 500/150 SILENT SERIES c/w ON/OFF switch rate of 100L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":189,"d":"189 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":190,"d":"190 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":191,"d":"191 "},null,"AMS Sound Attenuator SN015-030 300mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":192,"d":"192 "},null,"×¸200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":193,"d":"193 "},null,"×¸150",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":194,"d":"194 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":195,"d":"195 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":196,"d":"196 "},null,"×¸200 -  ×¸150",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":197,"d":"197 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":198,"d":"198 "},null,"×¸150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":199,"d":"199 "},null,"×¸150 Balancing damper",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":200,"d":"200 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":201,"d":"201 "},null,"Removal of Existing ceiling fans",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"BILL NO.14"]
[]
[null,null,"FAF 2,2 (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 2,2"]
[]
[{"v":202,"d":"202 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 140L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":203,"d":"203 "},null,"Weather louvre, natural anodised 300x250, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":204,"d":"204 "},null,"300x250 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":205,"d":"205 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":206,"d":"206 "},null,"×¸200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":207,"d":"207 "},null,"×¸150",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":208,"d":"208 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":209,"d":"209 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":210,"d":"210 "},null,"×¸200 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":211,"d":"211 "},null,"×¸150 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":212,"d":"212 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":213,"d":"213 "},null,"×¸150 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":214,"d":"214 "},null,"Rickard CCD 150  flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"BILL NO.15"]
[]
[null,null,"FAF 2,3 (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 2,3"]
[]
[{"v":215,"d":"215 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 130L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":216,"d":"216 "},null,"Weather louvre, natural anodised 300x250, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":217,"d":"217 "},null,"300x250 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":218,"d":"218 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":219,"d":"219 "},null,"×¸200",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":220,"d":"220 "},null,"×¸150",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":221,"d":"221 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":222,"d":"222 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":223,"d":"223 "},null,"×¸200 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":224,"d":"224 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":225,"d":"225 "},null,"×¸150 Spigot",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":226,"d":"226 "},null,"×¸200 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":227,"d":"227 "},null,"Trox Z_LVS ×¸200 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":228,"d":"228 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.16"]
[]
[null,null,"FAF 2,4 (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 2,4"]
[]
[{"v":229,"d":"229 "},null,"TD 800/200 SILENT SERIES c/w ON/OFF switch rate of 130L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":230,"d":"230 "},null,"Weather louvre, natural anodised 300x250, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":231,"d":"231 "},null,"300x250 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":232,"d":"232 "},null,"AMS Sound Attenuator SN020-060 600mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":233,"d":"233 "},null,"×¸200",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":234,"d":"234 "},null,"×¸150",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":235,"d":"235 "},null,"×¸100",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":236,"d":"236 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":237,"d":"237 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":238,"d":"238 "},null,"×¸200 -  ×¸150",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":239,"d":"239 "},null,"×¸200 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":240,"d":"240 "},null,"×¸150 45\"° Bend",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":241,"d":"241 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":242,"d":"242 "},null,"×¸150 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":243,"d":"243 "},null,"×¸100 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":244,"d":"244 "},null,"×¸150 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":245,"d":"245 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":246,"d":"246 "},null,"Trox Z_LVS ×¸100 disc valve   flex (or Equivalent)",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"BILL NO.17"]
[]
[null,null,"FAF 2,5 (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"FRESH AIR FAN 2,4"]
[]
[{"v":247,"d":"247 "},null,"TD 500/150 SILENT SERIES c/w ON/OFF switch rate of 110L/s @ 150 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":248,"d":"248 "},null,"Weather louvre, natural anodised 250x200, including frame",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":249,"d":"249 "},null,"250x200 Washable slide out filter  wall sleeve",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":250,"d":"250 "},null,"AMS Sound Attenuator SN015-030 300mm Long",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING"]
[]
[{"v":251,"d":"251 "},null,"×¸200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":252,"d":"252 "},null,"×¸150",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":253,"d":"253 "},null,"Filter to fan transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":254,"d":"254 "},null,"Fan to duct transformation",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":255,"d":"255 "},null,"×¸200 -  ×¸150",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":256,"d":"256 "},null,"×¸150 90\"° Bend",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":257,"d":"257 "},null,"×¸200 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":258,"d":"258 "},null,"×¸150 Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":259,"d":"259 "},null,"×¸100 Spigot",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":260,"d":"260 "},null,"×¸150 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":261,"d":"261 "},null,"×¸100 Balancing damper",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":262,"d":"262 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":263,"d":"263 "},null,"Trox Z_LVS ×¸100 disc valve   flex (or Equivalent)",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"REMOVAL"]
[]
[{"v":264,"d":"264 "},null,"Ceiling fan",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"BILL NO.18"]
[]
[null,null,"EAF1 (See Drawing CM0769-M200)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"EXTRACT AIR FAN 1"]
[]
[{"v":265,"d":"265 "},null,"AMS RDE03152AA5/,4 RDE SERIES  c/w ON/OFF switch rate of 750L/s @ 200 Pa",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.19"]
[]
[null,null,"C 2 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"CONDENSER 2"]
[]
[{"v":266,"d":"266 "},null,"DAIKIN RXYSQ10 (OUTDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":267,"d":"267 "},null,"×˜9,52 Liquid line (Incl. all fittings & bends)",null,"m",{"v":55,"d":"55 "}]
[]
[{"v":268,"d":"268 "},null,"×˜22,2 Gas line (Incl. all fittings & bends)",null,"m",{"v":55,"d":"55 "}]
[]
[{"v":269,"d":"269 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":270,"d":"270 "},null,"Cable tray",null,"m",{"v":55,"d":"55 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":271,"d":"271 "},null,"Refnet",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"AC G,2"]
[]
[{"v":272,"d":"272 "},null,"DAIKIN FXAQ32A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":273,"d":"273 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":274,"d":"274 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":275,"d":"275 "},null,"VP13(I.D.15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":276,"d":"276 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":277,"d":"277 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"AC G,3"]
[]
[{"v":278,"d":"278 "},null,"DAIKIN FXFQ50A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":279,"d":"279 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":280,"d":"280 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":281,"d":"281 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":282,"d":"282 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":283,"d":"283 "},null,"Cable tray",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"REMOVAL"]
[]
[{"v":284,"d":"284 "},null,"Cassette",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":285,"d":"285 "},null,"Console",null,"No",{"v":11,"d":"11 "}]
[]
[null,null,"RELOCATE"]
[]
[{"v":286,"d":"286 "},null,"Cassette",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":287,"d":"287 "},null,"Midwall Split",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":288,"d":"288 "},null,"Refridegrant piping",null,"No",{"v":45,"d":"45 "}]
[]
[null,null,"BILL NO.20"]
[]
[null,null,"AC G.4 & G.5(See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONING G.4"]
[]
[{"v":289,"d":"289 "},null,"DAIKIN FXSQ80A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":290,"d":"290 "},null,"×˜9,52 Liquid line (Incl. all fittings & bends)",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":291,"d":"291 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":292,"d":"292 "},null,"VP20(I.D20/O.D26) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":293,"d":"293 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":294,"d":"294 "},null,"Cable tray",null,"m",{"v":3,"d":"3 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":295,"d":"295 "},null,"300x250",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":296,"d":"296 "},null,"200x200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":297,"d":"297 "},null,"×˜150",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":298,"d":"298 "},null,"AC to Duct",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":299,"d":"299 "},null,"300x250 - 200x200",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":300,"d":"300 "},null,"×˜150  Spigot",null,"No",{"v":5,"d":"5 "}]
[]
[{"v":301,"d":"301 "},null,"200x200 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":302,"d":"302 "},null,"Rickard CCD150  flex",null,"No",{"v":5,"d":"5 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":303,"d":"303 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AIR CONDITIONING G,5"]
[]
[{"v":304,"d":"304 "},null,"DAIKIN FXSQ100A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":305,"d":"305 "},null,"×˜9,52 Liquid line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":306,"d":"306 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":307,"d":"307 "},null,"VP20(I.D20/O.D26) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":308,"d":"308 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":309,"d":"309 "},null,"Cable tray",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":310,"d":"310 "},null,"350x300",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":311,"d":"311 "},null,"300x200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":312,"d":"312 "},null,"200x200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":313,"d":"313 "},null,"×˜150",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":314,"d":"314 "},null,"AC to Duct",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":315,"d":"315 "},null,"350x300 - 300x200",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":316,"d":"316 "},null,"300x200 - 200x200",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":317,"d":"317 "},null,"×˜200  Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":318,"d":"318 "},null,"×˜150  Spigot",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":319,"d":"319 "},null,"200x200 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":320,"d":"320 "},null,"Rickard CCD200  flex",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":321,"d":"321 "},null,"Trox Z_LVS ×¸160 disc valve   flex (or Equivalent)",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":322,"d":"322 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.21"]
[]
[null,null,"AC (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER G.6"]
[]
[{"v":323,"d":"323 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":324,"d":"324 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":325,"d":"325 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":326,"d":"326 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":327,"d":"327 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":328,"d":"328 "},null,"Cable tray",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER G.7"]
[]
[{"v":329,"d":"329 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":330,"d":"330 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":331,"d":"331 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":332,"d":"332 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":333,"d":"333 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":334,"d":"334 "},null,"Cable tray",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER G.8"]
[]
[{"v":335,"d":"335 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":336,"d":"336 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":337,"d":"337 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":338,"d":"338 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":339,"d":"339 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":340,"d":"340 "},null,"Cable tray",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER G.11"]
[]
[{"v":341,"d":"341 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":342,"d":"342 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":343,"d":"343 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":344,"d":"344 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":345,"d":"345 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":346,"d":"346 "},null,"Cable tray",null,"No",{"v":20,"d":"20 "}]
[]
[null,null,"BILL NO.22"]
[]
[null,null,"AC G.9 & G.10 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER G.9"]
[]
[{"v":347,"d":"347 "},null,"DAIKIN FBA100A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":348,"d":"348 "},null,"×˜9,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":349,"d":"349 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":350,"d":"350 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":351,"d":"351 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":352,"d":"352 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":353,"d":"353 "},null,"300x250",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":354,"d":"354 "},null,"250x200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":355,"d":"355 "},null,"×˜150",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":356,"d":"356 "},null,"AC TO DUCT",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":357,"d":"357 "},null,"300x250 - 250x200",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":358,"d":"358 "},null,"×˜150 90\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":359,"d":"359 "},null,"×˜150 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":360,"d":"360 "},null,"250x200 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":361,"d":"361 "},null,"Rickard CCD 150  flex",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":362,"d":"362 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AIR CONDITIONER G.10"]
[]
[{"v":363,"d":"363 "},null,"DAIKIN FBA100A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":364,"d":"364 "},null,"×˜9,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":365,"d":"365 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":366,"d":"366 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":367,"d":"367 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":368,"d":"368 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":369,"d":"369 "},null,"300x250",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":370,"d":"370 "},null,"250x200",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":371,"d":"371 "},null,"×˜150",null,"m",{"v":8,"d":"8 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":372,"d":"372 "},null,"×˜150 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":373,"d":"373 "},null,"250x200 Stop-end",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":374,"d":"374 "},null,"Rickard CCD 150  flex",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":375,"d":"375 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.23"]
[]
[null,null,"AC G.12 (See Drawing CM0769-Y1)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER G.12"]
[]
[{"v":376,"d":"376 "},null,"DAIKIN FBA71A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":377,"d":"377 "},null,"×˜9,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":378,"d":"378 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":379,"d":"379 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":380,"d":"380 "},null,"Drain piping",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":381,"d":"381 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":382,"d":"382 "},null,"250x250",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":383,"d":"383 "},null,"×˜150",null,"m",{"v":4,"d":"4 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":384,"d":"384 "},null,"AC TO DUCT",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":385,"d":"385 "},null,"×˜150 90\"° Bend",null,"No",{"v":2,"d":"2 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":386,"d":"386 "},null,"×˜150 Spigot",null,"No",{"v":4,"d":"4 "}]
[]
[{"v":387,"d":"387 "},null,"250x250 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":388,"d":"388 "},null,"Rickard CCD 150  flex",null,"No",{"v":4,"d":"4 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":389,"d":"389 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.24"]
[]
[null,null,"AC (See Drawing CM0764-M120)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER 1,3"]
[]
[{"v":390,"d":"390 "},null,"DAIKIN FCAG50B (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":391,"d":"391 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":392,"d":"392 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":393,"d":"393 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":394,"d":"394 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":395,"d":"395 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":396,"d":"396 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AIR CONDITIONER 1,4"]
[]
[{"v":397,"d":"397 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":398,"d":"398 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":399,"d":"399 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":400,"d":"400 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":401,"d":"401 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":402,"d":"402 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AIR CONDITIONER 1,5"]
[]
[{"v":403,"d":"403 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":404,"d":"404 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":405,"d":"405 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":406,"d":"406 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":407,"d":"407 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":408,"d":"408 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AIR CONDITIONER 1,7"]
[]
[{"v":409,"d":"409 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":410,"d":"410 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":411,"d":"411 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":412,"d":"412 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":413,"d":"413 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":414,"d":"414 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AIR CONDITIONER 1,9"]
[]
[{"v":415,"d":"415 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":416,"d":"416 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":417,"d":"417 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":418,"d":"418 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":419,"d":"419 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":420,"d":"420 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER 1,10"]
[]
[{"v":421,"d":"421 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":422,"d":"422 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":423,"d":"423 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":424,"d":"424 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":425,"d":"425 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":426,"d":"426 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER 1,12"]
[]
[{"v":427,"d":"427 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":428,"d":"428 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":429,"d":"429 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":430,"d":"430 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":431,"d":"431 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":432,"d":"432 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"AIR CONDITIONER 1,13"]
[]
[{"v":433,"d":"433 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":434,"d":"434 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":435,"d":"435 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":436,"d":"436 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":437,"d":"437 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":438,"d":"438 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"AIR CONDITIONER 1,15"]
[]
[{"v":439,"d":"439 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":440,"d":"440 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":441,"d":"441 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":442,"d":"442 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":443,"d":"443 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":444,"d":"444 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"BILL NO.25"]
[]
[null,null,"AC (See Drawing CM0769-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER 1,16"]
[]
[{"v":445,"d":"445 "},null,"DAIKIN FTXF25E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":446,"d":"446 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":447,"d":"447 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":448,"d":"448 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":449,"d":"449 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":450,"d":"450 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AIR CONDITIONER 1,17"]
[]
[{"v":451,"d":"451 "},null,"DAIKIN FCAG35B (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":452,"d":"452 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":453,"d":"453 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":454,"d":"454 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":455,"d":"455 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":456,"d":"456 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":457,"d":"457 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AIR CONDITIONER 1,18"]
[]
[{"v":458,"d":"458 "},null,"DAIKIN FCAG35B (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":459,"d":"459 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":12,"d":"12 "}]
[]
[{"v":460,"d":"460 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":12,"d":"12 "}]
[]
[{"v":461,"d":"461 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":462,"d":"462 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":463,"d":"463 "},null,"Cable tray",null,"m",{"v":12,"d":"12 "}]
[]
[null,null,"BILL NO.26"]
[]
[null,null,"C 1,6 (See Drawing CM0764-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"CONDENSER 1,6"]
[]
[{"v":464,"d":"464 "},null,"DAIKIN RXYSQ6TY1 (OUTDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":465,"d":"465 "},null,"×˜9,52 Liquid line (Incl. all fittings & bends)",null,"m",{"v":30,"d":"30 "}]
[]
[{"v":466,"d":"466 "},null,"×˜19,1 Gas line (Incl. all fittings & bends)",null,"m",{"v":30,"d":"30 "}]
[]
[{"v":467,"d":"467 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":468,"d":"468 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":469,"d":"469 "},null,"Cable tray",null,"m",{"v":30,"d":"30 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":470,"d":"470 "},null,"REFNET",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"AC 1,6"]
[]
[{"v":471,"d":"471 "},null,"DAIKIN FXFQ50 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":472,"d":"472 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":473,"d":"473 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":474,"d":"474 "},null,"VP25(O,D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":475,"d":"475 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":476,"d":"476 "},null,"Cable tray",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"AC 1,11"]
[]
[{"v":477,"d":"477 "},null,"DAIKIN FXFQ50 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":478,"d":"478 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":479,"d":"479 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":3,"d":"3 "}]
[]
[{"v":480,"d":"480 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":481,"d":"481 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":482,"d":"482 "},null,"Cable tray",null,"m",{"v":3,"d":"3 "}]
[]
[null,null,"AC 1,14"]
[]
[{"v":483,"d":"483 "},null,"DAIKIN FXFQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":484,"d":"484 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":485,"d":"485 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":486,"d":"486 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":487,"d":"487 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":488,"d":"488 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"REMOVAL"]
[]
[{"v":489,"d":"489 "},null,"MIDWAL SPLIT UNIT",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":490,"d":"490 "},null,"Condenser",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":491,"d":"491 "},null,"Console unit",null,"No",{"v":15,"d":"15 "}]
[]
[null,null,"BILL NO.27"]
[]
[null,null,"C 1,6 AC 1,8 (See Drawing CM0764-Y2)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONING 1,8"]
[]
[{"v":492,"d":"492 "},null,"DAIKIN FXSQ63 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":493,"d":"493 "},null,"×˜9,52 Liquid line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":494,"d":"494 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":495,"d":"495 "},null,"VP20(1.D20/O.D26) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":496,"d":"496 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":497,"d":"497 "},null,"Cable tray",null,"m",{"v":2,"d":"2 "}]
[]
[null,null,"DUCTING (Insulated with FRK)"]
[]
[{"v":498,"d":"498 "},null,"250x250",null,"m",{"v":2,"d":"2 "}]
[]
[{"v":499,"d":"499 "},null,"200x200",null,"m",{"v":4,"d":"4 "}]
[]
[{"v":500,"d":"500 "},null,"150x150",null,"m",{"v":4,"d":"4 "}]
[]
[null,null,"TRANSFORMATION"]
[]
[{"v":501,"d":"501 "},null,"AC TO DUCT",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":502,"d":"502 "},null,"250x250 - 200x200",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":503,"d":"503 "},null,"200x200 - 150x150",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":504,"d":"504 "},null,"×˜150 Spigot",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":505,"d":"505 "},null,"150x150 Stop-end",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":506,"d":"506 "},null,"Rickard CCD 150  flex",null,"No",{"v":3,"d":"3 "}]
[]
[null,null,"RETURN AIR"]
[]
[{"v":507,"d":"507 "},null,"1200x600 RAG",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"BILL NO.28"]
[]
[null,null,"C 2 (See Drawing CM0764-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"CONDENSER 2"]
[]
[{"v":508,"d":"508 "},null,"DAIKIN REYQ14U (OUTDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":509,"d":"509 "},null,"×˜12,7 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":510,"d":"510 "},null,"×˜28,6 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":511,"d":"511 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":512,"d":"512 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"ANCILLARIES"]
[]
[{"v":513,"d":"513 "},null,"REFNET",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":514,"d":"514 "},null,"DAIKIN BS6Q14A",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":515,"d":"515 "},null,"DAIKIN BS8Q14A",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AC 2,1"]
[]
[{"v":516,"d":"516 "},null,"DAIKIN FXZQ32A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":517,"d":"517 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":518,"d":"518 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":519,"d":"519 "},null,"VP20(I,D20/O.D26) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":520,"d":"520 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":521,"d":"521 "},null,"Cable tray",null,"m",{"v":20,"d":"20 "}]
[]
[null,null,"AC 2,3"]
[]
[{"v":522,"d":"522 "},null,"DAIKIN FXZQ32A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":523,"d":"523 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":524,"d":"524 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":525,"d":"525 "},null,"VP20(I,D20/O.D26) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":526,"d":"526 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":527,"d":"527 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"AC 2,5"]
[]
[{"v":528,"d":"528 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":529,"d":"529 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":530,"d":"530 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":531,"d":"531 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":532,"d":"532 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":533,"d":"533 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AC 2,6"]
[]
[{"v":534,"d":"534 "},null,"DAIKIN FXFQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":535,"d":"535 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":536,"d":"536 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":537,"d":"537 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":538,"d":"538 "},null,"Cable tray",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":539,"d":"539 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"AC 2,7"]
[]
[{"v":540,"d":"540 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":541,"d":"541 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":542,"d":"542 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":543,"d":"543 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":544,"d":"544 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":545,"d":"545 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AC 2,8"]
[]
[{"v":546,"d":"546 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":547,"d":"547 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":548,"d":"548 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":549,"d":"549 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":550,"d":"550 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":551,"d":"551 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"AC 2,9"]
[]
[{"v":552,"d":"552 "},null,"DAIKIN FXFQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":553,"d":"553 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":554,"d":"554 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":555,"d":"555 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":556,"d":"556 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":557,"d":"557 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"BILL NO.29"]
[]
[null,null,"C 2 (See Drawing CM0764-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AC 2,10"]
[]
[{"v":558,"d":"558 "},null,"DAIKIN FXAQ32A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":559,"d":"559 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":560,"d":"560 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":561,"d":"561 "},null,"VP13(I,D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":562,"d":"562 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[null,null,"AC 2,11"]
[]
[{"v":563,"d":"563 "},null,"DAIKIN FXFQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":564,"d":"564 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":565,"d":"565 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":566,"d":"566 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":567,"d":"567 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":568,"d":"568 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"AC 2,12"]
[]
[{"v":569,"d":"569 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":570,"d":"570 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":571,"d":"571 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":572,"d":"572 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":573,"d":"573 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":574,"d":"574 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"AC 2,13"]
[]
[{"v":575,"d":"575 "},null,"DAIKIN FXAQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":576,"d":"576 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":577,"d":"577 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":578,"d":"578 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":579,"d":"579 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":580,"d":"580 "},null,"Cable tray",null,"No",{"v":0,"d":"0 "}]
[]
[null,null,"AC 2,14"]
[]
[{"v":581,"d":"581 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":582,"d":"582 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":583,"d":"583 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":15,"d":"15 "}]
[]
[{"v":584,"d":"584 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":585,"d":"585 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":586,"d":"586 "},null,"Cable tray",null,"m",{"v":15,"d":"15 "}]
[]
[null,null,"AC 2,15"]
[]
[{"v":587,"d":"587 "},null,"DAIKIN FXAQ25A (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":588,"d":"588 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":589,"d":"589 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":590,"d":"590 "},null,"VP13(I.D15/O.D18) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":591,"d":"591 "},null,"Condensate pump",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":592,"d":"592 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AC 2,16"]
[]
[{"v":593,"d":"593 "},null,"DAIKIN FXFQ32 (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":594,"d":"594 "},null,"×˜6,35 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":595,"d":"595 "},null,"×˜12,7 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":596,"d":"596 "},null,"VP25(O.D32/I.D25) Drain pipe (incl. all fittings & bends",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":597,"d":"597 "},null,"Controller",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":598,"d":"598 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"REMOVAL"]
[]
[{"v":599,"d":"599 "},null,"MIDWAL SPLIT UNIT",null,"No",{"v":2,"d":"2 "}]
[]
[{"v":600,"d":"600 "},null,"Condenser",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":601,"d":"601 "},null,"Console unit",null,"No",{"v":10,"d":"10 "}]
[]
[null,null,"BILL NO.30"]
[]
[null,null,"AC (See Drawing CM0769-Y3)"]
[]
[null,null,"Inclusive of supply, installation, consumables, flexible ducting, electrical controls, wiring, etc for completion as per specification Note: All ducting connection joints to be sealed Allow for scaffolding to work at roof level"]
[]
[null,null,"All equipment as per SABS approved standards: All costs for connecting, delivery, fittings, connections, bends, junctions and hanging materials to be included."]
[]
[null,null,"AIR CONDITIONER 2,2"]
[]
[{"v":602,"d":"602 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":603,"d":"603 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":604,"d":"604 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":605,"d":"605 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":606,"d":"606 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":607,"d":"607 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"AIR CONDITIONER 2,4"]
[]
[{"v":608,"d":"608 "},null,"DAIKIN FCAG71B (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":609,"d":"609 "},null,"×˜9,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":610,"d":"610 "},null,"×˜15,9 Gas line (Incl. all fittings & bends)",null,"m",{"v":5,"d":"5 "}]
[]
[{"v":611,"d":"611 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":612,"d":"612 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":613,"d":"613 "},null,"Cable tray",null,"m",{"v":5,"d":"5 "}]
[]
[null,null,"AIR CONDITIONER 2,17"]
[]
[{"v":614,"d":"614 "},null,"DAIKIN FCAG35B (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":615,"d":"615 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":616,"d":"616 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":617,"d":"617 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":618,"d":"618 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":619,"d":"619 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"AIR CONDITIONER 2,18"]
[]
[{"v":620,"d":"620 "},null,"DAIKIN FTXF35E (INDOOR)",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":621,"d":"621 "},null,"×˜6,5 Liquid line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":622,"d":"622 "},null,"×˜9,5 Gas line (Incl. all fittings & bends)",null,"m",{"v":10,"d":"10 "}]
[]
[{"v":623,"d":"623 "},null,"Bluchem treatment",null,"No",{"v":1,"d":"1 "}]
[]
[{"v":624,"d":"624 "},null,"Drain piping (Incl. all fitting & bends)",null,"m",{"v":20,"d":"20 "}]
[]
[{"v":625,"d":"625 "},null,"Cable tray",null,"m",{"v":10,"d":"10 "}]
[]
[null,null,"BILL NO.31"]
[]
[null,null,"GENERAL"]
[]
[{"v":626,"d":"626 "},null,"Test & commission the installation as per SABS",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":627,"d":"627 "},null,"Painting, labeling and identification as per SABS",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":628,"d":"628 "},null,"Workshop drawings",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":629,"d":"629 "},null,"Samples",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":630,"d":"630 "},null,"Liason with local Authority",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":631,"d":"631 "},null,"Attendance of final inspection with Local Authority",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":632,"d":"632 "},null,"Manuals & Instructions",null,"No",{"v":3,"d":"3 "}]
[]
[{"v":633,"d":"633 "},null,"Operator Training",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":634,"d":"634 "},null,"1 Year Maintenance Contract and Guarantee (2 Inspections; 1 every 6 Months)",null,"SUM",{"v":1,"d":"1 "}]
[]
[{"v":1,"d":"1 "},null,"PRELIMINARIES",null,"Page",{"v":197,"d":"197 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"FRESH AIR FAN B.1",null,"Page",{"v":200,"d":"200 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"FRESH AIR FAN G.1",null,"Page",{"v":203,"d":"203 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"FRESH AIR FAN G.2",null,"Page",{"v":206,"d":"206 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"FRESH AIR FAN G.3",null,"Page",{"v":209,"d":"209 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"FRESH AIR FAN G.4",null,"Page",{"v":212,"d":"212 "},{"v":0,"d":"0.00"}]
[]
[{"v":7,"d":"7 "},null,"FRESH AIR FAN G.5",null,"Page",{"v":215,"d":"215 "},{"v":0,"d":"0.00"}]
[]
[{"v":8,"d":"8 "},null,"FRESH AIR FAN 1.1",null,"Page",{"v":218,"d":"218 "},{"v":0,"d":"0.00"}]
[]
[{"v":9,"d":"9 "},null,"FRESH AIR FAN 1.2",null,"Page",{"v":221,"d":"221 "},{"v":0,"d":"0.00"}]
[]
[{"v":10,"d":"10 "},null,"FRESH AIR FAN 1.3",null,"Page",{"v":224,"d":"224 "},{"v":0,"d":"0.00"}]
[]
[{"v":11,"d":"11 "},null,"FRESH AIR FAN 1.4",null,"Page",{"v":227,"d":"227 "},{"v":0,"d":"0.00"}]
[]
[{"v":12,"d":"12 "},null,"FRESH AIR FAN 1.5",null,"Page",{"v":230,"d":"230 "},{"v":0,"d":"0.00"}]
[]
[{"v":13,"d":"13 "},null,"FRESH AIR FAN 2.1",null,"Page",{"v":233,"d":"233 "},{"v":0,"d":"0.00"}]
[]
[{"v":14,"d":"14 "},null,"FRESH AIR FAN 2.2",null,"Page",{"v":236,"d":"236 "},{"v":0,"d":"0.00"}]
[]
[{"v":15,"d":"15 "},null,"FRESH AIR FAN 2.3",null,"Page",{"v":239,"d":"239 "},{"v":0,"d":"0.00"}]
[]
[{"v":16,"d":"16 "},null,"FRESH AIR FAN 2.4",null,"Page",{"v":242,"d":"242 "},{"v":0,"d":"0.00"}]
[]
[{"v":17,"d":"17 "},null,"FRESH AIR FAN 2.5",null,"Page",{"v":245,"d":"245 "},{"v":0,"d":"0.00"}]
[]
[{"v":18,"d":"18 "},null,"EXTRACT AIR FAN 1",null,"Page",{"v":246,"d":"246 "},{"v":0,"d":"0.00"}]
[]
[{"v":19,"d":"19 "},null,"C2 GROUND FLOOR (GF)",null,"Page",{"v":249,"d":"249 "},{"v":0,"d":"0.00"}]
[]
[{"v":20,"d":"20 "},null,"STAND ALONE GROUND FLOOR G.4& G,5 (GF)",null,"Page",{"v":253,"d":"253 "},{"v":0,"d":"0.00"}]
[]
[{"v":21,"d":"21 "},null,"STAND ALONE GROUND FLOOR (GF)",null,"Page",{"v":256,"d":"256 "},{"v":0,"d":"0.00"}]
[]
[{"v":22,"d":"22 "},null," STAND ALONE G.9 & G.10 (GF)",null,"Page",{"v":260,"d":"260 "},{"v":0,"d":"0.00"}]
[]
[{"v":23,"d":"23 "},null,"STAND ALONE G.12 (GF)",null,"Page",{"v":263,"d":"263 "},{"v":0,"d":"0.00"}]
[]
[{"v":24,"d":"24 "},null,"STAND ALONE (FF)",null,"Page",{"v":268,"d":"268 "},{"v":0,"d":"0.00"}]
[]
[{"v":25,"d":"25 "},null,"STAND ALONE (FF)",null,"Page",{"v":271,"d":"271 "},{"v":0,"d":"0.00"}]
[]
[{"v":26,"d":"26 "},null,"C1.6 FLOOR (FF)",null,"Page",{"v":274,"d":"274 "},{"v":0,"d":"0.00"}]
[]
[{"v":27,"d":"27 "},null,"C1.6 AC 1.8 FIRST FLOOR (FF)",null,"Page",{"v":277,"d":"277 "},{"v":0,"d":"0.00"}]
[]
[{"v":28,"d":"28 "},null,"C2 SECOND FLOOR (SF)",null,"Page",{"v":282,"d":"282 "},{"v":0,"d":"0.00"}]
[]
[{"v":29,"d":"29 "},null,"C2 SECOND FLOOR (SF)",null,"Page",{"v":286,"d":"286 "},{"v":0,"d":"0.00"}]
[]
[{"v":30,"d":"30 "},null,"STAND ALONE SECOND FLOOR (SF)",null,"Page",{"v":289,"d":"289 "},{"v":0,"d":"0.00"}]
[]
[{"v":31,"d":"31 "},null,"GENERAL",null,"Page",{"v":290,"d":"290 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SECTION 7"]
[]
[null,null,"BILL NO. 1"]
[]
[null,null,"BUDGETARY ALLOWANCES ETC"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"General"]
[]
[null,null,"Work for which budgetary allowances are provided will be measured and valued in accordance with the contract and deducted in whole or in part if not required without any compensation for loss or profit on the said allowances"]
[]
[null,null,"Prime cost amounts and provisional sums are net.  Prime cost amounts include for delivery to site of all articles concerned Provisional sums are for material and equipment supplied and installed complete by firms of specialists"]
[]
[null,null,"Profit"]
[]
[null,null,"Where stated, the contractor may allow for profit if required"]
[]
[null,null,"Taking delivery"]
[]
[null,null,"Taking delivery of goods or articles by the contractor on site shall mean getting in, unpacking, checking that the quantity is correct and that the goods are complete and undamaged, submitting a report thereof to the interested parties and issuing vouchers for the receipt of such goods.  The contractor shall store the goods and will be held responsible for the safety thereof and indemnify the employer against any damage or loss which may occur"]
[]
[null,null,"Builder's work"]
[]
[null,null,"Builder's work in connection with specialist services is given elsewhere in these bills of quantities"]
[]
[null,null,"-----------------------------------------"]
[]
[null,null,"BUDGETARY ALLOWANCES"]
[]
[null,null,"Sundry building work"]
[]
[{"v":1,"d":"1 "},null,"Allow the budgetary sum of R 266 400.00 for the supply and installation of blinds",null,"Item",{"v":1,"d":"1 "},{"v":266400,"d":"266,400.00"},{"$f":"ROUND($F6065*G6065,2)","v":{"v":266400,"d":"266,400.00"}}]
[]
[{"v":2,"d":"2 "},null,"Allow the budgetary sum of R 202 756.00 for external work",null,"Item",{"v":1,"d":"1 "},{"v":202756,"d":"202,756.00"},{"$f":"ROUND($F6067*G6067,2)","v":{"v":202756,"d":"202,756.00"}}]
[]
[{"v":3,"d":"3 "},null,"Allow the budgetary sum of R 210 000.00 for the supply and installation fire screens",null,"Item",{"v":1,"d":"1 "},{"v":210000,"d":"210,000.00"},{"$f":"ROUND($F6069*G6069,2)","v":{"v":210000,"d":"210,000.00"}}]
[]
[{"v":4,"d":"4 "},null,"Allow the budgetary sum of R 269 000.00 for the supply of ironmongery",null,"Item",{"v":1,"d":"1 "},{"v":269000,"d":"269,000.00"},{"$f":"ROUND($F6071*G6071,2)","v":{"v":269000,"d":"269,000.00"}}]
[]
[{"v":5,"d":"5 "},null,"Allow the budgetary sum of R 493 500.00 for joinery fittings",null,"Item",{"v":1,"d":"1 "},{"v":493500,"d":"493,500.00"},{"$f":"ROUND($F6073*G6073,2)","v":{"v":493500,"d":"493,500.00"}}]
[]
[{"v":6,"d":"6 "},null,"Allow the budgetary sum of R 150 000.00 for the supply and installation of privacy pod",null,"Item",{"v":1,"d":"1 "},{"v":150000,"d":"150,000.00"},{"$f":"ROUND($F6075*G6075,2)","v":{"v":150000,"d":"150,000.00"}}]
[]
[{"v":7,"d":"7 "},null,"Allow the budgetary sum of R 50 000.00 for signage",null,"Item",{"v":1,"d":"1 "},{"v":50000,"d":"50,000.00"},{"$f":"ROUND($F6077*G6077,2)","v":{"v":50000,"d":"50,000.00"}}]
[]
[{"v":8,"d":"8 "},null,"Allow the budgetary sum of R 422 730.00 for the supply and installation of tiling",null,"Item",{"v":1,"d":"1 "},{"v":422730,"d":"422,730.00"},{"$f":"ROUND($F6079*G6079,2)","v":{"v":422730,"d":"422,730.00"}}]
[]
[{"v":9,"d":"9 "},null,"Allow the budgetary sum of R 100 000 for timber cladding",null,"Item",{"v":1,"d":"1 "},{"v":100000,"d":"100,000.00"},{"$f":"ROUND($F6081*G6081,2)","v":{"v":100000,"d":"100,000.00"}}]
[]
[{"v":10,"d":"10 "},null,"Allow the provisional sum of R 465 580.00 for specialist waterproofing",null,"Item",{"v":1,"d":"1 "},{"v":465580,"d":"465,580.00"},{"$f":"ROUND($F6083*G6083,2)","v":{"v":465580,"d":"465,580.00"}}]
[]
[{"v":1,"d":"1 "},null,"PRELIMINARIES",null,"Page",{"v":32,"d":"32 "},{"v":0,"d":"0.00"}]
[]
[{"v":2,"d":"2 "},null,"BUILDERS WORK",null,"Page",{"v":114,"d":"114 "},{"v":0,"d":"0.00"}]
[]
[{"v":3,"d":"3 "},null,"ELECTRICAL INSTALLATION",null,"Page",{"v":172,"d":"172 "},{"v":0,"d":"0.00"}]
[]
[{"v":4,"d":"4 "},null,"FIRE DETECTION INSTALLATION",null,"Page",{"v":187,"d":"187 "},{"v":0,"d":"0.00"}]
[]
[{"v":5,"d":"5 "},null,"FIRE PROTECTION SERVICES",null,"Page",{"v":196,"d":"196 "},{"v":0,"d":"0.00"}]
[]
[{"v":6,"d":"6 "},null,"VENTILATION & AIR CONDITIONING INSTALLATION",null,"Page",{"v":292,"d":"292 "},{"v":0,"d":"0.00"}]
[]
[{"v":7,"d":"7 "},null,"BUDGETARY ALLOWANCES",null,"Page",{"v":295,"d":"295 "},{"v":0,"d":"0.00"}]
[]
[null,null,"SUB-TOTAL",null,"ST",{"v":0,"d":"0 "}]
[]
[null,null,"VALUE ADDED TAX 15% RATE#",null,"TAX",{"v":15,"d":"15 "}]