{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["C&I Maintenance Services BoQ","C&I Servicing BoQ"],"not_rendered":{"defined_names":19},"read":"whole","date_system":"1900"}

{"sheet":"C&I Maintenance Services BoQ","index":0,"n_rows":87,"n_cols":8,"rows_kept":87,"merged":[[1,1,1,7]]}
[{"$nulls":7},"2024-02-17"]
[null,"PROJECT: C&I MAINTENANCE LABOUR SERVICES CONTRACT FOR A PERIOD OF FIVE (5) YEARS AT KUSILE POWER STATION"]
[]
[null,"ITEM NO.","DESCRIPTION","UNIT","NO. OFF","QTY","RATE","AMOUNT"]
[]
[null,null,"ITEM 1"]
[null,{"v":1,"d":"1.0"},"PRELIMINARIES AND GENERAL"]
[null,1.1,"Establishment of Facilities on the Site (Once Off Delivery of Containers)","Once Off",1,1]
[null,1.3,"Entry Medicals ","Yearly",18,1]
[null,1.4,"Exit Medicals ","Once Off",18,5]
[null,1.5,"PPE (Once Off)","Yearly",18,1]
[null,1.6,"Arch Flash","Yearly",18,5]
[null,1.7,"Security / Police Clearance certification ","Once Off",18,5]
[null,1.8,"Safety File","Once Off",1,1]
[null,1.9,"Site Office Container (1 Off Insulated, with Air-Con): 12m x 3m ","Once Off",1,1]
[null,{"v":1.1,"d":"1.10"},"Site Kitchen Container (1 Off): 9m x 3m","Once Off",1,1]
[null,1.11,"Site Storage Container (1 Off): 9m x 3m ","Once Off",1,1]
[null,1.12,"Ablution Unit (Serviced) (2 Off): 9m x 3m","Once Off",1,1]
[null,1.13,"Travelling (1 Off Kombi 14 Seater)","Monthly",1,60]
[null,1.14,"Site Bakkie (4x4 Double Cab Bakkie)","Monthly",1,60]
[null,null,"Sub-total Item 1 (P&Gs) carried to Summary"]
[]
[null,null,"ITEM 2"]
[null,{"v":2,"d":"2.0"},"C&I MAINTENANCE SERVICES (SITE RESOURCES)"]
[]
[null,"2.1","NORMAL TIME"]
[null,"2.1.1","C&I Maintenance Site Manager (10 years experience) (1 off)","Hours",1,{"$f":"163*60","v":9780}]
[null,"2.1.2","C&I Maintenance Technical Supervisor (7-10 years experience) (1 off)","Hours",1,9780]
[null,"2.1.3","C&I Maintenance Technician (7-10 years experience) (3 off)","Hours",3,9780]
[null,"2.1.4","C&I Maintenance Mechanician (5-7 years experience) (9 off)","Hours",9,9780]
[null,"2.1.5","C&I Fied Instrumentation Technicain  (5-7 years experience) (2 off)","Hours",2,9780]
[null,"2.1.6","C&I Maintenance Technician Assistant (0-2 years experience) (1 off)","Hours",1,9780]
[null,null,"Safety Officer (0-2 years experience) (1 off)","Hours",1,9780]
[null,null,"Subtotal Item 2.1 Normal Time "]
[]
[null,2.2,"NORMAL OVERTIME"]
[null,"2.2.1","C&I Maintenance Technical Supervisor (7-10 years experience) (1 off)","Hours",1,{"$f":"60*60","v":3600}]
[null,"2.2.2","C&I Maintenance Technician (7-10 years experience) (3 off)","Hours",3,{"$f":"100*60","v":6000}]
[null,"2.2.3","C&I Maintenance Mechanician (5-7 years experience) (9 off)","Hours",9,{"$f":"100*60","v":6000}]
[null,"2.2.4","C&I Fied Instrumentation Technicain  (5-7 years experience) (2 off)","Hours",2,{"$f":"100*60","v":6000}]
[null,"2.2.5","C&I Maintenance Technician Assistant (0-2 years experience) (1 off)","Hours",1,{"$f":"100*60","v":6000}]
[null,"2.2.6","Safety Officer (0-2 years experience) (1 off)","Hours",1,{"$f":"100*60","v":6000}]
[null,null,"Subtotal Item 2.2 Normal Overtime "]
[]
[null,2.3,"SUNDAYS & P/H OVER TIME"]
[null,"2.3.1","C&I Maintenance Technical Supervisor (7-10 years experience) (1 off)","Hours",1,{"$f":"24*60","v":1440}]
[null,"2.3.2","C&I Maintenance Technician (7-10 years experience) (3 off)","Hours",3,{"$f":"55*60","v":3300}]
[null,"2.3.3","C&I Maintenance Mechanician (5-7 years experience) (9 off)","Hours",9,{"$f":"55*60","v":3300}]
[null,"2.3.4","C&I Fied Instrumentation Technicain  (5-7 years experience) (2 off)","Hours",2,{"$f":"55*60","v":3300}]
[null,"2.3.5","C&I Maintenance Technician Assistant (0-2 years experience) (1 off)","Hours",1,{"$f":"55*60","v":3300}]
[null,"2.3.6","Safety Officer (0-2 years experience) (1 off)","Hours",1,{"$f":"55*60","v":3300}]
[null,null,"Subtotal Item 2.3  Sundays & P/H Overtime "]
[]
[null,2.4,"STANDBY ALLOWANCE"]
[null,"2.4.1","C&I Maintenance Technical Supervisor (7-10 years experience) (1 off)","Hours",1,{"$f":"7*4*60","v":1680}]
[null,"2.4.2","C&I Maintenance Technician (7-10 years experience) (3 off)","Hours",3,1680]
[null,"2.4.3","C&I Maintenance Mechanician (5-7 years experience) (9 off)","Hours",9,1680]
[null,"2.4.4","C&I Fied Instrumentation Technicain  (5-7 years experience) (2 off)","Hours",2,1680]
[null,"2.4.5","C&I Maintenance Technician Assistant (0-2 years experience) (1 off)","Hours",1,1680]
[null,"2.4.6","Safety Officer (0-2 years experience) (1 off)","Hours",1,1680]
[null,null,"Sub-total Item 2.4 Standby Allowance carried to Summary"]
[]
[null,null,"Sub-total Item 2 C&I Maintenance Service (Site Resources) carried to Summary"]
[]
[null,null,"ITEM 3"]
[null,{"v":3,"d":"3.0"},"C&I TOOLS "]
[null,3.1,"Gedore tool kit 65 piece","Once Off",16,1]
[null,3.2,"Cable stripper","Once Off",16,1]
[null,3.3,"Fluke 177 true RMS multimeter ","Once Off",16,1]
[null,3.4,"30 piece hex key set","Once Off",16,1]
[null,3.5,"Hirschmann wire set","Once Off",16,1]
[null,3.6,"Jeweller screwdriver set","Once Off",16,1]
[null,3.7,"Instrumentation Tool bag","Once Off",16,1]
[null,null,"Sub-total Item 3 C&I Tools carried to Summary"]
[]
[]
[null,null,"SUMMARY"]
[]
[null,"ITEM 1","PRELIMINARIES & GENERAL"]
[]
[null,"ITEM 2",{"$f":"C24","v":"C&I MAINTENANCE SERVICES (SITE RESOURCES)"}]
[]
[null,"ITEM 3",{"$f":"C66","v":"C&I TOOLS "}]
[]
[null,"ITEM 4","SERVICING OF MAJOR CONTROL AND INSTRUMENTATION COMPONENTS"]
[]
[null,null,"Final Summary Total"]

{"sheet":"C&I Servicing BoQ","index":1,"n_rows":412,"n_cols":8,"rows_kept":412,"merged":[[2,1,2,6],[6,1,6,3],[411,1,411,6]]}
[{"$nulls":7},"2024-02-17"]
[]
[null,"PROJECT: C&I MAINTENANCE LABOUR SERVICES CONTRACT FOR A PERIOD OF FIVE (5) YEARS AT KUSILE POWER STATION"]
[]
[null,"ITEM 4 "]
[]
[null,"SERVICING OF MAJOR CONTROL AND INSTRUMENTATION COMPONENTS"]
[]
[null,"ITEM NO.","MATERIAL NO.","EQUIPMENT SHORT DESCRIPTION","UNIT","QTY","SERVICING RATE","TOTAL AMOUNT"]
[null,"4.1","0579213","SENSOR TEMP:600 DEG C","Each",4]
[null,"4.2","0583425","SENSOR TEMP:0-100 DEG C;MEASURING INSECT","Each",4]
[null,"4.3","0608218","SENSOR TEMP:546 DEG C;OPTICAL;IP20","Each",4]
[null,"4.4","0608219","SENSOR TEMP:600 DEG C;IP20;4-20 MA","Each",4]
[null,"4.5","0608221","SENSOR TEMP:380 DEG C;IP20;4-20 MA","Each",4]
[null,"4.6","0608222","SENSOR TEMP:OTSC310-15M1/0;480 DEG C","Each",4]
[null,"4.7","0608743","SENSOR TEMP:P-10886;610 DEG C;IP20","Each",4]
[null,"4.8","0608745","SENSOR TEMP:OTSC310-15D2/0;480 DEG C","Each",4]
[null,"4.9","0608746","SENSOR TEMP:OTSC310-15P8/O;480 DEG C","Each",4]
[null,"4.10","0608747","SENSOR TEMP:TR88-AB8A1D1CC000TZ1-300MM","Each",4]
[null,"4.11","0608748","SENSOR TEMP:TR88-AB4A1D1CC000TZ1-XMM","Each",4]
[null,"4.12","0608749","SENSOR TEMP:TC88-AB8A1D1CA100TZ1;IP20","Each",4]
[null,"4.13","0608750","SENSOR TEMP:TC88-AB8A1D1CA100TZ1;IP20","Each",4]
[null,"4.14","0621894","MODULE:1KGZ056602;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.15","0621895","MODULE:1KGZ056600;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.16","0621896","MODULE:1KGZ056940;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.17","0621897","MODULE:1KGZ056932;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.18","0621903","MODULE:1KGZ056606;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.19","0622001","SENSOR TEMP:TN2531;-40 TO 150 DEG C","Each",4]
[null,"4.20","0622156","SENSOR:1KGZ049812;MEASUREMENT;1-12 PH","Each",4]
[null,"4.21","0629963","MODULE:1KGZ056593;LEVEL SENSOR","Each",4]
[null,"4.22","0633573","SENSOR TEMP:27-6AK1-9264-2U00","Each",4]
[null,"4.23","0633933","SENSOR TEMP:1100 DEG C;TEMPERATURE","Each",4]
[null,"4.24","0634161","SENSOR TEMP:TR88-AB9Y9D1CC009;TA30A","Each",4]
[null,"4.25","0659042","SENSOR, TEMPERATURE:MODULAR RTD ASSEMBLY","Each",4]
[null,"4.26","0659044","SENSOR, TEMPERATURE:MODULAR;600 DEG C","Each",4]
[null,"4.27","0659045","SENSOR, TEMPERATURE:MODULAR;601 DEG C","Each",4]
[null,"4.28","0550621","GAUGE:OIL TEMP IND; 6 M;0-120 DEG C","Each",4]
[null,"4.29","0643516","GAUGE:TMI100T;TEMPERATURE","Each",4]
[null,"4.30","0665713","GAUGE:TEMPERATURE;0-100 DEG C;SS 304","Each",4]
[null,"4.31","0659046","SENSOR, TEMPERATURE:MODULAR RTD ASSEMBLY","Each",4]
[null,"4.32","0661154","SENSOR TEMP:120 DEG C;PT100;IP55;SCREW","Each",4]
[null,"4.33","0662715","SENSOR TEMP:0-300 DEG C;LEVEL INDICATOR","Each",4]
[null,"4.34","0642067","SENSOR TEMP:3BHB015149R1001;0-100 DEG C","Each",4]
[null,"4.35","0642129","SENSOR TEMP:-30 TO 200 DEG C;BASE","Each",4]
[null,"4.36","0642130","SENSOR TEMP:IDD;0-30 DEG C;BOLTED","Each",4]
[null,"4.37","0634168","SENSOR TEMP:TR88-AB9A1D1CC000;DETECTOR","Each",4]
[null,"4.38","0634170","SENSOR TEMP:TR88-AB002X1CC009;DETECTOR","Each",4]
[null,"4.39","0634172","SENSOR TEMP:TR63-ABEAY9XYYCC0;DETECTOR","Each",4]
[null,"4.40","0643527","SENSOR TEMP:TSP11-Y0Z9M2U4S1D6P5B2B4Y1","Each",4]
[null,"4.41","0643528","SENSOR TEMP:DOUBLE THERMOMETER SUPPL P/N: TSP111-Y0K1M2U2S1D6P5S1B2H4A8","Each",4]
[null,"4.42","0643529","SENSOR TEMP:TSP111-A1K1M2U2S1D6P5S1B2Y1","Each",4]
[null,"4.43","0643530","SUPPL P/N: TSP111-A1K1M2U2S1D6P5S1B2H5A8;SENSOR TEMP:DOUBLE THERMOMETER","Each",4]
[null,"4.44","0643531","SUPPL P/N: TSP111-A1K1M2U2S1D6P5B2B2H2A8T1 SENSOR TEMP:DOUBLE THERMOMETER","Each",4]
[null,"4.45","0643536","SENSOR TEMP:W-GYI5","Each",4]
[null,"4.46","0643946","SENSOR TEMP:TEMP2","Each",4]
[null,"4.47","0645104","SENSOR TEMP:-40 TO 72 DEG C;FIBER OPTIC","Each",4]
[null,"4.48","0646092","SENSOR TEMP:STR-AF1111/17453-1111-310","Each",4]
[null,"4.49","0646093","SENSOR TEMP","Each",4]
[null,"4.50","0646218","SENSOR TEMP:EET22","Each",4]
[null,"4.51","0647067","SENSOR TEMP:F600-2;100 DEG C;MONITOR","Each",4]
[null,"4.52","0647583","SUPPL P/N: TC88-AB9A1D1CB100/920MM SENSOR TEMP","Each",4]
[null,"4.53","0647584","SUPPL P/N: OTSC310-YYXJ398A9YY+Z1+OTSC310-15J5/0 SENSOR TEMP","Each",4]
[null,"4.54","0647585","SUPPL P/N: TC88-AB8A1D1CB100 SENSOR TEMP","Each",4]
[null,"4.55","0647586","P/N: OTSC310-YYXJ398A9YY+Z1+OTSC310-15F3/0 SENSOR TEMP","Each",4]
[null,"4.56","0647587"," SUPPL P/N: TC88-AB9A1D1CB100/905MM SENSOR TEMP","Each",4]
[null,"4.57","0647588","SUPPL P/N: TC88-AB9Y9D1CB10Y/1.068MM SENSOR TEMP","Each",4]
[null,"4.58","0647589","SUPPL P/N: TC88-AB9Y9D1CB10Y/1.405MM SENSOR TEMP","Each",4]
[null,"4.59","0647590","SUPPL P/N: TC88-AB9Y9D1CB10Y/1.385MM SENSOR TEMP","Each",4]
[null,"4.60","0647591","SUPPL P/N: TC88AB002X1CA10Y/1.869MM SENSOR TEMP","Each",4]
[null,"4.61","0647592","SUPPL P/N: TC88-AB9Y9D1CA10Y/1.256MM SENSOR TEMP","Each",4]
[null,"4.62","0647593","SUPPL P/N: TC88AB002X1CA10Y/1.205MM SENSOR TEMP","Each",4]
[null,"4.63","0647594","SUPPL P/N: TC88-AB9Y9D1CA10Y/1.079MM SENSOR TEMP","Each",4]
[null,"4.64","0647595","SUPPL P/N: TC88-AB9Y9D1CA10Y/1.451MM SENSOR TEMP","Each",4]
[null,"4.65","0647596","SUPPL P/N: TC88-AB9Y9D1CA10Y/1.440MM SENSOR TEMP","Each",4]
[null,"4.66","0647598","SUPPL P/N: OTSC310-YYXJ398A9YY+Z1+OTSC310-15N7/0 SENSOR TEMP","Each",4]
[null,"4.67","0647599"," SUPPL P/N: TR88-AB9Y9D1CC009/1.565MM SENSOR TEMP","Each",4]
[null,"4.68","0647600","SENSOR TEMP:SMART FLUX;DIAMETER: 44.5MM","Each",4]
[null,"4.69","0647601","SENSOR TEMP:SMART FLUX;DIAMETER: 38MM","Each",4]
[null,"4.70","0647602","SENSOR TEMP:SMART FLUX;DIAMETER: 38MM","Each",4]
[null,"4.71","0647603","SENSOR TEMP:SMART FLUX;DIAMETER: 38MM","Each",4]
[null,"4.72","0647604","SENSOR TEMP:SMART FLUX;DIAMETER: 44.5MM","Each",4]
[null,"4.73","0647605","SENSOR TEMP:SMART FLUX;DIAMETER: 44.5MM","Each",4]
[null,"4.74","0647606","SUPPL P/N: TC88-AB8A1D1CB100 SENSOR TEMP","Each",4]
[null,"4.75","0647615","SENSOR TEMP","Each",4]
[null,"4.76","0662592","INDICATOR SGHT FLW:LEVEL/TEMPERATURE","Each",4]
[null,"4.77","0662652","INDICATOR SGHT FLW:LEVEL/TEMPERATURE","Each",4]
[null,"4.78","0662689","INDICATOR SGHT FLW:LEVEL/TEMPERATURE","Each",4]
[null,"4.79","0662715","SENSOR TEMP:0-300 DEG C;LEVEL INDICATOR","Each",4]
[null,"4.80","0662561","INDICATOR SGHT FLW:LEVEL/TEMPERATURE","Each",4]
[null,"4.81","0634168","SENSOR TEMP:TR88-AB9A1D1CC000;DETECTOR","Each",4]
[null,"4.82","0634170","SENSOR TEMP:TR88-AB002X1CC009;DETECTOR","Each",4]
[null,"4.83","0634172","SENSOR TEMP:TR63-ABEAY9XYYCC0;DETECTOR","Each",4]
[null,"4.84","0565803","SWITCH LVL:MWS-ST/SR-11;MICROWAVE;2 A","Each",4]
[null,"4.85","0574031","TRANSMITTER LVL:GHM 0250 M D60 1A1","Each",4]
[null,"4.86","0574045","TRANSMITTER LVL:7ML5033-1AA10-1A","Each",4]
[null,"4.87","0579211","SWITCH LVL:VIBRATING TUNING FORK CONTACT","Each",4]
[null,"4.88","0583429","TRANSMITTER LVL:0-400 MM;O/P 4-20 MA","Each",4]
[null,"4.89","0583430","TRANSMITTER LVL:0-500 MM;O/P 4-20 MA","Each",4]
[null,"4.90","0607312","TRANSMITTER LVL:0-40 M;O/P 4-20 MA","Each",4]
[null,"4.91","0609431","TRANSMITTER LVL:5303HA2S1K6BM00650SAE0","Each",4]
[null,"4.92","0609433","TRANSMITTER LVL:FMR250-AEE2GGJAA2K","Each",4]
[null,"4.93","0609481","SWITCH LVL:FTM50-AGG2A5A32SA1;8-16 MA","Each",4]
[null,"4.94","0618496","TRANSMITTER LVL: FMI51-A1EGDJA2Y1A","Each",4]
[null,"4.95","0621760","GLASS LVL GAUGE:FLAT;PVC;BLACK","Each",4]
[null,"4.96","0621772","TRANSMITTER LVL:0-400 MM;O/P 0-20 MA","Each",4]
[null,"4.97","0622174","TRANSMITTER LVL:1KGZ056589;0-2 M;CABLE","Each",4]
[null,"4.98","0622175","TRANSMITTER LVL:1KGZ056588;0-2 M;CABLE","Each",4]
[null,"4.99","0622176","TRANSMITTER LVL:1KGZ056601;0-8 M;NPT","Each",4]
[null,"4.100","0623933","SWITCH LVL:MAGNETIC FLOAT;24 VDC;SPST","Each",4]
[null,"4.101","0634042","SWITCH LVL:TILT;0-60 DEG C;230 VAC;3 A","Each",4]
[null,"4.102","0634050","TRANSMITTER LVL:ENS3216-3-0520-000-K","Each",4]
[null,"4.103","0636064","TRANSMITTER LVL:0-23 M;O/P 4-20 MA","Each",4]
[null,"4.104","0636065","TRANSMITTER LVL:0-20 M;O/P 4-20 MA","Each",4]
[null,"4.105","0636066","TRANSMITTER LVL:0-30 M;O/P 4-20 MA","Each",4]
[null,"4.106","0636385","TRANSMITTER LVL:FMU30-10A1/0;0-8 M","Each",4]
[null,"4.107","0636424","TRANSMITTER LVL:PMP71ABA1KC1GHA9E","Each",4]
[null,"4.108","0636426","TRANSMITTER LVL:0-300 KPA;O/P 4-20 MA","Each",4]
[null,"4.109","0637178","SWITCH LVL:VIBRATION FORK;50 DEG C","Each",4]
[null,"4.110","0639567","SWITCH LVL:FTI56-AAB2RVJ42A1A;55 VDC","Each",4]
[null,"4.111","0639568","SWITCH LVL:TYPE4;CAPACITANCE;230 VAC","Each",4]
[null,"4.112","0640287","SWITCH LVL:RELAY;200 MM;4-20 MA;DPDT","Each",4]
[null,"4.113","0641894","SWITCH LVL:BP-H24-Z11;ROLLER LEVER","Each",4]
[null,"4.114","0641926","TRANSMITTER LVL:FMP52-AAACCA0ACHK-JD","Each",4]
[null,"4.115","0642897","TRANSMITTER LVL:RHM0650MH021A01-EX;4 W","Each",4]
[null,"4.116","0643073","SWITCH LVL:TSCS-901;ELECTRODE;0-65 DEG C","Each",4]
[null,"4.117","0643222","TRANSMITTER LVL:FX62.AAAFD3HKMXX;0-2 M","Each",4]
[null,"4.118","0643436","SWITCH LVL:FTL51-G-GR2-DB7-G5A","Each",4]
[null,"4.119","0643542","SWITCH LVL:LS-800-5;SINGLE-POINT","Each",4]
[null,"4.120","0643547","TRANSMITTER LVL:TEH","Each",4]
[null,"4.121","0644181","SWITCH LVL:OLH-2","Each",4]
[null,"4.122","0644182","SWITCH LVL:31160NN/9","Each",4]
[null,"4.123","0644635","TRANSMITTER LVL:FMI51-A1AGDJA3A1A","Each",4]
[null,"4.124","0644654","TRANSMITTER LVL:VEGAFLEX 82;0-1750 MM","Each",4]
[null,"4.125","0644883","SWITCH LVL:FDMH16;FLOAT;-10 TO 120 DEG C","Each",4]
[null,"4.126","0644885","SWITCH LVL:FD7DFU4S441030KL;RELAY","Each",4]
[null,"4.127","0644888","TRANSMITTER LVL:NMC-T21G6E3Y;265-4000 MA","Each",4]
[null,"4.128","0645205","TRANSMITTER LVL:4193143-0","Each",4]
[null,"4.129","0645212","TRANSMITTER LVL:FMI51-A1EGEJB3Y1A0","Each",4]
[null,"4.130","0646123","TRANSMITTER LVL:4FV1CFJAC2A","Each",4]
[null,"4.131","0646125","SWITCH LVL:IGQ2BB4G7A","Each",4]
[null,"4.132","0646126","SWITCH LVL:IGQ2BB5G7A","Each",4]
[null,"4.133","0646173","SWITCH LVL:FTL50-AGQ2AA4G5A","Each",4]
[null,"4.134","0646410","SWITCH LVL:331-016","Each",4]
[null,"4.135","0647608","TRANSMITTER LVL","Each",4]
[null,"4.136","0648327","SWITCH LVL:CAPACITANCE;-0 TO 50 DEG C","Each",4]
[null,"4.137","0648328","SWITCH LVL:FLOAT;0-1 BAR 0-80 DEG C;48 V","Each",4]
[null,"4.138","0648384","TRANSMITTER LVL:0-3 M;O/P 4-20 MA;0.8 W","Each",4]
[null,"4.139","0648385","TRANSMITTER LVL:8 M;O/P 4-20 MA;24 VAC","Each",4]
[null,"4.140","0648571","SWITCH LVL","Each",4]
[null,"4.141","0648811","TRANSMITTER LVL:0-6.5 M;O/P 4-20 MA","Each",4]
[null,"4.142","0662226","TRANSMITTER LVL:0-500 MM;O/P 4-20 MA","Each",4]
[null,"4.143","0662567","SWITCH LVL:ELECTRONIC;-0 TO 65 DEG C","Each",4]
[null,"4.144","0662658","SWITCH LVL:OIL LEVEL;-0 TO 65 DEG C","Each",4]
[null,"4.145","0662687","SWITCH LVL:OIL LEVEL;-0 TO 80 DEG C;4 A","Each",4]
[null,"4.146","0665808","TRANSMITTER LVL:0-150 MM;O/P 0-1 MPA","Each",4]
[null,"4.147","0665809","TRANSMITTER LVL:0-150 MM;O/P 5 MPA","Each",4]
[null,"4.148","0666805","SWITCH LVL:FLOAT ACTUATING;230 V;0.5 A","Each",4]
[null,"4.149","0668747","SWITCH LVL:FLOAT;ADJUSTABLE;24-220 VDC","Each",4]
[null,"4.150","0672667","TRANSMITTER LVL:30 M;O/P 4-20 MA;24 VDC","Each",4]
[null,"4.151","0676400","SWITCH LVL:BINARY;1750 MM;19-253 VAC","Each",4]
[null,"4.152","0682761","TRANSMITTER LVL:265-4000 MM;O/P 4-20 MA","Each",4]
[null,"4.153","0626653","THERMOCOUPLE:T1 TEBKSS 30;K;3 MM;950 MM","Each",4]
[null,"4.154","0633290","THERMOCOUPLE:K;11 MM;200 MM;1100 DEG C","Each",17]
[null,"4.155","0634125","THERMOCOUPLE:K;2 MM;2.532 MM;SS;1","Each",17]
[null,"4.156","0634126","THERMOCOUPLE:K;2 MM;2.122 MM;SS;1","Each",17]
[null,"4.157","0634128","THERMOCOUPLE:K;2 MM;2.109 MM;SS;1","Each",17]
[null,"4.158","0634132","THERMOCOUPLE:K;2 MM;2.544 MM;SS;0","Each",17]
[null,"4.159","0634141","THERMOCOUPLE:K;2 MM;2.277 MM;SS;0","Each",17]
[null,"4.160","0634142","THERMOCOUPLE:K;2 MM;2.216 MM;SS;0","Each",17]
[null,"4.161","0634143","THERMOCOUPLE:K;2 MM;2.415 MM;SS;0","Each",17]
[null,"4.162","0634145","THERMOCOUPLE:K;2 MM;2.139 MM;SS;1","Each",17]
[null,"4.163","0634146","THERMOCOUPLE:K;2 MM;2.512 MM;SS;1","Each",17]
[null,"4.164","0634196","THERMOCOUPLE:K;11 MM;300 MM;0","Each",17]
[null,"4.165","0634197","THERMOCOUPLE:K;11 MM;1.604 MM;0","Each",17]
[null,"4.166","0634198","THERMOCOUPLE:K;11 MM;1.203 MM;0","Each",17]
[null,"4.167","0636427","THERMOCOUPLE:K;12 MM;2080 M;NICR/NICKEL","Each",17]
[null,"4.168","0636428","THERMOCOUPLE:K;12 MM;2.835 KM;DOUBLE","Each",17]
[null,"4.169","0636429","THERMOCOUPLE:K;12 MM;2.665 KM;DOUBLE","Each",17]
[null,"4.170","0636430","THERMOCOUPLE:K;12 MM;2.35 KM;DOUBLE","Each",17]
[null,"4.171","0636431","THERMOCOUPLE:K;12 MM;2235 M;NICR/NICKEL","Each",17]
[null,"4.172","0645171","THERMOCOUPLE:GMD2953576R0025;K;2","Each",17]
[null,"4.173","0645172","THERMOCOUPLE:GMD2953576R0024;K;2","Each",17]
[null,"4.174","0645173","THERMOCOUPLE:GMD2953576R0023;K;2","Each",17]
[null,"4.175","0645174","THERMOCOUPLE:GMD2953576R0022;K;2","Each",17]
[null,"4.176","0645175","THERMOCOUPLE:GMD2953576R0021;K;2","Each",17]
[null,"4.177","0645179","THERMOCOUPLE:GMD2953576R0020;K;2","Each",17]
[null,"4.178","0646022","THERMOCOUPLE:206.00996310","Each",17]
[null,"4.179","0646023","THERMOCOUPLE:206.00997110","Each",17]
[null,"4.180","0665650","THERMOCOUPLE:K;6 MM;402 MM;SS 2.4815","Each",17]
[null,"4.181","0665651","THERMOCOUPLE:RTD-PT100;6 MM;402 MM","Each",17]
[null,"4.182","0665654","THERMOCOUPLE:K;6 MM;260 MM;0-600 DEG C","Each",17]
[null,"4.183","0665658","THERMOCOUPLE:K;6 MM;375 MM;0-600 DEG C","Each",17]
[null,"4.184","0665716","THERMOCOUPLE:RTD; PT100;6 MM;402 MM","Each",17]
[null,"4.185","0669309","THERMOCOUPLE:K;6 MM;200 MM;0-600 DEG C","Each",17]
[null,"4.186","0621441","CONTROLLER ELECTRNC:LOW LEVEL SWITCH","Each",17]
[null,"4.187","0621894","MODULE:1KGZ056602;LEVEL SENSOR;RANGE:","Each",17]
[null,"4.188","0621895","MODULE:1KGZ056600;LEVEL SENSOR;RANGE:","Each",17]
[null,"4.189","0621896","MODULE:1KGZ056940;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.190","0621897","MODULE:1KGZ056932;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.191","0621903","MODULE:1KGZ056606;LEVEL SENSOR;RANGE:","Each",4]
[null,"4.192","0629963","MODULE:1KGZ056593;LEVEL SENSOR","Each",4]
[null,"4.193","0630751","INDICATOR:IL320-A4;OIL LEVEL;1-100 MA","Each",4]
[null,"4.194","0638868","INDICATOR:IL320-L1;OIL LEVEL;1-100 MA","Each",4]
[null,"4.195","0643520","SENSOR:LEVEL","Each",4]
[null,"4.196","0643521","SENSOR:LEVEL","Each",4]
[null,"4.197","0643532","SENSOR:LEVEL","Each",4]
[null,"4.198","0645016","DISPLAY:RIA261;LOCAL LEVEL DIGITAL","Each",4]
[null,"4.199","0645871","INDICATOR:SP-KUS-F2-22054;MAGNETIC LEVEL","Each",4]
[null,"4.200","0646048","INDICATOR:206.00866010;OIL LEVEL","Each",4]
[null,"4.201","0646310","INDICATOR SGHT FLW:092-301-02;OIL LEVEL","Each",4]
[null,"4.202","0646837","HOUSING:52010132;LEVEL INDICATOR","Each",4]
[null,"4.203","0646838","LEVEL:FTR325-A1A1;INDICATOR;NIVOTESTER","Each",4]
[null,"4.204","0646839","LEVEL:FDR50-B1GDA;MICROWAVE RECEIVER","Each",4]
[null,"4.205","0646841","LEVEL:FQR50-B1GDA;MICROWAVE TRANSMITTER","Each",4]
[null,"4.206","0648400","CAPACITOR:C1 0.26UF; INSULATION LEVEL:","Each",4]
[null,"4.207","0653285","TRANSMITTER, LEVEL","Each",4]
[null,"4.208","0653348","TRANSMITTER, LEVEL:INIDCATOR","Each",4]
[null,"4.209","0654716","SWITCH, LEVEL","Each",4]
[null,"4.210","0662544","TRANSDUCER:POSITION LEVEL;I/P 110 VDC","Each",4]
[null,"4.211","0636381","DETECTOR RT:PT100;0-100 DEG C;3;NO","Each",4]
[null,"4.212","0636384","DETECTOR RT:PT100;0-230 DEG C;260 MM;2","Each",4]
[null,"4.213","0641847","METER:MCB2;DETECTOR;-10 TO 50 DEG C;LCD","Each",4]
[null,"4.214","0645209","DETECTOR RT:TSP111-Y0W1M2U4S1D6P5S1B2T0","Each",4]
[null,"4.215","0646254","DETECTOR:Z884k302223;POS2","Each",4]
[null,"4.216","0646269","DETECTOR:117791/118297;POS2","Each",4]
[null,"4.217","0648325","DETECTOR RT:THERMOMETER;-50 TO 400 DEG C","Each",4]
[null,"4.218","0648326","DETECTOR RT:THERMOMETER;-50 TO 400 DEG C","Each",4]
[null,"4.219","0649050","DETECTOR RT:-40 TO 400 DEG C;160 MM","Each",4]
[null,"4.220","0662581","TRANSDUCER:POSITION LEVEL;I/P 153 VDC","Each",4]
[null,"4.221","0662658","SWITCH LVL:OIL LEVEL;-0 TO 65 DEG C","Each",4]
[null,"4.222","0662687","SWITCH LVL:OIL LEVEL;-0 TO 80 DEG C;4 A","Each",4]
[null,"4.223","0662694","TRANSDUCER:LEVEL;I/P -5 TO 5 MA;240 V","Each",4]
[null,"4.224","0665601","TRANSDUCER:OIL LEVEL;I/P 0-1 BAR;240 V","Each",4]
[null,"4.225","0153883","GAUGE PRESS:250 KPA;63 MM;BSP;1/4 IN;SS","Each",4]
[null,"4.226","0236953","GAUGE PRESS:923431005;300 PSI;1/4 IN","Each",4]
[null,"4.227","0579219","GAUGE DP:0-5 KPA;MAIN BOARD CONNECTION","Each",4]
[null,"4.228","0583423","GAUGE PRESS:0-10 BAR;50 MM;R1/8 IN;SS;SS","Each",4]
[null,"4.229","0585002","GAUGE PRESS:232.30.100;0-10 BAR;101 MM","Each",4]
[null,"4.230","0616083","GAUGE PRESS:W123X160Q1600KJ;0-1600 KPA","Each",4]
[null,"4.231","0616845","GAUGE PRESS:0-10 MPA;160 MM;THD;G1/2 IN","Each",4]
[null,"4.232","0616846","GAUGE PRESS:0-2.5 MPA;160 MM;THD;G1/2 IN","Each",4]
[null,"4.233","0621760","GLASS LVL GAUGE:FLAT;PVC;BLACK","Each",4]
[null,"4.234","0621769","GAUGE PRESS:0-16 MPA;100 MM;BRS FORGED","Each",4]
[null,"4.235","0621770","GAUGE PRESS:0-4 MPA;100 MM;BRS FORGED","Each",4]
[null,"4.236","0622134","GAUGE PRESS:1KGZ056397;0-1200 KPA;100 MM","Each",4]
[null,"4.237","0622135","GAUGE PRESS:1KGZ056401;0-3 KPA;160 MM","Each",4]
[null,"4.238","0622136","GAUGE PRESS:IKGZ056402;0-5 KPA;160 MM","Each",4]
[null,"4.239","0622137","GAUGE PRESS:1KGZ056266;0-60 KPA;160 MM","Each",4]
[null,"4.240","0622138","GAUGE PRESS:1KGZ056265;-100 TO 300 KPA","Each",4]
[null,"4.241","0622139","GAUGE PRESS:1KGZ056267;0-100 KPA;160 MM","Each",4]
[null,"4.242","0622140","GAUGE PRESS:1KGZ056268;0-160 KPA;160 MM","Each",4]
[null,"4.243","0622141","GAUGE PRESS:1KGZ056269;0-400 KPA;160 MM","Each",4]
[null,"4.244","0622142","GAUGE PRESS:1KGZ056270;0-600 KPA;160 MM","Each",4]
[null,"4.245","0622143","GAUGE PRESS:1KGZ056271;0-1000 KPA;160 MM","Each",4]
[null,"4.246","0622144","GAUGE PRESS:1KGZ056272;0-1600 KPA;160 MM","Each",4]
[null,"4.247","0622146","GAUGE PRESS:1KGZ056400;0-120 KPA;160 MM","Each",4]
[null,"4.248","0622147","GAUGE PRESS:1KGZ056399;0-18 KPA;160 MM","Each",4]
[null,"4.249","0622148","GAUGE PRESS:1KGZ056321;0-25 KPA;160 MM","Each",4]
[null,"4.250","0622149","GAUGE PRESS:1KGZ056318;0-4 KPA;160 MM","Each",4]
[null,"4.251","0622150","GAUGE PRESS:1KGZ056398;0-700 KPA;160 MM","Each",4]
[null,"4.252","0622151","GAUGE PRESS:1KGZ056273;0-2500 KPA;160 MM","Each",4]
[null,"4.253","0622152","GAUGE PRESS:1KGZ056403;0-100 KPA;160 MM","Each",4]
[null,"4.254","0630013","VALVE:1KGZ020341;GAUGE;G1/2 IN;300 KPA","Each",4]
[null,"4.255","0630307","GAUGE PRESS:-100 TO 1500 KPA;79 MM;BSP","Each",4]
[null,"4.256","0630308","GAUGE PRESS:-100 TO 900 KPA;100 MM;BSP","Each",4]
[null,"4.257","0635118","SCREW:VORECON;GAUGE;M12;LG 75 MM;METRIC","Each",4]
[null,"4.258","0637198","GAUGE PRESS:0-600 KPA;160 MM;BSP","Each",4]
[null,"4.259","0637199","GAUGE PRESS:0-250 KPA;160 MM;BSP","Each",4]
[null,"4.260","0637200","GAUGE PRESS:0-1000 KPA;160 MM;BSP","Each",4]
[null,"4.261","0637201","GAUGE PRESS:0-400 KPA;160 MM;BSP","Each",4]
[null,"4.262","0637202","GAUGE PRESS:0-100 KPA;150 MM;BSP","Each",4]
[null,"4.263","0637203","GAUGE PRESS:0-1600 KPA;150 MM;BSP","Each",4]
[null,"4.264","0638275","GAUGE PRESS:0-200 KPA;160 MM;NPT","Each",4]
[null,"4.265","0638276","GAUGE PRESS:0-2000 KPA;160 MM;NPT","Each",4]
[null,"4.266","0641173","GAUGE PRESS:0-3 KPA;77 MM;NPT;2.5 MM","Each",4]
[null,"4.267","0642137","GLASS LVL GAUGE:700072;DIA 254 MM;OIL;AL","Each",4]
[null,"4.268","0642541","GAUGE PRESS:0-25 BAR;BRS;CYLINDER","Each",4]
[null,"4.269","0642817","GAUGE PRESS:233.50.160;0-4000 KPA;161 MM","Each",4]
[null,"4.270","0643251","GAUGE PRESS:W199010WG/XSX4","Each",4]
[null,"4.271","0643545","GAUGE PRESS:233.30.100","Each",4]
[null,"4.272","0644175","GAUGE PRESS:233.50.100(0-60BAR)","Each",4]
[null,"4.273","0644176","GAUGE PRESS:233.50.100(0-10BAR)","Each",4]
[null,"4.274","0644177","GAUGE PRESS:233.50.100(0-6BAR)","Each",4]
[null,"4.275","0644178","GAUGE PRESS:233.50.100(0-25BAR)","Each",4]
[null,"4.276","0644179","GAUGE PRESS:233.50.100(0-600BAR)","Each",4]
[null,"4.277","0644180","GAUGE PRESS:233.50.100(0-250BAR)","Each",4]
[null,"4.278","0646047","GAUGE PRESS:TCR.42014770","Each",4]
[null,"4.279","0646127","GAUGE PRESS:272.2.20.1.1.160.2.1","Each",4]
[null,"4.280","0646129","GAUGE PRESS:271B","Each",4]
[null,"4.281","0646180","GAUGE PRESS:233.30.160","Each",4]
[null,"4.282","0646181","GAUGE PRESS:433.50.160","Each",4]
[null,"4.283","0646182","GAUGE PRESS:271/5/40/1/1/215/8/A","Each",4]
[null,"4.284","0648968","GAUGE PRESS:0-250 KPA;100 MM;G1/2B IN;SS","Each",4]
[null,"4.285","0648969","GAUGE PRESS:0-1000 KPA;100 MM;SCREW;AL","Each",4]
[null,"4.286","0653244","GAUGE, PRESSURE","Each",4]
[null,"4.287","0653245","GAUGE, PRESSURE","Each",4]
[null,"4.288","0653246","GAUGE, PRESSURE","Each",4]
[null,"4.289","0653247","GAUGE, PRESSURE","Each",4]
[null,"4.290","0653248","GAUGE, PRESSURE","Each",4]
[null,"4.291","0653602","GAUGE, PRESSURE:RNGE 0-25 BAR","Each",4]
[null,"4.292","0654707","GAUGE, PRESSURE:RNGE 0-4 MPA","Each",4]
[null,"4.293","0655318","GAUGE, PRESSURE:SPEC SF6","Each",4]
[null,"4.294","0655973","GAUGE, PRESSURE:0-1600 BAR;DIAL 160 MM","Each",4]
[null,"4.295","0655991","GAUGE, PRESSURE","Each",4]
[null,"4.296","0661456","GAUGE PRESS:0-1200 KPA;100 MM;G1/2B;SS","Each",4]
[null,"4.297","0662400","GAUGE PRESS:0-600 KPA;100 MM;STL;STL;STL","Each",4]
[null,"4.298","0662401","GAUGE PRESS:0-6000 KPA;201 MM;STL;STL","Each",4]
[null,"4.299","0662541","GAUGE PRESS:0-60 KPA;10 MM;STL;STL;STL","Each",4]
[null,"4.300","0662542","GAUGE PRESS:0-6000 KPA;100 MM;STL;STL","Each",4]
[null,"4.301","0662543","GAUGE PRESS:0-1600 KPA;100 MM;STL;STL","Each",4]
[null,"4.302","0662579","GAUGE PRESS:0-1700 KPA;100 MM;STL;STL","Each",4]
[null,"4.303","0662648","GAUGE PRESS:0-1700 KPA;100 MM;STL;STL","Each",4]
[null,"4.304","0662683","GAUGE PRESS:0-600 KPA;10 MM;SS 316","Each",4]
[null,"4.305","0662729","GAUGE PRESS:0-6000 KPA;100 MM;STL;STL","Each",4]
[null,"4.306","0662735","GAUGE PRESS:0-1700 KPA;200 MM;SS 316","Each",4]
[null,"4.307","0665477","GAUGE PRESS:-1 TO 5 BAR;200 MM;BSP","Each",4]
[null,"4.308","0665714","GAUGE PRESS:0-10 BAR;100 MM;SCREW THREAD","Each",4]
[null,"4.309","0670122","GAUGE PRESS:0-100 KPA;77 MM;BSP;1/4 IN","Each",4]
[null,"4.310","0670124","GAUGE PRESS:0-10 MPA;77 MM;BSP;1/4 IN;SS","Each",4]
[null,"4.311","0670125","GAUGE PRESS:0-10 KPA;100 MM;BSP;1/4 IN","Each",4]
[null,"4.312","0670126","GAUGE PRESS:0-1 MPA;101 MM;BSP;1/2 IN;SS","Each",4]
[null,"4.313","0670127","GAUGE PRESS:0-1 KPA;90 MM;BSPP;1/2 IN;SS","Each",4]
[null,"4.314","0684694","GAUGE PRESS:0-400 BAR;100 MM;G1/2B IN","Each",4]
[null,"4.315","0242189","DETECTOR RT:TSP131;DUAL;-50 TO 400 DEG C","Each",4]
[null,"4.316","0574050","DETECTOR RT:G RX96-.3-80-FM-100-C-4F4S","Each",4]
[null,"4.317","0574872","DETECTOR:TC806B1076;SMOKE;57 DEG C","Each",4]
[null,"4.318","0580207","DETECTOR RT:TMT122-A31BBA;0-150 DEG C","Each",4]
[null,"4.319","0580209","DETECTOR RT:TMT122-A41BBA;RTD-PT100;3","Each",4]
[null,"4.320","0580280","DETECTOR RT:DUPLEX RTD PT-100;3;NO","Each",4]
[null,"4.321","0580281","DETECTOR RT:SIMPLEX RTD-PT100;3;NO","Each",4]
[null,"4.322","0611051","DETECTOR RT:TLSR1-Y8D11H2;PT100;300;2","Each",4]
[null,"4.323","0611052","DETECTOR RT:PT100;-200 TO 600 DEG C;299","Each",4]
[null,"4.324","0649307","TRANSMITTER FLW:ELECTROMAGNETIC INDUCTOR","Each",4]
[null,"4.325",621509,"Pressure transmitter integrated LCD display","Each",4]
[null,"4.326","0622174","VEGAFLEX 81, coax 2000mm ","Each",4]
[null,"4.327","0622283","266GST-D-20600-S2E0-S0A1","Each",4]
[null,"4.328","0622297","266MST-D-410-12500-S2E0-S0","Each",4]
[null,"4.329","0622217","266MST-D-410-20020-S2E0-S0","Each",4]
[null,"4.330","0622284","266MST-D-410-20100-S2E0-S0","Each",4]
[null,"4.331","0622212","266AST-D-12500-S2E0-S0A1","Each",4]
[null,"4.332","0622298","266GST-D-10400-S2E1-S0A1","Each",4]
[null,"4.333","0622302","266GST-D-12500-S2E1-S0A1","Each",4]
[null,"4.334","0629910","US sensor DN50 - DN400","Each",4]
[null,"4.335","0629961","US sensor DN200-DN4000","Each",4]
[null,"4.336","0622173","US transmitter UFC300W","Each",4]
[null,"4.337","0622218","Vegabar 86, 4m ","Each",4]
[null,"4.338","0622222","Vegabar 86, 6m ","Each",4]
[null,"4.339","0622365","Vegabar 86, 10m ","Each",4]
[null,"4.340","0622175","VEGAFLEX 81, coax 1100mm ","Each",4]
[null,"4.341","0622176","VEGASON 62, G2 ","Each",4]
[null,"4.342","0622208","Temp Transmitter TTR200 SIL2","Each",4]
[null,"4.343","0622207","Temp Transmitter TTR200 SIL2, Ex i","Each",4]
[null,"4.344","0622221","266GST-D-10060-S2E0-S0A1","Each",4]
[null,"4.345","0622220","266GST-D-10400-S2E0-S0A1","Each",4]
[null,"4.346","0622295","266GST-D-12500-S2E0-S0A1","Each",4]
[null,"4.347","0622296","266GST-D-20010-S2E0-S0A1","Each",4]
[null,"4.348","0622219","266GST-D-20030-S2E0-S0A1","Each",4]
[null,"4.349","0622282","266GST-D-20100-S2E0-S0A1","Each",4]
[null,"4.350","0622288","266MST-D-160-10060-S2E0-S0","Each",4]
[null,"4.351","0622287","266MST-D-160-10400-S2E0-S0","Each",4]
[null,"4.352","0622226","266MST-D-160-12500-S2E0-S0","Each",4]
[null,"4.353","0622303","266MST-D-160-20020-S2E0-S0","Each",4]
[null,"4.354","0622367","266MRT-D-160-10400-S2E0-S0","Each",4]
[null,"4.355","0622366","266GRT-D-20010-S2E0-S1A0","Each",4]
[null,"4.356","0622211","266GRT-D-20100-S2E0-S1A0","Each",4]
[null,"4.357","0622225","266GRT-D-20100-S2E0-S1A0-D","Each",4]
[null,"4.358","0622224","266GRT-D-12500-S2E0-S1A0-D","Each",4]
[null,"4.359","0622223","266GDT-D-10400-S2E0-S0A1-D","Each",4]
[null,"4.360","0622285","266GDT-D-12500-S2E0-S0A1-D","Each",4]
[null,"4.361","0622286","266GDT-D-10400-S2E0-S0A1-3","Each",4]
[null,"4.362","0622294","266GDT-D-12500-S2E0-S0A1-3","Each",4]
[null,"4.363","0622214","266GRT-D-10400-S2E0-S1A0-3","Each",4]
[null,"4.364","0622213","266GRT-D-20010-S2E0-S1A0-3","Each",4]
[null,"4.365","0622368","266GRT-D-20030-S2E0-S1A0-3","Each",4]
[null,"4.366","0622210","266GRT-D-20010-S2E0-S0A1-1","Each",4]
[null,"4.367","0622209","266GRT-D-20010-S2E0-S0A1-1","Each",4]
[null,"4.368","0622370","266GRT-D-20030-S2E0-S0A1-1","Each",4]
[null,"4.369","0622215","266GDT-D-10400-S2E0-S0A1-D","Each",22]
[null,"4.370","0622216","266GDT-D-12500-S2E0-S0A1-D","Each",22]
[null,"4.371","0622369","266GRT-D-20030-S2E0-S0A1-D","Each",22]
[null,"4.372","0622304","266GDT-D-12500-S2E0-S0A1-4","Each",22]
[null,"4.373","0622000","THERMOSTAT 0/+60C 250VAC CONTACT NC","Each",22]
[null,"4.374","0502852","THERMOSTAT 20/+80°C 250VAC TYPE K TS011 1 CONTACT NO","Each",22]
[null,"4.375","0693018","SOLICAP M FTI56 CAPACITIVE PROBE ROPE","Each",22]
[null,"4.376","0696522","TEMPERATURE CONTROLLER THERMOCOUPLE","Each",22]
[null,"4.377","0653278","METER, FLOW","Each",22]
[null,"4.378","0653279","METER, FLOW:INDICATOR","Each",22]
[null,"4.379","0653281","TRANSMITTER, FLOW:INDICATOR","Each",22]
[null,"4.380","0653346","INDICATOR, SIGHT FLOW","Each",22]
[null,"4.381","0653350","TRANSMITTER, FLOW:INDICATOR","Each",22]
[null,"4.382","0659029","METER, FLOW:ELECTROMAGNETIC;0.5 PCT","Each",22]
[null,"4.383","0659030","METER, FLOW:THERMAL MASS;MTRL CAST AL","Each",22]
[null,"4.384","0659031","METER, FLOW:ELECTROMAGNETIC;MTRL AL","Each",14]
[null,"4.385","0665670","INDICATOR SGHT FLW:FLOW METER;LIQUID/GAS","Each",22]
[null,"4.386","0659033","METER, FLOW:ELECTROMAGNETIC;MTRL AL","Each",17]
[null,"4.387","0659034","TRANSMITTER, FLOW:ULTRASONIC;24 VDC","Each",22]
[null,"4.388","0659035","TRANSMITTER, FLOW:WATER FLOW;PN40","Each",22]
[null,"4.389","0659036","TRANSMITTER, FLOW:LIQUID;O/P 4-20 MA","Each",19]
[null,"4.390","0644654","TRANSMITTER LVL:82;0-1750 MM;O/P 4-20 MA","Each",22]
[null,"4.391","0653272","TRANSMITTER TEMP:AUXILIARY BOILER","Each",21]
[null,"4.392","0645212","TRANSMITTER LVL:CAPACITIVE LEVEL PROBE","Each",12]
[null,"4.393","0621772","TRANSMITTER LVL:0-400 MM;O/P 0-20 MA","Each",4]
[null,"4.394","0646408","TRANSMITTER FLW","Each",9]
[null,"4.395","0620127","TRANSMITTER FLW:53P1F-EAGB1AAOAAAA","Each",14]
[null,"4.396","0653348","TRANSMITTER LVL:INIDCATOR","Each",4]
[null,"4.397","0653350","TRANSMITTER FLW:INDICATOR","Each",6]
[null,"4.398","0653281","TRANSMITTER FLW:INDICATOR","Each",5]
[null,"4.399","0645203","TRANSMITTER TEMP","Each",16]
[null,"4.400","0700054","Endress+Hauser FTL51-6VP9/0 Liquiphant M FTL51","Each",4]
[null,"4.401","0695861","TRANSMITTER TEMPERATURE ","Each",17]
[null,"4.402","0695259","TRANSMITTER TEMPERATURE","Each",4]
[null,"TOTAL AMOUNT"]