{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"merged":[[1,2,7,2],[2,3,4,3],[5,4,7,4],[6,1,7,1],[9,2,16,2],[9,4,16,4],[13,0,16,1]]}
["Standards","Classification of equipment","Emissions - EMI (Electromagnetic Interference)\nImmunity - EMS\n(Electromagnetic Susceptibility)","Methods","Electricity Meters specific test requirement"]
["SANS 211","Industrial, Scientific and Medical Equipment","Emissions (EMI)","Conducted emissions","Not applicable"]
["SANS 213","Sound and Television and associted Equipment",null,"Radiated emissions","Not applicable"]
["SANS 214-1","Household Appliances, Electric tools and similar Equipment",null,null,"Not applicable"]
["SANS 222","Information Technology Equipment",null,null,"Test setup and test to eb done as per the requirements of IEC 62052-11:2003 clause 9.3"]
["SANS 2332","Multimedia Equipment \n(Note: This is a new standard that combines SANS 213 and SANS 222)",null,"Conducted and radiated emissions","Test setup and test to eb done as per the requirements of IEC 62052-11:2020 clause 9.3"]
["SANS 61000-3-2","Electrical and Electronic equipment having an input of up to and including 16A per phase, and intrended to be connected to public low-voltage distribution system of between 220V and 250V line to neutral at 50Hz",null,"Harmonic current emissions"]
["SANS 61000-3-3",null,null,"Voltage fluctuations and flicker"]
["Immunity main standards covering SANS 61000-4 series",null,null,"SANS 61000-4 Series standards"]
["SANS 214-2","Household Appliances, Electric tools and similar Equipment","Immunity (EMS)","SANS 61000-4-2 (Electrostatic Discharge)","Test setup and test to eb done as per the requirements of SANS/IEC 62052-11:2020 clause 9.3"]
["SANS 2200","Sound and Television and associted Equipment",null,"SANS 61000-4-3 (Radiate, radio frequency, electromagnetic field immunity test"]
["SANS 224","Information Technology Equipment",null,"SANS 61000-4-4 (Electrical Fast Transient)"]
["SANS 2335","Multimedia Equipment\n(Note: This is a new standard that combines SANS 2200 and SANS 224)",null,"SANS 61000-4-5 (Surge)"]
[{"$nulls":3},"SANS 61000-4-6 (Immunity to conducted disturbances, induced by radio-frequency fields)"]
[{"$nulls":3},"SANS 61000-4-8 (Power frequency magnetic field)"]
[{"$nulls":3},"SANS 61000-4-9 (Pulse magnetic field)"]
[{"$nulls":3},"SANS 61000-4-11 (Voltage dips, short interruptions and voltage variations)"]