{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Blink BOQ"],"read":"whole","date_system":"1900"}

{"sheet":"Blink BOQ","index":0,"n_rows":89,"n_cols":11,"rows_kept":89,"merged":[[0,1,0,10]]}
[null,"THE SUPPLY OF TESTING and SUBMITTING OF ENGINEERING SOILS LABORARORY TEST RESULTS - CONSTRUCTION SERVICES - CIVILS PORTFOLIO"]
[null,"",null,"",null,"Net","Net","Mark-up%","Mark-up%"]
["Level","Item","Bill DESCRIPTION","Unit","Bill quantity","Rate","Amount","%","Type","Rate","Amount"]
[]
[]
[1,null,"THE SUPPLY OF TESTING and SUBMITTING OF ENGINEERING SOILS LABORARORY TEST RESULTS - CONSTRUCTION SERVICES - GENERATION AND TRANSPORTATION.\n1) The supply of personnel, test equipment and transport as per  G&T required tests. \n2) Test procedures to comply to the relevant specified SANS, COLTO and TRH procedures.\n2) Supplier to comply to all Eskom SHEQ standards and requirements at all times. \n3) To contact Bester du Buisson for information, direction and before delivery is made.  \n5) Laboratory vehicle to comply to all relevant Eskom and site specifications and regulations","",null,null,4910437.22,null,""]
[]
[null,"1.1"," Supply of Site Personnel as per specified requests / instructions: Transport","per km",428050]
[null,"1.2"," Supply of Site Personnel as per specified requests / instructions: Manager","per hour",2500]
[null,"1.3"," Supply of Site Personnel as per specified requests / instructions: Technician","per hour",5750]
[null,"1.4"," Supply of Site Personnel as per specified requests / instructions: Assistant Materials Tester","per hour",30250]
[null,"1.5"," Supply of Site Personnel as per specified requests / instructions: Field Team","per hour",17500]
[null,"1.6"," Supply of Site Personnel as per specified requests / instructions: Drilling time","per hour",5503]
[null,"1.7"," Supply of instructed / specified soil tests: In-situ dry density sand replacement test.","per test",20000]
[null,"1.8"," Supply of instructed / specified soil tests: In-situ dry density nuclear method.","per test",55220]
[null,"1.9"," Supply of instructed / specified soil tests: Sieve analysis to 0.075mm","per test",15000]
[null,"2.0"," Supply of instructed / specified soil tests:  Sieve analysis to 0.075mm – including Atterberg Limits","per test",15025]
[null,"2.1"," Supply of instructed / specified soil tests:  Atterberg Limits","per test",15000]
[null,"2.2"," Supply of instructed / specified soil tests:  Foundation Indicator","per test",1000]
[null,"2.3"," Supply of instructed / specified soil tests:  Preparation of fines","per test",11000]
[null,"2.4"," Supply of instructed / specified soil tests:  Mod AAHSTO (unstabilized)","per test",30125]
[null,"2.5"," Supply of instructed / specified soil tests:  Standard Proctor (unstabilized)","per test",30000]
[null,"2.6"," Supply of instructed / specified soil tests:  Mod AAHSTO (stabilized)","per test",30015]
[null,"2.7"," Supply of instructed / specified soil tests:  Standard Proctor (stabilized)","per test",30000]
[null,"2.8"," Supply of instructed / specified soil tests:  Unstabilized CBR (Mod excluded)","per test",20008]
[null,"2.9"," Supply of instructed / specified soil tests:  Stabilized CBR (Mod excluded)","per test",20000]
[null,"3.0"," Supply of instructed / specified soil tests:  UCS","per briquette",17515]
[null,"3.1","Supply of instructed / specified concrete tests: Making of cubes on site, test for slump, 6 cubes (excluding establishment and cube test)","per test",25184]
[null,"3.2","Supply of instructed / specified concrete tests:  test for slump, 6 cubes (excluding establishment and cube test) and curing of cubes",null,"25184"]
[null,"3.3","Supply of instructed / specified concrete tests: Compressive strength of concrete cubes (6 cubes)","per test",25184]
[null,"3.4","Supply of instructed / specified concrete tests: Compressive strength of bricks","per test",3500]
[null,"3.5","Supply of instructed /specified aggregate tests: Aggregate Crushing Value (dry) ","per test",2500]
[null,"3.6","Supply of instructed /specified aggregate tests: 10% Aggregate Crushing Value (dry)","per test",2000]
[null,"3.7","Supply of instructed /specified aggregate tests: Flakiness index of aggregate (dry)","per test",2000]
[null,"3.8","Supply of instructed /specified aggregate tests: Sieve analysis of aggregate to 0.075mm","per test",2000]
[null,"3.9","Supply of instructed /specified aggregate tests: Relative density of aggregate","per test",15000]
[null,"4.0","Supply of instructed /specified aggregate tests: Collapse Potential Rapid Test (including RD)","per test",600]
[null,"4.1","Supply of instructed /specified aggregate tests: Relative Density of Soil","per test",15000]
[null,"4.2","Supply of instructed /specified aggregate tests: Moisture Content","per test",18000]
[null,"4.3","Supply of instructed /specified aggregate tests: Drilling of concrete cores 0 - 100mm OD","per drill","10166"]
[null,"4.4","Supply of instructed /specified aggregate tests: Drilling of concrete cores 100- 150mm OD","per drill","10166"]
[null,"4.5","Supply of instructed /specified aggregate tests: Drilling of concrete cores 150 -200mm OD","per drill","10166"]
[null,"4.6","Supply of instructed /specified aggregate tests: DCP to 1.0m (natural ground)","per test",15000]
[null,"4.7","Supply of instructed /specified aggregate tests: DCP to 2.0m (natural ground)","per test",15000]
[null,"4.8","Supply of instructed /specified aggregate tests: Concrete mix design (existing design)","per design",100]
[null,"4.9","Supply of instructed /specified aggregate tests: Marshal Control of 3 Briquettes","per test",7500]
[null,"5.0","Supply of instructed /specified aggregate tests: Bulk Relative Density (asphalt)","per test",2500]
[null,"5.1","Supply of instructed /specified aggregate tests: Determine of Rice's Relative Density (MTRD)","per test",750]
[null,"5.2","Supply of instructed /specified aggregate tests: Binder Content","per test",7500]
[null,"5.3","Supply of instructed /specified aggregate tests: Compaction of 3 Asphalt Briquette (Marshal)","per test",7500]
[null,"5.4","Supply of instructed /specified aggregate tests: Binder Content of Slurry Seal","per test",7500]
[null,"5.5","Supply of instructed /specified aggregate tests: Asphalt Control (Full Marshal)","per test",750]
[null,"5.6","Supply of instructed /specified aggregate tests: Indirect Tensile Strength on Asphalt","per Briq",7500]
[null,"5.7","Supply of instructed /specified aggregate tests: Drilling of 100mm Asphalt Cores <75mm","per test",7500]
[null,"5.8","Supply of instructed /specified aggregate tests: Drilling of 100mm Asphalt Cores 75 - 150mm","per test",1500]
[null,"5.9","Supply of instructed /specified aggregate tests: Indirect Tensile Strength on Asphalt","per test",500]
[null,"6.0","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Thickness","per test",12]
[null,"6.1","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Asperity Height (ASTM D5994)","per test",12]
[null,"6.2","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Density (ASTM D7466)","per test",12]
[null,"6.3","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Tensile Properties (ASTM D1505)","per test",12]
[null,"6.4","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Tensile Properties (ASTM D6693)","per test",12]
[null,"6.5","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Stress Crack (ASTM D5397)","per test",12]
[null,"6.6","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Carbon Content (ASTM D1603)","per test",12]
[null,"6.7","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Carbon Dispersion (ASTM D1603)","per test",12]
[null,"6.8","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Oxidative Industion Time 100 Minutes (ASTM D3895)","per test",12]
[null,"6.9","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - HP Oxidative Industion Time 400 Minutes (ASTM D5885)","per test",12]
[null,"7.0","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - Oven Aging w/ OIT & HPOIT, Baseline / Post-Exposure - 90 Days (ASTM D5721)","per test",12]
[null,"7.1","Supply of instructed / Specified Material Conformance Testing for HDPE Liner - QUV Resistance(ASTM D7238)","per test",12]
[null,"7.2","Transportation or Shipping of HDPE Liner to 3rd Party Lab","per trip",12]
[null,"7.3","Laboratory establishment","each",50]
[null,"7.4","Laboratory de-establishment","each",50]
[null,"7.5","Laboratory rental ","per month",44]
[null,"7.6","Accomodation Per Laboratory Personnel","per night",100]
[null,"7.7","Electrical Leak Location Survey for HDPE Liner","per m2",180000]
[null,"7.8","Full material classification","each",500]
[null,"7.9","Earth resitivity","each",200]
[null,"8.0","Thermal conductivity ","each",200]
[null,"8.1","Rebound hammer test","each",500]
[null,"8.2","Rental of equipment: DCP Hammer","per day",930]
[null,"8.3","Rental of equipment: Troxler","per day",930]
[null,"8.4","Rental of equipment: Cube moulds & Curing bath","per day",930]
[null,"8.5","Rental of equipment: Sample bags, Slump test cone & plate","per day",930]
[null,"8.6","Rental of equipment: Sample bags","per day",930]
[]
[null,null,"Sub total"]
[]
[null,null,"Value Added Tax (15%)"]
[]
[null,null,"GRAND TOTAL"]