{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":111,"n_cols":10,"rows_kept":111,"merged":[[1,4,1,5],[1,6,1,7],[1,8,1,9]]}
[]
[{"$nulls":4},"Year 1",null,"Year 2",null,"Year 3"]
[null,"list","Description","QTY","Unit price","Total Price","Unit price","Total Price","Unit price","Total Price"]
[null,null,"DOUGHNUT SEALS"]
[null,1,"20ID x 45OD x 17",2000]
[null,2,"ID 20 X OD 45 MM;RUBBER",2000]
[null,3,"ID 22 X OD 52 MM",2000]
[null,4,"ID 30 X OD 55 MM",2000]
[null,5,"42ID x 66OD x 25",2000]
[null,6,"42ID X 66OD X25 THICK",2000]
[null,7,"42ID X 86 OD x 30",2000]
[null,8,"ID 42 X OD 95 X THK 33 MM",2000]
[null,9,"54ID X 78OD x 18",2000]
[null,10,"56ID X 86OD X 32 THICK",2000]
[null,11,"30ID X 55OD x 25",2000]
[null,12,"46ID X 75OD x 28",2000]
[null,13,"ID 42 X OD 95 X THK 33 MM",2000]
[null,14,"ID 38 X OD 75 MM;VITON",2000]
[null,15," ID 55 X OD 95 X THK 33 MM",2000]
[null,16,"ID90 X OD116 X THK25.5 MM",2000]
[null,null,"CONICAL SEALS"]
[null,17,"SEAL:CONICAL;ID 10 X OD 18 X LG 18 MM",1500]
[null,18,"SEAL:CONICAL;ID12XOD17/29XLG19 MM",1500]
[null,19,"SEAL:CONICAL;ID16XOD22/40XLG19 MM",1500]
[null,20,"SEAL:CONICAL;IS20XOD24/40XLG19 MM",1500]
[null,21,"SEAL:CONICAL;ID25XOD32/48XLG17 MM",1500]
[null,22,"CONICAL SEAL 12x35x25mm",1500]
[null,23,"CONICAL SEAL 10x30x21mm",1500]
[null,24,"CONICAL SEAL 16x40x27mm",1500]
[null,25,"CONICAL SEAL 30x55x25mm",1500]
[null,null,"Triangular Ring Seal, Material: Viton, Colour: Black, Hardness: 90"]
[null,26,"3 INCH COUPLING (Set of 2)",2000]
[null,27,"8 INCH COUPLING (Set of 2)",2000]
[null,null,"O-RING, Material: Nitrile Butadiene Rubber, Hardness: 70"]
[null,28,"O RING Cord 6mm x 50m",3000]
[null,29,"O RING Cord 8mm x 50m",3000]
[null,30,"O RING Cord 10mm x 50m",3000]
[null,31,"O-RING NITRILE 6mm x 10m",3000]
[null,32,"O-RING NITRILE 8mm x 10m",3000]
[null,33,"O-RING NITRILE 10mm x 10m",3000]
[null,34,"O-RING ID90mm x 10mm THICK",5000]
[null,35,"O-RING 84.3x5.7",5000]
[null,36,"QUATRO RADIATOR O-RING",5000]
[null,37,"O-RING KIT METRIC -QUANTITY: 386; MATERIAL: NBR 70; SIZE RANGE: 3 - 44 MM",2000]
[null,38,"O-RING KIT IMPERIAL-QUANTITY: 386; MATERIAL: NBR 70; SIZE RANGE: 3 - 44 MM",2000]
[null,39,"SEAL: TYPE: UPPER GEAR “O” RINGS",2000]
[null,40,"O-RING  OD 102mmx6mm",2000]
[null,null,"SQUARE RUBBER"]
[null,41,"SEAL: MARSHALLING KIOSK DOORS, CUBICLES & TERMINAL BOXES SEAL:ACCESS PANEL;WD 20 X HT 15 MM",2000]
[null,42,"SEAL 12mm X 12mm SQUARE RUBBER",2000]
[null,null,"Washers: Flat, Type: Ring Material: Polytetrafluoroethylene, Application: transformer radiator bleed/drain nippples, Temp -200 deg to +260 deg Celcius, Dimensions: ID x OD x Thk in mm"]
[null,43,"GASKET, RADIATOR 25 X 30 X 3 PTFE RADIATOR PLUG",2000]
[null,44,"GASKET, RADIATOR 24 X 16 X 3 PTFE RADIATOR PLUG",2000]
[null,45,"GASKET, RADIATOR 28 X 21 X 3 PTFE RADIATOR PLUG",2000]
[null,46,"GASKET, RADIATOR 38 X 29 X 3 PTFE RADIATOR PLUG",2000]
[null,47,"GASKET, RADIATOR 35 X 26 X 3 PTFE RADIATOR PLUG",2000]
[null,48,"GASKET SET:PTFE 40 X 27 X 3;RADIATOR",2000]
[null,49,"GASKET, RADIATOR 36 X 26 X 3 PTFE RADIATOR PLUG",2000]
[null,50,"GASKET, RADIATOR 31 X 23 X 3 PTFE RADIATOR PLUG",2000]
[null,51,"GASKET:RADIATOR;33 X 26 X 3;PTFE",2000]
[null,52,"GASKET:RADIATOR;31 X 21 X 3 MM;PTFE",2000]
[null,53,"GASKET, RADIATOR 37 X 25 X 3 PTFE RADIATOR PLUG",2000]
[null,null,"VALVE PACKING GRAPHITE"]
[null,54,"VALVE PACKING 10MM X 10M",1500]
[null,55,"VALVE PACKING 8MM X 10M",1500]
[null,56,"VALVE PACKING 6MM X 10M",1500]
[null,57,"VALVE PACKING 4MM X 10M",1500]
[null,null,"VALVE PACKING ACRYLIC PTFE"]
[null,58,"VALVE PACKING 10MM X 8M",1500]
[null,59,"VALVE PACKING 8MM X 8M",1500]
[null,60,"VALVE PACKING 6MM X 8M",1500]
[null,61,"VALVE PACKING 4MM X 8M",1500]
[null,62,"O RING CRD:PTFE;THK 4 MM;LG 10.7 M 5/32 in X35 ft",3000]
[null,null,"Various"]
[null,63,"SEALANT:GASKET MAKER;TUBE;SILICON;RED 300 deg",1000]
[null,64,"TOOL:SILICON GUN;HAND",1000]
[null,65,"Klingersil C4400 sheet",1000]
[null,66,"Klingersil C4400 Cutting tool",1000]
[null,67,"Manufacture Transformer Seals and Gaskets",10000]
[null,68,"TAPCHANGER DOOR SEAL",1000]
[null,69,"COMPOUND SEALG: DOWSIL 888; GRAY JOINT SILICON",1000]
[null,null,"Transformer Bushings Seals"]
[null,70,"SEAL:ALB2 CONE;M12",1100]
[null,71,"SEAL:H CONE;M36;AVS-VERI SEAL",1100]
[null,72,"SEAL:H CONE;M18;NITRILE BUTADIENE RUBBER",1100]
[null,73,"SEAL:H CONE;M30;NITRILE BUTADIENE RUBBER",1100]
[null,74,"SEAL:CONE;M16;NITRILE BUTADIENE RUBBER",1100]
[null,75,"SEAL:NB CONE;M8;NITRILE BUTADIENE RUBBER",1100]
[null,76,"SEAL:H CONE;M36;NITRILE BUTADIENE RUBBER",1100]
[null,77,"SEAL:H CONE;M12;AVS-VERI SEAL",1100]
[null,78,"SEAL:H CONE;M20;AVS-VERI SEAL",1100]
[null,79,"SEAL:H CONE;M12;NITRILE BUTADIENE RUBBER",1100]
[null,80,"SEAL:NB CONE;M8;AVS-VERI SEAL",1100]
[null,81,"SEAL:H CONE;M10;NITRILE BUTADIENE RUBBER",1100]
[null,82,"SEAL:ALB2 CONE;M12;AVS-VERI SEAL",1100]
[null,83,"SEAL:GAL;M20;NITRILE BUTADIENE RUBBER",1100]
[null,84,"SEAL:H CONE;M24;AVS-VERI SEAL",1100]
[null,85,"SEAL:NB CONE;M6;NITRILE BUTADIENE RUBBER",1100]
[null,86,"SEAL:ALB1 CONE;M12",1100]
[null,87,"SEAL:H CONE;M30;AVS-VERI SEAL",1100]
[null,88,"SEAL:H CONE;M20;NITRILE BUTADIENE RUBBER",1100]
[null,89,"SEAL:H CONE;M42;NITRILE BUTADIENE RUBBER",1100]
[null,90,"SEAL:H CONE;M24;NITRILE BUTADIENE RUBBER",1100]
[null,91,"SEAL:H CONE;M14;AVS-VERI SEAL",1100]
[null,92,"SEAL:H CONE;M42;AVS-VERI SEAL",1000]
[null,93,"SEAL:ALB1 CONE;M12;AVS-VERI SEAL",1000]
[null,94,"SEAL:H CONE;M18;AVS-VERI SEAL",1100]
[null,95,"SEAL:H CONE;M10;AVS-VERI SEAL",1100]
[null,96,"SEAL:H CONE;M14;NITRILE BUTADIENE RUBBER",1109]
[]
[null,null,"Total",null,null,{"$f":"SUM(F5:F109)","v":{"v":0,"d":"R0"}},null,{"$f":"SUM(H5:H109)","v":{"v":0,"d":"R0"}},null,{"$f":"SUM(J5:J109)","v":{"v":0,"d":"R0"}}]