{"text_format":"3","workbook":"xlsx","n_sheets":16,"sheets":["P&G","Mechanical","Mechanical 2","Electrical","Electrical 2","Electrical 3","Electrical 4","Electrical 5","Electrical 6","Electrical 7","Electrical 8","Electrical 9","Building","Building 2","OHS","Summary"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"P&G","index":0,"n_rows":93,"n_cols":7,"rows_kept":93,"merged":[[0,0,0,2],[1,0,1,6],[2,0,2,5],[4,3,4,6],[5,3,5,6],[53,3,53,6],[77,3,78,6],[92,0,92,5]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL A:  Preliminary & General"]
["Item","Pay Ref","Description","Unit","Qty","Rate","Amount"]
[null,"SANS","Schedule 1"]
[null,1200,"Preliminary and general"]
[1.1,null,"Fixed charge items"]
["1.1.1","A8.3.1","Contractual requirements","sum",1]
[null,null,"affecting the Contractor"]
[null,"A8.3.2","The Contractor to provide "]
[null,null,"the following "]
[null,null,"items or as amended in the"]
[null,null,"Tender Document :"]
["1.1.2","PSAB 3.1","Name board (2 number) as","sum",1]
[null,null,"specified in the Tender"]
[null,null,"Document"]
["1.1.3","PSA8.3.2.1","Furnished office for the","sum",1]
[null,null,"Engineer's use"]
[null,"PSAB3.2"]
["1.1.4","PSAB 5.5","Survey assistant as & when","sum",1]
[null,null,"required by the Engineer"]
["1.1.5","PSAB 5.6","Survey equipments as & when","sum",1]
[null,null,"required by the Engineer"]
["1.1.6","PSAB4","Telephone facilities for the","Prov",1,{"v":26000,"d":"26,000.00"},{"v":26000,"d":"26,000.00"}]
[null,null,"Engineer"]
["1.1.7","PSAB5.7","Personnel computer & digital","sum",1]
[null,null,"camera"]
["1.1.8","A8.3.2.2a","Offices & storage facilities for","sum",1]
[null,null,"the Contractor"]
["1.1.9","A8.3.2.2b","Workshops for the Contractor","sum",1]
[null,null,"as required by The Contract"]
["1.1.10","A8.3.2.2d","Living accommodations for the","sum",1]
[null,null,"Contractor's personnel"]
["1.1.11","A8.3.2.2e","Ablution & latrine facilities for","sum",1]
[null,null,"the Contractor's personnel"]
["1.1.12","A8.3.2.2f","Supply tools & equipment’s as","sum",1]
[null,null,"required by The Contract"]
["1.1.13","A8.3.2.2g","Water, electricity &","sum",1]
[null,null,"communications as required"]
[null,null,"by The Contract"]
[null,null,"Other obligations by the "]
[null,null,"Contractor :"]
["1.1.14","A8.3.2.2h","Deal with rain and/or ground ","sum",1]
[null,null,"water in all type of excavations"]
[null,null,"on site"]
[null,null,"as described in SANS 1 200 A"]
[null,null,"section 5.5"]
["1.1.15","A8.8.1","Establish access road to site","sum",1]
[null,null,"where it is necessary"]
["1.1.16","A8.3.3","Fixed charge obligations by","sum",1]
[null,null,"the Contractor"]
["1.1.17","A8.3.4","Removal of site establishment","sum",1]
[]
[1.2,null,"Time related items"]
["1.2.1","A8.4.1","Contractual requirements on a","sum",1]
[null,null,"monthly bases affecting the"]
[null,null,"Contractor"]
[null,null,"The Contractor to maintain "]
[null,null,"the following items or as "]
[null,null,"amended in the"]
[null,null,"Tender Document - for the "]
[null,null,"duration of the Contract :"]
["1.2.2","A8.4.2.2","All facilities on the site for the","sum",1]
[null,null,"Engineer & for the Contractor"]
[null,null,"Other obligations by the "]
[null,null,"Contractor on a time bases "]
[null,null,"for the duration"]
[null,null,"of the Contract :"]
["1.2.3","A8.4.3","Full time supervision of the site","sum",1]
[null,null,"as specified in the Tender"]
[null,null,"Document"]
["1.2.4","A8.4.4","Company & head office","sum",1]
[null,null,"administration costs pertaining"]
[null,null,"to the Contract"]
["1.2.5","A8.4.5","Other time related obligations","sum",1]
[null,null,"by the Contractor"]
[]
[1.3,null,"Provisional sums by the"]
[null,null,"Engineer"]
["1.3.1","PSA5.10.1","Provisional sum for various","Prov",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[null,null,"tests requested by the"]
[null,null,"Engineer"]
["1.3.2","A8.8.2","Provision for traffic control as","Prov",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"}]
[null,null,"requested by the Engineer"]
["1.3.3","PSA5.10.1","Provisional sum for","Prov",1,{"v":120000,"d":"120,000.00"},{"v":120000,"d":"120,000.00"}]
[null,null,"community involvement/CLO"]
[null,null,"payment"]
[13.4,"PSA5.10.1","Provisional sum for","Prov",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[null,null,"Training of two (2) Students"]
["1.3.5","A8.5b","Contractor's overhead and","%"]
[null,null,"profit on Item 1.3.3"]
[]
["TOTAL CARRIED TO SUMMARY PAGE"]

{"sheet":"Mechanical","index":1,"n_rows":67,"n_cols":7,"rows_kept":67,"merged":[[0,0,0,2],[1,0,1,6],[2,0,2,6],[4,3,4,6],[5,0,5,6],[18,0,18,5],[20,3,20,6],[21,0,21,6],[34,0,34,5],[35,0,35,6],[36,3,36,6],[37,0,37,6],[50,0,50,5],[51,0,51,6],[52,3,52,6],[53,0,53,6],[66,0,66,5],[67,0,67,6],[143,0,143,6]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL B: MECHANICAL"]
["Item","Pay Ref.","Description","Unit","Qty","Rate","Amount"]
["1.",null,"Distribution Pump Sets (Option 1)"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[1.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[1.2,null,"Supply/ Manufacture of Pump Sets Complete.","Each",4]
[]
[1.3,null,"Supply/ Manufacture of Pipe Work Sets Complete.","Each",4]
[]
[1.4,null,"Install Pump Sets Complete.","Each",4]
[]
[1.5,null,"Install Pipe Work Sets Complete.","Each",4]
[]
[1.6,null,"Commission Pump & Pipe Work Sets.","Each",4]
[]
["TOTAL"]
[]
["2.",null,"Distribution Pump Sets (Option 2)"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[2.1,null,"Design & G.A. Drawings.","Sum",1,null,"Rate Only"]
[]
[2.2,null,"Supply/ Manufacture of Pump Sets Complete.","Each",4,null,"Rate Only"]
[]
[2.3,null,"Supply/ Manufacture of Pipe Work Sets Complete.","Each",4,null,"Rate Only"]
[]
[2.4,null,"Install Pump Sets Complete.","Each",4,null,"Rate Only"]
[]
[2.5,null,"Install Pipe Work Sets Complete.","Each",4,null,"Rate Only"]
[]
[2.6,null,"Commission Pump & Pipe Work Sets.","Each",4,null,"Rate Only"]
[]
["RATE ONLY"]
[]
["3.",null,"Suction Actuated Isolation Valves"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[3.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[3.2,null,"Supply/ Manufacture of Metal Seat Gate Valves Complete.","Each",4]
[]
[3.3,null,"Supply/ Manufacture of Valve Actuator Complete.","Each",4]
[]
[3.4,null,"Install Valves Complete.","Each",4]
[]
[3.5,null,"Install Actuators Complete.","Each",4]
[]
[3.6,null,"Commission Actuated Valves.","Each",4]
[]
["TOTAL"]
[]
["4.",null,"Delivery Actuated Isolation Valves"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[4.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[4.2,null,"Supply/ Manufacture of Metal Seat Gate Valves Complete.","Each",4]
[]
[4.3,null,"Supply/ Manufacture of Valve Actuator Complete.","Each",4]
[]
[4.4,null,"Install Valves Complete.","Each",4]
[]
[4.5,null,"Install Actuators Complete.","Each",4]
[]
[4.6,null,"Commission Actuated Valves.","Each",4]
[]
["TOTAL CARRIED TO NEXT PAGE"]

{"sheet":"Mechanical 2","index":2,"n_rows":70,"n_cols":7,"rows_kept":70,"merged":[[0,0,0,2],[1,0,1,6],[2,0,2,6],[4,0,4,5],[5,3,5,6],[6,0,6,6],[15,0,15,5],[16,0,16,6],[17,3,17,6],[18,0,18,6],[30,0,30,5],[31,0,31,6],[32,3,32,6],[33,0,33,6],[41,0,41,5],[42,0,42,6],[43,3,43,6],[44,0,44,6],[53,0,53,5],[54,0,54,6],[55,3,55,6],[56,0,56,6],[68,0,68,5],[69,0,69,5]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL B: MECHANICAL"]
["Item","Pay Ref.","Description","Unit","Qty","Rate","Amount"]
["Total carried from previous page"]
["5.",null,"Delivery Check Valves"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
["5.1",null,"Design & G.A. Drawings.","Sum",1]
[]
[5.2,null,"Supply/ Manufacture of Nozzle Check Valves Complete.","Each",4]
[]
[5.3,null,"Install Valves Complete.","Each",4]
[]
[5.4,null,"Commission Valves.","Each",4]
[]
["Total"]
[]
["6.",null,"Drainage Pump Sets"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[6.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[6.2,null,"Supply/ Manufacture of Pump Sets Complete.","Each",2]
[]
[6.3,null,"Supply/ Manufacture of Pipe Work Sets Complete.","Sum",1]
[]
[6.4,null,"Install Pump Sets Complete.","Each",2]
[]
[6.5,null,"Install Pipe Work Sets Complete.","Sum",1]
[]
[6.6,null,"Commission Pump & Pipe Work Sets.","Sum",1]
["TOTAL"]
[]
["7.",null,"Ventilation"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[7.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[7.2,null,"Supply/ Manufacture of Ventilation System Complete.","Sum",1]
[]
[7.3,null,"Install of Ventilation System Complete.","Sum",1]
[]
[7.4,null,"Commission of Ventilation System Complete.","Sum ",1]
["TOTAL"]
[]
["8.",null,"Lifting Equipment"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[8.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[8.2,null,"Supply/ Manufacture of Electrical Hoists Complete.","Each",2]
[]
[8.3,null,"Install of Electrical Hoists Complete.","Each",2]
[]
[8.4,null,"Commission of Electrical Hoists Complete.","Each",2]
[]
["TOTAL"]
[]
["9.",null,"Inflow Meter"]
["! The Contractor must include for the following; Design, G.A. drawings, manufacture/supply, deliver/store, install, commission, up-hold during the 12-month defects liability period and training, of the equipment listed below. All work and equipment must comply with the specifications forming part of the contract document."]
[9.1,null,"Design & G.A. Drawings.","Sum",1]
[]
[9.2,null,"Supply/ Manufacture of Electromagnetic Flow Meter Complete.","Each",1]
[]
[9.3,null,"Install of Electromagnetic Flow Meter Complete.","Each",1]
[]
[9.4,null,"Commission of Electromagnetic Flow Meter Complete.","Each",1]
[]
[9.5,null,"Provisional sum for modification to existing pipe work to fit flow meter.","PC Sum",1,{"v":350000,"d":"350,000.00"},{"v":350000,"d":"350,000.00"}]
[]
[9.6,null,"Provisional sum for modification to existing chamber to fit flow meter.","PC Sum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
["TOTAL"]
["TOTAL CARRIED TO SUMMARY PAGE"]

{"sheet":"Electrical","index":3,"n_rows":82,"n_cols":9,"rows_kept":82,"merged":[[0,0,0,2],[0,7,0,8],[1,0,1,6],[1,7,1,8],[2,0,2,8],[3,0,3,8],[4,0,5,0],[4,1,5,3],[4,4,5,5],[4,6,4,7],[5,6,5,7],[6,1,6,3],[6,4,6,5],[6,6,6,7],[7,1,7,3],[7,4,7,5],[7,6,7,7],[8,1,8,3],[8,4,8,5],[8,6,8,7],[9,1,9,3],[9,4,9,5],[9,6,9,7],[10,1,10,3],[10,4,10,5],[10,6,10,7],[11,1,11,3],[11,4,11,5],[11,6,11,7],[12,1,12,3],[12,4,12,5],[12,6,12,7],[13,1,13,3],[13,4,13,5],[13,6,13,7],[14,1,14,3],[14,4,14,5],[14,6,14,7],[15,1,15,3],[15,4,15,5],[15,6,15,7],[16,1,16,3],[16,4,16,5],[16,6,16,7],[17,1,17,3],[17,4,17,5],[17,6,17,7],[18,1,18,3],[18,4,18,5],[18,6,18,7],[19,1,19,3],[19,4,19,5],[19,6,19,7],[20,1,20,3],[20,4,20,5],[20,6,20,7],[21,1,21,3],[21,4,21,5],[21,6,21,7],[22,1,22,3],[22,4,22,5],[22,6,22,7],[23,1,23,3],[23,4,23,5],[23,6,23,7],[24,1,24,3],[24,4,24,5],[24,6,24,7],[25,1,25,3],[25,4,25,5],[25,6,25,7],[26,1,26,3],[26,4,26,5],[26,6,26,7],[27,1,27,3],[27,4,27,5],[27,6,27,7],[28,1,28,3],[28,4,28,5],[28,6,28,7],[29,1,29,3],[29,4,29,5],[29,6,29,7],[30,1,30,3],[30,4,30,5],[30,6,30,7],[31,1,31,3],[31,4,31,5],[31,6,31,7],[32,1,32,3],[32,4,32,5],[32,6,32,7],[33,1,33,3],[33,4,33,5],[33,6,33,7],[34,1,34,3],[34,4,34,5],[34,6,34,7],[35,1,35,3],[35,4,35,5],[35,6,35,7],[36,1,36,3],[36,4,36,5],[36,6,36,7],[37,1,37,3],[37,4,37,5],[37,6,37,7],[38,1,38,3],[38,4,38,5],[38,6,38,7],[39,1,39,3],[39,4,39,5],[39,6,39,7],[40,1,40,3],[40,4,40,5],[40,6,40,7],[41,1,41,3],[41,4,41,5],[41,6,41,7],[42,1,42,3],[42,4,42,5],[42,6,42,7],[43,1,43,3],[43,4,43,5],[43,6,43,7],[44,1,44,3],[44,4,44,5],[44,6,44,7],[45,1,45,3],[45,4,45,5],[45,6,45,7],[46,1,46,3],[46,4,46,5],[46,6,46,7],[47,1,47,3],[47,4,47,5],[47,6,47,7],[48,1,48,3],[48,4,48,5],[48,6,48,7],[49,1,49,3],[49,4,49,5],[49,6,49,7],[50,1,50,3],[50,4,50,5],[50,6,50,7],[51,1,51,3],[51,4,51,5],[51,6,51,7],[52,1,52,3],[52,4,52,5],[52,6,52,7],[53,1,53,3],[53,4,53,5],[53,6,53,7],[54,1,54,3],[54,4,54,5],[54,6,54,7],[55,1,55,3],[55,4,55,5],[55,6,55,7],[56,1,56,3],[56,4,56,5],[56,6,56,7],[57,1,57,3],[57,4,57,5],[57,6,57,7],[58,1,58,3],[58,4,58,5],[58,6,58,7],[59,1,59,3],[59,4,59,5],[59,6,59,7],[60,1,60,3],[60,4,60,5],[60,6,60,7],[61,1,61,3],[61,4,61,5],[61,6,61,7],[62,1,62,3],[62,4,62,5],[62,6,62,7],[63,1,63,3],[63,4,63,5],[63,6,63,7],[64,1,64,3],[64,4,64,5],[64,6,64,7],[65,1,65,3],[65,4,65,5],[65,6,65,7],[66,1,66,3],[66,4,66,5],[66,6,66,7],[67,0,68,0],[67,1,67,3],[67,4,68,5],[67,6,68,7],[67,8,68,8],[68,1,68,3],[69,1,69,3],[69,4,69,5],[69,6,69,7],[70,1,70,3],[70,4,70,5],[70,6,70,7],[71,1,71,3],[71,4,71,5],[71,6,71,7],[72,1,72,3],[72,4,72,5],[72,6,72,7],[73,1,73,3],[73,4,73,5],[73,6,73,7],[74,1,74,3],[74,4,74,5],[74,6,74,7],[75,0,75,1],[75,3,75,4],[75,5,75,6],[76,0,76,8],[77,0,77,6],[77,7,77,8],[78,0,78,8],[79,0,79,8],[80,0,80,8],[81,0,81,8]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL "]
["DISTRIBUTION TRANSFORMER"]
["Items ","Description ",null,null,"Unit",null,"Specified",null,"Offered"]
[{"$nulls":6},"Minimum Requirements",null,"To Be Completed By Contractor"]
[1,"Manufacturer",{"$nulls":4},"Stipulate"]
[2,"Country of manufacture",{"$nulls":4},"Stipulate"]
[3,"Delivery period",null,null,"Weeks",null,"Stipulate"]
[4,"Number of units required",null,null,"No",null,2]
[5,"Ambient temperature: Min/Max",null,null,"°C",null,{"$f":"5/50","v":0.1}]
[6,"Rating",null,null,"kVA",null,500]
[7,"Nominal system voltage and rated voltage on principal tapping: MV/LV",null,null,"kV rms",null,"11/0.4"]
[8,"Type",{"$nulls":4},"Outdoor"]
[9,"Tank Type",{"$nulls":4},"Sealed"]
[10,"Separate winding or auto-transformer",{"$nulls":4},"Separate winding"]
[11,"Number of Phases",{"$nulls":4},3]
[12,"Connection symbol (vector group) and neutral terminal",{"$nulls":4},"Dyn11"]
[13,"Winding tapped",{"$nulls":4},"LV"]
[14,"Parallel operation with other transformer matching impedance and tapings under same contract",{"$nulls":4},"Not Required"]
[15,"System fault current level",null,null,"kA",null,20]
[16,"Designed Short-circuit current: MV/LV",null,null,"kA",null,20]
[17,"Impedance on principal tapping",null,null,"%"]
[18,"Tap-changer type (OLTC or OCTS)",{"$nulls":4},"OCTS"]
[19,"Number of tapping positions (including transition positions)",null,null,"No"]
[20,"Lightning impulse insulation level (1,2/50 ms full wave) of tap-changer",null,null,"kV"]
[21,"Zero sequence impedance measurement required",{"$nulls":4},"Not Required"]
[22,"Automatic and remote control panels and equipment for the OLTC",{"$nulls":4},"Not Required"]
[23,"Tap local/remote switch",{"$nulls":4},"Local"]
[24,"Type of tap position indicator",{"$nulls":4},"Required"]
[25,"LV outdoor bushing rated for voltage",null,null,"kV",null,1]
[26,"Creepage distance for line terminals (min)",null,null,"kV/mm",null,31]
[27,"Primary connections",{"$nulls":4},"185 mm² x 3c Cu PILC / XLPE"]
[28,"Secondary connections",{"$nulls":4},"2 x 630 mm² x 1c Cu PVC"]
[29,"Disconnecting chamber",{"$nulls":4},"Not required"]
[30,"Drilling and bolting of flanges to comply with BS 4504 or DIN 2631",{"$nulls":4},"Required"]
[31,"Welded main tank cover joint",{"$nulls":4},"Required"]
[32,"Earthing connections to earth mat",{"$nulls":4},"Required"]
[33,"Brackets for surge arresters",{"$nulls":4},"Not Required"]
[34,"Bag in the main tank of the conservator",{"$nulls":4},"Not Required"]
[35,"Remote temperature indication",{"$nulls":4},"Not Required"]
[36,"Cooling",{"$nulls":4},"ONAN"]
[37,"OLTC control to be wired to the marshalling box",{"$nulls":4},"Not Required"]
[38,"Cables between the marshalling box and the control room",{"$nulls":4},"Not Required"]
[39,"Built- current transformers",{"$nulls":4},"Not Required"]
[40,"Winding-temperature thermometer(s)",{"$nulls":4},"Not Required"]
[41,"Oil-temperature thermometer",{"$nulls":4},"Required"]
[42,"Oil-actuated and gas-actuated relay",{"$nulls":4},"Not Required"]
[43,"Pressure-relief device",{"$nulls":4},"Required"]
[44,"Buchholz relay",{"$nulls":4},"Not Required"]
[45,"Tap-changer protective device",{"$nulls":4},"Not Required"]
[46,"Dehydrating breathers",{"$nulls":4},"Not Required"]
[47,"Conservator bag",{"$nulls":4},"Not Required"]
[48,"Oil filler plug",{"$nulls":4},"Required"]
[49,"Oil-level indicators",{"$nulls":4},"Not Required"]
[50,"Spares: 1 x MV bushing",{"$nulls":4},"Required"]
[51,"Spares: 1 x LV bushing",{"$nulls":4},"Required"]
[52,"Spares: 1 x cooling fan motor",{"$nulls":4},"Not Required"]
[53,"Spares: 1 x three-phase set of diverter switch contacts",{"$nulls":4},"Not Required"]
[54,"Spares: 1 x tap-changer drive motor",{"$nulls":4},"Not Required"]
[55,"Spares: 1 x contactor of each type",{"$nulls":4},"Not Required"]
[56,"Overall dimensions of tank: Width / Depth / Height",null,null,"mm",null,"Stipulate"]
[57,"Height over MV bushings",null,null,"mm",null,"Stipulate"]
[58,"Mass:  Transport/Filled",null,null,"kg",null,"Stipulate"]
[59,"Three-ply malthoid on plinth",{"$nulls":4},"Required"]
[60,"Bushings type",{"$nulls":4},"Stipulate"]
[61,"Training programme",null,null,"Prov",null,"Required",null," R 200 000.00"]
[61.1,"Contractor's overhead and",null,null,"%"]
[null,"profit on Item 61"]
[62,"Drawings and manuals in an electronic medium",{"$nulls":4},"dwg & pdf format"]
[63,"No-load loss on principal tapping at 1,00 Un",null,null,"kW",null,"Stipulate"]
[64,"Load loss (I2R + stray) at 75 °C and on principal tapping with LV unloaded:",null,null,"kW",null,"Stipulate"]
[65,"Fans (total)",null,null,"kW",null,"Not Required"]
[66,"Tolerance applicable to guaranteed impedances on principal tapping",null,null,"%",null,"Stipulate"]
[67,"Maximum acoustic sound level",null,null,"dB(A)",null,"Stipulate"]
[68,null,"SUPPLEMENTARY DETAILS"]
[]
["Carried forward to next page"]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
[]
[]
["Name (Print):                                                                Signature: ."]

{"sheet":"Electrical 2","index":4,"n_rows":181,"n_cols":5,"rows_kept":181,"merged":[[0,0,0,2],[0,7,0,8],[1,7,1,8],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,6,4],[11,0,11,4],[12,2,12,4],[34,0,34,4],[35,2,35,4],[36,0,37,0],[36,1,37,1],[36,2,37,2],[36,3,37,3],[36,4,37,4],[42,0,42,4],[43,2,43,4],[48,2,49,2],[48,4,49,4],[51,2,51,4],[60,0,60,4],[61,2,61,4],[71,0,71,4],[72,2,72,4],[81,0,81,4],[82,2,82,4],[90,0,90,4],[91,0,92,0],[91,1,92,1],[91,2,92,2],[91,3,92,3],[102,0,102,4],[103,2,103,4],[112,0,112,4],[113,0,114,0],[113,2,114,4],[121,0,121,4],[122,2,122,4],[125,0,126,0],[125,1,126,1],[125,2,126,2],[125,3,126,3],[125,4,126,4],[128,4,131,4],[132,0,133,0],[132,2,133,2],[132,3,133,3],[132,4,133,4],[134,0,134,4],[135,2,135,4],[138,0,139,0],[138,2,139,2],[138,3,139,3],[138,4,139,4],[141,0,141,4],[142,2,142,4],[143,0,145,0],[143,2,145,2],[143,3,145,3],[143,4,145,4],[146,0,146,4],[147,2,147,4],[154,0,154,4],[155,2,155,4],[173,0,173,4],[175,0,175,4],[176,0,176,3],[177,0,177,4],[178,0,178,4],[179,0,179,4],[180,0,180,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["VARIABLE FREQUENCY CONVERTERS"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[1,"GENERAL"]
[1.1,"Manufacturer"]
[1.2,"Model"]
[1.3,"Place of manufacture"]
[1.4,"Expected life (for spares availability)","Years"]
[]
[2,"ELECTRICAL SERVICE CONDITIONS"]
[2.1,"Normal service conditions varied in Project Specification","Yes/No","No"]
[2.2,"Unusual electrical service conditions specified","Yes/No","No"]
[2.3,"Supply network characteristics"]
["2.3.1","Voltage (nominal)","V",400]
["2.3.2","Frequency","Hz",50]
["2.3.3","Source impedance ( at minimum fault level) at PCC","Ohms","TBC"]
["2.3.4","Fault level (maximum) at PCC","MVA","TBC"]
["2.3.5","Fault level (n-1 contingency/minimum) at PCC","MVA","TBC"]
["2.3.6","Voltage total harmonic distortion limit at PCC","%",{"v":0.01,"d":"1%"}]
[2.4,"VFC input current harmonic limits and actual"]
["2.4.1","5th","%"]
["2.4.2","7th","%"]
["2.4.3","11th","%"]
["2.4.4","13th","%"]
["2.4.5","17th","%"]
["2.4.6","19th","%"]
["2.4.7","23rd","%"]
["2.4.8","25th","%"]
["2.4.9","29th","%"]
["2.4.10","31st","%"]
["2.4.11","THD","%"]
[]
[3,"ENVIRONMENTAL SERVICE CONDITIONS"]
[3.1,"Standard climatic conditions varied in Project","Yes/No","No"]
[]
[3.2,"Forced ventilation or air conditioning in VFC room","FV/AC","AC"]
[3.3,"Unusual mechanical installation conditions specified","Yes/No","No"]
[3.4,"Unusual environmental service conditions specified","Yes/No","No"]
[3.5,"Airflow required per VFC","m³/s"]
[]
[4,"LOAD DETAILS"]
[4.1,"Type of motor-driven load",null,"Pump"]
[4.2,"Load torque characteristic",null,"Quadratic"]
[4.3,"Number of operation quadrants",null,1]
[4.4,"Dynamic braking required",null,"No"]
[{"$nulls":3},"As per mechanical "]
[4.5,"Operating speed range",null,"specification"]
[]
[5,"CONVERTER TRANSFORMER"]
[5.1,"Type (oil-filled or dry)"]
[5.2,"Number of secondary windings"]
[5.3,"Primary rated voltage","V"]
[5.4,"Secondary rated voltage","V"]
[5.5,"Rated power","kVA"]
[5.6,"Free-standing (FS) or integral (I) to VFC","FS/I"]
[5.7,"No-load losses","W"]
[5.8,"Load losses","W"]
[]
[6,"CONVERTER CONFIGURATION"]
[6.1,"Form of converter (package/chassis/cabinet unit)",null,"Package"]
[6.2,"Rectifier type: diode- or active front end (DFE/AFE)",null,"DFE"]
[6.3,"Rectifier pulse number",null,6]
[6.4,"Bypass/redundancy arrangement specified","Yes/No","No"]
[6.5,"Input air circuit-breaker","Yes/No","No"]
[6.6,"Input switch-disconnector","Yes/No","No"]
[6.7,"Input semi-conductor fuses","Yes/No","Yes"]
[6.8,"Input contactor","Yes/No","Yes"]
[6.9,"Input earthing switch","Yes/No","No"]
[]
[7,"CONVERTER FILTERS"]
[7.1,"Line-side reactor","Yes/No","Yes"]
[7.2,"Line-side reactor relative short-circuit voltage","%"]
[7.3,"Line harmonic filters (LHF)","Yes/No"]
[7.4,"LHF free-standing (FS) or integral to VFC (I)","FS/I"]
[7.5,"Motor-side reactor","Yes/No"]
[7.6,"Motor-side dv/dt filter","Yes/No"]
[7.7,"Motor-side sine filter","Yes/No"]
[7.8,"Motor-side common-mode filter","Yes/No"]
[]
[8,"CONVERTER PROTECTION"]
[8.1,"Overcurrent and overload","Yes/No","Yes"]
[8.2,"Undervoltage and overvoltage","Yes/No","Yes"]
[8.3,"Phase loss and unbalance","Yes/No","Yes"]
[8.4,"Earth fault","Yes/No","Yes"]
[8.5,"Over-temperature","Yes/No","Yes"]
[8.6,"DC link overvoltage and overcurrent","Yes/No","Yes"]
[8.7,"Over-temperature of DC link reactor (if installed)","Yes/No","Yes"]
[]
[9,"MOTOR PROTECTION",null,null,"Indicate if provided "]
[{"$nulls":4},"by VFC or MPR"]
[9.1,"Short-circuit","Yes/No","Yes"]
[9.2,"Start(max starting time)/Stall","Yes/No","Yes"]
[9.3,"Earth fault","Yes/No","Yes"]
[9.4,"Overload","Yes/No","Yes"]
[9.5,"Number of starts","Yes/No","Yes"]
[9.6,"Loss of phase","Yes/No","Yes"]
[9.7,"Unbalance","Yes/No","Yes"]
[9.8,"Loss of load/undercurrent","Yes/No","Yes"]
[9.9,"Thermal by means of motor thermistors/RTDs","Yes/No","Yes"]
[]
[10,"CONVERTER RATINGS"]
[10.1,"Rated system voltage","V",400]
[10.2,"Line-side rated current","A"]
[10.3,"Input total power factor","pu"]
[10.4,"Line-side displacement power factor","pu"]
[10.5,"Rated continuous output current","A"]
[10.6,"Overload capability and time","A & s"]
[10.7,"Efficiency of complete drive module","%"]
[10.8,"Total losses of complete drive module","W"]
[]
[11,"CONTROL PERFORMANCE "]
[null,"REQUIREMENTS"]
[11.1,"Open loop speed control","Yes/No","Yes"]
[11.2,"Steady state deviation band","%","±1 to ±2"]
[11.3,"Closed loop speed control with indirect feedback","Yes/No","No"]
[11.4,"Steady state deviation band","%"]
[11.5,"Closed loop speed control with direct feedback","Yes/No","No"]
[11.6,"Steady state deviation band","%"]
[]
[12,"PROCESS CONTROL INTERFACE"]
[12.1,"Compliant with SANS 61800-7","No/Yes","Yes"]
[12.2,"Communications Interface Quantity","No."]
[12.3,"Communications Interface Type(s) and Connector(s)","No."]
[]
[12.4,"Communications Interface Protocol(s)","No."]
[null,null,"Process /"]
[12.5,"Communications Interface Power Drive System ","Drive/","Process"]
[null,"Profile","Motion"]
[null,null,"Control"]
[12.6,"Communications Interface Message Structure ",null,"Yes"]
[null,"to SANS 61800-7"]
[]
[13,"SPECIAL CONTROL FEATURES"]
[13.1,"Automatic restart facility","Yes/No","Yes"]
[13.2,"Flying restart facility","Yes/No","Yes"]
[13.3,"Adjustable ramp times ","Yes/No","Yes"]
[null,"(acceleration/deceleration)"]
[13.4,"Dip ride-through using load kinetic energy","Yes/No","Yes"]
[]
[14,"TESTING"]
[null,"Where indicated the following tests shall be "]
[null,"carried out in addition to the specified "]
[null,"mandatory tests."]
[]
[14.1,"Special Tests for Converter"]
["14.1.1","Overcurrent capability","Yes/No","No"]
["14.1.2","Measurement of ripple voltage and current","Yes/No","No"]
["14.1.3","Power factor measurement","Yes/No","No"]
["14.1.4","Measurement of inherent voltage regulation","Yes/No","No"]
["14.1.5","Audible noise","Yes/No","No"]
["14.1.6","Additional tests","Yes/No","No"]
[]
[14.2,"Drive System Site Tests"]
["14.2.1","Load duty","Yes/No","No"]
["14.2.2","Allowable full load current versus speed","Yes/No","No"]
["14.2.3","Temperature rise","Yes/No","No"]
["14.2.4","Efficiency","Yes/No","No"]
["14.2.5","Current sharing","Yes/No","No"]
["14.2.6","Voltage division","Yes/No","No"]
["14.2.7","Shaft current - bearing insulation","Yes/No","No"]
["14.2.8","Audible noise","Yes/No","No"]
["14.2.9","Motor vibration","Yes/No","No"]
["14.2.10","EMC tests","Yes/No","No"]
["14.2.11","Harmonic content of CDM output","Yes/No","No"]
["14.2.12","Current limit and current loop","Yes/No","No"]
["14.2.13","Speed loop","Yes/No","No"]
["14.2.14","Torque pulsation","Yes/No","No"]
["14.2.15","Automatic restart","Yes/No","No"]
["14.2.16","System full load test","Yes/No","No"]
["14.2.17","Overall drive system efficiency","Yes/No","No"]
[]
[14.3,"Witnessed factory acceptance test","Yes/No","No"]
[]
["Carried forward to next page"]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
[]
[]
["Name (Print):                                                                Signature: ."]

{"sheet":"Electrical 3","index":5,"n_rows":112,"n_cols":5,"rows_kept":112,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,7,2],[6,3,7,3],[6,4,7,4],[23,1,24,1],[23,3,24,3],[23,4,24,4],[26,0,26,4],[27,2,27,4],[41,0,41,4],[42,2,42,4],[46,2,47,2],[46,3,47,3],[46,4,47,4],[58,0,58,4],[59,2,59,4],[63,2,64,2],[63,3,64,3],[63,4,64,4],[67,2,68,2],[67,3,68,3],[67,4,68,4],[70,2,73,2],[70,3,73,3],[70,4,73,4],[76,0,76,4],[77,2,77,4],[81,2,83,2],[81,3,83,3],[81,4,83,4],[92,1,96,1],[92,2,96,2],[92,4,96,4],[99,0,99,4],[101,0,101,4],[102,0,102,3],[104,0,104,4],[105,0,105,4],[106,0,106,4],[107,0,107,4],[108,0,108,4],[109,0,109,4],[110,0,110,4],[111,0,111,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["PROGRAMMABLE LOGIC CONTROLLERS"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[null,"PROGRAMMABLE LOGIC"]
[1,"CONTROLLERS/Programmable RTU"]
[1.1,"Manufacturer"]
[1.2,"Model"]
[1.3,"CPU"]
[1.4,"CPU configuration"]
[1.5,"Digital Inputs","No."]
[1.6,"Digital Outputs","No."]
[1.7,"Analogue Inputs","No."]
[1.8,"Analogue Outputs","No."]
[1.9,"Spare I/O","%",{"v":0.3,"d":"30%"}]
[1.1,"Ports"]
["1.10.1","Ethernet","No."]
["1.10.2","Serial","No."]
["1.10.3","Other","No."]
[1.11,"Software"]
[1.12,"All engineering software included with PLC","Yes / No","Yes"]
[null,"Annual Software License renewal required",null,"No, should be once off fee"]
[1.13,null,"Yes / No"]
[1.14,"Programming Language",null,"IEC 61131"]
[]
[2,"REMOTE IO"]
[2.1,"Manufacturer"]
[2.2,"Model"]
[2.3,"CPU"]
[2.4,"CPU configuration"]
[2.5,"Digital Inputs","No."]
[2.6,"Digital Outputs","No."]
[2.7,"Analogue Inputs","No."]
[2.8,"Analogue Outputs","No."]
[2.9,"Spare I/O","%",{"v":0.3,"d":"30%"}]
[2.1,"Ports"]
["2.10.1","Ethernet","No."]
["2.10.2","Serial","No."]
["2.10.3","Other","No."]
[]
[3,"PLC, RTU AND RIO PANELS"]
[3.1,"Enclosure Material",null,"as per MCC"]
[3.2,"Enclosure Colour",null,"as per MCC"]
[3.3,"Enclosure Rating","IP",42]
[null,null,"Floor Standing / wall mounted","Floor Standing"]
[3.4,"Enclosure Mounting"]
[3.5,"Supply and Control Circuit Voltages","V","24V DC"]
[3.6,"Wire Colours",null,"as per spec"]
[3.7,"Glass door - viewing panel","Yes / No","Yes"]
[3.8,"Termination"]
[3.9,"Glanding"]
[3.1,"Power Supply Unit vendor preferences"]
[3.11,"Uninterruptible Power Supply requirement","Yes / No","Yes"]
[3.12,"Panel light required","Yes / No","Yes, LED"]
[3.13,"Socket outlet required","Yes / No","Yes"]
[3.14,"Physical Spare space","%",30]
[]
[4,"HUMAN MACHINE INTERFACE (HMI)"]
[4.1,"Manufacturer"]
[4.2,"Model"]
[4.3,"Screen Size","Inches","15\""]
[{"$nulls":3},"Colour LCD Display, 18 bit"]
[4.4,"Screen Type"]
[4.5,"Resolution","Pixels"]
[4.6,"Touch Screen","Yes / No","Yes"]
[null,null,"Capacitive/ Resistive"]
[4.7,"Type of Touch Screen"]
[4.8,"Enclosure Rating","IP",65]
[null,null,"Panel / Flush Fronted / Front","Flush Fronted"]
[]
[]
[4.9,"Position of Installation"]
[4.1,"Software"]
[4.11,"Datasheets included with tender","Yes / No","Yes"]
[]
[5,"UPS"]
[5.1,"Manufacturer"]
[5.2,"Model"]
[5.3,"Place of manufacture"]
[{"$nulls":3},"Industrial online double conversion with full static bypass"]
[]
[5.4,"Type"]
[5.5,"Power","W","Load + 30%"]
[5.6,"Backup Time","min",30]
[5.7,"Output Voltage","V","230V +-5%"]
[5.8,"Nominal Frequency","Hz",50]
[5.9,"Output Waveform",null,"Pure sine wave"]
[5.1,"Number of Phases","1 or 3",1]
[5.11,"Communication",null,"Serial/Ethernet"]
[5.12,"Battery Life","Years","Min 10."]
[null,"Battery Type",null,"Sealed, maintenance free, Lead"]
[{"$nulls":3},"acid contained in UPS"]
[]
[]
[5.13]
[5.14,"Battery Charger"]
[5.15,"Datasheets included with tender","Yes / No","Yes"]
[]
[6,"SUPPLEMENTARY DETAILS"]
[]
["Carried forward to next page"]
[]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
[]
[]
[]
[]
[]
[]
["Name (Print):                                                                                                      Signature: ."]

{"sheet":"Electrical 4","index":6,"n_rows":93,"n_cols":5,"rows_kept":93,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,6,4],[12,0,12,4],[13,2,13,4],[18,0,18,4],[19,2,19,4],[24,0,24,4],[26,0,26,4],[27,2,27,4],[42,0,42,4],[43,2,43,4],[50,0,50,4],[51,2,51,4],[63,0,63,4],[64,2,64,4],[68,0,68,4],[69,0,70,0],[69,2,70,4],[74,0,74,4],[75,2,75,4],[78,0,78,4],[79,2,79,4],[84,0,84,4],[85,0,85,3],[89,0,89,4],[90,0,90,4],[91,0,91,4],[92,0,92,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["LOW VOLTAGE SOFT STARTERS"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[1,"MAKES AND MODELS"]
[1.1,"Manufacturer"]
[1.2,"Rated power up to 15 kW","kW"]
[1.3,"Rated power over 15 kW up to 30 kW","kW"]
[1.4,"Rated power over 30 kW up to 55 kW","kW"]
[1.5,"Rated power over 55 kW","kW"]
[]
[2,"CHARACTERISTICS OF SOFT STARTERS"]
[2.1,"Type of Equipment"]
["2.1.1","Two phase control allowed up to 15 kW","Yes/No","Yes"]
["2.1.2","Controlled phases fully controlled"]
["2.1.3","In-delta connection allowed","Yes/No","No"]
[]
[2.2,"Ratings"]
["2.2.1","Rated operational voltage","V",400]
["2.2.2","Rated insulation voltage","V"]
["2.2.3","Rated impulse withstand voltage","kV"]
["2.2.4","Rated frequency","Hz",50]
[]
[2.3,"Utilization category",null,"AC-53a"]
[]
[2.4,"Protection Functions"]
["2.4.1","Overtemperature/thermal protection","Yes/No","Yes"]
["2.4.2","Electronic motor overload","Yes/No","Yes"]
["2.4.3","Phase loss","Yes/No","Yes"]
["2.4.4","Phase unbalance","Yes/No","Yes"]
["2.4.5","Phase sequence","Yes/No","Yes"]
["2.4.6","Overcurrent/short-circuit","Yes/No","Motors >55 kW"]
["2.4.7","Earth fault","Yes/No","Motors >55 kW"]
["2.4.8","Starts per hour","Yes/No","Motors >55 kW"]
["2.4.9","Stall (locked rotor under starting conditions)","Yes/No","Motors >55 kW"]
["2.4.10","Thermistor/RTD input","Yes/No","Motors >55 kW"]
["2.4.11","Underload (undercurrent)","Yes/No","Yes"]
["2.4.12","Over- and undervoltage","Yes/No","Yes"]
["2.4.13","Jam (locked rotor under running conditions)","Yes/No","Yes"]
["2.4.14","Type 2 co-ordination with upstream SCPD","Yes/No","Yes"]
[]
[2.5,"Control Settings"]
["2.5.1","Initial start voltage","Yes/No","Yes"]
["2.5.2","Start ramp time","Yes/No","Yes"]
["2.5.3","Motor full load current","Yes/No","Yes"]
["2.5.4","Current limit","Yes/No","Yes"]
["2.5.5","Kickstart (voltage/current boost)","Yes/No","Yes"]
["2.5.6","Torque control","Yes/No","Yes"]
[]
[3,"LINE-, BYPASS AND PFC CONTACTORS"]
[3.1,"Line Contactors"]
["3.1.1","Line contactor required","Yes/No","Yes"]
["3.1.2","Manufacturer"]
["3.1.3","Type 2 co-ordination with upstream SCPD","Yes/No","Yes"]
["3.1.4","Utilization category",null,"AC3"]
[]
[3.2,"Bypass Contactors"]
["3.2.1","Bypass contactor required","Yes/No","Yes"]
["3.2.2","Integral or separate"]
["3.2.3","Manufacturer (if separate)"]
["3.2.4","Utilization category (with/without line contactor)",null,"AC1/AC3"]
[]
[3.3,"PFC Contactors"]
["3.3.1","PFC contactor required","Yes/No","Yes"]
["3.3.2","Manufacturer"]
["3.3.3","Utilization category",null,"AC6b"]
[]
[4,"OPERATOR AND PROCESS CONTROL"]
[null,"INTERFACES"]
[4.1,"Operator Control Interface"]
["4.1.1","Integral operator control interface",null,"SS >30 kW"]
["4.1.2","Remote operator control interface in compartment door","Yes/No","Yes"]
[]
[4.2,"Process Control Interface"]
["4.2.1","Communication link",null,"SS >30 kW"]
["4.2.2","Communication interfaces and protocols",null,"Fieldbus/Ethernet"]
[]
[5,"TESTING"]
[8.1,"Type tests","Yes/No","Yes"]
[8.2,"Routine tests","Yes/No","Yes"]
[8.3,"Factory acceptance test","Yes/No","No"]
[8.4,"Site acceptance test","Yes/No","Yes"]
[]
["Carried forward to next page"]
[]
[]
[]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
[]
[]
["Name (Print):                                   Signature:                                    ."]

{"sheet":"Electrical 5","index":7,"n_rows":35,"n_cols":5,"rows_kept":35,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,6,4],[9,2,10,2],[9,4,10,4],[11,0,12,0],[11,1,12,1],[11,3,12,3],[11,4,12,4],[14,0,14,4],[15,2,15,4],[18,2,19,2],[18,3,19,3],[18,4,19,4],[20,0,21,0],[20,1,21,1],[20,3,21,3],[20,4,21,4],[25,0,25,4],[26,0,26,3],[30,0,30,4],[31,0,31,4],[32,0,32,4],[33,0,33,4],[34,0,34,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["CABLE SUPPORTS"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[1,"WIRE MESH TRAY"]
[1.1,"Manufacturer"]
[1.2,"Type"]
[{"$nulls":3},"HDG indoors,"]
[1.3,"Material",null,"Stainless Steel 316 Outdoors"]
[1.4,"Duty","Heavy/","Medium"]
[null,null," Medium"]
[1.5,"Application"]
[]
[2,"CABLE LADDER"]
[2.1,"Manufacturer"]
[2.2,"Type"]
[{"$nulls":3},"HDG indoors, Stainless Steel 316 Outdoors"]
[2.3,"Material"]
[2.4,"Duty","Heavy/","Heavy"]
[null,null," Medium"]
[2.5,"Application",null,"MV and LV cables"]
[]
[3,"SUPPLEMENTARY DETAILS"]
[]
["Carried forward to next page"]
[]
[]
[]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
[]
[]
[]
["Name (Print):                                      Signature:                                 ."]

{"sheet":"Electrical 6","index":8,"n_rows":41,"n_cols":5,"rows_kept":41,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,6,4],[14,3,15,3],[14,4,15,4],[16,2,17,2],[16,4,17,4],[19,0,19,4],[21,0,21,4],[22,0,22,3],[29,0,29,4],[30,0,30,4],[31,0,31,4],[32,0,32,4],[33,0,33,4],[34,0,34,4],[35,0,35,4],[36,0,36,4],[37,0,37,4],[38,0,38,4],[39,0,39,4],[40,0,40,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["LV CABLES"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[1,"LOW VOLTAGE CABLES"]
[1.1,"Manufacturer"]
[1.2,"Operating Voltage","V","600/1000"]
[1.3,"Number of Cores","No"]
[1.4,"Size","mm 2","See Specifications and SLDs"]
[1.5,"Conductor Type","Cu/Al"]
[1.6,"Cable Type"]
[1.7,"Full Load Current","A"]
[{"$nulls":3},"Yes, SWA or AWA for single core"]
[1.8,"Armouring","Yes/No"]
[null,null,"mm (to cable centre)"]
[1.9,"Depth of installation",null,650]
[1.1,"Outdoor Cable Markers","Yes/No","No"]
[]
[2,"SUPPLEMENTARY DETAILS"]
[]
["Carried forward to next page"]
[]
[]
[]
[]
[]
[]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements"]
{"$rows_empty":10}
["Name (Print):                                  Signature:                                     ."]

{"sheet":"Electrical 7","index":9,"n_rows":54,"n_cols":5,"rows_kept":54,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,2,6,4],[10,3,14,3],[16,0,16,4],[17,2,17,4],[24,0,24,4],[28,3,29,3],[28,4,29,4],[35,0,35,4],[36,2,36,4],[41,0,41,4],[42,2,42,4],[49,0,49,3],[50,0,50,4],[51,0,51,4],[52,0,52,4],[53,0,53,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["CONTROL, INSTRUMENTATION AND DATA CABLES"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Carried amount from previous page"]
[1,"CONTROL CABLES"]
[1.1,"Manufacturer"]
[1.2,"Size","mm 2",1.5]
[1.3,"Operating Voltage","V","24VDC/230VAC"]
[1.4,"Number of Cores","No","Refer to Instrumentation and Control cable schedule and drawings."]
[1.5,"Size","mm 2"]
[1.6,"Conductor Type","Cu/Al"]
[1.7,"Cable Type"]
[1.8,"Full Load Current","A"]
[1.9,"Armouring","Yes/No","Yes, SWA"]
[]
[2,"INSTRUMENTATION CABLES"]
[2.1,"Manufacturer"]
[2.2,"Operating Voltage","V","24VDC/230VAC"]
[2.3,"Size","mm 2",1.5]
[2.4,"Cable Type",null,"Twisted Pair"]
[2.5,"Screened",null,"Individually and Overall"]
[2.6,"Armouring","Yes/No","Yes, SWA"]
[]
[3,"FIBRE OPTIC",null,null,"N/A"]
[3.1,"Manufacturer"]
[3.2,"Type",null,"Multimode"]
[{"$nulls":3},"Yes, for outdoor and exposed cables."]
[3.3,"Armouring","Yes/No"]
[3.4,"Armouring Type",null,"Steel Tape Armoured"]
[3.5,"Termination preference type",null,"ST"]
[3.6,"Cores","No","min 12"]
[3.7,"Cable Category",null,"min OM 2"]
[3.8,"Modal Bandwidth","MHz.km","min 500 / 500"]
[]
[4,"ETHERNET CABLES"]
[4.1,"Manufacturer"]
[4.2,"Type",null,"CAT5 STP"]
[4.3,"Armouring","Yes/No","No"]
[4.4,"Termination Type",null,"RJ 45 (Moulded case type)"]
[]
[5,"FIELDBUS CABLE"]
[5.1,"Manufacturer"]
[5.2,"Type",null,"CAT5 STP"]
[5.3,"Armouring","Yes/No","No"]
[5.4,"Termination Type",null,"RJ 45 (Moulded case type)"]
[]
[6,"SUPPLEMENTARY DETAILS"]
["Carried forward to next page"]
["Regardless of any information provided in this technical data sheet, the equipment to be provided will comply with the specified requirements."]
[]
[]
["Name (Print):                                               Signature:                                       ."]

{"sheet":"Electrical 8","index":10,"n_rows":157,"n_cols":5,"rows_kept":157,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,0,6,4],[7,2,7,4],[11,0,12,0],[11,1,12,1],[11,2,12,2],[11,4,12,4],[13,0,14,0],[13,1,14,1],[13,2,14,2],[13,4,14,4],[16,0,17,0],[16,2,17,2],[16,3,17,3],[16,4,17,4],[18,0,18,4],[19,2,19,4],[23,0,23,4],[24,2,24,4],[25,4,26,4],[35,0,35,4],[36,2,36,4],[37,0,38,0],[37,1,38,1],[37,2,38,2],[37,4,38,4],[41,2,43,2],[41,4,43,4],[46,0,47,0],[46,2,47,2],[46,3,47,3],[46,4,47,4],[48,0,48,4],[49,0,50,0],[49,2,50,2],[49,3,50,3],[49,4,50,4],[59,0,59,4],[70,0,70,4],[82,0,82,4],[88,0,88,4],[101,0,101,4],[106,1,106,4],[114,0,114,4],[121,0,121,4],[130,0,130,4],[131,0,132,0],[131,2,132,2],[131,3,132,3],[131,4,132,4],[136,0,137,0],[136,1,137,1],[136,2,137,2],[136,4,137,4],[138,0,139,0],[138,1,139,1],[138,2,139,2],[138,4,139,4],[142,0,142,3],[143,0,143,4],[144,0,144,4],[145,0,145,4],[146,0,146,4],[147,0,147,4],[148,0,148,4],[149,0,149,4],[150,0,150,4],[151,0,151,4],[152,0,152,4],[153,0,153,4],[154,0,154,4],[155,0,155,4],[156,0,156,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["LV ELECTRICAL MOTORS"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Amount carried forward from previuos page"]
[]
[1,"ELECTRICAL OPERATING CONDITIONS"]
[1.1,"Supply voltage (nominal)","V",400]
[1.2,"Number of phases",null,3]
[1.3,"Frequency","Hz",50]
[1.4,"Voltage and frequency variations","%","As per SANS"]
[{"$nulls":3},"1804-2"]
[1.5,"Supply voltage harmonic voltage factor",null,"As per SANS"]
[{"$nulls":3}," 60034-1"]
[1.6,"Supply voltage negative sequence component","%",2]
[1.7,"Supply neutral earthed directly/resistively",null,"Directly"]
[null," (high/low)"]
[]
[2,"SITE OPERATING CONDITIONS"]
[2.1,"Altitude a.s.l.","m","As per"]
[2.2,"Maximum ambient temperature","°C"," Specification"]
[2.3,"Minimum ambient temperature","°C"]
[]
[3,"MOTOR RATING"]
[{"$nulls":3},"As per"]
[3.1,"Rated output","kW"," Specification"]
[3.2,"Duty type",null,"S1"]
[3.3,"Output margin above load absorbed power","%",15]
[3.4,"Speed (synchronous)","rpm",1500]
[3.5,"Speed at rated output, voltage and frequency","rpm"]
[3.6,"Rated voltage","V",400]
[3.7,"Full load current","A"]
[3.8,"Efficiency class (IE1/2/3)",null,"IE2"]
[3.9,"Rated torque","Nm"]
[]
[4,"ENCLOSURE, CONSTRUCTION & MOUNTING"]
[4.1,"Ingress protection rating",null,"IP55, IP68 for"]
[{"$nulls":3},"submersible"]
[4.2,"Cooling method",null,"IC411"]
[4.3,"Construction and mounting arrangement",null,"IM B3"]
[{"$nulls":3},"as per"]
[4.4,"Terminal box location (R/B/L/T)",null,"Contractor's"]
[{"$nulls":3},"design"]
[4.5,"Cable entry location",null,"Below"]
[4.6,"Cable type and size",null,"As per SLD"]
[4.7,"Corrosion protection (standard/corrosive",null,"Corrosive"]
[null,"environment)"]
[]
[5,"WINDINGS TYPE, INSULATION &"]
[null,"TEMPERATURE RISE"]
[]
[5.1,"Stator winding type (random/formed diamond coil)",null,"Formed"]
[5.2,"Insulation and impregnation system",null,"VPI"]
[5.3,"Insulation thermal class","(F/H)","F"]
[5.4,"Temperature rise class","(B/F)","B"]
[5.5,"Maximum temperature rise at rated output (Zone A supply)","K"]
[5.6,"Maximum temperature rise at rated output (Zone C supply)","K"]
[5.7,"Windings thermal protection (thermistor/PT100)",null,"Yes"]
[]
[6,"GENERAL PERFORMANCE"]
[]
[6.1,"Efficiency at rated output","%"]
[6.2,"Efficiency at rated 75% output","%"]
[6.3,"Efficiency at rated 50% output","%"]
[6.4,"Power factor at rated output","pu"]
[6.5,"Power factor at 75% rated output","pu"]
[6.6,"Power factor at 50% rated output","pu"]
[6.7,"Sound power level at rated load","dBA"]
[6.8,"Silencer required",null,"No"]
[]
[7,"STARTING PERFORMANCE"]
[]
[7.1,"Starting method",null,"As per SLDs"]
[7.2,"Motor moment of inertia","kg.m²"]
[7.3,"Number of starts per hour (cold/hot)",null,"2023-02-06"]
[7.4,"Starting current (x full load current)","A"]
[7.5,"Starting torque (x rated torque)","N m"]
[7.6,"Pull-up torque (x rated torque)","N m"]
[7.7,"Breakdown torque (x rated torque)","N m"]
[7.8,"Starting power factor","pu"]
[7.9,"Run up time of driven load (state pu starting current)","s"]
[]
[8,"DRIVEN LOAD AND COUPLING"]
[]
[8.1,"Load type",null,"Various"]
[8.2,"Load moment of inertia at motor speed","kg.m²"]
[8.3,"Coupling method (direct/gearbox/v-belt)"]
[]
[9,"BEARINGS"]
[]
[9.1,"Manufacturer"]
[9.2,"DE bearing type (ball/roller/sleeve)",null,"Ball/roller"]
[9.3,"DE bearing lubrication type (sealed/regreasable)"]
[9.4,"DE bearing life (L10)","h"]
[9.5,"DE bearing regrease interval","h"]
[9.6,"NDE bearing type (ball/roller/sleeve)",null,"Ball/roller"]
[9.7,"NDE bearing lubrication type (sealed/regreasable)"]
[9.8,"NDE bearing life (L10)","h"]
[9.9,"NDE bearing regrease interval","h"]
[9.1,"Bearing thermal protection (thermistor/PT100)"]
[]
[10,"DIMENSIONS AND WEIGHT"]
[]
[10.1,"Motor frame number"]
[10.2,"Motor weight","kg"]
[]
[11,"VARIABLE SPEED APPLICATIONS"]
[]
[11.1,"Operating speed range","rpm","As per load"]
[11.2,"Maximum safe operating speed","rpm"]
[11.3,"Peak voltage withstand level","V"]
[11.4,"Voltage gradient withstand level","V/s"]
[11.5,"Separately-powered cooling fan"]
[]
[12,"OPTIONAL ITEMS"]
[]
[12.1,"Anti-condensation heaters",null,"Yes"]
[12.2,"Slide rails (for v-belt drives)",null,"No"]
[12.3,"Surge protection devices",null,"No"]
[12.4,"Adjusting bolts required",null,"Yes"]
[]
[13,"FACTORY TESTS"]
[]
[13.1,"Routine tests in addition to SANS 1804-2 requirements"]
["13.1.1","Insulation resistance check",null,"Yes"]
["13.1.2","Vibration velocity measurement",null,"No"]
[13.2,"Type tests in addition to SANS 1804-2 requirements"]
["13.2.1","Current vs speed curve",null,"Yes"]
["13.2.2","Torque vs speed curve",null,"Yes"]
[]
[14,"DRAWINGS / CURVES TO BE PROVIDED WITH"]
[null,"TENDER"]
[]
[14.1,"Motor general arrangement with dimensions",null,"Yes"]
[14.2,"Main terminal box with fault rating indicated",null,"Yes"]
[14.3,"Current vs speed curve",null,"Yes for"]
[{"$nulls":3},">=30kW"]
[14.4,"Torque vs speed curve",null,"Yes for"]
[{"$nulls":3},">=30kW"]
[]
[]
["Amount carried forward to next page"]
["Regardless of any information provided in this technical data sheet, the equipment to be provided "]
["will comply with the specified requirements"]
{"$rows_empty":11}
["Name (Print):                                              Signature: ."]

{"sheet":"Electrical 9","index":11,"n_rows":166,"n_cols":5,"rows_kept":166,"merged":[[0,0,0,2],[2,0,2,4],[3,0,3,4],[5,0,5,3],[6,0,7,0],[6,2,7,2],[6,3,7,3],[6,4,7,4],[8,0,8,4],[9,2,9,4],[13,3,14,3],[13,4,14,4],[15,4,16,4],[17,0,17,4],[18,2,18,4],[23,0,24,0],[23,1,24,1],[23,2,24,2],[23,4,24,4],[26,0,27,0],[26,1,27,1],[26,2,27,2],[26,4,27,4],[30,4,32,4],[33,4,34,4],[41,2,43,2],[41,4,43,4],[44,0,44,4],[45,2,45,4],[49,0,50,0],[49,1,50,1],[49,4,50,4],[51,0,51,4],[60,4,63,4],[64,0,64,4],[65,2,65,4],[71,0,72,0],[71,1,72,1],[71,2,72,2],[71,4,72,4],[73,2,74,2],[73,4,74,4],[75,0,75,4],[80,0,81,0],[80,1,81,1],[80,2,81,2],[80,4,81,4],[82,0,82,4],[83,2,83,4],[84,0,84,4],[87,0,87,4],[88,2,88,4],[91,0,91,4],[92,2,92,4],[100,0,100,4],[101,2,101,4],[106,0,106,4],[107,2,107,4],[114,0,114,4],[115,2,115,4],[118,0,118,4],[119,2,119,4],[122,0,122,4],[123,2,123,4],[127,0,127,4],[128,2,128,4],[131,2,132,2],[131,4,132,4],[138,0,138,4],[139,2,139,4],[141,0,141,4],[142,2,142,4],[144,0,144,4],[150,0,150,4],[151,2,151,4],[157,0,157,4],[160,0,160,3],[161,0,161,4],[162,0,162,4],[163,0,163,4],[164,0,164,4],[165,0,165,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL C: ELECTRICAL"]
["LV SWITCHGEAR AND CONTROLGEAR ASSEMBLIES - MOTOR CONTROL CENTRES"]
[null,"DESCRIPTION","UNIT","SPECIFIED","OFFERED"]
["Amount carried from previous page"]
[null,"This data sheet is applicable to the following"]
[null,"Motor Control Centres"]
[]
[1,"GENERAL"]
[1.1,"MCC Manufacturer"]
[1.2,"Tested with Stated Deviations to SANS 1973-1","Yes/No","Yes"]
[1.3,"Type Test Certificate Required","Yes / No","Yes"]
[null,null,"230V/"]
[1.4,"Control Voltage","24VDC"]
[null,null,"pattern/"]
[1.5,"Compartment type","withdrawable","Fixed pattern"]
[]
[2,"CONSTRUCTION REQUIREMENTS"]
[2.1,"Steel Work Manufacturer"]
[2.2,"Form of Internal Separation",null,"3b/4a"]
[2.3,"Material of Construction",null,"3CR12"]
[2.4,"Ingress Protection (doors closed)","IP",42]
[2.5,"Method of Installation",null,"Floor"]
[{"$nulls":3},"Standing"]
[2.6,"Epoxy Powder Coated","Yes / No","Yes"]
[2.7,"Colour of Assembly",null,"Electric"]
[{"$nulls":3},"Orange"]
[2.8,"Size of Panel","HxWxD","H <2100"]
[2.9,"Spare Space Required","%",">=20"]
[null,null,"Back /"]
[2.1,"Access","Front/","Front & Rear"]
[null,null,"Side"]
[null,null,"Top/"]
[2.11,"Cable Entry","Bottom","Bottom"]
[2.12,"Doors / Removable Panels",null,"Doors"]
[2.13,"Door Locks","Yes / No","Yes"]
[2.14,"Door Locks - Type",null,"Square key"]
[2.15,"Door Locks - Material"]
[2.16,"Incomer Section Required","Yes / No","Yes"]
[2.17,"Corrosion protection",null,"Epoxy coated"]
[{"$nulls":3},"Not painted;"]
[{"$nulls":3},"Alu for single"]
[2.18,"Gland Plates",null,"core cables"]
[]
[3,"ELECTRICAL COMPONENTS"]
[3.1,"Busbars"]
["3.1.1","Material",null,"Copper"]
["3.1.2","Tinned","Yes / No","Yes"]
["3.1.3","Current Density",null,"<2 as per"]
[null,null,"A/mm ²","type test"]
[]
[3.2,"Air Circuit Breakers"]
["3.2.1","Manufacturer"]
["3.2.2","Type",null,"Fixed pattern"]
["3.2.3","Model"]
["3.2.4","Rated Current","A","As per SLD"]
["3.2.5","Service short-circuit breaking capacity (Ics)","kA","As per SLD"]
["3.2.6",null,null,"Electronic"]
["3.2.7","Short-circuit release",null,"Electronic"]
[{"$nulls":3},"Yes for MCCs"]
["3.2.8","Motorised",null,"With"]
[null,null,"Yes / No","Generator"]
[{"$nulls":3},"supply"]
[]
[3.3,"Moulded Case Circuit Breakers"]
["3.3.1","Manufacturer"]
["3.3.2","Type",null,"Fixed"]
["3.3.3","Model"]
["3.3.4","Rated Current","A","As per SLD"]
["3.3.5","Service short-circuit breaking capacity (Ics)","kA","As per SLD"]
["3.3.6","Overload release",null,"Thermal/"]
[{"$nulls":3},"electronic"]
[{"$nulls":3},"Magnetic/"]
["3.3.7","Short-circuit release",null,"electronic"]
[]
[3.4,"Miniature Circuit Breakers"]
["3.4.1","Manufacturer"]
["3.4.2","Type"]
["3.4.3","Model"]
["3.4.4","Tripping Curve",null,"C or as per"]
[{"$nulls":3},"SLD"]
[]
[3.5,"Fuse Switch-Disconnector"]
[]
["3.5.1","Manufacturer"]
["3.5.2","Model"]
[]
[3.6,"High Rupture Capacity (HRC) Fuse Links"]
["3.6.1","Manufacturer"]
["3.6.2","Model"]
[]
[3.7,"Surge Arrestors"]
["3.7.1","Power Circuits - Manufacturer"]
["3.7.2","Power Circuits - Model"]
["3.7.3","Power Circuits - Rating","kA"]
["3.7.4","Remote Indication to PLC","Yes / No","Yes"]
["3.7.5","Control Circuits - Manufacturer"]
["3.7.6","Control Circuits - Model"]
["3.7.7","Remote Indication to PLC","Yes / No"]
[]
[3.8,"Contactors"]
["3.8.1","Manufacturer"]
["3.8.2","Model"]
["3.8.3","Contactor rating",null,"AC3"]
["3.8.4","Coordination",null,"Type 2"]
[]
[3.9,"Overload Relays"]
["3.9.1","Manufacturer"]
["3.9.2","Type"]
["3.9.3","Model"]
["3.9.4","Rated Current","A","As per SLD"]
["3.9.5","Resetable from front of MCC","Yes / No","Yes"]
["3.9.6","LCD","Yes / No","No"]
[]
[3.1,"Miniature Relays"]
["3.10.1","Manufacturer"]
["3.10.2","Model"]
[]
[3.11,"Control switches and pushbuttons"]
["3.11.1","Manufacturer"]
["3.11.2","Model"]
[]
[3.12,"Indicating Lamps"]
["3.12.1","Manufacturer"]
["3.12.2","Model"]
["3.12.3","Type",null,"LED"]
[]
[3.13,"Power Meter for Incomer(s)"]
["3.13.1","Manufacturer"]
["3.13.2","Model"]
[{"$nulls":3},"Modbus/"]
["3.13.3","Communication Protocol",null,"Ethernet"]
["3.13.4","Harmonics Measurement","Yes / No","No"]
["3.13.6","Time of use measurement","Yes / No","No"]
["3.13.7","Bi-directional","Yes / No","No"]
["3.13.8","Datasheet provided with tender","Yes / No","Yes"]
["3.13.9","Data logging functionality","Yes / No","Yes"]
[]
[3.14,"Control-Circuit and auxiliary supply transformer"]
["3.14.1","Manufacturer"]
[]
[3.15,"Capacitors for Individual Power Factor Correction"]
["3.15.1","Manufacturer"]
[]
[4,"ACTIVE HARMONIC FILTER (if applicable)",null,null,"N/A"]
[4.1,"Manufacturer"]
[4.2,"Model"]
[4.3,"Type"]
[4.4,"Datasheets included with tender","Yes / No"]
[]
[5,"FIELD E-STOP/START CONTROL STATIONS"]
[5.1,"Method of Installation",null,"Pedestal"]
[5.2,"Material of Construction",null,"HDG"]
[5.3,"Manufacturer"]
[5.4,"Keyswitch Required","Yes / No","No"]
[5.5,"IP rating","IP",65]
[]
[6,"SUPPLEMENTARY DETAILS"]
[]
["Total Carried to summary"]
["Regardless of any information provided in this technical detail sheet, the equipment to be provided"]
["will comply with the specified requirements"]
[]
[]
["Name (Print):                                                           Signature: ."]

{"sheet":"Building","index":12,"n_rows":167,"n_cols":6,"rows_kept":167,"merged":[[0,0,0,2],[2,0,2,5],[3,1,3,5],[11,0,11,5],[12,2,12,5],[14,0,14,5],[15,2,15,5],[17,0,17,5],[18,2,18,5],[22,0,22,5],[23,2,23,5],[26,0,26,5],[27,2,27,5],[29,0,29,5],[30,2,30,5],[33,0,33,5],[34,2,34,5],[36,0,36,5],[37,2,37,5],[39,0,39,5],[40,2,40,5],[43,0,43,5],[44,2,44,5],[47,0,47,5],[48,2,48,5],[52,0,52,5],[53,2,53,5],[55,0,55,5],[56,2,56,5],[59,0,59,5],[60,2,60,5],[63,0,63,5],[64,2,64,5],[67,0,67,4],[135,0,135,5],[136,1,136,4],[137,1,137,4],[138,1,138,4],[139,1,139,4],[140,1,140,4],[141,1,141,4],[142,1,142,4],[143,1,143,4],[144,1,144,4],[145,1,145,4],[146,1,146,4],[147,1,147,4],[148,1,148,4],[149,1,149,4],[150,1,150,4],[151,1,151,4],[152,1,152,4],[153,1,153,4],[154,1,154,4],[155,1,155,4],[156,1,156,4],[157,1,157,4],[158,1,158,4],[159,1,159,4],[160,1,160,4],[161,1,161,4],[162,1,162,4],[163,1,163,4],[164,1,164,4],[165,1,165,4],[166,0,167,0],[166,1,167,4],[166,5,167,5]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
["BILL D: BUILDING & STRUCTURAL (2 Guard Houses) "]
[2,"Earthworks"]
["Item","Description","unit","quant","rate","amount"]
[2.1,"Site clearance","m2"," 12000"]
[2.2,"Setting out",1,"sum"]
[2.3,"Excavations","m3",20]
[2.4,"Landscape the Site ","Prov",1,"250 000","250 000.00"]
[2.5,"EO for hard rock","m3",50,"rate only"]
[2.6,"EO for soft rock","m3",50,"rate only"]
[]
[3,"Concrete works-foundations"]
[3.1,"Cast strip foundations with 20Mpa concrete","m3",10]
[]
[4,"DPC"]
[4.1,"Dpc under walls","m",60]
[]
[5,"Brickwork sub structure"]
[5.1,"one brickwall","m2",6,"rate only"]
[5.2,"Half brickwall","m2",30]
[5.3,"Brickforce in every course","m",200]
[]
[6,"Filling"]
[6.1,"Use filling from excavations and compact","m3",4]
[6.2,"Use imported approved gravel filling and compact","m3",12]
[]
[7,"DPM"]
[7.1,"Install 250mm micron damp proof membrane under concrete slab","m2",40]
[]
[8,"Electrical-first installation"]
[8.1,"Allow electrical installation for db sleeves under floor","Pc Sum",1,6000," 6000.00"]
[8.2,"Allow for installation of complete high must light on Site (cabling, Concrete footing, connection, and commission). The light must be both electrical and solar dependant","sum",1]
[]
[9,"Plumbing -first installation"]
[9.1,"Allow sleeves for under floor slab","pc sum",1,6000," 6000.00"]
[]
[10,"Concrete works-floor slab"]
[10.1,"Cast floor slab 75mm thick ","m3",4]
[]
[11,"Dpc under walls"]
[11.1,"110mm walls","m",12]
[11.2,"220mm walls","m",40]
[]
[12,"Brickwork superstructure"]
[12.1,"One brickwall","m2",100]
[12.2,"Half brickwall","m2",30]
[]
[13,"Brickforce"]
[13.1,"110mm brickforce","m",150]
[13.2,"220mm brickforse","m",200]
[13.3,"Allow for 6mm double anchor roof wires","each",12]
[]
[14,"Pre-cast lintels"]
[14.1,"SABS Approved concrete lintels","no",12]
[]
[15,"Steel windows"]
[15.1,"Type NC2F windows","no",4]
[15.2,"Type W1 windows (1.2x1.2m)","no",4]
[]
[16,"Steel door frames"]
[16.4,"Steel door frames","no",2]
[16.5,"Steel door -Heavy duty bugler door with lock","no",2]
[]
[17,"Timber doors"]
[17.1,"Meranti open braced door","each",2]
[17.2,"Veneer internal door","each",4]
["Subtotal carried to next page"]
{"$rows_empty":67}
["D: Total Summary Page for Building Works"]
["Item","Description",{"$nulls":3},"amount"]
[2,"Earthworks "]
[3,"Concrete works-foundations"]
[4,"DPC "]
[5,"Brickwork sub structure"]
[6,"Filling"]
[7,"DPM "]
[8,"Electrical-first installation"]
[9,"Plumbing -first installation"]
[10,"Concrete works-floor slab"]
[11,"Dpc under walls "]
[12,"Brickwork superstructure "]
[13,"Brickforce "]
[14,"Pre-cast lintels "]
[15,"Steel windows "]
[16,"Steel door frames/Steel door "]
[17,"Timber doors"]
[18,"Locksets"]
[19,"Plumbing"]
[20,"Electrical"]
[21,"Glazing"]
[22,"Window sills"]
[23,"Ceilings "]
[24,"Roofing "]
[25,"Fascias and Bargeboards"]
[26,"Plastering"]
[27,"Painting"]
[28,"Gutters and downpipes"]
[29,"Tiles "]
[30,"Renovation of Pump Station 1"]
[null,"SUB-TOTAL BILL D TO MAIN SUMMARY PAGE"]

{"sheet":"Building 2","index":13,"n_rows":55,"n_cols":6,"rows_kept":55,"merged":[[0,0,0,2],[2,1,2,4],[4,2,4,5],[8,2,8,5],[10,0,10,5],[11,2,11,5],[13,0,13,5],[17,0,17,5],[18,2,18,5],[22,0,22,5],[23,2,23,5],[26,0,26,5],[29,0,29,5],[30,2,30,5],[33,0,33,5],[34,2,34,5],[38,0,38,5],[39,2,39,5],[43,0,43,5],[44,2,44,5],[47,0,47,5],[48,2,48,5],[51,1,51,4],[52,1,52,4],[54,1,54,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
[null,"Amount brought forward from previous page"]
["Item","Description","unit","quant","rate","amount"]
[18,"Locksets"]
[18.1,"four lever locksets","each",2]
[18.2,"three lever locksets","each",4]
[]
[19,"Plumbing"]
[19.1,"PC Amount for Plumbing as per plan","Pc Sum",1,70000,"70000.00 "]
[]
[20,"Electrical"]
[20.1,"PC Amount for electrical as per plan","Pc Sum",1,40000,40000]
[]
[21,"Glazing"]
[21.1,"4mm obscure glass to bathroom windows","m2",10]
[21.2,"6mm Safety glass to w1 windows","m2",10]
[]
[22,"Windowsills"]
[22.1,"10mm approved fibre cement internal windowsills","m",12]
[22.2,"Approved concrete external windowsills","m",12]
[22.3,"Dpc to underside of sills","m",12]
[]
[23,"Ceilings"]
[23.1,"Pvc ceilings on Branderings to supplier’s details","m2",32]
[23.2,"Approved Cornice with Approved glue","m",72]
[]
[24,"Roofing"]
[24.1,"Allow pc sum for trusses and purlins","pc ",1,30000," 30000.00"]
[]
[25,"Fascia’s and Bargeboards"]
[25.1,"230mm Fascia","m",23]
[25.2,"230mm Bargeboards","m",40]
[]
[26,"Plastering"]
[26.1,"15mm plaster to internal and external walls","m2",180]
[26.2,"EO for Corners","m",56]
[26.3,"25mm screed to floors","m2",30]
[]
[27,"Painting"]
[27.1,"Plaster undercoat","m2",180]
[27.2,"2 layers Dulux Paint to walls","m2",180]
[27.3,"2 layers enamel paint to steel windows and door frames including primer coat","m2",80]
[]
[28,"Gutters and downpipes"]
[28.1,"Approved gutters on gutter brackets","m",10]
[28.2,"Approved downpipes with approved holder bats","m",6]
[]
[29,"Tiles"]
[29.1,"Ceramic floor tiles to floors","m2",30]
[29.2,"150mm white glazed tiles to walls and splash tiles at basins and sinks","m2",4]
[]
[30,"Renovation of Existing Pump Station 1 "]
[30.1,"Replacement of the existing roof structure (old trusses and old roof sheets) with steel roof structure and new roof sheets with new gutters and ceiling, paint work, replace existing wooden door with steel door, waterproofing the pump house","Prov",1,500000,500000]
[null,"total carried to summary page"]

{"sheet":"OHS","index":14,"n_rows":129,"n_cols":6,"rows_kept":129,"merged":[[0,0,0,2],[3,0,4,0],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[5,1,5,3],[6,0,8,0],[6,2,8,2],[6,3,8,3],[6,4,8,4],[6,5,8,5],[9,1,9,3],[10,0,39,0],[10,2,25,2],[10,3,25,3],[10,4,25,4],[10,5,25,5],[41,0,43,0],[41,2,43,2],[41,3,43,3],[41,4,43,4],[41,5,43,5],[45,0,48,0],[45,2,48,2],[45,3,48,3],[45,4,48,4],[45,5,48,5],[49,0,50,0],[49,2,50,2],[49,3,50,3],[49,4,50,4],[49,5,50,5],[51,0,52,0],[51,2,52,2],[51,3,52,3],[51,4,52,4],[51,5,52,5],[54,0,56,0],[54,2,56,2],[54,3,56,3],[54,4,56,4],[54,5,56,5],[58,2,60,2],[58,3,60,3],[58,4,60,4],[58,5,60,5],[61,2,85,2],[61,3,85,3],[61,4,85,4],[61,5,85,5],[97,0,105,0],[97,2,100,2],[97,3,100,3],[97,4,100,4],[97,5,100,5],[106,0,109,0],[106,2,109,2],[106,3,109,3],[106,4,109,4],[106,5,109,5],[110,0,113,0],[110,1,111,1],[110,2,113,2],[110,3,113,3],[110,4,113,4],[110,5,113,5],[115,0,117,0],[115,2,117,2],[115,3,117,3],[115,4,117,4],[115,5,117,5],[118,0,126,0],[128,0,128,4]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
[" Item","Description","unit","quant","rate","amount"]
[null,"BILL E - OCCUPATIONAL"]
[null,"HEALTH &  SAFETY"]
[1,"Notification of Construction Work"]
[null,"Allow for the costs on notification","sum",1]
[null,"of the Provincial Director of"]
[null,"construction work Regulation"]
[2,"Program"]
[null,"Allow for the costs on setting up a"]
[null,"Health and Safety Program"]
[null,"including File on site Regulation 3"]
[null,"& 5. Include the costs to compile"]
[null,"the following documents for the file"]
[null,"to be kept on site."]
[null,"Copy of Construction Regulations"]
[null,"Copy of tender document"]
[null,"Copy of drawings"]
[null,"Notification of construction work"]
[null,"Letters of appointment"]
[null,"Company safety Policy"]
[null,"Company organogramme"]
[null,"Notice in respect of machinery"]
[null,"Ten commandments of safety"]
[null,"Emergency telephone numbers"]
[null,"List of subcontractors"]
[null,"Proof of Registration with COID"]
[null,"Insurer"]
[null,"Training material"]
[null,"Risk Assessments and method"]
[null,"statements"]
[null,"Registers as specified elsewhere"]
[null,"Safe work procedures"]
[null,"The file shall be a lever arch file"]
[null,"With original colour documents of"]
[null,"acceptable standards."]
[null,"The file will be expanded during"]
[null,"The project as and when required"]
[null," By the Client.","sum",1]
[3,"Risk Assessment"]
[null,"Allow for the costs of a competent","sum",1]
[null," person to carry out a Risk"]
[null,"Assessment "]
[4,"She Co-ordinator"]
[null,"Allow for the appointment of a","months"]
[null,"SHE Coordinator to do monthly"]
[null,"Inspections (Control on SHE"]
[null,"Representative)"]
[5,"Health & Safety Induction "]
[null,"Trainer"]
[null,"Allow for the appointment of a H & S","sum",1]
[null,"Induction Trainer"]
[6,"Safe Work Procedures"]
[null,"Allow for the costs of setting up","sum",1]
[null,"safe work procedures by"]
[null,"competent person."]
[7,"She Representative"]
[null,"Allow for the appointment of a","months"]
[null,"SHE Representative to be"]
[null,"permanently on site."]
[null,"Allow for the following"]
[null,"appointments to be part of the"]
[null,"functions of the "]
[null,"SHE Representative"]
[null,"Accident Investigator"]
[null,"Allow for the appointment of an"]
[null,"Accident Investigator"]
[null,"Construction Vehicle and"]
[null,"Mobile Plant Inspectors"]
[null,"Allow for the appointment of a full"]
[null,"time inspector of construction"]
[null,"vehicles"]
[null,"Hand Tool Inspector"]
[null,"Allow for the appointment of a full"]
[null,"time Hand Tool Inspector"]
[null,"Portable Electrical Equipment"]
[null,"Inspector"]
[null,"Allow for the appointment of a full"]
[null,"time Portable Electrical"]
[null,"Equipment Inspector"]
[null,"Stacking and Storage"]
[null,"Inspector"]
[null,"Allow for the costs of a competent"]
[null,"person to supervise all stacking"]
[null,"and storage"]
[null,"Hygiene and Facility Inspector"]
[null,"Allow for the appointment of a full"]
[null,"time Hygiene and facility"]
[null,"Inspector"]
[null,"Fire Equipment Inspector"]
[null,"Allow for the costs of a competent"]
[null,"person to inspect all fire"]
[null,"equipment"]
[null,"First Aid Box Inspector"]
[null,"Allow for the costs of a competent"]
[null,"person to inspect the first -aid box","Sum"]
[]
[null,"Allow for the following"]
[null,"appointments of personnel"]
[null,"with responsibilities towards"]
[null,"H&S Supervisors"]
[null,"Allow for the appointment of full"]
[null,"time employees as the"]
[null,"construction supervisors"]
[null,null," months"]
[null,"Fire Fighting Equipment","ea",2]
[null,"Provide 3 kg firefighting"]
[null,"equipment suitable for electrical"]
[null,"fires on each site"]
[null,"First Aid","ea",1]
[]
[null,"Allow for the cost of a basic First"]
[null,"Aid Kit and Stretcher"]
[null,"Personal Protective clothing"]
[null,"Provisional rates for the following","ea",1]
[null,"Items will be remeasurable"]
[null,"Shoulder length PVC Gloves"]
[null,"Plastic Trousers","ea",1]
[null,"Safety Goggles","ea",1]
[null,"Gum Boots","ea",1]
[null,"Welding Helmet","ea",1]
[null,"Gas Welding Safety Goggles","ea",1]
[null,"Safety Shoes","ea",1]
[null,"Dust Masks","ea",1]
[null,"Leather Aprons","ea",1]
[null,"Hard Hats","ea",1]
[]
["Total Carried to Summary Page",{"$nulls":4}," "]

{"sheet":"Summary","index":15,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[0,0,0,5],[1,0,1,5],[2,1,2,3],[2,4,2,5],[3,1,3,3],[3,4,3,5],[4,1,4,3],[4,4,4,5],[5,1,5,3],[5,4,5,5],[6,1,6,3],[6,4,6,5],[7,1,7,3],[7,4,7,5],[8,1,8,3],[8,4,8,5],[9,1,9,3],[9,4,9,5],[10,1,10,3],[10,4,10,5],[11,1,11,3],[11,4,11,5],[12,1,12,3],[12,4,12,5]]}
["Project no. : 21/2022/23"]
["METSIMAHOLO LOCAL MUNICIPALITY"]
[null,"MAIN TOTAL SUMMARY PAGE",null,null,"TOTAL AMOUNT"]
["A","P & G,s"]
["B","MECHANICAL WORKS"]
["C","ELECTRICAL WORKS"]
["D","BUILDING WORKS"]
["E","OHS"]
["F","SUB-TOTAL"]
["G","CONTINGENCIES @ 10%"]
["H","TOTAL EXCL VAT"]
["I","VAT @ 15%"]
["J","TOTAL TENDER AMOUNT CARRIED TO FORM OF OFFER"]