{"text_format":"3","workbook":"xlsx","n_sheets":9,"sheets":["Buhlebethu Unpriced","SNP Kitchen","Borehole","New","Combined","Blk 8 Toilet","Blk 10 leaners Toilet","Blk 9 Toilet","Blk 11 Guard H"],"not_rendered":{"defined_names":8},"read":"whole","date_system":"1900"}

{"sheet":"Buhlebethu Unpriced","index":0,"n_rows":17321,"n_cols":7,"rows_kept":17321}
["Item","Description","Unit","Qty","Rate","Amount","Asbestos"]
[]
[null,"SECTION No. 1 "]
[]
[null,"Bill No. 1"]
[]
[null,"PRELIMINARIES  "]
[]
[null,"NOTES  "]
[]
[null,"The Principal Building Agreement JBCC Series 2000 (Edition 4.1 Code 2101  March 2005), recommended by the Joint Building Contracts Committee and  amended as hereinafter described, shall apply."]
[]
[null,"\tThe Preliminaries (May 2005 Edition) for use with the JBCC Series 2000 Principal Building Agreement as recommended by the Joint Building Contracts Committee  shall be deemed to be incorporated herein."]
[]
[null,"\tThe Model Preambles for Trades as published by the Association of South African  Quantity Surveyors (1999 Edition) shall be taken to be incorporated in these bills of  quantities and shall be applicable to the building works."]
[]
[null,"\tTenderers are referred to the above mentioned documents for the full intent and  meaning of each clause thereof.  These clauses are hereinafter referred to by clause  number and heading only.  Where standard clauses or alternatives are not applicable  to this contract, such modifications/corrections or additions as are necessary, are  given as far as possible under each relevant clause heading."]
[]
[null,"\tNo claim whatsoever shall be entertained in respect of errors or omissions in pricing due to brevity of descriptions of items which are fully described when read in  Preliminaries and Preambles."]
[]
[null,"\tThe Tenderers shall allow opposite each of the Clauses whatever costs and charges  he may consider necessary for the carrying out, comply with and due observance of the  provisions, conditions and requirements set out herein.  Only priced items will be  considered in respect of any adjustment of this Section.  Any items left unpriced will be  understood to be provided free of charge and no claim for any extras arising out of the  Tenderer's omission to price any item will be entertained."]
[]
[null,"\tWhere modifications or amendments as described are made, such modifications  and/or amendments shall supercede any conflicting provisions in the relevant Clauses of  the Preliminaries or the Principal Building Agreement and the tenderer shall make due  allowance for whatever costs and charges he may consider necessary for the carrying  out and observance of the provisions of the clauses as modified and/or amended."]
[]
[null,"\tAny item not relevant to this Contract is marked N/A."]
[]
[null,"\tIf alternative A for the adjustment of Preliminaries is selected (Clause 10.3) then each  priced item shall be clearly divided according to one or more of the following  denotations:"]
[]
[null,"\tF = Fixed amount"]
[null,"\tV = Variable in proportion to contract value"]
[null,"\tT = Variable in proportion to construction period"]
[]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING AGREEMENT  (JBCC SERIES 2000 -  EDITION 4.1 CODE 2101 MARCH 2005) "]
[]
[null,"DEFINITIONS "]
[]
[null,"Definitions and Interpretation (Clause 1.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.........................V:........................T:.........................."]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"OBJECTIVE AND PREPARATION "]
[]
[null,"Offer acceptance and Performance (Clause 2.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:........................ T:........................."]
[]
[null,"Documents (Clause 3.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"The Bills of Quantities shall not be used for ordering of materials"]
[]
[null,"Clause 3.1 shall be deleted in its entirety."]
[]
[null,"Clause 3.2.2 shall be deleted in its entirety."]
[]
[null,"Clause 3.3 shall be deleted and replaced with: \"The Contractor shall, before or at Site  Handover, sign and deliver to the Principal Agent, a waiver of contractor's lien\"."]
[]
[null,"F:........................ V:.........................T:............................."]
[]
[null,"Design responsibility (Clause 4.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"The following new clauses  are hereby added to this clause:"]
[]
[null,"Any sub-contractor whose subcontract involves design work will be required to sign  an indemnity in order to provide to the employer evidence of \"professional indemnity\"  insurance for such design work."]
[]
[null,"If the Contractor fails to obtain the necessary design warranties from the  subcontractors, the design responsibility shall be deemed to devolve upon the  Contractor."]
[]
[null,"F:......................... V:........................T:............................."]
[]
[null,"Employer's agents (Clause 5.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:..........................V:.........................T:............................."]
[]
[null,"Site representative (Clause 6.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 6 is amended by the addition of the following:"]
[]
[]
[null,"The names, CV's and organogram of the contractor's proposed management team  shall be submitted to the principal agent prior to commencement on site and, after the  principal agent's agreement on the composition and competence thereof has been  obtained, no changes shall be made nor shall any member of the said team be  removed from the project while remaining in the employ of the contractor, without the  principal agent's prior written approval."]
[]
[null,"F:........................ V:........................ T:..............................."]
[]
[null,"Compliance with regulations (Clause 7.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 7.0 is amended by the addition of the following clause:"]
[]
[null,"\tThe employer reserves the right to pay direct (i.e. not through the contractor) for all or any permanent connections to local or other authority  services, for which provisional amounts have been included within the  selected subcontract bill/section hereof.  In the event of the employer paying  direct for these charges, the contractor will not be entitled to a ten percent  (10%) mark-up in terms of Clause 32.4.  All such provisional amounts included  in the contract sum will be omitted."]
[]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"\tWithout limiting the generality of the provisions of clause 7.0 of the  agreement, the contractor's attention is drawn to the provisions of the  Construction Regulations, 2003 issued in terms of the Occupational Health  and Safety Act, 1993 in which it is specifically stated that the employer shall  prepare a documented health and safety specification for the works and that  the employer shall ensure that the contractor has made provision for the cost  of health and safety measures during the execution of the works. The principal  agent shall, on behalf of the employer, issue such health and safety  specification and the contractor shall price opposite this item for compliance  with the act and the regulations and the provisions of the aforementioned  health and safety specification, provided such provisions are reasonable in  terms of the act and the regulations."]
[]
[null,"F:...................... V:......................... T:............................"]
[]
[null,"Works risk (Clause 8.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 8.0 is amended by the addition of the following clause:"]
[]
[null,"8.2.3\tThe contractor shall be liable for and pay the deductibles."]
[]
[null,"Clause 8.6 is deleted and substituted with:"]
[]
[null,"The Contractor shall forthwith notify the principal agent, the Employer and  Employer's  Insurance Broker, as well as any other insurer involved of any physical  loss and damage to the works that comes to his attention. "]
[]
[null,"F:......................... V:............................ T:................................"]
[null,"Indemnities (Clause 9.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 9.1.1 is deleted and substituted with:"]
[]
[null,"Claims from other parties consequent upon the death or bodily injury or illness of  any person or physical loss or damage to any property, other than the works, arising  out of or due to the execution of the works or occupation of the Site by the Contractor  or his Subcontractors\"."]
[]
[null,"F:....................... V:..................... T:..........................."]
[]
[null,"Works insurances (Clause 10.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 10.0 is amended by the addition of the following clause:"]
[]
[null,"10.5\tThe Contractor shall be liable for and pay the deductibles."]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Liability insurances (Clause 11.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 11.0 is amended by the addition of the following clause:"]
[]
[null,"11.3\t The Contractor shall be liable for and pay the deductible."]
[]
[null,"F:....................... V:..................... T:............................"]
[]
[null,"Effecting insurances (Clause 12.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:......................."]
[]
[null,"No clause","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Security (Clause 14.0)","Item",{"v":1,"d":"1.00"}]
[]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Tenderers are required to submit proof with their tenders from the Guarantor that  security will be provided should their tender be accepted - such proof to be in the  form of a letter from the Guarantor stating the amount of security to be provided.  The  above security requirement shall also apply to all nominated/selected sub-contractors."]
[]
[null,"The following new sub-clause shall be added:"]
[]
[null,"In the event that the value of the works (excluding adjustments in terms of the  contract price adjustment provisions) were to increase during the course of the  contract by an amount of 15% or more of the contract sum, upon written request from  the Principal Agent, the Contractor shall immediately arrange to have the construction  guarantee  \"guaranteed sum\" increased accordingly, the verified cost of which shall  be added to the contract sum\"."]
[]
[null,"F:....................... V:......................... T:..........................."]
[]
[null,"EXECUTION "]
[]
[null,"Preparation for and execution of the works (Clause 15.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:....................... T:............................."]
[]
[null,"Access to the works (Clause 16.0)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:.........................."]
[]
[null,"Contract instructions (Clause 17.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Setting out of the works (Clause 18.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"The following sub-clauses are hereby added to this clause:"]
[]
[null,"18.5\tThe Contractor shall perform tolerance control checks regularly throughout  the contract period and report on these at regular intervals to the Principal Agent\"."]
[]
[null,"F:....................... V:....................... T:............................."]
[]
[null,"Assignment (Clause 19.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Nominated sub-contractors (Clause 20.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"All amounts allowed under Provisional Sums are intended to be awarded to  Nominated Subcontractors."]
[]
[null,"F:....................... V:...................... T:..........................."]
[]
[null,"Selected sub-contractors (Clause 21.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:...................... T:........................."]
[]
[null,"Employers Direct Contractors (Clause 22.0)","Item",{"v":1,"d":"1.00"}]
{"$rows_empty":12}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"The following sub-clauses are hereby added to this clause:"]
[]
[null,"The contractor shall not be entitled to any percentage profit or discount on the value  of any work executed by direct contractors but shall nevertheless allow direct  contractors and the employer's tenants and employees to have access to the works,  allocate reasonable space in the building for the storage of their material, tools and  equipment, all to the satisfaction of the principal agent. The contractor shall also allow  the direct contractors, etc. to use, free of charge, the ablution facilities and water and  power supply on the site, and shall not in any way hinder or prevent the execution of  their work."]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Contractors Domestic Subcontractors (Clause 23.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"COMPLETION "]
[]
[null,"Practical completion (Clause 24.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"The Contractor shall also compile his own practical completion list, a copy of which  must be available to the Principal Agent prior to the Contractor giving notice to the  Principal Agent to inspect the works."]
[]
[null,"F:....................... V:.................... T:.........................."]
[]
[null,"Works Completion (Clause 25.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:...................... T:........................."]
[]
[]
[null,"Final Completion (Clause 26.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:....................... T:..........................."]
[]
[null,"Latent defects liability period (Clause 27.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:........................ T:.........................."]
[]
[null,"Sectional completion (Clause 28.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:.................... T:............................."]
[]
[null,"Revision of date for practical completion (Clause 29.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"(1)\t  Clause 29.0 is amended by:"]
[]
[null,"\t\"29.9  Revision to the date for practical completion shall only be considered  when work on the critical path of the agreed programme for the works is  delayed\"."]
[]
[null,"(2)\t29.10   ACCELERATION"]
[]
[null,"29.10.1\tIrrespective of whether or not the Principal Agent rules that the  Contractor is entitled to an extension of time or a revision of the date for  practical completion, the Principal Agent shall nevertheless, at any time, be  entitled to instruct the Contractor, in writing, to accelerate the progress of the  remaining works, to ensure that the works are completed by the original date  for practical completion or revised date as the case may be."]
{"$rows_empty":9}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"29.10.2\tUpon receipt of such instruction, the contractor shall take necessary  steps to ensure that the works are completed timeously, including the  provision by him of additional resources, plant, manpower, etc. and the  working overtime or additional overtime beyond that contemplated at the time  of tender (at all times adhering to the regulations and requirements of all  authorities) and by all other adequate and   proper means and methods. The Contractor shall prove that such steps are  being taken if called upon to do so."]
[]
[null,"29.10.3\tThe Contractor's entitlement to compensation arising out of or in  respect of any revision to the date for practical completion that may have been  granted by the Principal Agent, or alternatively, where the Principal Agent has  instructed the Contractor to accelerate, shall be adjudicated strictly in terms of  Clause B10.3 hereof.  The Contractor shall not be entitled to any compensation  of any nature whatsoever, other than that provided for in terms of Clause  B10.3."]
[]
[null,"(3)\t29.11.1  The removal and replacement of material and/or workmanship that  does not conform with specification or drawings shall not constitute ground  for an extension of the construction period nor for an adjustment to the  contract sum."]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Penalty for non-completion (Clause 30.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"PAYMENT "]
[]
[null,"Interim payment to the contractor (Clause 31.0)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Materials and goods off site in terms of Clause 31.6.5 will not be included in the  amount authorized for payment."]
[]
[null,"Clause 31.9: The period of payment by the employer to the contractor of the payment  certificate shall be deemed to be amended from seven (7) to twenty one(21) calendar  days from receipt of contractors Tax invoice."]
[]
[null,"Clause 31.10: The employer shall not pay compensatory interest on any amounts  certified after practical completion."]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Adjustments to the contract value (Clause 32.0)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Where prices are submitted by the Contractor or Nominated/Selected Subcontractor  during the progress of the works in respect of contract instructions or in regard to a  claim under the terms of the contract and notwithstanding the fact that such prices  may be used in an interim payment certificate, there is to be no presumption of  acceptance.  Should the Principal Agent wish to accept any such prices prior to the  issue of the Final Certificate, it will be in writing."]
[]
[null,"This is a fixed price contract and no adjustment to the contract value due to  inflationary cost or other increases will be made"]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Recovery of expense and loss (Clause 33.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Final account and final payment (Clause 34.0)","Item",{"v":1,"d":"1.00"}]
[]
[null,"The Employer shall not pay any interest on amounts payable to the contractor for a  hundred and twenty days (120) after the date of issue of the certificate of practical  completion."]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"The first sentence of Clause 34.10 shall be amended as follows:"]
[]
[null,"The Employer shall pay the Contractor the amount certified for payment in the Final  Payment Certificate within twenty one (21) calendar days of the date of issue of the  Final Payment Certificate."]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Payment to other parties (Clause 35.0)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"CANCELLATION "]
[]
[null,"Cancellation by employer - Contractor's default (Clause 36.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Clause 36.3 is amended by the deletion of the words \"ten (10) working days\" and the  substitution with the words \"five (5) working days\""]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[]
[null,"Cancellation by employer - Loss and damage (Clause 37.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Cancellation by contractor - employer's default (Clause 38.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Cancellation - cessation of the works (Clause 39.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Dispute settlement (Clause 40.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"SUBSTITUTE PROVISIONS "]
[]
[null,"State clauses (Clause 41.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"PRE-TENDER INFORMATION  "]
[]
[null,"The schedule (Clause 42.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Information necessary for completion of those clauses contained in the schedule which are  necessary for tender purposes is given hereunder  "]
[]
[null,"CONTRACTING AND OTHER PARTIES "]
[]
[null,"Employer: "]
[]
[null,"…………………………………………………………….."]
[]
[null,"Tel No: "]
[null,"Fax No:"]
[]
[null,"Project Manager: "]
[]
[null,"………………………………………"]
[]
[null,"Tel No: "]
[null,"Fax No: "]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Architect: "]
[]
[null,"………………………………….."]
[]
[null,"Tel No: "]
[null,"Fax No: "]
[]
[null,"Electrical Engineer: "]
[]
[null,"……………………………………."]
[]
[null,"Tel No: "]
[null,"Fax No: "]
[]
[null,"Quantity Surveyor:"]
[]
[null,"Tel No: "]
[null,"Fax No: "]
[]
[null,"Civil Engineer: "]
[]
[null,"…………………………………………………"]
[]
[null,"Tel No: "]
[null,"Fax No: "]
[]
[null,"CONTRACT DETAILS "]
[]
[null,"\tWorks description:  "]
[]
[null,"The work comprises…."]
[]
[null,"\tSite description:"]
[]
[null,"\tThe sites for the works is:"]
[]
[null,"\tWork or installations by direct contractors: N/A"]
[]
[null,"\tThis agreement is for a government contract:  N/A"]
[null," "]
[null,"\tDate on which possession of the site is intended to be given"]
[null,"\t"]
[null,"\tPeriod for the commencement of the works after the contractor takes possession  of the site: One (1) working day"]
[]
[null,"\tFor the works as a whole :"]
[]
[null,"\tDate for practical completion"]
[]
[null,"\tPenalties per calendar day:  R 4 000.00"]
[]
[null,"\tFor the works in sections: "]
[]
[null,"\tDate of practical completion and the penalty per calendar day for: "]
[]
[null,"\tDate:  N/A"]
[null,"\tPenalty:  N/A"]
[]
[null,"\tThe law applicable to this agreement: Republic of South Africa"]
[]
[null,"INSURANCES "]
[]
[null,"\tThe Contractor shall be liable for the First Amount payable (deductible) in  respect of each claim in terms of all policies affected by either the Contractor  or Employer.          "]
[]
[null,"\tContract works insurance effected by: Contractor"]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"\tFor the amount of:  The contract sum plus 30%"]
[]
[null,"\tWith a deductible of: To be advised"]
[]
[null,"\tSupplementary insurance required: Employer"]
[]
[null,"\tFor the amount: To be advised"]
[]
[null,"\tWith a deductible of: To be advised"]
[]
[null,"\tPublic liability insurance to be effected by: Contractor"]
[]
[null,"\tFor the amount of:  R 3 000 000.00"]
[]
[null,"\tWith a deductible of: To be determined by the Contractor"]
[]
[null,"\tSupport insurance - N/A"]
[]
[null,"DOCUMENTS "]
[]
[null,"Waiver of the contractor's lien is required: Yes "]
[]
[null,"\tThe contractor's lien is hereby waived. The \tcontractor's right in terms of  clause 3.2 to receive a payment  guarantee from the Employer in terms of  clause 3.1 is also waived"]
[]
[null,"\tConstruction document copies to be supplied to the contractor free of charge: "]
[]
[null,"\tBills of Quantities: Two copies and Drawings: Four sets"]
[]
[null,"\tBills of quantities/schedule of rates drawn up in accordance with a system  other than the Standard System of Measuring Building Work:"]
[]
[null,"\tBuilding works is drawn up in accordance with the Standard System of  Measuring Building work (Sixth Edition)."]
[]
[null,"\tPriced Bills of Quantities to be submitted with tender : Yes"]
[]
[null,"\tJBCC Engineering General Conditions are to be included in the contract  documents:  Yes "]
[]
[null,"\tThe contract value is to be adjusted using CPAP indices: No  "]
[]
[null,"\tThis is a fixed price contract and no adjustment due to inflationary cost  increase will be entertained"]
[]
[null,"\tDetails of changes made to the provisions of JBCC standard documentation:"]
[null,"\t1.\tClause 3.2: No payment guarantee provided by the Employ"]
[]
[null,"\t2.\tClause 31.6.5:\tMaterial off site will not be included in payment certificates."]
[]
[null,"\t3.\tClause 31.9: Payment by Employer will be within 21 calendar days"]
[]
[null,"\t4.\tThe Employer shall not pay compensatory interen terms of"]
[null,"\t\tClause 31.10"]
[]
[null,"\t5.\tClause 34.0:  Amplification of payment interest amounts."]
[]
[null,"POST TENDER INFORMATION  "]
[]
[null,"\tThe latest day of the month for the issue of an interim payment certificate: "]
[]
[null,"\t2nd day \t"]
[]
[null,"\tPayment of preliminaries:  To be selected by Contractor (A or B) \t"]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"\tAdjustment of preliminaries: To be selected by Contractor (A or B) "]
[]
[null,"\tThe Employer will not effect a payment guarantee "]
[]
[null,"\tSecurities to be provided: To be selected by contractor"]
[]
[null,"\tAnnual building holiday period: To be advised"]
[]
[null,"SECTION B : PRELIMINARIES  "]
[]
[null,"Definitions and interpretation (Clause 1.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Documents  "]
[]
[null,"Checking of documents (Clause 2.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Drawings indicating the scope of work is issued with this bill of quantities. A complete  set of drawings is available at the offices of  the Principal Agent. The tenderer shall  scrutinise these drawings to ensure that all aspects of the works, requirements, scope  and programming are included in the tender sum"]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Provisional bills of quantities (Clause 2.2) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"These Bills of Quantities shall not be used for ordering purposes"]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Availability of construction documentation (Clause 2.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Interest of agents (Clause 2.4) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Priced documents (Clause 2.5) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Tender submission (Clause 2.6) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"The site  "]
[]
[null,"Defined works area (Clause 3.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"The area of the works to be occupied by the contractor for site establishment, material  deliveries, etc. will be pointed out at the site inspection."]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Geotechnical investigation (Clause 3.2) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Inspection of the site (Clause 3.3)","Item",{"v":1,"d":"1.00"}]
[]
[null,"No claims for extras arising from the contractor having failed to comply with this  clause will be entertained"]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Refer to compulsory site inspection in Notes to Tenderers"]
[]
[null,"F:....................... V:......................... T:............................."]
[]
[null,"Existing premises occupied (Clause 3.4) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Care shall be taken to allow full access on the site for surrounding tenants and public.  The contractor shall ensure adequate functioning of the building services to existing  occupied areas at all times"]
[]
[null,"Change over procedures for building services shall be agreed with the Principal Agent"]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Previous work - dimensional accuracy (Clause 3.5) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Previous work - defects (Clause 3.6) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Services - known (Clause 3.7) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Services - Unknown (Clause 3.8) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Protection of trees (Clause 3.9) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Articles of value (Clause 3.10) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Inspection of adjoining properties (Clause 3.11) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:........................ T:............................."]
[]
[null,"Management of contract  "]
[]
[null,"Management of the works (Clause 4.1)","CONT",{"v":1,"d":"1.00"}]
[]
[null,"Clause 4.1 shall be deemed to be amended by the addition of the following:"]
[]
[null,"The contractor shall, to the satisfaction of the Principal Agent, provide the services of  an experienced and competent Construction Manager and Site Agent supported by a  management team who shall, inter alia be responsible for all activities of the  contractor and all subcontractors and in particular:"]
[null,"(a) Programming"]
[null,"(b) Scheduling"]
[null,"(c)\t Reporting"]
[null,"(d)\t Production of shop drawings and samples"]
[null,"(e)\t Procurement and expediting"]
[null,"(f)\t Liaison and co-ordinating of construction"]
[null,"(g)\t Commissioning, instruction, handover and \tfollow up  "]
[null,"(h)\t Monitoring and reporting on building \tactivities  taking place on site"]
{"$rows_empty":8}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"The names and CV's of the contractor's site management team shall be submitted to  the principal agent prior to commencement on site and, after the principal agent's  agreement on the composition thereof has been obtained, no changes shall be made  nor shall any member of the said team be removed from the site while remaining in the  employ of the contractor without the principal agent's express written approval"]
[]
[null,"F:.................... V:..................... T:............................","Item",{"v":1,"d":"1.00"}]
[]
[null,"Programme for the works (Clause 4.2)","CONT",{"v":1,"d":"1.00"}]
[]
[null,"Clause 4.2 shall be deemed to be amended by the addition of the following:"]
[]
[null,"The program shall be prepared  by the contractor prior to commencement of  construction and shall be presented in the form of a network in accordance with the  procedures generally referred to as programme evaluation review techniques  (PERT)  or critical path method (CPM) in precedent format. The network shall be analysed and  shall include as a minimum, graphic representations (bar chart and network)  indicating all significant activities and critical paths, milestones and events involved  in the construction of the project."]
[]
[null,"The network analysis, as described, shall be agreed with the principal agent and no  subsequent changes are to be made without his prior written approval"]
[]
[null,"The contractor shall incorporate into his network analysis the work being performed  by all sub-contractors, selected, nominated or otherwise, so that all work involved is  shown in the network analysis for the complete project"]
[]
[null,"The network graphic representation must clearly depict the sequence of the activities  planned by the contractor, their interdependence and time required to perform each  activity. In developing the project network, the contractor shall use arrow or  precedence notation."]
[]
[null,"Activities shown on the network shall consist not only of the actual construction  operations, but shall also include the submission of shop drawings and samples and  approvals therefor, procurements of materials and equipment, fabrication and delivery  of materials, installation and testing of major and critical items, contiguous or related  work under sub-contracts or under other contracts and all other items pertinent to the  work. Related activities shall be grouped on the network for simplification. The  selection of all activities shall be subject to approval by the principal agent."]
[]
[null,"The contractor shall submit a separate schedule of information regarding selected  sub-contractors indicating dates of information required and dates of sub-contractors  required on site.","CONT",{"v":1,"d":"1.00"}]
[]
[null,"The contractor shall furnish, with the initial network analysis, a tabular listing of all  activities listed on the network analysis. For each activity there shall be listed the  earliest and latest start and finish times and the float. Activities on the critical path  shall be so indicated."]
[]
[null,"Only the latest drawings available shall be used by the contractor as a basis for  drawing up the network and not the quantities contained in these Bills of Quantities."]
[]
[null,"Programme Updates:"]
[]
[null,"During the progress of the work, the contractor shall agree progress on a two weekly  basis with the principal agent and update the network accordingly for reporting and  monitoring purposes. Items on the critical path shall be clearly identified"]
[]
[]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"In addition to the tabular report, the contractor shall provide a narrative report on the  construction progress and shall particularly note unusual conditions encountered that  may have delayed progress of the work. In the event of such delays, he shall describe  actions proposed to overcome adverse conditions to maintain the planned schedule  completion dates."]
[]
[null,"Variations/Amendments:"]
[]
[null,"The contractor shall throughout the progress of the contract amend and update the  network to incorporate all variations, new drawings and site instructions and all such  amendments are subject to the principal agent's approval."]
[]
[null,"The contractor shall not amend the completion dates of the project unless extensions  of time have been granted by the principal agent in terms of Clause 29.0 of the  agreement"]
[]
[null,"Work behind program:","Item",{"v":1,"d":"1.00"}]
[]
[null,"If in the opinion of the principal agent, the contractor, through causes under his  control, falls behind programme, the contractor shall take such steps as may be  necessary to improve his progress. The principal agent may require him to increase  the number of shifts and/or overtime operations, days of work and/or the amount of  construction plant, all without additional cost to the Employer. The contractor shall  submit for the approval of the principal agent, a revised network in the form required  above in order to demonstrate the manner in which the agreed rate of progress shall  be registered."]
[]
[null,"Float indicated on the contract programme shall be shared by the contractor and  Employer on a 50:50 basis"]
[]
[null,"F:............................. V:......................... T:..........................."]
[]
[null,"Progress meetings (Clause 4.3)","Item",{"v":1,"d":"1.00"}]
[]
[null,"The contractor shall provide the principal agent at the progress meetings, with all the  available information in report form concerning the condition and progress of his and  his sub-contractor's work"]
[]
[null,"The principal agent's progress meetings shall be held as notified and based on formal  agenda established by the principal agent. These meetings shall be attended by all  agents and by at least the contractor's contract manager and his site agent as  directed, and will be chaired and minuted by the principal agent."]
[]
[null,"The principal agent shall issue a schedule of progress meetings."]
[]
[null,"The Employer's Representative/internal project leader may attend progress meetings."]
[]
[null,"The contractor shall submit a summarised progress report at the progress meetings  covering all aspects of the work, including a statement of his assessment of the work  progress, any delays, labour complement and construction plant and equipment"]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Technical meetings (Clause 4.4) "]
[]
[null,"The contractor shall convene, under his chairmanship, regular meetings with  nominated, selected and other sub-contractors for the purpose of establishing  co-ordination and progress of the works and all other matters, queries, etc. , relating  to their individual sub-contracts and schedule in order to allow the contractor to  report at the progress meetings","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Labour and plant records (Clause 4.5) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Samples, shop drawings and manufacturer's instructions "]
[]
[null,"Samples of materials (Clause 5.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Workmanship samples (Clause 5.2)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Shop drawings (Clause 5.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Compliance with manufacturers instructions (Clause 5.4) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Temporary works and plant  "]
[]
[null,"Deposits and fees (Clause 6.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Enclosure of the works (Clause 6.2)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Advertising (Clause 6.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null," Plant, equipment, sheds and offices (Clause 6.4) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Main noticeboard (Clause 6.5) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Subcontractors noticeboard (Clause 6.6) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Temporary services  "]
[]
[null,"Location (Clause 7.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Water (Clause 7.2)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Alternative B will apply: Free of charge but contractor to install a meter for monitoring  purposes"]
[]
[null,"F:............................. V:.......................... T:..........................."]
[]
[null,"Electricity (Clause 7.3)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Alternative B will apply: Free of charge but contractor to install a meter for monitoring  purposes"]
[]
[null,"F:........................... V:........................... T:............................."]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Telecommunication facilities (Clause 7.4)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Alternative A:  Contractor to supply a telephone"]
[]
[null,"F:..................... V:...................... T:..........................."]
[]
[null,"Ablution facilities (Clause 7.5)","Item",{"v":1,"d":"1.00"}]
[]
[null,"Alternative A: Contractor to provide"]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Prime cost amounts  "]
[]
[null,"Responsibility for prime cost amounts (Clause 8.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Attendance on N/S subcontractors  "]
[]
[null,"General attendance (Clause 9.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Special attendance (Clause 9.2) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Commissioning -fuel, water and electricity (Clause 9.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Financial aspects  "]
[]
[null,"Statutory taxes duties and levies (Clause 10.1) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"Rates for quantities shall exclude VAT as provision is made in the summary of these  Bills for VAT"]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Payment of preliminaries (Clause 10.2)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Adjustment of preliminaries (Clause 10.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"Payment certificate cash flow (Clause 10.4) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[null,"General  "]
[]
[null,"Protection of the works (Clause 11.1)","Item",{"v":1,"d":"1.00"}]
[]
[null,"The contractor shall ensure that dust be contained to the absolute minimum - this will  be strictly monitored."]
[]
[null,"The contractor shall provide for the protection of all work for which a certificate of  practical completion has not been issued."]
[]
[null,"The contractor shall be responsible for any damage which may occur and shall make  good at his own expense "]
[]
[null,"F:......................... V:.......................... T:............................."]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Protection/isolation of existing/sectionally occupied works (Clause 11.2) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:......................... V:............................. T:............................."]
[]
[null,"Security of the works(Clause 11.3) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"All workmen shall be clearly identifiable at all times as authorized construction  workers and non-compliance will result in a person being evicted from site. "]
[]
[null,"Workers will be restricted to the immediate vicinity of building operations"]
[]
[null,"Refer also to Notes to Tenderers"]
[]
[null,"F:............................. V:....................... T:............................."]
[]
[null,"Notice before covering work (Clause 11.4)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:........................ V:......................... T:............................. "]
[]
[null,"Disturbance (Clause 11.5) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"To least interfere with the occupants of the buildings, connections to services will  have to be done after hours and over weekends and Tenders shall allow for this in  their tenders"]
[]
[null,"F:......................... V:............................. T:............................."]
[]
[null,"Environmental disturbance (Clause 11.6) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"Works cleaning and clearing (Clause 11.7)","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"Vermin (Clause 11.8) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"Overhand work (Clause 11.9) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"Instruction manuals and guarantees (Clause 11.10) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"As built information (Clause 11.11) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"Tenant installations (Clause 11.12) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
[]
[null,"SCHEDULE OF VARIABLES  "]
[]
[null,"The schedule (Clause 12.0) ","Item",{"v":1,"d":"1.00"}]
[]
[null,"F:.......................... V:....................... T:............................."]
{"$rows_empty":7}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"12.1 PRE-TENDER INFORMATION"]
[]
[null,"12.1.1\t  Provisional Bills of Quantities (2.2):  "]
[]
[null,"\tThe quantities are provisional: Yes"]
[]
[null,"12.1.2\t  Availability of construction documentation (2.3):  "]
[]
[null,"\tConstruction documentation is complete: No"]
[]
[null,"12.1.3  \tInterest of agents (2.4): No interest"]
[]
[null,"12.1.4\t  Defined work area (3.1): "]
[]
[null,"\tThe area of the works to be occupied by the contractor, any restriction to the  area and the limit of access or exit will be pointed out to the contractor by the  principal agent at the compulsory site inspection"]
[]
[null,"12.1.5\t  Geotechnical Investigation (3.2): No"]
[]
[null,"12.1.6\t  Existing premises occupied (3.4): Yes"]
[]
[null,"12.1.7\t  Previous work - dimensional accuracy (3.5):  All measurements to be taken from the existing buildings. "]
[null," "]
[null,"12.1.8\t   Previous work defects (3.6): Yes"]
[]
[null,"12.1.9\t  Services - known (3.7): Yes"]
[]
[null,"12.1.10\t  Protection of trees (3.9): Yes"]
[]
[null,"12.1.11\t  Inspection of adjoining properties (3.11): N/A"]
[]
[null,"12.1.12  Enclosure of the works (6.2): "]
[]
[null,"12.1.13\t  Offices (6.4.3): Offices to be suitable for meeting with at least 12  persons in attendance"]
[]
[null,"12.1.14  \tMain noticeboard (6.5): Yes"]
[]
[null,"12.1.15  \tSubcontractor's noticeboard (6.6): Yes"]
[]
[null,"12.1.16  \tWater (7.2):"]
[]
[null,"\tOption B ( by employer - free of charge but the contractor to install a meter for  monitoring purposes): Yes"]
[]
[null,"12.1.17\t  Electricity (7.3): "]
[]
[null,"\tOption B ( by employer - free of charge but the contractor to install a meter for  monitoring purposes): Yes"]
[]
[null,"12.1.18\t Telecommunications (7.4): "]
[]
[null,"\tOption A  (by contractor): Yes"]
[]
[null,"12.1.19\t  Ablution facilities  (7.5): "]
[]
[null,"\tOption A ( by contractor):  Yes"]
[]
[null,"12.1.20\t  Protection of existing/sectionally occupied works (11.2): Yes"]
[]
[null,"12.1.21\t  Special attendance (9.2): No"]
[]
[null,"12.1.22\t Protection of the works (11.1):  No specific requirements"]
[]
[null,"12.1.23\t  Disturbance (11.5): Refer to clause 11.5"]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"12.1.23  \tEnvironmental disturbance (11.6): No specific requirements"]
[]
[null,"12.2  POST TENDER INFORMATION"]
[]
[null,"12.2.1\t  Payment of preliminaries: "]
[]
[null,"\tOption A ( prorated): To be selected by contractor"]
[]
[null,"\tOption B ( calculated): To be selected by contractor"]
[]
[null,"12.2.2\t  Adjustment of preliminaries: "]
[]
[null,"\tOption A ( three categories): To be selected by contractor"]
[]
[null,"\tOption B ( detailed breakdown): To be selected by contractor"]
[]
[null,"SECTION C - SPECIFIC PRELIMINARIES "]
[]
[null,"Proprietary branded products","Item",{"v":1,"d":"1.00"}]
[]
[null,"The contractor shall take delivery of, handle, store, use, apply and/or fix all proprietary  branded products in strict accordance with the manufacturer's instructions after consultation  with the manufacturer's authorized representative"]
[]
[null,"As built drawings","Item",{"v":1,"d":"1.00"}]
[]
[null,"The position of construction breaks and the extent of individual concrete pours are to be  recorded by the contractor on the structural engineer's drawings and are to be submitted to  the principal agent and the structural engineer for their records"]
[]
[null,"Contract Instructions","Item",{"v":1,"d":"1.00"}]
[]
[null,"Contract instructions issued on site are to be recorded in triplicate in a contract instruction  book which is to be supplied and maintained on site by the contractor"]
[]
[null,"Labour Records","Item",{"v":1,"d":"1.00"}]
[]
[null,"At the end of each week the contractor shall provide the principal agent with a written record,  in schedule form, reflecting the number and descriptions of tradesmen and labourers  employed by him and all sub-contractors on the works of each day of that week. Content and  format of such reports shall be to the approval of the principal agent "]
[]
[null,"Plant Record","Item",{"v":1,"d":"1.00"}]
[]
[null,"At the end of each week the contractor shall provide the principal agent with a written record,  in schedule form, reflecting the number, type and capacity of all plant, excluding hand tools  used on the works each day of that week. These records to include plant of sub-contractors.  Content and format of such reports shall be to the approval of the principal agent "]
[]
[null,"Overtime","Item",{"v":1,"d":"1.00"}]
[]
[null,"Should overtime be required to be worked for any reason whatsoever, the cost of such  overtime are to be borne by the contractor unless the principal agent has specifically  authorized, in writing, prior to execution thereof, that costs for such overtime are to be borne  by the employer"]
{"$rows_empty":9}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Co-operation of contractor for cost management","Item",{"v":1,"d":"1.00"}]
[]
[null,"It is specifically agreed that the contractor accepts the obligation of assisting the professional  consultants in implementing proper cost management. The contractor will be advised by the  principal agent of all cost management procedures which will be implemented to ensure that  the final building cost does not exceed the budget. The quantity surveyor undertakes to make  available to the contractor all budgetary allowances and cost assessments/reports to enable  the proper procedures to be implemented and the contractor will attend all cost plan review  and cost management meetings. The contractor undertakes to extend these procedures in  regard to all sub-contractors"]
[]
[null,"GENERAL PREAMBLES"]
[]
[null,"The document \"Specification of Materials and Methods to be used (PW371)\" is obtainable on the Department's website (http://www.publicworks.gov.za/ under \"Consultants Guidelines\"), and shall be read in conjunction with the bills of quantities / lump sum document and be referred to for the full descriptions of work to be done and materials to be used "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"TRADE NAMES"]
[]
[null,"Wherever a trade name for any product has been described in the bills of quantities / lump sum document, the tenderer's attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing date for submission of tenders If prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"IMPORTED MATERIALS AND EQUIPMENT"]
[]
[null,"Where imported items are listed in the tender documents, the tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency fluctuations. (refer to Schedule of Imported Materials and Equipment DPW-23(EC) to be completed by tenderer)  Notwithstanding any provisions elsewhere regarding the adjustment of contract prices, the price of any item, material or equipment listed in terms of this clause shall be excluded from the Contract Price Adjustment Provisions (if applicable)"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"HIV/AIDS AWARENESS"]
[]
[null,"It is required of the contractor to thoroughly study the HIV/AIDS Specification (PW 1544) of the Department that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document. Provision for pricing of HIV/AIDS awareness is made under items C10.1 to C10.5 hereafter and it is explicitly pointed out that all requirements of the aforementioned specification are deemed to be priced hereunder, as the said items represent the only method of measurement and no additional items or extras to the contract in this regard shall be entertained  The contractor must take note that compliance with the HIV/AIDS Specification is compulsory. In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A 31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance. The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment"]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"AWARENESS CHAMPION"]
[]
[null,"Selection, appointment, briefing and making available of an Awareness Champion including provision of all relevant services, all in accordance with the HIV/AIDS Specification  "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"AWARENESS WORKSHOPS"]
[]
[null,"Selection and appointment of a competent Service Provider approved by the principal agent, provision of a Service Provider Workshop Plan and a suitable venue, conducting of awareness workshops by means of traditional and/or modern multi-media techniques, including follow-up courses, making available all tuition material and performing assessment procedures, all in accordance with the HIV/AIDS Specification "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"POSTERS, BOOKLETS, VIDEOS, ETC"]
[]
[null,"Provision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the duration of the construction period, all in accordance with the HIV/AIDS Specification","Item",1]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"ACCESS TO CONDOMS"]
[]
[null,"Provision and maintenance of condom dispensers fixed in position, including male and female condoms, replenishing male and female condoms on a daily basis as required for the duration of the construction period, all in accordance with the HIV/AIDS Specification"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"MONITORING"]
[]
[null,"Monitoring HIV/AIDS awareness of workers, providing the principal agent with access to information including making available all reports, thoroughly completed and reflecting the correct information, for the duration of the construction period and close out, all in accordance with the HIV/AIDS Specification "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"COVID-19 Compliance"]
[]
[null,"The contractor is to ensure the site is compliant with the COVID-19 protocols as gazetted and provided for with regards to the OHS specification"]
[]
[null,"Infra-red scanner","Item",1]
[null,"Cloth Masks (at least 3 per person)","Item",1]
[null,"Dust Mask FFP2","Item",1]
[null,"Hand sanitizer","Item",1]
[null,"Awareness and Warning Signage","Item",1]
[null,"Hand washing station","Item",1]
{"$rows_empty":10}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"OCCUPATIONAL HEALTH AND SAFETY"]
[]
[null,"The contractor shall comply with all the requirements set out in the Construction Regulations, 2003 issued under the Occupational Health and Safety Act, 1993 (Act No 85 of 1993)  It is required of the contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document  The contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.  In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment  Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced hereunder and no additional claims in this regard shall be entertained"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"NOTIFICATION OF CONSTRUCTION WORK"]
[]
[null," (Construction Regulation 3) The Contractor shall, before commencing work, notify the Department of Labour of the intended construction work in terms of Regulation 3.  The Contractor shall submit the notification in writing, on the appropriate form, prior to commencement of work "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"HEALTH AND SAFETY PLAN"]
[]
[null,"(Construction Regulation 5.4) The Contractor shall provide and demonstrate to the Principal Agent a suitable and sufficiently documented health and safety plan based on the Act, Construction Regulations and the health and safety specification, which shall be applied from the date of commencement of and for the duration of the construction work.  The Contractor shall ensure that a copy of the health and safety plan is available on request to an employee, inspector, sub contractor or principal agent all in terms of Regulation 5"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"REGISTRATION WITH COMPENSATION FUND"]
[]
[null,"(Construction Regulation 5.3 f) The Contractor shall provide proof of his registration and good standing with the Compensation Fund or a licensed compensation insurer prior to the commencement of work"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"HEALTH AND SAFETY FILE"]
[]
[null,"( Construction Regulation 5.7)  The Contractor shall ensure that a health and safety file, which shall include all documentation required in terms of the health and safety specification, the Act and the Construction Regulations, is opened and kept on site and made available to the Principal Agent or Inspector upon request.  Upon completion of the works, the Contractor shall hand over a consolidated health and safety file to the principal agent"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"SUPERVISION OF CONSTRUCTION WORK (SAFETY OFFICER)"]
[]
[null,"(Construction Regulation 6)  The Contractor shall appoint a full-time competent employee in writing as the construction supervisor, with the duty of supervising the construction work. The Contractor shall appoint a full-time or part-time construction safety officer in writing to assist in the control of all safety related aspects on the site. Such appointments are required to ensure that at all times the requirements of the Act and Construction Regulations are adhered to. Refer to Regulation 6 "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"RISK ASSESSMENT AND SAFETY POLICY"]
[]
[null," (Construction Regulation 7)  Before commencing work the Contractor shall cause a risk assessment to be performed by a competent person appointed in writing and the risk assessment shall form part of the health and safety plan. A copy of the risk assessment shall be available on site at all times for inspection. The Contractor shall at all time carry out the works in a manner to avoid the risk of bodily harm to persons or risk of damage to any property.  He shall take all precautions regarding training of employees in any hazards and the related work procedures, health and safety induction training of employees, visitors or any other persons entering the site and provide personal protective equipment to all employees and visitors to site which are necessary and adequate to eliminate any conditions which contribute to the risk of injury to persons or damage to property in terms of Regulation 7 "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"SIGNIFICANT HAZARD IDENTIFICATION RISK ASSESSMENT"]
[]
[null,"The contractor shall allow for additional financial provision, if any, to take the necessary precautions regarding the significant hazards and risks identified and assessed by the design consultants "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"ADDITIONAL FINANCIAL PROVISION"]
[]
[null,"The Contractor shall allow for additional financial provision, if any, to comply with the requirements of the Occupational Health and Safety Act  (Act No 85 of 1993) and the Construction Regulations issued there under which have not been specifically elsewhere provided"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"FALL PROTECTION PLAN"]
[]
[null,"(Construction Regulation 8)  The contractor shall, before commencing any construction work submit a fall protection plan identified all steps to be taken in order to ensure the continued adherence to the fall protection plan and shall include a risk assessment of all work carried out from an relevant position. The fall protection plan shall form part of the health and safety plan and file "]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"PHYSICAL AND PSYCHOLOGICAL FITNESS"]
[]
[null,"(Construction Regulation 8.2(b))  The contractor and sub-contractors shall before commencing any construction work submit proof of his employees that shall carried out work from an elevated position their physical and psychological fitness. And shall be recorded in the health and safety file "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[]
[]
[]
[]
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"CONSTRUCTION VEHICLES AND MOBILE PLANT"]
[]
[null,"(Construction Regulation 21)  The contractor and sub-contractors shall ensure that all operated workers received training and been certified competent to operate such vehicle, and are physical and psychological fit to operate such construction vehicles and mobile plants. And shall be recorded in the health and safety file "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"TRAINING"]
[]
[null,"(Construction Regulation 8 (c))  The contractor and sub-contractors shall, before commencing any construction work, submit his training program of all his employees. This program shall from part of the health and safety plan  "]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"DEMOLITION WORK"]
[]
[null,"(Construction Regulation 12)  The contractor shall, before any demolition work shall carried out, submit all method of demolition to be used. This method shall form part of the health and safety plan and file."]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"REMOVAL AND DISPOSAL OF ASBESTOS MATERIAL"]
[]
[null,"(Asbestos Regulation) The principal contractor shall appoint a contractor that is registered with the Department of Labour as an AIA. The contractor must allow for; NOTIFICATION OF ASBESTOS PROCESSING PERSONAL PROTECTIVE EQUIPMENT PACKAGING AND TRANSPORT AND STORAGE TO DISPOSAL SITE DEMOLITION WORK OF SHEETS LABELLING AND INFORMATION"]
[]
[null,"F:.......................... V:....................... T:.............................","Item",1]
[]
[null,"Category: Fixed","Item",1]
[null,"Category: Value","Item",1]
[null,"Category: Time","Item",1]
{"$rows_empty":29}
[null,"Carried to Collection"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"MAIN COLLECTION","Page"]
[]
[null,"Brought forward ",1]
[]
[null,null,{"$f":"C1302+1","v":2}]
[]
[null,null,{"$f":"C1304+1","v":3}]
[]
[null,null,{"$f":"C1306+1","v":4}]
[]
[null,null,{"$f":"C1308+1","v":5}]
[]
[null,null,{"$f":"C1310+1","v":6}]
[]
[null,null,{"$f":"C1312+1","v":7}]
[]
[null,null,{"$f":"C1314+1","v":8}]
[]
[null,null,{"$f":"C1316+1","v":9}]
[]
[null,null,{"$f":"C1318+1","v":10}]
[]
[null,null,{"$f":"C1320+1","v":11}]
[]
[null,null,{"$f":"C1322+1","v":12}]
[]
[null,null,{"$f":"C1324+1","v":13}]
[]
[null,null,{"$f":"C1326+1","v":14}]
[]
[null,null,{"$f":"C1328+1","v":15}]
[]
[null,null,{"$f":"C1330+1","v":16}]
[]
[null,null,{"$f":"C1332+1","v":17}]
[]
[null,null,{"$f":"C1334+1","v":18}]
[]
[null,null,{"$f":"C1336+1","v":19}]
[]
[null,null,{"$f":"C1338+1","v":20}]
[]
[null,null,{"$f":"C1340+1","v":21}]
[]
[null,null,{"$f":"C1342+1","v":22}]
[]
[null,null,{"$f":"C1344+1","v":23}]
{"$rows_empty":20}
[null,"Carried to Final Summary"]
[null,"Bill No. 1 "]
[null,"Preliminaries"]
[]
[null,"Bill No. 2"]
[]
[2.1,"DEMOLITIONS"]
[]
[null,"ALL BLOCKS"]
[]
[null,"REMOVAL OF ASBESTOS ROOF SHEETING"]
[]
[null,"Tenderers are requested to inspect the works and check for themselves the site conditions which are likely to affect the progress of their work. No claims by the contractor will be considered by the Principal Agent afterwards"]
[]
[null,"The contractor entrusted to carry out the works should be experienced in such demolition work involving the handling and removal of asbestos contaminated materials, and must be fully aware of the risks involved when working with asbestos. A brief description of works is to be submitted with the tender documents."]
[]
[null,"The contractor is responsible to provide the appropriate personal protective equipment and be proficient in the different work practices which are appropriate for such works.  Monitoring of the atmosphere for possible contamination during the works is to be carried out in accordance with the Occupational Health and Safety Act 85 of 1993 and/or any other equivalent legislation."]
[]
[null,"A written authorization from the OHS Authority is to be obtained, setting out the conditions and procedures to be followed in the handling and removal of asbestos containing  material"]
[]
[null,"The contractor shall obtain from the competent authorities all permits, and licences required by law for the removal and disposal of asbestos containing material."]
[null,"A copy of these permits to be handed to the Principal Agent prior to commencement of the works"]
[]
[null,"The work procedure as approved by the OHS is to be made available to the Principal Agent. The contractor is to inform the relevant authorities and the Principal Agent if changes are to be made to this work procedure."]
[]
[null,"The contractor is to take full responsibility of the asbestos contaminated material once it has been removed from site. He will be responsible for the transportation to an approved dumping site."]
[]
[null,"The contractor is to submit to the Principal Agent a certificate showing that the asbestos has been disposed of."]
[]
[null,"On completion of the works the contractor should use appropriate cleaning methods to clean the site where work was carried out of any traces of dust or debris."]
[]
[null,"All fees paid in connection with the application for the works shall be borne by the contractor."]
[]
[null,"Allow for any cost not included in the price of the above items arising from the contractor's obligation to adhere to the conditions for the handling of asbestos"]
[]
[null,"Carefully remove the existing Asbestos roof sheeting from roof trusses and/or rafters inclusive of the dismantling, repairing of the support framework, load and cartaway from site. (Rate to include for sealing off building)."]
[]
[null,"Allow for cost and charges for the disposal of asbestos "]
{"$rows_empty":7}
[null,"Carried to Collection"]
[null,{"$f":"B1371","v":"Bill No. 2"}]
[null,"Demolitions: Removal of Asbestos"]
[]
[null,"Allow for any costs for the cleaning of the site, including the roof structure from any traces of asbestos dust or debris."]
[]
["2.1.1","Guard House","m2",{"v":4,"d":"4.00"}]
["2.1.2","Mini Administration Block","m2",{"v":49.025,"d":"49.03"}]
["2.1.3","4 Classroom Block","m2",{"v":322,"d":"322.00"}]
["2.1.4","5 Classroom Block","m2",{"v":417.9,"d":"417.90"}]
["2.1.5","Tuckshop, Computer Room and 2 Classroom Block","m2",{"v":322,"d":"322.00"}]
["2.1.6","Staff Room and 3 Classroom Block","m2",{"v":334.4,"d":"334.40"}]
["2.1.7","4 Classroom Block and 2 HOD Offices","m2",{"v":365.2,"d":"365.20"}]
["2.1.8","2 Classroom Block","m2",{"v":190.3,"d":"190.30"}]
[2.2,"Completely remove existing wire mesh fencing and prepare surfaces to receive new","m",{"v":380,"d":"380.00"}]
{"$rows_empty":55}
[null,"Carried to Collection"]
[null,{"$f":"B1413","v":"Bill No. 2"}]
[null,{"$f":"B1414","v":"Demolitions: Removal of Asbestos"}]
[]
[null,{"$f":"B1483","v":"Bill No. 2"}]
[null,{"$f":"B1484","v":"Demolitions: Removal of Asbestos"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",25]
[]
[null,null,26]
{"$rows_empty":62}
[null,"Carried to Summary"]
[null,{"$f":"B1483","v":"Bill No. 2"}]
[null,{"$f":"B1484","v":"Demolitions: Removal of Asbestos"}]
[]
[]
[]
[]
[null,"Block A: Guard House"]
[]
["A.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["A.1.2","One brick walls.","m2",2]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["A.1.3","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",4]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and  making good surfaces to receive new"]
[]
["A.1.4","Timber door 813 x 2032mm high","No",1]
["A.1.5","Steel windows in various sizes not exceeding 1.5 m²","No",2]
[]
[null,"Taking out and removing joinery fittings etc and making good to  surfaces to receive new.",{"$nulls":4},{"$f":"D1583*E1583","v":0}]
[{"$nulls":6},{"$f":"D1584*E1584","v":0}]
["A.1.6","Fascia boards","m",4,null,null,{"$f":"D1585*E1585","v":0}]
["A.1.7","Barge boards.","m",4,null,null,{"$f":"D1586*E1586","v":0}]
["A.1.8","Roof gutters","m",2]
["A.1.9","Downpipes","m",3]
[]
[null,"Taking out and removing ironmongery "]
[]
["A.1.10","Mortice lock and striking plate from timber door and steel frame","No",1]
["A.1.11","Stays, latches, handles, etc from window steel frame","No",2]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["A.1.12","Chipping of screed in floors to receive new screed. ","m2",4]
["A.1.13","Cleaning internal walls to receive paint.","m2",{"v":22.4,"d":"22"}]
["A.1.14","Cleaning external walls to receive paint.","m2",{"v":22.4,"d":"22"}]
["A.1.15","Hack off existing plaster and make good to receive new.","m2",3]
["A.1.16","Cleaning and removing broken glazing, putty and paint to window frames","m2",2,null,null,{"$f":"SUM(G1564:G1598)","v":0}]
{"$rows_empty":25}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-1 Alterations"]
[]
[]
[null,{"$f":"B1627","v":"Block A: Guard House: A-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",28]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B1627","v":"Block A: Guard House: A-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["A.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["A.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",1]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["A.2.2","Soft rock","m3",1]
[]
["A.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["A.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",1]
[]
["A.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["A.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",1]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["A.2.7","Soil Poisoning under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",1]
[]
["A.2.8","To bottoms and sides of trenches etc","m2",1,null,null,{"$f":"SUM(G1704:G1733)","v":0}]
{"$rows_empty":32}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-2 Earthworks"]
[]
[]
[null,{"$f":"B1769","v":"Block A: Guard House: A-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",30]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B1769","v":"Block A: Guard House: A-2 Earthworks"}]
[]
[]
["A.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["A.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",1]
[]
[null,"TEST BLOCKS"]
[]
["A.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",1]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood float finish"]
[]
["A.3.3","Surface beds, slabs, etc","m2",2]
[]
[null,"Rough formwork to sides"]
[]
["A.3.4","To sides n.e. 300mm","m2",1]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["A.3.5","15mm Joints not exceeding 300mm high or wide","m",1]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["A.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",1]
[]
[null,"Saw cut joints"]
[]
["A.3.7","50 x 3mm Saw cut joints in top of concrete","m",1]
[]
[null,"Fabric reinforcement"]
[]
["A.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",1,null,null,{"$f":"SUM(G1847:G1880)","v":0}]
{"$rows_empty":28}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B1912","v":"Block A: Guard House: A-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",32]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B1912","v":"Block A: Guard House: A-3  Concrete, Formwork and Reinforcement"}]
[]
["A.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
["A.4.1","One brick walls","m2",2]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["A.4.2","150mm Wide reinforcement built in horizontally","m",{"$f":"D1993*2.94","v":5.88}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["A.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",2,null,null,{"$f":"SUM(G1991:G2002)","v":0}]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-4 Masonry"]
[]
[]
[null,{"$f":"B2056","v":"Block A: Guard House: A-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",34]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2056","v":"Block A: Guard House: A-4 Masonry"}]
[]
["A.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications.",{"$nulls":4},{"$f":"D2137*E2137","v":0}]
[]
["A.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",4,null,null,{"$f":"D2139*E2139","v":0}]
[]
["A.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",2,null,null,{"$f":"D2141*E2141","v":0}]
[]
["A.5.3","Narrow and broad flute closers","m",2,null,null,{"$f":"D2143*E2143","v":0}]
[]
["A.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",2]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation",{"$nulls":4},{"$f":"D2149*E2149","v":0}]
[]
["A.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",{"$f":"D2137","v":4},null,null,{"$f":"SUM(G2132:G2148)","v":0}]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-5 Roof Coverings"]
[]
[]
[null,{"$f":"B2194","v":"Block A: Guard House: A-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",36]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2194","v":"Block A: Guard House: A-5 Roof Coverings"}]
[]
["A.6","CARPENTRY AND JOINERY"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement",{"$nulls":4},{"$f":"D2275*E2275","v":0}]
[]
["A.6.1","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",4,null,null,{"$f":"D2277*E2277","v":0}]
[]
["A.6.2","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",4]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["A.6.4","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",1,null,null,{"$f":"SUM(G2269:G2282)","v":0}]
{"$rows_empty":49}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B2335","v":"Block A: Guard House: A-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",38]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2335","v":"Block A: Guard House: A-6 Carpentry and Joinery"}]
[]
["A.7","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["A.7.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",1]
["A.7.2","Stays, latches, handles, hinges, etc to existing window frames","No",2]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["A.7.3","50mm High plastic letter or numeral","No",1]
[]
["A.7.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",1,null,null,{"$f":"SUM(G1982:G2422)","v":0}]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-7 Ironmongery"]
[]
[]
[null,{"$f":"B2478","v":"Block A: Guard House: A-7 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",40]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2478","v":"Block A: Guard House: A-7 Ironmongery"}]
[]
["A.8","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete",{"$nulls":4},{"$f":"D2559*E2559","v":0}]
[{"$nulls":6},{"$f":"D2560*E2560","v":0}]
["A.8.1","23mm Thick on floors and landings ","m2",4]
["A.8.2","25mm Thick on floors and landings to verandas and steps","m2",1]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork",{"$nulls":4},{"$f":"D2566*E2566","v":0}]
[{"$nulls":6},{"$f":"D2567*E2567","v":0}]
["A.8.3","On walls in patches and repairing cracks","m2",22.4]
["A.8.4","On narrow widths","m2",2]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork",{"$nulls":4},{"$f":"D2573*E2573","v":0}]
[{"$nulls":6},{"$f":"D2574*E2574","v":0}]
["A.8.5","On walls in patches and repairing cracks","m2",22.4]
["A.8.6","On narrow widths","m2",2]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["A.8.7","Granolithic paved floors and skirtings","m2",4,null,null,{"$f":"SUM(G2552:G2566)","v":0}]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-8 Plastering"]
[]
[]
[null,{"$f":"B2620","v":"Block A: Guard House: A-8 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",42]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2620","v":"Block A: Guard House: A-8 Plastering"}]
[]
["A.9","TILING"]
[]
[null,"WALL TILING"]
[]
[null,"300 x 300 x 6mm ceramic wall tiles fixed with adhesive to cement render (cement render elsewhere) and flush pointed with tinted grout",{"$nulls":4},{"$f":"D2701*E2701","v":0}]
[]
["A.9.1","On splashbacks","m2",1,null,null,{"$f":"SUM(G2694:G2700)","v":0}]
{"$rows_empty":61}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-9 Tiling "]
[]
[]
[null,{"$f":"B2765","v":"Block A: Guard House: A-9 Tiling "}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",44]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2765","v":"Block A: Guard House: A-9 Tiling "}]
[]
["A.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium",{"$nulls":4},{"$f":"D2846*E2846","v":0}]
[]
["A.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",4,null,null,{"$f":"D2848*E2848","v":0}]
[]
["A.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",3,null,null,{"$f":"D2850*E2850","v":0}]
[{"$nulls":6},{"$f":"D2851*E2851","v":0}]
["A.10.3","Extra for angle","No",2,null,null,{"$f":"D2852*E2852","v":0}]
["A.10.4","Extra for stop end","No",2,null,null,{"$f":"D2853*E2853","v":0}]
["A.10.5","Extra for outlet for 100mm pipe","No",1]
["A.10.6","Extra for eaves or plinth offset","No",1]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["A.10.7","4,5kg Carbon dioxide fire extinguisher","No",1]
{"$rows_empty":47}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B2909","v":"Block A: Guard House: A-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",46]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B2909","v":"Block A: Guard House: A-10 Plumbing and Drainage"}]
[]
["A.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["A.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",1,null,null,{"$f":"SUM(G2983:G2989)","v":0}]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-11 Glazing"]
[]
[]
[null,{"$f":"B3055","v":"Block A: Guard House: A-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",48]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3055","v":"Block A: Guard House: A-11 Glazing"}]
[]
["A.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on",{"$nulls":4},{"$f":"D3134*E3134","v":0}]
[{"$nulls":6},{"$f":"D3135*E3135","v":0}]
["A.12.1","Internal walls including gypsum coat where necessary","m2",22.4]
["A.12.2","In narrow widths","m2",2]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on",{"$nulls":4},{"$f":"D3139*E3139","v":0}]
[{"$nulls":6},{"$f":"D3140*E3140","v":0}]
["A.12.3","External walls including gypsum coat where necessary","m2",{"v":22.4,"d":"22"}]
["A.12.4","In narrow widths","m2",2]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on",{"$nulls":4},{"$f":"D3144*E3144","v":0}]
[]
["A.12.5","Fascias and barge boards","m",8]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel",{"$nulls":4},{"$f":"D3148*E3148","v":0}]
[{"$nulls":6},{"$f":"D3149*E3149","v":0}]
["A.12.6","Door frames","m2",1]
["A.12.7","Windows","m2",2]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint",{"$nulls":4},{"$f":"D3153*E3153","v":0}]
[]
["A.12.8","Doors","m2",3,null,null,{"$f":"SUM(G3132:G3152)","v":0}]
{"$rows_empty":37}
[null,"Carried to Collection"]
[]
[null,"Block A: Guard House: A-12 Paintwork"]
[]
[]
[null,{"$f":"B3193","v":"Block A: Guard House: A-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",50]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3193","v":"Block A: Guard House: A-12 Paintwork"}]
[]
[]
[null,"Block A: Guard House"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",29]
[]
[2,"Earthworks",31]
[]
[3,"Concrete, Formwork and Reinforcement",33]
[]
[4,"Masonry",35]
[]
[5,"Roof Coverings",37]
[]
[6,"Carpentry and Joinery",39]
[]
[7,"Ironmongery",41]
[]
[8,"Plastering",43]
[]
[9,"Tiling",45]
[]
[10,"Plumbing and Drainage",47]
[]
[11,"Glazing",49]
[]
[12,"Paintwork",51]
{"$rows_empty":41}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B3269","v":"Block A: Guard House"}]
[]
[]
[]
[]
[null,"Block B: Laboratory"]
[]
["B.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["B.1.1","One brick walls.","m²",10]
[]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
["B.1.2","Damaged shelving","No",2]
["B.1.3","Damaged chemical wash hand basin.","No",2]
["B.1.4","Fascia boards","m",29.82]
["B.1.5","Barge boards.","m",24]
["B.1.6","Roof gutters","m",29.82]
["B.1.7","Downpipes","m",12]
[]
[null,"Taking out and removing ironmongery "]
[]
["B.1.8","Mortice lock and striking plate from timber door and steel frame","No",3]
["B.1.9","Stays, latches, handles, etc from window steel frame","No",8]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["B.1.10","Cleaning internal walls to receive paint.","m²",{"v":169.736,"d":"170"}]
["B.1.11","Cleaning and removing broken glazing, putty and paint to window frames","m²",12]
{"$rows_empty":39}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-1 Alterations"]
[]
[]
[null,{"$f":"B3411","v":"Block B: Laboratory: B-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",53]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3411","v":"Block B: Laboratory: B-1 Alterations"}]
[]
["B.2","CARPENTRY AND JOINERY"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["B.2.1","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",29.82]
[]
["B.2.2","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",24]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["B.2.3","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",60.62]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["B.2.4","44mm Framed batten door 813 x 2032m high.","No",3]
{"$rows_empty":44}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-2 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B3553","v":"Block B: Laboratory: B-2 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",55]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3553","v":"Block B: Laboratory: B-2 Carpentry and Joinery"}]
[]
["B.3","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["B.3.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",30]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["B.3.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses (elsewhere measured).","m2",30]
[]
["B.3.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",4]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["B.3.4","75mm Coved cornices","m",20]
{"$rows_empty":46}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-3 Ceilings, Partitions and Access Flooring"]
[]
[]
[null,{"$f":"B3693","v":"Block B: Laboratory: B-3 Ceilings, Partitions and Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",57]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3693","v":"Block B: Laboratory: B-3 Ceilings, Partitions and Access Flooring"}]
[]
["B.4","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["B.4.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",3]
["B.4.2","Stays, latches, handles, hinges, etc to existing window frames","No",8]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["B.4.3","50mm High plastic letter or numeral","No",3]
[]
["B.4.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",3]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-4 Ironmongery"]
[]
[]
[null,{"$f":"B3836","v":"Block B: Laboratory: B-4 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",59]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3836","v":"Block B: Laboratory: B-4 Ironmongery"}]
[]
["B.5","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["B.5.1","23mm Thick on floors and landings ","m2",30]
["B.5.2","25mm Thick on floors and landings to verandas and steps","m2",{"v":22.256,"d":"22"}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["B.5.3","On walls in patches and repairing cracks","m2",10]
["B.5.4","On narrow widths","m2",5]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["B.5.5","Granolithic paved floors and skirtings","m2",30]
{"$rows_empty":36}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-5 Plastering"]
[]
[]
[null,{"$f":"B3978","v":"Block B: Laboratory: B-5 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",61]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B3978","v":"Block B: Laboratory: B-5 Plastering"}]
[]
["B.6","TILING"]
[]
[null,"WALL TILING"]
[]
[null,"300 x 300 x 6mm ceramic wall tiles fixed with adhesive to cement render (cement render elsewhere) and flush pointed with tinted grout"]
[]
["B.6.1","On splashbacks","m2",4]
{"$rows_empty":61}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-6 Tiling "]
[]
[]
[null,{"$f":"B4123","v":"Block B: Laboratory: B-6 Tiling "}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",63]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4123","v":"Block B: Laboratory: B-6 Tiling "}]
[]
["B.7","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["B.7.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",29]
[]
["B.7.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",12]
[]
["B.7.3","Extra for angle","No",8]
["B.7.4","Extra for stop end","No",4]
["B.7.5","Extra for outlet for 100mm pipe","No",4]
["B.7.6","Extra for eaves or plinth offset","No",4]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["B.7.7","4,5kg Carbon dioxide fire extinguisher","No",2]
[]
[null,"CHEMICAL LAB ACCESSORIES"]
[]
["B.7.8","Chemical lab wash hand basin to match existing.","No",2]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["B.7.9","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":32}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-7 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B4262","v":"Block B: Laboratory: B-7 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",65]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4262","v":"Block B: Laboratory: B-7 Plumbing and Drainage"}]
[]
["B.8","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["B.8.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",12]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-8 Glazing"]
[]
[]
[null,{"$f":"B4408","v":"Block B: Laboratory: B-8 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",67]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4408","v":"Block B: Laboratory: B-8 Glazing"}]
[]
["B.9","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["B.9.1","Internal walls including gypsum coat where necessary","m2",10]
["B.9.2","Narrow widths","m2",2]
["B.9.3","Internal ceilings","m2",97.37]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["B.9.4","Fascias and barge boards","m",29]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["B.9.5","Door frames","m2",3]
["B.9.6","Windows","m2",8]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["B.9.7","Doors","m2",9]
["B.9.8","Cornices, etc not exceeding 300mm girth","m",60.62]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["B.9.9","Skirtings, rails, etc not exceeding 300mm girth","m",60.62]
{"$rows_empty":37}
[null,"Carried to Collection"]
[]
[null,"Block B: Laboratory: B-9 Paintwork"]
[]
[]
[null,{"$f":"B4547","v":"Block B: Laboratory: B-9 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",69]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4547","v":"Block B: Laboratory: B-9 Paintwork"}]
[]
[]
[null,"Block B: Laboratory"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",54]
[]
[2,"Carpentry and Joinery",56]
[]
[3,"Ceilings, Partitions & Access Flooring",58]
[]
[4,"Ironmongery",60]
[]
[5,"Plastering",62]
[]
[6,"Tiling",64]
[]
[7,"Plumbing and Drainage",66]
[]
[8,"Glazing",68]
[]
[9,"Paintwork",70]
{"$rows_empty":47}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B4623","v":"Block B: Laboratory"}]
[]
[]
[]
[]
[null,"Block C: Mini Admin Block"]
[]
["C.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["C.1.1","One brick walls.","m2",{"v":10,"d":"10.00"}]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["C.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",{"v":5,"d":"5.00"}]
[]
["C.1.3","Tank stand","m2",{"v":9,"d":"9.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good surfaces to receive new"]
[]
["C.1.4","Timber door 813 x 2032mm high","No",{"v":3,"d":"3.00"}]
[]
[null,"Taking out and removing ironmongery "]
[]
["C.1.5","Mortice lock and striking plate from timber door and steel frame","No",{"v":3,"d":"3.00"}]
["C.1.6","Stays, latches, handles, etc from window steel frame","No",{"v":3,"d":"3.00"}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["C.1.7","Chipping of screed in floors to receive new screed. ","m2",39.59]
["C.1.8","Cleaning internal walls to receive paint.","m2",{"v":121.52000000000001,"d":"121.52"}]
["C.1.9","Cleaning external walls to receive paint.","m2",80.08]
["C.1.10","Hack off existing plaster and make good to receive new.","m2",{"v":50,"d":"50.00"}]
["C.1.11","Cleaning and removing broken glazing, putty and paint to window frames","m2",{"v":4,"d":"4.00"}]
{"$rows_empty":32}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-1 Alterations"]
[]
[]
[null,{"$f":"B4764","v":"Block C: Mini Admin Block: C-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",72]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4764","v":"Block C: Mini Admin Block: C-1 Alterations"}]
[]
["C.2","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["C.2.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",49.02500000000001]
[]
["C.2.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",8]
[]
["C.2.3","Narrow and broad flute closers","m",8]
[]
["C.2.4","Moulded narrow and broad rib polyethylene filler blocks","m",8]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["C.2.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",49.02500000000001]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-2 Roof Coverings"]
[]
[]
[null,{"$f":"B4902","v":"Block C: Mini Admin Block: C-2 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",74]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B4902","v":"Block C: Mini Admin Block: C-2 Roof Coverings"}]
[]
["C.3","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["C.3.1","38 x 114mm Wall plates","m",10]
[]
["C.3.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",24]
[]
[null,"Sundries"]
[]
["C.3.3","Two coats ABE Provinite on wrought timbers","m2",6]
[]
["C.3.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",8]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["C.3.5","Double pitched prefabricated plate nailed roof truss spanning approximately 3700mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",6]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["C.3.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",16]
[]
["C.3.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",12]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["C.3.8","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",3]
{"$rows_empty":28}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-3 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B5038","v":"Block C: Mini Admin Block: C-3 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",76]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5038","v":"Block C: Mini Admin Block: C-3 Carpentry and Joinery"}]
[]
["C.4","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["C.4.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",49.02500000000001]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["C.4.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",49.02500000000001]
[]
["C.4.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",1]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["C.4.4","75mm Coved cornices","m",43.400000000000006]
{"$rows_empty":46}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-4 Ceilings, Partitions and Access Flooring"]
[]
[]
[null,{"$f":"B5178","v":"Block C: Mini Admin Block: C-4 Ceilings, Partitions and Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",78]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5178","v":"Block C: Mini Admin Block: C-4 Ceilings, Partitions and Access Flooring"}]
[]
["C.5","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["C.5.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",3]
["C.5.2","Stays, latches, handles, hinges, etc to existing window frames","No",2]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["C.5.3","50mm High plastic letter or numeral","No",3]
[]
["C.5.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",3]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-5 Ironmongery"]
[]
[]
[null,{"$f":"B5320","v":"Block C: Mini Admin Block: C-5 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",80]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5320","v":"Block C: Mini Admin Block: C-5 Ironmongery"}]
[]
["C.6","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["C.6.1","23mm Thick on floors and landings","m2",{"v":49.02500000000001,"d":"49"}]
["C.6.2","25mm Thick on floors and landings to verandas and steps","m2",5]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["C.6.3","Granolithic paved floors and skirtings","m2",{"v":49.02500000000001,"d":"49"}]
{"$rows_empty":43}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-6 Plastering"]
[]
[]
[null,{"$f":"B5462","v":"Block C: Mini Admin Block: C-6 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",82]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5462","v":"Block C: Mini Admin Block: C-6 Plastering"}]
[]
["C.7","TILING"]
[]
[null,"WALL TILING"]
[]
[null,"300 x 300 x 6mm ceramic wall tiles fixed with adhesive to"]
[null,"cement render (cement render elsewhere) and flush"]
[null,"pointed with tinted grout"]
[]
["C.7.1","On splashbacks","m2",2]
{"$rows_empty":60}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-7 Tiling "]
[]
[]
[null,{"$f":"B5608","v":"Block C: Mini Admin Block: C-7 Tiling "}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",84]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5608","v":"Block C: Mini Admin Block: C-7 Tiling "}]
[]
["C.8","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["C.8.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",16]
[]
["C.8.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",9]
[]
["C.8.3","Extra for angle","No",6]
["C.8.4","Extra for stop end","No",4]
["C.8.5","Extra for outlet for 100mm pipe","No",3]
["C.8.6","Extra for eaves or plinth offset","No",3]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["C.8.7","4,5kg Carbon dioxide fire extinguisher","No",1]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["C.8.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":36}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-8 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B5747","v":"Block C: Mini Admin Block: C-8 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",86]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5747","v":"Block C: Mini Admin Block: C-8 Plumbing and Drainage"}]
[]
["C.9","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["C.9.1","Panes exceeding 0,5m2 and not exceeding 2m2","m2",3]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-9 Glazing"]
[]
[]
[null,{"$f":"B5893","v":"Block C: Mini Admin Block: C-9 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",88]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B5893","v":"Block C: Mini Admin Block: C-9 Glazing"}]
[]
["C.10","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["C.10.1","Internal walls including gypsum coat where necessary","m2",121.52000000000001]
["C.10.2","In narrow widths","m2",2]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["C.10.3","External walls including gypsum coat where necessary","m2",{"v":80.63999999999999,"d":"81"}]
["C.10.4","In narrow widths","m2",2]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["C.10.5","Fascias and barge boards","m",22]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["C.10.6","Door frames","m2",3]
["C.10.7","Windows","m2",3]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["C.10.8","Doors","m2",9]
{"$rows_empty":37}
[null,"Carried to Collection"]
[]
[null,"Block C: Mini Admin Block: C-10 Paintwork"]
[]
[]
[null,{"$f":"B6031","v":"Block C: Mini Admin Block: C-10 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",90]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6031","v":"Block C: Mini Admin Block: C-10 Paintwork"}]
[]
[]
[null,"Block C: Mini Admin Block"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C6113-2","v":72}]
[]
[2,"Roof Coverings",{"$f":"C6115-2","v":74}]
[]
[3,"Carpentry and Joinery",{"$f":"C6117-2","v":76}]
[]
[4,"Ceilings, Partitions and Access Flooring",{"$f":"C6119-2","v":78}]
[]
[5,"Ironmongery",{"$f":"C6121-2","v":80}]
[]
[6,"Plastering",{"$f":"C6123-2","v":82}]
[]
[7,"Tiling",{"$f":"C6125-2","v":84}]
[]
[8,"Plumbing and Drainage",{"$f":"C6127-2","v":86}]
[]
[9,"Glazing",{"$f":"C6129-2","v":88}]
[]
[10,"Paintwork",90]
{"$rows_empty":45}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B6107","v":"Block C: Mini Admin Block"}]
[]
[]
[]
[]
[null,"Block D: 4 Classroom Block"]
[]
["D.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["D.1.1","One brick walls.","m2",50]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["D.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",58]
[]
["D.1.3","Tank stand","m2",9]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good surfaces to receive new"]
[]
["D.1.4","Timber door 813 x 2032mm high","No",4]
[]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
["D.1.5","Fascia boards","m",60]
["D.1.6","Barge boards.","m",36]
["D.1.7","Roof gutters","m",60]
["D.1.8","Downpipes","m",30]
[]
[null,"Taking out and removing ironmongery "]
[]
["D.1.9","Mortice lock and striking plate from timber door and steel frame","No",4]
["D.1.10","Stays, latches, handles, etc from window steel frame","No",12]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["D.1.11","Chipping of screed in floors to receive new screed. ","m2",413]
["D.1.12","Cleaning internal walls to receive paint.","m2",327]
["D.1.13","Cleaning external walls to receive paint.","m2",220]
["D.1.14","Hack off existing plaster and make good to receive new.","m2",120]
["D.1.15","Cleaning and removing broken glazing, putty and paint to window frames","m2",17]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-1 Alterations"]
[]
[]
[null,{"$f":"B6247","v":"Block D: 4 Classroom Block: D-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",93]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6247","v":"Block D: 4 Classroom Block: D-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["D.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["D.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",5]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["D.2.2","Soft rock","m3",1]
["D.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["D.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",5]
[]
["D.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["D.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",30]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["D.2.7","Soil Poisoning under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",30]
[]
["D.2.8","To bottoms and sides of trenches etc","m2",10]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-2 Earthworks"]
[]
[]
[null,{"$f":"B6389","v":"Block D: 4 Classroom Block: D-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",95]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6389","v":"Block D: 4 Classroom Block: D-2 Earthworks"}]
[]
[]
["D.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["D.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",5]
[]
[null,"TEST BLOCKS"]
[]
["D.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",2]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood float finish"]
[]
["D.3.3","Surface beds, slabs, etc","m2",30]
[]
[null,"Rough formwork to sides"]
[]
["D.3.4","To sides n.e. 300mm","m2",10]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["D.3.5","15mm Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["D.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Saw cut joints"]
[]
["D.3.7","50 x 3mm Saw cut joints in top of concrete","m",34]
[]
[null,"Fabric reinforcement"]
[]
["D.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",30]
{"$rows_empty":28}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B6532","v":"Block D: 4 Classroom Block: D-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",97]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6532","v":"Block D: 4 Classroom Block: D-3  Concrete, Formwork and Reinforcement"}]
[]
["D.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["D.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["D.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["D.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",20]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-4 Masonry"]
[]
[]
[null,{"$f":"B6675","v":"Block D: 4 Classroom Block: D-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",99]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6675","v":"Block D: 4 Classroom Block: D-4 Masonry"}]
[]
["D.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["D.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",322]
[]
["D.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",31]
[]
["D.5.3","Narrow and broad flute closers","m",31]
[]
["D.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",31]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["D.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",322]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-5 Roof Coverings"]
[]
[]
[null,{"$f":"B6813","v":"Block D: 4 Classroom Block: D-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",101]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6813","v":"Block D: 4 Classroom Block: D-5 Roof Coverings"}]
[]
["D.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["D.6.1","38 x 114mm Wall plates","m",60]
[]
["D.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",310]
[]
[null,"Sundries"]
[]
["D.6.3","Two coats ABE Provinite on wrought timbers","m2",100]
[]
["D.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",30]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["D.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 8800mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",10]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["D.6.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",62]
[]
["D.6.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",36]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["D.6.8","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",117]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["D.6.9","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",4]
{"$rows_empty":22}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B6949","v":"Block D: 4 Classroom Block: D-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",103]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B6949","v":"Block D: 4 Classroom Block: D-6 Carpentry and Joinery"}]
[]
["D.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["D.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",220]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["D.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",213]
[]
["D.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",4]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["D.7.4","75mm Coved cornices","m",116.8]
{"$rows_empty":46}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B7089","v":"Block D: 4 Classroom Block: D-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",105]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7089","v":"Block D: 4 Classroom Block: D-7 Ceilings, Partitions & Access Flooring"}]
[]
["D.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["D.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",4]
["D.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",10]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["D.8.3","50mm High plastic letter or numeral","No",4]
[]
["D.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",4]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-8 Ironmongery"]
[]
[]
[null,{"$f":"B7232","v":"Block D: 4 Classroom Block: D-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",107]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7232","v":"Block D: 4 Classroom Block: D-8 Ironmongery"}]
[]
["D.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["D.9.1","23mm Thick on floors and landings ","m2",213]
["D.9.2","25mm Thick on floors and landings to verandas and steps","m2",45]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["D.9.3","On walls in patches and repairing cracks","m2",327.03999999999996]
["D.9.4","On narrow widths","m2",20]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["D.9.5","On walls in patches and repairing cracks","m2",208.87999999999997]
["D.9.6","On narrow widths","m2",20]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["D.9.7","Granolithic paved floors and skirtings","m2",322]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-9 Plastering"]
[]
[]
[null,{"$f":"B7374","v":"Block D: 4 Classroom Block: D-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",109]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7374","v":"Block D: 4 Classroom Block: D-9 Plastering"}]
[]
["D.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["D.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",62]
[]
["D.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",18]
[]
["D.10.3","Extra for angle","No",12]
["D.10.4","Extra for stop end","No",4]
["D.10.5","Extra for outlet for 100mm pipe","No",6]
["D.10.6","Extra for eaves or plinth offset","No",6]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["D.10.7","4,5kg Carbon dioxide fire extinguisher","No",4]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["D.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":36}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B7513","v":"Block D: 4 Classroom Block: D-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",111]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7513","v":"Block D: 4 Classroom Block: D-10 Plumbing and Drainage"}]
[]
["D.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["D.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",12]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-11 Glazing"]
[]
[]
[null,{"$f":"B7659","v":"Block D: 4 Classroom Block: D-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",113]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7659","v":"Block D: 4 Classroom Block: D-11 Glazing"}]
[]
["D.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["D.12.1","Internal walls including gypsum coat where necessary","m2",327.03999999999996]
["D.12.2","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["D.12.3","External walls including gypsum coat where necessary","m2",{"v":208.87999999999997,"d":"209"}]
["D.12.4","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["D.12.5","Fascias and barge boards","m",98]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["D.12.6","Door frames","m2",4]
["D.12.7","Windows","m2",12]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["D.12.8","Doors","m2",12]
["D.12.9","Cornices, etc not exceeding 300mm girth","m",116.8]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["D.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",116.8]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block D: 4 Classroom Block: D-12 Paintwork"]
[]
[]
[null,{"$f":"B7796","v":"Block D: 4 Classroom Block: D-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",115]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B7796","v":"Block D: 4 Classroom Block: D-12 Paintwork"}]
[]
[]
[]
[null,"Block D: 4 Classroom Block"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C7879-2","v":94}]
[]
[2,"Earthworks",{"$f":"C7881-2","v":96}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C7883-2","v":98}]
[]
[4,"Masonry",{"$f":"C7885-2","v":100}]
[]
[5,"Roof Coverings",{"$f":"C7887-2","v":102}]
[]
[6,"Carpentry and Joinery",{"$f":"C7889-2","v":104}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C7891-2","v":106}]
[]
[7,"Ironmongery",{"$f":"C7893-2","v":108}]
[]
[8,"Plastering",{"$f":"C7895-2","v":110}]
[]
[9,"Plumbing and Drainage",{"$f":"C7897-2","v":112}]
[]
[11,"Glazing",{"$f":"C7899-2","v":114}]
[]
[12,"Paintwork",116]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B7873","v":"Block D: 4 Classroom Block"}]
[]
[]
[]
[]
[null,"Block E: 5 Classroom Block"]
[]
["E.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["E.1.1","One brick walls.","m2",50]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["E.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",{"v":63.68,"d":"64"}]
[]
["E.1.3","Tank stand","m2",9]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good surfaces to receive new"]
[]
["E.1.4","Timber door 813 x 2032mm high","No",5]
["E.1.5","Steel windows approximately 0.95 x 1.40m high.","No",20]
["E.1.6","Steel windows approximately 0.9 x 1.20m high.","No",13]
[]
[]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
["E.1.7","Fascia boards","m",81]
["E.1.8","Barge boards.","m",24]
["E.1.9","Roof gutters","m",81]
["E.1.10","Downpipes","m",36]
[]
[null,"Taking out and removing ironmongery "]
[]
["E.1.11","Mortice lock and striking plate from timber door and steel frame","No",5]
["E.1.12","Stays, latches, handles, etc from window steel frame","No",15]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["E.1.13","Chipping of screed in floors to receive new screed. ","m2",{"v":270.64,"d":"271"}]
["E.1.14","Cleaning internal walls to receive paint.","m2",{"v":413.2799999999999,"d":"413"}]
["E.1.15","Cleaning external walls to receive paint.","m2",{"v":260.96,"d":"261"}]
["E.1.16","Hack off existing plaster and make good to receive new.","m2",80]
["E.1.17","Cleaning and removing broken glazing, putty and paint to window frames","m2",18]
{"$rows_empty":21}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-1 Alterations"]
[]
[]
[null,{"$f":"B8012","v":"Block E: 5 Classroom Block: E-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",118]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8012","v":"Block E: 5 Classroom Block: E-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["E.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["E.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",{"v":14.459999999999997,"d":"14"}]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["E.2.2","Soft rock","m3",2]
["E.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["E.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",{"v":14.459999999999997,"d":"14"}]
[]
["E.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["E.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",{"v":96.39999999999999,"d":"96"}]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["E.2.7","Soil Poisoning under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",{"v":96.39999999999999,"d":"96"}]
[]
["E.2.8","To bottoms and sides of trenches etc","m2",{"v":14.459999999999997,"d":"14"}]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-2 Earthworks"]
[]
[]
[null,{"$f":"B8154","v":"Block E: 5 Classroom Block: E-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",120]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8154","v":"Block E: 5 Classroom Block: E-2 Earthworks"}]
[]
[]
["E.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["E.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",{"v":14.459999999999997,"d":"14"}]
[]
[null,"TEST BLOCKS"]
[]
["E.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",3]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood float finish"]
[]
["E.3.3","Surface beds, slabs, etc","m2",{"v":96.39999999999999,"d":"96"}]
[]
[null,"Rough formwork to sides"]
[]
["E.3.4","To sides n.e. 300mm","m2",{"v":14.459999999999997,"d":"14"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["E.3.5","15mm Joints not exceeding 300mm high or wide","m",64]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["E.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",64]
[]
[null,"Saw cut joints"]
[]
["E.3.7","50 x 3mm Saw cut joints in top of concrete","m",64]
[]
[null,"Fabric reinforcement"]
[]
["E.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",{"v":96.39999999999999,"d":"96"}]
{"$rows_empty":28}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B8297","v":"Block E: 5 Classroom Block: E-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",122]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8297","v":"Block E: 5 Classroom Block: E-3  Concrete, Formwork and Reinforcement"}]
[]
["E.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["E.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["E.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["E.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",30]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-4 Masonry"]
[]
[]
[null,{"$f":"B8440","v":"Block E: 5 Classroom Block: E-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",124]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8440","v":"Block E: 5 Classroom Block: E-4 Masonry"}]
[]
["E.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["E.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",417.9]
[]
["E.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",40.8]
[]
["E.5.3","Narrow and broad flute closers","m",40.8]
[]
["E.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",40.8]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["E.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",417.9]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-5 Roof Coverings"]
[]
[]
[null,{"$f":"B8578","v":"Block E: 5 Classroom Block: E-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",126]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8578","v":"Block E: 5 Classroom Block: E-5 Roof Coverings"}]
[]
["E.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["E.6.1","38 x 114mm Wall plates","m",79.6]
[]
["E.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",244.79999999999998]
[]
[null,"Sundries"]
[]
["E.6.3","Two coats ABE Provinite on wrought timbers","m2",120]
[]
["E.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",50]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["E.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 8000mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",10]
[]
[null,"EAVES, VERGES, ETC"]
[null,"Everite medium density plain nutec-cement"]
[]
["E.6.6","12 x 225mm Medium density fibre-cement fascia boards with aluminium H-profile fascia joiners, drill for and fix with hot-dip galvanised drive screws and washers","m",81.6]
[]
["E.6.7","80 x 200mm Socketless barge boards with aluminium H-profile barge board joiners, drill for and fix with hot-dip galvanised screws and washers","m",24]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["E.6.8","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",147.6]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["E.6.9","44mm Framed batten door 813 x 2032m high, as per Architect's Specification","No",5]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B8715","v":"Block E: 5 Classroom Block: E-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",128]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8715","v":"Block E: 5 Classroom Block: E-6 Carpentry and Joinery"}]
[]
["E.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["E.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",{"v":270.64,"d":"271"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["E.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",270.64]
[]
["E.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",5]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["E.7.4","75mm Coved cornices","m",147.6]
{"$rows_empty":46}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B8855","v":"Block E: 5 Classroom Block: E-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",130]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8855","v":"Block E: 5 Classroom Block: E-7 Ceilings, Partitions & Access Flooring"}]
[]
["E.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["E.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",5]
["E.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",12]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["E.8.3","50mm High plastic letter or numeral","No",5]
[]
["E.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",5]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-8 Ironmongery"]
[]
[]
[null,{"$f":"B8998","v":"Block E: 5 Classroom Block: E-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",132]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B8998","v":"Block E: 5 Classroom Block: E-8 Ironmongery"}]
[]
["E.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["E.9.1","23mm Thick on floors and landings ","m2",{"v":270.64,"d":"271"}]
["E.9.2","25mm Thick on floors and landings to verandas and steps","m2",64]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["E.9.3","On walls in patches and repairing cracks","m2",{"v":413.2799999999999,"d":"413"}]
["E.9.4","On narrow widths","m2",30]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["E.9.5","On walls in patches and repairing cracks","m2",{"v":260.96,"d":"261"}]
["E.9.6","On narrow widths","m2",21]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["E.9.7","Granolithic paved floors and skirtings","m2",{"v":270.64,"d":"271"}]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-9 Plastering"]
[]
[]
[null,{"$f":"B9140","v":"Block E: 5 Classroom Block: E-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",134]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9140","v":"Block E: 5 Classroom Block: E-9 Plastering"}]
[]
["E.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["E.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",41]
[]
["E.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",36]
[]
["E.10.3","Extra for angle","No",24]
["E.10.4","Extra for stop end","No",4]
["E.10.5","Extra for outlet for 100mm pipe","No",12]
["E.10.6","Extra for eaves or plinth offset","No",12]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["E.10.7","4,5kg Carbon dioxide fire extinguisher","No",5]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["E.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":36}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B9279","v":"Block E: 5 Classroom Block: E-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",136]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9279","v":"Block E: 5 Classroom Block: E-10 Plumbing and Drainage"}]
[]
["E.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["E.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",27]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-11 Glazing"]
[]
[]
[null,{"$f":"B9425","v":"Block E: 5 Classroom Block: E-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",138]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9425","v":"Block E: 5 Classroom Block: E-11 Glazing"}]
[]
["E.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["E.12.1","Internal walls including gypsum coat where necessary","m2",413.2799999999999]
["E.12.2","In narrow widths","m2",30]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["E.12.3","External walls including gypsum coat where necessary","m2",{"v":260.96,"d":"261"}]
["E.12.4","In narrow widths","m2",21]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["E.12.5","Fascias and barge boards","m",106]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["E.12.6","Door frames","m2",5]
["E.12.7","Windows","m2",22]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["E.12.8","Doors","m2",15]
["E.12.9","Cornices, etc not exceeding 300mm girth","m",147.6]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["E.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",147.6]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block E: 5 Classroom Block: E-12 Paintwork"]
[]
[]
[null,{"$f":"B9562","v":"Block E: 5 Classroom Block: E-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",140]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9562","v":"Block E: 5 Classroom Block: E-12 Paintwork"}]
[]
[]
[]
[null,"Block E: 5 Classroom Block"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C9645-2","v":119}]
[]
[2,"Earthworks",{"$f":"C9647-2","v":121}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C9649-2","v":123}]
[]
[4,"Masonry",{"$f":"C9651-2","v":125}]
[]
[5,"Roof Coverings",{"$f":"C9653-2","v":127}]
[]
[6,"Carpentry and Joinery",{"$f":"C9655-2","v":129}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C9657-2","v":131}]
[]
[7,"Ironmongery",{"$f":"C9659-2","v":133}]
[]
[8,"Plastering",{"$f":"C9661-2","v":135}]
[]
[9,"Plumbing and Drainage",{"$f":"C9663-2","v":137}]
[]
[11,"Glazing",{"$f":"C9665-2","v":139}]
[]
[12,"Paintwork",141]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B9639","v":"Block E: 5 Classroom Block"}]
[]
[]
[]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block"]
[]
["F.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["F.1.1","One brick walls.","m2",50]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["F.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new. ","m2",10]
[]
["F.1.3","Tank stand","m2",18]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good surfaces to receive new"]
[]
["F.1.4","Timber door 813 x 2032mm high","No",4]
["F.1.5","Steel windows approximately 980 x 1400m high.","No",12]
[]
[]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
["F.1.6","Fascia boards","m",62]
["F.1.7","Barge boards.","m",24]
["F.1.8","Roof gutters","m",62]
["F.1.9","Downpipes","m",24]
[]
[null,"Taking out and removing ironmongery "]
[]
["F.1.10","Mortice lock and striking plate from timber door and steel frame","No",4]
["F.1.11","Stays, latches, handles, etc from window steel frame","No",12]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["F.1.1.12","Chipping of screed in floors to receive new screed. ","m2",{"v":212.79999999999998,"d":"213"}]
["F.1.1.13","Cleaning internal walls to receive paint.","m2",{"v":327.03999999999996,"d":"327"}]
["F.1.1.14","Cleaning external walls to receive paint.","m2",220]
["F.1.1.15","Hack off existing plaster and make good to receive new.","m2",120]
["F.1.1.16","Cleaning and removing broken glazing, putty and paint to window frames","m2",17]
{"$rows_empty":22}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-1 Alterations"]
[]
[]
[null,{"$f":"B9778","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",143]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9778","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["F.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["F.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",5]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["F.2.2","Soft rock","m3",1]
["F.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["F.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",5]
[]
["F.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["F.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",30]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["F.2.7","Soil Poisoning under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",30]
[]
["F.2.8","To bottoms and sides of trenches etc","m2",10]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-2 Earthworks"]
[]
[]
[null,{"$f":"B9919","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",145]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B9919","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-2 Earthworks"}]
[]
[]
["F.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["F.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",5]
[]
[null,"TEST BLOCKS"]
[]
["F.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",2]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 woodfloat finish"]
[]
["F.3.3","Surface beds, slabs, etc","m2",30]
[]
[null,"Rough formwork to sides"]
[]
["F.3.4","To sides n.e. 300mm","m2",10]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["F.3.5","15mm Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["F.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Saw cut joints"]
[]
["F.3.7","50 x 3mm Saw cut joints in top of concrete","m",34]
[]
[null,"Fabric reinforcement"]
[]
["F.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",30]
{"$rows_empty":27}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B10060","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",147]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10060","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-3  Concrete, Formwork and Reinforcement"}]
[]
["F.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["F.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["F.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["F.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",20]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-4 Masonry"]
[]
[]
[null,{"$f":"B10202","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",149]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10202","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-4 Masonry"}]
[]
["F.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["F.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",322]
[]
["F.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",31]
[]
["F.5.3","Narrow and broad flute closers","m",31]
[]
["F.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",31]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["F.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",322]
{"$rows_empty":41}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-5 Roof Coverings"]
[]
[]
[null,{"$f":"B10339","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",151]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10339","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-5 Roof Coverings"}]
[]
["F.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["F.6.1","38 x 114mm Wall plates","m",60]
[]
["F.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",310]
[]
[null,"Sundries"]
[]
["F.6.3","Two coats ABE Provinite on wrought timbers","m2",100]
[]
["F.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",30]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["F.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 8800mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",10]
[]
[null,"EAVES, VERGES, ETC"]
[null,"Everite medium density plain nutec-cement"]
[]
["F.6.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",62]
[]
["F.6.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",36]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[]
["F.6.8","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",117]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["F.6.9","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",4]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B10472","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",153]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10472","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-6 Carpentry and Joinery"}]
[]
["F.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["F.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",220]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["F.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",213]
[]
["F.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",1]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["F.7.4","75mm Coved cornices","m",116.8]
{"$rows_empty":45}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B10609","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",155]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10609","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-7 Ceilings, Partitions & Access Flooring"}]
[]
["F.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["F.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",4]
["F.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",10]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["F.8.3","50mm High plastic letter or numeral","No",4]
[]
["F.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",4]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-8 Ironmongery"]
[]
[]
[null,{"$f":"B10750","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",157]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10750","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-8 Ironmongery"}]
[]
["F.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["F.9.1","23mm Thick on floors and landings","m2",213]
["F.9.2","25mm Thick on floors and landings to verandas and steps","m2",45]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["F.9.3","On walls in patches and repairing cracks","m2",327.03999999999996]
["F.9.4","On narrow widths","m2",20]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["F.9.5","On walls in patches and repairing cracks","m2",208.87999999999997]
["F.9.6","On narrow widths","m2",20]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["F.9.7","Granolithic paved floors and skirtings","m2",213]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-9 Plastering"]
[]
[]
[null,{"$f":"B10891","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",159]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B10891","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-9 Plastering"}]
[]
["F.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["F.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",62]
[]
["F.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",18]
[]
["F.10.3","Extra for angle","No",12]
["F.10.4","Extra for stop end","No",4]
["F.10.5","Extra for outlet for 100mm pipe","No",6]
["F.10.6","Extra for eaves or plinth offset","No",6]
[]
[null,"FIRE APPLIANCES ETC"]
[]
[null,"Chubb"]
[]
["F.10.7","4,5kg Carbon dioxide fire extinguisher","No",4]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["F.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":35}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B11028","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",161]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11028","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-10 Plumbing and Drainage"}]
[]
["F.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["F.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",12]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-11 Glazing"]
[]
[]
[null,{"$f":"B11172","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",163]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11172","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-11 Glazing"}]
[]
["F.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["F.12.1","Internal walls including gypsum coat where necessary","m2",327.03999999999996]
["F.12.2","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["F.12.3","External walls including gypsum coat where necessary","m2",{"v":208.87999999999997,"d":"209"}]
["F.12.4","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["F.12.5","Fascias and barge boards","m",98]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["F.12.6","Door frames","m2",4]
["F.12.7","Windows","m2",12]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["F.12.8","Doors","m2",12]
["F.12.9","Cornices, etc not exceeding 300mm girth","m",116.8]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["F.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",116.8]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-12 Paintwork"]
[]
[]
[null,{"$f":"B11308","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",165]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11308","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block: F-12 Paintwork"}]
[]
[]
[]
[null,"Block F: Tuckshop, Computer Room & 2 Classroom Block"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C11390-2","v":144}]
[]
[2,"Earthworks",{"$f":"C11392-2","v":146}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C11394-2","v":148}]
[]
[4,"Masonry",{"$f":"C11396-2","v":150}]
[]
[5,"Roof Coverings",{"$f":"C11398-2","v":152}]
[]
[6,"Carpentry and Joinery",{"$f":"C11400-2","v":154}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C11402-2","v":156}]
[]
[7,"Ironmongery",{"$f":"C11404-2","v":158}]
[]
[8,"Plastering",{"$f":"C11406-2","v":160}]
[]
[9,"Plumbing and Drainage",{"$f":"C11408-2","v":162}]
[]
[11,"Glazing",{"$f":"C11410-2","v":164}]
[]
[12,"Paintwork",166]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B11384","v":"Block F: Tuckshop, Computer Room & 2 Classroom Block"}]
[]
[]
[]
[]
[null,"Block G: Staffroom & 3 Classroom Block"]
[]
["G.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["G.1.1","One brick walls.","m2",{"v":50,"d":"50.00"}]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["G.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",{"v":5,"d":"5.00"}]
[]
["G.1.3","Tank stand","m2",{"v":9,"d":"9.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good surfaces to receive new"]
[]
["G.1.4","Timber door 813 x 2032mm high","No",{"v":4,"d":"4.00"}]
[]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
["G.1.5","Fascia boards","m",{"v":62,"d":"62.00"}]
["G.1.6","Barge boards.","m",{"v":24,"d":"24.00"}]
["G.1.7","Roof gutters","m",{"v":62,"d":"62.00"}]
["G.1.8","Downpipes","m",{"v":24,"d":"24.00"}]
[]
[null,"Taking out and removing ironmongery "]
[]
["G.1.9","Mortice lock and striking plate from timber door and steel frame","No",{"v":4,"d":"4.00"}]
["G.1.10","Stays, latches, handles, etc from window steel frame","No",{"v":12,"d":"12.00"}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["G.1.11","Chipping of screed in floors to receive new screed. ","m2",{"v":212.79999999999998,"d":"212.80"}]
["G.1.12","Cleaning internal walls to receive paint.","m2",{"v":327.03999999999996,"d":"327.04"}]
["G.1.13","Cleaning external walls to receive paint.","m2",{"v":220,"d":"220.00"}]
["G.1.14","Hack off existing plaster and make good to receive new.","m2",{"v":120,"d":"120.00"}]
["G.1.15","Cleaning and removing broken glazing, putty and paint to window frames","m2",{"v":17,"d":"17.00"}]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-1 Alterations"]
[]
[]
[null,{"$f":"B11523","v":"Block G: Staffroom & 3 Classroom Block: G-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",168]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11523","v":"Block G: Staffroom & 3 Classroom Block: G-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["G.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["G.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",5]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["G.2.2","Soft rock","m3",1]
["G.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["G.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",5]
[]
["G.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["G.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",30]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["G.2.7","Soil Poisoning under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",30]
[]
["G.2.8","To bottoms and sides of trenches etc","m2",10]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-2 Earthworks"]
[]
[]
[null,{"$f":"B11665","v":"Block G: Staffroom & 3 Classroom Block: G-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",170]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11665","v":"Block G: Staffroom & 3 Classroom Block: G-2 Earthworks"}]
[]
[]
["G.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["G.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",5]
[]
[null,"TEST BLOCKS"]
[]
["G.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",2]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 woodfloat finish"]
[]
["G.3.3","Surface beds, slabs, etc","m2",30]
[]
[null,"Rough formwork to sides"]
[]
["G.3.4","To sides n.e. 300mm","m2",10]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["G.3.5","15mm Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["G.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",34]
[]
[null,"Saw cut joints"]
[]
["G.3.7","50 x 3mm Saw cut joints in top of concrete","m",34]
[]
[null,"Fabric reinforcement"]
[]
["G.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",30]
{"$rows_empty":27}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B11807","v":"Block G: Staffroom & 3 Classroom Block: G-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",172]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11807","v":"Block G: Staffroom & 3 Classroom Block: G-3  Concrete, Formwork and Reinforcement"}]
[]
["G.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["G.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[null,"Brick reinforcement"]
[]
["G.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["G.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",20]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-4 Masonry"]
[]
[]
[null,{"$f":"B11949","v":"Block G: Staffroom & 3 Classroom Block: G-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",174]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B11949","v":"Block G: Staffroom & 3 Classroom Block: G-4 Masonry"}]
[]
["G.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["G.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",334.4]
[]
["G.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",31]
[]
["G.5.3","Narrow and broad flute closers","m",31]
[]
["G.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",31]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["G.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",334.4]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-5 Roof Coverings"]
[]
[]
[null,{"$f":"B12087","v":"Block G: Staffroom & 3 Classroom Block: G-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",176]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12087","v":"Block G: Staffroom & 3 Classroom Block: G-5 Roof Coverings"}]
[]
["G.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["G.6.1","38 x 114mm Wall plates","m",60]
[]
["G.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",310]
[]
[null,"Sundries"]
[]
["G.6.3","Two coats ABE Provinite on wrought timbers","m2",100]
[]
["G.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",30]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["G.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 8800mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",10]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["G.6.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",62]
[]
["G.6.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",36]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["G.6.8","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",117]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["G.6.9","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",4]
{"$rows_empty":22}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B12223","v":"Block G: Staffroom & 3 Classroom Block: G-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",178]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12223","v":"Block G: Staffroom & 3 Classroom Block: G-6 Carpentry and Joinery"}]
[]
["G.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["G.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",206.72]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["G.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",206.72]
[]
["G.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",4]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["G.7.4","75mm Coved cornices","m",117]
{"$rows_empty":45}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B12362","v":"Block G: Staffroom & 3 Classroom Block: G-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",180]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12362","v":"Block G: Staffroom & 3 Classroom Block: G-7 Ceilings, Partitions & Access Flooring"}]
[]
["G.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["G.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",4]
["G.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",10]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["G.8.3","50mm High plastic letter or numeral","No",4]
[]
["G.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",4]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-8 Ironmongery"]
[]
[]
[null,{"$f":"B12503","v":"Block G: Staffroom & 3 Classroom Block: G-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",182]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12503","v":"Block G: Staffroom & 3 Classroom Block: G-8 Ironmongery"}]
[]
["G.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["G.9.1","23mm Thick on floors and landings ","m2",{"v":206.72,"d":"207"}]
["G.9.2","25mm Thick on floors and landings to verandas and steps","m2",45]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["G.9.3","On walls in patches and repairing cracks","m2",327.03999999999996]
["G.9.4","On narrow widths","m2",20]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["G.9.5","On walls in patches and repairing cracks","m2",208.87999999999997]
["G.9.6","On narrow widths","m2",20]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["G.9.7","Granolithic paved floors and skirtings","m2",{"v":206.72,"d":"207"}]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-9 Plastering"]
[]
[]
[null,{"$f":"B12645","v":"Block G: Staffroom & 3 Classroom Block: G-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",184]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12645","v":"Block G: Staffroom & 3 Classroom Block: G-9 Plastering"}]
[]
["G.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["G.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",62]
[]
["G.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",18]
[]
["G.10.3","Extra for angle","No",12]
["G.10.4","Extra for stop end","No",4]
["G.10.5","Extra for outlet for 100mm pipe","No",6]
["G.10.6","Extra for eaves or plinth offset","No",6]
[]
[null,"FIRE APPLIANCES ETC"]
[]
["G.10.7","4,5kg Carbon dioxide fire extinguisher","No",4]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["G.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":38}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B12784","v":"Block G: Staffroom & 3 Classroom Block: G-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",186]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12784","v":"Block G: Staffroom & 3 Classroom Block: G-10 Plumbing and Drainage"}]
[]
["G.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["G.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",12]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-11 Glazing"]
[]
[]
[null,{"$f":"B12929","v":"Block G: Staffroom & 3 Classroom Block: G-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",188]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B12929","v":"Block G: Staffroom & 3 Classroom Block: G-11 Glazing"}]
[]
["G.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["G.12.1","Internal walls including gypsum coat where necessary","m2",327.03999999999996]
["G.12.2","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["G.12.3","External walls including gypsum coat where necessary","m2",{"v":208.87999999999997,"d":"209"}]
["G.12.4","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["G.12.5","Fascias and barge boards","m",98]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["G.12.6","Door frames","m2",4]
["G.12.7","Windows","m2",12]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["G.12.8","Doors","m2",12]
["G.12.9","Cornices, etc not exceeding 300mm girth","m",116.8]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["G.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",116.8]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block G: Staffroom & 3 Classroom Block: G-12 Paintwork"]
[]
[]
[null,{"$f":"B13066","v":"Block G: Staffroom & 3 Classroom Block: G-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",190]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13066","v":"Block G: Staffroom & 3 Classroom Block: G-12 Paintwork"}]
[]
[]
[]
[null,"Block G: Staffroom & 3 Classroom Block"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C13149-2","v":169}]
[]
[2,"Earthworks",{"$f":"C13151-2","v":171}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C13153-2","v":173}]
[]
[4,"Masonry",{"$f":"C13155-2","v":175}]
[]
[5,"Roof Coverings",{"$f":"C13157-2","v":177}]
[]
[6,"Carpentry and Joinery",{"$f":"C13159-2","v":179}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C13161-2","v":181}]
[]
[7,"Ironmongery",{"$f":"C13163-2","v":183}]
[]
[8,"Plastering",{"$f":"C13165-2","v":185}]
[]
[9,"Plumbing and Drainage",{"$f":"C13167-2","v":187}]
[]
[11,"Glazing",{"$f":"C13169-2","v":189}]
[]
[12,"Paintwork",191]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B13143","v":"Block G: Staffroom & 3 Classroom Block"}]
[]
[]
[]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices"]
[]
["H.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["H.1.1","One brick walls.","m2",50]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["H.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",50]
[]
["H.1.3","Tank stand","m2",18]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and  making good surfaces to receive new"]
[]
["H.1.4","Timber door 813 x 2032mm high","No",6]
[]
[]
[null,"Taking out and removing joinery fittings etc and making good to  surfaces to receive new."]
[]
["H.1.5","Fascia boards","m",34]
["H.1.6","Barge boards.","m",24]
["H.1.7","Roof gutters","m",34]
["H.1.8","Downpipes","m",24]
[]
[null,"Taking out and removing ironmongery "]
[]
["H.1.9","Mortice lock and striking plate from timber door and steel frame","No",5]
["H.1.10","Stays, latches, handles, etc from window steel frame","No",12]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
["H.1.11","Chipping of screed in floors to receive new screed. ","m2",{"v":245.68,"d":"246"}]
["H.1.12","Cleaning internal walls to receive paint.","m2",{"v":428.96,"d":"429"}]
["H.1.13","Cleaning external walls to receive paint.","m2",{"v":227.35999999999999,"d":"227"}]
["H.1.14","Hack off existing plaster and make good to receive new.","m2",80]
["H.1.15","Cleaning and removing broken glazing, putty and paint to window frames","m2",21]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-1 Alterations"]
[]
[]
[null,{"$f":"B13283","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",193]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13283","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["H.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["H.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",4]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["H.2.2","Soft rock","m3",1]
["H.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["H.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",4]
[]
["H.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["H.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",28]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["H.2.7","Soil Poisoning: Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",28]
[]
["H.2.8","To bottoms and sides of trenches etc","m2",5]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-2 Earthworks"]
[]
[]
[null,{"$f":"B13425","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",195]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13425","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-2 Earthworks"}]
[]
[]
["H.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["H.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",4]
[]
[null,"TEST BLOCKS"]
[]
["H.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",1]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 woodfloat finish"]
[]
["H.3.3","Surface beds, slabs, etc","m2",28]
[]
[null,"Rough formwork to sides"]
[]
["H.3.4","To sides n.e. 300mm","m2",5]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["H.3.5","15mm Joints not exceeding 300mm high or wide","m",54]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["H.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",54]
[]
[null,"Saw cut joints"]
[]
["H.3.7","50 x 3mm Saw cut joints in top of concrete","m",54]
[]
[null,"Fabric reinforcement"]
[]
["H.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m2",28]
{"$rows_empty":27}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B13567","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",197]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13567","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-3  Concrete, Formwork and Reinforcement"}]
[]
["H.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["H.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["H.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["H.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",16]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-4 Masonry"]
[]
[]
[null,{"$f":"B13709","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",199]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13709","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-4 Masonry"}]
[]
["H.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
[]
["H.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",365.20000000000005]
[]
["H.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",41.7]
[]
["H.5.3","Narrow and broad flute closers","m",41.7]
[]
["H.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",41.7]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["H.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",365.20000000000005]
{"$rows_empty":41}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-5 Roof Coverings"]
[]
[]
[null,{"$f":"B13847","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",201]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13847","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-5 Roof Coverings"}]
[]
["H.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["H.6.1","38 x 114mm Wall plates","m",68]
[]
["H.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",75]
[]
[null,"Sundries"]
[]
["H.6.3","Two coats ABE Provinite on wrought timbers","m2",35]
[]
["H.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",30]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["H.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 8800mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",10]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["H.6.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",68]
[]
["H.6.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",24]
[]
[null,"SHELVING AND CUPBOARDS"]
[]
["H.6.8","Lockable floor cupboard 3000 x 500 x 875mm high with top, sides, bottom, adjustable shelf, back and six hinged doors","No",2]
[]
["H.6.9","300x32mm Laminated SA pine shelves 5000mm x 1585mm high","m",4]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["H.6.10","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",153.20000000000002]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["H.6.11","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",6]
{"$rows_empty":15}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B13982","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",203]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B13982","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-6 Carpentry and Joinery"}]
[]
["H.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["H.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",245.68]
[]
[null,"NAILED UP CEILINGS"]
[]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["H.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",245.68]
[]
["H.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",5]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["H.7.4","75mm Coved cornices","m",153.20000000000002]
{"$rows_empty":44}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B14120","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",205]
{"$rows_empty":62}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14120","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-7 Ceilings, Partitions & Access Flooring"}]
[]
["H.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["H.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",6]
["H.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",12]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["H.8.3","50mm High plastic letter or numeral","No",6]
[]
["H.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",6]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-8 Ironmongery"]
[]
[]
[null,{"$f":"B14261","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",207]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14261","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-8 Ironmongery"}]
[]
["H.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["H.9.1","23mm Thick on floors and landings","m2",{"v":245.68,"d":"246"}]
["H.9.2","25mm Thick on floors and landings to verandas and steps","m2",{"v":49.800000000000004,"d":"50"}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["H.9.3","On walls in patches and repairing cracks","m2",{"v":428.96,"d":"429"}]
["H.9.4","On narrow widths","m2",20]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["H.9.5","On walls in patches and repairing cracks","m2",{"v":227.35999999999999,"d":"227"}]
["H.9.6","On narrow widths","m2",20]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["H.9.7","Granolithic paved floors and skirtings","m2",{"v":245.68,"d":"246"}]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-9 Plastering"]
[]
[]
[null,{"$f":"B14403","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",209]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14403","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-9 Plastering"}]
[]
["H.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["H.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",68]
[]
["H.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",12]
[]
["H.10.3","Extra for angle","No",16]
["H.10.4","Extra for stop end","No",4]
["H.10.5","Extra for outlet for 100mm pipe","No",8]
["H.10.6","Extra for eaves or plinth offset","No",8]
[]
[null,"FIRE APPLIANCES ETC"]
[]
["H.10.7","4,5kg Carbon dioxide fire extinguisher","No",6]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["H.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",1]
{"$rows_empty":38}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B14542","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",211]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14542","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-10 Plumbing and Drainage"}]
[]
["H.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["H.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",21]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-11 Glazing"]
[]
[]
[null,{"$f":"B14687","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",213]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14687","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-11 Glazing"}]
[]
["H.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["H.12.1","Internal walls including gypsum coat where necessary","m2",428.96]
["H.12.2","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["H.12.3","External walls including gypsum coat where necessary","m2",{"v":227.35999999999999,"d":"227"}]
["H.12.4","In narrow widths","m2",20]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["H.12.5","Fascias and barge boards","m",68]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["H.12.6","Door frames","m2",6]
["H.12.7","Windows","m2",18]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["H.12.8","Doors","m2",18]
["H.12.9","Cornices, etc not exceeding 300mm girth","m",153.20000000000002]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["H.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",153.20000000000002]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:: H-12 Paintwork"]
[]
[]
[null,{"$f":"B14824","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",215]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B14824","v":"Block H: 4 Classroom Block & 2 HOD Offices:: H-12 Paintwork"}]
[]
[]
[]
[null,"Block H: 4 Classroom Block & 2 HOD Offices:"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C14907-2","v":194}]
[]
[2,"Earthworks",{"$f":"C14909-2","v":196}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C14911-2","v":198}]
[]
[4,"Masonry",{"$f":"C14913-2","v":200}]
[]
[5,"Roof Coverings",{"$f":"C14915-2","v":202}]
[]
[6,"Carpentry and Joinery",{"$f":"C14917-2","v":204}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C14919-2","v":206}]
[]
[7,"Ironmongery",{"$f":"C14921-2","v":208}]
[]
[8,"Plastering",{"$f":"C14923-2","v":210}]
[]
[9,"Plumbing and Drainage",{"$f":"C14925-2","v":212}]
[]
[11,"Glazing",{"$f":"C14927-2","v":214}]
[]
[12,"Paintwork",216]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B14901","v":"Block H: 4 Classroom Block & 2 HOD Offices:"}]
[]
[]
[]
[]
[null,"Block I: 2 Classroom Block"]
[]
["I.1","ALTERATIONS"]
[]
[null,"Repairs to cracked walls."]
[]
["I.1.1","One brick walls.","m2",50]
[]
[null,"Breaking down and removing concrete, etc "]
[]
["I.1.2","Surface bed approximately 80mm thick (verandas, external steps, etc) and prepare surface to receive new.","m2",15]
[]
["I.1.3","Tank stand","m2",9]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and  making good surfaces to receive new"]
[]
["I.1.4","Timber door 813 x 2032mm high","No",3]
["I.1.5"]
[null,"Taking out and removing joinery fittings etc and making good to surfaces to receive new."]
[]
[null,"Fascia boards","m",37]
["I.1.6","Barge boards.","m",24]
["I.1.7","Roof gutters","m",37]
["I.1.8","Downpipes","m",12]
["I.1.9"]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3]
["I.1.10","Stays, latches, handles, etc from window steel frame","No",12]
["I.1.11"]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to receive new screed. ","m2",{"v":128.01999999999998,"d":"128"}]
["I.1.12","Cleaning internal walls to receive paint.","m2",{"v":213.91999999999996,"d":"214"}]
["I.1.13","Cleaning external walls to receive paint.","m2",{"v":138.32,"d":"138"}]
["I.1.14","Hack off existing plaster and make good to receive new.","m2",30]
["I.1.15","Cleaning and removing broken glazing, putty and paint to window frames","m2",12]
{"$rows_empty":24}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-1 Alterations"]
[]
[]
[null,{"$f":"B15040","v":"Block I: 2 Classroom Block:: I-1 Alterations"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",218]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15040","v":"Block I: 2 Classroom Block:: I-1 Alterations"}]
[]
[null,"NEW WORKS"]
[]
["I.2","EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["I.2.1","Open face excavation to expose foundations for inspection and underpinning","m3",4]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["I.2.2","Soft rock","m3",1]
["I.2.3","Hard rock","m3",1]
[]
[null,"Extra over all excavations for carting away"]
[]
["I.2.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",4]
[]
["I.2.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["I.2.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",28]
[]
[null,"SOIL POISONING"]
[]
[null,"Soil insecticide"]
[]
["I.2.7","Soil Poisoning: Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",28]
[]
["I.2.8","To bottoms and sides of trenches etc","m2",5]
{"$rows_empty":33}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-2 Earthworks"]
[]
[]
[null,{"$f":"B15182","v":"Block I: 2 Classroom Block:: I-2 Earthworks"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",220]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15182","v":"Block I: 2 Classroom Block:: I-2 Earthworks"}]
[]
[]
["I.3","CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["I.3.1","Concrete to V-drain cast in panels, laid to fall in 1:200, with control joints filled with polysulphide sealant, every 3000mm centres","m3",4]
[]
[null,"TEST BLOCKS"]
[]
["I.3.2","Making and testing of three 150 x 150 x 150mm concrete strength test cubes","No",1]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 woodfloat finish"]
[]
["I.3.3","Surface beds, slabs, etc","m2",28]
[]
[null,"Rough formwork to sides"]
[]
["I.3.4","To sides n.e. 300mm","m2",5]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete surfaces"]
[]
["I.3.5","15mm Joints not exceeding 300mm high or wide","m",54]
[]
[null,"Expansion joints with bitumen-impregnated softboard between vertical concrete and brickwork surfaces"]
[]
["I.3.6","10mm Isolation Joints not exceeding 300mm high or wide","m",54]
[]
[null,"Saw cut joints"]
[]
["I.3.7","50 x 3mm Saw cut joints in top of concrete","m",54]
[]
[null,"Fabric reinforcement"]
[]
["I.3.8","Type 193 fabric reinforcement in concrete surface beds, slabs, etc","m2",28]
{"$rows_empty":28}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-3  Concrete, Formwork and Reinforcement"]
[]
[]
[null,{"$f":"B15325","v":"Block I: 2 Classroom Block:: I-3  Concrete, Formwork and Reinforcement"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",222]
{"$rows_empty":63}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15325","v":"Block I: 2 Classroom Block:: I-3  Concrete, Formwork and Reinforcement"}]
[]
["I.4","MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including galvanised crimp wire wall ties (7 per m² laid staggered)"]
[]
["I.4.1","One brick walls","m2",50]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Brick reinforcement"]
[]
["I.4.2","150mm Wide reinforcement built in horizontally","m",147]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[]
["I.4.3","30 x 1,6mm Cramp 500mm long with one end fixed to wood and other end built into brickwork","No",16]
{"$rows_empty":50}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-4 Masonry"]
[]
[]
[null,{"$f":"B15468","v":"Block I: 2 Classroom Block:: I-4 Masonry"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",224]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15468","v":"Block I: 2 Classroom Block:: I-4 Masonry"}]
[]
["I.5","ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with Z275 to both sides, on sisalation, fixed to timber intermediate purlins (purlins as per manufacturer's spec, taking into account windloads) secured with saflok 700 clips screw fixed to purlins as per manufacturer's recommendations and specifications."]
[]
["I.5.1","Roof covering with 15 degree pitch, in transportable lengths not exceeding 20m. The description includes all related items.","m2",190.3]
[]
["I.5.2","AG 150 G550 ridge capping with broad flute closures to suit roof profile with pre-painted factory finish.","m",18]
[]
["I.5.3","Narrow and broad flute closers","m",18]
[]
["I.5.4","Moulded narrow and broad rib polyethylene filler blocks","m",18]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial grade aluminium foil based insulation"]
[]
["I.5.5","Insulation laid taut over purlins (at approximately 1,80m centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires","m2",190.3]
{"$rows_empty":42}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-5 Roof Coverings"]
[]
[]
[null,{"$f":"B15606","v":"Block I: 2 Classroom Block:: I-5 Roof Coverings"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",226]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15606","v":"Block I: 2 Classroom Block:: I-5 Roof Coverings"}]
[]
["I.6","CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[]
["I.6.1","38 x 114mm Wall plates","m",36]
[]
["I.6.2","50 x 76mm Purlins not exceeding 6.6 m in length, to manufacturer's specification","m",108]
[]
[null,"Sundries"]
[]
["I.6.3","Two coats ABE Provinite on wrought timbers","m2",35]
[]
["I.6.4","Teco two way hurricane clips secured to purlins and trusses at every intersection externally and internally galvanised wire is to be used","No",30]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
["I.6.5","Double pitched prefabricated plate nailed roof truss spanning approximately 7400mm and 1689mm high, truss to be hoisted and fixed approximately 3m above ground level as per manufacture's details. The description includes all related items","No",8]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
["I.6.6","12 x 225mm Medium density fibre-cement fascia boards (Product No.041-202) with aluminium H-profile fascia joiners (Product No. 685-195), drill for and fix with hot-dip galvanised drive screws and washers","m",36]
[]
["I.6.7","80 x 200mm Socketless barge boards (Product No.721-800) with aluminium H-profile barge board joiners (Product No. 685-187), drill for and fix with hot-dip galvanised screws and washers","m",24]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
["I.6.8","19 x 75mm Skirtings including 19mm quadrant bead plugged","m",77]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
["I.6.9","44mm (D1) Framed batten door 813 x 2032m high, as per Architect's Specification","No",3]
{"$rows_empty":22}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-6 Carpentry and Joinery"]
[]
[]
[null,{"$f":"B15742","v":"Block I: 2 Classroom Block:: I-6 Carpentry and Joinery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",228]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15742","v":"Block I: 2 Classroom Block:: I-6 Carpentry and Joinery"}]
[]
["I.7","CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
["I.7.1","76mm Insulation blanket closely fitted and laid on top of brandering between roof timbers, etc","m2",128.02]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed steel jointing strips"]
[]
["I.7.2","Horizontal ceilings, including 38 x 38mm sawn softwood brandering at maximum 400mm centres in one direction only to trusses ( elsewhere measured).","m2",128.02]
[]
["I.7.3","Extra over ceiling for 900 x 900mm trap door of 6mm wrought softwood rebated framing with one 50 x 50mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No",1]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
["I.7.4","75mm Coved cornices","m",77]
{"$rows_empty":46}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-7 Ceilings, Partitions & Access Flooring"]
[]
[]
[null,{"$f":"B15882","v":"Block I: 2 Classroom Block:: I-7 Ceilings, Partitions & Access Flooring"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",230]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B15882","v":"Block I: 2 Classroom Block:: I-7 Ceilings, Partitions & Access Flooring"}]
[]
["I.8","IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
["I.8.1","Three lever mortice lockset and satin chrome plated handles Solid Art 390/313","No",3]
["I.8.2","Stays, latches, handles, hinges, etc to existing window frames","No",12]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and numerals fixed with two self-tapping screws to steel and reading as follows:-"]
[]
["I.8.3","50mm High plastic letter or numeral","No",3]
[]
["I.8.4","38mm Diameter rubber door stop plugged and screwed to floor with a 50mm long brass screw","No",3]
{"$rows_empty":52}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-8 Ironmongery"]
[]
[]
[null,{"$f":"B16025","v":"Block I: 2 Classroom Block:: I-8 Ironmongery"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",232]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B16025","v":"Block I: 2 Classroom Block:: I-8 Ironmongery"}]
[]
["I.9","PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
["I.9.1","23mm Thick on floors and landings ","m2",{"v":128.02,"d":"128"}]
["I.9.2","25mm Thick on floors and landings to verandas and steps","m2",25.950000000000003]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["I.9.3","On walls in patches and repairing cracks","m2",{"v":213.91999999999996,"d":"214"}]
["I.9.4","On narrow widths","m2",10]
[]
[null,"EXTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
["I.9.5","On walls in patches and repairing cracks","m2",{"v":138.32,"d":"138"}]
["I.9.6","On narrow widths","m2",10]
[]
[null,"SPECIALIST FLOOR AND WALL COATINGS"]
[]
[null,"Prime surfaces and apply two coats 'Flowcrete Flowcoat Quartz' or other approved non-slip self levelling epoxy floor finish with anti-microbial additive having finished thickness of 3mm on"]
[]
[null,"The rate to include for : "]
[]
[null,"- All specialist plant, labour and materials for executing the works under this item "]
[null,"- Preparation of the surface by means of diamond grinding"]
[null,"- Priming the surface with Abecote Primer at 4m² per litre"]
[null,"- Application of Abecote 400 Hi-Build epoxy resin at 2mm with a non-slip finish using notched trowels "]
[null,"- Re-cutting and sealing expansion joints"]
[]
["I.9.7","Granolithic paved floors and skirtings","m2",{"v":128.02,"d":"128"}]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-9 Plastering"]
[]
[]
[null,{"$f":"B16167","v":"Block I: 2 Classroom Block:: I-9 Plastering"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",234]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B16167","v":"Block I: 2 Classroom Block:: I-9 Plastering"}]
[]
["I.10","PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
["I.10.1","155 x 100 x 115mm ogee gutter with baked enamel finish fixed with concealed brackets (all to supplies spec).","m",36]
[]
["I.10.2","100 x 75 mm fluted downpipes with baked enamel finish as per supplier's details","m",12]
[]
["I.10.3","Extra for angle","No",8]
["I.10.4","Extra for stop end","No",4]
["I.10.5","Extra for outlet for 100mm pipe","No",4]
["I.10.6","Extra for eaves or plinth offset","No",4]
[]
[null,"FIRE APPLIANCES ETC"]
[]
["I.10.7","4,5kg Carbon dioxide fire extinguisher","No",2]
[]
[null,"TANKS"]
[]
[null,"JoJo Polyproline water tank"]
[]
["I.10.8","5000 litre Polyproline water tank with 35mm diameter inlet at top and 50mm overflow outlet and 25mm outlet at base of tank including access hatch on top fitted with vermin-proof vent, and including 1.6 x 50mm galvanised hoop iron or other approved holding down material secured around pedestal complete including pedestal, including concrete, brickwork for stand as per engineer's or Architect's drawings.","No",2]
{"$rows_empty":38}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-10 Plumbing and Drainage"]
[]
[]
[null,{"$f":"B16306","v":"Block I: 2 Classroom Block:: I-10 Plumbing and Drainage"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",236]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B16306","v":"Block I: 2 Classroom Block:: I-10 Plumbing and Drainage"}]
[]
["I.11","GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm Anodised"]
[]
["I.11.1","Panes exceeding 0,5m² and not exceeding 2m²","m2",12]
{"$rows_empty":62}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-11 Glazing"]
[]
[]
[null,{"$f":"B16452","v":"Block I: 2 Classroom Block:: I-11 Glazing"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",238]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B16452","v":"Block I: 2 Classroom Block:: I-11 Glazing"}]
[]
["I.12","PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["I.12.1","Internal walls including gypsum coat where necessary","m2",213.91999999999996]
["I.12.2","In narrow widths","m2",15]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N' ALL' emulsion paint (colour to be approved by the Department of Education) on"]
[]
["I.12.3","External walls including gypsum coat where necessary","m2",{"v":138.32,"d":"138"}]
["I.12.4","In narrow widths","m2",18]
[]
[null,"Prepare and apply one coat primer and two coats PVC emulsion paint (colour to be approved by the Department of Education) on"]
[]
["I.12.5","Fascias and barge boards","m",61]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc phosphate metal primer, one coat universal undercoat and two coats super universal enamel paint on steel"]
[]
["I.12.6","Door frames","m2",3]
["I.12.7","Windows","m2",12]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one coat undercoat and one coat gloss enamel paint"]
[]
["I.12.8","Doors","m2",9]
["I.12.9","Cornices, etc not exceeding 300mm girth","m",77]
[]
[null,"One coat oil wood primer, one coat universal undercoat and two coats varnish on"]
[]
["I.12.10","Skirtings, rails, etc not exceeding 300mm girth","m",77]
{"$rows_empty":31}
[null,"Carried to Collection"]
[]
[null,"Block I: 2 Classroom Block:: I-12 Paintwork"]
[]
[]
[null,{"$f":"B16589","v":"Block I: 2 Classroom Block:: I-12 Paintwork"}]
[null,"Main Collection","Page"]
[]
[null,"Brought forward ",240]
{"$rows_empty":64}
[null,"Carried to Summary"]
[]
[null,{"$f":"B16589","v":"Block I: 2 Classroom Block:: I-12 Paintwork"}]
[]
[]
[]
[null,"Block I: 2 Classroom Block:"]
[null,"Summary","Page"]
[]
[]
[1,"Alterations",{"$f":"C16672-2","v":219}]
[]
[2,"Earthworks",{"$f":"C16674-2","v":221}]
[]
[3,"Concrete, Formwork and Reinforcement",{"$f":"C16676-2","v":223}]
[]
[4,"Masonry",{"$f":"C16678-2","v":225}]
[]
[5,"Roof Coverings",{"$f":"C16680-2","v":227}]
[]
[6,"Carpentry and Joinery",{"$f":"C16682-2","v":229}]
[]
[7,"Ceilings, Partitions and Access Flooring",{"$f":"C16684-2","v":231}]
[]
[7,"Ironmongery",{"$f":"C16686-2","v":233}]
[]
[8,"Plastering",{"$f":"C16688-2","v":235}]
[]
[9,"Plumbing and Drainage",{"$f":"C16690-2","v":237}]
[]
[11,"Glazing",{"$f":"C16692-2","v":239}]
[]
[12,"Paintwork",241]
{"$rows_empty":40}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B16666","v":"Block I: 2 Classroom Block:"}]
[]
[]
[]
["J","External Works"]
[]
[null,"Perimeter Fencing"]
[]
["J.1","EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
["J.1.1","Open face excavation to expose foundations for inspection and underpinning","m3",60]
[]
[null,"Extra over trench and hole excavations in earth for excavation in"]
[]
["J.1.2","Soft rock","m3",6]
["J.1.3","Hard rock","m3",3]
[]
[null,"Extra over all excavations for carting away"]
[]
["J.1.4","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",60]
[]
["J.1.5","Keeping excavations free of all water other than subterranean water","Item",1]
[]
[null,"Compaction of surfaces"]
[]
["J.1.6","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",152]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
["J.1.7","Concrete to 400 x 400 x 600mm deep footings, 1500mm centre to centre  spacing","m3",31]
[]
["J.1.8","Concrete to 200 wide x 200mm deep ground beam","m3",20]
[]
[null,"Fencing Panels and Poles"]
[]
["J.1.9","Supply and fit 3m high Clearvu fencing including gates, etc or equivalent","m",380]
{"$rows_empty":27}
[null,"Carried to Collection"]
[]
[null,{"$f":"B16739","v":"External Works"}]
[]
[]
[]
[null,{"$f":"B16804","v":"External Works"}]
[null,"Summary","Page"]
[]
[]
[null,"Summary brought forward",243]
{"$rows_empty":62}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B16808","v":"External Works"}]
[]
[]
[]
[null,"Electrical Works"]
[]
[null,"SECTION 1 : LT DISTRIBUTION"]
[]
[null,"DISTRIBUTION BOARDS AND ACCESSORIES"]
[]
[null,"Supply the following Distribution Boards complete with all switchgear, accessories as specified on the schematic layouts, all fitted in the factory and tested, including delivery to Site and off-loading but excluding cable terminations. Install and connect up, including earthing and conduit terminations but excluding cable terminations."]
[]
["K.13.1","Classroom Block DB (Prewired 12 Way - 3CR12)","No.",7]
["K.13.2","Ablution Block DB (6 Way - 3CR12)","No.",1]
["K.13.3","Guard House DB (6 Way - 3CR12)","No.",1]
[]
[null,"CABLES AND EARTH WIRE (PROVISIONAL)"]
[]
[null,"Rates to include for supply, delivery and installation via sleeves, cable tray or fixed to surface but excluding terminations, joints, cable trays or sleeves for 600/1000 Volts cables and earth wires:-"]
[]
[null,"PVC/PVC/SWA/ECC/PVC/ copper cables"]
["K.13.4","6mm²  2 Core PVC ECC Copper Cable","m",150]
["K.13.5","16mm²  2 Core PVC ECC Copper Cable","m",75]
[]
[null,"CABLE TERMINATIONS"]
[]
[null,"Supply, delivery, installation and labour for making-off, terminating and connecting cables and earth wires including glands, shrouds, lugs and connections for the following cables and earth wires:-"]
[]
[null,"PVC/PVC/SWA/ECC/PVC/ copper cables"]
[]
["K.13.6","6mm²  2 Core PVC ECC Copper Cable","No.",16]
["K.13.7","16mm²  2 Core PVC ECC Copper Cable","No.",2]
[]
[null,"SUNDRIES"]
[]
["K.13.8","Draw Wire","m",1200]
[]
[null,"TEST AND COMMISSION"]
[]
["K.13.9","Test and Commision the complete installation in accordance with the Specifications and SANS Standards","Sum",1]
[]
["K.13.1","Issue a Certificate of Compliance (CoC) in accordance with the SANS 10142-1 (2006) requirements per DB.","Sum",8]
[]
[null,"LIGHTNING PROTECTION AND EARTHING"]
[]
["K.13.11","Allow for the execution of a Soil Resistivity Survey for the site and for submitting a copy of the reports to the Engineer.","No",1]
[]
["K.13.12","Allow for the testing of the complete scheme, including lightning protection earth electrodes and the issuing of test certificates.","No",1]
[]
["K.13.K.13","50mm² PVC insulated for bonding down conductors to earth rods, etc.  inclusive of lugs, ferrules, bolts, etc.","m",80]
[]
["K.13.14","Supply and install corrosion resistant stainless steel terminal for roof connection points and and aluminium bond to take aluminium down conductor from roof terminals.","No",80]
[]
[]
[]
[]
[null,"Carried to Collection"]
[]
[null,{"$f":"B16881","v":"Electrical Works"}]
[]
["K.13.15","Supply and Install ferrules and lugs for bonding of any metalwork to air terminal system.","No",60]
[]
["K.13.16","Supply and install 1.5m copper clad steel earth rods driven into the ground including jointing to copper bonding conductor.","No",24]
[]
["K.13.17","Supply and install test point connection in each down conductor COMPLETE with 132x82x55mm deep screw lid enclosure.","No",24]
[]
["K.13.18","Supply and Install 25mm pvc pipe","m",120]
[]
["K.13.19","Supply and Install 50mm aluminium conductor","m",120]
[]
[null,"WIRING TRUNKING & MESH TRAY"]
[]
[null,"Supply and install 2 compartment P/Skirt complete with all fixings, separate covers and accessories. (EQUAL OR SIMILAR APPROVED TO BUFF DUCT OR LEGRANDE)"]
[]
["K.13.2","Supply and install Power skirting complete with all fixings, end caps, separate covers and accessories.","m",45]
[]
[null,"Supply and install telephone and data outlets in power skirting including cover plates and all accessories."]
[]
["K.13.21","Telephone outlet","No",2]
[]
["K.13.22","Data Outlet","No",2]
[]
[null,"SECTION 2 : EXCAVATIONS AND SLEEVES"]
[]
[null,"SLEEVES"]
[]
[null,"Supply and install the following underground sleeves"]
[]
["K.13.23","110mm Diameter","m",100]
["K.13.24","110mm Diameter slow radius bends","No",4]
["K.13.25","50mm Diameter","m",50]
[]
[null,"SECTION 3 : POWER - GENERAL PURPOSE OUTLETS AND LIGHTING"]
[]
[null,"CONDUITS"]
[]
[null,"Supply and install PVC conduit complete with all accessories including couplings, bending, fixings and waste fixed as specified."]
[]
["K.13.26","20 mm - chased in brickwork","m",1200]
["K.13.27","20 mm - ceiling void","m",800]
["K.13.28","25 mm - chased in brickwork","m",800]
["K.13.29","32 mm - chased in brickwork","m",20]
["K.13.3","50 mm - surface on brickwork (BOSAL)","m",50]
[]
[null,"CONDUIT BOXES"]
[]
[null,"Supply and install boxes complete with all accessories, including conduit terminations"]
[]
["K.13.31","60 mm round, 60 mm deep PVC box for 20 mm conduit fixed in sofit or brickwork or ceiling void","No",130]
["K.13.32","100 x 50 x 50 mm galv. box, flush mounted in brickwork","No",40]
["K.13.33","100 x 100 x 50 mm galv. box, flush mounted in brickwork","No",80]
{"$rows_empty":8}
[null,"Carried to Collection"]
[]
[null,{"$f":"B16935","v":"Electrical Works"}]
[]
[null,"CONDUCTORS AND CABLES"]
[]
[null,"Supply and install PVC insulated copper conductors in required colours drawn into conduit or in trunking"]
[]
["K.13.34","1.5 mm² pvc conductor","m",2400]
["K.13.35","1.5 mm² BCEW","m",1200]
["K.13.36","2.5 mm² pvc conductor","m",1200]
["K.13.37","2.5 mm² BCEW","m",600]
[]
[null,"LIGHT SWITCHES"]
[]
[null,"Flush mounted switch unit complete with cover plate and all accessories"]
[]
["K.13.38","16A, Single Lever, One Way","No",40]
["K.13.39","Photocell poly-carbonate bulkhead","No",13]
[]
[null,"LIGHT FITTINGS"]
[]
[null,"Suppy, deliver and store the following light fittings complete; inclusive of lamps (please refer to the Lightfitting Schedule for full specifications of the fittings):"]
[]
["K.13.4","20W LED Bulkhead IP55 (EQUAL OR SIMILAR APPROVED TO BEKA OR SWANLITE)","No",40]
["K.13.41","GLS LFL-100W ECG","No",10]
["K.13.42","GLS FC/R-235 TS ECG","No",140]
[]
[null,"SWITCHED SOCKET OUTLETS"]
[]
["K.13.43","Supply, install and connect switch socket outlets as specified including cover plates and all accessories 16 Amp double switched socket outlet installed flush on wall","No",100]
[]
[null,"ISOLATORS"]
[]
[null,"Supply and install isolators mounted as specified complete with cover plate and all accessories"]
[]
["K.13.44","20 Amp Single Pole isolators installed surface on wall in a weatherproof enclosure.","No",5]
["K.13.45","40 Amp Single Pole isolators installed surface on wall for stove","No",1]
["K.13.46","IP65 Junction Box with 10A single pole circuit breaker","No",2]
{"$rows_empty":25}
[null,"Carried to Collection"]
[]
[null,{"$f":"B16998","v":"Electrical Works"}]
[]
[]
[]
[null,{"$f":"B17062","v":"Electrical Works"}]
[null,"Summary","Page"]
[]
[]
[null,"Summary brought forward",245]
[]
[null,null,246]
[]
[null,null,247]
{"$rows_empty":58}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B17066","v":"Electrical Works"}]
[]
[]
[]
["L","Provisional Sums"]
[]
["L.1","CLO",{"$nulls":4},0]
[{"$nulls":6},0]
["L.1.1","Provide the sum of R100,000.00 for the Client Liaison Officer","PS",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
["L.1.2","Allow for Profit ","%"]
["L.1.3","Allow for Attendance","%"]
[]
["L.2","DISLUDGING",{"$nulls":4},0]
[{"$nulls":6},0]
["L.2.1","Provide the sum of R40,000.00 for disludging ablution blocks","PS",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"40,000.00"}]
["L.2.2","Allow for Profit ","%"]
["L.2.3","Allow for Attendance","%",{"$nulls":3},{"$f":"SUM(G17141:G17150)","v":0}]
[]
["L.3","CPD BUILD PROGRAMME"]
[]
[null,"Note to tenderers: As CPGs may not provide any bidder a competitive advantage. Provisional amounts and fixed percentages for profit and attendance have been provided. Only the provisional amount will be adjusted once the awarded tender amount and/or the beneficiaries have been appointed, and the final values have been ascertained. "]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL MANUFACTURERS"]
[null,"Provision is made for the Minimum Targeted Local Building Material Manufacturers CPG in the execution of this project as described in   C3.1 Project Specifications.  Allowance for monitoring and monthly reporting on material purchased from Local Building Material Manufacturers by main contractor and subcontractors based on determination by Employer taking into account specific project variables","PS",1,{"v":19377.110635937508,"d":"19,377.11"}]
[null,"Allowance for profit and attendance, all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL SUPPLIERS "]
[null,"Provision is made for the Minimum Targeted Local Building Material Suppliers CPG in the execution of this project as described in   C3.1 Project Specifications. Allowance for monitoring and monthly reporting on material purchased from Local Building Material Suppliers by main contractor and subcontractors based on determination by Employer  taking into account specific project variables ","PS",1,{"v":19377.110635937508,"d":"19,377.11"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED ENTERPRISE DEVELOPMENT"]
[null,"A provisional amount has been allowed for in the execution of this project as described in  C3.1 Project Specifications. The provisional amount allowed is for the appointment of training coordinator, mentor, training service providers and training of the beneficiary enterprises including monitoring and monthly reporting.","PS",1,{"v":193771.10635937506,"d":"193,771.11"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"LABOUR INTENSIVE PARTICIPATION GOAL"]
[null,"Labour Intensive Participation Goal - Allowance for monthly reporting of labour intensive works by main contractor based on determination by Employer taking into account specific project variables. Allowance for monitoring and monthly reporting on Works executed by means of Labour Intensive methods by main contractor and subcontractors based on determination by Employer taking into account specific project variables ",null,1,{"v":72000,"d":"72,000.00"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
{"$rows_empty":29}
[null,"Carried to Collection"]
[]
[null,{"$f":"B17139","v":"Provisional Sums"}]
[]
[]
[]
[null,{"$f":"B17208","v":"Provisional Sums"}]
[null,"Summary","Page"]
[]
[]
[null,"Summary brought forward",249]
{"$rows_empty":62}
[null,"Carried to Final Summary"]
[]
[null,{"$f":"B17212","v":"Provisional Sums"}]
[]
["Bill","Summary","Page"]
[]
[1,"PRELIMINARIES AND GENERAL",24]
[]
[2,"DEMOLITIONS",27]
[]
[3,"BLOCK A: GUARD HOUSE",52]
[]
[4,"BLOCK B: LABORATORY",71]
[]
[5,"BLOCK C: MINI ADMIN BLOCK",92]
[]
[6,"BLOCK D: 4 CLASSROOM BLOCK",117]
[]
[7,"BLOCK E: 5 CLASSROOM BLOCK",142]
[]
[8,"BLOCK F: TUCHSHOP, COMPUTER ROOM & 2 CLASSROOM BLOCK",167]
[]
[9,"BLOCK G: STAFFROOM & 3 CLASSROOM BLOCK",192]
[]
[10,"BLOCK H: 4 CLASSROOM BLOCK & 2 HOD OFFICES",217]
[]
[11,"BLOCK J: 2 CLASSROOM BLOCK",242]
[]
[12,"EXTERNAL WORKS",244]
[]
[13,"ELECTRICAL WORKS",248]
[]
[14,"PROVISIONAL SUMS",250]
[]
[null,"SUB-TOTAL"]
[]
[null,"CONTINGENCY AT 5%"]
[]
[null,"SUB-TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"GRAND TOTAL"]

{"sheet":"SNP Kitchen","index":1,"n_rows":1533,"n_cols":6,"rows_kept":1533,"hidden":true}
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 1"]
[]
[null,"FOUNDATIONS (ALL TRADES) (PROVISIONAL)"]
[]
[null,"Excavation in earth not exceeding 2m deep for:"]
[]
[1,"Reducing levels under solid floors.","m3",10,{"v":45,"d":"R45.00"},{"$f":"D9*E9","v":{"v":450,"d":"R450.00"}}]
[]
[2,"Trenches.","m3",26,{"v":60,"d":"R60.00"},{"$f":"D11*E11","v":{"v":1560,"d":"R1,560.00"}}]
[]
[null,"Extra over trench and hole excavations in earth for excavation in:"]
[]
[3,"Soft rock","m3",8,{"v":250,"d":"R250.00"},{"$f":"D15*E15","v":{"v":2000,"d":"R2,000.00"}}]
[]
[4,"Hard rock.","m3",10,{"v":450,"d":"R450.00"},{"$f":"D17*E17","v":{"v":4500,"d":"R4,500.00"}}]
[]
[null,"Keeping excavations free of water:"]
[]
[5,"Allow for keeping all excavations free of water.","Item",1,{"v":1000,"d":"R1,000.00"},{"$f":"D21*E21","v":{"v":1000,"d":"R1,000.00"}}]
[]
[null,"Risk of collapse of excavations:"]
[]
[6,"Vertical sides of excavation for trenches, etc., from"]
[null,"ground level to not exceeding 1,5m deep.","m2",48,{"v":10,"d":"R10.00"},{"$f":"D26*E26","v":{"v":480,"d":"R480.00"}}]
[]
[null,"Extra only over all excavations for loading and carting away"]
[]
[7,"Surplus spoil away from site (by volume as measured"]
[null,"for excavation - Contractor to make allowance for increase in bulk","m3",10,{"v":60,"d":"R60.00"},{"$f":"D31*E31","v":{"v":600,"d":"R600.00"}}]
[]
[null,"Selected earth filling from the excavations deposited in"]
[null,"layers not exceeding 150mm thick after compaction and"]
[null,"compacted to a density of 95% Modified AASHTO"]
[null,"maximum density:"]
[]
[8,"In backfilling to foundations around foundation walls","m3",7,{"v":65,"d":"R65.00"},{"$f":"D38*E38","v":{"v":455,"d":"R455.00"}}]
[]
[null,"Selected granular G5 filling material supplied and"]
[null,"carted onto the site by the Contractor and having a"]
[null,"plasticity index of less than 12, deposited in layers not"]
[null,"exceeding 150mm thick after compaction and"]
[null,"compacted to a density of 95% Modified AASHTO"]
[null,"maximum density:"]
[]
[9,"In filling under solid floors.","m3",7,{"v":455,"d":"R455.00"},{"$f":"D47*E47","v":{"v":3185,"d":"R3,185.00"}}]
[]
[null,"Selected granular G7 filling material supplied and"]
[null,"carted onto the site by the Contractor and having a"]
[null,"plasticity index of less than 12, deposited in layers not"]
[null,"exceeding 150mm thick after compaction and"]
[null,"compacted to a density of 93% Modified AASHTO"]
[null,"maximum density:"]
[]
[12,"In filling under solid floors.","m3",7,{"v":355,"d":"R355.00"},{"$f":"D56*E56","v":{"v":2485,"d":"R2,485.00"}}]
[]
[null,"Selected coarse river sand filling material supplied and"]
[null,"carted onto the site by the Contractor:"]
[]
[10,"50mm (Consolidated) layer of clean river sand well"]
[null,"watered and rolled to a hard true and even surface"]
[null,"under solid floors.","m2",50,{"v":90,"d":"R90.00"},{"$f":"D63*E63","v":{"v":4500,"d":"R4,500.00"}}]
[]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F3:F63)","v":{"v":21215,"d":"R21,215.00"}}]
[]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F66","v":{"v":21215,"d":"R21,215.00"}}]
[]
[null,"Compaction of ground surfaces:"]
[]
[11,"Stabilize in-situ reduced levels by scarifying to a depth"]
[null,"of 150mm and compacting to a density of 98%","m2",50,{"v":60,"d":"R60.00"},{"$f":"D74*E74","v":{"v":3000,"d":"R3,000.00"}}]
[null,"Modified AASHTO maximum density."]
[]
[null,"Prescribed density tests on filling:"]
[]
[12,"Allow for the execution of all prescribed density tests"]
[null,"on filling, etc., as pointed out by the Principal Agent on","No",4,{"v":350,"d":"R350.00"},{"$f":"D80*E80","v":{"v":1400,"d":"R1,400.00"}}]
[null,"site."]
[]
[null,"Soil poisoning applied by a registered pest control"]
[null,"company and guaranteed against termite infestation for"]
[null,"five years:"]
[]
[13,"Antproofing ground under solid foundations and to"]
[null,"vertical sides of excavations with a solution of Aldrin"]
[null,"or other approved emulsifiable concentrates","m2",50,{"v":20,"d":"R20.00"},{"$f":"D89*E89","v":{"v":1000,"d":"R1,000.00"}}]
[null,"complying with SABS 1164 and applied in accordance"]
[null,"with SABS 0124."]
[]
[14,"Antproofing ground under solid floors ditto including"]
[null,"raking out V-shaped channel 75mm wide against"]
[null,"walls, etc., and thoroughly saturate with antproofing","m2",17,{"v":20,"d":"R20.00"},{"$f":"D95*E95","v":{"v":340,"d":"R340.00"}}]
[null,"solution and fill in and tamp down."]
[]
[null,"CONCRETE"]
[]
[null,"Unreinforced Concrete"]
[]
[null,"15 MPa/19 mm concrete in:"]
[]
[15,"In blinding to foundations to walls cast against"]
[null,"excavated surfaces","m3",3,{"v":1100,"d":"R1,100.00"},{"$f":"D105*E105","v":{"v":3300,"d":"R3,300.00"}}]
[]
[null,"Reinforced Concrete"]
[]
[null,"25 MPa/19 mm concrete in:"]
[]
[16,"Foundations to walls cast against excavated surfaces","m3",8,{"v":1800,"d":"R1,800.00"},{"$f":"D111*E111","v":{"v":14400,"d":"R14,400.00"}}]
[]
[null,"CONCRETE TESTING"]
[]
[null,"Concrete test cubes:"]
[]
[17,"Allow for all necessary concrete test cubes size 150 x"]
[null,"150 x 150mm cast from batches of concrete required"]
[null,"for the entire contract as specified, made, stored,"]
[null,"cured and tested in accordance with SABS Methods"]
[null,"861 and 863, including use and waste of approved","No",4,{"v":450,"d":"R450.00"},{"$f":"D121*E121","v":{"v":1800,"d":"R1,800.00"}}]
[null,"cube moulds, transporting to an approved testing"]
[null,"laboratory for testing, paying all charges and"]
[null,"submitting reports to the Principal Agent."]
[]
[null,"FORMWORK"]
[]
[null,"Formwork (use and waste) to concrete to:"]
[]
[18,"Edges of foundation steppings not exceeding 300mm high","m",28,{"v":10,"d":"R10.00"},{"$f":"D130*E130","v":{"v":280,"d":"R280.00"}}]
[]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F69:F130)","v":{"v":46735,"d":"R46,735.00"}}]
[]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F133","v":{"v":46735,"d":"R46,735.00"}}]
[null,"REINFORCEMENT"]
[]
[null,"Steel bar reinforcement to concrete:"]
[]
[19,"Mild steel bars 6mm diameter in reinforcement to","kg",288,{"v":12.5,"d":"R12.50"},{"$f":"D141*E141","v":{"v":3600,"d":"R3,600.00"}}]
[null,"foundations, etc."]
[]
[20,"High tensile steel bars 12mm diameter ditto","kg",1008,{"v":16.5,"d":"R16.50"},{"$f":"D144*E144","v":{"v":16632,"d":"R16,632.00"}}]
[]
[null,"BRICKWORK"]
[]
[null,"Brickwork of 'Corobrik NFX' extra hard burnt bricks"]
[null,"(14MPa compressive strength) in Class I mortar:"]
[]
[21,"Half brick wall.","m2",9,{"v":300,"d":"R300.00"},{"$f":"D151*E151","v":{"v":2700,"d":"R2,700.00"}}]
[]
[22,"One brick wall in English bond.","m2",20,{"v":450,"d":"R450.00"},{"$f":"D153*E153","v":{"v":9000,"d":"R9,000.00"}}]
[]
[23,"One brick wall of two half brick skins in stretcher bond (no wire ties)","m2",0,{"v":450,"d":"R450.00"},{"$f":"D155*E155","v":{"v":0,"d":"R0.00"}}]
[]
[null,"Brickwork Sundries"]
[]
[null,"Brickwork reinforcement:"]
[]
[24,"High tensile steel fabric reinforcement 75mm wide to"]
[null,"every course of brick walls lapped full widths at angles","m",{"$f":"7.5*6","v":45},{"v":5,"d":"R5.00"},{"$f":"D162*E162","v":{"v":225,"d":"R225.00"}}]
[null,"and junctions and building in."]
[]
[25,"Ditto 150mm wide ditto.","m",165,{"v":7,"d":"R7.00"},{"$f":"D165*E165","v":{"v":1155,"d":"R1,155.00"}}]
[]
[null,"FACE BRICKWORK"]
[]
[null,"Facings"]
[]
[null,"Corobrik Firelight Satin FBX face bricks in stretcher"]
[null,"bond, in class I cement mortar, pointed with square"]
[null,"recessed horizontal and vertical joints (all brick skins to be"]
[null,"bagged and sealed)"]
[]
[28,"Extra over ordinary brickwork for facing in stretcher"]
[null,"bond and pointing.","m2",5,{"v":575,"d":"R575.00"},{"$f":"D177*E177","v":{"v":2875,"d":"R2,875.00"}}]
{"$rows_empty":19}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F136:F195)","v":{"v":82922,"d":"R82,922.00"}}]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 2"]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"VIBRATED REINFORCED CONCRETE"]
[]
[null,"25MPa/19mm concrete in:"]
[]
[1,"Surface beds laid in panels","m3",2,{"v":1800,"d":"R1,800.00"},{"$f":"D212*E212","v":{"v":3600,"d":"R3,600.00"}}]
[]
[2,"Turndowns to edges of surface beds including"]
[null,"additional excavations, filling in and ramming","m3",0.5,{"v":1800,"d":"R1,800.00"},{"$f":"D215*E215","v":{"v":900,"d":"R900.00"}}]
[]
[null,"25MPa/19mm concrete in:"]
[]
[3,"Surface beds laid in panels","m3",{"$f":"50*0.1","v":5},{"v":1800,"d":"R1,800.00"},{"$f":"D219*E219","v":{"v":9000,"d":"R9,000.00"}}]
[]
[4,"In veranda and play area","m3",5,{"v":1800,"d":"R1,800.00"},{"$f":"D221*E221","v":{"v":9000,"d":"R9,000.00"}}]
[]
[5,"In V drains","m3",3,{"v":1800,"d":"R1,800.00"},{"$f":"D223*E223","v":{"v":5400,"d":"R5,400.00"}}]
[]
[null,"CONCRETE TESTING"]
[]
[null,"Concrete testing:"]
[]
[6,"Allow for all necessary concrete test cubes size 150 x"]
[null,"150 x 150mm cast from batches of concrete required"]
[null,"for the entire contract as specified, made, stored,"]
[null,"cured and tested in accordance with SABS Methods"]
[null,"861 and 863, including use and waste of approved","No",12,{"v":450,"d":"R450.00"},{"$f":"D233*E233","v":{"v":5400,"d":"R5,400.00"}}]
[null,"cube moulds, transporting to an approved laboratory"]
[null,"for testing, paying all charges and submitting reports"]
[null,"to the Principal Agent"]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top of concrete to a non-slip finish obtained"]
[null,"by brushing with a stiff bristle broom before the"]
[null,"concrete has set:"]
[]
[7,"Surface beds.","m2",50,{"v":50,"d":"R50.00"},{"$f":"D244*E244","v":{"v":2500,"d":"R2,500.00"}}]
[]
[null,"FORMWORK"]
[]
[null,"Formwork (use and waste) to concrete to:"]
[]
[8,"Edges, risers, ends and reveals not exceeding 300mm"]
[null,"high or wide","m",28,{"v":10,"d":"R10.00"},{"$f":"D251*E251","v":{"v":280,"d":"R280.00"}}]
[]
[null,"MOVEMENT JOINTS"]
[]
[null,"10mm Bitumen impregnated insulation board"]
[null,"expansion joint filler closely butt jointed at"]
[null,"intersections including all cutting and waste and"]
[null,"maintaining in position during concreting in:"]
[]
[9,"Expansion joint between abutting edges of concrete"]
[null,"surface beds not exceeding 300mm high","m",24,{"v":10,"d":"R10.00"},{"$f":"D261*E261","v":{"v":240,"d":"R240.00"}}]
[]
[10,"Expansion joint between abutting edges of concrete"]
[null,"surface beds and brickwork not exceeding 300mm","m",24,{"v":10,"d":"R10.00"},{"$f":"D264*E264","v":{"v":240,"d":"R240.00"}}]
[null,"high."]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F211:F264)","v":{"v":36560,"d":"R36,560.00"}}]
[]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F267","v":{"v":36560,"d":"R36,560.00"}}]
[null,"REINFORCEMENT"]
[]
[null,"Steel fabric reinforcement to concrete"]
[]
[11,"Welded high tensile steel square mesh fabric"]
[null,"reinforcement reference 617 (mass 6,17kg/m2) to"]
[null,"surface beds laid in panels and lapped 200mm at"]
[null,"sides and ends including all cutting and waste","m2",50,{"v":60,"d":"R60.00"},{"$f":"D278*E278","v":{"v":3000,"d":"R3,000.00"}}]
[null,"(measured nett)."]
{"$rows_empty":52}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F270:F318)","v":{"v":39560,"d":"R39,560.00"}}]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 3"]
[]
[null,"MASONRY"]
[]
[null,"BRICKWORK IN CEMENT MORTAR"]
[]
[1,"Half brick wall.","m2",20,{"v":300,"d":"R300.00"},{"$f":"D344*E344","v":{"v":6000,"d":"R6,000.00"}}]
[]
[2,"Half brick beamfilling","m2",4,{"v":300,"d":"R300.00"},{"$f":"D346*E346","v":{"v":1200,"d":"R1,200.00"}}]
[]
[3,"Half brick wall above wall plate level inside roof space","m2",9,{"v":300,"d":"R300.00"},{"$f":"D348*E348","v":{"v":2700,"d":"R2,700.00"}}]
[]
[4,"One brick wall of two half brick skins in stretcher bond"]
[null,"(no wire ties).","m2",12,{"v":450,"d":"R450.00"},{"$f":"D351*E351","v":{"v":5400,"d":"R5,400.00"}}]
[]
[5,"One brick wall of two half brick skins in stretcher bond"]
[null,"above wall plate level inside roof space (no wire ties).","m2",8,{"v":450,"d":"R450.00"},{"$f":"D354*E354","v":{"v":3600,"d":"R3,600.00"}}]
[]
[6,"One brick wall of two half brick skins in stretcher bond"]
[null,"bagged and sealed (no wire ties).","m2",72,{"v":450,"d":"R450.00"},{"$f":"D357*E357","v":{"v":32400,"d":"R32,400.00"}}]
[]
[null,"Brickwork Sundries"]
[]
[null,"Flashings, etc:"]
[]
[7,"Cut groove in brickwork for turn-in of metal flashings and"]
[null,"point with an approved polysulphide joint sealant","m",1,{"v":10,"d":"R10.00"},{"$f":"D364*E364","v":{"v":10,"d":"R10.00"}}]
[]
[null,"Brickwork reinforcement"]
[]
[8,"High tensile steel fabric reinforcement 75mm wide to"]
[null,"brick walls lapped full width at angles and junctions and","m",68,{"v":5,"d":"R5.00"},{"$f":"D369*E369","v":{"v":340,"d":"R340.00"}}]
[null,"building in (measured nett)."]
[]
[9,"High tensile steel fabric reinforcement 150mm wide to"]
[null,"brick walls lapped full width at angles and junctions and"]
[null,"building in (measured nett).","m",248,{"v":7,"d":"R7.00"},{"$f":"D374*E374","v":{"v":1736,"d":"R1,736.00"}}]
[]
[null,"Galvanised hoop iron cramps, ties, etc:"]
[]
[10,"1,2 x 25mm Galvanised iron articulation anchor 365mm"]
[null,"girth bent once in centre and built into brickwork at","No",14,{"v":20,"d":"R20.00"},{"$f":"D379*E379","v":{"v":280,"d":"R280.00"}}]
[null,"425mm centres vertically"]
[]
[11,"1,2 x 25mm Galvanised iron articulation anchor 665mm"]
[null,"girth ditto","No",14,{"v":20,"d":"R20.00"},{"$f":"D383*E383","v":{"v":280,"d":"R280.00"}}]
[]
[12,"2 x 38mm Galvanised hoop iron roof truss anchor"]
[null,"1620mm girth with one end bent around timber roof truss"]
[null,"and spiked to timber wall plate and the other end"]
[null,"wrapped around and including 10mm diameter mild steel","No",14,{"v":30,"d":"R30.00"},{"$f":"D388*E388","v":{"v":420,"d":"R420.00"}}]
[null,"rod 150mm long and built six courses deep into top of"]
[null,"brick wall in cement mortar."]
[]
[null,"Air bricks, etc:"]
[]
[13,"Set of four 229 x 152mm Terra cotta vermin proof air"]
[null,"bricks and building in.","No",2,{"v":150,"d":"R150.00"},{"$f":"D395*E395","v":{"v":300,"d":"R300.00"}}]
[]
[14,"229 x 152mm Terra cotta vermin proof air brick and"]
[null,"building in.","No",16,{"v":200,"d":"R200.00"},{"$f":"D398*E398","v":{"v":3200,"d":"R3,200.00"}}]
[]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F341:F398)","v":{"v":57866,"d":"R57,866.00"}}]
[]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F401","v":{"v":57866,"d":"R57,866.00"}}]
[]
[null,"Turning pieces, etc., (use and waste) including propping,"]
[null,"struts, etc:"]
[]
[15,"To soffit of flat brick lintel 110mm wide.","m",1,{"v":120,"d":"R120.00"},{"$f":"D409*E409","v":{"v":120,"d":"R120.00"}}]
[]
[16,"To soffit of flat brick lintel 220mm wide","m",5,{"v":190,"d":"R190.00"},{"$f":"D411*E411","v":{"v":950,"d":"R950.00"}}]
[]
[null,"FACE BRICKWORK"]
[]
[null,"External"]
[]
[null,"Corobrik Firelight Satin FBX face bricks in stretcher"]
[null,"bond, in class I cement mortar, pointed with square"]
[null,"recessed horizontal and vertical joints (all brick skins to be"]
[null,"bagged and sealed)"]
[]
[17,"Extra over ordinary brickwork for face brickwork in half brick walls","m2",8,{"v":350,"d":"R350.00"},{"$f":"D422*E422","v":{"v":2800,"d":"R2,800.00"}}]
[]
[18,"Extra over ordinary brickwork for face brickwork on one side","m2",44,{"v":575,"d":"R575.00"},{"$f":"D424*E424","v":{"v":25300,"d":"R25,300.00"}}]
[]
[19,"Extra over ordinary brickwork for face brickwork on both sides","m2",28,{"v":575,"d":"R575.00"},{"$f":"D426*E426","v":{"v":16100,"d":"R16,100.00"}}]
[]
[20,"Extra over brickwork for facing brickwork in beamfilling","m2",5,{"v":350,"d":"R350.00"},{"$f":"D428*E428","v":{"v":1750,"d":"R1,750.00"}}]
[]
[21,"Fair raking cutting","m",14,{"v":20,"d":"R20.00"},{"$f":"D430*E430","v":{"v":280,"d":"R280.00"}}]
[]
[null,"Corobrik Firelight Satin FBX face bricks in stretcher"]
[null,"bond, in class I cement mortar, pointed with square"]
[null,"recessed horizontal and vertical joints (all brick skins to be"]
[null,"bagged and sealed)"]
[]
[22,"110mm Brick-on-edge sills with dpc sandwiched in mortar set","m",10,{"v":120,"d":"R120.00"},{"$f":"D437*E437","v":{"v":1200,"d":"R1,200.00"}}]
[null,"sloping at 15 degrees and slightly projecting"]
[]
[23,"Extra over ordinary brickwork for brick-on-edge header"]
[null,"course lining to soffit of one brick wall over opening and","m",10,{"v":190,"d":"R190.00"},{"$f":"D441*E441","v":{"v":1900,"d":"R1,900.00"}}]
[null,"pointing on one face and soffit 220mm wide."]
[]
[null,"PRESSED FIBRE REINFORCED CEMENT SILLS"]
[]
[null,"Pressed fibre reinforced cement sills:"]
[]
[24,"15 x 150mm Natural colour sills in single lengths set flat"]
[null,"and slightly projecting on front edge. (In No. 23).","m",10,{"v":190,"d":"R190.00"},{"$f":"D449*E449","v":{"v":1900,"d":"R1,900.00"}}]
{"$rows_empty":16}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F404:F464)","v":{"v":110166,"d":"R110,166.00"}}]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 4"]
[]
[null,"WATERPROOFING"]
[]
[null,"DAMPPROOFING OF WALLS AND FLOORS"]
[]
[null,"DAMP PROOF COURSES"]
[]
[null,"One layer of 375 micron 'Consol Plastics Brikgrip DPC'"]
[null,"embossed damp proof course:"]
[]
[1,"In walls.","m2",177,{"v":60,"d":"R60.00"},{"$f":"D483*E483","v":{"v":10620,"d":"R10,620.00"}}]
[]
[null,"VAPOUR BARRIERS"]
[]
[null,"One layer of 250 micron 'Gunplas USB Green' or other"]
[null,"approved waterproof sheeting sealed at laps with 'Gunplas"]
[null,"Pressure Sensitive Tape':"]
[]
[2,"Under concrete surface beds including turning up edges"]
[null,"against walls.","m2",98,{"v":60,"d":"R60.00"},{"$f":"D492*E492","v":{"v":5880,"d":"R5,880.00"}}]
[]
[null,"EXPANSION JOINT SEALANTS"]
[]
[null,"Polysulphide joint sealant:"]
[]
[null,"Elastomeric gun-grade two component polysulphide joint"]
[null,"sealant complying with SABS 110 including priming all"]
[null,"joint surfaces."]
[]
[3,"In filling to 10 x 15mm horizontal open joints including"]
[null,"raking out softboard.","m",9,{"v":10,"d":"R10.00"},{"$f":"D503*E503","v":{"v":90,"d":"R90.00"}}]
[]
[null,"WATERPROOF POINTING TO WINDOWS (PROVISIONAL"]
[]
[null,"Clear silicone non-hardening sealant:"]
[]
[4,"In pointing to one side of steel window frame against"]
[null,"masonry with a pressure gun in strict accordance with the"]
[null,"manufacturers instructions","m",18,{"v":30,"d":"R30.00"},{"$f":"D511*E511","v":{"v":540,"d":"R540.00"}}]
{"$rows_empty":20}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F482:F530)","v":{"v":17130,"d":"R17,130.00"}}]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 5"]
[]
[null,"ROOF COVERINGS, ETC"]
[]
[null,"GALVANISED MILD STEEL PROFILED ROOF SHEETING"]
[null,"AND ACCESSORIES"]
[]
[null,"0,58mm Thick galvanised (275g/m²) S-profile corrugated"]
[null,"Z275 spelter galvanised sheet steel with 'Chromadek ISQ"]
[null,"550' finsh one side in single lenghts fixed to timber purlins"]
[null,"at 1200mm centres with 'Leak King' roof screws and"]
[null,"washers all in accordance with the manufacturer's"]
[null,"instructions:"]
[]
[1,"Roof covering with pitch not exceeding 25 degrees.","m2",72,{"v":350,"d":"R350.00"},{"$f":"D553*E553","v":{"v":25200,"d":"R25,200.00"}}]
[]
[2,"Extra over for fixing every crown of roof covering at ends"]
[null,"of sheets","m",14,{"v":150,"d":"R150.00"},{"$f":"D556*E556","v":{"v":2100,"d":"R2,100.00"}}]
[]
[3,"Extra over for fixing every crown of roof covering at"]
[null,"ridges.","m",9,{"v":150,"d":"R150.00"},{"$f":"D559*E559","v":{"v":1350,"d":"R1,350.00"}}]
[]
[null,"0,58mm Thick galvanised (275g/m²) pressed steel fittings"]
[null,"with 'Chromadek ISQ 550' polyester finish on one side:"]
[]
[4,"Sidewall flashing 305mm girth","m",12,{"v":150,"d":"R150.00"},{"$f":"D564*E564","v":{"v":1800,"d":"R1,800.00"}}]
[]
[5,"Ridge capping 460mm girth.","m",9,{"v":150,"d":"R150.00"},{"$f":"D566*E566","v":{"v":1350,"d":"R1,350.00"}}]
[]
[null,"Sundries:"]
[]
[6,"Sondor corrugated pattern polyethelene polyclosers to"]
[null,"corrugated iron sheeting at ridge.","m",9,{"v":25,"d":"R25.00"},{"$f":"D571*E571","v":{"v":225,"d":"R225.00"}}]
[]
[7,"Sondor corrugated pattern polyethelene polyclosers to"]
[null,"corrugated iron sheeting at eaves.","m",14,{"v":25,"d":"R25.00"},{"$f":"D574*E574","v":{"v":350,"d":"R350.00"}}]
[]
[8,"Purpose made cover flashing to detail, 205mm girth,"]
[null,"twice bent with top edge wedged into groove (elsewhere"]
[null,"measured) and with bottom edge fixed to side wall"]
[null,"flashing with and including galvanised steel self-tapping"]
[null,"screws at 450mm centres","m",1,{"v":120,"d":"R120.00"},{"$f":"D580*E580","v":{"v":120,"d":"R120.00"}}]
[]
[null,"'Sisalation 420' heavy industrial grade reinforced"]
[null,"aluminium foil and polyethylene insulation:"]
[]
[9,"Reinforced aluminium foil insulation and waterproofing"]
[null,"lapped 140mm at all intersections as underlay to"]
[null,"galvanised sheet steel roofing and supported on and"]
[null,"including 1,6mm diameter galvanised wire supports"]
[null,"spaced at 300mm centres and wound around and"]
[null,"screwed to rafters of timber trusses including cutting and"]
[null,"waste (measured nett).","m2",{"$f":"50*1.3","v":65},{"v":60,"d":"R60.00"},{"$f":"D591*E591","v":{"v":3900,"d":"R3,900.00"}}]
{"$rows_empty":8}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F549:F591)","v":{"v":36395,"d":"R36,395.00"}}]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 6"]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"CARPENTRY"]
[]
[null,"SAWN SOFTWOOD"]
[]
[null,"Prices for all sawn timbers are to include for all"]
[null,"notchings, splay cuttings, housings, scarfing, etc., cutting"]
[null,"timbers to required lengths, spiking, clinching, bolting,"]
[null,"hoisting and fixing timbers in positions."]
[]
[null,"In roofs:"]
[]
[1,"38 x 114mm Wall plate.","m",21,{"v":100,"d":"R100.00"},{"$f":"D621*E621","v":{"v":2100,"d":"R2,100.00"}}]
[]
[2,"50 x 76mm Purlins.","m",48,{"v":80,"d":"R80.00"},{"$f":"D623*E623","v":{"v":3840,"d":"R3,840.00"}}]
[]
[3,"38 x 228mm Gangboard. (Provisional","m",22,{"v":125,"d":"R125.00"},{"$f":"D625*E625","v":{"v":2750,"d":"R2,750.00"}}]
[]
[null,"WROT SOFTWOOD"]
[]
[null,"In roofs"]
[]
[4,"50 X 76mm Purlins.","m",48,{"v":80,"d":"R80.00"},{"$f":"D631*E631","v":{"v":3840,"d":"R3,840.00"}}]
[]
[5,"50 x 76mm Counter battens for barge board fixing.","m",14,{"v":80,"d":"R80.00"},{"$f":"D633*E633","v":{"v":1120,"d":"R1,120.00"}}]
[]
[6,"50 x 76mm Eaves and verge trimmers","m",17,{"v":80,"d":"R80.00"},{"$f":"D635*E635","v":{"v":1360,"d":"R1,360.00"}}]
[]
[7,"76 x 76mm Splayed eaves purlins","m",17,{"v":90,"d":"R90.00"},{"$f":"D637*E637","v":{"v":1530,"d":"R1,530.00"}}]
[]
[null,"Sundries:"]
[]
[8,"Teco galvanised two way hurricane clip.","No",13,{"v":5,"d":"R5.00"},{"$f":"D641*E641","v":{"v":65,"d":"R65.00"}}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES"]
[]
[null,"Prefabricated roof trusses having a pitch of 15 degrees"]
[]
[null,"Double pitched trusses"]
[]
[9,"Double pitched truss for a clear span of 7,01m between"]
[null,"bearing walls of rafters, tie beam, posts and struts, with"]
[null,"110mm bearing each end and with tie beam projecting"]
[null,"1,81m beyond outer wall face and rafter end projecting"]
[null,"1m beyond outer wall face.","No",7,{"v":5000,"d":"R5,000.00"},{"$f":"D653*E653","v":{"v":35000,"d":"R35,000.00"}}]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"'Everite Nutec' or other approved fascias:"]
[]
[10,"12 x 225mm medium density fibre reinforced cement"]
[null,"plain fascia boarding fixed to ends of softwood rafters at"]
[null,"400mm centres in one direction including standard"]
[null,"plastic 'H'-section jointing strips fixed between abutting"]
[null,"edges of boarding and countersunk screwed on","m",17,{"v":180,"d":"R180.00"},{"$f":"D663*E663","v":{"v":3060,"d":"R3,060.00"}}]
[]
[11,"80 x 200mm medium density fibre reinforced cement"]
[null,"plain barge boarding fixed to ends of softwood counter"]
[null,"battens ditto.","m",14,{"v":180,"d":"R180.00"},{"$f":"D667*E667","v":{"v":2520,"d":"R2,520.00"}}]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F618:F667)","v":{"v":57185,"d":"R57,185.00"}}]
[]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F669","v":{"v":57185,"d":"R57,185.00"}}]
[null,"JOINERY"]
[]
[null,"DOORS"]
[]
[null,"EXTERIOR QUALITY FRAMED DOORS"]
[]
[null,"Exterior quality laminated batten framed, ledged and"]
[null,"braced doors faced on both sides with wrot saligna"]
[null,"battens:"]
[]
[12,"2032 x 813 x 40mm 'Meranti' ledged and braced battened door with "]
[null,"40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm","No",3,{"v":2400,"d":"R2,400.00"},{"$f":"D684*E684","v":{"v":7200,"d":"R7,200.00"}}]
[null,"bottom ledge and 20 x 110mm braces. (D1)"]
[]
[null,"FLUSH DOORS"]
[]
[null,"Semi-solid flush doors with 3,2mm hardboard covering on"]
[null,"both sides suitable for painting and with hardwood edge"]
[null,"strips"]
[]
[13,"2032 x 813 x 40mm thick Solid flush panel door with hardwood on both sides"]
[null,"and two hardwood edge strips completely as per Architect Specifications (D2)","No",2,{"v":2100,"d":"R2,100.00"},{"$f":"D694*E694","v":{"v":4200,"d":"R4,200.00"}}]
[]
[null,"SHELF AND WORKTOPS "]
[]
[14,"\"L\" Shaped wall shelves overall size 3 500mm long x 332mm wide x","No",3,{"v":8000,"d":"R8,000.00"},{"$f":"D698*E698","v":{"v":24000,"d":"R24,000.00"}}]
[null," 2100mm high completely according to Architect's drawings  (Detail No DT41B)"]
[]
[null,"WORKTOPS, etc"]
[]
[15,"3129 x 600mm wide at 900mm high from floor level counter top with a drawer ","No",1,{"v":8000,"d":"R8,000.00"},{"$f":"D703*E703","v":{"v":8000,"d":"R8,000.00"}}]
[null,"and lockable cupboard underneath comprising 19mm quadrant,22mm "]
[null,"chipboard shelves with hardwood veneer including 19 x 70mm S.A Pine wall "]
[null,"strip bolted to wall with 600 x 22mm Chipboard work top with 6mm bavelled"]
[null," edges screwed to support  brackets from underneath against the wall, finished "]
[null,"with melamine incliding 50 x 50 x 3mm angle-iron brackets welded together "]
[null,"with gusset plate to shape and fixed securely to the wall with 8 x 70 masonry"]
[null," anchors at 1000mm centres. Finished with one coat zinc-chromate primer. "]
[null,"One coat universal undercoat and 2 coats high gloss enamel paint in "]
[null,"appoved colour and all in accordance to Architect's specifications."]
[]
[null,"SKIRTING"]
[]
[16,"Meranti skirting","m",135,{"v":35,"d":"R35.00"},{"$f":"D716*E716","v":{"v":4725,"d":"R4,725.00"}}]
{"$rows_empty":16}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F672:F731)","v":{"v":105310,"d":"R105,310.00"}}]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 7"]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"25mm Thick Lambdaboard\" or other similar approved laminated "]
[null,"polyisocyanurate core board (PIR), minimum of 34kg/m3 core density, "]
[null,"uperfacing to be natural matt mineral-coated fibre glass tissue: lower "]
[null,"facing to be white matt mineral - coated fibreglass tissue, laminated on"]
[null,"both sides. Supplied in 1220mm widths to be fixed to ceiling brandering. "]
[null,"all including tapping and skiming as per supplier's instructions."]
[]
[1,"Ceilings fixed to and including 50 x 50mm sawn softwood"]
[null,"brandering spaced at 1000mm centres (or to manufacture's instructions) ","m2",42,{"v":200,"d":"R200.00"},{"$f":"D754*E754","v":{"v":8400,"d":"R8,400.00"}}]
[null,"in one direction and spiked to softwood tie beams."]
[]
[null,"Gypsum plasterboard:"]
[]
[2,"75mm Stock coved cornice with top edge nailed through"]
[null,"ceiling sheets to softwood brandering and bottom edge"]
[null,"bedded in gypsum plaster against and steel nailed to"]
[null,"wall.","m",39,{"v":35,"d":"R35.00"},{"$f":"D762*E762","v":{"v":1365,"d":"R1,365.00"}}]
[]
[null,"Ceiling insulation"]
[]
[3,"50mm Resin-bonded fibreglass insulation laid loose on"]
[null,"top of brandering between tie beams.","m2",42,{"v":220,"d":"R220.00"},{"$f":"D767*E767","v":{"v":9240,"d":"R9,240.00"}}]
[]
[null,"Wrot hardwood:"]
[]
[4,"Extra over ceilings for 600 x 600mm trap door of 32 x"]
[null,"44mm wrot hardwood rebated framing and 38 x 114mm"]
[null,"sawn softwood kerb spiked to rafters, etc., and filled in"]
[null,"with matching ceiling board in void. (Ceiling plate not"]
[null,"deducted).","No",2,{"v":900,"d":"R900.00"},{"$f":"D775*E775","v":{"v":1800,"d":"R1,800.00"}}]
{"$rows_empty":26}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F756:F800)","v":{"v":12405,"d":"R12,405.00"}}]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 8"]
[]
[null,"FLOOR TILES ECT"]
[]
[null,"VINYL FLOOR COVERINGS, ETC."]
[]
[null,"FLOOR/WALL TILES"]
[]
[null,"330 x 330 x 7mm 'Johnson Granito GN 573' ceramic floor"]
[null,"tiles of selected colour fixed with 'Tal Gold Star 6' rapid"]
[null,"setting tile adhesive with 6mm wide joints continuous in"]
[null,"both directions with joints pointed with 'Tal Fine Epoxy"]
[null,"Grout' on"]
[]
[1,"Non-slip to Floors","m2",48,{"v":300,"d":"R300.00"},{"$f":"D821*E821","v":{"v":14400,"d":"R14,400.00"}}]
[]
[2,"Skirting to walls 100mm high.","m",39,{"v":120,"d":"R120.00"},{"$f":"D823*E823","v":{"v":4680,"d":"R4,680.00"}}]
[]
[3,"Walls","m2",2,{"v":300,"d":"R300.00"},{"$f":"D825*E825","v":{"v":600,"d":"R600.00"}}]
{"$rows_empty":41}
[null,"Carried to Summary ",{"$nulls":3},{"v":19680,"d":"R19,680.00"}]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 9"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"Union' or other similar approved:"]
[]
[1,"Padlock as 'Union UN332500000010'.","No",2,{"v":500,"d":"R500.00"},{"$f":"E882*D882","v":{"v":1000,"d":"R1,000.00"}}]
[]
[null,"Solid' or other similar approved:"]
[]
[2,"Art 390/313 four lever lockset with striking plate fixed to"]
[null,"metal.","No",6,{"v":750,"d":"R750.00"},{"$f":"E887*D887","v":{"v":4500,"d":"R4,500.00"}}]
[]
[null,"Sundries:"]
[]
[3,"38mm Diameter rubber door stop plugged","No",5,{"v":60,"d":"R60.00"},{"$f":"E891*D891","v":{"v":300,"d":"R300.00"}}]
{"$rows_empty":41}
[null,"Carried to Summary ",{"$nulls":3},{"v":5800,"d":"R5,800.00"}]
[]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 10"]
[]
[null,"METALWORK"]
[]
[null,"GALVANISED MILD STEEL GATES AND FRAMES"]
[]
[null,"Galvanised mild steel gates and frames:"]
[]
[1,"Gate and frame to detail size 1,1 x 2,20m overall, the"]
[null,"gate in single leaf size 0,98 x 2,16m overall, with 50 x 30"]
[null,"x 3mm hollow section surround mitred and welded at"]
[null,"angles, two 30 x 6mm flat section intermediate rails"]
[null,"welded at ends to surrounds and holed for seven 12mm"]
[null,"diameter vertical bars welded at ends to surround and to"]
[null,"intermediate rails and with 55 x 40 x 8mm locking plate"]
[null,"holed for padlock (elsewhere measured) and welded to"]
[null,"surround, fitted with 40 x 60 x 2mm stop plate welded on"]
[null,"end to surround and 150mm galvanised steel heavy duty"]
[null,"barrel bolt welded to bottom of stile with brass ferrule"]
[null,"sunk flush in concrete floor as bolt socket; hang gate on"]
[null,"one and a half pairs of 25mm diameter x 80mm long"]
[null,"heavy duty pin hinges, each welded to gate surround and"]
[null,"to 60 x 40 x 3mm hollow section frame mitred and"]
[null,"welded at angles and each jamb four times holed and"]
[null,"head twice holed for and bolted to wall with four 12mm"]
[null,"diameter expanding bolts each 80mm long including"]
[null,"holing side of frame for passage of bolt heads.","No",3,{"v":4500,"d":"R4,500.00"},{"$f":"D967*E967","v":{"v":13500,"d":"R13,500.00"}}]
[]
[null,"GALVANISED MILD STEEL PRESSED DOOR FRAMES"]
[null,"BUILT INTO BRICKWORK"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls:"]
[]
[2,"Frame for door 813 x 2032mm high.","No",2,{"v":900,"d":"R900.00"},{"$f":"D974*E974","v":{"v":1800,"d":"R1,800.00"}}]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls:"]
[]
[3,"Frame for door 813 x 2032mm high","No",4,{"v":1200,"d":"R1,200.00"},{"$f":"D978*E978","v":{"v":4800,"d":"R4,800.00"}}]
[]
[null,"GALVANISED MILD STEEL WINDOWS BUILT INTO"]
[null,"BRICKWORK"]
[]
[null,"Standard industrial type windows with burglar guards to"]
[null,"opening and fixed sections:"]
[]
[4,"Window type SS41. Size 1302 x 511mm (W3).","No",4,{"v":2200,"d":"R2,200.00"},{"$f":"D986*E986","v":{"v":8800,"d":"R8,800.00"}}]
[]
[null,"Serranda' or other approved roller shutter:"]
[]
[5,"Approved hot dipped galvanised steel 46mm interlocking 11,5kg/m2"]
[null,"slatted roller shutter door with push up action supplied complete with the"]
[null,"manufacture's recommendations "]
[null,"complete with guides, brackets, barrel, counterbalance"]
[null,"canopy, crank handle, gearbox, drive shaft, gears, etc.,"]
[null,"and suitable locking device, all assembled and erected in"]
[null,"accordance with the manufaturer's instructions including"]
[null,"bolting hood, guides, etc., to wall, oiling, greasing and"]
[null,"adjusting until working perfectly.(D7)","No",1,{"v":18000,"d":"R18,000.00"},{"$f":"D998*E998","v":{"v":18000,"d":"R18,000.00"}}]
[]
[]
[]
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F966:F998)","v":{"v":46900,"d":"R46,900.00"}}]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[]
[null,"BILL NO. 11"]
[]
[null,"PLASTERING"]
[]
[null,"PAVINGS"]
[]
[null,"Cement (1:3) steel trowelled to a smooth even surface on"]
[null,"concrete:"]
[]
[1,"30mm Screed on floors for vinyl tiles.","m2",48,{"v":75,"d":"R75.00"},{"$f":"D1018*E1018","v":{"v":3600,"d":"R3,600.00"}}]
[]
[null,"Dividing strips, etc:"]
[]
[2,"3 x 30mm Brass dividing strips in single lengths and"]
[null,"embedding in floor screed with top edge set projecting to"]
[null,"finish flush with floor finish","m",7,{"v":120,"d":"R120.00"},{"$f":"D1024*E1024","v":{"v":840,"d":"R840.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"Internal"]
[]
[null,"Render one coat plaster composed of four parts sand to"]
[null,"one part cement steel trowelled to a smooth even surface"]
[null,"on concrete or brickwork:"]
[]
[3,"On walls.","m2",166,{"v":60,"d":"R60.00"},{"$f":"D1034*E1034","v":{"v":9960,"d":"R9,960.00"}}]
[]
[4,"On narrow widths.","m2",4,{"v":60,"d":"R60.00"},{"$f":"D1036*E1036","v":{"v":240,"d":"R240.00"}}]
{"$rows_empty":30}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F1017:F1065)","v":{"v":14640,"d":"R14,640.00"}}]
[]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 12"]
[]
[null,"PLUMBING"]
[]
[]
[null,"The Tenderer is referred to the relevent Clauses in the"]
[null,"Model Preambles to All Trades and to the Supplementary"]
[null,"Preambles which are incorporated at the back of these"]
[null,"Bills of Quantities"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Note"]
[]
[null,"All notes and supplementary preambles in the various"]
[null,"trades shall apply equally to this trade insofar as they are"]
[null,"relevant"]
[]
[null,"EXTERNAL"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"0.6mm Sheet iron with 'Chromadek' white powder-coated"]
[null,"finish seamless gutters or other similar approved"]
[]
[1,"125 x 100 x 0.6mm seamless aluminium gutters, all according to architects "]
[null,"specification","m",{"$f":"10.077*2","v":{"v":20.154,"d":"20"}},{"v":180,"d":"R180.00"},{"$f":"D1101*E1101","v":{"v":3627.72,"d":"R3,627.72"}}]
[]
[2,"Extra over 125 x 100mm eaves gutter for stopped end","No",6,{"v":165,"d":"R165.00"},{"$f":"D1103*E1103","v":{"v":990,"d":"R990.00"}}]
[]
[3,"Extra over 125 x 100mm eaves gutter for outlet for 125 x"]
[null," 75mm pipe","No",5,{"v":165,"d":"R165.00"},{"$f":"D1106*E1106","v":{"v":825,"d":"R825.00"}}]
[]
[4,"75mm diameter hollowed steel post Rainwater pipes.","m",{"$f":"2.635*5","v":{"v":13.174999999999999,"d":"13"}},{"v":165,"d":"R165.00"},{"$f":"D1108*E1108","v":{"v":2173.875,"d":"R2,173.88"}}]
[]
[5,"Extra over 100 x 75mm rainwater pipe for bend","No",10,{"v":165,"d":"R165.00"},{"$f":"D1110*E1110","v":{"v":1650,"d":"R1,650.00"}}]
[]
[6,"Extra over 100 x 75mm rainwater pipe for shoe.","No",5,{"v":165,"d":"R165.00"},{"$f":"D1112*E1112","v":{"v":825,"d":"R825.00"}}]
[]
[null,"SANITARY FITTINGS "]
[]
[null,"L G Green "]
[]
[null,"Franke Kitchen System (Pty) Ltd (trading as Citimal)"]
[null,"Stainless steel or other similar approved"]
[]
[7,"Franke Model SIRX342 Wash trough, 500x450x240mm deep,","No",2,{"v":1800,"d":"R1,800.00"},{"$f":"D1121*E1121","v":{"v":3600,"d":"R3,600.00"}}]
[null,"with a 40mm waste outlet, including all necessary accessories completely."]
[]
[8,"Soap dish","No",1,{"v":500,"d":"R500.00"},{"$f":"D1124*E1124","v":{"v":500,"d":"R500.00"}}]
{"$rows_empty":13}
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F1099:F1136)","v":{"v":14191.595,"d":"R14,191.60"}}]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F1138","v":{"v":14191.595,"d":"R14,191.60"}}]
[]
[null,"TRAPS ETC "]
[]
[null,"\"Cobra Watertech\" or other similar approved"]
[]
[9,"40mm 340 CP Bottle trap","No",2,{"v":450,"d":"R450.00"},{"$f":"D1149*E1149","v":{"v":900,"d":"R900.00"}}]
[]
[null,"TAPS, VALVES, ETC "]
[]
[null,"Brass "]
[]
[10,"22mm Fullway gate valve ","No",1,{"v":120,"d":"R120.00"},{"$f":"D1155*E1155","v":{"v":120,"d":"R120.00"}}]
[]
[null,"Chromium Plated "]
[]
[11,"20mm Angle regulating valve","No",1,{"v":150,"d":"R150.00"},{"$f":"D1159*E1159","v":{"v":150,"d":"R150.00"}}]
[]
[null,"WASTE PIPES "]
[]
[null,"uPVC pipes "]
[]
[12,"40mm Pipes ","m",12,{"v":65,"d":"R65.00"},{"$f":"D1165*E1165","v":{"v":780,"d":"R780.00"}}]
[]
[null,"Extra over uPVC pipes for fittings "]
[]
[13,"40mm Bend","No",2,{"v":65,"d":"R65.00"},{"$f":"D1169*E1169","v":{"v":130,"d":"R130.00"}}]
[]
[14,"40mm Junction ","No",1,{"v":75,"d":"R75.00"},{"$f":"D1171*E1171","v":{"v":75,"d":"R75.00"}}]
[]
[null,"Class 0 copper pipes "]
[]
[15,"15mm Pipes","m",5,{"v":30,"d":"R30.00"},{"$f":"D1175*E1175","v":{"v":150,"d":"R150.00"}}]
[]
[16,"22mm Pipes ","m",5,{"v":35,"d":"R35.00"},{"$f":"D1177*E1177","v":{"v":175,"d":"R175.00"}}]
[]
[17,"15mm Pipe in and including chase","m",3,{"v":30,"d":"R30.00"},{"$f":"D1179*E1179","v":{"v":90,"d":"R90.00"}}]
[]
[18,"22mm Pipe in and including chase","m",3,{"v":35,"d":"R35.00"},{"$f":"D1181*E1181","v":{"v":105,"d":"R105.00"}}]
[]
[19,"15mm Fittings","m",5,{"v":30,"d":"R30.00"},{"$f":"D1183*E1183","v":{"v":150,"d":"R150.00"}}]
[]
[20,"22mm Fittings ","No",4,{"v":35,"d":"R35.00"},{"$f":"D1185*E1185","v":{"v":140,"d":"R140.00"}}]
[]
[null,"Testing "]
[]
[21,"Testing waste pipe system ","Item",1,{"v":1000,"d":"R1,000.00"},{"$f":"D1189*E1189","v":{"v":1000,"d":"R1,000.00"}}]
[]
[null,"WATER SUPPLIES "]
[]
[null,"Class 9 uPVC pressure pipes "]
[]
[22,"50mm Pipe","m",25,{"v":90,"d":"R90.00"},{"$f":"D1195*E1195","v":{"v":2250,"d":"R2,250.00"}}]
[]
[null,"Extra over uPVC Class 9 pressure pipes for fittings with rubber"]
[null," ring joints "]
[]
[23,"63mm Reducer ","No",2,{"v":110,"d":"R110.00"},{"$f":"D1200*E1200","v":{"v":220,"d":"R220.00"}}]
[]
[24,"50mm Bend ","No",1,{"v":90,"d":"R90.00"},{"$f":"D1202*E1202","v":{"v":90,"d":"R90.00"}}]
[]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F1143:F1202)","v":{"v":20716.595,"d":"R20,716.60"}}]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F1205","v":{"v":20716.595,"d":"R20,716.60"}}]
[]
[25,"63mm Bend ","No",1,{"v":110,"d":"R110.00"},{"$f":"D1212*E1212","v":{"v":110,"d":"R110.00"}}]
[]
[null,"HDPE pipes "]
[]
[26,"63mm Pipe in and including trenches","m",20,{"v":110,"d":"R110.00"},{"$f":"D1216*E1216","v":{"v":2200,"d":"R2,200.00"}}]
[]
[null,"Extra over HDPE pipes for fittings "]
[]
[27,"63mm Bend","No",1,{"v":110,"d":"R110.00"},{"$f":"D1220*E1220","v":{"v":110,"d":"R110.00"}}]
[]
[28,"63mm Tee","No",1,{"v":110,"d":"R110.00"},{"$f":"D1222*E1222","v":{"v":110,"d":"R110.00"}}]
[]
[29,"63 x 40 x 63mm Reducing Tee","No",1,{"v":110,"d":"R110.00"},{"$f":"D1224*E1224","v":{"v":110,"d":"R110.00"}}]
[]
[null,"Extra over HDPE Pipes for cast iron fittings "]
[]
[30,"63mm Gate valve including all necessary flanges, drilling, bolts","No",1,{"v":250,"d":"R250.00"},{"$f":"D1228*E1228","v":{"v":250,"d":"R250.00"}}]
[null,"and connection to HDPE pipe"]
[]
[null,"Testing "]
[]
[31,"Testing water pipe system","Item",1,{"v":1000,"d":"R1,000.00"},{"$f":"D1233*E1233","v":{"v":1000,"d":"R1,000.00"}}]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"\"ZIP\" or other similar approved HydroBoil"]
[]
[32,"5 Litre Stainless Steel instant boiling water unit. Outer case manufactured","No",1,{"v":4500,"d":"R4,500.00"},{"$f":"D1239*E1239","v":{"v":4500,"d":"R4,500.00"}}]
[null,"from Stainless Steel with a two-way tap, complete with twin-chamber"]
[null,"technology. Unit to be installed in accordance with manufacturer’s"]
[null,"installation instruction."]
[]
[null,"Chubb' or other approved"]
[]
[33,"Portable 4,5kg dry chemical powder all-purpose hand fire"]
[null,"extinguisher complying with SABS 1151 including"]
[null,"charging and complete with wall mounting bracket and"]
[null,"fixing to hardwood backboard (elsewhere measured).","No",1,{"v":1200,"d":"R1,200.00"},{"$f":"D1249*E1249","v":{"v":1200,"d":"R1,200.00"}}]
[]
[34,"19 x 225mm Wrot all red meranti chamfered and oil"]
[null,"polished backboard 750mm long four times plugged and"]
[null,"countersunk screwed to plastered wall","No",1,{"v":500,"d":"R500.00"},{"$f":"D1253*E1253","v":{"v":500,"d":"R500.00"}}]
[]
[35,"\"Everyway\" hose reel complete with 30m plastic hose,","No",1,{"v":1900,"d":"R1,900.00"},{"$f":"D1255*E1255","v":{"v":1900,"d":"R1,900.00"}}]
[null," chromium plated stopcock, shut-off nozzle and wall bracket."]
[]
[null,"Concrete Wash hand basin"]
[]
[36,"Supply and install precast made concrete wash hand basin"]
[null,"fixed to external walls of the kitchen","No",3,{"v":950,"d":"R950.00"},{"$f":"D1261*E1261","v":{"v":2850,"d":"R2,850.00"}}]
{"$rows_empty":9}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F1209:F1269)","v":{"v":35556.595,"d":"R35,556.60"}}]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 13"]
[]
[null,"GLAZING"]
[]
[null,"CLEAR FLOAT GLASS AND GLAZING"]
[]
[null,"4mm Pacific obscure glass and glazing to:"]
[]
[1,"Steel sashes in panes exceeding 0,1m2 but not"]
[null,"exceeding 0,5m2.","m2",3,{"v":90,"d":"R90.00"},{"$f":"D1285*E1285","v":{"v":270,"d":"R270.00"}}]
{"$rows_empty":49}
[null,"Carried to Summary ",{"$nulls":3},{"v":270,"d":"R270.00"}]
[]
[]
[]
[]
[]
[]
["Item","Descriptions","Unit","Quantity","Rate","Amount"]
[null,"BILL NO. 14"]
[]
[null,"PAINTWORK"]
[]
[null,"PAINT ON WALLS, CEILINGS, ETC"]
[]
[null,"Prepare and apply one coat acrylic fillercoat to SABS 1416"]
[null,"and two finishing coats acrylic polyvinyl acetate emulsion"]
[null,"paint to SABS 1586 on:"]
[]
[1,"Internal plastered walls.","m2",166,{"v":60,"d":"R60.00"},{"$f":"D1353*E1353","v":{"v":9960,"d":"R9,960.00"}}]
[]
[null,"PAINT ON PLASTERBOARD"]
[]
[null,"Prepare and apply one sealer undercoat to SABS 1416 and"]
[null,"two finishing coats acrylic polyvinyl acetate emulsion paint"]
[null,"to SABS 1586 on"]
[]
[2,"Ceilings with primed steel jointing strips and cornices"]
[null,"including stopping up and priming nailheads","m2",42,{"v":60,"d":"R60.00"},{"$f":"D1362*E1362","v":{"v":2520,"d":"R2,520.00"}}]
[]
[null,"PAINT ON FIBRE CEMENT"]
[]
[null,"Prepare and apply one sealer undercoat to SABS 1416 and"]
[null,"two finishing coats acrylic polyvinyl acetate emulsion paint"]
[null,"to SABS 1586 on:"]
[]
[3,"External fibre reinforced cement fascias and barge"]
[null,"boards","m",31,{"v":30,"d":"R30.00"},{"$f":"D1371*E1371","v":{"v":930,"d":"R930.00"}}]
[]
[4,"Internal sill not exceeding 300mm girth.","m",2,{"v":30,"d":"R30.00"},{"$f":"D1373*E1373","v":{"v":60,"d":"R60.00"}}]
[]
[null,"PAINT ON METAL"]
[]
[null,"Prepare and apply two coats approved bitumen paint on"]
[null,"galvanised mild steel:"]
[]
[5,"Back of pressed steel door frames","m2",6,{"v":60,"d":"R60.00"},{"$f":"D1380*E1380","v":{"v":360,"d":"R360.00"}}]
[]
[null,"Prepare and apply two coats 'Silvershine' aluminium paint"]
[null,"on galvanised mild steel to SABS 630 on"]
[]
[6,"Pressed steel door frames. (Provisional).","m2",6,{"v":60,"d":"R60.00"},{"$f":"D1385*E1385","v":{"v":360,"d":"R360.00"}}]
[]
[7,"Steel windows with glazing bars (both sides measured)."]
[null,"(Provisional).","m2",7,{"v":60,"d":"R60.00"},{"$f":"D1388*E1388","v":{"v":420,"d":"R420.00"}}]
[]
[8,"Steel 'brick-pattern' burglar guards (both sides"]
[null,"measured). (Provisional).","m2",7,{"v":60,"d":"R60.00"},{"$f":"D1391*E1391","v":{"v":420,"d":"R420.00"}}]
[]
[9,"Steel gates (both sides measured). (Provisional).","m2",12,{"v":60,"d":"R60.00"},{"$f":"D1393*E1393","v":{"v":720,"d":"R720.00"}}]
[]
[10,"Gate frame not exceeding 300mm girth. (Provisional).","m",4,{"v":30,"d":"R30.00"},{"$f":"D1395*E1395","v":{"v":120,"d":"R120.00"}}]
[]
[11,"Rafters, bracing, wall ties, etc., not exceeding 300mm"]
[null,"girth. (Provisional).","m",120,{"v":30,"d":"R30.00"},{"$f":"D1398*E1398","v":{"v":3600,"d":"R3,600.00"}}]
[]
[null,"PAINT ON WOOD"]
[]
[null,"Prepare and apply two coats 'ABE Provonite' on:"]
[]
[12,"General surfaces at eaves and verges. (Provisional).","m2",5,{"v":60,"d":"R60.00"},{"$f":"D1404*E1404","v":{"v":300,"d":"R300.00"}}]
[]
[]
[null,"Carried Forward",{"$nulls":3},{"$f":"SUM(F1352:F1404)","v":{"v":19770,"d":"R19,770.00"}}]
[]
[null,"Brought Forward",{"$nulls":3},{"$f":"F1407","v":{"v":19770,"d":"R19,770.00"}}]
[]
[null,"Prepare and apply one coat general purpose wood primer"]
[null,"to SABS 678 Type III, one coat universal undercoat to"]
[null,"SABS 681 Type II and two coats 'Velvaglo' polyurethane"]
[null,"enamel to SABS 630 on:"]
[]
[13,"Doors","m2",23,{"v":30,"d":"R30.00"},{"$f":"D1416*E1416","v":{"v":690,"d":"R690.00"}}]
{"$rows_empty":53}
[null,"Carried to Summary ",{"$nulls":3},{"$f":"SUM(F1409:F1468)","v":{"v":20460,"d":"R20,460.00"}}]
{"$rows_empty":7}
[null,"SUMMARY"]
[]
[]
[1,"FOUNDATIONS (ALL TRADES) (PROVISIONAL)",{"$nulls":3},{"$f":"F197","v":{"v":82922,"d":"R82,922.00"}}]
[]
[2,"CONCRETE, FORMWORK AND REINFORCEMENT",{"$nulls":3},{"$f":"F332","v":{"v":39560,"d":"R39,560.00"}}]
[]
[3,"MASONRY",{"$nulls":3},{"$f":"F466","v":{"v":110166,"d":"R110,166.00"}}]
[]
[4,"WATERPROOFING",{"$nulls":3},{"$f":"F532","v":{"v":17130,"d":"R17,130.00"}}]
[]
[5,"ROOF COVERINGS, ETC",{"$nulls":3},{"$f":"F600","v":{"v":36395,"d":"R36,395.00"}}]
[]
[6,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F733","v":{"v":105310,"d":"R105,310.00"}}]
[]
[7,"CEILINGS PARTITIONS AND ACCESS FLOORING",{"$nulls":3},{"$f":"F802","v":{"v":12405,"d":"R12,405.00"}}]
[]
[8,"FLOOR TILES, ETC",{"$nulls":3},{"$f":"F867","v":{"v":19680,"d":"R19,680.00"}}]
[]
[9,"IRONMONGERY",{"$nulls":3},{"$f":"F933","v":{"v":5800,"d":"R5,800.00"}}]
[]
[10,"METALWORK",{"$nulls":3},{"$f":"F1002","v":{"v":46900,"d":"R46,900.00"}}]
[]
[11,"PLASTERING",{"$nulls":3},{"$f":"F1067","v":{"v":14640,"d":"R14,640.00"}}]
[]
[12,"PLUMBING",{"$nulls":3},{"$f":"F1271","v":{"v":35556.595,"d":"R35,556.60"}}]
[]
[13,"GLAZING",{"$nulls":3},{"$f":"F1335","v":{"v":270,"d":"R270.00"}}]
[]
[14,"PAINTWORK",{"$nulls":3},{"$f":"F1470","v":{"v":20460,"d":"R20,460.00"}}]
{"$rows_empty":25}
[null,"Carried to Final Summary",{"$nulls":3},{"$f":"SUM(F1478:F1530)","v":{"v":547194.595,"d":"R547,194.60"}}]

{"sheet":"Borehole","index":2,"n_rows":97,"n_cols":7,"rows_kept":97,"hidden":true}
["Item","Description","Unit","Qty","Rate","Water & Sanitation","Maintenance"]
[]
[null,"BOREHOLE"]
[]
[null,"Feasibility Study"]
[]
[null,"Visit to the construction site, establishthe availability of reliable power supply, take the site coordinates","No",1,{"v":2000,"d":"2,000.00"},{"$f":"D7*E7","v":{"v":2000,"d":"2,000.00"}}]
[]
[null,"Sighting"]
[]
[null,"Preparation of Desktop report to locate possible underground water, exploration exercise report","No",1,{"v":15000,"d":"15,000.00"},{"$f":"D11*E11","v":{"v":15000,"d":"15,000.00"}}]
[]
[null,"Locating of the position to drill for underground water","No",1,{"v":3500,"d":"3,500.00"},{"$f":"D13*E13","v":{"v":3500,"d":"3,500.00"}}]
[]
[null,"Establishment"]
[]
[null,"Site establishment","Item",1,{"v":5000,"d":"5,000.00"},{"$f":"D17*E17","v":{"v":5000,"d":"5,000.00"}}]
[]
[null,"Setting up","No",1,{"v":2500,"d":"2,500.00"},{"$f":"D19*E19","v":{"v":2500,"d":"2,500.00"}}]
[]
[null,"Drilling"]
[]
[null,"216mm rotary percussion 0-25","m",25,{"v":250,"d":"250.00"},{"$f":"D23*E23","v":{"v":6250,"d":"6,250.00"}}]
[]
[null,"165mm rotary percussion 0-100","m",75,{"v":350,"d":"350.00"},{"v":26250,"d":"26,250.00"}]
[]
[null,"165mm rotary percussion100-150","m",50,{"v":375,"d":"375.00"},{"v":18750,"d":"18,750.00"}]
[]
[null,"Steel Casing"]
[]
[null,"Supply and Install 6.5X0.3mm casing, say 20meters","No",5,{"v":300,"d":"300.00"},{"$f":"D31*E31","v":{"v":1500,"d":"1,500.00"}}]
[]
[null,"Development"]
[]
[null,"Estimate yield, constant discharge test & deflowering of borehole","Hr",24,{"v":625,"d":"625.00"},{"$f":"D35*E35","v":{"v":15000,"d":"15,000.00"}}]
[]
[null,"Sanitary Seal"]
[]
[null,"Sanitary seal around casing","Each",1,{"v":1200,"d":"1,200.00"},{"$f":"D39*E39","v":{"v":1200,"d":"1,200.00"}}]
[]
[null,"Capping"]
[]
[null,"Cut, bend and weld casing closed","Each",1,{"v":350,"d":"350.00"},{"$f":"D43*E43","v":{"v":350,"d":"350.00"}}]
[]
[null,"De-establishment"]
[]
[null,"Borehole marking","No",1,{"v":500,"d":"500.00"},{"$f":"D47*E47","v":{"v":500,"d":"500.00"}}]
[]
[null,"Gravel parking","m3",3,{"v":450,"d":"450.00"},{"v":1350,"d":"1,350.00"}]
[]
[null,"Construction of concrete plinth","m3",2,{"v":2000,"d":"2,000.00"},{"v":4000,"d":"4,000.00"}]
[]
[null,"Dissemble setting out","Item",1,{"v":2500,"d":"2,500.00"},{"v":2500,"d":"2,500.00"}]
[]
[null,"Water Quality Test"]
[]
[null,"Take three water samples to Laboratory for Bacterial and for chemical presence (takes 5 days)","No",1,{"v":4500,"d":"4,500.00"},{"$f":"D57*E57","v":{"v":4500,"d":"4,500.00"}}]
[]
[null,"Ironmongery"]
[]
[null,"Construction of the Galvanized Tank Stand 4.5 M, inclusive of Manufacture, delivery to site, construction of foundations, installation and issuing of the COC 10,000 litres","No",1,{"v":60000,"d":"60,000.00"},{"$f":"D61*E61","v":{"v":60000,"d":"60,000.00"}}]
[]
[null,"Plumbing"]
[]
[null,"Installation of submersible pump, SVM 3038 Pump, 1.1 Kw 230V motor, including the subtronic controlbox, 82A2 Joint Kit, 16mm 4 core submersible cable, 32mm Baseplate","No",1,{"v":25000,"d":"25,000.00"},{"$f":"D65*E65","v":{"v":25000,"d":"25,000.00"}}]
[]
[null,"Reticulation trenching from the borehole to the school reservoir , distance not greater than 300meters, pipe size unknown but we shall use 32mm","m",300,{"v":15,"d":"15.00"},{"$f":"D67*E67","v":{"v":4500,"d":"4,500.00"}}]
[]
[null,"Reticulation to the School Kitchen and the Drinking Fountain using the 32mm HDPE pipe,distance not greater than 300meters (each come in 100m)","No",1,{"v":1500,"d":"1,500.00"},{"v":1500,"d":"1,500.00"}]
[]
[null,"Installation of 10 000l plastic Tank","No",1,{"v":12000,"d":"12,000.00"},{"v":12000,"d":"12,000.00"}]
[]
[null,"Electrical Works"]
[]
[null,"Cable trenching to the nearest electrical supply point, for intermediate material distance not greater than 100 meters, 2,5mm 4 core cable","m",100,{"v":75,"d":"75.00"},{"$f":"D75*E75","v":{"v":7500,"d":"7,500.00"}}]
[]
[null,"Fitment of the circuit board and circuit breakers","Provisional",1,{"v":5500,"d":"5,500.00"},{"$f":"D77*E77","v":{"v":5500,"d":"5,500.00"}}]
[]
[null,"Masonry"]
[]
[null,"Construction of Generator Room","Provisional",1,{"v":12000,"d":"12,000.00"},{"$f":"D81*E81","v":{"v":12000,"d":"12,000.00"}}]
[]
[null,"Travelling"]
[]
[null,"Traveling and Tollgates","No",2,{"v":3650,"d":"3,650.00"},{"$f":"D85*E85","v":{"v":7300,"d":"7,300.00"}}]
[]
[null,"Labour"]
[]
[null,"Labour rate for period of 2 days","No ",12,{"v":480,"d":"480.00"},{"$f":"D89*E89","v":{"v":5760,"d":"5,760.00"}}]
[]
[null,"De-establishment"]
[]
[null,"Moving off the construction site","Item",1,{"v":2500,"d":"2,500.00"},{"$f":"D93*E93","v":{"v":2500,"d":"2,500.00"}}]
[]
[]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F7:F96)","v":{"v":253710,"d":"R 253,710.00"}},{"$f":"SUM(G9:G96)","v":{"v":0,"d":"R 0.00"}}]

{"sheet":"New","index":3,"n_rows":1044,"n_cols":10,"rows_kept":1044,"hidden":true,"merged":[[1043,4,1043,5]]}
["Item","Description","Unit","Qty","Rate","Amount"]
[]
["A","PRELIMINARY AND GENERAL"]
[]
[null,"NOTES"]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition) prepared by the Joint Building Contract Committee"]
[null,"shall be the applicable building agreement, amended as"]
[null,"hereinafter described The ASAQS Preliminaries (November"]
[null," 2007 edition) published by the Association of South African"]
[null," Quantity Surveyors for use with the said JBCC Principal"]
[null," Building Agreement shall be deemed to be incorporated in"]
[null," these bills of quantities Contractors are referred to the"]
[null," abovementioned documents for the full intent and meaning of"]
[null," each clause thereof"]
[]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the abovementioned documents"]
[null,"Where any item is not relevant to this specific contract such"]
[null,"item is marked N/A, signifying \"not applicable\""]
[null," "]
[]
[null,"PREAMBLES FOR TRADES "]
[]
[null,"The Model Preambles for Trades (1999 edition) as published"]
[null,"by the Association of South African Quantity Surveyors shall be"]
[null," deemed to be incorporated in these bills of quantities and no"]
[null," claims arising from brevity of description of items fully"]
[null,"described in the said Model Preambles will be entertained"]
[null,"Supplementary preambles are incorporated in these bills of"]
[null,"quantities to satisfy the requirements of this project Such"]
[null,"supplementary preambles shall take precedence over the"]
[null,"provisions of the said Model Preambles"]
[null,"The contractor's prices for all items throughout these bills of"]
[null,"quantities must take account of and include for all of the"]
[null,"obligations, requirements and specifications given in the said"]
[null,"Model Preambles and in any supplementary preambles"]
[]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"CPAP WORK GROUP "]
[]
[null,"Unless otherwise stated all items in this bill will be Work Group"]
[null,"PRICING OF PRELIMINARIES"]
[null,"Should the contractor select Option A in terms of subclause"]
[null,"32.1 in the Contract Data - Contractor to Employer (CE) for the"]
[null,"purpose of adjustment of these preliminaries, the amount"]
[null,"entered into the amount column in these preliminaries is to be"]
[null,"divided into one or more of the three categories provided"]
[null,"namely Fixed (F), Value Related (V) and Time Related (T)"]
[]
[null,"SECTION A - PRINCIPAL BUILDING"]
[]
[null,"AGREEMENT"]
[]
[null,"Definitions"]
[]
[1,"Clause 1.0 - Definitions and interpretation","Item",1]
[]
[null,"Objective and preparations"]
[]
[2,"Clause 2.0 - Offer acceptance and performance obligations","Item",1]
[3,"Clause 3.0 - Documents","Item",1]
[4,"Clause 4.0 - Design responsibility","Item",1]
[5,"Clause 5.0 - Employer's agents","Item",1]
[6,"Clause 6.0 - Contractor's site representative","Item",1]
[7,"Clause 7.0 - Compliance with laws and regulations","Item",1]
[8,"Clause 8.0 - Works risk","Item",1]
[9,"Clause 9.0 - Indemnities","Item",1]
[10,"Clause 10.0 - General insurances","Item",1]
[11,"Clause 11.0 - Special insurances","Item",1]
[12,"Clause 12.0 - Effecting insurances","Item",1]
[13,"Clause 13.0 - Assignment","Item",1]
[14,"Clause 14.0 - Security","Item",1]
[]
[null,"Execution"]
[]
[15,"Clause 15.0 -Preparation for and execution of the works","Item",1]
[16,"Clause 16.0 - Site and access","Item",1]
[17,"Clause 16.7 - Known services","Item",1]
[18,"Clause 16.8 - Protection of trees","Item",1]
[19,"Clause 17.0 - Contract instructions","Item",1]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[20,"Clause 18.0 - Setting out of the works","Item",1]
[]
[null,"The contractor shall notify the principal agent if any"]
[null,"encroachments of adjoining foundations, buildings, structures,"]
[null,"pavements, boundaries, etc exist in order that the necessary"]
[null,"arrangements may be made for the rectification of any such"]
[null,"encroachments"]
[]
[21,"Clause 19.0 - Temporary works and plant","Item",1]
[]
[22,"Subclause 19.1.1 - Enclosure of the works","Item",1]
[]
[23,"Subclause 19.1.2 - Office accommodation","Item",1]
[]
[24,"Clause 19.2 - Notice boards","Item",1]
[]
[25,"Clause 20.0 - Nominated subcontractors","Item",1]
[]
[26,"Clause 21.0 - Selected subcontractors","Item",1]
[]
[27,"Clause 22.0 - Employer's direct contractors","Item",1]
[]
[28,"Clause 23.0 - Contractor's domestic subcontractors","Item",1]
[]
[null,"Completion"]
[]
[29,"Clause 24.0 - Practical completion","Item",1]
[30,"Clause 25.0 - Works completion","Item",1]
[31,"Clause 26.0 - Final completion","Item",1]
[32,"Clause 27.0 - Latent defects liability period","Item",1]
[33,"Clause 28.0 - Sectional completion","Item",1]
[]
[34,"Clause 29.0 - Revision of date for practical completion","Item",1]
[null,"The removal and replacement of materials and/or workmanship"]
[null,"which do not conform to specification or drawing shall not"]
[null,"constitute grounds for the extension of the construction period"]
[null,"nor for the adjustment of the contract value (Clause 29.3)"]
[]
[35,"Clause 30.0 - Penalty for late or non-completion","Item",1]
[]
[null,"Payment"]
[]
[36,"Clause 31.0 - Interim payment","Item",1]
[null,"Materials and goods stored off site shall not be included in the"]
[null,"amount authorised for payment unless Advanced Payment"]
[null," Guarantee provided"]
[37,"Clause 32.0 - Adjustment to the contract value","Item",1]
[38,"Clause 33.0 - Recovery of expense and loss","Item",1]
[39,"Clause 34.0 - Final account and final payment","Item",1]
[40,"Clause 35.0 - Payment to other parties","Item",1]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"Termination"]
[]
[41,"Clause 37.0 - Termination by employer - loss and damage","Item",1]
[]
[42,"Clause 38.0 - Termination by contractor - employer's default","Item",1]
[]
[43,"Clause 39.0 - Termination - cessation of the works","Item",1]
[44,"Clause 40.0 - Settlement of disputes","Item",1]
[45,"Clause 41.0 - Post tender provisions","Item",1]
[]
[null,"The required post tender information shall be inserted in the"]
[null,"post tender provisions after consultation with the contractor"]
[]
[46,"Clause 42 0 - Contractual agreement","Item",1]
[]
[null,"The required information of the contracting parties and the"]
[null,"amount of the accepted contract sum shall be inserted in the"]
[null,"contractual agreement for signature of the agreement by the"]
[null,"contracting parties"]
[]
[null,"SECTION B - PRELIMINARIES"]
[]
[null,"Definitions and interpretation"]
[]
[47,"Clause 1.0 - Definitions and interpretation","Item",1]
[48,"Clause 36.0 - Termination by employer - contractor's default","Item",1]
[]
[null,"Documents"]
[]
[49,"Clause 2.1 - Checking of documents","Item",1]
[50,"Clause 2.2 - Provisional bills of quantities","Item",1]
[]
[null,"Previous work and adjoining properties"]
[]
[51,"Clause 3.1 - Previous work - dimensional accuracy","Item",1]
[52,"Clause 2.3 - Availability of construction documentation","Item",1]
[]
[null,"The budgetary allowances and selected subcontract amounts"]
[null," allocated for subsequent trades included in this document will"]
[null," be separately procured, based on selected subcontractors"]
[null," during the construction period"]
[]
[53,"Clause 3.2 - Previous work - defects","Item",1]
[54,"Clause 3.3 - Inspection of adjoining properties","Item",1]
[]
[null,"Samples, shop drawings and manufacturer's instructions"]
[]
[55,"Clause 4.1 - Samples of materials","Item",1]
[56,"Clause 4.2 - Workmanship samples","Item",1]
[57,"Clause 4.3 - Shop drawings","Item",1]
[58,"Clause 4.4 - Compliance with manufacturer's instructions","Item",1]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"Deposits and fees"]
[]
[59,"Clause 5.1 - Deposits and fees","Item",1]
[]
[null,"Temporary services"]
[]
[60,"Clause 6.1 - Water","Item",1]
[]
[61,"Clause 6.2 - Electricity","Item",1]
[]
[62,"Clause 6.3 - Telecommunication facilities","Item",1]
[]
[63,"Clause 6.4 - Ablution facilities","Item",1]
[]
[null,"Prime cost amounts"]
[]
[64,"Clause 7.1 - Responsibility for prime cost amounts","Item",1]
[]
[null,"Special attendance on nls subcontractors"]
[]
[65,"Clause 8.1 - Special attendance","Item",1]
[]
[null,"General"]
[]
[66,"Clause 9.1 - Protection of the works","Item",1]
[67,"Clause 9.2 -Protection/isolation of existing/sectionally occupied","Item",1]
[null,"works"]
[68,"Clause 9.3 - Security of the works","Item",1]
[69,"Clause 9.4 - Notice before covering work","Item",1]
[70,"Clause 9.5 - Disturbance","Item",1]
[71,"Clause 9.6 - Environmental disturbance","Item",1]
[72,"Clause 9.7 - Works cleaning and clearing (please price","Item",1]
[null," according to assessment of the site at the site inspection)"]
[73,"Clause 9.8 - Vermin","Item",1]
[74,"Clause 9.9 - Overhand work","Item",1]
[]
[null,"Schedule of variables"]
[]
[null,"Information necessary for elections and completion of those"]
[null,"clauses contained in the schedule which are necessary for"]
[null,"tender purposes is given hereunder Where no information is"]
[null,"given it shall mean that no specific requirements are expected"]
[null," or that the clause is not relevant to this specific contract"]
[]
[null,"10.1 - Provisional bills of quantities [clause 2.2]"]
[null,"The quantities are provisional   Yes"]
[]
[null,"10.2 - Availability of construction documentation [clause 2 3]"]
[null,"Construction documentation is complete  No"]
[]
[null,"10.3 - Previous work - dimensional accuracy [clause 3.1]"]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"10.4 - Previous work - defects [clause 32]"]
[null,"10.5 - Inspection of adjoining properties [clause 33]"]
[null,"10.6 - Water [clause 7.2]"]
[]
[null,"Option A (by contractor)  yes"]
[null,"Option B (by employer - free of charge) no"]
[null,"Option C (by employer - metered) no"]
[]
[null,"10.7 - Electricity [clause 7.3]"]
[]
[null,"Option A (by contractor) yes"]
[null,"Option B (by employer - free of charge) no"]
[null,"Option C (by employer - metered) no"]
[]
[null,"10.8 - Telecommunications [clause 7.4]"]
[null,"Telephone  yes"]
[null,"Facsimile no"]
[null,"E-mail no"]
[]
[null,"10.9 - Ablution facilities [clause 7 5]"]
[null,"Option A (by contractor)  yes"]
[null,"Option B (by employer) no"]
[null,"10.10 - Protection of the works [clause 9 1]"]
[null,"10.11 - Protection/isolation of existing/sectionally occupied"]
[null,"works [clause 9 2]"]
[null,"Protection/isolation is required No"]
[null,"10.12 - Disturbance [clause 9 5]"]
[null,"10.13 - Environmental disturbance [clause 9.6]"]
[]
[null,"SECTION C - SPECIFIC PRELIMINARIES"]
[]
[75,"Site instructions","Item",1]
[]
[null,"Instructions issued on site are to be recorded in triplicate in a"]
[null,"site instruction book which is to be maintained on site by the"]
[null,"contractor"]
[]
[76,"Warranties for material and workmanship","Item",1]
[null,"Where warranties for materials and/or workmanship are called"]
[null,"for, the contractor shall obtain a written warranty, addressed to"]
[null,"the employer, from the firm supplying the materials and/or"]
[null,"doing the work and shall deliver same to the principal agent on"]
[null,"the certified completion of the contract. The warranty shall state"]
[null,"that workmanship, materials and installation are warranteed for"]
[null,"a specified period from the date of final completion and that any"]
[null,"defects that may arise during the specified period shall be"]
[null,"made good at the expense of the firm supplying the materials"]
[null,"and/or doing the work, upon written notice to do so The"]
[null,"warranty will not be enforced if the work is damaged by defects"]
[null,"in the construction of the building in which case the"]
[null,"responsibility for replacement shall rest entirely with the"]
[null,"contractor"]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[77,"Co-operation of contractor for cost management","Item",1]
[]
[null,"It is specifically agreed that the contractor accepts the"]
[null,"obligation of assisting the principai agent in implementing"]
[null,"proper cost management The contractor will be advised by the"]
[null,"principai agent of all cost management procedures which will"]
[null,"be implemented to ensure that the final building cost does not"]
[null,"exceed the budget The principal agent undertakes to make"]
[null,"available to the contractor all budgetary allowances and cost"]
[null,"assessments/reports to enable the proper procedure to be"]
[null,"implemented and the contractor shall attend all cost plan review"]
[null,"and cost management meetings The contractor undertakes to"]
[null,"extend these procedures, as necessary, to all subcontractors"]
[]
[78,"Propping of floors below","Item",1]
[]
[null,"The contractor is advised that propping of floors below may be"]
[null,"required if he wishes to use any areas of completed suspended"]
[null,"reinforced concrete slabs for vehicle access, storage of"]
[null,"materials and goods and location of plant, scaffolding, etc The"]
[null,"location of these areas and any necessary propping shall be"]
[null,"approved by the principal agent and the cost thereof shall be"]
[null,"borne by the contractor"]
[]
[79,"Testing of windows for watertightness","Item",1]
[]
[null,"Each window shall be tested for watertightness with water"]
[null,"sprayed on using adequate pressure. If in the opinion of the"]
[null,"principal agent, the pressure proves to be inadequate, then the"]
[null,"pressure shall be boosted by means of compressed air or other"]
[null,"approved means"]
[]
[80,"Completion of Works","Item",1]
[]
[null,"This is a completion project. The contractor will be liable to"]
[null," notify the Principal Agent of any defects or damage noticed on"]
[null," the existing works which will negatively affect the structural"]
[null," intergrity of the new works or works as a whole. Once the"]
[null," contractor has commenced with the works, the responsibility of"]
[null," the complete structure lies with the contractor. "]
[]
[null,"SUMMARY OF CATEGORIES"]
[]
[81,"Category: Fixed","Item",1]
[82,"Category: Value","Item",1]
[83,"Category: Time","Item",1]
[]
[null,"ALTERATIONS "]
[]
[null,"Tenderers are to refer to the Model Preambles for Trades"]
[null," (Latest Edition) and Supplementary Preambles for further"]
[null," description and amplification of work in this section"]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"PREAMBLES "]
[]
[null,"Tenderers are referred to the relevant clauses in the Model"]
[null," Preambles for Trades (Latest Edition) as published by the"]
[null," Association of South African Quantity Surveyors and to the"]
[null," Supplementary Preambles which are incorporated in these Bills"]
[null," of Quantities."]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Descriptions and Preambles "]
[null,"The full descriptions of the items and all preambles in the"]
[null," previous and following trades, shall, unless otherwise stated,"]
[null," also be applicable to the relevant items in this trade. "]
[]
[null,"View site "]
[null,"Before submitting this tender, the contractor shall visit the site"]
[null," and satisfy himself as to the nature and extent of the work to be"]
[null," done and the value of the materials contained in the buildings"]
[null," or portions of the buildings to be demolished.  No claim for any"]
[null," variations of the contract sum in respect of the nature and"]
[null," extent of the work or of inferior or damaged materials will be"]
[null," entertained."]
[]
[null,"Explosives "]
[null,"No explosives whatsoever may be used for demolition"]
[null," purposes unless otherwise stated."]
[]
[null,"General "]
[null,"The contractor shall carry out the whole of the works with as"]
[null,"little mess and noise as possible and with a minimum of"]
[null,"disturbance to adjoining premises and their tenants. He"]
[null,"shall provide proper protection and provide, erect and"]
[null,"remove when directed, any temporary tarpaulins that may"]
[null,"be necessary during the progress of the works, all to the"]
[null,"satisfaction of the principal agent"]
[]
[null,"Water supply pipes and other piping that may be encountered"]
[null," and found necessary to disconnect or cut, shall be effectively"]
[null," stopped off or grubbed up and removed, and any new"]
[null," connections that may be necessary shall be made with proper"]
[null," fittings, to the satisfaction of the principal agent."]
[]
[null,"Doors, fanlights, fittings, frames, linings, etc which are to be"]
[null," re-used shall be thoroughly overhauled before refixing including"]
[null," taking off, easing and rehanging, cramping up, re-wedging as"]
[null," required and making good cramps, dowels, etc, and easing,"]
[null," oiling, adjusting and repairing ironmongery as necessary,"]
[null," replacing any glass damaged in removal or subsequently and"]
[null," stopping up all nail and screw holes with tinted plastic wood to"]
[null," match timber, unless otherwise described. Re-painting or"]
[null," re-varnishing is given separately."]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"Prices for taking out of windows, doors and frames, etc shall"]
[null," include for removal of all beads, architraves, ironmongery,"]
[null," doorstops, cabin hooks, etc and making good floor and wall"]
[null," finishes to match existing."]
[]
[null,"With regard to building up of openings in existing walls, cement"]
[null," screeds and pavings, granolithic, tops of walls, etc, shall be"]
[null," levelled and prepared for raising of brickwork."]
[]
[null,"Making good of finishes shall include making good of the brick"]
[null," and concrete surfaces onto which the new finishes are applied"]
[null," where necessary."]
[]
[null,"The contractor will be required to take all dimensions affecting"]
[null," the existing buildings on the site and he will be held solely"]
[null," responsible for the accuracy of all such dimensions where used"]
[null," in the manufacture of new items (doors, windows, fittings, etc)"]
[]
[null,"The contractor must note that the demolition of all existing"]
[null," electrical and mechanical work has been measured and"]
[null," addressed under the electrical and mechanical tender"]
[null," documents."]
[]
[null,"Any damage to existing electrical work will be for the"]
[null," contractors account."]
[]
[null,"Removal of asbestos materials shall be executed in compliance"]
[null," with the regulations set out in the Occupational Health and"]
[null," Saftey Act"]
[]
[null,"Old materials to be carted away "]
[null,"Old materials from the alterations, except where described to"]
[null," be re-used or handed over, as well as all rubbish, etc., must be"]
[null," regularly carted from the site and not be allowed to accumulate"]
[null," on or around the site."]
[]
[null,"Old materials not to be re-used "]
[null,"None of the old materials are to be used for new work except"]
[null," where specifically described to be set aside for re-use."]
[]
[null,"Where certain materials or articles from demolitions or articles"]
[null," are described as to be handed over by the Contractor to the"]
[null," Client, such materials or articles shall be properly stored by the"]
[null," contractor, until handing over thereof. The contractor must"]
[null," obtain an official receipt listing the materials or articles and"]
[null," dates of handing over. "]
[]
[null,"If the contractor fails to submit the receipt when requested, it"]
[null," shall be deemed that the materials or articles are still in his"]
[null," possession and he will be held liable to the Client for the full"]
[null," replacement value thereof, which amount will be deducted from"]
[null," any monies due to the contractor. "]
[null,"Carried Forward"]
[null,"Brought Forward"]
[]
[null,"Handing over of materials "]
[]
[null,"Abbreviations "]
[null,"For the purpose of this bill certain abbreviations have been "]
[null,"made use of, the full meanings of which are as follows: "]
[]
[null,"Breaking down and removing walls, etc implies that the"]
[null,"wall is to be taken down to the extent shown on the drawings or"]
[null," as may be described and that all necessary shoring is to be"]
[null," provided and allowed for to ensure the safety of the building"]
[null," during the pulling down or until new walls are erected and all"]
[null," portions of the remaining walls where disturbed or affected by"]
[null," the removal are to be made good and left ready for the plaster"]
[null," or other finishings"]
[]
[null,"Taking out and removing doors, windows, etc implies that"]
[null," the door, etc is to be carefully taken down together with the"]
[null," frame, linings, architraves, window sills, etc complete and"]
[null,"where brick lintels occur, it must be supported and propped"]
[null,"until the openings are built up or new doors or windows built in"]
[null," position"]
[]
[null,"Making good implies that all necessary repairs are to be"]
[null,"made to reinstate articles that may be damaged through the"]
[null,"removal or otherwise, and the supplying of any new materials to"]
[null," match existing work, and is to include any necessary repairs to"]
[null," adjacent finishings such as floors, skirtings, plaster, painting,"]
[null," etc and such making good is to match adjoining work in all"]
[null," respects and in all trades"]
[]
[null,"GENERAL "]
[]
[null,"Protection from damage "]
[1,"All floors, doors, windows, fittings, ceilings, roofs, etc not to be","Item",1]
[null," removed and become the property of the Contractor shall be"]
[null," adequately protected from damage during the progress of the"]
[null," works and any damage resulting from the repairs, renovations,"]
[null," alterations or demolitions shall be made good by the Contractor"]
[null," at his own expense"]
[]
[null,"Temporary barriers, screens, etc including removal "]
[2,"Security and safety warning tapes and signage to enclose the","Item",1]
[null," Works where necessary"]
[]
[3,"Any temporary tarpaulins, dust and weatherproof screens and","Item",1]
[null," barriers that may be necessary for protection of the Works"]
[]
[null,"Watering the Works "]
[4,"Wherever and whenever necessary, or when directed by the","Item",1]
[null," Representative/Agent, the Works shall be well watered with a"]
[null," jet or spray from a hose sufficient to prevent any nuisance from"]
[null," dust"]
[null,"Carried to Summary"]
[]
[1,"DEMOLITION"]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[1.1,"Existing hoarding with poles","m",32,{"v":80,"d":"R 80.00"},{"$f":"E533*D533","v":{"v":2560,"d":"R 2,560.00"}}]
[]
[1.2,"Existing shadecloth hoarding 1,8m high on Bonnox","m",32,{"v":150,"d":"R 150.00"},{"$f":"E535*D535","v":{"v":4800,"d":"R 4,800.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[1.3,"Double gate size 6000 x 1800mm high formed of suitable","No",1,{"v":1600,"d":"R 1,600.00"},{"$f":"E539*D539","v":{"v":1600,"d":"R 1,600.00"}}]
[null,"tubular steel frame filled in with Bonnox fencing and covered"]
[null,"with shadecloth including all necessary gate posts, locking"]
[null,"mechanism, etc"]
[]
[1.4,"One brick walls in parapet","m²",20,{"v":380,"d":"R 380.00"},{"$f":"E544*D544","v":{"v":7600,"d":"R 7,600.00"}}]
[]
[1.5,"One brick walls in beam filling","m²",62,{"v":380,"d":"R 380.00"},{"$f":"E546*D546","v":{"v":23560,"d":"R 23,560.00"}}]
[]
[1.6,"229 x 152mm Terra-cotta vermin proof air brick including making good surface to 25mm screed and prepare surface to receive new","No",64,{"v":100,"d":"R 100.00"},{"$f":"E548*D548","v":{"v":6400,"d":"R 6,400.00"}},{"$f":"D548+24","v":88}]
[]
[1.7,"25mm screeds (varendas, external steps, etc) and prepare surface to receive new","m²",268,{"v":120,"d":"R 120.00"},{"$f":"E550*D550","v":{"v":32160,"d":"R 32,160.00"}},{"$f":"D550+67","v":335}]
[]
[1.8,"25mm screeds and prepare surface to receive new tiles","m²",{"$f":"4.5*6*3","v":81},{"v":120,"d":"R 120.00"},{"$f":"E552*D552","v":{"v":9720,"d":"R 9,720.00"}}]
[]
[1.9,"5000litres concrete water tanks including grubbing up bases, etc","No",2,{"v":3000,"d":"R 3,000.00"},{"$f":"E554*D554","v":{"v":6000,"d":"R 6,000.00"}}]
[]
[1.1,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"v":1024,"d":"1,024"},{"v":85,"d":"R 85.00"},{"$f":"E556*D556","v":{"v":87040,"d":"R 87,040.00"}},{"$f":"D556+68","v":{"v":1092,"d":"1,092"}}]
[null,"goods and dispose off as per the SHE  regulations."]
[]
[1.11,"Ceiling board","m2",626,{"v":50,"d":"R 50.00"},{"$f":"E559*D559","v":{"v":31300,"d":"R 31,300.00"}},{"$f":"D559+81","v":707}]
[]
[1.12,"Timber door 813 x 2032mm high","No",21,{"v":50,"d":"R 50.00"},{"$f":"E561*D561","v":{"v":1050,"d":"R 1,050.00"}}]
[]
[1.13,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",16,{"v":50,"d":"R 50.00"},{"$f":"E563*D563","v":{"v":800,"d":"R 800.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[1.14,"Greenboard 2400 x 1140mm high","No",9,{"v":50,"d":"R 50.00"},{"$f":"E566*D566","v":{"v":450,"d":"R 450.00"}}]
[]
[1.15,"Roof trusses including purlins","No",60,{"v":50,"d":"R 50.00"},{"$f":"E568*D568","v":{"v":3000,"d":"R 3,000.00"}},{"$nulls":3},{"$f":"30/1.2","v":25}]
[]
[1.16,"Fascia boards","m",333,{"v":10,"d":"R 10.00"},{"$f":"E570*D570","v":{"v":3330,"d":"R 3,330.00"}},{"$f":"D570+36","v":369}]
[]
[1.17,"Roof gutters","m",319,{"v":10,"d":"R 10.00"},{"$f":"E572*D572","v":{"v":3190,"d":"R 3,190.00"}},{"$f":"D572+36","v":355}]
[]
[1.18,"Downpipes","m",151,{"v":10,"d":"R 10.00"},{"$f":"E574*D574","v":{"v":1510,"d":"R 1,510.00"}},{"$f":"D574+25","v":176}]
[]
[1.19,"Mortice lock and striking plate from timber door and steel frame","No",19,{"v":50,"d":"R 50.00"},{"$f":"E576*D576","v":{"v":950,"d":"R 950.00"}}]
[]
[1.2,"Stays, latches, handles, etc from window steel frame","No",63,{"v":50,"d":"R 50.00"},{"$f":"E578*D578","v":{"v":3150,"d":"R 3,150.00"}},{"$f":"D578+25","v":88}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[1.21,"Chipping of screed in floors to recieve new screed. ","m²",{"v":1013,"d":"1,013"},{"v":25,"d":"R 25.00"},{"$f":"E582*D582","v":{"v":25325,"d":"R 25,325.00"}},{"$f":"D582+20","v":{"v":1033,"d":"1,033"}}]
[]
[1.22,"Cleaning walls to recieve paint.","m²",{"v":3588,"d":"3,588"},{"v":10,"d":"R 10.00"},{"$f":"E584*D584","v":{"v":35880,"d":"R 35,880.00"}},{"$f":"D584+614","v":{"v":4202,"d":"4,202"}}]
[]
[1.23,"Cleaning and removing broken glazing, putty and paint to window frames","m²",66,{"v":20,"d":"R 20.00"},{"$f":"E586*D586","v":{"v":1320,"d":"R 1,320.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F533:F587)","v":{"v":292695,"d":"R 292,695.00"}}]
[]
[2,"EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[2.1,"Open face excavation to expose foundations for inspection and underpinning","m3",{"$f":"32*1.8*0.9*2*2+(0.6)","v":207.96},{"v":50,"d":"R 50.00"},{"$f":"E595*D595","v":{"v":10398,"d":"R 10,398.00"}},{"$f":"D595+31","v":238.96}]
[]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in"]
[2.2,"Soft rock","m3",8,{"v":150,"d":"R 150.00"},{"v":1200,"d":"R 1,200.00"}]
[]
[2.3,"Hard rock","m3",3,{"v":250,"d":"R 250.00"},{"v":750,"d":"R 750.00"}]
[]
[null,"Extra over all excavations for carting away"]
[2.4,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",208,{"v":50,"d":"R 50.00"},{"v":10400,"d":"R 10,400.00"}]
[]
[null,"Risk of collapse of excavations"]
[2.5,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",100,{"v":45,"d":"R 45.00"},{"$f":"E608*D608","v":{"v":4500,"d":"R 4,500.00"}}]
[]
[2.6,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":600,"d":"R 600.00"},{"v":600,"d":"R 600.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[2.7,"Under floors, steps, pavings, etc","m3",208,{"v":350,"d":"R 350.00"},{"v":72800,"d":"R 72,800.00"}]
[]
[2.8,"Backfilling to trenches, holes, etc","m3",8,{"v":350,"d":"R 350.00"},{"v":2800,"d":"R 2,800.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[2.9,"Under floors etc","m3",72,{"v":350,"d":"R 350.00"},{"v":25200,"d":"R 25,200.00"}]
[]
[null,"Compaction of surfaces"]
[2.1,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",{"$f":"(32*2*2)+(7.3*2)+0.4","v":143},{"v":45,"d":"R 45.00"},{"v":6435,"d":"R 6,435.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming"]
[]
[2.11,"To bottoms and sides of trenches etc","m2",143,{"v":20,"d":"R 20.00"},{"v":2860,"d":"R 2,860.00"}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F592:F640)","v":{"v":137943,"d":"R 137,943.00"}}]
[]
[3,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[3.1,"Verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",20,{"v":1800,"d":"R 1,800.00"},{"v":36000,"d":"R 36,000.00"}]
[]
[3.2,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",10,{"v":1800,"d":"R 1,800.00"},{"v":18000,"d":"R 18,000.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[3.3,"25 Mpa: Strip footings","m3",4,{"v":1800,"d":"R 1,800.00"},{"v":7200,"d":"R 7,200.00"}]
[]
[3.4,"25 Mpa: Pile Caps","m3",70,{"v":1800,"d":"R 1,800.00"},{"$f":"E660*D660","v":{"v":126000,"d":"R 126,000.00"}}]
[]
[null,"TEST BLOCKS"]
[3.5,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",8,{"v":150,"d":"R 150.00"},{"v":1200,"d":"R 1,200.00"}]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[3.6,"Surface beds, slabs, etc","m2",128,{"v":45,"d":"R 45.00"},{"$f":"E671*D671","v":{"v":5760,"d":"R 5,760.00"}}]
[]
[null,"Rough formwork to sides"]
[]
[3.7,"To sides n.e. 300mm","m2",128,{"v":65,"d":"R 65.00"},{"v":8320,"d":"R 8,320.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[3.8,"15mm Joints not exceeding 300mm high or wide","m",24,{"v":15,"d":"R 15.00"},{"v":360,"d":"R 360.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[3.9,"10mm Isolation Joints not exceeding 300mm high or wide","m",24,{"v":15,"d":"R 15.00"},{"v":360,"d":"R 360.00"}]
[]
[null,"Saw cut joints"]
[3.1,"50 x 3mm Saw cut joints in top of concrete","m",24,{"v":15,"d":"R 15.00"},{"v":360,"d":"R 360.00"}]
[]
[null,"Fabric reinforcement"]
[]
[3.11,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",128,{"v":145,"d":"R 145.00"},{"v":18560,"d":"R 18,560.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F647:F695)","v":{"v":222120,"d":"R 222,120.00"}}]
[]
[4,"MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[4.1,"Half brick walls in beamfilling","m2",124,{"v":380,"d":"R 380.00"},{"$f":"E705*D705","v":{"v":47120,"d":"R 47,120.00"}},{"$f":"D705+31","v":155}]
[]
[4.2,"One brick walls","m2",104,{"v":480,"d":"R 480.00"},{"$f":"E707*D707","v":{"v":49920,"d":"R 49,920.00"}},{"$f":"D707+26","v":130}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[4.3,"75mm Wide Brickwork reinforcement built in horizontally","m",768,{"v":45,"d":"R 45.00"},{"$f":"E713*D713","v":{"v":34560,"d":"R 34,560.00"}},{"$f":"D713+192","v":960}]
[]
[4.4,"150mm Wide reinforcement built in horizontally","m",176,{"v":45,"d":"R 45.00"},{"$f":"E715*D715","v":{"v":7920,"d":"R 7,920.00"}},{"$f":"D715+44","v":220}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[4.5,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",32,{"v":150,"d":"R 150.00"},{"$f":"E719*D719","v":{"v":4800,"d":"R 4,800.00"}}]
[]
[null,"Air bricks etc"]
[4.6,"229 x 152mm Terra-cotta vermin proof air brick (pair)","No",64,{"v":150,"d":"R 150.00"},{"$f":"E722*D722","v":{"v":9600,"d":"R 9,600.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F705:F723)","v":{"v":153920,"d":"R 153,920.00"}}]
[]
[5,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[5.1,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",1169,{"v":280,"d":"R 280.00"},{"$f":"E738*D738","v":{"v":327320,"d":"R 327,320.00"}},{"$f":"D738+23","v":1192}]
[]
[5.2,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",142,{"v":65,"d":"R 65.00"},{"$f":"E741*D741","v":{"v":9230,"d":"R 9,230.00"}},{"$f":"D741+9","v":151}]
[]
[5.3,"Narrow and broad flute closers","m",142,{"v":65,"d":"R 65.00"},{"$f":"E743*D743","v":{"v":9230,"d":"R 9,230.00"}}]
[]
[5.4,"Moulded narrow and broad rib polyethylene filler blocks","m",142,{"v":65,"d":"R 65.00"},{"$f":"E745*D745","v":{"v":9230,"d":"R 9,230.00"}}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[5.5,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",1166,{"v":25,"d":"R 25.00"},{"$f":"E754*D754","v":{"v":29150,"d":"R 29,150.00"}},{"$f":"D754+270","v":1436}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F729:F755)","v":{"v":384160,"d":"R 384,160.00"}}]
[]
[6,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[6.1,"38 x 114mm Wall plates","m",256,{"v":65,"d":"R 65.00"},{"$f":"E761*D761","v":{"v":16640,"d":"R 16,640.00"}},{"$f":"D761+64","v":320}]
[]
[6.2,"50 x 76mm Purlins not exceeding 6.6 m in length, to"]
[null,"manufacturer's specification","m",1280,{"v":85,"d":"R 85.00"},{"$f":"E764*D764","v":{"v":108800,"d":"R 108,800.00"}},{"$f":"D764+320","v":1600}]
[]
[null,"Sundries"]
[6.3,"Two coats ABE Provinite on wrought timbers","m2",308,{"v":150,"d":"R 150.00"},{"$f":"E767*D767","v":{"v":46200,"d":"R 46,200.00"}},{"$f":"D767+77","v":385}]
[]
[6.4,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",320,{"v":25,"d":"R 25.00"},{"$f":"E771*D771","v":{"v":8000,"d":"R 8,000.00"}},{"$f":"D771+80","v":400}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[6.5,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 7300mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",36,{"v":2500,"d":"R 2,500.00"},{"$f":"E778*D778","v":{"v":90000,"d":"R 90,000.00"}}]
[null,"related items"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[6.6,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",319,{"v":110,"d":"R 110.00"},{"$f":"E787*D787","v":{"v":35090,"d":"R 35,090.00"}},{"$f":"D787+36","v":355}]
[null,"drive screws and washers"]
[]
[6.7,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",114,{"v":100,"d":"R 100.00"},{"$f":"E793*D793","v":{"v":11400,"d":"R 11,400.00"}},{"$f":"D793+18","v":132}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[6.8,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",772,{"v":45,"d":"R 45.00"},{"$f":"E797*D797","v":{"v":34740,"d":"R 34,740.00"}},{"$f":"D797+131","v":903}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[6.9,"44mm Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",21,{"v":2000,"d":"R 2,000.00"},{"$f":"E803*D803","v":{"v":42000,"d":"R 42,000.00"}}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[6.1,"Flortime Premier pinning boards size 7000 x 1400mm high","No",14,{"v":4500,"d":"R 4,500.00"},{"$f":"E808*D808","v":{"v":63000,"d":"R 63,000.00"}}]
[]
[null,"WHITE BOARDS, GREEN BOARDS, etc"]
[null,"'Vitrex' Green board Wall mounted All steel fabricated board with rear "]
[null,"stiffeners and sound deadener surround fixed 3 no. times at the top and "]
[null,"bottom with aluminium brackets, sleeve and screw"]
[]
[6.11,"Standard Green chalk boards 3500 x 1140mm high with two side swinging leaves  in ","No",9,{"v":4500,"d":"R 4,500.00"},{"$f":"E815*D815","v":{"v":40500,"d":"R 40,500.00"}}]
[null,"an epoxy coated tubular steel frame with a hinged bracket (top) and a pivot pin"]
[null,"(bottom). and one permanent leaf, with aluminium chalk tray at the bottom"]
[]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F760:F819)","v":{"v":496370,"d":"R 496,370.00"}}]
[]
[7,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[7.1,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",1095,{"v":250,"d":"R 250.00"},{"$f":"E830*D830","v":{"v":273750,"d":"R 273,750.00"}},{"$f":"D830+81","v":1176}]
[]
[7.2,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",22,{"v":650,"d":"R 650.00"},{"$f":"E835*D835","v":{"v":14300,"d":"R 14,300.00"}}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[7.3,"75mm Coved cornices","m",689,{"v":65,"d":"R 65.00"},{"$f":"E839*D839","v":{"v":44785,"d":"R 44,785.00"}},{"$f":"D839+123","v":812}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F824:F840)","v":{"v":332835,"d":"R 332,835.00"}}]
[]
[8,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[8.1,"2mm vinyl tiles ","m2",936,{"v":250,"d":"R 250.00"},{"$f":"D848*E848","v":{"v":234000,"d":"234,000.00"}},{"$f":"D848+234","v":{"v":1170,"d":"1,170"}}]
[]
[8.2,"Two coats wax polish on vinyl flooring including sealing","m2",{"$f":"D848","v":936},{"v":15,"d":"R 15.00"},{"$f":"D850*E850","v":{"v":14040,"d":"14,040.00"}}]
[]
[null,"Floors tiles"]
[8.3,"Clean ceramic tiles with suitable chemicals and repair grout","m2",78,{"v":90,"d":"R 90.00"},{"$f":"D853*E853","v":{"v":7020,"d":"7,020.00"}}]
[]
[8.4,"Supply and install new 305 x 305mm non slip ceramic tiles","m2",81,{"v":280,"d":"R 280.00"},{"$f":"D855*E855","v":{"v":22680,"d":"22,680.00"}}]
[]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F845:F857)","v":{"v":277740,"d":"R 277,740.00"}}]
[]
[9,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[9.1,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",25,{"v":450,"d":"R 450.00"},{"$f":"E865*D865","v":{"v":11250,"d":"R 11,250.00"}}]
[]
[9.2,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":50000,"d":"50,000.00"},{"$f":"C867*E867","v":{"v":50000,"d":"50,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[9.3,"50mm High plastic letter or numeral","No",24,{"v":150,"d":"R 150.00"},{"$f":"E875*D875","v":{"v":3600,"d":"R 3,600.00"}}]
[]
[9.4,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",24,{"v":45,"d":"R 45.00"},{"$f":"E878*D878","v":{"v":1080,"d":"R 1,080.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F859:F879)","v":{"v":65930,"d":"R 65,930.00"}}]
[]
[10,"METALWORK"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[10.1,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",1,{"v":35000,"d":"R 35,000.00"},{"$f":"E891*D891","v":{"v":35000,"d":"R 35,000.00"}}]
[]
[10.2,"Double ended strongroom ventilator","No",1,{"v":1500,"d":"R 1,500.00"},{"v":1500,"d":"R 1,500.00"}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F891:F894)","v":{"v":36500,"d":"R 36,500.00"}},{"$f":"SUM(G890:G893)","v":{"v":0,"d":"R 0.00"}}]
[]
[11,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[11.1,"23mm Thick on floors and landings to receive floor tiles","m2",{"v":1251,"d":"1,251"},{"v":75,"d":"R 75.00"},{"$f":"E903*D903","v":{"v":93825,"d":"R 93,825.00"}},{"$f":"D903+81","v":{"v":1332,"d":"1,332"}}]
[]
[11.2,"25mm Thick on floors and landings to varendas and steps","m2",335,{"v":75,"d":"R 75.00"},{"$f":"E905*D905","v":{"v":25125,"d":"R 25,125.00"}},{"$f":"D905+67","v":402}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[11.3,"On walls in patches and repairing cracks","m2",569,{"v":75,"d":"R 75.00"},{"$f":"E911*D911","v":{"v":42675,"d":"R 42,675.00"}},{"$f":"D911+199","v":768}]
[]
[11.4,"On narrow widths","m2",21,{"v":75,"d":"R 75.00"},{"$f":"E913*D913","v":{"v":1575,"d":"R 1,575.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F903:F914)","v":{"v":163200,"d":"R 163,200.00"}}]
[]
[12,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[12.1,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",319,{"v":110,"d":"R 110.00"},{"$f":"E924*D924","v":{"v":35090,"d":"R 35,090.00"}},{"$f":"D924+36","v":355}]
[]
[12.2,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",118,{"v":100,"d":"R 100.00"},{"$f":"E927*D927","v":{"v":11800,"d":"R 11,800.00"}},{"$f":"D927+38","v":156}]
[]
[12.3,"Extra for angle","No",38,{"v":250,"d":"R 250.00"},{"$f":"E929*D929","v":{"v":9500,"d":"R 9,500.00"}}]
[]
[12.4,"Extra for stop end","No",38,{"v":250,"d":"R 250.00"},{"$f":"E931*D931","v":{"v":9500,"d":"R 9,500.00"}}]
[]
[12.5,"Extra for outlet for 100mm pipe","No",38,{"v":250,"d":"R 250.00"},{"$f":"E933*D933","v":{"v":9500,"d":"R 9,500.00"}}]
[]
[12.6,"Extra for eaves or plinth offset","No",38,{"v":250,"d":"R 250.00"},{"$f":"E935*D935","v":{"v":9500,"d":"R 9,500.00"}}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[12.7,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",5,{"v":10000,"d":"R 10,000.00"},{"$f":"E945*D945","v":{"v":50000,"d":"R 50,000.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F919:F946)","v":{"v":134890,"d":"R 134,890.00"}}]
[]
[13,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[13.1,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",70,{"v":400,"d":"R 400.00"},{"$f":"E953*D953","v":{"v":28000,"d":"R 28,000.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F950:F954)","v":{"v":28000,"d":"R 28,000.00"}}]
[]
[14,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[14.1,"Internal walls including gypsum coat where necessary","m2",{"v":2144,"d":"2,144"},{"v":70,"d":"R 70.00"},{"$f":"E963*D963","v":{"v":150080,"d":"R 150,080.00"}},{"$f":"D963+335","v":{"v":2479,"d":"2,479"}}]
[]
[14.2,"External walls including gypsum coat where necessary","m2",{"v":1129,"d":"1,129"},{"v":70,"d":"R 70.00"},{"$f":"E965*D965","v":{"v":79030,"d":"R 79,030.00"}},{"$f":"D965+56","v":{"v":1185,"d":"1,185"}}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[14.3,"Cornices, etc not exceeding 300mm girth","m",246,{"v":20,"d":"R 20.00"},{"$f":"E970*D970","v":{"v":4920,"d":"R 4,920.00"}},{"$f":"D970+123","v":369}]
[14.4,"Fascias and barge boards","m",515,{"v":20,"d":"R 20.00"},{"$f":"E971*D971","v":{"v":10300,"d":"R 10,300.00"}},{"$f":"D971+54","v":569}]
[14.5,"Internal ceilings","m2",{"v":1329,"d":"1,329"},{"v":70,"d":"R 70.00"},{"$f":"E972*D972","v":{"v":93030,"d":"R 93,030.00"}},{"$f":"D972+81","v":{"v":1410,"d":"1,410"}}]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[14.6,"Door frames","m2",119,{"v":70,"d":"R 70.00"},{"$f":"E977*D977","v":{"v":8330,"d":"R 8,330.00"}},{"$f":"D977+45","v":164}]
[14.7,"Windows","m2",494,{"v":70,"d":"R 70.00"},{"$f":"E978*D978","v":{"v":34580,"d":"R 34,580.00"}},{"$f":"D978+87","v":581}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[14.8,"Doors","m2",110,{"v":70,"d":"R 70.00"},{"$f":"E983*D983","v":{"v":7700,"d":"R 7,700.00"}},{"$f":"D983+14","v":124}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[14.9,"Skirtings, rails, etc not exceeding 300mm girth","m",828,{"v":20,"d":"R 20.00"},{"$f":"E988*D988","v":{"v":16560,"d":"R 16,560.00"}},{"$f":"D988+56","v":884}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F963:F989)","v":{"v":404530,"d":"R 404,530.00"}}]
[]
[15,"PROVISIONAL SUMS",{"$nulls":3},{"$f":"E992*D992","v":0}]
[]
[null,"Electrical Works"]
[15.1,"Provide the sum of R350,000.00 for the electrical selected sub -","PS",1,{"v":350000,"d":"350,000.00"},{"$f":"E995*D995","v":{"v":350000,"d":"350,000.00"}}]
[null,"contractor"]
[]
[15.2,"Allow for Profit & Attendance",null,0.1,{"v":350000,"d":"350,000.00"},{"$f":"E998*D998","v":{"v":35000,"d":"35,000.00"}}]
[]
[null,"Perimeter Fencing"]
[15.3,"Provide the sum of R245,000.00 for the repair of damaged fence ","PS",1,{"$f":"(88+62)*2*650+50000","v":{"v":245000,"d":"245,000.00"}},{"$f":"E1001*D1001","v":{"v":245000,"d":"245,000.00"}}]
[]
[15.4,"Allow for Profit & Attendance",null,0.1,{"$f":"E1001","v":{"v":245000,"d":"245,000.00"}},{"$f":"E1003*D1003","v":{"v":24500,"d":"24,500.00"}}]
[]
[null,"Woodborer Fumigation"]
[15.5,"Provide the sum of R100,000.00 for Diamond fence","PS",1,{"v":100000,"d":"100,000.00"},{"$f":"E1006*D1006","v":{"v":100000,"d":"100,000.00"}}]
[]
[15.6,"Allow for Profit & Attendance",null,0.1,{"$f":"E1006","v":{"v":100000,"d":"100,000.00"}},{"$f":"E1008*D1008","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"CLO"]
[15.7,"Provide the sum of R40,000.00 for CLO","PS",1,{"v":40000,"d":"40,000.00"},{"$f":"E1011*D1011","v":{"v":40000,"d":"40,000.00"}}]
[]
[15.8,"Allow for Profit & Attendance",null,0.1,{"$f":"E1011","v":{"v":40000,"d":"40,000.00"}},{"$f":"E1013*D1013","v":{"v":4000,"d":"4,000.00"}}]
[]
[null,"To Summary",{"$nulls":3},{"$f":"SUM(F995:F1014)","v":{"v":808500,"d":"808,500.00"}}]
[]
[null,"SUMMARY "]
["A","PRELIMINARIES",{"$nulls":3},{"v":473000,"d":"R 473,000.00"}]
[1,"DEMOLITION",{"$nulls":3},{"$f":"F588","v":{"v":292695,"d":"R 292,695.00"}}]
[{"$f":"A1019+1","v":2},"EARTHWORKS",{"$nulls":3},{"$f":"F641","v":{"v":137943,"d":"R 137,943.00"}}]
[{"$f":"A1020+1","v":3},"MASONRY",{"$nulls":3},{"$f":"F724","v":{"v":153920,"d":"R 153,920.00"}}]
[4,"CONCRETE",{"$nulls":3},{"$f":"F696","v":{"v":222120,"d":"R 222,120.00"}}]
[5,"ROOF COVERING",{"$nulls":3},{"$f":"F756","v":{"v":384160,"d":"R 384,160.00"}}]
[6,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F820","v":{"v":496370,"d":"R 496,370.00"}}]
[7,"CEILING",{"$nulls":3},{"$f":"F841","v":{"v":332835,"d":"R 332,835.00"}}]
[8,"FLOOR COVERING",{"$nulls":3},{"$f":"F858","v":{"v":277740,"d":"R 277,740.00"}}]
[9,"IRONMONGERY",{"$nulls":3},{"$f":"F880","v":{"v":65930,"d":"R 65,930.00"}}]
[10,{"$f":"B882","v":"METALWORK"},{"$nulls":3},{"$f":"F895","v":{"v":36500,"d":"R 36,500.00"}}]
[11,"PLASTERING",{"$nulls":3},{"$f":"F915","v":{"v":163200,"d":"R 163,200.00"}}]
[12,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F947","v":{"v":134890,"d":"R 134,890.00"}}]
[13,"GLAZING",{"$nulls":3},{"$f":"F955","v":{"v":28000,"d":"R 28,000.00"}}]
[14,"PAINT WORK",{"$nulls":3},{"$f":"F990","v":{"v":404530,"d":"R 404,530.00"}}]
[15,{"$f":"B992","v":"PROVISIONAL SUMS"},{"$nulls":3},{"$f":"F1015","v":{"v":808500,"d":"R 808,500.00"}}]
[null,"Sub Total",{"$nulls":3},{"$f":"SUM(F1018:F1033)","v":{"v":4412333,"d":"R 4,412,333.00"}},{"$f":"F1034*12%","v":{"v":529479.96,"d":"R 529,479.96"}}]
[]
[null,"CONTINGENCY @ 10%",{"$nulls":3},{"$f":"F1034*10%","v":{"v":441233.30000000005,"d":"441,233.30"}}]
[]
[null,"SUB TOTAL",{"$nulls":3},{"$f":"F1036+F1034","v":{"v":4853566.3,"d":"4,853,566.30"}}]
[]
[null,"ADD VAT @ 15%",{"$nulls":3},{"$f":"F1038*15%","v":{"v":728034.945,"d":"728,034.95"}}]
[]
[null,"GRAND TOTAL",{"$nulls":3},{"$f":"F1040+F1038","v":{"v":5581601.245,"d":"5,581,601.25"}}]
[]
[null,"CARRIED TO TENDER",null,null,{"$f":"F1042","v":{"v":5581601.245,"d":"5,581,601.25"}}]

{"sheet":"Combined","index":4,"n_rows":2868,"n_cols":11,"rows_kept":2868,"hidden":true,"merged":[[2867,5,2867,6]]}
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[]
[null,"BLOCK 1: 3 CLASSROOM"]
[null,"Demolition"]
[null,"Temporary barriers, screens, etc including removal "]
[]
[null,"Existing hoarding with poles","m",32,{"v":80,"d":"R 80.00"},{"$f":"E7*D7","v":{"v":2560,"d":"R 2,560.00"}}]
[]
[null,"Existing shadecloth hoarding 1,8m high on Bonnox","m",32,{"v":150,"d":"R 150.00"},{"$f":"E9*D9","v":{"v":4800,"d":"R 4,800.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[null,"Double gate size 6000 x 1800mm high formed of suitable","No",1,{"v":1600,"d":"R 1,600.00"},{"$f":"E13*D13","v":{"v":1600,"d":"R 1,600.00"}}]
[null," tubular steel frame filled in with Bonnox fencing and covered"]
[null," with shadecloth including all necessary gate posts, locking"]
[null," mechanism, etc"]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"One brick walls in parapet","m²",5,{"v":380,"d":"R 380.00"},{"$f":"E20*D20","v":{"v":1900,"d":"R 1,900.00"}}]
[]
[null,"One brick walls in beam filling","m²",{"$f":"(32*0.45*2)+(0.5*1.8*2)","v":30.6},{"v":380,"d":"R 380.00"},{"$f":"E22*D22","v":{"v":11628,"d":"R 11,628.00"}}]
[]
[null,"229 x 152mm Terra-cotta vermin proof air brick including making good surface to ","No",8,{"v":100,"d":"R 100.00"},{"$f":"E24*D24","v":{"v":800,"d":"R 800.00"}}]
[null,"receive new (new air brick elsewhere measured)"]
[]
[null,"Breaking down and removing concrete, etc "]
[]
[null,"25mm screeds (varendas, external steps, etc) and prepare surface to receive new","m²",67,{"v":120,"d":"R 120.00"},{"$f":"E29*D29","v":{"v":8040,"d":"R 8,040.00"}}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing off site"]
[]
[null,"5000litres concrete water tanks including grubbing up bases, etc","No",2,{"v":3000,"d":"R 3,000.00"},{"$f":"E35*D35","v":{"v":6000,"d":"R 6,000.00"}}]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},{"$f":"E39*D39","v":{"v":11680,"d":"R 11,680.00"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",4,{"v":50,"d":"R 50.00"},{"$f":"E45*D45","v":{"v":200,"d":"R 200.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",3,{"v":50,"d":"R 50.00"},{"$f":"E49*D49","v":{"v":150,"d":"R 150.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Greenboard 2400 x 1140mm high","No",3,{"v":50,"d":"R 50.00"},{"$f":"E52*D52","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Roof trusses including purlins","No",30,{"v":50,"d":"R 50.00"},{"$f":"E54*D54","v":{"v":1500,"d":"R 1,500.00"}},{"$nulls":4},{"$f":"30/1.2","v":25}]
[]
[null,"Fascia boards","m",{"$f":"32*2","v":64},{"v":10,"d":"R 10.00"},{"$f":"E56*D56","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Roof gutters","m",64,{"v":10,"d":"R 10.00"},{"$f":"E58*D58","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Downpipes","m",25,{"v":10,"d":"R 10.00"},{"$f":"E60*D60","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},{"$f":"E64*D64","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",3,{"v":50,"d":"R 50.00"},{"$f":"E66*D66","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},{"$f":"E70*D70","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)+((32+7.3)*2)*3.1","v":{"v":614.3399999999999,"d":"614"}},{"v":20,"d":"R 20.00"},{"$f":"E72*D72","v":{"v":12286.8,"d":"R 12,286.80"}}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D502","v":22},{"v":20,"d":"R 20.00"},{"$f":"E74*D74","v":{"v":440,"d":"R 440.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F7:F75)","v":{"v":77244.8,"d":"R 77,244.80"}},{"$f":"SUM(G5:G75)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"EARTHWORKS"]
[]
[null,"EXCAVATIONS"]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[null,"Open face excavation to expose foundations for inspection and underpinning","m3",{"$f":"32*1.8*0.9*2*2+(0.6)","v":207.96},{"v":50,"d":"R 50.00"},{"$f":"E85*D85","v":{"v":10398,"d":"R 10,398.00"}}]
[]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in"]
[null,"Soft rock","m3",8,{"v":150,"d":"R 150.00"},{"v":1200,"d":"R 1,200.00"}]
[]
[null,"Hard rock","m3",3,{"v":250,"d":"R 250.00"},{"v":750,"d":"R 750.00"}]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",208,{"v":50,"d":"R 50.00"},{"v":10400,"d":"R 10,400.00"}]
[]
[null,"Risk of collapse of excavations"]
[null,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",100,{"v":45,"d":"R 45.00"},{"$f":"E98*D98","v":{"v":4500,"d":"R 4,500.00"}}]
[]
[null,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":600,"d":"R 600.00"},{"v":600,"d":"R 600.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[null,"Under floors, steps, pavings, etc","m3",208,{"v":350,"d":"R 350.00"},{"v":72800,"d":"R 72,800.00"}]
[]
[null,"Backfilling to trenches, holes, etc","m3",8,{"v":350,"d":"R 350.00"},{"v":2800,"d":"R 2,800.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[null,"Under floors etc","m3",72,{"v":350,"d":"R 350.00"},{"v":25200,"d":"R 25,200.00"}]
[]
[null,"Compaction of surfaces"]
[null,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",{"$f":"(32*2*2)+(7.3*2)+0.4","v":143},{"v":45,"d":"R 45.00"},{"v":6435,"d":"R 6,435.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming","m2",143,{"v":20,"d":"R 20.00"},{"v":2860,"d":"R 2,860.00"}]
[]
[null,"To bottoms and sides of trenches etc","m2",143,{"v":20,"d":"R 20.00"},{"v":2860,"d":"R 2,860.00"}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F82:F130)","v":{"v":140803,"d":"R 140,803.00"}}]
[]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"Verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",{"$f":"32*2*0.15","v":9.6},{"v":1800,"d":"R 1,800.00"},{"v":17280,"d":"R 17,280.00"}]
[]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",5,{"v":1800,"d":"R 1,800.00"},{"v":9000,"d":"R 9,000.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",2,{"v":1800,"d":"R 1,800.00"},{"v":3600,"d":"R 3,600.00"}]
[]
[null,"25 Mpa: Pile Caps","m3",{"$f":"0.65*0.65*0.65*64*2","v":35.15200000000001},{"v":1800,"d":"R 1,800.00"},{"$f":"E152*D152","v":{"v":63273.60000000001,"d":"R 63,273.60"}}]
[]
[null,"TEST BLOCKS"]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",4,{"v":150,"d":"R 150.00"},{"v":600,"d":"R 600.00"}]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",{"$f":"32*2","v":64},{"v":45,"d":"R 45.00"},{"$f":"E163*D163","v":{"v":2880,"d":"R 2,880.00"}}]
[]
[null,"Rough formwork to sides"]
[]
[null,"To sides n.e. 300mm","m2",64,{"v":65,"d":"R 65.00"},{"v":4160,"d":"R 4,160.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",{"$f":"2*6","v":12},{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",12,{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",12,{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"12mm Diameter bars","t",1,{"v":13000,"d":"R 13,000.00"},{"$f":"E189*D189","v":{"v":13000,"d":"R 13,000.00"}}]
[]
[null,"10mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"8mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",64,{"v":145,"d":"R 145.00"},{"v":9280,"d":"R 9,280.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F139:F202)","v":{"v":143113.6,"d":"R 143,113.60"}}]
[]
[null,"PILING"]
[]
[null,"Precast concrete piles including reinforcement, couplings, all including driving"]
[null," to required set, grouting, ground water treatment, rock shoe, shafts, carting away"]
[null," displaced soil, bore tests, boring, temporary casing, casing, formwork, etc "]
[null,"completely to Engineer's Instructions. Contractor to determine/recommend "]
[null,"most suitable methodology upon thorough site investigations and exposing "]
[null,"existing foundations."]
[]
[null,"450mm Diameter piles driven to existing bedrock approximately not exceeding "]
[null,"10m deep below ground level through all classes of strata to the required "]
[null,"set in 35MPa reinforced concrete","No",64,{"v":2500,"d":"R 2,500.00"},{"$f":"E216*D216","v":{"v":160000,"d":"R 160,000.00"}}]
[]
[null,"Drilling in strata of a more difficult character","No",64,{"v":2500,"d":"R 2,500.00"},{"$f":"E218*D218","v":{"v":160000,"d":"R 160,000.00"}}]
[]
[null,"EXPOSING PILES FOR INSPECTION"]
[]
[null,"Exposing pile for inspection including excavation 2m deep and backfilling","No",64,{"v":180,"d":"R 180.00"},{"$f":"E222*D222","v":{"v":11520,"d":"R 11,520.00"}}]
[]
[null,"Exposing pile for inspection including excavation 4m deep and backfilling compacted to 98% MOD AASHTO density","No",64,{"v":300,"d":"R 300.00"},{"$f":"E224*D224","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"TRIMMING ETC"]
[]
[null,"Stripping back head of concrete pile for a height to a minimum of 450mm to "]
[null,"expose reinforcement including trimming to defined level and bending reinforcement "]
[null,"as necessary for casting into pile cap"]
[]
[null,"450mm Diameter pile","No",64,{"v":300,"d":"R 300.00"},{"$f":"E232*D232","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"Cutting off and removing excess length of precast concrete pile as necessary "]
[null,"including stripping back for a height not exceeding ?mm to expose reinforcement, "]
[null,"trimming to defined level and bending reinforcement as necessary for casting "]
[null,"into pile cap"]
[]
[null,"450mm Diameter pile","No",64,{"v":300,"d":"R 300.00"},{"$f":"E239*D239","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"TESTING"]
[null,"Transporting and establishment on site of necessary testing plant for the execution of the work and removal thereof on completion","Item",1,{"v":90000,"d":"R 90,000.00"},{"$f":"E242*D242","v":{"v":90000,"d":"R 90,000.00"}}]
[]
[null,"Testing all piles, maximum load to be determinerd by the Engineer.","No",1,{"v":10000,"d":"R 10,000.00"},{"$f":"E244*D244","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"Installing 450mm diameter pile to a depth not exceeding 10m below ground level ","No",1,{"v":20000,"d":"R 20,000.00"},{"$f":"E246*D246","v":{"v":20000,"d":"R 20,000.00"}}]
[null,"and testing to a maximum load determined by the Engineer."]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F211:F248)","v":{"v":509120,"d":"R 509,120.00"}},{"$f":"SUM(G211:G248)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls in beamfilling","m2",31,{"v":380,"d":"R 380.00"},{"$f":"E258*D258","v":{"v":11780,"d":"R 11,780.00"}}]
[null,"One brick walls","m2",{"$f":"(32*0.2*2)+(0.5*7.3*1.8*2)+0.06","v":26},{"v":480,"d":"R 480.00"},{"$f":"E259*D259","v":{"v":12480,"d":"R 12,480.00"}}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"75mm Wide Brickwork reinforcement built in horizontally","m",{"$f":"32*3*2","v":192},{"v":45,"d":"R 45.00"},{"$f":"E265*D265","v":{"v":8640,"d":"R 8,640.00"}}]
[null,"150mm Wide reinforcement built in horizontally","m",{"$f":"7.3*3*2+0.2","v":44},{"v":45,"d":"R 45.00"},{"$f":"E266*D266","v":{"v":1980,"d":"R 1,980.00"}}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",16,{"v":150,"d":"R 150.00"},{"$f":"E270*D270","v":{"v":2400,"d":"R 2,400.00"}}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick (pair)","No",8,{"v":150,"d":"R 150.00"},{"$f":"E273*D273","v":{"v":1200,"d":"R 1,200.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F258:F274)","v":{"v":38480,"d":"R 38,480.00"}},{"$f":"SUM(G258:G274)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",270,{"v":350,"d":"R 350.00"},{"$f":"E289*D289","v":{"v":94500,"d":"R 94,500.00"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",32,{"v":65,"d":"R 65.00"},{"$f":"E292*D292","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"Narrow and broad flute closers","m",32,{"v":65,"d":"R 65.00"},{"$f":"E294*D294","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",32,{"v":65,"d":"R 65.00"},{"$f":"E296*D296","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",270,{"v":25,"d":"R 25.00"},{"$f":"E305*D305","v":{"v":6750,"d":"R 6,750.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F280:F306)","v":{"v":107490,"d":"R 107,490.00"}},{"$f":"SUM(G280:G306)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",{"$f":"32*2","v":64},{"v":65,"d":"R 65.00"},{"$f":"E312*D312","v":{"v":4160,"d":"R 4,160.00"}}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in length, to"]
[null,"manufacturer's specification","m",{"$f":"32*10","v":320},{"v":85,"d":"R 85.00"},{"$f":"E315*D315","v":{"v":27200,"d":"R 27,200.00"}}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",{"$f":"(320*0.08*3)+0.2","v":77.00000000000001},{"v":150,"d":"R 150.00"},{"$f":"E318*D318","v":{"v":11550.000000000002,"d":"R 11,550.00"}}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",{"$f":"8*5*2","v":80},{"v":25,"d":"R 25.00"},{"$f":"E322*D322","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 7300mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",18,{"v":2500,"d":"R 2,500.00"},{"$f":"E329*D329","v":{"v":45000,"d":"R 45,000.00"}}]
[null,"related items"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",64,{"v":110,"d":"R 110.00"},{"$f":"E338*D338","v":{"v":7040,"d":"R 7,040.00"}}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",18,{"v":100,"d":"R 100.00"},{"$f":"E344*D344","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",123,{"v":45,"d":"R 45.00"},{"$f":"E348*D348","v":{"v":5535,"d":"R 5,535.00"}}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",3,{"v":2000,"d":"R 2,000.00"},{"$f":"E354*D354","v":{"v":6000,"d":"R 6,000.00"}}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards size 7000 x 1400mm high","No",3,{"v":4500,"d":"R 4,500.00"},{"$f":"E359*D359","v":{"v":13500,"d":"R 13,500.00"}}]
[]
[null,"WHITE BOARDS, GREEN BOARDS, etc"]
[null,"'Vitrex' Green board Wall mounted All steel fabricated board with rear "]
[null,"stiffeners and sound deadener surround fixed 3 no. times at the top and "]
[null,"bottom with aluminium brackets, sleeve and screw"]
[]
[null,"Standard Green chalk boards 3500 x 1140mm high with two side swinging leaves  in ","No",3,{"v":4500,"d":"R 4,500.00"},{"$f":"E366*D366","v":{"v":13500,"d":"R 13,500.00"}}]
[null,"an epoxy coated tubular steel frame with a hinged bracket (top) and a pivot pin"]
[null," (bottom). and one permanent leaf, with aluminium chalk tray at the bottom"]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted capboards comprising approximately 900 x 1800mm high door and","No",4,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F311:F376)","v":{"v":137285,"d":"R 137,285.00"}},{"$f":"SUM(G311:G376)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",234,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",234,{"v":250,"d":"R 250.00"},{"$f":"E393*D393","v":{"v":58500,"d":"R 58,500.00"}}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",4,{"v":650,"d":"R 650.00"},{"$f":"E398*D398","v":{"v":2600,"d":"R 2,600.00"}}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",123,{"v":65,"d":"R 65.00"},{"$f":"E402*D402","v":{"v":7995,"d":"R 7,995.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F385:F403)","v":{"v":69095,"d":"R 69,095.00"}},{"$f":"SUM(G385:G403)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"2mm vinyl tiles ","m2",234,{"v":280,"d":"R 280.00"},{"$f":"D411*E411","v":{"v":65520,"d":"65,520.00"}}]
[]
[null,"Two coats wax polish on vinyl flooring including sealing","m2",234,{"v":25,"d":"R 25.00"},{"$f":"D413*E413","v":{"v":5850,"d":"5,850.00"}}]
[]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F408:F415)","v":{"v":71370,"d":"R 71,370.00"}},{"$f":"SUM(G408:G415)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},{"$f":"E423*D423","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},{"$f":"C425*E425","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",4,{"v":150,"d":"R 150.00"},{"$f":"E433*D433","v":{"v":600,"d":"R 600.00"}}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},{"$f":"E436*D436","v":{"v":180,"d":"R 180.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F417:F437)","v":{"v":12580,"d":"R 12,580.00"}},{"$f":"SUM(G417:G437)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",{"$f":"D411","v":234},{"v":75,"d":"R 75.00"},{"$f":"E447*D447","v":{"v":17550,"d":"R 17,550.00"}}]
[]
[null,"25mm Thick on floors and landings to varendas and steps","m2",{"$f":"D29","v":67},{"v":75,"d":"R 75.00"},{"$f":"E449*D449","v":{"v":5025,"d":"R 5,025.00"}}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",150,{"v":75,"d":"R 75.00"},{"$f":"E455*D455","v":{"v":11250,"d":"R 11,250.00"}}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},{"$f":"E457*D457","v":{"v":225,"d":"R 225.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F447:F458)","v":{"v":34050,"d":"R 34,050.00"}},{"$f":"SUM(G442:G458)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",64,{"v":110,"d":"R 110.00"},{"$f":"E468*D468","v":{"v":7040,"d":"R 7,040.00"}}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",14,{"v":100,"d":"R 100.00"},{"$f":"E471*D471","v":{"v":1400,"d":"R 1,400.00"}}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},{"$f":"E473*D473","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},{"$f":"E474*D474","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},{"$f":"E475*D475","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},{"$f":"E476*D476","v":{"v":1000,"d":"R 1,000.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",1,{"v":4500,"d":"R 4,500.00"},{"$f":"E482*D482","v":{"v":4500,"d":"R 4,500.00"}}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",3,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},{"$f":"E494*D494","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F463:F495)","v":{"v":26940,"d":"R 26,940.00"}},{"$f":"SUM(G463:G495)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",22,{"v":400,"d":"R 400.00"},{"$f":"E502*D502","v":{"v":8800,"d":"R 8,800.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F499:F503)","v":{"v":8800,"d":"R 8,800.00"}},{"$f":"SUM(G499:G503)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)","v":{"v":370.67999999999995,"d":"371"}},{"v":70,"d":"R 70.00"},{"$f":"E512*D512","v":{"v":25947.599999999995,"d":"R 25,947.60"}}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1","v":{"v":243.66,"d":"244"}},{"v":70,"d":"R 70.00"},{"$f":"E518*D518","v":{"v":17056.2,"d":"R 17,056.20"}}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D338+D344","v":82},{"v":20,"d":"R 20.00"},{"$f":"E524*D524","v":{"v":1640,"d":"R 1,640.00"}}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E530*D530","v":{"v":980,"d":"R 980.00"}}]
[null,"Windows","m2",87,{"v":70,"d":"R 70.00"},{"$f":"E531*D531","v":{"v":6090,"d":"R 6,090.00"}}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E536*D536","v":{"v":980,"d":"R 980.00"}}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D402","v":123},{"v":20,"d":"R 20.00"},{"$f":"E537*D537","v":{"v":2460,"d":"R 2,460.00"}}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D348","v":123},{"v":20,"d":"R 20.00"},{"$f":"E542*D542","v":{"v":2460,"d":"R 2,460.00"}}]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E543*D543","v":{"v":980,"d":"R 980.00"}}]
[null,"Fittings, shelves, cupboards, etc ","m2",150,{"v":70,"d":"R 70.00"},{"$f":"E544*D544","v":{"v":10500,"d":"R 10,500.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F512:F545)","v":{"v":69093.79999999999,"d":"R 69,093.80"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F552:F553)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G552:G553)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":3},{"$f":"F76","v":{"v":77244.8,"d":"R 77,244.80"}},{"$f":"G76","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F275","v":{"v":38480,"d":"R 38,480.00"}},{"$f":"G275","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CONCRETE",{"$nulls":3},{"$f":"F203","v":{"v":143113.6,"d":"R 143,113.60"}},{"$f":"G80","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PILING",{"$nulls":3},{"$f":"F249","v":{"v":509120,"d":"R 509,120.00"}},{"$f":"G279","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F307","v":{"v":107490,"d":"R 107,490.00"}},{"$f":"G307","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F377","v":{"v":137285,"d":"R 137,285.00"}},{"$f":"G377","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F404","v":{"v":69095,"d":"R 69,095.00"}},{"$f":"G404","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F416","v":{"v":71370,"d":"R 71,370.00"}},{"$f":"G416","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F438","v":{"v":12580,"d":"R 12,580.00"}},{"$f":"G438","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F459","v":{"v":34050,"d":"R 34,050.00"}},{"$f":"G459","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F496","v":{"v":26940,"d":"R 26,940.00"}},{"$f":"G496","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F504","v":{"v":8800,"d":"R 8,800.00"}},{"$f":"G504","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F546","v":{"v":69093.79999999999,"d":"R 69,093.80"}},{"$f":"G546","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F554","v":{"v":0,"d":"R 0.00"}},{"$f":"G548","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F559:F587)","v":{"v":1304662.2,"d":"R 1,304,662.20"}},{"$f":"SUM(G561:G587)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"BLOCK 2: HALL"]
[null,"Demolition"]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"One brick walls in parapet","m²",5,{"v":380,"d":"R 380.00"},{"$f":"E596*D596","v":{"v":1900,"d":"R 1,900.00"}}]
[]
[null,"One brick walls in beam filling","m²",31,{"v":380,"d":"R 380.00"},{"$f":"E598*D598","v":{"v":11780,"d":"R 11,780.00"}}]
[]
[null,"229 x 152mm Terra-cotta vermin proof air brick including making good surface to ","No",8,{"v":100,"d":"R 100.00"},{"$f":"E600*D600","v":{"v":800,"d":"R 800.00"}}]
[null,"receive new (new air brick elsewhere measured)"]
[]
[null,"Breaking down and removing concrete, etc "]
[]
[null,"25mm screeds (varendas, external steps, etc) and prepare surface to receive new","m²",67,{"v":120,"d":"R 120.00"},{"$f":"E605*D605","v":{"v":8040,"d":"R 8,040.00"}}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},{"$f":"E611*D611","v":{"v":11680,"d":"R 11,680.00"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",4,{"v":50,"d":"R 50.00"},{"$f":"E617*D617","v":{"v":200,"d":"R 200.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",3,{"v":50,"d":"R 50.00"},{"$f":"E621*D621","v":{"v":150,"d":"R 150.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Greenboard 2400 x 1140mm high","No",3,{"v":50,"d":"R 50.00"},{"$f":"E624*D624","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Roof trusses including purlins","No",30,{"v":50,"d":"R 50.00"},{"$f":"E626*D626","v":{"v":1500,"d":"R 1,500.00"}}]
[]
[null,"Fascia boards","m",{"$f":"32*2","v":64},{"v":10,"d":"R 10.00"},{"$f":"E628*D628","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Roof gutters","m",64,{"v":10,"d":"R 10.00"},{"$f":"E630*D630","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Downpipes","m",25,{"v":10,"d":"R 10.00"},{"$f":"E632*D632","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},{"$f":"E636*D636","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",3,{"v":50,"d":"R 50.00"},{"$f":"E638*D638","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},{"$f":"E642*D642","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)+((32+7.3)*2)*3.1","v":{"v":614.3399999999999,"d":"614"}},{"v":20,"d":"R 20.00"},{"$f":"E644*D644","v":{"v":12286.8,"d":"R 12,286.80"}}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D1020","v":11},{"v":20,"d":"R 20.00"},{"$f":"E646*D646","v":{"v":220,"d":"R 220.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F593:F647)","v":{"v":62216.8,"d":"R 62,216.80"}},{"$f":"SUM(G593:G647)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PILING"]
[]
[null,"Precast concrete piles including reinforcement, couplings, all including driving"]
[null," to required set, grouting, ground water treatment, rock shoe, shafts, carting away"]
[null," displaced soil, bore tests, boring, temporary casing, casing, formwork, etc "]
[null,"completely to Engineer's Instructions. Contractor to determine/recommend "]
[null,"most suitable methodology upon thorough site investigations and exposing "]
[null,"existing foundations."]
[]
[null,"450mm Diameter piles driven to existing bedrock approximately not exceeding "]
[null,"10m deep below ground level through all classes of strata to the required "]
[null,"set in 35MPa reinforced concrete","No",64,{"v":2500,"d":"R 2,500.00"},{"$f":"E661*D661","v":{"v":160000,"d":"R 160,000.00"}}]
[]
[null,"Drilling in strata of a more difficult character","No",64,{"v":2500,"d":"R 2,500.00"},{"$f":"E663*D663","v":{"v":160000,"d":"R 160,000.00"}}]
[]
[null,"EXPOSING PILES FOR INSPECTION"]
[]
[null,"Exposing pile for inspection including excavation 2m deep and backfilling","No",64,{"v":180,"d":"R 180.00"},{"$f":"E667*D667","v":{"v":11520,"d":"R 11,520.00"}}]
[]
[null,"Exposing pile for inspection including excavation 4m deep and backfilling compacted to 98% MOD AASHTO density","No",64,{"v":300,"d":"R 300.00"},{"$f":"E669*D669","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"TRIMMING ETC"]
[]
[null,"Stripping back head of concrete pile for a height to a minimum of 450mm to "]
[null,"expose reinforcement including trimming to defined level and bending reinforcement "]
[null,"as necessary for casting into pile cap"]
[]
[null,"450mm Diameter pile","No",64,{"v":300,"d":"R 300.00"},{"$f":"E677*D677","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"Cutting off and removing excess length of precast concrete pile as necessary "]
[null,"including stripping back for a height not exceeding ?mm to expose reinforcement, "]
[null,"trimming to defined level and bending reinforcement as necessary for casting "]
[null,"into pile cap"]
[]
[null,"450mm Diameter pile","No",64,{"v":300,"d":"R 300.00"},{"$f":"E684*D684","v":{"v":19200,"d":"R 19,200.00"}}]
[]
[null,"TESTING"]
[null,"Transporting and establishment on site of necessary testing plant for the execution of the work and removal thereof on completion","Item",1,{"v":90000,"d":"R 90,000.00"},{"$f":"E687*D687","v":{"v":90000,"d":"R 90,000.00"}}]
[]
[null,"Testing all piles, maximum load to be determinerd by the Engineer.","No",1,{"v":10000,"d":"R 10,000.00"},{"$f":"E689*D689","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"Installing 450mm diameter pile to a depth not exceeding 10m below ground level ","No",1,{"v":20000,"d":"R 20,000.00"},{"$f":"E691*D691","v":{"v":20000,"d":"R 20,000.00"}}]
[null,"and testing to a maximum load determined by the Engineer."]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F656:F693)","v":{"v":509120,"d":"R 509,120.00"}},{"$f":"SUM(G656:G693)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"Verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",{"$f":"32*2*0.15","v":9.6},{"v":1800,"d":"R 1,800.00"},{"$f":"E704*D704","v":{"v":17280,"d":"R 17,280.00"}}]
[]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",5,{"v":1800,"d":"R 1,800.00"},{"v":9000,"d":"R 9,000.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",2,{"v":1800,"d":"R 1,800.00"},{"v":3600,"d":"R 3,600.00"}]
[]
[null,"25 Mpa: Pile Caps","m3",{"$f":"0.65*0.65*0.65*64*2","v":35.15200000000001},{"v":1800,"d":"R 1,800.00"},{"$f":"E716*D716","v":{"v":63273.60000000001,"d":"R 63,273.60"}}]
[]
[null,"TEST BLOCKS"]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",4,{"v":150,"d":"R 150.00"},{"v":600,"d":"R 600.00"}]
[]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",{"$f":"32*2","v":64},{"v":45,"d":"R 45.00"},{"$f":"E727*D727","v":{"v":2880,"d":"R 2,880.00"}}]
[]
[null,"Rough formwork to sides"]
[]
[null,"To sides n.e. 300mm","m2",64,{"v":65,"d":"R 65.00"},{"v":4160,"d":"R 4,160.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",{"$f":"2*6","v":12},{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",12,{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",12,{"v":15,"d":"R 15.00"},{"v":180,"d":"R 180.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"12mm Diameter bars","t",1,{"v":13000,"d":"R 13,000.00"},{"$f":"E753*D753","v":{"v":13000,"d":"R 13,000.00"}}]
[]
[null,"10mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"8mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",0.5,{"v":13000,"d":"R 13,000.00"},{"v":6500,"d":"R 6,500.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",64,{"v":145,"d":"R 145.00"},{"v":9280,"d":"R 9,280.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F703:F766)","v":{"v":143113.6,"d":"R 143,113.60"}}]
[]
[null,"MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls in beamfilling","m2",31,{"v":380,"d":"R 380.00"},{"$f":"E776*D776","v":{"v":11780,"d":"R 11,780.00"}}]
[null,"One brick walls","m2",{"$f":"(32*0.2*2)+(0.5*7.3*1.8*2)+0.06","v":26},{"v":480,"d":"R 480.00"},{"$f":"E777*D777","v":{"v":12480,"d":"R 12,480.00"}}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"75mm Wide Brickwork reinforcement built in horizontally","m",{"$f":"32*3*2","v":192},{"v":45,"d":"R 45.00"},{"$f":"E783*D783","v":{"v":8640,"d":"R 8,640.00"}}]
[null,"150mm Wide reinforcement built in horizontally","m",{"$f":"7.3*3*2+0.2","v":44},{"v":45,"d":"R 45.00"},{"$f":"E784*D784","v":{"v":1980,"d":"R 1,980.00"}}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",16,{"v":150,"d":"R 150.00"},{"$f":"E788*D788","v":{"v":2400,"d":"R 2,400.00"}}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick (pair)","No",8,{"v":150,"d":"R 150.00"},{"$f":"E791*D791","v":{"v":1200,"d":"R 1,200.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F770:F792)","v":{"v":38480,"d":"R 38,480.00"}},{"$f":"SUM(G776:G792)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",270,{"v":280,"d":"R 280.00"},{"$f":"E807*D807","v":{"v":75600,"d":"R 75,600.00"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",32,{"v":65,"d":"R 65.00"},{"$f":"E810*D810","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"Narrow and broad flute closers","m",32,{"v":65,"d":"R 65.00"},{"$f":"E812*D812","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",32,{"v":65,"d":"R 65.00"},{"$f":"E814*D814","v":{"v":2080,"d":"R 2,080.00"}}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",270,{"v":25,"d":"R 25.00"},{"$f":"E823*D823","v":{"v":6750,"d":"R 6,750.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F798:F824)","v":{"v":88590,"d":"R 88,590.00"}},{"$f":"SUM(G798:G824)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",{"$f":"32*2","v":64},{"v":65,"d":"R 65.00"},{"$f":"E830*D830","v":{"v":4160,"d":"R 4,160.00"}}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in length, to"]
[null,"manufacturer's specification","m",{"$f":"32*10","v":320},{"v":85,"d":"R 85.00"},{"$f":"E833*D833","v":{"v":27200,"d":"R 27,200.00"}}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",{"$f":"(320*0.08*3)+0.2","v":77.00000000000001},{"v":150,"d":"R 150.00"},{"$f":"E836*D836","v":{"v":11550.000000000002,"d":"R 11,550.00"}}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",{"$f":"8*5*2","v":80},{"v":25,"d":"R 25.00"},{"$f":"E840*D840","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 7300mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",18,{"v":2500,"d":"R 2,500.00"},{"$f":"E847*D847","v":{"v":45000,"d":"R 45,000.00"}}]
[null,"related items"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",64,{"v":110,"d":"R 110.00"},{"$f":"E856*D856","v":{"v":7040,"d":"R 7,040.00"}}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",18,{"v":100,"d":"R 100.00"},{"$f":"E862*D862","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",123,{"v":45,"d":"R 45.00"},{"$f":"E866*D866","v":{"v":5535,"d":"R 5,535.00"}}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",3,{"v":2000,"d":"R 2,000.00"},{"$f":"E872*D872","v":{"v":6000,"d":"R 6,000.00"}}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards size 7000 x 1400mm high","No",3,{"v":4500,"d":"R 4,500.00"},{"$f":"E877*D877","v":{"v":13500,"d":"R 13,500.00"}}]
[]
[null,"WHITE BOARDS, GREEN BOARDS, etc"]
[null,"'Vitrex' Green board Wall mounted All steel fabricated board with rear "]
[null,"stiffeners and sound deadener surround fixed 3 no. times at the top and "]
[null,"bottom with aluminium brackets, sleeve and screw"]
[]
[null,"Standard Green chalk boards 3500 x 1140mm high with two side swinging leaves  in ","No",3,{"v":4500,"d":"R 4,500.00"},{"$f":"E884*D884","v":{"v":13500,"d":"R 13,500.00"}}]
[null,"an epoxy coated tubular steel frame with a hinged bracket (top) and a pivot pin"]
[null," (bottom). and one permanent leaf, with aluminium chalk tray at the bottom"]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted capboards comprising approximately 900 x 1800mm high door and","No",4,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F829:F894)","v":{"v":137285,"d":"R 137,285.00"}},{"$f":"SUM(G829:G894)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",234,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",234,{"v":250,"d":"R 250.00"},{"$f":"E911*D911","v":{"v":58500,"d":"R 58,500.00"}}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",4,{"v":650,"d":"R 650.00"},{"$f":"E916*D916","v":{"v":2600,"d":"R 2,600.00"}}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",123,{"v":65,"d":"R 65.00"},{"$f":"E920*D920","v":{"v":7995,"d":"R 7,995.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F903:F921)","v":{"v":69095,"d":"R 69,095.00"}},{"$f":"SUM(G903:G921)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"2mm vinyl tiles ","m2",234,{"v":280,"d":"R 280.00"},{"$f":"D929*E929","v":{"v":65520,"d":"65,520.00"}}]
[]
[null,"Two coats wax polish on vinyl flooring including sealing","m2",234,{"v":25,"d":"R 25.00"},{"$f":"D931*E931","v":{"v":5850,"d":"5,850.00"}}]
[]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F926:F933)","v":{"v":71370,"d":"R 71,370.00"}},{"$f":"SUM(G926:G933)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},{"$f":"E941*D941","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},{"$f":"C943*E943","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",4,{"v":150,"d":"R 150.00"},{"$f":"E951*D951","v":{"v":600,"d":"R 600.00"}}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},{"$f":"E954*D954","v":{"v":180,"d":"R 180.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F935:F955)","v":{"v":12580,"d":"R 12,580.00"}},{"$f":"SUM(G935:G955)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",{"$f":"D929","v":234},{"v":75,"d":"R 75.00"},{"$f":"E965*D965","v":{"v":17550,"d":"R 17,550.00"}}]
[]
[null,"25mm Thick on floors and landings to varendas and steps","m2",{"$f":"D605","v":67},{"v":75,"d":"R 75.00"},{"$f":"E967*D967","v":{"v":5025,"d":"R 5,025.00"}}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",50,{"v":75,"d":"R 75.00"},{"$f":"E973*D973","v":{"v":3750,"d":"R 3,750.00"}}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},{"$f":"E975*D975","v":{"v":225,"d":"R 225.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F960:F976)","v":{"v":26550,"d":"R 26,550.00"}},{"$f":"SUM(G960:G976)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",64,{"v":110,"d":"R 110.00"},{"$f":"E986*D986","v":{"v":7040,"d":"R 7,040.00"}}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",14,{"v":100,"d":"R 100.00"},{"$f":"E989*D989","v":{"v":1400,"d":"R 1,400.00"}}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},{"$f":"E991*D991","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},{"$f":"E992*D992","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},{"$f":"E993*D993","v":{"v":1000,"d":"R 1,000.00"}}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},{"$f":"E994*D994","v":{"v":1000,"d":"R 1,000.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",1,{"v":4500,"d":"R 4,500.00"},{"$f":"E1000*D1000","v":{"v":4500,"d":"R 4,500.00"}}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",3,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},{"$f":"E1012*D1012","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F981:F1013)","v":{"v":26940,"d":"R 26,940.00"}},{"$f":"SUM(G981:G1013)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",11,{"v":400,"d":"R 400.00"},{"$f":"E1020*D1020","v":{"v":4400,"d":"R 4,400.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F1017:F1021)","v":{"v":4400,"d":"R 4,400.00"}},{"$f":"SUM(G1017:G1021)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)","v":{"v":370.67999999999995,"d":"371"}},{"v":70,"d":"R 70.00"},{"$f":"E1030*D1030","v":{"v":25947.599999999995,"d":"R 25,947.60"}}]
[null,"Internal ceilings","m2",{"$f":"D965","v":234},{"v":70,"d":"R 70.00"},{"$f":"E1031*D1031","v":{"v":16380,"d":"R 16,380.00"}}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1","v":{"v":243.66,"d":"244"}},{"v":70,"d":"R 70.00"},{"$f":"E1037*D1037","v":{"v":17056.2,"d":"R 17,056.20"}}]
[null,"External ceilings","m2",64,{"v":70,"d":"R 70.00"},{"$f":"E1038*D1038","v":{"v":4480,"d":"R 4,480.00"}}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D856+D862","v":82},{"v":20,"d":"R 20.00"},{"$f":"E1044*D1044","v":{"v":1640,"d":"R 1,640.00"}}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E1050*D1050","v":{"v":980,"d":"R 980.00"}}]
[null,"Windows","m2",87,{"v":70,"d":"R 70.00"},{"$f":"E1051*D1051","v":{"v":6090,"d":"R 6,090.00"}}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E1056*D1056","v":{"v":980,"d":"R 980.00"}}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D920","v":123},{"v":20,"d":"R 20.00"},{"$f":"E1057*D1057","v":{"v":2460,"d":"R 2,460.00"}}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D866","v":123},{"v":20,"d":"R 20.00"},{"$f":"E1062*D1062","v":{"v":2460,"d":"R 2,460.00"}}]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},{"$f":"E1063*D1063","v":{"v":980,"d":"R 980.00"}}]
[null,"Fittings, shelves, cupboards, etc ","m2",150,{"v":70,"d":"R 70.00"},{"$f":"E1064*D1064","v":{"v":10500,"d":"R 10,500.00"}}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F1030:F1065)","v":{"v":89953.79999999999,"d":"R 89,953.80"}},{"$f":"SUM(G1030:G1065)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":3},{"$f":"SUM(F1072:F1073)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G1072:G1073)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":3},{"$f":"F648","v":{"v":62216.8,"d":"R 62,216.80"}},{"$f":"G648","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PILING",{"$nulls":3},{"$f":"F694","v":{"v":509120,"d":"R 509,120.00"}},{"$f":"G819","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CONCRETE",{"$nulls":3},{"$f":"F767","v":{"v":143113.6,"d":"R 143,113.60"}},{"$f":"G889","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F793","v":{"v":38480,"d":"R 38,480.00"}},{"$f":"G793","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F825","v":{"v":88590,"d":"R 88,590.00"}},{"$f":"G825","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F895","v":{"v":137285,"d":"R 137,285.00"}},{"$f":"G895","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F922","v":{"v":69095,"d":"R 69,095.00"}},{"$f":"G922","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F934","v":{"v":71370,"d":"R 71,370.00"}},{"$f":"G934","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F956","v":{"v":12580,"d":"R 12,580.00"}},{"$f":"G956","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F977","v":{"v":26550,"d":"R 26,550.00"}},{"$f":"G977","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F1014","v":{"v":26940,"d":"R 26,940.00"}},{"$f":"G1014","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F1022","v":{"v":4400,"d":"R 4,400.00"}},{"$f":"G1022","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F1066","v":{"v":89953.79999999999,"d":"R 89,953.80"}},{"$f":"G1066","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F1074","v":{"v":0,"d":"R 0.00"}},{"$f":"G1068","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F1079:F1107)","v":{"v":1279694.2,"d":"R 1,279,694.20"}},{"$f":"SUM(G1085:G1107)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[]
[null,"BLOCK 3: 3 CLASSROOM AND 1 STRONGROOM"]
[null,"Demolition"]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"One brick walls in parapet","m²",5,{"v":380,"d":"R 380.00"},null,{"$f":"E1117*D1117","v":{"v":1900,"d":"R 1,900.00"}}]
[]
[null,"229 x 152mm Terra-cotta vermin proof air brick including making good surface to ","No",24,{"v":100,"d":"R 100.00"},null,{"v":2400,"d":"R 2,400.00"}]
[null,"receive new (new air brick elsewhere measured)"]
[]
[null,"Breaking down and removing concrete, etc "]
[]
[null,"25mm screeds (varendas, external steps, etc) and prepare surface to receive new","m²",67,{"v":120,"d":"R 120.00"},null,{"$f":"E1124*D1124","v":{"v":8040,"d":"R 8,040.00"}}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1130*D1130","v":{"v":11680,"d":"R 11,680.00"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Ceiling board","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1133*D1133","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",3,{"v":50,"d":"R 50.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Taking out and removing fittings and making good surfaces to receive new"]
[]
[null,"Ceiling fan","No",1,{"v":50,"d":"R 50.00"},null,{"$f":"E1142*D1142","v":{"v":50,"d":"R 50.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1146*D1146","v":{"v":150,"d":"R 150.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Greenboard 2400 x 1140mm high","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1149*D1149","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Fascia boards","m",{"$f":"32*2","v":64},{"v":10,"d":"R 10.00"},null,{"$f":"E1151*D1151","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Roof gutters","m",64,{"v":10,"d":"R 10.00"},null,{"$f":"E1153*D1153","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Downpipes","m",25,{"v":10,"d":"R 10.00"},null,{"$f":"E1155*D1155","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1159*D1159","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1161*D1161","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1165*D1165","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)+((32+7.3)*2)*3.1","v":{"v":614.3399999999999,"d":"614"}},{"v":20,"d":"R 20.00"},null,{"v":12286.8,"d":"R 12,286.80"}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D1438","v":11},{"v":20,"d":"R 20.00"},null,{"$f":"E1169*D1169","v":{"v":220,"d":"R 220.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1114:G1170)","v":{"v":62216.8,"d":"R 62,216.80"}}]
[]
[null,"NEW WORKS"]
[]
[null,"MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls in beamfilling","m2",31,{"v":380,"d":"R 380.00"},null,{"$f":"E1182*D1182","v":{"v":11780,"d":"R 11,780.00"}}]
[null,"One brick walls","m2",{"$f":"(32*0.2*2)+(0.5*7.3*1.8*2)+0.06","v":26},{"v":480,"d":"R 480.00"},null,{"v":12480,"d":"R 12,480.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"75mm Wide Brickwork reinforcement built in horizontally","m",{"$f":"32*3*2","v":192},{"v":45,"d":"R 45.00"},null,{"v":8640,"d":"R 8,640.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",{"$f":"7.3*3*2+0.2","v":44},{"v":45,"d":"R 45.00"},null,{"v":1980,"d":"R 1,980.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick (pair)","No",24,{"v":150,"d":"R 150.00"},null,{"v":3600,"d":"R 3,600.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1182:G1194)","v":{"v":38480,"d":"R 38,480.00"}}]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",270,{"v":280,"d":"R 280.00"},null,{"$f":"E1209*D1209","v":{"v":75600,"d":"R 75,600.00"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"Narrow and broad flute closers","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",270,{"v":25,"d":"R 25.00"},null,{"$f":"E1225*D1225","v":{"v":6750,"d":"R 6,750.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1200:G1226)","v":{"v":88590,"d":"R 88,590.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",{"$f":"32*2","v":64},{"v":65,"d":"R 65.00"},null,{"v":4160,"d":"R 4,160.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in length, to"]
[null,"manufacturer's specification","m",{"$f":"32*10","v":320},{"v":85,"d":"R 85.00"},null,{"v":27200,"d":"R 27,200.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",{"$f":"(320*0.08*3)+0.2","v":77.00000000000001},{"v":150,"d":"R 150.00"},null,{"v":11550.000000000002,"d":"R 11,550.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",{"$f":"8*5*2","v":80},{"v":25,"d":"R 25.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",64,{"v":110,"d":"R 110.00"},null,{"v":7040,"d":"R 7,040.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",18,{"v":100,"d":"R 100.00"},null,{"v":1800,"d":"R 1,800.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",131,{"v":45,"d":"R 45.00"},null,{"v":5895,"d":"R 5,895.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",3,{"v":2000,"d":"R 2,000.00"},null,{"v":6000,"d":"R 6,000.00"}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards size 7000 x 1400mm high","No",3,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E1271*D1271","v":{"v":13500,"d":"R 13,500.00"}}]
[]
[null,"WHITE BOARDS, GREEN BOARDS, etc"]
[null,"'Vitrex' Green board Wall mounted All steel fabricated board with rear "]
[null,"stiffeners and sound deadener surround fixed 3 no. times at the top and "]
[null,"bottom with aluminium brackets, sleeve and screw"]
[]
[null,"Standard Green chalk boards 3500 x 1140mm high with two side swinging leaves  in ","No",3,{"v":4500,"d":"R 4,500.00"},null,{"v":13500,"d":"R 13,500.00"}]
[null,"an epoxy coated tubular steel frame with a hinged bracket (top) and a pivot pin"]
[null," (bottom). and one permanent leaf, with aluminium chalk tray at the bottom"]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted cupboards comprising approximately 900 x 1800mm high door and","No",4,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"Ceiling fan","No",1,{"v":5000,"d":"R 5,000.00"}]
[]
[null,"Shelving","item",1,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1231:G1292)","v":{"v":92645,"d":"R 92,645.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",234,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",234,{"v":250,"d":"R 250.00"},null,{"v":58500,"d":"R 58,500.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",4,{"v":650,"d":"R 650.00"},null,{"v":2600,"d":"R 2,600.00"}]
[]
[null,"9mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured). (externally at eaves)","m2",{"$f":"32*2","v":64},{"v":250,"d":"R 250.00"},null,{"$f":"E1320*D1320","v":{"v":16000,"d":"R 16,000.00"}}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",123,{"v":65,"d":"R 65.00"},null,{"v":7995,"d":"R 7,995.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1301:G1325)","v":{"v":85095,"d":"R 85,095.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"2mm vinyl tiles ","m2",234,{"v":280,"d":"R 280.00"},null,{"$f":"D1333*E1333","v":{"v":65520,"d":"65,520.00"}}]
[]
[null,"Two coats wax polish on vinyl flooring including sealing","m2",234,{"v":25,"d":"R 25.00"},null,{"$f":"D1335*E1335","v":{"v":5850,"d":"5,850.00"}}]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1330:G1337)","v":{"v":71370,"d":"R 71,370.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},null,{"$f":"E1345*D1345","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},null,{"$f":"C1347*E1347","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",4,{"v":150,"d":"R 150.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},null,{"v":180,"d":"R 180.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1339:G1359)","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"METALWORK"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[null,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",1,{"v":35000,"d":"R 35,000.00"},{"$f":"E1371*D1371","v":{"v":35000,"d":"R 35,000.00"}}]
[]
[null,"Double ended strongroom ventilator","No",1,{"v":1500,"d":"R 1,500.00"},{"v":1500,"d":"R 1,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1370:G1373)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",{"$f":"D1333","v":234},{"v":75,"d":"R 75.00"},null,{"$f":"E1383*D1383","v":{"v":17550,"d":"R 17,550.00"}}]
[]
[null,"25mm Thick on floors and landings to varendas and steps","m2",{"$f":"D1124","v":67},{"v":75,"d":"R 75.00"},null,{"$f":"E1385*D1385","v":{"v":5025,"d":"R 5,025.00"}}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",50,{"v":75,"d":"R 75.00"},null,{"v":3750,"d":"R 3,750.00"}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1378:G1394)","v":{"v":26550,"d":"R 26,550.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",64,{"v":110,"d":"R 110.00"},null,{"v":7040,"d":"R 7,040.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",14,{"v":100,"d":"R 100.00"},null,{"v":1400,"d":"R 1,400.00"}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",1,{"v":4500,"d":"R 4,500.00"},null,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",3,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},null,{"$f":"E1430*D1430","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1399:G1431)","v":{"v":26940,"d":"R 26,940.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",11,{"v":400,"d":"R 400.00"},null,{"v":4400,"d":"R 4,400.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1435:G1439)","v":{"v":4400,"d":"R 4,400.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)","v":{"v":370.67999999999995,"d":"371"}},{"v":70,"d":"R 70.00"},null,{"v":25947.599999999995,"d":"R 25,947.60"}]
[null,"Ceilings","m2",{"$f":"D1383","v":234},{"v":70,"d":"R 70.00"},null,{"v":16380,"d":"R 16,380.00"}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1","v":{"v":243.66,"d":"244"}},{"v":70,"d":"R 70.00"},null,{"$f":"E1455*D1455","v":{"v":17056.2,"d":"R 17,056.20"}}]
[null,"External Ceilings to eaves","m2",64,{"v":70,"d":"R 70.00"},null,{"v":4480,"d":"R 4,480.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D1250+D1256","v":82},{"v":20,"d":"R 20.00"},null,{"v":1640,"d":"R 1,640.00"}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Windows","m2",87,{"v":70,"d":"R 70.00"},null,{"v":6090,"d":"R 6,090.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D1324","v":123},{"v":20,"d":"R 20.00"},null,{"v":2460,"d":"R 2,460.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D1260","v":131},{"v":20,"d":"R 20.00"},null,{"v":2620,"d":"R 2,620.00"}]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Fittings, shelves, cupboards, etc ","m2",150,{"v":70,"d":"R 70.00"},null,{"v":10500,"d":"R 10,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1448:G1483)","v":{"v":90113.79999999999,"d":"R 90,113.80"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1490:G1491)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":3},{"$f":"F1171","v":{"v":0,"d":"R 0.00"}},{"$f":"G1171","v":{"v":62216.8,"d":"R 62,216.80"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F1195","v":{"v":0,"d":"R 0.00"}},{"$f":"G1195","v":{"v":38480,"d":"R 38,480.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F1227","v":{"v":0,"d":"R 0.00"}},{"$f":"G1227","v":{"v":88590,"d":"R 88,590.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F1293","v":{"v":0,"d":"R 0.00"}},{"$f":"G1293","v":{"v":92645,"d":"R 92,645.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F1326","v":{"v":0,"d":"R 0.00"}},{"$f":"G1326","v":{"v":85095,"d":"R 85,095.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F1338","v":{"v":0,"d":"R 0.00"}},{"$f":"G1338","v":{"v":71370,"d":"R 71,370.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F1360","v":{"v":0,"d":"R 0.00"}},{"$f":"G1360","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"METALWORK",{"$nulls":3},{"$f":"F1362","v":{"v":0,"d":"R 0.00"}},{"$f":"G1375","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F1395","v":{"v":0,"d":"R 0.00"}},{"$f":"G1395","v":{"v":26550,"d":"R 26,550.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F1432","v":{"v":0,"d":"R 0.00"}},{"$f":"G1432","v":{"v":26940,"d":"R 26,940.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F1440","v":{"v":0,"d":"R 0.00"}},{"$f":"G1440","v":{"v":4400,"d":"R 4,400.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F1484","v":{"v":0,"d":"R 0.00"}},{"$f":"G1484","v":{"v":90113.79999999999,"d":"R 90,113.80"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F1486","v":{"v":0,"d":"R 0.00"}},{"$f":"G1492","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F1496:F1522)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G1498:G1522)","v":{"v":536763.8,"d":"R 536,763.80"}}]
[]
[]
[]
[]
[null,"BLOCK 4: 4 CLASSROOM"]
[null,"Demolition"]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"One brick walls in parapet","m²",5,{"v":380,"d":"R 380.00"},null,{"$f":"E1533*D1533","v":{"v":1900,"d":"R 1,900.00"}}]
[]
[null,"229 x 152mm Terra-cotta vermin proof air brick including making good surface to ","No",24,{"v":100,"d":"R 100.00"},null,{"v":2400,"d":"R 2,400.00"}]
[null,"receive new (new air brick elsewhere measured)"]
[]
[null,"Breaking down and removing concrete, etc "]
[]
[null,"25mm screeds (varendas, external steps, etc) and prepare surface to receive new","m²",67,{"v":120,"d":"R 120.00"},null,{"$f":"E1540*D1540","v":{"v":8040,"d":"R 8,040.00"}}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1546*D1546","v":{"v":11680,"d":"R 11,680.00"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Ceiling board","m2",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1549*D1549","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",3,{"v":50,"d":"R 50.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Taking out and removing fittings and making good surfaces to receive new"]
[]
[null,"Ceiling fan","No",4,{"v":50,"d":"R 50.00"},null,{"$f":"E1558*D1558","v":{"v":200,"d":"R 200.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1562*D1562","v":{"v":150,"d":"R 150.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Greenboard 2400 x 1140mm high","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1565*D1565","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Fascia boards","m",{"$f":"32*2","v":64},{"v":10,"d":"R 10.00"},null,{"$f":"E1567*D1567","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Roof gutters","m",64,{"v":10,"d":"R 10.00"},null,{"$f":"E1569*D1569","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Downpipes","m",25,{"v":10,"d":"R 10.00"},null,{"$f":"E1571*D1571","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1575*D1575","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",25,{"v":50,"d":"R 50.00"},null,{"$f":"E1577*D1577","v":{"v":1250,"d":"R 1,250.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",{"$f":"7.3*32","v":{"v":233.6,"d":"234"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1581*D1581","v":{"v":11680,"d":"R 11,680.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)+((32+7.3)*2)*3.1","v":{"v":614.3399999999999,"d":"614"}},{"v":20,"d":"R 20.00"},null,{"v":12286.8,"d":"R 12,286.80"}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D1836","v":11},{"v":20,"d":"R 20.00"},null,{"$f":"E1585*D1585","v":{"v":220,"d":"R 220.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1530:G1586)","v":{"v":63466.8,"d":"R 63,466.80"}}]
[]
[null,"NEW WORKS"]
[]
[null,"MASONRY"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls in beamfilling","m2",31,{"v":380,"d":"R 380.00"},null,{"$f":"E1598*D1598","v":{"v":11780,"d":"R 11,780.00"}}]
[null,"One brick walls","m2",{"$f":"(32*0.2*2)+(0.5*7.3*1.8*2)+0.06","v":26},{"v":480,"d":"R 480.00"},null,{"v":12480,"d":"R 12,480.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"75mm Wide Brickwork reinforcement built in horizontally","m",{"$f":"32*3*2","v":192},{"v":45,"d":"R 45.00"},null,{"v":8640,"d":"R 8,640.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",{"$f":"7.3*3*2+0.2","v":44},{"v":45,"d":"R 45.00"},null,{"v":1980,"d":"R 1,980.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick (pair)","No",24,{"v":150,"d":"R 150.00"},null,{"v":3600,"d":"R 3,600.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1598:G1610)","v":{"v":38480,"d":"R 38,480.00"}}]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",270,{"v":250,"d":"R 250.00"},null,{"$f":"E1625*D1625","v":{"v":67500,"d":"R 67,500.00"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"Narrow and broad flute closers","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",32,{"v":65,"d":"R 65.00"},null,{"v":2080,"d":"R 2,080.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",270,{"v":25,"d":"R 25.00"},null,{"$f":"E1641*D1641","v":{"v":6750,"d":"R 6,750.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1616:G1642)","v":{"v":80490,"d":"R 80,490.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",{"$f":"32*2","v":64},{"v":65,"d":"R 65.00"},null,{"v":4160,"d":"R 4,160.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in length, to"]
[null,"manufacturer's specification","m",{"$f":"32*10","v":320},{"v":85,"d":"R 85.00"},null,{"v":27200,"d":"R 27,200.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",{"$f":"(320*0.08*3)+0.2","v":77.00000000000001},{"v":150,"d":"R 150.00"},null,{"v":11550.000000000002,"d":"R 11,550.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",{"$f":"8*5*2","v":80},{"v":25,"d":"R 25.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",64,{"v":110,"d":"R 110.00"},null,{"v":7040,"d":"R 7,040.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",18,{"v":100,"d":"R 100.00"},null,{"v":1800,"d":"R 1,800.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",131,{"v":45,"d":"R 45.00"},null,{"v":5895,"d":"R 5,895.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",4,{"v":2000,"d":"R 2,000.00"},null,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards size 7000 x 1400mm high","No",4,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E1687*D1687","v":{"v":18000,"d":"R 18,000.00"}}]
[]
[null,"WHITE BOARDS, GREEN BOARDS, etc"]
[null,"'Vitrex' Green board Wall mounted All steel fabricated board with rear "]
[null,"stiffeners and sound deadener surround fixed 3 no. times at the top and "]
[null,"bottom with aluminium brackets, sleeve and screw"]
[]
[null,"Standard Green chalk boards 3500 x 1140mm high with two side swinging leaves  in ","No",3,{"v":4500,"d":"R 4,500.00"},null,{"v":13500,"d":"R 13,500.00"}]
[null,"an epoxy coated tubular steel frame with a hinged bracket (top) and a pivot pin"]
[null," (bottom). and one permanent leaf, with aluminium chalk tray at the bottom"]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted cupboards comprising approximately 900 x 1800mm high door and","No",4,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"Ceiling fan","No",1,{"v":5000,"d":"R 5,000.00"}]
[]
[null,"Shelving","item",1,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1647:G1708)","v":{"v":99145,"d":"R 99,145.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",234,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",234,{"v":250,"d":"R 250.00"},null,{"v":58500,"d":"R 58,500.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",4,{"v":650,"d":"R 650.00"},null,{"v":2600,"d":"R 2,600.00"}]
[]
[null,"9mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured). (externally at eaves)","m2",{"$f":"32*2","v":64},{"v":250,"d":"R 250.00"},null,{"$f":"E1736*D1736","v":{"v":16000,"d":"R 16,000.00"}}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",123,{"v":65,"d":"R 65.00"},null,{"v":7995,"d":"R 7,995.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1717:G1741)","v":{"v":85095,"d":"R 85,095.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"2mm vinyl tiles ","m2",234,{"v":280,"d":"R 280.00"},null,{"$f":"D1749*E1749","v":{"v":65520,"d":"65,520.00"}}]
[]
[null,"Two coats wax polish on vinyl flooring including sealing","m2",234,{"v":25,"d":"R 25.00"},null,{"$f":"D1751*E1751","v":{"v":5850,"d":"5,850.00"}}]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1746:G1753)","v":{"v":71370,"d":"R 71,370.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},null,{"$f":"E1761*D1761","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},null,{"$f":"C1763*E1763","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",4,{"v":150,"d":"R 150.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},null,{"v":180,"d":"R 180.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1755:G1775)","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",{"$f":"D1749","v":234},{"v":75,"d":"R 75.00"},null,{"$f":"E1784*D1784","v":{"v":17550,"d":"R 17,550.00"}}]
[]
[null,"25mm Thick on floors and landings to varendas and steps","m2",{"$f":"D1540","v":67},{"v":75,"d":"R 75.00"},null,{"$f":"E1786*D1786","v":{"v":5025,"d":"R 5,025.00"}}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",50,{"v":75,"d":"R 75.00"},null,{"v":3750,"d":"R 3,750.00"}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1779:G1795)","v":{"v":26550,"d":"R 26,550.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",64,{"v":110,"d":"R 110.00"},null,{"v":7040,"d":"R 7,040.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",14,{"v":100,"d":"R 100.00"},null,{"v":1400,"d":"R 1,400.00"}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",4,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},null,{"$f":"E1828*D1828","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1800:G1829)","v":{"v":22440,"d":"R 22,440.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",11,{"v":400,"d":"R 400.00"},null,{"v":4400,"d":"R 4,400.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1833:G1837)","v":{"v":4400,"d":"R 4,400.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*4)","v":{"v":413.02,"d":"413"}},{"v":70,"d":"R 70.00"},null,{"v":28911.399999999998,"d":"R 28,911.40"}]
[null,"Ceilings","m2",{"$f":"D1784","v":234},{"v":70,"d":"R 70.00"},null,{"v":16380,"d":"R 16,380.00"}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((32+7.3)*2)*3.1","v":{"v":243.66,"d":"244"}},{"v":70,"d":"R 70.00"},null,{"$f":"E1853*D1853","v":{"v":17056.2,"d":"R 17,056.20"}}]
[null,"External Ceilings to eaves","m2",64,{"v":70,"d":"R 70.00"},null,{"v":4480,"d":"R 4,480.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D1666+D1672","v":82},{"v":20,"d":"R 20.00"},null,{"v":1640,"d":"R 1,640.00"}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Windows","m2",87,{"v":70,"d":"R 70.00"},null,{"v":6090,"d":"R 6,090.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D1740","v":123},{"v":20,"d":"R 20.00"},null,{"v":2460,"d":"R 2,460.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D1676","v":131},{"v":20,"d":"R 20.00"},null,{"v":2620,"d":"R 2,620.00"}]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Fittings, shelves, cupboards, etc ","m2",150,{"v":70,"d":"R 70.00"},null,{"v":10500,"d":"R 10,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1846:G1881)","v":{"v":93077.59999999999,"d":"R 93,077.60"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1888:G1889)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G1587","v":{"v":63466.8,"d":"R 63,466.80"}}]
[]
[null,"MASONRY",{"$nulls":4},{"$f":"G1611","v":{"v":38480,"d":"R 38,480.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F1643","v":{"v":0,"d":"R 0.00"}},{"$f":"G1643","v":{"v":80490,"d":"R 80,490.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F1709","v":{"v":0,"d":"R 0.00"}},{"$f":"G1709","v":{"v":99145,"d":"R 99,145.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F1742","v":{"v":0,"d":"R 0.00"}},{"$f":"G1742","v":{"v":85095,"d":"R 85,095.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F1754","v":{"v":0,"d":"R 0.00"}},{"$f":"G1754","v":{"v":71370,"d":"R 71,370.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F1776","v":{"v":0,"d":"R 0.00"}},{"$f":"G1776","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F1796","v":{"v":0,"d":"R 0.00"}},{"$f":"G1796","v":{"v":26550,"d":"R 26,550.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F1830","v":{"v":0,"d":"R 0.00"}},{"$f":"G1830","v":{"v":22440,"d":"R 22,440.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F1838","v":{"v":0,"d":"R 0.00"}},{"$f":"G1838","v":{"v":4400,"d":"R 4,400.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F1882","v":{"v":0,"d":"R 0.00"}},{"$f":"G1882","v":{"v":93077.59999999999,"d":"R 93,077.60"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F1884","v":{"v":0,"d":"R 0.00"}},{"$f":"G1890","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F1894:F1918)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G1896:G1918)","v":{"v":533627.6,"d":"R 533,627.60"}}]
[]
[]
[]
[null,"BLOCK 5: ADMINISTRATION"]
[null,"Demolition"]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"8.5*7*1.15","v":{"v":68.425,"d":"68"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1930*D1930","v":{"v":3421.25,"d":"R 3,421.25"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Ceiling board","m2",{"$f":"8.2*7","v":{"v":57.39999999999999,"d":"57"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1933*D1933","v":{"v":2869.9999999999995,"d":"R 2,870.00"}}]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",3,{"v":50,"d":"R 50.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Taking out and removing fittings and making good surfaces to receive new"]
[]
[null,"Ceiling fan","No",1,{"v":50,"d":"R 50.00"},null,{"$f":"E1942*D1942","v":{"v":50,"d":"R 50.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1946*D1946","v":{"v":150,"d":"R 150.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Fascia boards","m",31,{"v":10,"d":"R 10.00"},null,{"$f":"E1949*D1949","v":{"v":310,"d":"R 310.00"}}]
[]
[null,"Roof gutters","m",17,{"v":10,"d":"R 10.00"},null,{"$f":"E1951*D1951","v":{"v":170,"d":"R 170.00"}}]
[]
[null,"Downpipes","m",13,{"v":10,"d":"R 10.00"},null,{"$f":"E1953*D1953","v":{"v":130,"d":"R 130.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1957*D1957","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E1959*D1959","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",{"$f":"8.2*7","v":{"v":57.39999999999999,"d":"57"}},{"v":50,"d":"R 50.00"},null,{"$f":"E1963*D1963","v":{"v":2869.9999999999995,"d":"R 2,870.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((8.2+7.3)*2)*3.1+(7.3*2.9*2*3)+((8.2+7.3)*2)*3.1","v":{"v":319.22,"d":"319"}},{"v":20,"d":"R 20.00"},null,{"v":6384.400000000001,"d":"R 6,384.40"}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D2160","v":5},{"v":20,"d":"R 20.00"},null,{"$f":"E1967*D1967","v":{"v":100,"d":"R 100.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1925:G1968)","v":{"v":16905.65,"d":"R 16,905.65"}}]
[]
[null,"NEW WORKS"]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",{"$f":"D1963*1.15","v":66.00999999999999},{"v":250,"d":"R 250.00"},null,{"$f":"E1985*D1985","v":{"v":16502.499999999996,"d":"R 16,502.50"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",9,{"v":65,"d":"R 65.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"Narrow and broad flute closers","m",9,{"v":65,"d":"R 65.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",9,{"v":65,"d":"R 65.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",58,{"v":25,"d":"R 25.00"},null,{"$f":"E2001*D2001","v":{"v":1450,"d":"R 1,450.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G1976:G2002)","v":{"v":19707.499999999996,"d":"R 19,707.50"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",17,{"v":110,"d":"R 110.00"},null,{"v":1870,"d":"R 1,870.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",14,{"v":100,"d":"R 100.00"},null,{"v":1400,"d":"R 1,400.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",131,{"v":45,"d":"R 45.00"},null,{"v":5895,"d":"R 5,895.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",3,{"v":2000,"d":"R 2,000.00"},null,{"v":6000,"d":"R 6,000.00"}]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards size 2000 x 1400mm high","No",1,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E2034*D2034","v":{"v":4500,"d":"R 4,500.00"}}]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted cupboards comprising approximately 900 x 1800mm high door and","No",4,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"Ceiling fan","No",1,{"v":5000,"d":"R 5,000.00"}]
[]
[null,"Shelving","item",1,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2007:G2046)","v":{"v":19665,"d":"R 19,665.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",58,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",58,{"v":250,"d":"R 250.00"},null,{"v":14500,"d":"R 14,500.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",1,{"v":650,"d":"R 650.00"},null,{"v":650,"d":"R 650.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",56,{"v":65,"d":"R 65.00"},null,{"v":3640,"d":"R 3,640.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2055:G2073)","v":{"v":18790,"d":"R 18,790.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"Clean ceramic tiles with suitable chemicals and repair grout","m2",58,{"v":90,"d":"R 90.00"},null,{"$f":"D2081*E2081","v":{"v":5220,"d":"5,220.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2078:G2082)","v":{"v":5220,"d":"R 5,220.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},null,{"$f":"E2090*D2090","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},null,{"$f":"C2092*E2092","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral (HEADMASTER, etc)","No",4,{"v":150,"d":"R 150.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},null,{"v":180,"d":"R 180.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2084:G2104)","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",50,{"v":75,"d":"R 75.00"},null,{"$f":"E2113*D2113","v":{"v":3750,"d":"R 3,750.00"}}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2108:G2116)","v":{"v":3975,"d":"R 3,975.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",17,{"v":110,"d":"R 110.00"},null,{"v":1870,"d":"R 1,870.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",14,{"v":100,"d":"R 100.00"},null,{"v":1400,"d":"R 1,400.00"}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",1,{"v":4500,"d":"R 4,500.00"},null,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",1,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},null,{"$f":"E2152*D2152","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2121:G2153)","v":{"v":21770,"d":"R 21,770.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",5,{"v":400,"d":"R 400.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2157:G2161)","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((8.2+7.3)*2)*3.1+(7.3*2.9*2*2)","v":{"v":180.78,"d":"181"}},{"v":70,"d":"R 70.00"},null,{"v":12654.6,"d":"R 12,654.60"}]
[null,"Ceilings","m2",58,{"v":70,"d":"R 70.00"},null,{"v":4060,"d":"R 4,060.00"}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((8.2+7.3)*2)*3.1","v":{"v":96.10000000000001,"d":"96"}},{"v":70,"d":"R 70.00"},null,{"$f":"E2177*D2177","v":{"v":6727.000000000001,"d":"R 6,727.00"}}]
[null,"External Ceilings to eaves","m2",5,{"v":70,"d":"R 70.00"},null,{"v":350,"d":"R 350.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D2013+D2019","v":31},{"v":20,"d":"R 20.00"},null,{"v":620,"d":"R 620.00"}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Windows","m2",45,{"v":70,"d":"R 70.00"},null,{"v":3150,"d":"R 3,150.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D2072","v":56},{"v":20,"d":"R 20.00"},null,{"v":1120,"d":"R 1,120.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D2023","v":131},{"v":20,"d":"R 20.00"},null,{"v":2620,"d":"R 2,620.00"}]
[null,"Doors","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[null,"Fittings, shelves, cupboards, etc ","m2",150,{"v":70,"d":"R 70.00"},null,{"v":10500,"d":"R 10,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2170:G2205)","v":{"v":44741.6,"d":"R 44,741.60"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2212:G2213)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G1969","v":{"v":16905.65,"d":"R 16,905.65"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F2003","v":{"v":0,"d":"R 0.00"}},{"$f":"G2003","v":{"v":19707.499999999996,"d":"R 19,707.50"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F2047","v":{"v":0,"d":"R 0.00"}},{"$f":"G2047","v":{"v":19665,"d":"R 19,665.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F2074","v":{"v":0,"d":"R 0.00"}},{"$f":"G2074","v":{"v":18790,"d":"R 18,790.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F2083","v":{"v":0,"d":"R 0.00"}},{"$f":"G2083","v":{"v":5220,"d":"R 5,220.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F2105","v":{"v":0,"d":"R 0.00"}},{"$f":"G2105","v":{"v":12580,"d":"R 12,580.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F2117","v":{"v":0,"d":"R 0.00"}},{"$f":"G2117","v":{"v":3975,"d":"R 3,975.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F2154","v":{"v":0,"d":"R 0.00"}},{"$f":"G2154","v":{"v":21770,"d":"R 21,770.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F2162","v":{"v":0,"d":"R 0.00"}},{"$f":"G2162","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F2206","v":{"v":0,"d":"R 0.00"}},{"$f":"G2206","v":{"v":44741.6,"d":"R 44,741.60"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F2208","v":{"v":0,"d":"R 0.00"}},{"$f":"G2214","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F2218:F2240)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G2220:G2240)","v":{"v":148449.1,"d":"R 148,449.10"}}]
[]
[]
[]
[]
[null,"BLOCK 6: KITCHEN"]
[null,"Demolition"]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Metal roof covering including fascias, bargeboards  and rainwater","m2",{"$f":"4*5","v":20},{"v":50,"d":"R 50.00"},null,{"$f":"E2253*D2253","v":{"v":1000,"d":"R 1,000.00"}}]
[null," goods and dispose off as per the SHE  regulations."]
[null," "]
[null,"Ceiling board","m2",20,{"v":50,"d":"R 50.00"},null,{"$f":"E2256*D2256","v":{"v":1000,"d":"R 1,000.00"}}]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",1,{"v":50,"d":"R 50.00"},null,{"v":50,"d":"R 50.00"}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber cupboard comprising door size 900 x 1800mm high with a timber frame,","No",1,{"v":50,"d":"R 50.00"},null,{"$f":"E2265*D2265","v":{"v":50,"d":"R 50.00"}}]
[null," shelves, etc and making good surfaces to receive new"]
[]
[null,"Fascia boards","m",10,{"v":10,"d":"R 10.00"},null,{"$f":"E2268*D2268","v":{"v":100,"d":"R 100.00"}}]
[]
[null,"Roof gutters","m",10,{"v":10,"d":"R 10.00"},null,{"$f":"E2270*D2270","v":{"v":100,"d":"R 100.00"}}]
[]
[null,"Downpipes","m",13,{"v":10,"d":"R 10.00"},null,{"$f":"E2272*D2272","v":{"v":130,"d":"R 130.00"}}]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",1,{"v":50,"d":"R 50.00"},null,{"$f":"E2276*D2276","v":{"v":50,"d":"R 50.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",1,{"v":50,"d":"R 50.00"},null,{"$f":"E2278*D2278","v":{"v":50,"d":"R 50.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of screed in floors to recieve new screed. ","m²",20,{"v":50,"d":"R 50.00"},null,{"$f":"E2282*D2282","v":{"v":1000,"d":"R 1,000.00"}}]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((4+5)*2)*3.1*2+(5*2.9*2*3)","v":{"v":198.60000000000002,"d":"199"}},{"v":20,"d":"R 20.00"},null,{"v":3972.0000000000005,"d":"R 3,972.00"}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",1,{"v":20,"d":"R 20.00"},null,{"$f":"E2286*D2286","v":{"v":20,"d":"R 20.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2248:G2287)","v":{"v":7522,"d":"R 7,522.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",{"$f":"D2282*1.15","v":23},{"v":280,"d":"R 280.00"},null,{"$f":"E2304*D2304","v":{"v":6440,"d":"R 6,440.00"}}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",5,{"v":65,"d":"R 65.00"},null,{"v":325,"d":"R 325.00"}]
[]
[null,"Narrow and broad flute closers","m",5,{"v":65,"d":"R 65.00"},null,{"v":325,"d":"R 325.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",5,{"v":65,"d":"R 65.00"},null,{"v":325,"d":"R 325.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",20,{"v":25,"d":"R 25.00"},null,{"$f":"E2320*D2320","v":{"v":500,"d":"R 500.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2295:G2321)","v":{"v":7915,"d":"R 7,915.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",10,{"v":110,"d":"R 110.00"},null,{"v":1100,"d":"R 1,100.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",10,{"v":100,"d":"R 100.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",{"$f":"18","v":18},{"v":45,"d":"R 45.00"},null,{"v":810,"d":"R 810.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",1,{"v":2000,"d":"R 2,000.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"TABLES, FITTINGS, ETC (AS PER ARCHITECT'S DETAILS) "]
[]
[null,"Fittings"]
[]
[null,"Wall mounted cupboards comprising approximately 900 x 1800mm high door and","No",1,{"v":5000,"d":"R 5,000.00"}]
[null," frame, 4No. 900 x 900 shelves, all including hinges, brackets, lockset, etc"]
[]
[null,"Ceiling fan","No",1,{"v":5000,"d":"R 5,000.00"}]
[]
[null,"Shelving","item",1,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2326:G2360)","v":{"v":4910,"d":"R 4,910.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",20,{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",20,{"v":250,"d":"R 250.00"},null,{"$f":"E2377*D2377","v":{"v":5000,"d":"R 5,000.00"}}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",1,{"v":650,"d":"R 650.00"},null,{"v":650,"d":"R 650.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",18,{"v":65,"d":"R 65.00"},null,{"v":1170,"d":"R 1,170.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2369:G2387)","v":{"v":6820,"d":"R 6,820.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"Floors","m2",20,{"v":90,"d":"R 90.00"},null,{"$f":"D2395*E2395","v":{"v":1800,"d":"1,800.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2392:G2396)","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",1,{"v":450,"d":"R 450.00"},null,{"$f":"E2404*D2404","v":{"v":450,"d":"R 450.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":5000,"d":"5,000.00"},null,{"$f":"C2406*E2406","v":{"v":5000,"d":"5,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral (KITCHEN)","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",1,{"v":45,"d":"R 45.00"},null,{"v":45,"d":"R 45.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2398:G2418)","v":{"v":5645,"d":"R 5,645.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",{"$f":"D2284","v":{"v":198.60000000000002,"d":"199"}},{"v":75,"d":"R 75.00"},null,{"$f":"E2427*D2427","v":{"v":14895.000000000002,"d":"R 14,895.00"}}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2422:G2430)","v":{"v":15120.000000000002,"d":"R 15,120.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",10,{"v":110,"d":"R 110.00"},null,{"v":1100,"d":"R 1,100.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",10,{"v":100,"d":"R 100.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"Extra for angle","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for stop end","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for outlet for 100mm pipe","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[null,"Extra for eaves or plinth offset","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",1,{"v":4500,"d":"R 4,500.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},null,{"$f":"E2463*D2463","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2435:G2464)","v":{"v":16100,"d":"R 16,100.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",5,{"v":400,"d":"R 400.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2468:G2472)","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"((5+4)*2)*3.1+(4*2.9*2*2)","v":{"v":102.2,"d":"102"}},{"v":70,"d":"R 70.00"},null,{"v":7154,"d":"R 7,154.00"}]
[null,"Ceilings","m2",20,{"v":70,"d":"R 70.00"},null,{"v":1400,"d":"R 1,400.00"}]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"External walls including gypsum coat where necessary","m2",{"$f":"((4+5)*2)*3.1","v":{"v":55.800000000000004,"d":"56"}},{"v":70,"d":"R 70.00"},null,{"$f":"E2488*D2488","v":{"v":3906.0000000000005,"d":"R 3,906.00"}}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D2332+D2338","v":20},{"v":20,"d":"R 20.00"},null,{"v":400,"d":"R 400.00"}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",4,{"v":70,"d":"R 70.00"},null,{"v":280,"d":"R 280.00"}]
[null,"Windows","m2",14,{"v":70,"d":"R 70.00"},null,{"v":980,"d":"R 980.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",4,{"v":70,"d":"R 70.00"},null,{"v":280,"d":"R 280.00"}]
[null,"Cornices, etc not exceeding 300mm girth","m",{"$f":"D2386","v":18},{"v":20,"d":"R 20.00"},null,{"v":360,"d":"R 360.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",{"$f":"D2342","v":18},{"v":20,"d":"R 20.00"},null,{"v":360,"d":"R 360.00"}]
[null,"Doors","m2",4,{"v":70,"d":"R 70.00"},null,{"v":280,"d":"R 280.00"}]
[null,"Fittings, shelves, cupboards, etc ","m2",45,{"v":70,"d":"R 70.00"},null,{"v":3150,"d":"R 3,150.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2481:G2515)","v":{"v":18550,"d":"R 18,550.00"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2522:G2523)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G2288","v":{"v":7522,"d":"R 7,522.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F2322","v":{"v":0,"d":"R 0.00"}},{"$f":"G2322","v":{"v":7915,"d":"R 7,915.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F2361","v":{"v":0,"d":"R 0.00"}},{"$f":"G2361","v":{"v":4910,"d":"R 4,910.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F2388","v":{"v":0,"d":"R 0.00"}},{"$f":"G2388","v":{"v":6820,"d":"R 6,820.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F2397","v":{"v":0,"d":"R 0.00"}},{"$f":"G2397","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F2419","v":{"v":0,"d":"R 0.00"}},{"$f":"G2419","v":{"v":5645,"d":"R 5,645.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F2431","v":{"v":0,"d":"R 0.00"}},{"$f":"G2431","v":{"v":15120.000000000002,"d":"R 15,120.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F2465","v":{"v":0,"d":"R 0.00"}},{"$f":"G2465","v":{"v":16100,"d":"R 16,100.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F2473","v":{"v":0,"d":"R 0.00"}},{"$f":"G2473","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F2516","v":{"v":0,"d":"R 0.00"}},{"$f":"G2516","v":{"v":18550,"d":"R 18,550.00"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F2518","v":{"v":0,"d":"R 0.00"}},{"$f":"G2524","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F2528:F2549)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G2530:G2549)","v":{"v":78860,"d":"R 78,860.00"}}]
[]
[]
[]
[]
[null,"BLOCK 7: 3 NO ABLUTION BLOCKS "]
[null,"Demolition"]
[]
[null,"Breaking down and removing concrete, etc "]
[]
[null,"25mm screeds and prepare surface to receive new tiles","m²",{"$f":"4.5*6*3","v":81},{"v":120,"d":"R 120.00"},null,{"$f":"E2560*D2560","v":{"v":9720,"d":"R 9,720.00"}}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Taking down and removing roofs, floors, panelling,  ceilings, partitions, etc "]
[]
[null,"Ceiling board","m2",{"$f":"D2560","v":81},{"v":50,"d":"R 50.00"},null,{"$f":"E2566*D2566","v":{"v":4050,"d":"R 4,050.00"}}]
[]
[null,"Taking out and removing doors, windows, etc from brickwork and making good"]
[null,"surfaces to receive new"]
[]
[null,"Timber door 813 x 2032mm high","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E2571*D2571","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Fascia boards","m",{"$f":"6*3*2","v":36},{"v":10,"d":"R 10.00"},null,{"$f":"E2575*D2575","v":{"v":360,"d":"R 360.00"}}]
[]
[null,"Roof gutters","m",36,{"v":10,"d":"R 10.00"},null,{"$f":"E2577*D2577","v":{"v":360,"d":"R 360.00"}}]
[]
[null,"Downpipes","m",25,{"v":10,"d":"R 10.00"},null,{"$f":"E2579*D2579","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"VIP type washdown pan complete with seat including making good floors to","No",18,{"v":100,"d":"R 100.00"},null,{"$f":"E2581*D2581","v":{"v":1800,"d":"R 1,800.00"}}]
[null," receive new"]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",3,{"v":50,"d":"R 50.00"},null,{"$f":"E2586*D2586","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"Stays, latches, handles, etc from window steel frame","No",25,{"v":50,"d":"R 50.00"},null,{"$f":"E2588*D2588","v":{"v":1250,"d":"R 1,250.00"}}]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Cleaning walls to recieve paint.","m²",{"$f":"((32+7.3)*2)*3.1+(7.3*2.9*2*3)+((32+7.3)*2)*3.1","v":{"v":614.3399999999999,"d":"614"}},{"v":20,"d":"R 20.00"},null,{"$f":"E2592*D2592","v":{"v":12286.8,"d":"R 12,286.80"}}]
[]
[null,"Cleaning and removing broken glazing, putty and paint to window frames","m²",{"$f":"D2740","v":5},{"v":20,"d":"R 20.00"},null,{"$f":"E2594*D2594","v":{"v":100,"d":"R 100.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2557:G2595)","v":{"v":30476.8,"d":"R 30,476.80"}}]
[]
[null,"NEW WORKS"]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",{"$f":"D2575","v":36},{"v":110,"d":"R 110.00"},null,{"$f":"E2608*D2608","v":{"v":3960,"d":"R 3,960.00"}}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",18,{"v":100,"d":"R 100.00"},null,{"v":1800,"d":"R 1,800.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",131,{"v":45,"d":"R 45.00"},null,{"v":5895,"d":"R 5,895.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed batten door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",4,{"v":2000,"d":"R 2,000.00"},null,{"v":8000,"d":"R 8,000.00"}]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",{"$f":"D2566","v":81},{"v":35,"d":"R 35.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",{"$f":"D2631","v":81},{"v":250,"d":"R 250.00"},null,{"$f":"E2639*D2639","v":{"v":20250,"d":"R 20,250.00"}}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of 6mm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",4,{"v":650,"d":"R 650.00"},null,{"v":2600,"d":"R 2,600.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",123,{"v":65,"d":"R 65.00"},null,{"v":7995,"d":"R 7,995.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2631:G2649)","v":{"v":30845,"d":"R 30,845.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Floors"]
[null,"305 x 305mm non slip ceramic tiles","m2",81,{"v":280,"d":"R 280.00"},null,{"$f":"D2657*E2657","v":{"v":22680,"d":"22,680.00"}}]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2654:G2659)","v":{"v":22680,"d":"R 22,680.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",4,{"v":450,"d":"R 450.00"},null,{"$f":"E2667*D2667","v":{"v":1800,"d":"R 1,800.00"}}]
[]
[null,"Stays, latches, handles, hinges, etc to existing window frames",1,"item",{"v":10000,"d":"10,000.00"},null,{"$f":"C2669*E2669","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",3,{"v":150,"d":"R 150.00"},null,{"v":450,"d":"R 450.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",4,{"v":45,"d":"R 45.00"},null,{"v":180,"d":"R 180.00"}]
[]
[null,"Kimberley-Clark' 405597 or other similar approved lockable toilet roll","No",18,{"v":450,"d":"R 450.00"},null,{"$f":"E2682*D2682","v":{"v":8100,"d":"R 8,100.00"}}]
[null," holder plugged 750mm above floor finish"]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2661:G2684)","v":{"v":20530,"d":"R 20,530.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",{"$f":"D2657","v":81},{"v":75,"d":"R 75.00"},null,{"$f":"E2693*D2693","v":{"v":6075,"d":"R 6,075.00"}}]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls in patches and repairing cracks","m2",20,{"v":75,"d":"R 75.00"},null,{"v":1500,"d":"R 1,500.00"}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2688:G2702)","v":{"v":7800,"d":"R 7,800.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",{"$f":"6*3*2","v":36},{"v":110,"d":"R 110.00"},null,{"v":3960,"d":"R 3,960.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",38,{"v":100,"d":"R 100.00"},null,{"v":3800,"d":"R 3,800.00"}]
[]
[null,"Extra for angle","No",12,{"v":250,"d":"R 250.00"},null,{"v":3000,"d":"R 3,000.00"}]
[null,"Extra for stop end","No",12,{"v":250,"d":"R 250.00"},null,{"v":3000,"d":"R 3,000.00"}]
[null,"Extra for outlet for 100mm pipe","No",12,{"v":250,"d":"R 250.00"},null,{"v":3000,"d":"R 3,000.00"}]
[null,"Extra for eaves or plinth offset","No",12,{"v":250,"d":"R 250.00"},null,{"v":3000,"d":"R 3,000.00"}]
[]
[null,"VIP type washdown pan complete with seat","No",18,{"v":3500,"d":"R 3,500.00"},null,{"$f":"E2722*D2722","v":{"v":63000,"d":"R 63,000.00"}}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",1,{"v":10000,"d":"R 10,000.00"},null,{"$f":"E2732*D2732","v":{"v":10000,"d":"R 10,000.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2707:G2733)","v":{"v":92760,"d":"R 92,760.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",5,{"v":400,"d":"R 400.00"},null,{"v":2000,"d":"R 2,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2737:G2741)","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education) on"]
[]
[null,"Internal walls including gypsum coat where necessary","m2",{"$f":"(((6+4.5)*2)*3.1+(2*2.9*2*4))*3","v":{"v":334.5,"d":"335"}},{"v":70,"d":"R 70.00"},null,{"v":23415,"d":"R 23,415.00"}]
[null,"Ceilings","m2",{"$f":"D2693","v":81},{"v":70,"d":"R 70.00"},null,{"v":5670,"d":"R 5,670.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education) on"]
[]
[null,"Fascias and barge boards","m",{"$f":"D2608+D2614","v":54},{"v":20,"d":"R 20.00"},null,{"v":1080,"d":"R 1,080.00"}]
[]
[null,"Sanding and Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",45,{"v":70,"d":"R 70.00"},null,{"v":3150,"d":"R 3,150.00"}]
[null,"Windows","m2",87,{"v":70,"d":"R 70.00"},null,{"v":6090,"d":"R 6,090.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",50,{"v":70,"d":"R 70.00"},null,{"v":3500,"d":"R 3,500.00"}]
[null,"Cornices, etc not exceeding 300mm girth","m",56,{"v":20,"d":"R 20.00"},null,{"v":1120,"d":"R 1,120.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats varnish on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",56,{"v":20,"d":"R 20.00"},null,{"v":1120,"d":"R 1,120.00"}]
[null,"Doors","m2",50,{"v":70,"d":"R 70.00"},null,{"v":3500,"d":"R 3,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2750:G2777)","v":{"v":48645,"d":"R 48,645.00"}}]
[]
[null,"ELECTRICAL WORKS"]
[]
[null,"Inspect existing works and decommission"]
[]
[null,"Allow for repair of all electrical works","item",1,{"v":20000,"d":"R 20,000.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G2784:G2785)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G2596","v":{"v":30476.8,"d":"R 30,476.80"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F2650","v":{"v":0,"d":"R 0.00"}},{"$f":"G2650","v":{"v":30845,"d":"R 30,845.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F2660","v":{"v":0,"d":"R 0.00"}},{"$f":"G2660","v":{"v":22680,"d":"R 22,680.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F2685","v":{"v":0,"d":"R 0.00"}},{"$f":"G2685","v":{"v":20530,"d":"R 20,530.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F2703","v":{"v":0,"d":"R 0.00"}},{"$f":"G2703","v":{"v":7800,"d":"R 7,800.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F2734","v":{"v":0,"d":"R 0.00"}},{"$f":"G2734","v":{"v":92760,"d":"R 92,760.00"}}]
[]
[null,"GLAZING",{"$nulls":3},{"$f":"F2742","v":{"v":0,"d":"R 0.00"}},{"$f":"G2742","v":{"v":2000,"d":"R 2,000.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F2778","v":{"v":0,"d":"R 0.00"}},{"$f":"G2778","v":{"v":48645,"d":"R 48,645.00"}}]
[]
[null,"ELECTRICAL WORKS",{"$nulls":3},{"$f":"F2780","v":{"v":0,"d":"R 0.00"}},{"$f":"G2786","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F2790:F2808)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G2792:G2808)","v":{"v":225260,"d":"R 225,260.00"}}]
[]
[]
[]
[null,"GENERAL WORKS"]
[]
[null,"PROVISIONAL SUMS",{"$nulls":3},{"$f":"E2815*D2815","v":0},{"$f":"F2815*E2815","v":0}]
[{"$nulls":6},{"$f":"F2816*E2816","v":0}]
[null,"Electrical Works"]
[null,"Provide the sum of R350,000.00 for the electrical selected sub -","PS",1,{"v":350000,"d":"350,000.00"},null,{"$f":"E2818*D2818","v":{"v":350000,"d":"350,000.00"}}]
[null,"contractor",{"$nulls":4},{"$f":"F2819*E2819","v":0}]
[{"$nulls":6},{"$f":"F2820*E2820","v":0}]
[null,"Allow for Profit & Attendance",null,0.1,{"v":350000,"d":"350,000.00"},null,{"$f":"E2821*D2821","v":{"v":35000,"d":"35,000.00"}}]
[]
[null,"Perimeter Fencing"]
[null,"Provide the sum of R245,000.00 for the repair of damaged fence by selected sub -","PS",1,{"$f":"(88+62)*2*650+50000","v":{"v":245000,"d":"245,000.00"}},null,{"$f":"E2824*D2824","v":{"v":245000,"d":"245,000.00"}}]
[null,"contractor. New fence to match the existing",{"$nulls":4},{"$f":"F2825*E2825","v":0}]
[{"$nulls":6},{"$f":"F2826*E2826","v":0}]
[null,"Allow for Profit & Attendance",null,0.1,{"$f":"E2824","v":{"v":245000,"d":"245,000.00"}},null,{"$f":"E2827*D2827","v":{"v":24500,"d":"24,500.00"}}]
[]
[null,"Woodborer Fumigation"]
[null,"Provide the sum of R200,000.00 for Diamond fence","PS",1,{"v":100000,"d":"100,000.00"},null,{"$f":"E2830*D2830","v":{"v":100000,"d":"100,000.00"}}]
[]
[null,"Allow for Profit & Attendance",null,0.1,{"$f":"E2830","v":{"v":100000,"d":"100,000.00"}},null,{"$f":"E2832*D2832","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,"To Summary",{"$nulls":3},{"$f":"SUM(F2818:F2822)","v":0},{"$f":"SUM(G2815:G2833)","v":{"v":764500,"d":"764,500.00"}}]
[]
[]
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[null,"FINAL SUMMARY"]
[]
[null,"PRELIMINARIES",{"$nulls":3},{"v":310000,"d":"310,000.00"},{"v":275000,"d":"275,000.00"}]
[]
[null,"BLOCK 1: 3 CLASSROOM BLOCK",{"$nulls":3},{"$f":"F588","v":{"v":1304662.2,"d":"1,304,662.20"}},{"$f":"G588","v":0}]
[]
[null,"BLOCK 2: HALL",{"$nulls":3},{"$f":"F1108","v":{"v":1279694.2,"d":"1,279,694.20"}},{"$f":"G1108","v":0}]
[]
[null,"BLOCK 3: 3 CLASSROOM BLOCK & 1 STRONG-ROOM",{"$nulls":3},{"$f":"F1523","v":0},{"$f":"G1523","v":{"v":536763.8,"d":"536,763.80"}}]
[]
[null,"BLOCK 4: 4 CLASSROOM BLOCK",{"$nulls":3},{"$f":"F1919","v":0},{"$f":"G1919","v":{"v":533627.6,"d":"533,627.60"}}]
[]
[null,"BLOCK 5: ADMINISTRATION BLOCK",{"$nulls":3},{"$f":"F2241","v":0},{"$f":"G2241","v":{"v":148449.1,"d":"148,449.10"}}]
[]
[null,"BLOCK 6: KITCHEN",{"$nulls":3},{"$f":"F2550","v":0},{"$f":"G2550","v":{"v":78860,"d":"78,860.00"}}]
[]
[null,"BLOCK 7: 3 NO. ABLUTION BLOCKS",{"$nulls":3},{"$f":"F2809","v":0},{"$f":"G2809","v":{"v":225260,"d":"225,260.00"}}]
[]
[null,"PROVISIONAL SUMS",{"$nulls":3},{"$f":"F2834","v":0},{"$f":"G2834","v":{"v":764500,"d":"764,500.00"}}]
[]
[null,"SUB TOTAL",{"$nulls":3},{"$f":"SUM(F2839:F2857)","v":{"v":2894356.4,"d":"2,894,356.40"}},{"$f":"SUM(G2839:G2857)","v":{"v":2562460.5,"d":"2,562,460.50"}},{"$f":"F2858*12%","v":{"v":347322.768,"d":"347,322.77"}},{"$f":"G2858*12%","v":{"v":307495.26,"d":"307,495.26"}}]
[]
[null,"CONTINGENCY @ 10%",{"$nulls":3},{"$f":"F2858*10%","v":{"v":289435.64,"d":"289,435.64"}},{"$f":"G2858*10%","v":{"v":256246.05000000002,"d":"256,246.05"}}]
[]
[null,"SUB TOTAL",{"$nulls":3},{"$f":"F2860+F2858","v":{"v":3183792.04,"d":"3,183,792.04"}},{"$f":"G2860+G2858","v":{"v":2818706.55,"d":"2,818,706.55"}}]
[]
[null,"ADD VAT @ 15%",{"$nulls":3},{"$f":"F2862*15%","v":{"v":477568.806,"d":"477,568.81"}},{"$f":"G2862*15%","v":{"v":422805.9825,"d":"422,805.98"}}]
[]
[null,"GRAND TOTAL",{"$nulls":3},{"$f":"F2864+F2862","v":{"v":3661360.846,"d":"3,661,360.85"}},{"$f":"G2864+G2862","v":{"v":3241512.5324999997,"d":"3,241,512.53"}}]
[]
[null,"CARRIED TO TENDER",{"$nulls":3},{"$f":"G2866+F2866","v":{"v":6902873.3785,"d":"6,902,873.38"}}]

{"sheet":"Blk 8 Toilet","index":5,"n_rows":790,"n_cols":15,"rows_kept":790,"hidden":true}
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[]
["A","STAFF TOILET  -  BLOCK 8"]
[1,"Demolition"]
[null,"Temporary barriers, screens, etc including removal "]
[]
[null,"Existing hoarding with poles","m",null,{"v":80,"d":"R 80.00"},null,{"$f":"E7*D7","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Existing shadecloth hoarding 1,8m high on Bonnox","m",{"$nulls":3},{"$f":"E9*D9","v":{"v":0,"d":"R 0.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[null,"Double gate size 6000 x 1800mm high formed of suitable","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," tubular steel frame filled in with Bonnox fencing and covered"]
[null," with shadecloth including all necessary gate posts, locking"]
[null," mechanism, etc"]
[]
[null,"RELOCATION OF EXISTING STRUCTURES "]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"Half brick wall ","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Carefully disconnect all existing electrical, water and"]
[null," drainage service connections, etc and relocate existing"]
[null," park home including creating a new platform in the new"]
[null," position within the existing site boundary and"]
[null," re-connecting all services complete as per Architect's site"]
[null," plan "]
[]
[null,"Relocate existing Parking Home 9 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 14,5 x 7 x 3m high wide ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 28 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Breaking up and removing reinforced concrete including"]
[null," cutting off and removing reinforcement and cart away to a"]
[null," dumping site to be located by the contractor "]
[]
[null,"100mm Thick surface bed","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Taking out and removing doors, windows, etc from"]
[null," brickwork to be demolished "]
[]
[null,"Glazed steel window not exceeding 2,5m2","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Taking down and removing roofs, floors, panelling,"]
[null," ceilings, partitions, etc "]
[]
[null,"Asbestors/metal roof covering including fascias and bardgeboards","m2",13,{"v":50,"d":"R 50.00"},null,{"v":650,"d":"R 650.00"}]
[null," and rainwater goods adn dispose off as per the SHE"]
[null," regulations. "]
[]
[null,"Wooden floors tiles including skirting, joints, bearers etc","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Gypsum plasterboard ceilings, including cornices, timber","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brandering, etc "]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber door 1610 x 2032mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Timber door 910 x 2032mm high","No",3,{"v":150,"d":"R 150.00"},null,{"v":450,"d":"R 450.00"}]
[]
[null,"Taking up and removing vinyl floor coverings, carpeting,"]
[null," etc "]
[]
[null,"Vinyl tile floor covering including preparing screed for new vinyl","m²",{"$nulls":3},{"$f":"E73*D73","v":{"v":0,"d":"R 0.00"}}]
[null," floor covering "]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Take out and remove mirror and replace with new.","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Roof trusses including purlins","No",null,{"v":50,"d":"R 50.00"},null,{"$f":"E82*D82","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Fascia boards","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E84*D84","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Roof gutters","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E86*D86","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Downpipes","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E88*D88","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Taking  out and removing piping, sanitary fittings, etc"]
[null," including disconnecting  piping  from fittings  and  making"]
[null," good floor and wall finishes (making good tiling and"]
[null," paintwork elsewhere) "]
[]
[null,"50mm Cast iron piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Copper piping not exceeding 50mm dia including fittings and","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brackets"]
[]
[null,"100mm PVC piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Piping exceeding 150mm and not exceeding 200mm.","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china wash hand basin ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china WC pan with cistern ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Stainless steel urinal including breaking up and removing","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," concrete urinal step."]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of plaster in walls to recieve new all tiles. (Tiles","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," elesewhere measured)"]
[{"$nulls":10},17,17,null,{"$f":"L115+K115","v":34}]
[null,"Chipping of screed in floors to recieve new screed. ","m²",13,{"v":50,"d":"R 50.00"},null,{"v":650,"d":"R 650.00"},{"$nulls":3},8,8,8,{"$f":"M116+L116+K116","v":24}]
[{"$nulls":13},{"$f":"N115+N116","v":58}]
[null,"Cleaning walls to recieve paint.","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"},{"$nulls":6},{"$f":"N117*2","v":116}]
[{"$nulls":13},{"$f":"N118*3","v":348}]
[null,"Walls in patches ","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"OPENINGS THROUGH EXISTING WALLS ETC "]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new doors and frames including necessary precast"]
[null," concrete lintels and making good plaster on both sides"]
[null," and into reveals (new doors and frames and making good"]
[null," paintwork elsewhere) "]
[]
[null,"Opening for door with Aluminium frame 2032 x 900mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," overall through 230mm brick wall."]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new windows including necessary precast concrete"]
[null," lintels and making good plaster on one side and into"]
[null," reveals and face brickwork on other side and into reveals"]
[null," and with 230mm Wide facebrick sill set sloping and slightly"]
[null," projecting on outside and flat plastered sill on inside (new"]
[null," windows and making good paintwork elsewhere) "]
[]
[null,"Opening for window 600 x 654mm high through one brick wall","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"MAKING GOOD OF FINISHES ETC "]
[]
[null,"Making good brickwork to face of wall where half brick have","m",{"$nulls":3},{"$f":"E145*D145","v":{"v":0,"d":"R 0.00"}}]
[null," been demolished."]
[]
[null,"Making good brickwork to face of wall where one brickwall was","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," removed"]
[]
[null,"Carefully inspect timber roof structure, report findings to"]
[null," Representative/Agent and repair as instructed by cutting"]
[null," out rotten or damaged timber, inserting new like sized and"]
[null," graded timber and joining old to new timber as described "]
[]
[null,"Allow the net sum of R…………………………. (………….. Rand) for the ","Item",1,null,null,{"v":0,"d":"R 0.00"}]
[null,"inspection of timber roof structure on plan by a registered"]
[null," entomologist"]
[]
[null,"Carefully inspect, repair and make good existing roof"]
[null," coverings and other related elements "]
[]
[null,"Inspect existing IRB roofsheeting, refix or replace any damaged","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," areas with new to match existing"]
[]
[null,"Clean with a high pressure cleaner to remove stains,"]
[null," marks, algae, etc "]
[]
[null,"IBR roof sheeting covering with a pitch not exceeding 25⁰","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G5:G170)","v":{"v":1750,"d":"R 1,750.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"EARTHWORKS"]
[]
[null,"Site clearance"]
[null,"Digging up and removing rubbish, debris, vegetation, hedges,"]
[null,"shrubs and trees not exceeding 200mm girth, bush, etc","m2",null,{"v":15,"d":"R 15.00"},null,{"$f":"E179*D179","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Stripping average 100mm thick layer of top soil and stockpiling"]
[null,"on site","m2",null,{"v":25,"d":"R 25.00"},null,{"$f":"E182*D182","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"EXCAVATIONS"]
[]
[null,"Open face excavation to reduce levels \"cut to fill'","m3",3,{"v":50,"d":"R 50.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[null,"Trenches for V-drains","m3",4,{"v":50,"d":"R 50.00"},null,{"v":200,"d":"R 200.00"},null,null,34,20,{"$f":"K189+J189","v":54},0.6,0.7,{"$f":"N189*M189*L189","v":22.68}]
[{"$nulls":14},{"$f":"O189*2","v":45.36}]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in",{"$nulls":9},54,0.6,{"$f":"M192*L192","v":32.4}]
[null,"Soft rock","m3",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Hard rock","m3",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Risk of collapse of excavations"]
[null,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",13,{"v":45,"d":"R 45.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":200,"d":"R 200.00"},null,{"v":200,"d":"R 200.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[null,"Under floors, steps, pavings, etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Backfilling to trenches, holes, etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[null,"Under floors etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Compaction of surfaces"]
[null,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",13,{"v":45,"d":"R 45.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming","m2",13,{"v":20,"d":"R 20.00"},null,{"v":260,"d":"R 260.00"}]
[]
[null,"To bottoms and sides of trenches etc","m2",13,{"v":20,"d":"R 20.00"},null,{"v":260,"d":"R 260.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G179:G234)","v":{"v":2640,"d":"R 2,640.00"}}]
[]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"$f":"E244*D244","v":{"v":0,"d":"R 0.00"}}]
[{"$nulls":10},54,0.6,0.25,{"$f":"M245*L245*K245","v":8.1}]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",3,{"v":1800,"d":"R 1,800.00"},null,{"v":5400,"d":"R 5,400.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Slab to cover pit","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TEST BLOCKS",{"$nulls":8},54,{"$f":"K258/2.4","v":22.5},{"$f":"L258*0.6","v":13.5}]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[{"$nulls":10},54,0.6,{"$f":"L261*K261","v":32.4}]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",10,{"v":45,"d":"R 45.00"},null,{"v":450,"d":"R 450.00"}]
[]
[null,"Rough formwork to sides"]
[]
[null,"pit slabs propped up exceeding 1,5m and not exceeding 3.5m"]
[null,"high, including removal from confined area.","m2",16,{"v":65,"d":"R 65.00"},null,{"v":1040,"d":"R 1,040.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",4,{"v":15,"d":"R 15.00"},null,{"v":60,"d":"R 60.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",4,{"v":15,"d":"R 15.00"},null,{"v":60,"d":"R 60.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",4,{"v":15,"d":"R 15.00"},null,{"v":60,"d":"R 60.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"10mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"8mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",10,{"v":145,"d":"R 145.00"},null,{"v":1450,"d":"R 1,450.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G243:G305)","v":{"v":8670,"d":"R 8,670.00"}}]
[]
[]
[]
[null,"PRECAST CONCRETE"]
[]
[null,"450 x 450 x Precast concrete inspection chamber covers","No",{"$nulls":3},{"$f":"E312*D312","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Joint sealants"]
[]
[null,"Stalton or similar and approved prestressed fabricated"]
[null,"lintels:"]
[]
[null,"110 x 75mm Lintels in lengths not exceeding 3m.","No",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G311:G320)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"MASONRY"]
[]
[null,"FOUNDATIONS"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive"]
[null,"strength) in class 1 mortar including galvanised crimp wire"]
[null,"wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Half brick walls in beamfilling","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"On brick walls, piers, etc","m2",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Brickwork reinforcement","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Turning pieces"]
[null,"150mm Wide turning piece to lintels etc","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"FACE BRICKWORK"]
[null,"Corobrik FBA face bricks pointed with recessed"]
[null,"horizontal and vertical joints"]
[null,"Extra over brickwork for face brickwork","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Extra over brickwork for brick-on-edge header course lintel","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Brick-on-edge header course copings, sills, etc., of"]
[null,"Corobrik Firelight Travertine FBX face bricks pointed"]
[null,"with recessed joints on all exposed faces"]
[]
[null,"220mm wide window sill set sloping and slightly projecting"]
[null,"(refer architect's specification","m",null,{"v":85,"d":"R 85.00"},null,{"$f":"E374*D374","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection"]
[]
[]
[null,"WATERPROOFING"]
[]
[null,"One layer of 375 micron \"Consol Plastics Brikgrip DPC\""]
[null,"embossed damp proof course"]
[null,"dpc - In walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One layer of 250 micron \"Consol Plastics Gunplas USB"]
[null,"Green\" waterproof sheeting sealed at laps with \"Gunplas"]
[null,"Pressure Sensitive Tape\""]
[]
[null,"Under surface beds","m2",13,{"v":25,"d":"R 25.00"},null,{"v":325,"d":"R 325.00"}]
[]
[null,"Two coats of \"Brixeal\" or similar and approved bitumen"]
[null,"waterproofing compound:"]
[null,"On walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"JOINT SEALANTS ETC"]
[]
[null,"Silicone rubber base sealing compound"]
[null,"In joints between frames and walls","m",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Polysulphide sealant including backing cord, bond",{"$nulls":7},2.4]
[null,"breaker, primer, etc"]
[]
[null,"10 x 10mm in expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[null,"12 x 10mm expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G381:G405)","v":{"v":325,"d":"R 325.00"}}]
[]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",16,{"v":350,"d":"R 350.00"},null,{"v":5600,"d":"R 5,600.00"}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Narrow and broad flute closers","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",14,{"v":25,"d":"R 25.00"},null,{"$f":"E437*D437","v":{"v":350,"d":"R 350.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G412:G438)","v":{"v":5950,"d":"R 5,950.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",9,{"v":65,"d":"R 65.00"},null,{"v":585,"d":"R 585.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in lenght, to"]
[null,"manufacturer's specification","m",25,{"v":85,"d":"R 85.00"},null,{"v":2125,"d":"R 2,125.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",12,{"v":25,"d":"R 25.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 10848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",null,{"v":2500,"d":"R 2,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"related items"]
[]
[null,"Lean to prefabricated plate nailed roof"]
[null,"truss spanning approximately 10848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",6,{"v":1200,"d":"R 1,200.00"},null,{"v":7200,"d":"R 7,200.00"}]
[]
[null,"Double pitched prefabricated plate nailed roof truss spanning"]
[null,"approximately 8970mm and 1689mm high, truss to be hoisted"]
[null,"and fixed approximately 4m above ground level as per","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacture's details.The description includes all related items."]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",10,{"v":110,"d":"R 110.00"},null,{"v":1100,"d":"R 1,100.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",6,{"v":100,"d":"R 100.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed double door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",null,{"v":2000,"d":"R 2,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Solid flush panel doors"]
[null,"44mm (D3) Solid flush panel hollow core doors with approved"]
[null,"hardwood veneer on both sides and two hardwood edge strips"]
[null,"hung to steel frames, size 813 x 2032mm high.Refer Architect's","No",3,{"v":1200,"d":"R 1,200.00"},null,{"v":3600,"d":"R 3,600.00"}]
[null,"Schedule"]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards","No",null,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E507*D507","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Chalk boards (2420mm x 1230mm)","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"WHITE BOARDS"]
[null,"'Vitrex Execuboard' magnetic whiteboard with aluminium"]
[null,"surround fixed 3 no. times at the top and bottom with"]
[null,"aluminium brackets, sleeve and screw"]
[]
[null,"2400 x 1140mm Whiteboards","No",null,{"v":0,"d":"R 0.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TABLES (AS PER ARCHITECT'S DETAILS)"]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G443:G520)","v":{"v":15510,"d":"R 15,510.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS"]
[null,"AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of Xmm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",null,{"v":650,"d":"R 650.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G526:G548)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[]
[null,null,"m2",null,{"v":280,"d":"R 280.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G553:G557)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"100mm Galvanised steel loose-pin hinges welded in position as"]
[null,"per architect's specification","No",9,{"v":250,"d":"R 250.00"},null,{"v":2250,"d":"R 2,250.00"}]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":450,"d":"R 450.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Five lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",3,{"v":550,"d":"R 550.00"},null,{"$f":"E571*D571","v":{"v":1650,"d":"R 1,650.00"}}]
[]
[null,"Seven lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"4mm Perspex signs painted white on back with letters and"]
[null,"numerals reverse engraved and painted black"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G559:G589)","v":{"v":4050,"d":"R 4,050.00"}}]
[]
[null,"METALWORK"]
[]
[null,"STEEL HANDRAILS, BALUSTRADES, ETC"]
[]
[null,"100mm diameter galvanised steel posts on the veranda, with"]
[null,"an extreme height of 2600mm (Including connecting brackets"]
[null,"and all other related items, as per engineer's details).","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL DOOR FRAMES"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls"]
[]
[null,"Frame for door 877 x 2032 mm high","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls"]
[null,"complete with straps for building in"]
[]
[null,"Frame for door size 813 x 2032 mm high","No",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL WINDOWS, LOUVRES,"]
[null,"DOORS,etc"]
[]
[null,"Window (SS32) Size 987 x 978 mm high - as per Architect's"]
[null,"Specification. Making good to existing","No",null,{"v":500,"d":"R 500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"STEEL ROLLER SHUTTERS ETC"]
[]
[null,"Galvanised hot dipped mild steel"]
[]
[null,"Door Gate (G1) size 813 x 2032 mm high, including handles,"]
[null,"lockset and hinges, as per Architect's Specification or","No",null,{"v":1500,"d":"R 1,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacturer's detail"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[null,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",null,{"v":35000,"d":"R 35,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Double ended strongroom ventilator","No",null,{"v":1500,"d":"R 1,500.00"},null,{"$f":"E634*D634","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G593:G635)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",10,{"v":75,"d":"R 75.00"},null,{"v":750,"d":"R 750.00"}]
[]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls","m2",132,{"v":75,"d":"R 75.00"},null,{"v":9900,"d":"R 9,900.00"}]
[]
[null,"On narrow widths","m2",2,{"v":75,"d":"R 75.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G639:G654)","v":{"v":10800,"d":"R 10,800.00"}}]
[]
[null,"TILING"]
[]
[null,"FLOOR TILING"]
[]
[null,"300 x 300 x 2.5mm Johnson ceramic floor tiles with all the adhesive"]
[null,"On floors","m2",10,{"v":280,"d":"R 280.00"},null,{"v":2800,"d":"R 2,800.00"}]
[]
[null,"Tile skirting","m",28,{"v":150,"d":"R 150.00"},null,{"v":4200,"d":"R 4,200.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G658:G665)","v":{"v":7000,"d":"R 7,000.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",5,{"v":110,"d":"R 110.00"},null,{"v":550,"d":"R 550.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",3,{"v":100,"d":"R 100.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"Extra for angle","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for stop end","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for outlet for 100mm pipe","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for eaves or plinth offset","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Vaal"]
[null,"Aquasave duct type wc pan as per Architect's Specification,"]
[null,"including forming opening through the concrete slab.","No",3,{"v":2000,"d":"R 2,000.00"},null,{"$f":"E690*D690","v":{"v":6000,"d":"R 6,000.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No"]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",null,{"v":10000,"d":"R 10,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G670:G709)","v":{"v":7850,"d":"R 7,850.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",null,{"v":200,"d":"R 200.00"},null,{"$f":"E716*D716","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G713:G717)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education)"]
[]
[null,"Internal walls","m2",132,{"v":90,"d":"R 90.00"},null,{"v":11880,"d":"R 11,880.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education)"]
[null,"Fascias and barge boards","m",46,{"v":20,"d":"R 20.00"},null,{"v":920,"d":"R 920.00"}]
[]
[null,"Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",3,{"v":90,"d":"R 90.00"},null,{"v":270,"d":"R 270.00"}]
[null,"Windows","m2",null,{"v":90,"d":"R 90.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",10,{"v":90,"d":"R 90.00"},null,{"v":900,"d":"R 900.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats super universal enamel paint on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G725:G749)","v":{"v":13970,"d":"R 13,970.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G171","v":{"v":1750,"d":"R 1,750.00"}}]
[]
[null,"EARTHWORK",{"$nulls":3},{"$f":"F235","v":{"v":0,"d":"R 0.00"}},{"$f":"G235","v":{"v":2640,"d":"R 2,640.00"}}]
[]
[null,"CONCRETE, FORMWORK, REINFORCEMENT",{"$nulls":3},{"$f":"F306","v":{"v":0,"d":"R 0.00"}},{"$f":"G306","v":{"v":8670,"d":"R 8,670.00"}}]
[]
[null,"PRECAST CONCRETE",{"$nulls":3},{"$f":"F321","v":{"v":0,"d":"R 0.00"}},{"$f":"G321","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F376","v":{"v":0,"d":"R 0.00"}},{"$f":"G376","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"WATERPROOFING",{"$nulls":3},{"$f":"F406","v":{"v":0,"d":"R 0.00"}},{"$f":"G406","v":{"v":325,"d":"R 325.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F439","v":{"v":0,"d":"R 0.00"}},{"$f":"G439","v":{"v":5950,"d":"R 5,950.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F521","v":{"v":0,"d":"R 0.00"}},{"$f":"G521","v":{"v":15510,"d":"R 15,510.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F549","v":{"v":0,"d":"R 0.00"}},{"$f":"G549","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F558","v":{"v":0,"d":"R 0.00"}},{"$f":"G558","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F590","v":{"v":0,"d":"R 0.00"}},{"$f":"G590","v":{"v":4050,"d":"R 4,050.00"}}]
[]
[null,"METAL WORKS",{"$nulls":3},{"$f":"F636","v":{"v":0,"d":"R 0.00"}},{"$f":"G636","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F655","v":{"v":0,"d":"R 0.00"}},{"$f":"G655","v":{"v":10800,"d":"R 10,800.00"}}]
[]
[null,"TILING",{"$nulls":3},{"$f":"F666","v":{"v":0,"d":"R 0.00"}},{"$f":"G666","v":{"v":7000,"d":"R 7,000.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F710","v":{"v":0,"d":"R 0.00"}},{"$f":"G710","v":{"v":7850,"d":"R 7,850.00"}}]
[]
[null,"GALZING",{"$nulls":3},{"$f":"F718","v":{"v":0,"d":"R 0.00"}},{"$f":"G718","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F750","v":{"v":0,"d":"R 0.00"}},{"$f":"G750","v":{"v":13970,"d":"R 13,970.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F757:F789)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G757:G789)","v":{"v":76765,"d":"R 76,765.00"}}]

{"sheet":"Blk 10 leaners Toilet","index":6,"n_rows":790,"n_cols":15,"rows_kept":790,"hidden":true}
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[]
["A","LEANERS TOILET  -  BLOCK 10"]
[1,"Demolition"]
[null,"Temporary barriers, screens, etc including removal "]
[]
[null,"Existing hoarding with poles","m",null,{"v":80,"d":"R 80.00"},null,{"$f":"E7*D7","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Existing shadecloth hoarding 1,8m high on Bonnox","m",{"$nulls":3},{"$f":"E9*D9","v":{"v":0,"d":"R 0.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[null,"Double gate size 6000 x 1800mm high formed of suitable","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," tubular steel frame filled in with Bonnox fencing and covered"]
[null," with shadecloth including all necessary gate posts, locking"]
[null," mechanism, etc"]
[]
[null,"RELOCATION OF EXISTING STRUCTURES "]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"Half brick wall ","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Carefully disconnect all existing electrical, water and"]
[null," drainage service connections, etc and relocate existing"]
[null," park home including creating a new platform in the new"]
[null," position within the existing site boundary and"]
[null," re-connecting all services complete as per Architect's site"]
[null," plan "]
[]
[null,"Relocate existing Parking Home 9 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 14,5 x 7 x 3m high wide ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 28 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Breaking up and removing reinforced concrete including"]
[null," cutting off and removing reinforcement and cart away to a"]
[null," dumping site to be located by the contractor "]
[]
[null,"100mm Thick surface bed","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Taking out and removing doors, windows, etc from"]
[null," brickwork to be demolished "]
[]
[null,"Glazed steel window not exceeding 2,5m2","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Taking down and removing roofs, floors, panelling,"]
[null," ceilings, partitions, etc "]
[]
[null,"Asbestors/metal roof covering including fascias and bardgeboards","m2",36,{"v":50,"d":"R 50.00"},null,{"v":1800,"d":"R 1,800.00"}]
[null," and rainwater goods adn dispose off as per the SHE"]
[null," regulations. "]
[]
[null,"Wooden floors tiles including skirting, joints, bearers etc","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Gypsum plasterboard ceilings, including cornices, timber","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brandering, etc "]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber door 1610 x 2032mm high","No"]
[]
[null,"Timber door 910 x 2032mm high","No",8,{"v":150,"d":"R 150.00"},null,{"v":1200,"d":"R 1,200.00"}]
[]
[null,"Taking up and removing vinyl floor coverings, carpeting,"]
[null," etc "]
[]
[null,"Vinyl tile floor covering including preparing screed for new vinyl","m²"]
[null," floor covering "]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",null,{"v":50,"d":"R 50.00"},null,{"$f":"E78*D78","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Take out and remove mirror and replace with new.","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Roof trusses including purlins","No",null,{"v":50,"d":"R 50.00"},null,{"$f":"E82*D82","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Fascia boards","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E84*D84","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Roof gutters","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E86*D86","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Downpipes","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E88*D88","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Taking  out and removing piping, sanitary fittings, etc"]
[null," including disconnecting  piping  from fittings  and  making"]
[null," good floor and wall finishes (making good tiling and"]
[null," paintwork elsewhere) "]
[]
[null,"50mm Cast iron piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Copper piping not exceeding 50mm dia including fittings and","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brackets"]
[]
[null,"100mm PVC piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Piping exceeding 150mm and not exceeding 200mm.","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china wash hand basin ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china WC pan with cistern ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Stainless steel urinal including breaking up and removing","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," concrete urinal step."]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of plaster in walls to recieve new all tiles. (Tiles","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," elesewhere measured)"]
[{"$nulls":10},17,17,null,{"$f":"L115+K115","v":34}]
[null,"Chipping of screed in floors to recieve new screed. ","m²",36,{"v":50,"d":"R 50.00"},null,{"v":1800,"d":"R 1,800.00"},{"$nulls":3},8,8,8,{"$f":"M116+L116+K116","v":24}]
[{"$nulls":13},{"$f":"N115+N116","v":58}]
[null,"Cleaning walls to recieve paint.","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"},{"$nulls":6},{"$f":"N117*2","v":116}]
[{"$nulls":13},{"$f":"N118*3","v":348}]
[null,"Walls in patches ","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"OPENINGS THROUGH EXISTING WALLS ETC "]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new doors and frames including necessary precast"]
[null," concrete lintels and making good plaster on both sides"]
[null," and into reveals (new doors and frames and making good"]
[null," paintwork elsewhere) "]
[]
[null,"Opening for door with Aluminium frame 2032 x 900mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," overall through 230mm brick wall."]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new windows including necessary precast concrete"]
[null," lintels and making good plaster on one side and into"]
[null," reveals and face brickwork on other side and into reveals"]
[null," and with 230mm Wide facebrick sill set sloping and slightly"]
[null," projecting on outside and flat plastered sill on inside (new"]
[null," windows and making good paintwork elsewhere) "]
[]
[null,"Opening for window 600 x 654mm high through one brick wall","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"MAKING GOOD OF FINISHES ETC "]
[]
[null,"Making good brickwork to face of wall where half brick have","m",{"$nulls":3},{"$f":"E145*D145","v":{"v":0,"d":"R 0.00"}}]
[null," been demolished."]
[]
[null,"Making good brickwork to face of wall where one brickwall was","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," removed"]
[]
[null,"Carefully inspect timber roof structure, report findings to"]
[null," Representative/Agent and repair as instructed by cutting"]
[null," out rotten or damaged timber, inserting new like sized and"]
[null," graded timber and joining old to new timber as described "]
[]
[null,"Allow the net sum of R…………………………. (………….. Rand) for the ","Item",1,null,null,{"v":0,"d":"R 0.00"}]
[null,"inspection of timber roof structure on plan by a registered"]
[null," entomologist"]
[]
[null,"Carefully inspect, repair and make good existing roof"]
[null," coverings and other related elements "]
[]
[null,"Inspect existing IRB roofsheeting, refix or replace any damaged","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," areas with new to match existing"]
[]
[null,"Clean with a high pressure cleaner to remove stains,"]
[null," marks, algae, etc "]
[]
[null,"IBR roof sheeting covering with a pitch not exceeding 25⁰","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G5:G170)","v":{"v":4800,"d":"R 4,800.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"EARTHWORKS"]
[]
[null,"Site clearance"]
[null,"Digging up and removing rubbish, debris, vegetation, hedges,"]
[null,"shrubs and trees not exceeding 200mm girth, bush, etc","m2",null,{"v":15,"d":"R 15.00"},null,{"$f":"E179*D179","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Stripping average 100mm thick layer of top soil and stockpiling"]
[null,"on site","m2",30,{"v":25,"d":"R 25.00"},null,{"$f":"E182*D182","v":{"v":750,"d":"R 750.00"}}]
[]
[null,"EXCAVATIONS"]
[]
[null,"Open face excavation to reduce levels \"cut to fill'","m3",15,{"v":50,"d":"R 50.00"},null,{"v":750,"d":"R 750.00"}]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[null,"Trenches for V-drains","m3",15,{"v":50,"d":"R 50.00"},null,{"v":750,"d":"R 750.00"},null,null,34,20,{"$f":"K189+J189","v":54},0.6,0.7,{"$f":"N189*M189*L189","v":22.68}]
[{"$nulls":14},{"$f":"O189*2","v":45.36}]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in",{"$nulls":9},54,0.6,{"$f":"M192*L192","v":32.4}]
[null,"Soft rock","m3",2,{"v":150,"d":"R 150.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"Hard rock","m3",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",null,{"v":50,"d":"R 50.00"}]
[]
[null,"Risk of collapse of excavations"]
[null,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",18,{"v":45,"d":"R 45.00"},null,{"v":810,"d":"R 810.00"}]
[]
[null,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":400,"d":"R 400.00"},null,{"v":400,"d":"R 400.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[null,"Under floors, steps, pavings, etc","m3",7,{"v":350,"d":"R 350.00"},null,{"v":2450,"d":"R 2,450.00"}]
[]
[null,"Backfilling to trenches, holes, etc","m3",3,{"v":350,"d":"R 350.00"},null,{"v":1050,"d":"R 1,050.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[null,"Under floors etc","m3",7,{"v":350,"d":"R 350.00"},null,{"v":2450,"d":"R 2,450.00"}]
[]
[null,"Compaction of surfaces"]
[null,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",15,{"v":45,"d":"R 45.00"},null,{"v":675,"d":"R 675.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming","m2",15,{"v":20,"d":"R 20.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"To bottoms and sides of trenches etc","m2",15,{"v":20,"d":"R 20.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G179:G234)","v":{"v":11235,"d":"R 11,235.00"}}]
[]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"$f":"E244*D244","v":{"v":0,"d":"R 0.00"}}]
[{"$nulls":10},54,0.6,0.25,{"$f":"M245*L245*K245","v":8.1}]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",4,{"v":1800,"d":"R 1,800.00"},null,{"v":7200,"d":"R 7,200.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Slab to cover pit","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TEST BLOCKS",{"$nulls":8},54,{"$f":"K258/2.4","v":22.5},{"$f":"L258*0.6","v":13.5}]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",2,{"v":150,"d":"R 150.00"},null,{"v":300,"d":"R 300.00"}]
[{"$nulls":10},54,0.6,{"$f":"L261*K261","v":32.4}]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",15,{"v":45,"d":"R 45.00"},null,{"v":675,"d":"R 675.00"}]
[]
[null,"Rough formwork to sides"]
[]
[null,"pit slabs propped up exceeding 1,5m and not exceeding 3.5m"]
[null,"high, including removal from confined area.","m2",24,{"v":65,"d":"R 65.00"},null,{"v":1560,"d":"R 1,560.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",6,{"v":15,"d":"R 15.00"},null,{"v":90,"d":"R 90.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",6,{"v":15,"d":"R 15.00"},null,{"v":90,"d":"R 90.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",6,{"v":15,"d":"R 15.00"},null,{"v":90,"d":"R 90.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"10mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"8mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",15,{"v":145,"d":"R 145.00"},null,{"v":2175,"d":"R 2,175.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G243:G305)","v":{"v":12180,"d":"R 12,180.00"}}]
[]
[]
[]
[null,"PRECAST CONCRETE"]
[]
[null,"450 x 450 x Precast concrete inspection chamber covers","No",{"$nulls":3},{"$f":"E312*D312","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Joint sealants"]
[]
[null,"Stalton or similar and approved prestressed fabricated"]
[null,"lintels:"]
[]
[null,"110 x 75mm Lintels in lengths not exceeding 3m.","No",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G311:G320)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"MASONRY"]
[]
[null,"FOUNDATIONS"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive"]
[null,"strength) in class 1 mortar including galvanised crimp wire"]
[null,"wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Half brick walls in beamfilling","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"On brick walls, piers, etc","m2",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Brickwork reinforcement","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Turning pieces"]
[null,"150mm Wide turning piece to lintels etc","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"FACE BRICKWORK"]
[null,"Corobrik FBA face bricks pointed with recessed"]
[null,"horizontal and vertical joints"]
[null,"Extra over brickwork for face brickwork","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Extra over brickwork for brick-on-edge header course lintel","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Brick-on-edge header course copings, sills, etc., of"]
[null,"Corobrik Firelight Travertine FBX face bricks pointed"]
[null,"with recessed joints on all exposed faces"]
[]
[null,"220mm wide window sill set sloping and slightly projecting"]
[null,"(refer architect's specification","m",null,{"v":85,"d":"R 85.00"},null,{"$f":"E374*D374","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection"]
[]
[]
[null,"WATERPROOFING"]
[]
[null,"One layer of 375 micron \"Consol Plastics Brikgrip DPC\""]
[null,"embossed damp proof course"]
[null,"dpc - In walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One layer of 250 micron \"Consol Plastics Gunplas USB"]
[null,"Green\" waterproof sheeting sealed at laps with \"Gunplas"]
[null,"Pressure Sensitive Tape\""]
[]
[null,"Under surface beds","m2",15,{"v":25,"d":"R 25.00"},null,{"v":375,"d":"R 375.00"}]
[]
[null,"Two coats of \"Brixeal\" or similar and approved bitumen"]
[null,"waterproofing compound:"]
[null,"On walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"JOINT SEALANTS ETC"]
[]
[null,"Silicone rubber base sealing compound"]
[null,"In joints between frames and walls","m",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Polysulphide sealant including backing cord, bond",{"$nulls":7},2.4]
[null,"breaker, primer, etc"]
[]
[null,"10 x 10mm in expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[null,"12 x 10mm expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G381:G405)","v":{"v":375,"d":"R 375.00"}}]
[]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",52,{"v":350,"d":"R 350.00"},null,{"v":18200,"d":"R 18,200.00"}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Narrow and broad flute closers","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",36,{"v":25,"d":"R 25.00"},null,{"$f":"E437*D437","v":{"v":900,"d":"R 900.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G412:G438)","v":{"v":19100,"d":"R 19,100.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",24,{"v":65,"d":"R 65.00"},null,{"v":1560,"d":"R 1,560.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in lenght, to"]
[null,"manufacturer's specification","m",60,{"v":85,"d":"R 85.00"},null,{"v":5100,"d":"R 5,100.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",50,{"v":25,"d":"R 25.00"},null,{"v":1250,"d":"R 1,250.00"}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 10848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",null,{"v":2500,"d":"R 2,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"related items"]
[]
[null,"Lean to prefabricated plate nailed roof"]
[null,"truss spanning approximately 12848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",4,{"v":1200,"d":"R 1,200.00"},null,{"v":4800,"d":"R 4,800.00"}]
[]
[null,"Double pitched prefabricated plate nailed roof truss spanning"]
[null,"approximately 8970mm and 1689mm high, truss to be hoisted"]
[null,"and fixed approximately 4m above ground level as per","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacture's details.The description includes all related items."]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",24,{"v":110,"d":"R 110.00"},null,{"v":2640,"d":"R 2,640.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",6,{"v":100,"d":"R 100.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed double door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",null,{"v":2000,"d":"R 2,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Solid flush panel doors"]
[null,"44mm (D3) Solid flush panel hollow core doors with approved"]
[null,"hardwood veneer on both sides and two hardwood edge strips"]
[null,"hung to steel frames, size 813 x 2032mm high.Refer Architect's","No",8,{"v":1200,"d":"R 1,200.00"},null,{"v":9600,"d":"R 9,600.00"}]
[null,"Schedule"]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards","No",null,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E507*D507","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Chalk boards (2420mm x 1230mm)","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"WHITE BOARDS"]
[null,"'Vitrex Execuboard' magnetic whiteboard with aluminium"]
[null,"surround fixed 3 no. times at the top and bottom with"]
[null,"aluminium brackets, sleeve and screw"]
[]
[null,"2400 x 1140mm Whiteboards","No",null,{"v":0,"d":"R 0.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TABLES (AS PER ARCHITECT'S DETAILS)"]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G443:G520)","v":{"v":25550,"d":"R 25,550.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS"]
[null,"AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of Xmm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",null,{"v":650,"d":"R 650.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G526:G548)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[]
[null,null,"m2",null,{"v":280,"d":"R 280.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G553:G557)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"100mm Galvanised steel loose-pin hinges welded in position as"]
[null,"per architect's specification","No",16,{"v":250,"d":"R 250.00"},null,{"v":4000,"d":"R 4,000.00"}]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",8,{"v":450,"d":"R 450.00"},null,{"v":3600,"d":"R 3,600.00"}]
[]
[null,"Five lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":550,"d":"R 550.00"},null,{"$f":"E571*D571","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Seven lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"4mm Perspex signs painted white on back with letters and"]
[null,"numerals reverse engraved and painted black"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G559:G589)","v":{"v":7750,"d":"R 7,750.00"}}]
[]
[null,"METALWORK"]
[]
[null,"STEEL HANDRAILS, BALUSTRADES, ETC"]
[]
[null,"100mm diameter galvanised steel posts on the veranda, with"]
[null,"an extreme height of 2600mm (Including connecting brackets"]
[null,"and all other related items, as per engineer's details).","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL DOOR FRAMES"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls"]
[]
[null,"Frame for door 877 x 2032 mm high","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls"]
[null,"complete with straps for building in"]
[]
[null,"Frame for door size 813 x 2032 mm high","No",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL WINDOWS, LOUVRES,"]
[null,"DOORS,etc"]
[]
[null,"Window (SS32) Size 987 x 978 mm high - as per Architect's"]
[null,"Specification. Making good to existing","No",null,{"v":500,"d":"R 500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"STEEL ROLLER SHUTTERS ETC"]
[]
[null,"Galvanised hot dipped mild steel"]
[]
[null,"Door Gate (G1) size 813 x 2032 mm high, including handles,"]
[null,"lockset and hinges, as per Architect's Specification or","No",null,{"v":1500,"d":"R 1,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacturer's detail"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[null,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",null,{"v":35000,"d":"R 35,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Double ended strongroom ventilator","No",null,{"v":1500,"d":"R 1,500.00"},null,{"$f":"E634*D634","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G593:G635)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",36,{"v":75,"d":"R 75.00"},null,{"v":2700,"d":"R 2,700.00"}]
[]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls","m2",120,{"v":75,"d":"R 75.00"},null,{"v":9000,"d":"R 9,000.00"}]
[]
[null,"On narrow widths","m2",4,{"v":75,"d":"R 75.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G639:G654)","v":{"v":12000,"d":"R 12,000.00"}}]
[]
[null,"TILING"]
[]
[null,"FLOOR TILING",{"$nulls":3},{"$f":"E659*D659","v":{"v":0,"d":"R 0.00"}},{"v":0,"d":"R 0.00"}]
[{"$nulls":5},{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,"300 x 300 x 2.5mm Johnson ceramic floor tiles with all the adhesive",{"$nulls":3},{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,"On floors","m2",36,{"v":280,"d":"R 280.00"},null,{"v":10080,"d":"R 10,080.00"}]
[]
[null,"Tile skirting","m",72,{"v":150,"d":"R 150.00"},null,{"v":10800,"d":"R 10,800.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G658:G665)","v":{"v":20880,"d":"R 20,880.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",12,{"v":110,"d":"R 110.00"},null,{"v":1320,"d":"R 1,320.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",6,{"v":100,"d":"R 100.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"Extra for angle","No",2,{"v":250,"d":"R 250.00"},null,{"v":500,"d":"R 500.00"}]
[null,"Extra for stop end","No",2,{"v":250,"d":"R 250.00"},null,{"v":500,"d":"R 500.00"}]
[null,"Extra for outlet for 100mm pipe","No",2,{"v":250,"d":"R 250.00"},null,{"v":500,"d":"R 500.00"}]
[null,"Extra for eaves or plinth offset","No",2,{"v":250,"d":"R 250.00"},null,{"v":500,"d":"R 500.00"}]
[]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Vaal"]
[null,"Aquasave duct type wc pan as per Architect's Specification,"]
[null,"including forming opening through the concrete slab.","No",8,{"v":2000,"d":"R 2,000.00"},null,{"$f":"E690*D690","v":{"v":16000,"d":"R 16,000.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",null,{"v":10000,"d":"R 10,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G670:G709)","v":{"v":19920,"d":"R 19,920.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",null,{"v":200,"d":"R 200.00"},null,{"$f":"E716*D716","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G713:G717)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education)"]
[]
[null,"Internal walls","m2",120,{"v":90,"d":"R 90.00"},null,{"v":10800,"d":"R 10,800.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education)"]
[null,"Fascias and barge boards","m",30,{"v":20,"d":"R 20.00"},null,{"v":600,"d":"R 600.00"}]
[]
[null,"Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",5,{"v":90,"d":"R 90.00"},null,{"v":450,"d":"R 450.00"}]
[null,"Windows","m2",null,{"v":90,"d":"R 90.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",32,{"v":90,"d":"R 90.00"},null,{"v":2880,"d":"R 2,880.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats super universal enamel paint on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G725:G749)","v":{"v":14730,"d":"R 14,730.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G171","v":{"v":4800,"d":"R 4,800.00"}}]
[]
[null,"EARTHWORK",{"$nulls":3},{"$f":"F235","v":{"v":0,"d":"R 0.00"}},{"$f":"G235","v":{"v":11235,"d":"R 11,235.00"}}]
[]
[null,"CONCRETE, FORMWORK, REINFORCEMENT",{"$nulls":3},{"$f":"F306","v":{"v":0,"d":"R 0.00"}},{"$f":"G306","v":{"v":12180,"d":"R 12,180.00"}}]
[]
[null,"PRECAST CONCRETE",{"$nulls":3},{"$f":"F321","v":{"v":0,"d":"R 0.00"}},{"$f":"G321","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F376","v":{"v":0,"d":"R 0.00"}},{"$f":"G376","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"WATERPROOFING",{"$nulls":3},{"$f":"F406","v":{"v":0,"d":"R 0.00"}},{"$f":"G406","v":{"v":375,"d":"R 375.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F439","v":{"v":0,"d":"R 0.00"}},{"$f":"G439","v":{"v":19100,"d":"R 19,100.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F521","v":{"v":0,"d":"R 0.00"}},{"$f":"G521","v":{"v":25550,"d":"R 25,550.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F549","v":{"v":0,"d":"R 0.00"}},{"$f":"G549","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F558","v":{"v":0,"d":"R 0.00"}},{"$f":"G558","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F590","v":{"v":0,"d":"R 0.00"}},{"$f":"G590","v":{"v":7750,"d":"R 7,750.00"}}]
[]
[null,"METAL WORKS",{"$nulls":3},{"$f":"F636","v":{"v":0,"d":"R 0.00"}},{"$f":"G636","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F655","v":{"v":0,"d":"R 0.00"}},{"$f":"G655","v":{"v":12000,"d":"R 12,000.00"}}]
[]
[null,"TILING",{"$nulls":3},{"$f":"F666","v":{"v":0,"d":"R 0.00"}},{"$f":"G666","v":{"v":20880,"d":"R 20,880.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F710","v":{"v":0,"d":"R 0.00"}},{"$f":"G710","v":{"v":19920,"d":"R 19,920.00"}}]
[]
[null,"GALZING",{"$nulls":3},{"$f":"F718","v":{"v":0,"d":"R 0.00"}},{"$f":"G718","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F750","v":{"v":0,"d":"R 0.00"}},{"$f":"G750","v":{"v":14730,"d":"R 14,730.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F757:F789)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G757:G789)","v":{"v":143720,"d":"R 143,720.00"}}]

{"sheet":"Blk 9 Toilet","index":7,"n_rows":789,"n_cols":15,"rows_kept":789,"hidden":true}
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[]
["A","  -  BLOCK 9"]
[1,"Demolition"]
[null,"Temporary barriers, screens, etc including removal "]
[]
[null,"Existing hoarding with poles","m",null,{"v":80,"d":"R 80.00"},null,{"$f":"E7*D7","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Existing shadecloth hoarding 1,8m high on Bonnox","m",{"$nulls":3},{"$f":"E9*D9","v":{"v":0,"d":"R 0.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[null,"Double gate size 6000 x 1800mm high formed of suitable","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," tubular steel frame filled in with Bonnox fencing and covered"]
[null," with shadecloth including all necessary gate posts, locking"]
[null," mechanism, etc"]
[]
[null,"RELOCATION OF EXISTING STRUCTURES "]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"Half brick wall ","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Carefully disconnect all existing electrical, water and"]
[null," drainage service connections, etc and relocate existing"]
[null," park home including creating a new platform in the new"]
[null," position within the existing site boundary and"]
[null," re-connecting all services complete as per Architect's site"]
[null," plan "]
[]
[null,"Relocate existing Parking Home 9 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 14,5 x 7 x 3m high wide ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 28 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Breaking up and removing reinforced concrete including"]
[null," cutting off and removing reinforcement and cart away to a"]
[null," dumping site to be located by the contractor "]
[]
[null,"100mm Thick surface bed","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Taking out and removing doors, windows, etc from"]
[null," brickwork to be demolished "]
[]
[null,"Glazed steel window not exceeding 2,5m2","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Taking down and removing roofs, floors, panelling,"]
[null," ceilings, partitions, etc "]
[]
[null,"Asbestors/metal roof covering including fascias and bardgeboards","m2",25,{"v":50,"d":"R 50.00"},null,{"v":1250,"d":"R 1,250.00"}]
[null," and rainwater goods adn dispose off as per the SHE"]
[null," regulations. "]
[]
[null,"Wooden floors tiles including skirting, joints, bearers etc","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Gypsum plasterboard ceilings, including cornices, timber","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brandering, etc "]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber door 1610 x 2032mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Timber door 910 x 2032mm high","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Taking up and removing vinyl floor coverings, carpeting,"]
[null," etc "]
[]
[null,"Vinyl tile floor covering including preparing screed for new vinyl","m²",{"$nulls":3},{"$f":"E73*D73","v":{"v":0,"d":"R 0.00"}}]
[null," floor covering "]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Take out and remove mirror and replace with new.","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Roof trusses including purlins","No",null,{"v":50,"d":"R 50.00"},null,{"$f":"E82*D82","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Fascia boards","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E84*D84","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Roof gutters","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E86*D86","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Downpipes","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E88*D88","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Taking  out and removing piping, sanitary fittings, etc",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null," including disconnecting  piping  from fittings  and  making"]
[null," good floor and wall finishes (making good tiling and"]
[null," paintwork elsewhere) "]
[]
[null,"50mm Cast iron piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Copper piping not exceeding 50mm dia including fittings and","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brackets"]
[]
[null,"100mm PVC piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Piping exceeding 150mm and not exceeding 200mm.","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china wash hand basin ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china WC pan with cistern ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Stainless steel urinal including breaking up and removing","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," concrete urinal step."]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of plaster in walls to recieve new all tiles. (Tiles","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," elesewhere measured)"]
[{"$nulls":10},17,17,null,{"$f":"L115+K115","v":34}]
[null,"Chipping of screed in floors to recieve new screed. ","m²",36,{"v":50,"d":"R 50.00"},null,{"v":1800,"d":"R 1,800.00"},{"$nulls":3},8,8,8,{"$f":"M116+L116+K116","v":24}]
[{"$nulls":13},{"$f":"N115+N116","v":58}]
[null,"Cleaning walls to recieve paint.","m²",118,{"v":20,"d":"R 20.00"},null,{"v":2360,"d":"R 2,360.00"},{"$nulls":6},{"$f":"N117*2","v":116}]
[{"$nulls":13},{"$f":"N118*3","v":348}]
[null,"Walls in patches ","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"OPENINGS THROUGH EXISTING WALLS ETC "]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new doors and frames including necessary precast"]
[null," concrete lintels and making good plaster on both sides"]
[null," and into reveals (new doors and frames and making good"]
[null," paintwork elsewhere) "]
[]
[null,"Opening for door with Aluminium frame 2032 x 900mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," overall through 230mm brick wall."]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new windows including necessary precast concrete"]
[null," lintels and making good plaster on one side and into"]
[null," reveals and face brickwork on other side and into reveals"]
[null," and with 230mm Wide facebrick sill set sloping and slightly"]
[null," projecting on outside and flat plastered sill on inside (new"]
[null," windows and making good paintwork elsewhere) "]
[]
[null,"Opening for window 600 x 654mm high through one brick wall","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"MAKING GOOD OF FINISHES ETC "]
[]
[null,"Making good brickwork to face of wall where half brick have","m",{"$nulls":3},{"$f":"E145*D145","v":{"v":0,"d":"R 0.00"}}]
[null," been demolished."]
[]
[null,"Making good brickwork to face of wall where one brickwall was","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," removed"]
[]
[null,"Carefully inspect timber roof structure, report findings to"]
[null," Representative/Agent and repair as instructed by cutting"]
[null," out rotten or damaged timber, inserting new like sized and"]
[null," graded timber and joining old to new timber as described "]
[]
[null,"Allow the net sum of R…………………………. (………….. Rand) for the ","Item",1,null,null,{"v":0,"d":"R 0.00"}]
[null,"inspection of timber roof structure on plan by a registered"]
[null," entomologist"]
[]
[null,"Carefully inspect, repair and make good existing roof"]
[null," coverings and other related elements "]
[]
[null,"Inspect existing IRB roofsheeting, refix or replace any damaged","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," areas with new to match existing"]
[]
[null,"Clean with a high pressure cleaner to remove stains,"]
[null," marks, algae, etc "]
[]
[null,"IBR roof sheeting covering with a pitch not exceeding 25⁰","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G5:G170)","v":{"v":5410,"d":"R 5,410.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"EARTHWORKS"]
[]
[null,"Site clearance"]
[null,"Digging up and removing rubbish, debris, vegetation, hedges,"]
[null,"shrubs and trees not exceeding 200mm girth, bush, etc","m2",null,{"v":15,"d":"R 15.00"},null,{"$f":"E179*D179","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Stripping average 100mm thick layer of top soil and stockpiling"]
[null,"on site","m2",20,{"v":25,"d":"R 25.00"},null,{"$f":"E182*D182","v":{"v":500,"d":"R 500.00"}}]
[]
[null,"EXCAVATIONS"]
[]
[null,"Open face excavation to reduce levels \"cut to fill'","m3",5,{"v":50,"d":"R 50.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[null,"Trenches for V-drains","m3",7,{"v":50,"d":"R 50.00"},null,{"v":350,"d":"R 350.00"},null,null,34,20,{"$f":"K189+J189","v":54},0.6,0.7,{"$f":"N189*M189*L189","v":22.68}]
[{"$nulls":14},{"$f":"O189*2","v":45.36}]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in",{"$nulls":9},54,0.6,{"$f":"M192*L192","v":32.4}]
[null,"Soft rock","m3",2,{"v":150,"d":"R 150.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"Hard rock","m3",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Risk of collapse of excavations"]
[null,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",20,{"v":45,"d":"R 45.00"},null,{"v":900,"d":"R 900.00"}]
[]
[null,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":400,"d":"R 400.00"},null,{"v":400,"d":"R 400.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[null,"Under floors, steps, pavings, etc","m3",2,{"v":350,"d":"R 350.00"},null,{"v":700,"d":"R 700.00"}]
[]
[null,"Backfilling to trenches, holes, etc","m3",1,{"v":350,"d":"R 350.00"},null,{"v":350,"d":"R 350.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[null,"Under floors etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Compaction of surfaces"]
[null,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",12,{"v":45,"d":"R 45.00"},null,{"v":540,"d":"R 540.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming","m2",12,{"v":20,"d":"R 20.00"},null,{"v":240,"d":"R 240.00"}]
[]
[null,"To bottoms and sides of trenches etc","m2",12,{"v":20,"d":"R 20.00"},null,{"v":240,"d":"R 240.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G179:G234)","v":{"v":5020,"d":"R 5,020.00"}}]
[]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"$f":"E244*D244","v":{"v":0,"d":"R 0.00"}}]
[{"$nulls":10},54,0.6,0.25,{"$f":"M245*L245*K245","v":8.1}]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",3,{"v":1800,"d":"R 1,800.00"},null,{"v":5400,"d":"R 5,400.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Slab to cover pit","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TEST BLOCKS",{"$nulls":8},54,{"$f":"K258/2.4","v":22.5},{"$f":"L258*0.6","v":13.5}]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",2,{"v":150,"d":"R 150.00"},null,{"v":300,"d":"R 300.00"}]
[{"$nulls":10},54,0.6,{"$f":"L261*K261","v":32.4}]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",12,{"v":45,"d":"R 45.00"},null,{"v":540,"d":"R 540.00"}]
[]
[null,"Rough formwork to sides"]
[]
[null,"pit slabs propped up exceeding 1,5m and not exceeding 3.5m"]
[null,"high, including removal from confined area.","m2",20,{"v":65,"d":"R 65.00"},null,{"v":1300,"d":"R 1,300.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"10mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"8mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",12,{"v":145,"d":"R 145.00"},null,{"v":1740,"d":"R 1,740.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G243:G305)","v":{"v":9505,"d":"R 9,505.00"}}]
[]
[]
[]
[null,"PRECAST CONCRETE"]
[]
[null,"450 x 450 x Precast concrete inspection chamber covers","No",0,null,null,{"$f":"E312*D312","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Joint sealants"]
[]
[null,"Stalton or similar and approved prestressed fabricated"]
[null,"lintels:"]
[]
[null,"110 x 75mm Lintels in lengths not exceeding 3m.","No",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G311:G320)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"MASONRY"]
[]
[null,"FOUNDATIONS"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive"]
[null,"strength) in class 1 mortar including galvanised crimp wire"]
[null,"wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Half brick walls in beamfilling","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"On brick walls, piers, etc","m2",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Brickwork reinforcement","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Turning pieces"]
[null,"150mm Wide turning piece to lintels etc","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"FACE BRICKWORK"]
[null,"Corobrik FBA face bricks pointed with recessed"]
[null,"horizontal and vertical joints"]
[null,"Extra over brickwork for face brickwork","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Extra over brickwork for brick-on-edge header course lintel","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Brick-on-edge header course copings, sills, etc., of"]
[null,"Corobrik Firelight Travertine FBX face bricks pointed"]
[null,"with recessed joints on all exposed faces"]
[]
[null,"220mm wide window sill set sloping and slightly projecting"]
[null,"(refer architect's specification","m",null,{"v":85,"d":"R 85.00"},null,{"$f":"E374*D374","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection"]
[]
[]
[null,"WATERPROOFING"]
[]
[null,"One layer of 375 micron \"Consol Plastics Brikgrip DPC\""]
[null,"embossed damp proof course"]
[null,"dpc - In walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One layer of 250 micron \"Consol Plastics Gunplas USB"]
[null,"Green\" waterproof sheeting sealed at laps with \"Gunplas"]
[null,"Pressure Sensitive Tape\""]
[]
[null,"Under surface beds","m2",12,{"v":25,"d":"R 25.00"},null,{"v":300,"d":"R 300.00"}]
[]
[null,"Two coats of \"Brixeal\" or similar and approved bitumen"]
[null,"waterproofing compound:"]
[null,"On walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"JOINT SEALANTS ETC"]
[]
[null,"Silicone rubber base sealing compound"]
[null,"In joints between frames and walls","m",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Polysulphide sealant including backing cord, bond"]
[null,"breaker, primer, etc"]
[]
[null,"10 x 10mm in expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[null,"12 x 10mm expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G381:G405)","v":{"v":300,"d":"R 300.00"}}]
[]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",25,{"v":350,"d":"R 350.00"},null,{"v":8750,"d":"R 8,750.00"}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Narrow and broad flute closers","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",20,{"v":25,"d":"R 25.00"},null,{"$f":"E437*D437","v":{"v":500,"d":"R 500.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G412:G438)","v":{"v":9250,"d":"R 9,250.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",24,{"v":65,"d":"R 65.00"},null,{"v":1560,"d":"R 1,560.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in lenght, to"]
[null,"manufacturer's specification","m",40,{"v":85,"d":"R 85.00"},null,{"v":3400,"d":"R 3,400.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",25,{"v":25,"d":"R 25.00"},null,{"v":625,"d":"R 625.00"}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 10848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",null,{"v":2500,"d":"R 2,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"related items"]
[]
[null,"Lean to prefabricated plate nailed roof"]
[null,"truss spanning approximately 12848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",4,{"v":1200,"d":"R 1,200.00"},null,{"v":4800,"d":"R 4,800.00"}]
[]
[null,"Double pitched prefabricated plate nailed roof truss spanning"]
[null,"approximately 8970mm and 1689mm high, truss to be hoisted"]
[null,"and fixed approximately 4m above ground level as per","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacture's details.The description includes all related items."]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",10,{"v":110,"d":"R 110.00"},null,{"v":1100,"d":"R 1,100.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",9,{"v":100,"d":"R 100.00"},null,{"v":900,"d":"R 900.00"}]
[{"$nulls":6},{"v":0,"d":"R 0.00"}]
[null,"SKIRTINGS",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null,"Wrought meranti",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed double door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",null,{"v":2000,"d":"R 2,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Solid flush panel doors"]
[null,"44mm (D3) Solid flush panel hollow core doors with approved"]
[null,"hardwood veneer on both sides and two hardwood edge strips"]
[null,"hung to steel frames, size 813 x 2032mm high.Refer Architect's","No",2,{"v":1200,"d":"R 1,200.00"},null,{"v":2400,"d":"R 2,400.00"}]
[null,"Schedule"]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards","No",null,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E507*D507","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Chalk boards (2420mm x 1230mm)","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"WHITE BOARDS"]
[null,"'Vitrex Execuboard' magnetic whiteboard with aluminium"]
[null,"surround fixed 3 no. times at the top and bottom with"]
[null,"aluminium brackets, sleeve and screw"]
[]
[null,"2400 x 1140mm Whiteboards","No",null,{"v":0,"d":"R 0.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TABLES (AS PER ARCHITECT'S DETAILS)"]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G443:G520)","v":{"v":14785,"d":"R 14,785.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS"]
[null,"AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of Xmm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",null,{"v":650,"d":"R 650.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G526:G548)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[]
[null,null,"m2",null,{"v":280,"d":"R 280.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G553:G557)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"100mm Galvanised steel loose-pin hinges welded in position as"]
[null,"per architect's specification","No",4,{"v":250,"d":"R 250.00"},null,{"v":1000,"d":"R 1,000.00"}]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",2,{"v":450,"d":"R 450.00"},null,{"v":900,"d":"R 900.00"}]
[]
[null,"Five lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":550,"d":"R 550.00"},null,{"$f":"E571*D571","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Seven lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"4mm Perspex signs painted white on back with letters and"]
[null,"numerals reverse engraved and painted black"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G559:G589)","v":{"v":2050,"d":"R 2,050.00"}}]
[]
[null,"METALWORK"]
[]
[null,"STEEL HANDRAILS, BALUSTRADES, ETC"]
[]
[null,"100mm diameter galvanised steel posts on the veranda, with"]
[null,"an extreme height of 2600mm (Including connecting brackets"]
[null,"and all other related items, as per engineer's details).","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL DOOR FRAMES"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls"]
[]
[null,"Frame for door 877 x 2032 mm high","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls"]
[null,"complete with straps for building in"]
[]
[null,"Frame for door size 813 x 2032 mm high","No",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL WINDOWS, LOUVRES,"]
[null,"DOORS,etc"]
[]
[null,"Window (SS32) Size 987 x 978 mm high - as per Architect's"]
[null,"Specification. Making good to existing","No",null,{"v":500,"d":"R 500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"STEEL ROLLER SHUTTERS ETC"]
[]
[null,"Galvanised hot dipped mild steel"]
[]
[null,"Door Gate (G1) size 813 x 2032 mm high, including handles,"]
[null,"lockset and hinges, as per Architect's Specification or","No",null,{"v":1500,"d":"R 1,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacturer's detail"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[null,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",null,{"v":35000,"d":"R 35,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Double ended strongroom ventilator","No",null,{"v":1500,"d":"R 1,500.00"},null,{"$f":"E634*D634","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G593:G635)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",20,{"v":75,"d":"R 75.00"},null,{"v":1500,"d":"R 1,500.00"}]
[]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls","m2",118,{"v":75,"d":"R 75.00"},null,{"v":8850,"d":"R 8,850.00"}]
[]
[null,"On narrow widths","m2",3,{"v":75,"d":"R 75.00"},null,{"v":225,"d":"R 225.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G639:G654)","v":{"v":10575,"d":"R 10,575.00"}}]
[]
[null,"TILING"]
[]
[null,"FLOOR TILING"]
[]
[null,"300 x 300 x 2.5mm Johnson ceramic floor tiles with all the adhesive"]
[null,"On floors","m2",20,{"v":280,"d":"R 280.00"},null,{"v":5600,"d":"R 5,600.00"}]
[]
[null,"Tile skirting","m",28,{"v":150,"d":"R 150.00"},null,{"v":4200,"d":"R 4,200.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G658:G665)","v":{"v":9800,"d":"R 9,800.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",5,{"v":110,"d":"R 110.00"},null,{"v":550,"d":"R 550.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",1,{"v":100,"d":"R 100.00"},null,{"v":100,"d":"R 100.00"}]
[]
[null,"Extra for angle","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for stop end","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for outlet for 100mm pipe","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for eaves or plinth offset","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Vaal"]
[null,"Aquasave duct type wc pan as per Architect's Specification,"]
[null,"including forming opening through the concrete slab.","No",2,{"v":2000,"d":"R 2,000.00"},null,{"$f":"E689*D689","v":{"v":4000,"d":"R 4,000.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",null,{"v":10000,"d":"R 10,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G670:G708)","v":{"v":5650,"d":"R 5,650.00"}}]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"4mm Anodised"]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",null,{"v":200,"d":"R 200.00"},null,{"$f":"E715*D715","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G712:G716)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education)"]
[]
[null,"Internal walls","m2",118,{"v":90,"d":"R 90.00"},null,{"v":10620,"d":"R 10,620.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education)"]
[null,"Fascias and barge boards","m",19,{"v":20,"d":"R 20.00"},null,{"v":380,"d":"R 380.00"}]
[]
[null,"Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",3,{"v":90,"d":"R 90.00"},null,{"v":270,"d":"R 270.00"}]
[null,"Windows","m2",null,{"v":90,"d":"R 90.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",8,{"v":90,"d":"R 90.00"},null,{"v":720,"d":"R 720.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats super universal enamel paint on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G724:G748)","v":{"v":11990,"d":"R 11,990.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G171","v":{"v":5410,"d":"R 5,410.00"}}]
[]
[null,"EARTHWORK",{"$nulls":3},{"$f":"F235","v":{"v":0,"d":"R 0.00"}},{"$f":"G235","v":{"v":5020,"d":"R 5,020.00"}}]
[]
[null,"CONCRETE, FORMWORK, REINFORCEMENT",{"$nulls":3},{"$f":"F306","v":{"v":0,"d":"R 0.00"}},{"$f":"G306","v":{"v":9505,"d":"R 9,505.00"}}]
[]
[null,"PRECAST CONCRETE",{"$nulls":3},{"$f":"F321","v":{"v":0,"d":"R 0.00"}},{"$f":"G321","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F376","v":{"v":0,"d":"R 0.00"}},{"$f":"G376","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"WATERPROOFING",{"$nulls":3},{"$f":"F406","v":{"v":0,"d":"R 0.00"}},{"$f":"G406","v":{"v":300,"d":"R 300.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F439","v":{"v":0,"d":"R 0.00"}},{"$f":"G439","v":{"v":9250,"d":"R 9,250.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F521","v":{"v":0,"d":"R 0.00"}},{"$f":"G521","v":{"v":14785,"d":"R 14,785.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F549","v":{"v":0,"d":"R 0.00"}},{"$f":"G549","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F558","v":{"v":0,"d":"R 0.00"}},{"$f":"G558","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F590","v":{"v":0,"d":"R 0.00"}},{"$f":"G590","v":{"v":2050,"d":"R 2,050.00"}}]
[]
[null,"METAL WORKS",{"$nulls":3},{"$f":"F636","v":{"v":0,"d":"R 0.00"}},{"$f":"G636","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F655","v":{"v":0,"d":"R 0.00"}},{"$f":"G655","v":{"v":10575,"d":"R 10,575.00"}}]
[]
[null,"TILING",{"$nulls":3},{"$f":"F666","v":{"v":0,"d":"R 0.00"}},{"$f":"G666","v":{"v":9800,"d":"R 9,800.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F709","v":{"v":0,"d":"R 0.00"}},{"$f":"G709","v":{"v":5650,"d":"R 5,650.00"}}]
[]
[null,"GALZING",{"$nulls":3},{"$f":"F717","v":{"v":0,"d":"R 0.00"}},{"$f":"G717","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F749","v":{"v":0,"d":"R 0.00"}},{"$f":"G749","v":{"v":11990,"d":"R 11,990.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F756:F788)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G756:G788)","v":{"v":78925,"d":"R 78,925.00"}}]

{"sheet":"Blk 11 Guard H","index":8,"n_rows":790,"n_cols":15,"rows_kept":790,"hidden":true}
["Item","Description","Unit","Qty","Rate","Storm Damage","Maintenance"]
[]
["A"," GUARD HOUSE -  BLOCK 10"]
[1,"Demolition"]
[null,"Temporary barriers, screens, etc including removal "]
[]
[null,"Existing hoarding with poles","m",8,{"v":80,"d":"R 80.00"},null,{"$f":"E7*D7","v":{"v":640,"d":"R 640.00"}}]
[]
[null,"Existing shadecloth hoarding 1,8m high on Bonnox","m",{"$nulls":3},{"$f":"E9*D9","v":{"v":0,"d":"R 0.00"}}]
[null," fence fixed to gumpoles at suitable centres and refix in new"]
[null," position all to the Architect's approval"]
[]
[null,"Double gate size 6000 x 1800mm high formed of suitable","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," tubular steel frame filled in with Bonnox fencing and covered"]
[null," with shadecloth including all necessary gate posts, locking"]
[null," mechanism, etc"]
[]
[null,"RELOCATION OF EXISTING STRUCTURES "]
[]
[null,"Breaking down and removing brickwork etc "]
[]
[null,"Half brick wall ","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Carefully disconnect all existing electrical, water and"]
[null," drainage service connections, etc and relocate existing"]
[null," park home including creating a new platform in the new"]
[null," position within the existing site boundary and"]
[null," re-connecting all services complete as per Architect's site"]
[null," plan "]
[]
[null,"Relocate existing Parking Home 9 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 14,5 x 7 x 3m high wide ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Relocate existing Parking Home 28 x 7 x 3m high ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"REMOVAL OF EXISTING WORK "]
[]
[null,"Breaking up and removing reinforced concrete including"]
[null," cutting off and removing reinforcement and cart away to a"]
[null," dumping site to be located by the contractor "]
[]
[null,"100mm Thick surface bed","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Taking out and removing doors, windows, etc from"]
[null," brickwork to be demolished "]
[]
[null,"Glazed steel window not exceeding 2,5m2","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Taking down and removing roofs, floors, panelling,"]
[null," ceilings, partitions, etc "]
[]
[null,"Asbestors/metal roof covering including fascias and bardgeboards","m2",9,{"v":50,"d":"R 50.00"},null,{"v":450,"d":"R 450.00"}]
[null," and rainwater goods adn dispose off as per the SHE"]
[null," regulations. "]
[]
[null,"Wooden floors tiles including skirting, joints, bearers etc","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Gypsum plasterboard ceilings, including cornices, timber","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brandering, etc "]
[]
[null,"Taking out and removing joinery fittings etc "]
[]
[null,"Timber door 1610 x 2032mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Timber door 910 x 2032mm high","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Taking up and removing vinyl floor coverings, carpeting,"]
[null," etc "]
[]
[null,"Vinyl tile floor covering including preparing screed for new vinyl","m²",{"$nulls":3},{"$f":"E73*D73","v":{"v":0,"d":"R 0.00"}}]
[null," floor covering "]
[]
[null,"Taking out and removing ironmongery "]
[]
[null,"Mortice lock and striking plate from timber door and steel frame","No",null,{"v":50,"d":"R 50.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Take out and remove mirror and replace with new.","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Roof trusses including purlins","No",null,{"v":50,"d":"R 50.00"},null,{"$f":"E82*D82","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Fascia boards","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E84*D84","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Roof gutters","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E86*D86","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Downpipes","m",null,{"v":10,"d":"R 10.00"},null,{"$f":"E88*D88","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Taking  out and removing piping, sanitary fittings, etc"]
[null," including disconnecting  piping  from fittings  and  making"]
[null," good floor and wall finishes (making good tiling and"]
[null," paintwork elsewhere) "]
[]
[null,"50mm Cast iron piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Copper piping not exceeding 50mm dia including fittings and","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," brackets"]
[]
[null,"100mm PVC piping including fittings and brackets","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Piping exceeding 150mm and not exceeding 200mm.","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china wash hand basin ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Vitreous china WC pan with cistern ","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"Stainless steel urinal including breaking up and removing","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," concrete urinal step."]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[null,"Chipping of plaster in walls to recieve new all tiles. (Tiles","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," elesewhere measured)"]
[{"$nulls":10},17,17,null,{"$f":"L115+K115","v":34}]
[null,"Chipping of screed in floors to recieve new screed. ","m²",7,{"v":50,"d":"R 50.00"},null,{"v":350,"d":"R 350.00"},{"$nulls":3},8,8,8,{"$f":"M116+L116+K116","v":24}]
[{"$nulls":13},{"$f":"N115+N116","v":58}]
[null,"Cleaning walls to recieve paint.","m²",51,{"v":20,"d":"R 20.00"},null,{"v":1020,"d":"R 1,020.00"},{"$nulls":6},{"$f":"N117*2","v":116}]
[{"$nulls":13},{"$f":"N118*3","v":348}]
[null,"Walls in patches ","m²",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"OPENINGS THROUGH EXISTING WALLS ETC "]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new doors and frames including necessary precast"]
[null," concrete lintels and making good plaster on both sides"]
[null," and into reveals (new doors and frames and making good"]
[null," paintwork elsewhere) "]
[]
[null,"Opening for door with Aluminium frame 2032 x 900mm high","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," overall through 230mm brick wall."]
[]
[null,"Breaking out for and forming openings through brick walls"]
[null," for new windows including necessary precast concrete"]
[null," lintels and making good plaster on one side and into"]
[null," reveals and face brickwork on other side and into reveals"]
[null," and with 230mm Wide facebrick sill set sloping and slightly"]
[null," projecting on outside and flat plastered sill on inside (new"]
[null," windows and making good paintwork elsewhere) "]
[]
[null,"Opening for window 600 x 654mm high through one brick wall","No",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"MAKING GOOD OF FINISHES ETC "]
[]
[null,"Making good brickwork to face of wall where half brick have","m",{"$nulls":3},{"$f":"E145*D145","v":{"v":0,"d":"R 0.00"}}]
[null," been demolished."]
[]
[null,"Making good brickwork to face of wall where one brickwall was","m",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," removed"]
[]
[null,"Carefully inspect timber roof structure, report findings to"]
[null," Representative/Agent and repair as instructed by cutting"]
[null," out rotten or damaged timber, inserting new like sized and"]
[null," graded timber and joining old to new timber as described "]
[]
[null,"Allow the net sum of R…………………………. (………….. Rand) for the ","Item",1,null,null,{"v":0,"d":"R 0.00"}]
[null,"inspection of timber roof structure on plan by a registered"]
[null," entomologist"]
[]
[null,"Carefully inspect, repair and make good existing roof"]
[null," coverings and other related elements "]
[]
[null,"Inspect existing IRB roofsheeting, refix or replace any damaged","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null," areas with new to match existing"]
[]
[null,"Clean with a high pressure cleaner to remove stains,"]
[null," marks, algae, etc "]
[]
[null,"IBR roof sheeting covering with a pitch not exceeding 25⁰","m²",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G5:G170)","v":{"v":2610,"d":"R 2,610.00"}}]
[]
[null,"NEW WORKS"]
[]
[null,"EARTHWORKS"]
[]
[null,"Site clearance"]
[null,"Digging up and removing rubbish, debris, vegetation, hedges,"]
[null,"shrubs and trees not exceeding 200mm girth, bush, etc","m2",null,{"v":15,"d":"R 15.00"},null,{"$f":"E179*D179","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Stripping average 100mm thick layer of top soil and stockpiling"]
[null,"on site","m2",10,{"v":25,"d":"R 25.00"},null,{"$f":"E182*D182","v":{"v":250,"d":"R 250.00"}}]
[]
[null,"EXCAVATIONS"]
[]
[null,"Open face excavation to reduce levels \"cut to fill'","m3",3,{"v":50,"d":"R 50.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[null,"Trenches for V-drains","m3",4,{"v":50,"d":"R 50.00"},null,{"v":200,"d":"R 200.00"},null,null,34,20,{"$f":"K189+J189","v":54},0.6,0.7,{"$f":"N189*M189*L189","v":22.68}]
[{"$nulls":14},{"$f":"O189*2","v":45.36}]
[null,"Extra over trench and hole excavations in earth for"]
[null,"excavation in",{"$nulls":9},54,0.6,{"$f":"M192*L192","v":32.4}]
[null,"Soft rock","m3",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Hard rock","m3",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to"]
[null,"a dumping site to be located by the contractor","m3",null,{"v":50,"d":"R 50.00"}]
[]
[null,"Risk of collapse of excavations"]
[null,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",10,{"v":45,"d":"R 45.00"},null,{"v":450,"d":"R 450.00"}]
[]
[null,"Keeping excavations free of all water other than subterranean"]
[null,"water","Item",1,{"v":200,"d":"R 200.00"},null,{"v":200,"d":"R 200.00"}]
[]
[null,"FILLING ETC"]
[]
[null,"Earth filling supplied by the contractor, compacted to 95%"]
[null,"Mod AASHTO density"]
[]
[null,"Under floors, steps, pavings, etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Backfilling to trenches, holes, etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Coarse river sand filling compacted to a density of at least"]
[null,"95% Mod. AASHTO density"]
[null,"Under floors etc","m3",null,{"v":350,"d":"R 350.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Compaction of surfaces"]
[null,"Compaction of ground surface under floors etc including"]
[null,"scarifying for a depth of 150mm, breaking down oversize"]
[null,"material, adding suitable material where necessary and"]
[null,"compacting to 95% Mod AASHTO density","m2",6,{"v":45,"d":"R 45.00"},null,{"v":270,"d":"R 270.00"}]
[]
[null,"SOIL POISONING"]
[null,"Soil insecticide"]
[]
[null,"Soil Poisoning: Under floors etc, including forming and"]
[null,"poisoning shallow furrows against foundation walls etc, filling in"]
[null,"furrows and ramming","m2",10,{"v":20,"d":"R 20.00"},null,{"v":200,"d":"R 200.00"}]
[]
[null,"To bottoms and sides of trenches etc","m2",10,{"v":20,"d":"R 20.00"},null,{"v":200,"d":"R 200.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G179:G234)","v":{"v":2320,"d":"R 2,320.00"}}]
[]
[]
[null,"CONCRETE, FORMWORK"]
[null,"AND REINFORCEMENT"]
[]
[null,"20Mpa/19mm concrete"]
[]
[null,"verandah floor cast in panels of 1850 centres, with controlled"]
[null,"joints every 7400 centres","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"$f":"E244*D244","v":{"v":0,"d":"R 0.00"}}]
[{"$nulls":10},54,0.6,0.25,{"$f":"M245*L245*K245","v":8.1}]
[null,"Concrete aprons cast in panels, laid to fall in 1:200, with control"]
[null,"joints filled with polysulphide sealant, every 3000mm centres","m3",2,{"v":1800,"d":"R 1,800.00"},null,{"v":3600,"d":"R 3,600.00"}]
[]
[null,"REINFORCED CONCRETE CAST AGAINST"]
[null,"EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[null,"25 Mpa: Strip footings","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Slab to cover pit","m3",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TEST BLOCKS",{"$nulls":8},54,{"$f":"K258/2.4","v":22.5},{"$f":"L258*0.6","v":13.5}]
[null,"Making and testing of three 150 x 150 x 150mm concrete"]
[null,"strength test cubes","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[{"$nulls":10},54,0.6,{"$f":"L261*K261","v":32.4}]
[null,"CONCRETE SUNDRIES"]
[]
[null,"Finishing top surfaces of concrete to a Class U2 wood"]
[null,"float finish"]
[]
[null,"Surface beds, slabs, etc","m2",6,{"v":45,"d":"R 45.00"},null,{"v":270,"d":"R 270.00"}]
[]
[null,"Rough formwork to sides"]
[]
[null,"pit slabs propped up exceeding 1,5m and not exceeding 3.5m"]
[null,"high, including removal from confined area.","m2",6,{"v":65,"d":"R 65.00"},null,{"v":390,"d":"R 390.00"}]
[]
[null,"MOVEMENT JOINTS ETC"]
[]
[null,"Expansion joints with softboard between vertical concrete"]
[null,"surfaces"]
[]
[null,"15mm Joints not exceeding 300mm high or wide","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"Expansion joints with bitumen-impregnated softboard"]
[null,"between vertical concrete and brickwork surfaces"]
[]
[null,"10mm Isolation Joints not exceeding 300mm high or wide","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"Saw cut joints"]
[null,"50 x 3mm Saw cut joints in top of concrete","m",5,{"v":15,"d":"R 15.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"REINFORCEMENT (PROVISIONAL) (CPAP Work"]
[null,"Group 114)"]
[]
[null,"Mild steel reinforcement to structural concrete work"]
[]
[null,"10mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"8mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"High tensile steel reinforcement to structural concrete"]
[null,"work"]
[null,"25mm Diameter bars","t",null,{"v":13000,"d":"R 13,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Fabric reinforcement"]
[]
[null,"Type 193 fabric reinforcement in concrete surface beds, slabs,","m2",6,{"v":145,"d":"R 145.00"},null,{"v":870,"d":"R 870.00"}]
[null,"etc"]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G243:G305)","v":{"v":5505,"d":"R 5,505.00"}}]
[]
[]
[]
[null,"PRECAST CONCRETE"]
[]
[null,"450 x 450 x Precast concrete inspection chamber covers","No",{"$nulls":3},{"$f":"E312*D312","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Joint sealants"]
[]
[null,"Stalton or similar and approved prestressed fabricated"]
[null,"lintels:"]
[]
[null,"110 x 75mm Lintels in lengths not exceeding 3m.","No",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G311:G320)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
[null,"MASONRY"]
[]
[null,"FOUNDATIONS"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive"]
[null,"strength) in class 1 mortar including galvanised crimp wire"]
[null,"wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Brickwork of NFP bricks in class II mortar including"]
[null,"galvanised crimp wire wall ties ( 7 per m2 laid staggered)"]
[]
[null,"Half brick walls","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Half brick walls in beamfilling","m2",null,{"v":380,"d":"R 380.00"},null,{"v":0,"d":"R 0.00"}]
[null,"One brick walls","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"BRICKWORK SUNDRIES"]
[]
[null,"Bagging of 1:3 cement and sand mixture"]
[]
[null,"On brick walls, piers, etc","m2",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Brickwork reinforcement","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[null,"150mm Wide reinforcement built in horizontally","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Turning pieces"]
[null,"150mm Wide turning piece to lintels etc","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Galvanised hoop iron cramps, ties, etc"]
[null,"30 x 1,6mm Cramp 500mm long with one end fixed to wood"]
[null,"and other end built into brickwork","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Air bricks etc"]
[null,"229 x 152mm Terra-cotta vermin proof air brick","No",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"FACE BRICKWORK"]
[null,"Corobrik FBA face bricks pointed with recessed"]
[null,"horizontal and vertical joints"]
[null,"Extra over brickwork for face brickwork","m2",null,{"v":480,"d":"R 480.00"},null,{"v":0,"d":"R 0.00"}]
[null,"Extra over brickwork for brick-on-edge header course lintel","m",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Brick-on-edge header course copings, sills, etc., of"]
[null,"Corobrik Firelight Travertine FBX face bricks pointed"]
[null,"with recessed joints on all exposed faces"]
[]
[null,"220mm wide window sill set sloping and slightly projecting"]
[null,"(refer architect's specification","m",null,{"v":85,"d":"R 85.00"},null,{"$f":"E374*D374","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection"]
[]
[]
[null,"WATERPROOFING"]
[]
[null,"One layer of 375 micron \"Consol Plastics Brikgrip DPC\""]
[null,"embossed damp proof course"]
[null,"dpc - In walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"One layer of 250 micron \"Consol Plastics Gunplas USB"]
[null,"Green\" waterproof sheeting sealed at laps with \"Gunplas"]
[null,"Pressure Sensitive Tape\""]
[]
[null,"Under surface beds","m2",6,{"v":25,"d":"R 25.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"Two coats of \"Brixeal\" or similar and approved bitumen"]
[null,"waterproofing compound:"]
[null,"On walls","m2",null,{"v":25,"d":"R 25.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"JOINT SEALANTS ETC"]
[]
[null,"Silicone rubber base sealing compound"]
[null,"In joints between frames and walls","m",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Polysulphide sealant including backing cord, bond",{"$nulls":7},2.4]
[null,"breaker, primer, etc"]
[]
[null,"10 x 10mm in expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[null,"12 x 10mm expansion joints in floors","m",null,{"v":15,"d":"R 15.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G381:G405)","v":{"v":150,"d":"R 150.00"}}]
[]
[]
[null,"ROOF COVERINGS ETC"]
[]
[null,"ROOF SHEETING AND ACCESSORIES"]
[]
[null,"Saflock 700 AZ150 G550 interlocking roof sheeting with"]
[null,"Z275 to both sides, on sisalation, fixed to timber"]
[null,"intermediate purlins (purlins as per manufacturer's spec,"]
[null,"taking into account windloads) secured with saflok 700"]
[null,"clips srcrew fixed to purlins as per manufacturer's"]
[null,"recommendations and specifications."]
[]
[null,"Roof covering with 15 degree pitch, in transportable lengths not"]
[null,"exceeding 20m. The description includes all related items.","m2",9,{"v":350,"d":"R 350.00"},null,{"v":3150,"d":"R 3,150.00"}]
[]
[null,"AG 150 G550 ridge capping with broad flute closures to suit"]
[null,"roof profile with pre-painted factory finish.","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Narrow and broad flute closers","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Sisalation 420 or equal and approved heavy industrial"]
[null,"grade aluminium foil based insulation"]
[]
[null,"Insulation laid taut over purlins (at approximately 1,80m"]
[null,"centres) and fixed concurrent with roof covering, including"]
[null,"taped laps and nylon straining wires","m2",9,{"v":25,"d":"R 25.00"},null,{"$f":"E437*D437","v":{"v":225,"d":"R 225.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G412:G438)","v":{"v":3375,"d":"R 3,375.00"}}]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Sawn softwood"]
[null,"38 x 114mm Wall plates","m",5,{"v":65,"d":"R 65.00"},null,{"v":325,"d":"R 325.00"}]
[]
[null,"50 x 76mm Purlins not exceeding 6.6 m in lenght, to"]
[null,"manufacturer's specification","m",17,{"v":85,"d":"R 85.00"},null,{"v":1445,"d":"R 1,445.00"}]
[]
[null,"Sundries"]
[null,"Two coats ABE Provinite on wrought timbers","m2",null,{"v":150,"d":"R 150.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Teco two way hurricane clips secured to purlins and trusses"]
[null,"at every intersection externally and internally galvanised wire is"]
[null,"to be used","No",16,{"v":25,"d":"R 25.00"},null,{"v":400,"d":"R 400.00"}]
[]
[null,"PREFABRICATED TIMBER ROOF TRUSSES, ETC"]
[]
[null,"Double pitched prefabricated plate nailed roof"]
[null,"truss spanning approximately 10848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",null,{"v":2500,"d":"R 2,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"related items"]
[]
[null,"Lean to prefabricated plate nailed roof"]
[null,"truss spanning approximately 12848mm and 1689mm high,"]
[null,"truss to be hoisted and fixed approximately 4m above ground"]
[null,"level as per manufacture's details.The description includes all","No",3,{"v":1200,"d":"R 1,200.00"},null,{"v":3600,"d":"R 3,600.00"}]
[]
[null,"Double pitched prefabricated plate nailed roof truss spanning"]
[null,"approximately 8970mm and 1689mm high, truss to be hoisted"]
[null,"and fixed approximately 4m above ground level as per","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacture's details.The description includes all related items."]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Everite medium density plain nutec-cement"]
[]
[null,"12 x 225mm Medium density fibre-cement fascia boards"]
[null,"(Product No.041-202) with aluminium H-profile fascia joiners"]
[null,"(Product No. 685-195), drill for and fix with hot-dip galvanised","m",5,{"v":110,"d":"R 110.00"},null,{"v":550,"d":"R 550.00"}]
[null,"drive screws and washers"]
[]
[null,"80 x 200mm Socketless barge boards (Product No.721-800)"]
[null,"with aluminium H-profile barge board joiners (Product No."]
[null,"685-187), drill for and fix with hot-dip galvanised screws and"]
[null,"washers","m",5,{"v":100,"d":"R 100.00"},null,{"v":500,"d":"R 500.00"}]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 75mm Skirtings including 19mm quadrant bead plugged","m",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DOORS, ETC"]
[null,"Wrought meranti doors hung to steel frame, etc"]
[]
[null,"44mm (D1) Framed double door 813 x 2032m high, as per"]
[null,"Architect's Specification","No",null,{"v":2000,"d":"R 2,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Solid flush panel doors"]
[null,"44mm (D3) Solid flush panel hollow core doors with approved"]
[null,"hardwood veneer on both sides and two hardwood edge strips"]
[null,"hung to steel frames, size 813 x 2032mm high.Refer Architect's","No",1,{"v":1200,"d":"R 1,200.00"},null,{"v":1200,"d":"R 1,200.00"}]
[null,"Schedule"]
[]
[null,"PINNING BOARDS"]
[null,"Flortime Premier pinning boards"]
[]
[null,"Flortime Premier pinning boards","No",null,{"v":4500,"d":"R 4,500.00"},null,{"$f":"E507*D507","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Chalk boards (2420mm x 1230mm)","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"WHITE BOARDS"]
[null,"'Vitrex Execuboard' magnetic whiteboard with aluminium"]
[null,"surround fixed 3 no. times at the top and bottom with"]
[null,"aluminium brackets, sleeve and screw"]
[]
[null,"2400 x 1140mm Whiteboards","No",null,{"v":0,"d":"R 0.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TABLES (AS PER ARCHITECT'S DETAILS)"]
[]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G443:G520)","v":{"v":8020,"d":"R 8,020.00"}}]
[]
[]
[null,"CEILINGS, PARTITIONS"]
[null,"AND ACCESS FLOORING"]
[]
[null,"Glasswool insulation"]
[]
[null,"76mm Insulation blanket closely fitted and laid on top of"]
[null,"brandering between roof timbers, etc","m2",null,{"v":35,"d":"R 35.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"NAILED UP CEILINGS"]
[]
[null,"6,4mm \"Rhino\" gypsum plasterboard with H-type pressed"]
[null,"steel jointing strips"]
[null,"Horizontal ceilings, including 38 x 38mm sawn softwood"]
[null,"brandering at maximum 400mm centres in one direction only to"]
[null,"trusses ( elsewhere measured).","m2",null,{"v":250,"d":"R 250.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Extra over ceiling for 900 x 900mm trap door of Xmm wrought"]
[null,"softwood rebated framing with one 50 x 50mm sawn softwood"]
[null,"cross brander covered with ceiling board and fitted flush in"]
[null,"opening","No",null,{"v":650,"d":"R 650.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DECORATIVE MOULDINGS AND CORNICES"]
[]
[null,"75mm Coved cornices","m",null,{"v":65,"d":"R 65.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G526:G548)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC"]
[]
[null,"FLOOR COVERINGS"]
[]
[]
[null,null,"m2",null,{"v":280,"d":"R 280.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G553:G557)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"100mm Galvanised steel loose-pin hinges welded in position as"]
[null,"per architect's specification","No",2,{"v":250,"d":"R 250.00"},null,{"v":500,"d":"R 500.00"}]
[]
[null,"Three lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",1,{"v":450,"d":"R 450.00"},null,{"v":450,"d":"R 450.00"}]
[]
[null,"Five lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":550,"d":"R 550.00"},null,{"$f":"E571*D571","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"Seven lever mortice lockset and satin chrome plated handles"]
[null,"Solid Art 390/313","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"4mm Perspex signs painted white on back with letters and"]
[null,"numerals reverse engraved and painted black"]
[]
[null,"200 x 30mm High signs with 15mm high letters and"]
[null,"numerals fixed with two self-tapping screws to steel and"]
[null,"reading as follows:-"]
[]
[null,"50mm High plastic letter or numeral","No",1,{"v":150,"d":"R 150.00"},null,{"v":150,"d":"R 150.00"}]
[]
[null,"38mm Diameter rubber door stop plugged and screwed to floor"]
[null,"with a 50mm long brass screw","No",null,{"v":45,"d":"R 45.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G559:G589)","v":{"v":1100,"d":"R 1,100.00"}}]
[]
[null,"METALWORK"]
[]
[null,"STEEL HANDRAILS, BALUSTRADES, ETC"]
[]
[null,"100mm diameter galvanised steel posts on the veranda, with"]
[null,"an extreme height of 2600mm (Including connecting brackets"]
[null,"and all other related items, as per engineer's details).","No",null,{"v":850,"d":"R 850.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL DOOR FRAMES"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls"]
[]
[null,"Frame for door 877 x 2032 mm high","No",null,{"v":3000,"d":"R 3,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls"]
[null,"complete with straps for building in"]
[]
[null,"Frame for door size 813 x 2032 mm high","No",null,{"v":1800,"d":"R 1,800.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"GALVANISED STEEL WINDOWS, LOUVRES,"]
[null,"DOORS,etc"]
[]
[null,"Window (SS32) Size 987 x 978 mm high - as per Architect's"]
[null,"Specification. Making good to existing","No",null,{"v":500,"d":"R 500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"STEEL ROLLER SHUTTERS ETC"]
[]
[null,"Galvanised hot dipped mild steel"]
[]
[null,"Door Gate (G1) size 813 x 2032 mm high, including handles,"]
[null,"lockset and hinges, as per Architect's Specification or","No",null,{"v":1500,"d":"R 1,500.00"},null,{"v":0,"d":"R 0.00"}]
[null,"manufacturer's detail"]
[]
[null,"STEEL STRONGROOM DOORS, VENTILATORS, ETC"]
[]
[null,"Category 2, record room strongroom doors with non"]
[null,"deteriorating insulation material etc suitable for 230mm"]
[null,"walls, fixed to brickwork or concrete"]
[]
[null,"Strongroom door (D5), Size 948 x 1980mm with 2 hour fire test"]
[null,"rating or equal approved, as per Architect's specification","No",null,{"v":35000,"d":"R 35,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"Double ended strongroom ventilator","No",null,{"v":1500,"d":"R 1,500.00"},null,{"$f":"E634*D634","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G593:G635)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds on concrete"]
[]
[null,"23mm Thick on floors and landings to receive floor tiles","m2",7,{"v":75,"d":"R 75.00"},null,{"v":525,"d":"R 525.00"}]
[]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Cement plaster on brickwork"]
[]
[null,"On walls","m2",51,{"v":75,"d":"R 75.00"},null,{"v":3825,"d":"R 3,825.00"}]
[]
[null,"On narrow widths","m2",1,{"v":75,"d":"R 75.00"},null,{"v":75,"d":"R 75.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G639:G654)","v":{"v":4425,"d":"R 4,425.00"}}]
[]
[null,"TILING"]
[]
[null,"FLOOR TILING"]
[]
[null,"300 x 300 x 2.5mm Johnson ceramic floor tiles with all the adhesive"]
[null,"On floors","m2",7,{"v":280,"d":"R 280.00"},null,{"v":1960,"d":"R 1,960.00"}]
[]
[null,"Tile skirting","m",10,{"v":150,"d":"R 150.00"},null,{"v":1500,"d":"R 1,500.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G658:G665)","v":{"v":3460,"d":"R 3,460.00"}}]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"RAINWATER DISPOSAL"]
[]
[null,"Seamless Aluminium"]
[]
[null,"155 x 100 x 115mm ogee gutter with baked enamel finish fixed"]
[null,"with concealed brackets (all to supplies spec).","m",3,{"v":110,"d":"R 110.00"},null,{"v":330,"d":"R 330.00"}]
[]
[null,"100 x 75 mm fluted downpipes with baked enamel afinish as"]
[null,"per supplier's details","m",1,{"v":100,"d":"R 100.00"},null,{"v":100,"d":"R 100.00"}]
[]
[null,"Extra for angle","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for stop end","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for outlet for 100mm pipe","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[null,"Extra for eaves or plinth offset","No",1,{"v":250,"d":"R 250.00"},null,{"v":250,"d":"R 250.00"}]
[]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Vaal"]
[null,"Aquasave duct type wc pan as per Architect's Specification,"]
[null,"including forming opening through the concrete slab.","No",null,{"v":2000,"d":"R 2,000.00"},null,{"$f":"E690*D690","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FIRE APPLIANCES ETC"]
[null,"Chubb"]
[]
[null,"Everyway\" hose reel complete with 30m plastic hose,"]
[null,"chromium plated stopcock, shut-off nozzle and wall bracket","No"]
[]
[null,"4,5kg Carbon dioxide fire extinguisher","No",null,{"v":4500,"d":"R 4,500.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"TANKS"]
[null,"Jojo Polyproline water tank"]
[null,"5000 litre Polyproline water tank with 35mm diameter inlet at"]
[null,"top and 50mm overflow outlet and 25mm outlet at base of tank"]
[null,"including access hatch on top fitted with vernim-proof vent, and"]
[null,"including 1.6 x 50mm galvanised hoop iron or other approved"]
[null,"holding down material secured around pedestal complete"]
[null,"including pedestal, including concrete, brickwork for stand as per"]
[null,"engineer's or Architect's drawings.","No",null,{"v":10000,"d":"R 10,000.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G670:G709)","v":{"v":1430,"d":"R 1,430.00"}}]
[{"$nulls":6},{"$f":"E711*D711","v":{"v":0,"d":"R 0.00"}}]
[null,"GLAZING",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[{"$nulls":6},{"v":0,"d":"R 0.00"}]
[null,"GLAZING TO STEEL WITH PUTTY",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null,"4mm Anodised",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null,"Panes exceeding 0,5m2 and not exceeding 2m2","m2",null,{"v":200,"d":"R 200.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G713:G717)","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINTWORK"]
[]
[null,"Prepare and apply one coat primer and two coats 'WALL N'"]
[null,"ALL' emulsion paint ( colour to be approved by the"]
[null,"Department of Education)"]
[]
[null,"Internal walls","m2",51,{"v":90,"d":"R 90.00"},null,{"v":4590,"d":"R 4,590.00"}]
[]
[null,"Prepare and apply one coat primer and two coats PVC"]
[null,"emulsion paint ( colour to be approved by the Department"]
[null,"of Education)"]
[null,"Fascias and barge boards","m",10,{"v":20,"d":"R 20.00"},null,{"v":200,"d":"R 200.00"}]
[]
[null,"Spot priming defects in pre-primed surfaces with zinc"]
[null,"phosphate metal primer, one coat universal undercoat and"]
[null,"two coats super universal enamel paint on steel"]
[]
[null,"Door frames","m2",1,{"v":90,"d":"R 90.00"},null,{"v":90,"d":"R 90.00"}]
[null,"Windows","m2",1,{"v":90,"d":"R 90.00"},null,{"v":90,"d":"R 90.00"}]
[]
[null,"Prepare and apply one coat calcium plumbate primer, one"]
[null,"coat undercoat and one coat gloss enamel paint"]
[]
[null,"Doors","m2",4,{"v":90,"d":"R 90.00"},null,{"v":360,"d":"R 360.00"}]
[]
[null,"One coat oil wood primer, one coat universal undercoat"]
[null,"and two coats super universal enamel paint on"]
[]
[null,"Skirtings, rails, etc not exceeding 300mm girth","m",null,{"v":20,"d":"R 20.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"To Collection",{"$nulls":4},{"$f":"SUM(G725:G749)","v":{"v":5330,"d":"R 5,330.00"}}]
[]
[]
[null,"SUMMARY BUILDING WORKS"]
[]
[null,"DEMOLITION",{"$nulls":4},{"$f":"G171","v":{"v":2610,"d":"R 2,610.00"}}]
[]
[null,"EARTHWORK",{"$nulls":3},{"$f":"F235","v":{"v":0,"d":"R 0.00"}},{"$f":"G235","v":{"v":2320,"d":"R 2,320.00"}}]
[]
[null,"CONCRETE, FORMWORK, REINFORCEMENT",{"$nulls":3},{"$f":"F306","v":{"v":0,"d":"R 0.00"}},{"$f":"G306","v":{"v":5505,"d":"R 5,505.00"}}]
[]
[null,"PRECAST CONCRETE",{"$nulls":3},{"$f":"F321","v":{"v":0,"d":"R 0.00"}},{"$f":"G321","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"MASONRY",{"$nulls":3},{"$f":"F376","v":{"v":0,"d":"R 0.00"}},{"$f":"G376","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"WATERPROOFING",{"$nulls":3},{"$f":"F406","v":{"v":0,"d":"R 0.00"}},{"$f":"G406","v":{"v":150,"d":"R 150.00"}}]
[]
[null,"ROOF COVERING",{"$nulls":3},{"$f":"F439","v":{"v":0,"d":"R 0.00"}},{"$f":"G439","v":{"v":3375,"d":"R 3,375.00"}}]
[]
[null,"CARPENTRY AND JOINERY",{"$nulls":3},{"$f":"F521","v":{"v":0,"d":"R 0.00"}},{"$f":"G521","v":{"v":8020,"d":"R 8,020.00"}}]
[]
[null,"CEILING",{"$nulls":3},{"$f":"F549","v":{"v":0,"d":"R 0.00"}},{"$f":"G549","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"FLOOR COVERING",{"$nulls":3},{"$f":"F558","v":{"v":0,"d":"R 0.00"}},{"$f":"G558","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"IRONMONGERY",{"$nulls":3},{"$f":"F590","v":{"v":0,"d":"R 0.00"}},{"$f":"G590","v":{"v":1100,"d":"R 1,100.00"}}]
[]
[null,"METAL WORKS",{"$nulls":3},{"$f":"F636","v":{"v":0,"d":"R 0.00"}},{"$f":"G636","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PLASTERING",{"$nulls":3},{"$f":"F655","v":{"v":0,"d":"R 0.00"}},{"$f":"G655","v":{"v":4425,"d":"R 4,425.00"}}]
[]
[null,"TILING",{"$nulls":3},{"$f":"F666","v":{"v":0,"d":"R 0.00"}},{"$f":"G666","v":{"v":3460,"d":"R 3,460.00"}}]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":3},{"$f":"F710","v":{"v":0,"d":"R 0.00"}},{"$f":"G710","v":{"v":1430,"d":"R 1,430.00"}}]
[]
[null,"GALZING",{"$nulls":3},{"$f":"F718","v":{"v":0,"d":"R 0.00"}},{"$f":"G718","v":{"v":0,"d":"R 0.00"}}]
[]
[null,"PAINT WORK",{"$nulls":3},{"$f":"F750","v":{"v":0,"d":"R 0.00"}},{"$f":"G750","v":{"v":5330,"d":"R 5,330.00"}}]
[]
[]
[null,"Carried to summary",{"$nulls":3},{"$f":"SUM(F757:F789)","v":{"v":0,"d":"R 0.00"}},{"$f":"SUM(G757:G789)","v":{"v":35115,"d":"R 35,115.00"}}]