{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["Summary","Fire Protection","HVAC","Wet services","Kitchen Equipment","LPG Installation","Fume Cupboards"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":15,"n_cols":3,"rows_kept":15,"merged":[[0,0,0,2],[1,0,1,2],[14,0,14,1]]}
["CN LEKALAKE SECONDARY SCHOOL"]
["SUMMARY: MECHANICAL INSTALLATION"]
["SECTION","DESCRIPTION","AMOUNT"]
[1,"Preliminary and General"]
[1,"Fire Protection"]
[2,"HVAC "]
[3,"Wet services"]
[4,"Kitchen Equipment"]
[5,"LPG Installation"]
[6,"Fume Cupboards"]
[null,"SUB TOTAL "]
[]
[]
[]
["TOTAL BID PRICE CARRIED TO MAIN BoQ PAGE 157"]

{"sheet":"Fire Protection","index":1,"n_rows":99,"n_cols":7,"rows_kept":99,"merged":[[56,0,56,5],[58,0,58,5],[98,0,98,5]]}
["ITEM","REF","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[2,null,"FIRE PROTECTION"]
[]
[null,null,"SITE WORKS"]
[null,null,"Supply, delivery, installation, commissioning and testing of Fire Protection Systems complete with connections and fittings in Accordance with SANS 10400 Part T and SANS 10400 Part W"]
[]
[2.1,"FHR/FH","Supply, delivery, installation, commissioning and testing of Fire Hydrants & Fire Hose Reels"]
[]
["2.1.1",null,"Φ100 Two Port Booster with Pressure Guage","No",1]
[]
["2.1.2",null,"Φ100mm Storz Hydrant – Φ100mm female BSP inlet & Φ100mm Storz outlet","No",1]
[]
["2.1.3",null,"Φ65mm Outlet Outdoor Type Fire Hydrant","No",4]
[]
["2.1.4",null,"Φ65mm, 30m MET Lay flat hose with coupling","No",2]
[]
["2.1.5",null,"Φ100mm Non Return Valve","No",8]
[]
["2.1.6",null,"Φ100mm Gate valves","No",18]
[]
["2.1.7",null,"Φ25mm Galvanised Steel (SABS 62) Piping for Connection of Fire Hose Reel","m",280]
[]
["2.1.8",null,"Φ50mm Galvanised Steel (SABS 62) Piping for Connection of Fire Hose Reel","m",350]
[]
["2.1.9",null,"Φ50mm Brass Non Return Valve (NRV)","No",12]
[]
["2010-02-01",null,"Φ50mm Brass Gate Valve (GV)","No",18]
[]
["2011-02-01",null,"Φ110mm Class 16 HDPE Piping Mains Connection","m",550]
[]
["2012-02-01",null,"Reducing Valves, Fittings and Accessories (Fire Hose Reels)","Sum",1]
[]
["2013-02-01",null,"Red Enamel Paint","L",20]
[]
["2014-02-01",null,"20 000 L Polyethylene water stoarge tank, 10 years warranty, food grade, LLDPE UV stabilised with inner black lining manufactured to SANS 1731 and 50mm outlet). Tank mounted on a concrete slab. ","No",4]
[]
["2015-02-01",null,"End suction Vertical centrifugal pump type, fire pump complete with 20 L/sec at a total head of 35m including by pass arrangement for periodical testing of the working of the pump. The pump shall be provided with mechanical seals and outlet manifolds. The above mounted on a base, pre-piped, pre-wired and tested, complete with control panels.","No",2]
[]
["2016-02-01",null,"Jockey Pump: 1 L/s @ 36m Head Jockey Electrically driven","No",0,"Incl."]
[]
[null,null,"PUMP ROOM PUMPHOUSE PIPEWORK & ELECTRICAL CONNECTIONS"]
["2017-02-01",null,"All pumphouse pipework and necessary valves as per tender drawings and specification","Sum",1,"Incl."]
[]
["2018-02-01",null,"All electrical panels, cabling,  safeties, switches, etc for electrical pump, jockey pump and any other equipment housed within the pump house","Sum",1,"Incl."]
[]
[2.2,"FE","Supply, delivery, installation, commissioning and testing of Fire Extinguishers complete with chevron board"]
[]
["2.2.1",null,"30m, 20mm diameter, non-swinging rotary pattern type Fire Hose Reels c/w Pressure Gauge","No",16]
[]
["2.2.2",null,"5 kg Carbon Dioxide Portable Fire Extinguishers","No",2]
[]
["2.2.3",null,"4.5 kg Dry Chemical Powder Portable Fire Extinguishers","No",46]
[]
["2.2.4",null,"Fire Extinguishers Cabinet for 5kg CO2","No",2]
[]
["TOTAL CARRIED FORWARD"]
["ITEM","REF","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD"]
[]
["2.2.5",null,"Fire Extinguishers Cabinet for 4.5kg DCP","No",46]
[]
["2.2.6",null,"Fire Blanket, 1.8mx1.8m Woven Fibreglass Fire Resistant Fabric with PVC Sleeve.","No",1]
[]
[2.3,"ES","Supply, delivery and installation of Evacuation Signage and Fire Escape Doors"]
[]
["2.3.1",null,"E1/E2, Size: 190mm x 380mm (h x w) Double sided photoluminescent sign framed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",2]
[]
["2.3.2",null,"E3, Size: 190mm x 380mm (h x w)  Double sided photoluminescent sign with back plate framed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",50]
[]
[2.4,"FS","Supply, delivery and installation of Fire Equipment Signage"]
["2.4.1",null,"F4, Size: 190mm x 570mm (h x w)  Double sided photoluminescent sign with back plate framed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",9]
[]
["2.4.2",null,"F16/F19, Size: 190mm x 380mm (h x w)  Double sided photoluminescent sign with back plate\nframed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",0]
[]
["2.4.3",null,"F13, Size: 190mm x 380mm (h x w)  Double sided photoluminescent sign with back plate\nframed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",23]
[]
["2.4.4",null,"F14, Size: 190mm x 380mm (h x w)  Double sided photoluminescent sign with back plate\nframed in natural anodised aluminium. Supply and install with steel wire and ceiling hook/onto mild steel bracket at 3.0 meters from finished floor level/mechanically mounted onto wall/fixture.","No",3]
[]
["2.5",null,"Supply, Delivery, Testing and Commissioning of an Manually Operated Alarm System  Complete to Comply with SANS 10139 and SANS 10400: T"]
[]
["2.5.1",null,"4 Loop Addressable Fire Control Panel with Batteries","No",1]
["2.5.2",null,"Addresseable ziton smoke detectors and bases","No",11]
["2.5.3",null,"Call points with bases","No",8]
["2.5.4",null,"Sounder, Red, Shallow Base, 100db with Complimentary Strobe Lights ","No",1]
["2.5.5",null,"2 Core PH 60 Cable, 1mm","m",800]
["2.5.6",null,"Conduit","m",400]
["2.5.7",null,"Fire Department Link - Remrad/SMS Communicator","No",1]
[]
[]
[]
["2.6",null,"Testing and Commissioning of all Fire Protection Installations"]
["2.6.1",null,"Testing and Commissioning of all Fire Protection Installations","Sum",1]
[]
[]
[]
[]
[]
["TOTAL CARRIED TO SUMMARY"]

{"sheet":"HVAC","index":2,"n_rows":224,"n_cols":10,"rows_kept":224,"merged":[[1,3,7,3],[1,4,7,4],[1,5,7,5],[1,6,7,6],[47,0,47,5],[49,0,49,5],[92,0,92,5],[94,0,94,5],[138,0,138,5],[140,0,140,5],[175,0,175,5],[177,0,177,5],[223,0,223,5]]}
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[3]
[null,null,"AIR CONDITIONING"]
[]
[null,null,"Supply and install Floor Plan Inverter heat pump air- conditioning units complete with fittings and fixtures, avm and (R410a) refrigerant gas for commisioning as specified and shown on the drawing. All units shall be IP addressable ready for BMS connection by others."]
[]
[]
[3.1,"MWSU - 01","Supply, delivery, installation, commissioning and testing of 2.7kW cooling capacityMid Wall Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection,\nremote controls and top-up refrigerant"]
["3.1.1",null,"Mid-Wall Split Unit, 2.7 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",8]
[]
["3.1.2",null,"Wired Controller","No",8]
[]
["3.1.3",null,"Chord for Wired Controller","m",40]
[]
["3.1.4",null,"Interface Adapter for Wired Controller","No",8]
[]
["3.1.5",null,"Refrigerant piping - Liquid","m",120]
[]
["3.1.6",null,"Refrigerant piping - Gas","m",120]
[]
["3.1.7",null,"Drain piping ID (Φ 25mm)","m",120]
[]
[]
["3.2","MWSU - 02","Supply, delivery, installation, commissioning and testing of 3.5kW cooling capacityMid Wall Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
["3.2.1",null,"Mid-Wall Split Unit, 3.5 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",3]
[]
["3.2.2",null,"Wired Controller","No",3]
[]
["3.2.3",null,"Chord for Wired Controller","m",15]
[]
["3.2.4",null,"Interface Adapter for Wired Controller","No",3]
[]
["3.2.5",null,"Refrigerant piping - Liquid","m",45]
[]
["3.2.6",null,"Refrigerant piping - Gas","m",45]
[]
["3.2.7",null,"Drain piping ID (Φ 25mm)","m",45]
{"$rows_empty":10}
["TOTAL CARRIED FORWARD"]
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD"]
[]
["3.3","MWSU - 03","Supply, delivery, installation, commissioning and testing of 5.3kW cooling capacity Mid Wall Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
["3.3.1",null,"Mid-Wall Split Unit, 5.3 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",1]
[]
["3.3.2",null,"Wired Controller","No",1]
[]
["3.3.3",null,"Chord for Wired Controller","m",5]
[]
["3.3.4",null,"Interface Adapter for Wired Controller","No",1]
[]
["3.3.5",null,"Refrigerant piping - Liquid","m",15]
[]
["3.3.6",null,"Refrigerant piping - Gas","m",15]
[]
["3.3.7",null,"Drain piping ID (Φ 25mm)","m",15]
[]
["3.4","MWSU - 04","Supply, delivery, installation, commissioning and testing of 6,4kW cooling capacity Mid Wall Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
["3.4.1",null,"Mid-Wall Split Unit, 6,4 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",3]
[]
["3.4.2",null,"Wired Controller","No",3]
[]
["3.4.3",null,"Chord for Wired Controller","m",15]
[]
["3.4.4",null,"Interface Adapter for Wired Controller","No",3]
[]
["3.4.5",null,"Refrigerant piping - Liquid","m",45]
[]
["3.4.6",null,"Refrigerant piping - Gas","m",45]
[]
["3.4.7",null,"Drain piping ID (Φ 25mm)","m",45]
[]
["3.5","RFCSU-05","Supply, delivery, installation, commissioning and testing of 8,0kW cooling capacity Ceiling Cassette Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
["3.5.1",null,"Round Flow Cassettee Unit, 8,0 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",1]
[]
["3.5.2",null,"Wired Controller","No",1]
[]
["3.5.3",null,"Chord for Wired Controller","m",6]
[]
["3.5.4",null,"Interface Adapter for Wired Controller","No",1]
[]
[]
[]
["TOTAL CARRIED FORWARD"]
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":8},"`"]
["3.5.5",null,"Refrigerant piping - Liquid","m",15]
[]
["3.5.6",null,"Refrigerant piping - Gas","m",15]
[]
["3.5.7",null,"Drain piping ID (Φ 25mm)","m",15]
[]
["3.6","RFCSU-06","Supply, delivery, installation, commissioning and testing of 10kW cooling capacityCeiling Cassette Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and\nconnection, remote controls and top-up refrigerant"]
["3.6.1",null,"Round Flow Cassettee Unit, 10 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",2]
[]
["3.6.2",null,"Wired Controller","No",1]
[]
["3.6.3",null,"Chord for Wired Controller","m",6]
[]
["3.6.4",null,"Interface Adapter for Wired Controller","No",1]
[]
["3.6.5",null,"Refrigerant piping - Liquid","m",30]
[]
["3.6.6",null,"Refrigerant piping - Gas","m",30]
[]
["3.6.7",null,"Drain piping ID (Φ 25mm)","m",30]
[]
["3.7","RFCSU-08","Supply, delivery, installation, commissioning and testing of 16,0kW cooling capacityCeiling Cassette Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
["3.7.1",null,"Round Flow Cassettee Unit, 16,0 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",1]
[]
["3.7.2",null,"Wired Controller","No",1]
[]
["3.7.3",null,"Chord for Wired Controller","m",6]
[]
["3.7.4",null,"Interface Adapter for Wired Controller","No",1]
[]
["3.7.5",null,"Refrigerant piping - Liquid","m",15]
[]
["3.7.6",null,"Refrigerant piping - Gas","m",15]
[]
["3.7.7",null,"Drain piping ID (Φ 25mm)","m",15]
{"$rows_empty":8}
["TOTAL CARRIED FORWARD"]
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":8},"`"]
[]
["3.7","DSU-01","Supply, delivery, installation, commissioning and testing of 16,0kW cooling capacity Ducted Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, drain pump, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
[]
["3.7.1",null,"Ducted Split Unit, 28 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",1]
[]
["3.7.2",null,"Wired Controller","No",1]
[]
["3.7.3",null,"Chord for Wired Controller","m",6]
[]
["3.7.4",null,"Interface Adapter for Wired Controller","No",1]
[]
["3.7.5",null,"Refrigerant piping - Liquid","m",15]
[]
["3.7.6",null,"Refrigerant piping - Gas","m",15]
[]
["3.7.7",null,"Drain piping ID (Φ 25mm)","m",15]
[]
["3.8","DSU-02","Supply, delivery, installation, commissioning and testing of 20,0kW cooling capacity Ducted Split Unit(Heat Pump, Inverter, R410) complete with insulated refrigerant piping, drain pump, condensate drains, trunking, electric wiring and connection, remote controls and top-up refrigerant"]
[]
["3.8.1",null,"Ducted Split Unit, 20 kW cooling capacity Inverter Heat Pump (SABS Approved or Equivalent)","No",2]
[]
["3.8.2",null,"Wired Controller","No",2]
[]
["3.8.3",null,"Chord for Wired Controller","m",12]
[]
["3.8.4",null,"Interface Adapter for Wired Controller","No",2]
[]
["3.8.5",null,"Refrigerant piping - Liquid","m",30]
[]
["3.8.6",null,"Refrigerant piping - Gas","m",30]
[]
["3.8.7",null,"Drain piping ID (Φ 25mm)","m",30]
[]
[]
["TOTAL CARRIED FORWARD"]
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["TOTAL BROUGHT FORWARD",{"$nulls":8},"`"]
[null,null,"Ventilation"]
[null,null,""]
["3.9",null,"Supply and install Inline axial flow fans complete with  in lined attenuators, vibration isolation, square to round transformations, supports and electric controls."]
[]
["3.9.1","FASF-01","Dia 150mm Inline tube Fresh air Fan 120l/s @ 102 Pa c/w 2 x 1.50 Sound Attenuators with pods and electric box, timer controlled.","No",1]
["3.9.2","FASF-02","Dia 200mm Inline tube Fresh air Fan 217l/s @ 102 Pa c/w 2 x 1.50 Sound Attenuators with pods and electric box, timer controlled.","No",1]
["3.9.3","FASF-03","Dia 300mm Inline tube Fresh air Fan 300l/s @ 150 Pa c/w 2 x 1.50 Sound Attenuators with pods and electric box, timer controlled.","No",1]
["3.9.4","WEF-01","Wall mounted Extract Fan with a duty of 50l/s @ 50 pa c/w inside and outside louvres, outside louvre to be weather proof and have a birds barrier, electrical box, timer controlled.","No",1]
["3.9.5","EAF-01","Dia 300mm Inline tube Extract air Fan 225l/s @ 150 Pa c/w 2 x 1.50 Sound Attenuators with pods and electric box, timer controlled.","No",3]
["3.9.6","WL-01","Weather louvre (200 x 200) C/W inspect screen","No",2]
["3.9.7","WL-02","Weather louvre (300 x 300) C/W inspect screen","No",1]
["3.9.8","WL-03","Weather louvre (350 x 350) C/W inspect screen","No",4]
[]
["3.10",null,"Supply and install Round un-insulated galvanized low pressure ducting below concrete soffits, including support mechanisms."]
[]
["3.10.1",null,"Ø500 circular duct","m",{"v":20.7,"d":"21"}]
[]
["3.10.2",null,"Ø400 circular duct","m",{"v":16.099999999999998,"d":"16"}]
[]
["3.10.3",null,"Ø350 circular duct","m",{"v":9.2,"d":"9"}]
[]
["3.10.4",null,"Ø300 circular duct","m",{"v":13.799999999999999,"d":"14"}]
[]
["3.10.5",null,"Ø250 circular duct","m",{"v":34.5,"d":"35"}]
[]
["3.10.6",null,"Ø200 circular duct","m",{"v":32.199999999999996,"d":"32"}]
[]
["3.10.7",null,"Ø150 circular duct","m",{"v":9.2,"d":"9"}]
[]
["3.10.8",null,"Ø100 circular duct","m",{"v":9.2,"d":"9"}]
[]
["3.11",null,"ACCESSORIES"]
[]
["3.11.1",null,"150mm dia. Extract Air Disc Valves complete with\n150mm dia. spigot connection","No",18]
[]
["3.11.2",null,"200mm dia. Supply Air Disc Valves complete with\n200mm dia. spigot connection","No",8]
[]
["3.11.3",null,"250mm dia. Supply Air Disc Valves complete with\n250mm dia. spigot connection","No",12]
[]
["3.11.4",null,"600 x 1200mm Return Air Grille, Complete with plenum box with filters and connection spigots.","No",6]
[]
["3.12",null,"Testing and Commissioning"]
[null,null,""]
["3.12.1",null,"Testing and Commissioning of all Installations, and CoC","Sum",1]
[]
["TOTAL CARRIED TO SUMMARY"]

{"sheet":"Wet services","index":3,"n_rows":48,"n_cols":7,"rows_kept":48,"merged":[[47,0,47,5]]}
["ITEM","REF ","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[4,null,"WET SERVICES "]
[]
[null,null,"Supply, delivery, installation, commissioning and testing of new water supply piping, c/w connections and fittings. "]
[]
["4.1","SW","Supply, delivery, installation, commissioning and testing of cold/hot water supply system"]
["4.1.1",null,"Φ15mm PN10 PPR (Polypropylene Random Copolymer) piping for Connection of Hot Water Supply Piping complete with connections, reducers and fittings","m","0"]
["4.1.2",null,"Φ15mm PN16 PPR (Polypropylene Random Copolymer) Piping for Connection of Cold Water Supply Piping complete with connections, reducers and fittings","m","0"]
["4.1.3",null,"Φ22mm PN16 PPR (Polypropylene Random Copolymer) Piping for Connection of Hot Water Supply Piping complete with connections, reducers and fittings","m","0"]
["4.1.4",null,"Φ22mm  PN10 PPR (Polypropylene Random Copolymer) Piping for Connection of Cold Water Supply Piping complete with connections, reducers and fittings","m","0"]
["4.1.5",null,"Φ28mm PN16 PPR (Polypropylene Random Copolymer) Ring Main Piping for Connection of Cold Water Supply Piping complete with connections, reducers and fittings","m","0"]
["4.1.6",null,"Φ28mm  PN 10 PPR (Polypropylene Random Copolymer) Ring Main Piping for Connection of Cold Water Supply Piping complete with connections, reducers and fittings","m","0"]
[]
["4.2",null,"Supply and installation of copper pipes with fittings chased into the wall"]
["4.2.1",null,"15mm copper pipe","m","120"]
["4.2.2",null,"22mm copper pipe","m","80"]
["4.2.3",null,"28mm copper pipe","m","40"]
["4.2.4",null,"63mm copper pipe","m","0"]
[]
["4.3",null,"Ancillaries"]
["4.3.1",null,"SABS Approved CopperAdjustable Pressure Reducing Valves","Sum","8"]
["4.3.2",null,"Stop/Gate Valves","Sum","2"]
["4.3.3",null,"Accessories (Braided Connectors, Elbows, Tees and etc.)","Sum","1"]
[]
["4.4",null,"Solar Geysers"]
["4.4.1",null,"150L Indirect Solar Geyser","No","4"]
["4.4.2",null,"250L Indirect Solar Geyser","No","4"]
["4.4.3",null,"2.5m² Flat Plate Collector (SABS)","No","8"]
["4.4.4",null,"Glycol 5L Bottle (food grade)","No","4"]
["4.4.5",null,"Pipe 22x5.5m 460/0 Copper Tube","No","12"]
["4.4.6",null,"Insul 7/8x1/2 Insuflex 22x13mmx1.83m","m","60"]
["4.4.7",null,"Bottom Angle Bracket","No","12"]
["4.4.8",null,"Consumables","Sum","1"]
["4.4.9",null,"Parts Kit","Sum","12"]
["4.4.10",null,"Hydroboil","sum","4"]
[]
["4.5","TC","Testing and Commissioning  "]
["4.5.1",null,"Testing and Commissioning of all Installations","Sum","1"]
{"$rows_empty":9}
["TOTAL CARRIED TO SUMMARY"]

{"sheet":"Kitchen Equipment","index":4,"n_rows":38,"n_cols":7,"rows_kept":38,"merged":[[37,0,37,5]]}
["`","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[5,null,"KITCHEN EQUIPMENT"]
[]
["5.1",null,"Supply, delivery, installation, comissioning and testing of New Kitchen Equipment."]
["5.1.1",null,"Boiling Table Gas - Commercial - 4 Burner Straight","No",1]
["5.1.2",null,"Boiling Table Gas - Commercial - 4 Burner Staggered","No",1]
["5.1.3",null,"Tilting Pans - Electric","No",1]
["5.1.4",null,"3 Pan Gas Fryer (20 Lt Pan)","No",1]
["5.1.5",null,"Double Bowl Pot Sink - 1700 X 650 X900Mm","No",1]
["5.1.6",null,"Crockery Rack Mobile - F/Standing -1130Mm (1130 X 600 X 1700Mm)","No",1]
["5.1.7",null,"Double Bowl Sink - 1700 X 650 X900Mm","No",1]
["5.1.8",null,"1700 Tier Dirties Receiving Table","No",1]
["5.1.9",null,"4 Tier Pot Rack - Floor Standing","No",1]
["5.1.10",null,"Knee Activated Hand Wash Basin","No",1]
["5.1.11",null,"6 Division Floor Model Bain Marie No Storage","No",1]
["5.1.12",null,"Splashback Table - 1100 X 650 X 900Mm","No",2]
["5.1.13",null,"Splashback Table - 1700 X 650 X 900Mm","No",3]
["5.1.14",null,"5 Tier Shelving-Galvanized-380Mm","No",18]
["5.1.15",null,"Xevc-0511-Ezrm Combi Steam Oven - Unox Cheftop 5","No",1]
["5.1.16",null,"Potato Peeler Anvil - 12Kg With Timer","No",1]
["5.1.17",null,"Veg Prep Machine - Cl52E - (400 Servings)","No",1]
["5.1.18",null,"Dunnage Rack - 900X600X300Mm","No",4]
["5.1.19",null,"Chest Freezers","No",1]
["5.1.20",null,"Coldroom 1.8M X 1.8M","No",1]
["5.1.21",null,"Extraction Canopy 2600 X 2250 X600mm Boxed Type Island Canopy.","No",1]
[null,null,{"$f":"PROPER(J27)","v":""}]
["5.2",null,"Testing and Commissioning"]
["5.2.1",null,"Testing and Commissioning of all Installations, and CoC","Sum",1]
[null,null,""]
[null,null,""]
[null,null,""]
[]
[]
[]
[]
[]
["TOTAL CARRIED TO SUMMARY"]

{"sheet":"LPG Installation","index":5,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[50,0,50,5]]}
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[6,null,"LPG INSTALLATIONS"]
[]
[6.1,null,"Supply, delivery, installation, comissioning and testing of LPG reticulation, complete with CoC."]
["6.1.1",null,"48kg LPG Cylinder","No",6]
["6.1.2",null,"4x48kg Gas Cage","No",1]
["6.1.3",null,"2x48kg Gas Cage","No",1]
["6.1.4",null,"LPG supply Manifold (2 Points), complete with regulator, isolation valves and fittings","No",3]
["6.1.5",null,"1/2'' Corrugated TracPipe per Meter","m",80]
["6.1.6",null,"1/2'' Gas Valves","No",15]
[]
[]
["6.2",null,"Testing and Commissioning"]
["6.2.1",null,"Testing and Commissioning of all Installations, and CoC","Sum",1]
{"$rows_empty":35}
["TOTAL CARRIED TO SUMMARY"]

{"sheet":"Fume Cupboards","index":6,"n_rows":44,"n_cols":7,"rows_kept":44,"merged":[[43,0,43,5]]}
["ITEM","REFERENCE","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[7,null,"FUME CABINETS"]
[]
[null,null,"Supply, delivery, installation and commissioning of fume cabines complets with extraction fans, ductting, electrical connections and controls."]
[]
["7.1","FC01","X-Flo 900 white powdercoated Fume Cabinet, complete with 0.37kW, 230V Single Phase wall/roof munted Fan and ducting.","No",1]
[]
["7.2",null,"TEST & COMMISSION"]
["7.2.1",null,"Test and Commission","Item",1]
{"$rows_empty":33}
["TOTAL CARRIED TO SUMMARY"]