{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["0164307","Deviation Schedule","Test Schedule","Eskom Drawing"],"not_rendered":{"images":3,"external_links":2,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"0164307","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,0,3,7],[5,1,5,6],[6,1,6,6],[9,2,9,3],[10,2,10,3],[11,3,11,4],[17,3,17,4],[24,3,24,4],[27,2,27,4],[28,2,28,4],[29,3,29,4],[31,3,31,4],[33,3,33,4],[38,0,38,6],[39,1,40,6],[41,1,41,6],[43,0,43,6],[45,0,45,1],[50,2,50,3]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"BRACKET,STRUT SWIVEL WOOD POLE D3150"]
["NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",164307,{"v":164307,"d":"0164307"}]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier indelibly marked. \n- All products must be properly identified by a durable label that cannot be torn or pulled off for 12 months after purchased to indicate manufacturer, size/stranding of conductor, batch number and catalogue number.\n- The label shall be durable enough to ensure that it remains in place and is legible up to at least 12 months after installation. \n\n","240-75883830\n\n\n\n\n\n\n\n\n\n","YES"]
[null,"1.1.7","·","Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.1.7.1",null," For use on:\n- Wood strut pole to wood pole                                           "," Eskom DDT-3150","YES"]
[null,"1.1.7.2",null,"Swivel braket "," Eskom DDT-3150","YES"]
[null,"1.1.7.3",null,"Dimensions and angles                                                                                                                                                                                                                                                                                         - All dimensions and angles are in accordance with the Eskom specificaion."," Eskom DDT-3150","YES"]
[null,"1.1.7.4",null,"Fasteners                              - Are all fasterners (bolts, nuts,threaded rods and screws)  complying with their relevant SANS specifications?",null,"YES"]
[null,"1.1.7.5",null,"Welds                                      - All welds to be 8mm continuous seal weld and conform to SANS 10162-1"," Eskom DDT-3150","YES"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom  (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Material"," Eskom DDT-3150, 240-75883830","GRADE S355JR STEEL "]
[null,"1.2.2",null,"Has the steel been hot dip galvanized as per SANS 121"," Eskom DDT-3150, 240-75883830","YES"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,3,null,"Packaging"]
[null,3.1,null,"All of the assembly components to be packaged as a unit","DDT-3150","YES"]
[null,3.2,null,"All packaging is to be suitable for storage outdoors","DDT-3150","YES"]
[null,3.3,null,"Installation instructions provided in packaging",null,"YES"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[null,"NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":43,"n_cols":6,"rows_kept":43,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[5,0,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[32,0,32,6],[33,0,33,6],[35,0,35,6],[37,0,37,1],[38,2,38,3],[42,2,42,3]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" DDT-3150 - STRUT BRACKET  FOR WOOD, CONCRETE AND STEEL POLES"]
["SAP No: 164307"]
[]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom.The deviation must be filled even if there are no deviations. Post evaluation,  the letter of garantee to confim that the product is not compromised even though it was not tested according to the latest  Standard (240-75883830)"]
["Item","Clause","Description of Deviation"]
{"$rows_empty":25}
["ESKOM TENDER E2719DXLIMOU"]
["NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":26,"n_cols":6,"rows_kept":26,"merged":[[0,0,0,6],[1,0,1,7],[2,0,2,7],[3,1,3,5],[4,1,4,5],[5,0,5,7],[16,1,16,5],[17,1,17,8],[18,1,18,8],[21,1,21,2],[25,1,25,2]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[" DDT-3150 - STRUT BRACKET  FOR WOOD, CONCRETE AND STEEL POLES"]
[null,"The test reports are required for the stated SAP number listed on this sheet"]
[]
["SAP No: 164307"]
[]
[null,1,2,3,null,4]
[null,"Item ","Description","Standard","Clause No.","Report No."]
[null,"2.2.1","Tensile properties","240-75883830","3.2.2.1"]
[null,"2.2.2","Impact resistance tests","240-75883830","3.2.2.2"]
[null,"2.2.3","Bending properties","240-75883830","3.2.2.3 "]
[null,"2.2.4","Material hardness","240-75883830","3.2.2.4 "]
[null,"2.2.5","Non-destructive testing of welds","240-75883830","4.2.3"]
[null,"2.2.6","Galvanizing of the product body","240-75883830","6. "]
[]
[null,"NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Eskom Drawing","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}