{"text_format":"3","workbook":"xls","n_sheets":24,"sheets":["1200","1300","1400","1500","1600","1700","1800","2100","2300","3100","3200","3300","3400","3500","4100","4200","5600","5700","5900","8100","D","Summary","Scope of Work","Sheet1"],"not_rendered":{"external_links":9,"defined_names":171},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1200","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[39,1,40,1],[44,1,44,3]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL OF QUANTITIES"]
["NB:               TENDERERS MUST COMPLETE THE BILL OF QUANTITIES IN BLACK INK."]
["BILL A : ROAD CONSTRUCTION                                                                                                               ",{"$nulls":4},"SECTION 1200"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["B12.04","Existing services to be relocated and/or protected\n"]
[null,"\n"]
[null,"(a)    Allow a provisional sum for existing services to be relocated and/or protected as ordered by the engineer","Pro Sum",{"v":1,"d":"1.00"},{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[null,"(b)    Handling costs and profit in respect of subitem B12.06(a)","%",{"v":20000,"d":"20,000.00"}]
[]
["B12.05","Alterations to services by the Contractor"]
[]
[null,"(a)    All services","Pro Sum",{"v":1,"d":"1.00"},{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
["12/22.07L","Cast in situ concrete and formwork:"]
[]
[null,"(a) In class A bedding, screeds and the encasing for pipes including formwork"]
[null,"(i)     Class 15/19 concrete","m³",{"v":5,"d":"5.00"}]
[]
["12/22.26L","Hand excavation to determine the positions of existing services","m³",{"v":100,"d":"100.00"}]
[null,"PROVISIONAL SUM"]
[]
[null,"(a) Payment for EMP services","Pro Sum",{"v":1,"d":"1.00"},80000,{"v":80000,"d":"80,000.00"}]
[null,"(b) Payment for OHS Agent","Pro Sum",{"v":1,"d":"1.00"},60000,{"v":60000,"d":"60,000.00"}]
[null,"(c) Payment for Social Facilitation","Pro Sum",{"v":1,"d":"1.00"},120000,{"v":120000,"d":"120,000.00"}]
[null,"(d) Handling cost and profit in respect of subitem 12.04 (a-c)","%",{"v":260000,"d":"260,000.00"}]
[]
[null,"Liaison Officer"]
[null,"(a) Remuneration of Community Liaison Officer","Pro Sum",{"v":4,"d":"4.00"},{"v":4500,"d":"4,500.00"},{"v":18000,"d":"18,000.00"}]
[null,"(b) Contractor's charge to allow for handling costs and profit on item B12.02 (a)","%",{"v":18000,"d":"18,000.00"}]
[]
[null,"(c) Stipend for PSC members","Pro Sum",{"v":1,"d":"1.00"},{"v":4000,"d":"4,000.00"},{"v":4000,"d":"4,000.00"}]
[null,"(d) Contractor's charge to allow for handling costs and profit on item B12.02 (c)","%",{"v":4000,"d":"4,000.00"}]
[]
[null,"Project Nameboard as per drawing KG2022/74/09","No.",{"v":1,"d":"1.00"}]
[]
[]
[]
[]
[1200,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"1300","index":1,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1300"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS"]
[]
["B13.01","The Contractor's general obligations:"]
[null,"(a)    Fixed obligations","Lump Sum",{"v":1,"d":"1.00"}]
[]
[null,"(b)    Value-related obligations","Lump Sum",{"v":1,"d":"1.00"}]
[]
[null,"(c)    Time-related obligations ","months",{"v":4,"d":"4.00"}]
[]
[null,"NB    The combined total tendered for subitems (a), (b) and (c) shall not exceed 15% of the Tender Sum (excl VAT)"]
[]
[]
[null,"NB   The combined total tendered for Items E13.01, E13.02, E13.03 shall not be less\nthan 15% of the Tender Sum."]
[null,"(excluding CPA, contingencies"]
[null,"and VAT)."]
{"$rows_empty":21}
[1300,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"1400","index":2,"n_rows":105,"n_cols":6,"rows_kept":105,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[51,0,51,5],[52,0,52,5],[53,0,53,5],[55,4,55,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1400"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"HOUSING, OFFICES AND LABORATORIES FOR THE ENGINEER'S SITE PERSONNEL"]
[]
[14.01,"Office and laboratory accommodation:"]
[]
[null,"(a)    Offices (interior floor space only) ","m²",{"v":60,"d":"60.00"}]
[]
[null,"(e)    Ablution units x 2","m²",{"v":10,"d":"10.00"}]
[]
[]
[14.02,"Office and laboratory furniture:"]
[]
[null,"(a)    Chairs","number",{"v":12,"d":"12.00"}]
[]
[null,"(d)    Desks, complete with drawers and locks","number",{"v":2,"d":"2.00"}]
[]
[null,"(e)    Drawing tables","number",{"v":1,"d":"1.00"}]
[]
[null,"(f)     Conference tables","number",{"v":1,"d":"1.00"}]
[]
[14.03,"Office and laboratory fittings, installations and equipment:"]
[null,"(a)    Items measured by number:"]
[]
[null,"(i)     220/250 volt power points","number",{"v":2,"d":"2.00"}]
[]
[null,"(iii)    Double 80 watt fluorescent-light fittings complete with ballast and tubes","number",{"v":2,"d":"2.00"}]
[]
[null,"(xi)    Air-conditioning units with 2,2 kW minimum capacity, mounted and with own power connection","number",{"v":1,"d":"1.00"}]
[]
[null,"(xii)   Heater, space-heating type, minimum capacity 1,5 kW","number",{"v":1,"d":"1.00"}]
[]
[null,"(xiv)  General-purpose steel cupboards with shelves","number",{"v":1,"d":"1.00"}]
[]
[null,"(xvi)  Refrigerators","number",{"v":1,"d":"1.00"}]
[]
[null,"(x)    Fire extinguishers, 9,0 kg all purpose dry powder type, complete, mounted on wall with brackets","number",{"v":2,"d":"2.00"}]
[]
[]
[]
[]
[]
[]
[1400,"Carried forward"]
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":3},"SECTION 1400"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"Brought forward"]
[]
[]
["14.03   (b)(cont)","(b)    Prime-cost items and items paid for in a lump           sum:"]
[null,"(i)     The provision of telephone service,"]
[null,"         including the cost of calls in"]
[null," connection with contract administration "]
[null," and telephone rental","Prov Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[null,"(ii)     Handling costs and profit in respect of"]
[null,"         subsubitem B14.03(b)(i) above","%",{"v":10000,"d":"10,000.00"}]
[]
[null,"(iii)    The provision of a direct independent"]
[null,"         telephone line for the Engineer,"]
[null,"         including the cost of calls in "]
[null,"         connection with contract administration"]
[null,"         and telephone rental","Prov Sum",{"v":1,"d":"1.00"},{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"}]
[]
[null,"(iv)   Handling costs and profit in respect of"]
[null,"        subsubitem 14.03(b)(iii) above","%",{"v":5000,"d":"5,000.00"}]
[]
[]
[14.04,"Car-ports",{"$nulls":3},""]
[{"$nulls":5},""]
[null,"Car ports as specified, at offices and laboratory buildings","No",4]
[]
[14.08,"Services: "]
[]
[null,"(a) Services at offices and laboratories:"]
[]
[null,"      (i) Fixed costs","Lump Sum",1]
[]
[null,"      (ii) Running costs","Month",4]
[]
[14.09,"Combined office and laboratory accommodation","Lump Sum",1]
[]
["14.10","Provision of photostat facilities","Month",4]
[{"$nulls":5},""]
{"$rows_empty":8}
[1400,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"1500","index":3,"n_rows":103,"n_cols":8,"rows_kept":103,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[59,0,59,5],[60,0,60,5],[61,0,61,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1500"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"ACCOMMODATION OF TRAFFIC"]
[]
["B15.01","Accommodating traffic and maintaining"]
[null,"temporary deviations","km",{"v":0.815,"d":"0.82"}]
[]
[15.02,"Earthworks for temporary deviations:"]
[]
[null,"(a)    Shaping of temporary deviations","km",{"v":0.815,"d":"0.82"}]
[]
[null,"(b)     Cut and borrow to fill","m³",{"v":200,"d":"200.00"}]
[]
[null,"(c)    Cut to spoil","m³",{"v":50,"d":"50.00"}]
[]
[]
["B15.03","Temporary traffic-control facilities:"]
[]
[null,"(a)    Flagmen","Man-day",{"v":440,"d":"440.00"}]
[]
[null,"(b)    Portable STOP and GO-RY signs","number",{"v":4,"d":"4.00"}]
[]
[null,"(e)    Road signs, R- and TR-series, (900mm dia)","number",{"v":8,"d":"8.00"}]
[]
[null,"(f)     Road signs, TW-series, (1200mm sides)"]
[]
[null,"(i)     Single","number",{"v":4,"d":"4.00"}]
[]
[null,"(ii)     Mounted back to back","number",{"v":4,"d":"4.00"}]
[]
[null,"(h)    Delineators (DTG50J)"]
[]
[null,"(i)     Single","number",{"v":40,"d":"40.00"}]
[]
[null,"(ii)     Mounted back to back","number",{"v":40,"d":"40.00"}]
[]
[null,"(i)     Movable barricade/road sign combination"]
[null,"        Chevron and Road Closed type","number",{"v":4,"d":"4.00"}]
[]
[null,"(j)   Traffic Cones","number",{"v":40,"d":"40.00"}]
[]
[null,"(n)    Provision of high visibility safety jackets ","number",{"v":6,"d":"6.00"}]
[]
[15.04,"Relocation of traffic-control facilities","Lump Sum",{"v":1,"d":"1.00"}]
[]
[15.06,"Watering of temporary deviations ","kilolitre",{"v":2200,"d":"2,200.00"}]
[]
[]
[]
[1500,"Carried forward"]
[]
[]
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1500"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"brought forward"]
[]
[]
["B15.10","Accommodation of traffic where the road "]
[null,"is constructed in half-widths","km",{"v":0.815,"d":"0.82"}]
[]
[]
["B15.14","Provision of traffic safety equipment for use"]
[null,"by the engineer:"]
[]
[null,"(a)  Emergency rotating mini lightbar for mobile ","No",{"v":3,"d":"3.00"}]
[null,"       use"]
[]
["B15.16","Provision of traffic safety "]
[]
[null,"(c) Traffic Satety Officer","month",{"v":4,"d":"4.00"}]
[]
[null,"(d) Traffic Safety Vehicle (s)","month",{"v":4,"d":"4.00"},{"$nulls":3},0]
{"$rows_empty":18}
[1500,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"1600","index":4,"n_rows":3901,"n_cols":8,"rows_kept":3901,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[6,0,6,7]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION",{"$nulls":5},"SECTION 1600"]
[]
[]
["ITEM","DESCRIPTION",null,null,"UNIT","QUANTITY","RATE","AMOUNT"]
["NO"]
[]
[]
[null,"OVERHAUL"]
[]
[]
[]
["16.01","Overhaul on material hauled in excess of a "]
[null,"free-haul distance of 0,5 km, for haul up to"]
[null,"or through 1,0 km (restricted overhaul)",null,null,"m³",{"v":5190,"d":"5,190"}]
[]
[]
["16.02","Overhaul on material hauled in excess of "]
[null,"1,0 km (ordinary overhaul)",null,null,"m³-km",{"v":2595,"d":"2,595"}]
{"$rows_empty":51}
[" 1600","TOTAL CARRIED TO SUMMARY"]
{"$rows_empty":3616}
[null,null,"Rock fill (as specified in Subclause 3209(c))"]
[]
[]
[]
[]
[]
[]
[null,"Sand fills (as described in Clause 3302,  including "]
{"$rows_empty":177}
[null,"Contractor, including all haul:"]
{"$rows_empty":23}
[null,null,"Rock fill (as specified in Subclause 3209(c))"]

{"sheet":"1700","index":5,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1700"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"CLEARING AND GRUBBING"]
[]
[]
[]
[17.05,"Cleaning out of hydraulic structures:"]
[]
[null,"(a)    Pipes with an internal diameter up to and"]
[null," including 750 mm","m³",{"v":10,"d":"10.00"}]
{"$rows_empty":28}
[1700,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"1800","index":6,"n_rows":67,"n_cols":6,"rows_kept":67,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 1800"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[{"v":18,"d":"18.00"},"DAYWORKS"]
[]
["B18.01","PERSONNEL"]
[]
[null,"(a) Unskilled","Hour",{"v":200,"d":"200.00"}]
[]
[null,"(b) Semi-skilled","Hour",{"v":150,"d":"150.00"}]
[]
[null,"(c) Skilled","Hour",{"v":300,"d":"300.00"}]
[]
[null,"(d) Foremen","Hour",{"v":450,"d":"450.00"}]
[]
["B18.02","Equipment"]
[]
["(a)","Motor grader (140G/H)","Hour",{"v":50,"d":"50.00"}]
[]
["(b)","Excavator (30 ton)","Hour",{"v":60,"d":"60.00"}]
[]
["(c)","Dozer (kW)","Hour",{"v":10,"d":"10.00"}]
[]
["(d)","Rubber tyred loader (60 kW)","Hour",{"v":50,"d":"50.00"}]
[]
["(e)","Tractor-loader-backhoe (55 kW)","Hour",{"v":10,"d":"10.00"}]
[]
["(f)","Pedestrian vibrating roller (0,5 ton)","Hour",{"v":10,"d":"10.00"}]
[]
["(g)","Pedestrian vibrating roller (1,4 ton)","Hour",{"v":10,"d":"10.00"}]
[]
["(h)","Self propelled vibrating roller (80 kW)","Hour",{"v":10,"d":"10.00"}]
[]
["(i)","Pneumatic tyred roller (60 kW, 20 ton)","Hour",{"v":10,"d":"10.00"}]
[]
["(j)","Tip truck"]
[null,"      (i) 6m³","Hour",{"v":10,"d":"10.00"}]
[]
[null,"      (ii) 10m³","Hour",{"v":10,"d":"10.00"}]
[]
["(k)","Water spray truck (18000 litre)","Hour",{"v":30,"d":"30.00"}]
[]
["(l)","250 cmf compressor (7 m³/min) complete"]
[null,"with 2 tools and operators","Hour",{"v":10,"d":"10.00"}]
[]
["(m)","600 cmf compressor (17 m³/min) complete"]
[null,"4 tools and operators","Hour",{"v":10,"d":"10.00"}]
[]
["B18.03","Materials:"]
[]
[null,"(a)Procurement of materials","Prov sum",{"v":1,"d":"1.00"},20000,{"v":20000,"d":"20,000.00"}]
[]
[null,"(b) Contractor's handling costs, profit and all other charges in respect of B18.03","%",{"v":20000,"d":"20,000.00"}]
[]
["B18.04","Transport:"]
[]
[null,"(a) LDV (1 ton)","km",{"v":30,"d":"30.00"}]
[]
[null,"(b) Flatbed truck (5 ton)","km",{"v":30,"d":"30.00"}]
[]
[null,"(c') Lowbed truck max (30 ton)","km",{"v":10,"d":"10.00"}]
[]
[1800,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"2100","index":7,"n_rows":3640,"n_cols":9,"rows_kept":3640,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6],[6,0,6,8]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION",{"$nulls":6},"SECTION 2100"]
[]
[]
["ITEM",null,"DESCRIPTION",null,null,"UNIT","QUANTITY","RATE","AMOUNT"]
["NO"]
[]
[]
["LIC",null,"DRAINS"]
[]
["21.01","LI","Excavation for open drains:"]
[]
[null,null,"(a)","Excavating soft material situated within the "]
[{"$nulls":3},"following depth ranges below the surface "]
[{"$nulls":3},"level:"]
[]
[{"$nulls":3},"(i)","0 m up to 1,5 m","m³",{"v":4575,"d":"4,575"}]
[]
[null,null,"(b)","Extra over subitem 21.01(a)(i) for excavation "]
[{"$nulls":3},"in hard material, irrespective of depth",null,"m³",915]
[]
["21.02","LI","Clearing and shaping existing open drains",null,null,"m³",500]
{"$rows_empty":46}
[" 2100",null,"TOTAL CARRIED TO SUMMARY"]
{"$rows_empty":3357}
[{"$nulls":3},"Rock fill (as specified in Subclause 3209(c))"]
[]
[]
[]
[]
[]
[]
[null,null,"Sand fills (as described in Clause 3302,  including "]
{"$rows_empty":177}
[null,null,"Contractor, including all haul:"]
{"$rows_empty":23}
[{"$nulls":3},"Rock fill (as specified in Subclause 3209(c))"]

{"sheet":"2300","index":8,"n_rows":120,"n_cols":6,"rows_kept":120,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[61,0,61,5],[62,0,62,5],[63,0,63,5],[64,0,64,5]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 2300"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"CONCRETE KERBING, CONCRETE CHANNELLING, CHUTES AND DOWNPIPES, AND CONCRETE LINING"]
[]
[23.01,"Concrete kerbing, Straight and Curved"]
[null,"including Joints, class 25/19 concrete:"]
[]
[null,"(a) Prefaricated mountable kerb, SABS 927 Fig 8c,","m",{"v":1352,"d":"1,352"}]
[null,"as shown on the drawings"]
[]
[23.03,"Concrete chutes(typical designs):"]
[]
[null,"(a) Inlet structures, for chutes down side slopes,"]
[null," class 30/19 concrete, complete as shown on"]
[null," the drawings: KG2022/74/06","m",20]
[23.05,"Inlet, outlet, transition and similar "]
[null,"structures (Typical designs)"]
[]
[null,"(a) Inlet structures, for chutes down side slopes,","No",3]
[null," class 30/19 concrete, complete as shown on"]
[null," the drawings: KG2022/74/06"]
[]
[null,"(c) Combined double kerb inlet and manhole Class25/19","No",3]
[null,"concrete"]
["23.07","Trimming of excavations for concrete-lined"]
[null,"open drains:"]
[null,null,"m²",250]
[null,"(a) In soft material"]
[null,null,"m²",100]
[null,"(b) In hard material"]
[]
["23.08","Concrete lining for open drains:"]
[]
[null,"(a) Cast in situ class 30/19 concrete ","m³",100]
[null,"lining in side drains complete as shown on"]
[null," the drawings: KG2022/74/06"]
[]
[null,"(b) Class U2 surface finish to cast in situ ","m²",25]
[null,"concrete in side drains"]
[]
["23.09","Formwork to cast in situ concrete lining for "]
[null,"open drains (class F2 surface finish):"]
[]
[null,"(a) To sides with formwork on the internal face "]
[null,"only","m²",15,null,"Rate Only"]
[]
[null,"(c) To ends of slabs","m²",5,null,"Rate Only"]
[]
["23.10","Sealed joints in concrete linings of open drains"]
[null,"(as detailed on the drawing)","m","-",null,"Rate Only"]
[]
[]
[]
[2300,"Carried forward"]
[]
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 2300"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"brought forward"]
[]
["23.12","Steel reinforcement:"]
[]
[null,"(a) Mild steel bars","t","-",null,"Rate Only"]
[]
[null,"(b) High-tensile steel bars","t",0.08]
[]
[null,"(c) Welded steel fabric","kg",null,null,"Rate Only"]
[]
["23.13","Polyethylene sheeting (0,15 mm thick) for "]
[null,"concrete-lined open drains","m²","-",null,"Rate Only"]
[]
["B 23.18","Concrete edge beam",{"$nulls":3},""]
[{"$nulls":5},""]
[null,"(a) Cast in situ concrete edge beam 300 mm wide",{"$nulls":3},""]
[null,"      x 150 mm deep (Class 25/19 concrete)","m³",{"v":0.8999999999999999,"d":"1"}]
{"$rows_empty":7}
[{"$nulls":5},""]
[{"$nulls":5},""]
[{"$nulls":5},""]
[{"$nulls":5},""]
[{"$nulls":5},""]
[{"$nulls":5},""]
{"$rows_empty":20}
[2300,"TOTAL CARRIED FORWARD TO SUMMARY "]

{"sheet":"3100","index":9,"n_rows":3846,"n_cols":9,"rows_kept":3846,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6],[6,0,6,8]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION",{"$nulls":6},"SECTION 3100"]
[]
[]
["ITEM",null,"DESCRIPTION",null,null,"UNIT","QUANTITY","RATE","AMOUNT"]
["NO"]
[]
[]
[null,null,"BORROW MATERIALS"]
[]
[" 31.01","LI","Excess overburden                       ",null,null,"m³",450]
[]
[" 31.03",null,"Finishing-off borrow areas in:"]
[]
[null,null,"(a)","Hard material",null,"ha",0.1]
[]
[null,"LI","(b)","Intermediate material",null,"ha",0.1]
{"$rows_empty":52}
["3100",null,"TOTAL  CARRIED TO SUMMARY"]
{"$rows_empty":3300}
[{"$nulls":3},"Rock fill (as specified in Subclause 3209(c))"]
[]
[]
[]
[]
[]
[]
[null,null,"Sand fills (as described in Clause 3302,  including "]
{"$rows_empty":177}
[null,null,"Contractor, including all haul:"]
{"$rows_empty":23}
[{"$nulls":3},"Rock fill (as specified in Subclause 3209(c))"]
{"$rows_empty":261}
[null,null,"provided by the Contractor, including all haul:"]

{"sheet":"3200","index":10,"n_rows":45,"n_cols":11,"rows_kept":45,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 3200"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[3200,"SELECTION, STOCKPILING AND BREAKING-"]
[null,"DOWN THE MATERIAL FROM BORROW PITS,"]
[null,"CUTTINGS AND EXISTING PAVEMENT"]
[null,"LAYERS, AND PLACING AND COMPACTING"]
[null,"THE GRAVEL LAYERS"]
[]
[]
["B32.06"," Stockpiling of material                 "]
[]
[null,"(a) Existing road layers","m³",850]
{"$rows_empty":12}
[{"$nulls":10},0]
{"$rows_empty":13}
[3200,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"3300","index":11,"n_rows":59,"n_cols":6,"rows_kept":59,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 3300"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"MASS EARTHWORKS"]
[]
["B33.01","Cut and borrow/stockpile to fill, including free-"]
[null,"haul up to 1 km:"]
[]
[null,"(a)    Material in compacted layer thicknesses"]
[null," of 200 mm and less:"]
[]
[null,"(ii)     Compacted to 93% of modified"]
[null,"  AASHTO density","m³",141]
[]
[]
["B33.04","Cut to spoil, including free-haul up to 1 km."]
[null,"Material obtained from:"]
[]
[null,"(a)    Soft excavation","m³",682]
[]
[null,"(b)    Intermediate excavation","m³",877]
[]
[null,"(c)    Hard excavation","m³",390]
[]
[33.07,"Removal of unsuitable material(including free-haul of 0.5km)"]
[]
[null,"(a) In layer thickness of 200mm and less:"]
[]
[null,"(i) Stable material","m³","-",null,"Rate Only"]
[]
[null,"(ii) Unstable material","m³",595]
[]
["33.10","Roadbed preparation and the compaction",{"$nulls":3},""]
[null,"of material",{"$nulls":3},""]
[{"$nulls":5},""]
[null,"(a) Compaction to 90% of modified AASHTO ",{"$nulls":3},""]
[null,"      density","m³","-",null,"Rate Only"]
[null,"(b) Compaction to 93% of modified AASHTO ",{"$nulls":3},""]
[null,"      density","m³",{"v":1000,"d":"1,000.0"}]
[]
[33.12,"In situ treatment of roadbed:",{"$nulls":3},""]
[{"$nulls":5},""]
[null,"(a) In situ treatment by ripping (200mm deep)","m³",{"v":1000,"d":"1,000.0"}]
[]
["33.13","Finishing-off cut and fill slopes, median "]
[null,"and interchange areas"]
[]
[null,"(a) Cut Slopes","m²",{"v":50,"d":"50.0"}]
[]
[null,"(b) Fill slopes","m²",1450]
[]
[]
[]
[3300,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"3400","index":12,"n_rows":74,"n_cols":10,"rows_kept":74,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6],[6,0,6,7],[21,9,21,14],[22,9,22,14]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION",{"$nulls":5},"SECTION 3400"]
[]
[]
["ITEM","DESCRIPTION",null,null,"UNIT","QUANTITY","RATE","AMOUNT"]
["NO"]
[]
[]
[null,"PAVEMENT LAYERS OF GRAVEL MATERIAL"]
[]
["34.01","Pavement layers constructed from gravel "]
[null,"taken from cut or borrow including free-haul "]
[null,"up to 1,0 km:"]
[]
[null,"(a)","Gravel selected layer compacted to:"]
[]
[null,null,"(i)","93% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150mm","m³",{"v":1000,"d":"1,000"},{"$nulls":3},"DICHOEUNG INTERNAL STREET"]
[{"$nulls":9},"BID NO.: 8/3/342"]
[null,"(c)","Gravel subbase (unstabilized gravel)"]
[null,null,"compacted to:"]
[]
[null,null,"(i)","95% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150mm","m³",900]
[]
[null,"(f)","Gravel base (2% cement stabilised)"]
[]
[null,null,"(i)","98% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150mm","m³",800]
[]
[null,"(g)","Gravel shoulders compacted to:"]
[]
[null,null,"(i)","93% of modified AASHTO density for a"]
[{"$nulls":3},"compacted layer thickness of 150mm","m³",400]
[]
[]
["34.02","Extra over item 34.01 for excavation of"]
[null,"material in:"]
[]
[null,"(a)","Intermediate excavation",null,"m³",{"v":1395,"d":"1,395"}]
[]
[null,"(b)","Hard excavation",null,"m³",{"v":1705.0000000000002,"d":"1,705"}]
{"$rows_empty":27}
[3400,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"3500","index":13,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 3500"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"STABILIZATION"]
[]
[35.01,"Chemical stabilization extra over unstabilized"]
[null,"compacted layers:"]
[]
[null,"(c)    Gravel base, 150mm thick","m³",820]
[]
[35.02,"Chemical stabilizing agent:"]
[]
[null,"(a)    CEMII B-M","t",67.24]
[]
[null,"(b) lime","t",null,null,"Rate Only"]
[]
[]
[35.04,"Provision and application of water for curing","kilolitre",280,null,""]
[]
[35.05,"Curing by covering with subsequent layer","m²",{"v":737.9999999999999,"d":"738"}]
{"$rows_empty":28}
[3500,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"4100","index":14,"n_rows":52,"n_cols":6,"rows_kept":52,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 4100"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"PRIME COAT"]
[]
["B41.01","Prime coat:",{"$nulls":3},""]
[{"$nulls":5},""]
[null,"(c) MC-30 Cut-back bitumen"," litre",{"v":3823.2000000000003,"d":"3,823"}]
[{"$nulls":5},""]
[null,"(d)MC-70 cut-back bitumen","litre","-",null,"Rate Only"]
[{"$nulls":5},""]
[null,"(e)Invert bituminous emulsion","litre","-",null,"Rate Only"]
[]
[null,"(f) Eco Prime","litre","-",null,"Rate Only"]
[{"$nulls":5},""]
[{"$nulls":5},""]
[" 41.02","Aggregate for blinding                  ","m²",{"v":4720,"d":"4,720.0"}]
[]
[]
[" 41.03","Extra over item 41.01 for applying the prime"]
[null,"coat in areas accessible only to hand held "]
[null,"equipment","litre",{"v":4244,"d":"4,244"}]
{"$rows_empty":24}
[4100,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"4200","index":15,"n_rows":53,"n_cols":6,"rows_kept":53,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 4200"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"PRIME COAT"]
[]
[4200,"ASPHALT BASE AND SURFACING"]
[]
["B42.02","Asphalt surfacing :"]
[]
[null,"(a) Continuously graded, medium grade,"]
[null,"using 60/70 penetration grade bitumen:"]
[]
[null,"(i) 30 mm thick, normal mixture with conventional","     m²",4720]
[null,"binder"]
[]
[]
["42.04","Tack Coat "]
[]
[null,"(a)    Tack coat using 30% stable-grade emulsion","litre",{"v":3823.2000000000003,"d":"3823"}]
[null," applied at a rate of 0.5l/m²"]
[]
["42.05","Binder variations"]
[]
[null,"(a) 60/70 pen. grade bitumen","      t",0.2]
[]
[]
["42.06","Variations in active filler content:"]
[]
[null,"(a) Cement","      t",0.2]
[]
[null,"(b) Hydrated Lime","      t",0.2]
[]
["42.07","Trial sections:"]
[]
[null,"(a) 30 mm thick, continuously graded","     m²",200]
[null,"medium grade, normal mixture"]
[]
["42.08","100 mm cores in asphalt","     No",6]
{"$rows_empty":9}
[4200,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"5600","index":16,"n_rows":56,"n_cols":6,"rows_kept":56,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 5600"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"ROAD SIGNS"]
[]
["B56.01","Road sign boards with painted or coloured"]
[null,"semi-matt background. Symbols, lettering"]
[null,"and borders in diamond grade"]
[null,"retro-reflective material, where the sign board is constructed from:"]
[]
[null,"(d) Prepainted galvanized steel profiles (200 mm"]
[null,"      high chromadek or approved equivalent):"]
[]
[null,"        (i)     Area not exceeding 2 m²","m²",6]
[]
[null,"        (ii)     Area exceeding 2 m² but not 10 m²","m²",4]
[]
[56.02,"Extra over item 56.01 for using:"]
[]
[null,"   (b) Lettering, symbols, numbers, arrows,"]
[null,"        emblems and borders of retro-reflective"]
[null,"        material:"]
[]
[null,"        (ii) Class III","m²",4]
[]
[]
[56.03,"Road sign supports (overhead road sign"]
[null,"structures excluded):"]
[]
[null,"         (a) Steel tubing (diameter and wall thickness","t",1]
[null,"               indicated)"]
[]
[56.05,"Excavation and backfilling for road sign "]
[null,"supports (not applicable to kilometre posts)","m³",2]
[]
[56.06,"Extra over item 56.05 for cement-treated soil"]
[null,"backfill","m³",2]
[]
[56.09,"Dismantling and storing road signs with a "]
[null,"surface area of:"]
[]
[null,"(a) Up to 2 m²","No.",3]
[]
[null,"(b) Exceeding 2 m² but not 10 m²","No.",3]
[]
[]
[]
[]
[]
[]
[5600,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"5700","index":17,"n_rows":55,"n_cols":6,"rows_kept":55,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 5700"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"ROAD MARKINGS"]
[]
[57.02,"Retro-reflective road-marking paint:"]
[]
[null,"(a)    White lines (broken or unbroken):"]
[]
[null,"(i)     100 mm wide","km",0.82]
[]
[]
[null,"(d)    White lettering and symbols","m²",81]
[]
[null,"(f)     Transverse lines, painted island and arrestor"]
[null,"         bed markings (any colour)","m²",63]
[]
[null,"(g)       Kerb markings(any colour)","m²",485]
[]
[]
[57.06,"Setting out and premarking the lines"]
[null,"(excluding traffic-island markings, lettering"]
[null,"and symbols)","km",0.82]
[]
["57.07","Re-establishing the painting unit at the end of "]
[null,"the maintenance period","Lump Sum",{"v":1,"d":"1.00"}]
{"$rows_empty":23}
[5700,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"5900","index":18,"n_rows":50,"n_cols":6,"rows_kept":50,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 5900"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"FINISHING THE ROAD AND ROAD RESERVE"]
[null,"AND TREATING OLD ROADS"]
[]
[59.01,"Finishing the road and road reserve:"]
[]
[null,"(b)    Single carriageway road","km",0.82]
{"$rows_empty":35}
[5900,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"8100","index":19,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION                                                                                                            ",{"$nulls":4},"SECTION 8100"]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"TESTING MATERIALS AND WORKMANSHIP"]
[]
[81.02,"Other special tests requested by the Engineer:"]
[]
[null,"(a)    Cost of testing","PC Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[null,"(b)    Charge on Prime Cost Sum","%",{"v":100000,"d":"100,000.00"}]
[]
[81.03,"Providing testing equipment:"]
[]
[null,"(a)    Rolling straight-edge","number",{"v":1,"d":"1.00"}]
{"$rows_empty":34}
[8100,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"D","index":20,"n_rows":3814,"n_cols":8,"rows_kept":3814,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6]],"flags":["formulas_cached_only"]}
[]
["BILL OF QUANTITIES"]
["DICHOEUNG INTERNAL STREET"]
["TENDER NO.: EPMLM 8/3/427"]
[]
["BILL A : ROAD CONSTRUCTION",{"$nulls":6},"SECTION D"]
[]
[]
["ITEM","DESCRIPTION",null,null,"UNIT","QUANTITY","RATE","AMOUNT"]
["NO"]
[]
[{"$nulls":7},""]
[null,"PROVISION OF STRUCTURED TRAINING",{"$nulls":5},""]
[{"$nulls":7},""]
["D07.01","Training ",{"$nulls":5},""]
[{"$nulls":7},""]
[null,"(a)","Technical skills",null,"Prov Sum",1,{"v":16250,"d":"16,250.00"},{"v":16250,"d":"16,250.00"}]
[{"$nulls":7},""]
[null,"(b)","Generic and Management skills",null,"Prov Sum",1,{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"}]
[]
[null,"(c)","Training venue",null,"Prov Sum",1,{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"}]
[]
[null,"(d)","Remuneration of workers undergoing",{"$nulls":4},""]
[null,null,"technical skills training",null,"Prov Sum",1,{"v":35000,"d":"35,000.00"},{"v":35000,"d":"35,000.00"}]
[]
[null,"(e)","Contractor's handling costs, profit and all",{"$nulls":4},""]
[null,null,"other charges in respect of sub-items"]
[null,null,"D07.01 (a), (b) and (c )"]
[]
[null,null,"(i)","Technical skills","%",{"v":16250,"d":"16,250"}]
[]
[null,null,"(ii)","Generic and Management skills","%",{"v":15000,"d":"15,000"}]
[]
[null,null,"(iii)","Training venue","%",{"v":5000,"d":"5,000"}]
[]
[]
[{"$nulls":7},""]
[{"$nulls":7},""]
[{"$nulls":7},""]
[{"$nulls":7},""]
[{"$nulls":7},""]
[{"$nulls":7},""]
[{"$nulls":7},""]
{"$rows_empty":17}
[{"$nulls":7},""]
[]
[" 5900","TOTAL CARRIED TO SUMMARY"]
{"$rows_empty":52}
[{"$nulls":7},""]
{"$rows_empty":64}
[{"$nulls":7},""]
{"$rows_empty":3161}
[null,null,"Rock fill (as specified in Subclause 3209(c))"]
[]
[]
[]
[]
[]
[]
[null,"Sand fills (as described in Clause 3302,  including "]
{"$rows_empty":177}
[null,"Contractor, including all haul:"]
{"$rows_empty":23}
[null,null,"Rock fill (as specified in Subclause 3209(c))"]
{"$rows_empty":261}
[null,"provided by the Contractor, including all haul:"]

{"sheet":"Summary","index":21,"n_rows":73,"n_cols":7,"rows_kept":73,"merged":[[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"BILL OF QUANTITIES"]
[null,"DICHOEUNG INTERNAL STREET"]
[null,"TENDER NO. EPMLM 8/3/427"]
[]
[]
["DICHOEUNG INTERNAL STREET:  SUMMARY OF BILL OF QUANTITIES"]
[]
["BILL A : ROAD CONSTRUCTION"]
["BILL ","DESCRIPTION ","AMOUNT"]
[1200,"GENERAL OBLIGATIONS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[1300,"CONTRACTOR'S ESTABLISHMENT ON SITE AND. . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[null,"GENERAL OBLIGATIONS"]
[1400,"HOUSING, OFFICES AND LABORATORIES FOR THE . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[null,"ENGINEER'S SITE PERSONNEL"]
[1500,"ACCOMMODATION OF TRAFFIC  . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[1600,"OVERHAUL","R"]
[1700,"CLEARING AND GRUBBING . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[1800,"DAYWORK . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[2100,"DRAINS","R"]
[2300,"CONCRETE KERBING  . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[3100,"BORROW MATERIALS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[3200,"SELECTION, STOCKPILING AND BREAKING DOWN THE "]
[null,"MATERIAL FROM BORROW PITS, CUTTINGS AND EXISTING"]
[null,"PAVEMENT LAYERS, AND PLACING AND COMPACTING THE "]
[null,"GRAVEL LAYERS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[3300,"MASS EARTHWORKS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[3400,"PAVEMENT LAYERS OF GRAVEL MATERIAL . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
[3500,"STABILIZATION . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[4100,"PRIME COAT  . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[4200,"ASPHALT SURFACING  . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[5600,"ROAD SIGNS  . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[5700,"ROAD MARKINGS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ","R"]
[5900,"FINISHING THE ROAD AND ROAD RESERVE AND",{"$nulls":4},"="]
[null,"TREATING OLD ROADS. . . . . . . . . . . . . . . . . . . . . . . ","R"]
[8100,"TESTING MATERIAL AND WORKMANSHIP . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .","R"]
["D","PROVISION OF STRUCTURED TRAINING","R"]
[]
[]
["TOTAL BILL A : ROAD CONSTRUCTION ",null,"R"]
[]
["CALCULATION OF TENDER SUM"]
[]
["TOTAL OF BILL OF QUANTITIES. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
["CONTINGENCIES"]
["The sum provided here is under the sole control of the"]
["Engineer and may be deducted in whole or in part.  (The Tenderer"]
["must add 10% of the total of BILL of quantities) . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
["SUBTOTAL (1). . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
[]
["VALUE-ADDED TAX (15%)"]
["The tenderer shall add 15% of subtotal (2) for VAT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . ."," ","R"]
[]
[]
["TENDER SUM CARRIED TO FORM OF TENDER",null,"R"]
{"$rows_empty":15}
[{"$nulls":3},0]

{"sheet":"Scope of Work","index":22,"n_rows":28,"n_cols":6,"rows_kept":28,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[30,0,30,1],[32,0,32,1]],"flags":["formulas_cached_only"]}
[]
["SCHEDULE OF QUANTITIES"]
["CONSTRUCTION OF TZANEEN EXTENSION 13 STREET"]
["BID NO.: SCMU 05/2016"]
[]
["CALCULATION OF TENDER SUM"]
[]
["TOTAL OF SCHEDULE OF QUANTITIES. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R",null,null,0]
[]
["CONTINGENCIES"]
["The sum provided here is under the sole control of the"]
["Engineer and may be deducted in whole or in part.  (The Tenderer"]
["must add 5% of the total of schedule of quantities) . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
["SUBTOTAL (1). . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
["CONTRACT PRICE ADJUSTMENT"]
["Sum provided in terms of the provisions of"]
["the General Conditions of Contract (The Tenderer must add 5%"]
["of Subtotal (1))                                                                                                     ",null,"R"]
[]
["SUBTOTAL (2) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
["VALUE-ADDED TAX (VAT)"]
["The tenderer shall add 15% of subtotal (2) for VAT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .",null,"R"]
[]
[]
["TENDER SUM CARRIED TO FORM OF TENDER",null,"R",null,null,0]

{"sheet":"Sheet1","index":23,"n_rows":11,"n_cols":20,"rows_kept":11,"flags":["formulas_cached_only"]}
[{"$nulls":3},"FILL","INSITU","G7","G5/G6","UNSTABILISED"]
[{"$nulls":4},"ROADBED","SELECTED","LOWER SUB","UPPER SUB","BASE","ASPHALT",null,null,3300,3400,3500,3600,4100,4200,4500,4800]
["LENGTH",2640,null,12,2640,2640,2640,2640,2640,2640]
[]
["WIDTH",{"$nulls":3},10.4,9.8,9.2,8.6,8,7.4]
[]
["THICKNESS",0.15,null,null,0.15,0.15,0.15,0.15,0.15,0]
[]
[{"$nulls":4},4118.4,3880.8,3643.1999999999994,3405.6,3168,19536]
[]
[{"$nulls":4},4530.24,4268.88,4007.5199999999995,3746.1600000000003,3484.8,21489.600000000002]