{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Classification"],"read":"whole","date_system":"1900"}

{"sheet":"Classification","index":0,"n_rows":92,"n_cols":14,"rows_kept":92}
["Classification","SAP Code","Order Product Name","Basic Product Name","Functional Description","Brand","Category","Product Line","Sales Status","Regional Warranty(CN)","Remark","Related Solution","IsOptional","Quantity"]
["Hantam NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Hantam NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Hantam NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Hantam NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Hantam NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","1"]
["Hantam NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","2"]
["Hantam NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","1"]
["Hantam NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","10"]
["Hantam NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","6"]
["Harold Porter NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Harold Porter NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Harold Porter NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Harold Porter NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Harold Porter NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","1"]
["Harold Porter NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","2"]
["Harold Porter NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","1"]
["Harold Porter NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","12"]
["Harold Porter NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","4"]
["Karoo Desert NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Karoo Desert NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Karoo Desert NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Karoo Desert NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Karoo Desert NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","1"]
["Karoo Desert NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","2"]
["Karoo Desert NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","1"]
["Karoo Desert NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","4"]
["Karoo Desert NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","12"]
["Kirsternbosch NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Kirsternbosch NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Kirsternbosch NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Kirsternbosch NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Kirsternbosch NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","4"]
["Kirsternbosch NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","8"]
["Kirsternbosch NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","4"]
["Kirsternbosch NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","35"]
["Kirsternbosch NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","16"]
["Free State NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Free State NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Free State NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Free State NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Free State NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","2"]
["Free State NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","4"]
["Free State NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","2"]
["Free State NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","26"]
["Free State NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","6"]
["KZNH","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["KZNH","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KZNH","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KZNH","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KZNH","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","2"]
["KZNH","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","4"]
["KZNH","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","2"]
["KZNH","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","14"]
["KZNH","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","8"]
["KwaZulu-Natal NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["KwaZulu-Natal NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KwaZulu-Natal NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KwaZulu-Natal NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["KwaZulu-Natal NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","2"]
["KwaZulu-Natal NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","4"]
["KwaZulu-Natal NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","2"]
["KwaZulu-Natal NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","14"]
["KwaZulu-Natal NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","8"]
["Lowveld NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Lowveld NBG","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Lowveld NBG","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Lowveld NBG","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Lowveld NBG","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","3"]
["Lowveld NBG","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","6"]
["Lowveld NBG","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","3"]
["Lowveld NBG","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","35"]
["Lowveld NBG","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","13"]
["Mokopane BCC","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Mokopane BCC","301801376","DS-3E0510P-E(O-STD)","DS-3E0510P-E","L2, Unmanaged, 8 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 110w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Mokopane BCC","301801380","DS-3E0526P-E(O-STD)","DS-3E0526P-E","L2, Unmanaged, 24 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 370w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Mokopane BCC","301801378","DS-3E0518P-E(O-STD)","DS-3E0518P-E","L2, Unmanaged, 16 Gigabit POE ports, 1 Gigabit RJ45 uplink port, 1 Gigabit SFP uplink port, 802.3af/at, PoE power budget 230w","HIKVISION","Transmission","Network Switches","Released","24",null,null,"FALSE","1"]
["Mokopane BCC","302502499","DS-D5032QE(O-STD)(European standard)","DS-D5032QE","31.5\" 1080P, HDMI/VGA input, view angle:178°/178°, 300cd/㎡, plastic casing, VESA, base bracket included, 7*24h","HIKVISION","Display and Control","Monitors","Released","24",null,null,"FALSE","2"]
["Mokopane BCC","303801090","HDD,WD101PURA-64B5KY0,10TB,7200,3.5,S3",null,null,"Outsource","HDD","Surveillance","Released","36",null,null,"FALSE","4"]
["Mokopane BCC","303616121","DS-7616NXI-K2(STD)","DS-7616NXI-K2","All-ch Motion Detection 2.0\nUp to 2-ch false alarm reduction through human and vehicle target classification based on deep learning\nUp to 1-ch video stream face recognition based on deep learning algorithm\nUp to 16 face databases with 20,000 face images in total\nUp to 2-ch @ 12MP or 3-ch @ 8MP or 6-ch @ 4MP or 12-ch @ 1080P decoding capacity","HIKVISION","IP Products","Network Video Recorders","Released","24",null,null,"FALSE","2"]
["Mokopane BCC","311315192","DS-2CD2646G2-IZS(2.8-12mm)(C)(O-STD)","DS-2CD2646G2-IZS","1/3\" Progressive Scan CMOS((C) model);  H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR; EXIR; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service; Audio/Alarm I/O\n*non-(C) model:1/2.7\" Progressive Scan CMOS","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","28"]
["Mokopane BCC","311314613","DS-2CD2146G2-I(2.8mm)(C)(O-STD)","DS-2CD2146G2-I(SU)","1/3\" Progressive Scan CMOS; H.265+/H.265/H.264+/H.264/MJPEG; \nPowered by Darkfighter technology,Color: 0.003 lux @(F1.4, AGC ON), 0 lux with IR; 25fps/30fps(2688×1520,1920×1080); VCA functions; 3 streams; 3D DNR; BLC; ICR;EXIR:30m; DC12V&PoE; Built-in micro SD/SDHC/SDXC slot; HIK-Connect cloud service;\n*-SU model: Audio/Alarm I/O, Built-in microphone","HIKVISION","IP Products","Network Cameras","Released","24",null,null,"FALSE","4"]
["Pretoria NBG","307400150","DS-1LN6U-SC0(O-STD)","DS-1LN6U-SC0","UTP CAT 6, 305 meters,Core diameter: 0.55mm,Solid Copper, Orange","HIKVISION","Transmission","Cables","Released","60",null,null,"FALSE","1"]
["Pretoria NBG","300406474","DS-A71024R/240","DS-A71024R/240","4U, 180 Ch(2Mbps)Record+playback with IPSAN mode, 320 Ch(2Mbps)Record+playback with Direct steaming mode,24 HDD(SATA), Redundant power supply.With 24 pcs 10TB SATA IOT HDD.","HIKVISION","IP Products","Storage","Released","36",null,null,"FALSE","2"]
["Pretoria NBG","190115431","DS-DN49B4M/F","DS-DN49B4M/F","Modular bracket, frame part, available  for DS-D2049NL-B, DS-D2049NL-B/Y, DS-D2049LU-Y,","HIKVISION","Display and Control","Commercial Display Accessories","Released","12",null,null,"FALSE","4"]
["Pretoria NBG","190115432","DS-DN49B4M/B","DS-DN49B4M/B","Modular bracket, Pedestal part, available for DS-D2049NL-B, DS-D2049NL-B/Y, DS-D2049LU-Y, Hight: 800mm","HIKVISION","Display and Control","Commercial Display Accessories","Released","12",null,null,"FALSE","2"]
["Pretoria NBG","302504695","DS-D2049LU-Y(O-STD)(1 IN 1 Package)","DS-D2049LU-Y","49\",1080P,500cd/㎡,bezelwidth:3.5mm,Input: VGA/DVI/DP/HDMI, output: HDMI, support 4K input and loop up to 30 screens with HDMI interface, support VESA","HIKVISION","Display and Control","LCD Video Walls","Sample","24",null,null,"FALSE","4"]
["Pretoria NBG","303500921","DS-6916UDI(B)(STD)","DS-6916UDI(B)","Decoder, supports Output: 16*HDMI/8*BNC, Input: 1*VGA/1*DVI, odd HDMI support 3840*2160@30HZ, decoding capacity 24MP@30fps: 8-ch, 12MP@20fps:16-ch, 8MP@30fps: 32-ch, 5MP@30fps: 48-ch, 3MP@30fps: 80-ch, 1080p@30fps/3 Mbps: 128-ch, max 36 division","HIKVISION","Display and Control","Control","Released","36",null,null,"FALSE","1"]
["Pretoria NBG","401000005","HikCentral-P-SmartWall-Module","HikCentral Professional","Smart Wall Module package - including all functions of Smart Wall module without resourse limitation.Prerequisite:Video Surveillance Base package.Supported:Decoder&Controller&Keyboard management, Mutiple smart walls management, Grapic Card video wall management，Camera live view/playback/alarm linkage on video wall, Spanning/Roaming window,View scedule,etc.","HIKVISION","Software","HikCentral","Released","0",null,null,"FALSE","1"]
["Pretoria NBG","400101055","HikCentral-P-VSS-1Ch","HikCentral Professional","Video Surveillance Expansion package. Prerequisite:Video Surveillance Base package . Supported:1 camera manageable.","HIKVISION","Software","HikCentral","Released","0",null,null,"FALSE","15"]
["Pretoria NBG","310805468","HikCentral-P-VSS-Base/HW/300Ch(O-STD)","HikCentral-P-VSS-Base/HW/300Ch","Video Surveillance Base package -Hardware mode-\nIncluding preinstalled all fundamental features of video surveillance system,300 cameras manageable and Dell server with E2124 CPU\nSupported:3 years free SUP,Main/Auxiliary Storage,Alarm Management,Google Map,Evidence Management, Running on Virtual Machine, 100 Users Logged In Simultaneously,Heath Monitoring/History Maintemance Data, Client Operation (e.g.Visual Tracking, Custom Window Division),etc.","HIKVISION","IP Products","Data Center","Released","36",null,null,"FALSE","1"]
["Pretoria NBG",null,"Remote viewing PCs ",null,"Core i7 with 16GB RAM and also 4Gig GPU graphics cards",{"$nulls":8},9]