{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":659,"n_cols":6,"rows_kept":659,"merged":[[6,0,6,5],[7,0,7,5],[16,1,16,4],[54,1,54,4],[60,1,60,4],[65,1,65,4],[66,1,66,4],[67,1,67,4],[127,1,127,4],[128,1,128,4],[183,1,183,4],[184,1,184,4],[185,1,185,4],[221,1,221,4],[250,1,250,4],[251,1,251,4],[252,1,252,4],[271,1,271,4],[279,1,279,4],[280,1,280,4],[281,1,281,4],[282,1,282,4],[285,0,285,5],[286,0,286,5],[344,1,344,4],[345,0,345,4],[346,0,346,4],[354,1,354,4],[373,1,373,4],[378,1,378,4],[393,1,393,4],[394,1,394,4],[395,1,395,4],[431,1,431,4],[466,1,466,4],[485,0,485,4],[486,0,486,4],[505,1,505,4],[548,0,548,4],[549,0,549,4],[567,1,567,4],[580,1,580,4],[591,1,591,4],[601,1,601,4],[608,1,608,4],[613,1,613,4],[614,0,614,4],[615,0,615,4],[629,1,629,4],[650,1,650,4],[651,1,651,4],[652,1,652,4],[653,1,653,4],[654,1,654,5],[655,1,655,4],[656,1,656,4],[657,1,657,4],[658,1,658,4],[659,1,659,4]]}
[null,"TNPA MARINE SERVICES"]
[null,"REQUEST FOR PROPOSAL [RFP] No\t\t\t:\tTNPA/2023/09/0007/43278/RFP"]
[null,"FOR THE PROVISION OF:"]
[null,"DRYDOCK OF PILOTBOAT IVUBU AND TUG QUNU FOR A ONCE-OFF PERIOD"]
[]
[]
[" LAY-UP LIST PORT ELIZABETH  - 2023/2024"]
["TASK 1 - PILOTBOAT IVUBU"]
["Item no","Description","Unit","Qty","Rate","Amount"]
[1,"SERVICES AND SURVEYS"]
[]
[1.1,"SERVICES REQUIRED"]
["1.1.1","Provision of Fire Watch Man (8hrs/day)","Days",2]
["1.1.2","Provision of Hot Work Permit (8hrs/day)","Days",2]
["1.1.3","Provision of X-Ray, Crack and Thickness Testing Where Needed","m²",150]
["1.1.4","Mobile Crane (1 Ton) (4hrs/day)","Days",3]
[null,"Sub-Total"]
[2,"ENGINE ROOM WORK"]
[]
[2.1,"VALVES"]
[]
["2.1.1","Remove, Overhaul and Assemble Discharge Valves as Per South African Maritime Safety Authority Requirements and;"]
["2.1.2","Remove, Overhaul and Assemble Suction Valves as Per Samsa Requirements and;"]
["2.1.3","Pressure Test Certificates for Valves to Be Supplied for the olloing valves "]
[null,"LIST OF VALVES"]
["V1","Sea Water Suction Dn 40 Scew Down Non Return","No.",2]
["V2","General Service  Pump Overboard Dn50 Globe Non Return ","No.",2]
["V3","Soft Patch Drain Dn50 Globe Nr","No.",1]
["V4","Sewage Plant Discharge  Overboard Dn50 Storm Valve","No.",1]
["V5","Archor Chain Locker Suction Dn50 Globe Valve","No.",1]
["V6","Steering Flat Drain Dn50 Flap Valve","No.",1]
["V7","Bilge Valve To Engine Room Dn50 Globe Nr","No.",1]
["V8","Overhaul Miscellaneous Valves As Per Request  Dn 50 Globe Valve","No.",2]
[]
["2.1.4","Fabricate and supply gaskets (non-metallic) (200 mm)","No.",20]
[]
[2.2,"PIPING"]
["2.2.1","Engine Room Sea Water Piping to Be Renewed Subject to Condition 2m X Φ 50mm","No.",10]
["2.2.2","Engine Room Fresh Water Piping to Be Renewed Subject to Condition 2m X Φ 50mm","No.",10]
["2.2.3","Engine Room Bilge Piping to Be Renewed Subject to Condition 2m X Φ 25mm","No.",10]
[]
[2.3,"BILGES"]
["2.3.1","Entire Engine Room Bilges to Be Washed and Cleaned","m³",5]
["2.3.2","Bilges To Be Pumped Out After Cleaned","m³",5]
[]
[2.4,"SW STRAINERS"]
["2.4.1","Port And Starboard Main Sea Water Strainers to Be Opened and Cleaned","No.",2]
["2.4.2","Two Coats of Antifouling to Be Painted","No.",2]
[]
[2.5,"STEERING FLAT"]
["2.5.1","Steering Flat Bulkheads to Be High Pressure Washed","m²",25]
["2.5.2","Steering Flat to Be Mechanically Descaled","m²",10]
["2.5.3","Steering Flat to Be Primed With 2 Coats","m²",10]
["2.5.4","Steering Flat to Be Painted Fully With 2 Coats of With Paint","m²",25]
[null,"Sub-Total"]
[3,"ENGINE WORK"]
[]
[3.1,"EXHAUST HEAT GUARD (LAGGING)"]
["3.1.1","Remove, Access,Repair OR place as and when required, including assembling in the ENGINE ROOM","m²",1]
["3.1.2","Remove, Access,Repair OR place as and when required, including assembling in the STEERING FLAT","m²",1]
[null,"Sub-Total"]
[4,"ALTERNATOR WORK"]
[]
[4.1,"EXHAUST LAGGING"]
["4.1.1","Remove, Access,Repair OR place as and when required, including assembling in the ENGINE ROOM","m²",1]
[null,"Sub-Total "]
[null,"Total carried forward"]
[null,"Total brought forward"]
[5,"HULL AND SUPERSTRUCTURE WORK PREPARATION"]
[]
[5.1,"HULL CLEANING"]
["5.1.1","Barnicles to be scraped off entire hull","m²",150]
["5.1.2","Entire hull to be pressure washed  (220bar) ","m²",150]
["5.1.3","Clean slipway and barnicles to be disposed off as per legislation","Kg",50]
["5.1.4","Mechanically descale hull below waterline using small angle grinder with wire brush","m²",10]
["5.1.5","Open and clean sea chest","No.",2]
["5.1.6","Seachest grids to be cleaned and HP blasted","No.",2]
[]
[5.2,"ANODES"]
["5.2.1","Remove anodes from hull (APPROX 66)","No.",66]
["5.2.2","Replace anodes after hull painting","No.",66]
["5.2.3","Fit anodes in seachest","No.",2]
["5.2.4","Supply Nyloc nuts ","No.",150]
[]
[5.3,"SUPERSTRUCTURE"]
["5.3.1","High presure wash (220 BARS)","m²",15]
["5.3.2","Chemically clean using paint rollers and paint brushes","m²",15]
["5.3.3","CLEANING AGENT FOR CHEMICALLY CLEAN TO BE PROVIDED BY CONTRACTOR"]
["5.3.4","MDS INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["5.3.5","Mechanically descale using small angle grinders with wire brushes","m²",8]
["5.3.6","Treat/Derust area and apply primer (INTERGARD 269)","m²",8]
[]
[5.4,"MAST AND MONKEY ISLAND ( RAILINGS, DECKS, AND STAIRCASE INCLUDED)"]
["5.4.1","High Pressure  Wash (220 Bars)","m²",10]
["5.4.2","Chemically Clean Using Paint Rollers And Pant Brushes","m²",10]
[6.4,"CLEANING AGENT FOR CHEMICALLY CLEAN TO BE PROVIDED BY CONTRACTOR"]
["5.4.3","MDS INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["5.4.4","Mechanically Descale Using Samll Angle Grinder With Wire Brush","m²",2]
["5.4.5","Treat / Derust Area And Apply Primer (Intergard 269) (TNPA TO SUPPLY PAINT)","m²",2]
[]
[5.5,"MAIN DECK"]
["5.5.1","High presure wash","m²",80]
["5.5.2","Chemically clean using paint rollers and paint brushes","m²",80]
[6.5,"CLEANING AGENT FOR CHEMICALLY CLEAN TO BE PROVIDED BY CONTRACTOR"]
["5.5.3","MDS INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["5.5.4","Mechanically descale using small angle grinders with wire brushes","m²",10]
["5.5.5","Treat/Derust area and apply primer (INTERGARD 269)","m²",10]
[]
[5.6,"BELTING AND GUNNEL ( INSIDE AND OUTSIDE)"]
["5.6.1","High presure wash","m²",70]
["5.6.2","Chemically clean using paint rollers and paint brushes","m²",70]
["5.6.3","CLEANING AGENT FOR CHEMICALLY CLEAN TO BE PROVIDED BY CONTRACTOR"]
["5.6.4","MDS INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["5.6.5","Mechanically descale using small angle grinders with wire brushes","m²",10]
["5.6.6","Treat/Derust area and apply primer (INTERGARD 269)","m²",10]
[]
[5.7,"BOW"]
["5.7.1","Remove bow fenders, (X3)","No.",3]
["5.7.2","Remove vertical fenders (SIZE 250 X 350 MM)","No.",38]
["5.7.3","Bent pins to be straightened OR replaced  (SIZE 25 X 350 MM) ","No.",10]
["5.7.4","Crop out damage plate and replace metal to fit fender ","m²",2.4]
["5.7.5","Metal behind bow fender to be mechanically descaled using small angle grinder with wire brush and primed  - (TNPA TO SUPPLY PAINT)","m²",10]
["5.7.6","Metal bow fender to be painted black  - (TNPA TO SUPPLY PAINT)","m²",10]
["5.7.7","Metal behind vertical fenders to be mechanically descaled using small angle grinder with wire brush and primed  - (TNPA TO SUPPLY PAINT)","m²",10]
["5.7.8","Metal behind vertical fenders to be painted black - (TNPA TO SUPPLY PAINT)","m²",10]
["5.7.9","Vertical fenders to be refitted after painting","No.",38]
["5.7.10","Bow fenders to be refitted after painting (X3)","No.",3]
[null,"Total carried forward"]
[null,"Total brought forward"]
[5.8,"ANCHOR AND CHAIN"]
["5.8.1","Anchor And Chain To Be Dropped And Ranged","No.",1]
["5.8.2","Anchor And Chain To Be High Pressure Cleaned At 220 Bars","No.",1]
["5.8.3","Chain To Be Coated With Boiled Linseed Oil","ltr",10]
["5.8.4","Anchor To Be Painted - (Tnpa To Supply Paint)","No.",1]
["5.8.5","Chain To Be Remarked 8 Shackles - (Tnpa To Supply Paint)","ltr",5]
["5.8.6","Chain And Anchor To Be Restowed","No.",1]
[]
[5.9,"CHAIN LOCKER"]
["5.9.1","Manhole Cover To Be Removed","No.",1]
["5.9.2","Mud To Be Removed And Disposed Of","Kg",10]
["5.9.3","Chain Locker To Be Washed Out, Spot Chipped And Painted - (TNPA TO SUPPLY PAINT)","m²",2]
["5.9.4","Grids To Be Removed Washed And Painted - 1.5M (TNPA TO SUPPLY PAINT)","No.",2]
["5.9.5","New Gasket To Be Made Up - 1.5M², Material","No.",1]
["5.9.6","Manhole Cover To Be Replaced","No.",1]
[]
[{"v":5.1,"d":"5.10"},"FORWARD STORE"]
["5.10.1","Forward Store To Be Mechanically Descaled","m²",10]
["5.10.2","Forward Store To Be Primed - (TNPA WILL SUPPLY PRIMER) ","m²",10]
["5.10.3","Forward Store To Be Painted(Full Coat) - (TNPA TO SUPPLY PAINT)","m²",30]
["5.10.4","Foward Store Hatch Cover Dogs To Be Overhauled And Greased (4 Dogs)","No.",4]
[]
[5.11,"VOID SPACE - GALLEY"]
["5.11.1","Void Space Under Galley Floor To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush","m²",10]
["5.11.2","Void Space Under Galley Floor To Be Fully Primed - (TNPA TO SUPPLY THE PAINT)","m²",24]
[]
[5.12,"VOID SPACE - CREW ACCOMODATION"]
["5.12.1","Void Space In Crews Accommodation  To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush","m²",10]
["5.12.2","Void Space In Crews Acommodation To Be Primed - (TNPA TO SUPPLY THE PAINT)","m²",10]
["5.12.3","Void Space In Crew Accommodation To Be Painted (Full Coat) - TNPA TO SUPPLY THE PAINT)","m²",20]
[]
[5.13,"AFT STORE"]
["5.13.1","AFT Store To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush","m²",20]
["5.13.2","AFT Store To Be Fully Primed - (TNPA TO SUPPLY PAINT)","m²",20]
["5.13.3","AFT Store To Be Fully Painted - (TNPA TO SUPPLY PAINT)","m²",20]
[]
[5.14,"PROPELLERS"]
["5.14.1","Propellers To Be Cleaned And Polished/ Buffed Up -Angle Grinder With Wire Brush","No.",2]
[]
[5.15,"RUDDERS"]
["5.15.1","Clearances To Be Taken On Both Rudders And Report To Be Submitted","No.",2]
[null,"NB: CALIBRATIONS TO BE RECORDED FOR SAMSA AND OWNERS RECORDS"]
[]
[5.16,"STARBOARD STERN TUBE SEALS"]
["5.16.1","Clearances To Be Taken Of Shafts (Both Shafts)  And Report To Be Submitted","No.",2]
[null,"NB: CALIBRATIONS TO BE RECORDED FOR SAMSA AND OWNERS RECORDS"]
[]
[5.17,"BREATHER PIPES"]
["5.17.1","Breather Pipes To Be Sand Blasted And Repaired As Needed ","No.",6]
["5.17.2","Breather Pipes To Be Primed And Painted (Colour Coded) - (TNPA TO SUPPLY PAINT)","No.",6]
[]
[5.18,"FILLING PIPES"]
["5.18.1","Filling Pipes To Be Replaced As Needed ","No.",6]
["5.18.2","Filling Pipes To Be Primed And Painted (Colour Coded)  -  (TNPA TO SUPPLY PAINT)","No.",6]
[null,"Sub-Total"]
[null,"Total carried forward"]
[null,"Total brought forward"]
[6,"TANKS"]
[]
[6.1,"PORT AND STARBOARD FRESHWATER TANKS  (1.19m³ EACH)"]
["6.1.1","Fresh Water Tanks To Be Drained (Port And Starboard) ","No.",2]
["6.1.2","Fresh Water Tanks To Be Opened And Vented ","No.",2]
["6.1.3","Fresh Water Tanks To Be High Pressure Washed At 220 Bars","No.",2]
["6.1.4","Fresh Water Tanks To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",2]
["6.1.5","Fresh Water Tanks To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",2]
["6.1.6","New None Metallic Gasket To Be Made Up For Manhole Covers (Φ 250Mm)","No.",2]
[]
[6.2,"BLACKWATER TANK (SEWAGE)  (0.516m³)"]
["6.2.1","Blackwater Tank To Be Drained","No.",1]
["6.2.2","Blackwater Tank To Be Opened And Vented","No.",1]
["6.2.3","Blackwater Tank To Be High Pressure Washed At 220 Bars","No.",1]
["6.2.4","Blackwater Tank To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",1]
["6.2.5","Blackwater Tank To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",1]
["6.2.6","New None Metallic Gasket To Be Made Up For Manhole Cover Φ 250Mm)","No.",1]
[]
[6.3,"GREYWATER TANK (0.733m³) "]
["6.3.1","Greywater Tank To Be Drained"]
["6.3.2","Greywater Tank To Be Opened And Vented","No.",1]
["6.3.3","Greywater Tank To Be High Pressure Washed At 220 Bars","No.",1]
["6.3.4","Greywater Tank To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",1]
["6.3.5","Greywater Tank To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",1]
["6.3.6","New None Metallic Gasket To Be Made Up For Manhole Cover Φ 250Mm)","No.",1]
[]
[6.4,"FUEL DOUBLE BOTTOM TANKS (9.47m³ EACH) "]
["6.4.1","Fuel Double Bottom Tanks (Port And Starboard) To Be Opened And Vented","No.",2]
["6.4.2","Fuel Double Bottom (Port And Starboard) Tanks To Be High Pressure Cleaned","No.",2]
["6.4.3","Gas Free Certificate To Be Issued Before Entry","No.",4]
[]
[6.5,"SERVICE TANKS(2.7m³ EACH)  (X2)"]
["6.5.1","Port And Starboard Service Tanks To Be Opened And Vented","No.",2]
["6.5.2","Port And Starboard Service Tanks To Be High Pressure Cleaned","No.",2]
["6.5.3","Gas Free Certificate To Be Issued Before Entry","No.",4]
[null,"Sub-Total"]
[7,"PAINTING "]
[]
[7.1,"MAST AND MONKEY ISLAND (RAILINGS, DECKS, AND STAIRCASE INCLUDED)"]
["7.1.1","Mast To Be Painted (Interlac 990 White) - (TNPA TO SUPPLY PAINT)","m²",5]
["7.1.2","Monkey Island To Be Painted (Interlac 990 Green) (Full Coat) - (TNPA TO SUPPLY PAINT)","m²",20]
[]
[7.2,"SUPERSTRUCTURE"]
["7.2.1","Apply Top Coat As Per Paint Spec (Interlac 990 White) To Required Areas (Full Coat) - (TNPA TO SUPPLY PAINT)","m²",20]
[]
[7.3,"MAIN DECK"]
["7.3.1","(TNPA TO SUPPLY PAINT)","m²",80]
[]
[7.4,"BELTING AND GUNNEL"]
["7.4.1","Treat/ De Rust And Apply Primer (Intergard 269) - (TNPA TO SUPPLY PAINT)","m²",70]
["7.4.2","Entire Belting And Gunnel To Be Painted As Per Paint Spec (Interlac 665 Black) (Full Coat) - (TNPA TO SUPPLY PAINT)","m²",70]
[]
[7.5,"WATERLINE TO MAIN DECK (14m²)"]
["7.5.1","Apply Primer Intergard 269 - (TNPA TO SUPPLY PAINT)","m²",5]
["7.5.2","One Coat Entire Hull Above Waterline To Be Painted With International Interlac 665 - (TNPA TO SUPPLY PAINT)","m²",14]
["7.5.3","Paint Name And Port of Registry - (TNPA TO SUPPLY PAINT)","No.",1]
[]
[7.6,"HULL"]
["7.6.1","Apply Primer As Per Paint Spec (Intergard 269) - (TNPA TO SUPPLY PAINT)","m²",20]
["7.6.2","Apply Undercoat (X1) As Per Paint Spec (Intergard 203) - (TNPA TO SUPPLY PAINT)","m²",150]
["7.6.3","Apply Antifouling (X2) As Per Paint Spec (Interspeed 6400 Dark Red) - (TNPA TO SUPPLY PAINT)","m²",150]
["7.6.4","Seachest To Be Painted With Antifouling ( 2 Coats) - (TNPA TO SUPPLY PAINT)","m²",2]
["7.6.5","Seachest Grids To Be Painted With Antifouling (X2) - (TNPA TO SUPPLY PAINT)","No.",2]
["7.6.6","Draught And Plimsol Marks To Be Painted - (TNPA TO SUPPLY PAINT)","No.",2]
[null,"Sub-Total"]
[null,"Total carried forward"]
[null,"Total brought forward"]
[8,"MISCELLANEOUS WORK"]
[]
[8.1,"MISCELLANEOUS WORK"]
["8.1.1","Budget R100 000 For Unplanned Work Identified After Inspection","Prov. Sum",1,{"v":100000,"d":"R100,000.00"},{"$f":"D257*E257","v":{"v":100000,"d":"R100,000.00"}}]
["8.1.2","Skilled Labour ","hrs.",20]
["8.1.3","Semi-Skiled Labour ","hrs.",20]
["8.1.4","Machine Shop Cost","hrs.",10]
["8.1.5","Signage And Stickers To Be Replaced After Painting Completed","No.",100]
["8.1.6","Budget For R10 000 For Additional Material Needed","Sum",1,{"v":10000,"d":"R10,000.00"},{"$f":"D262*E262","v":{"v":10000,"d":"R10,000.00"}}]
["8.1.7","Scaffolding","Days",14]
["8.1.8","She File, She Plan And Risk Assessment","Prov. Sum",1]
[]
[8.2,"GENERAL CLEANING"]
["8.2.1","Provide Labour 8 Hrs For Cleaning And Assisting Tnpa Engine Room Staff","Days",2]
[]
[8.3,"METAL WORK"]
["8.3.1","Metal For Repairs","Ton",0.5]
[]
[null,"Sub-Total"]
[9,"SUNDRIES"]
[]
[9.1,"DISBURSEMENTS"]
["9.1.1","Travelling Expenses ","Days ",28]
["9.1.2","Accomodation","Days ",28]
["9.1.3","Other disbursements","Days ",28]
[]
[null,"Sub-Total"]
[null,"Total  for Task 1 excluding VAT"]
[null,"VAT 15%"]
[null,"Total  for Task 1 including VAT carried forward to FINAL SUMMARY"]
[]
[]
[" LAY-UP LIST EAST LONDON  - 2023/2024"]
["TASK 2 - TUG QUNU"]
["Item no","Description","Unit","Qty","Rate","Amount"]
[1,"ENGINE ROOM WORK"]
[]
[1.1,"VALVES"]
["1.1.1","Remove, Overhaul And Assembley Discharge Valves As Per Samsa Requirements And;"]
["1.1.2","Remove, Overhaul And Assembley Suction Valves As Per Samsa Requirements And;"]
["1.1.3","Pressure Test Certificates For Valves To Be Supplied For The Following Valves:"]
["V1","Black Water Overboard Valve 150 Nb","No.",1]
["V2","Grey Water Overboard Valve   80Nb","No.",1]
["V3","Air Conditioning Plant Overboard Valve   32Nb","No.",1]
["V4","Starboard Main Engine Sw Overboard Valve  100Nb","No.",1]
["V5","Aft General Service Overboard Discharge Valve 80Nb","No.",1]
["V6","Forward General Service Overboard Discharge Valve 80Nb","No.",1]
["V7","Oil Water Separator Overboard Valve 25Nb","No.",1]
["V8","Galley Overboard Valve 80Nb","No.",1]
["V9","Port Main Engine Sea Water Overboard Valve 100Nb","No.",1]
["V10","Starboard Fire Pump Isolation  Valve ","No.",1]
["V11","Butterfly Valve To Be Cleaned In Place. Inspect And Clean Rubber Seats For Samsa Survey 350Nb","No.",1]
["V12","Port Fire Pump Isolating Valve","No.",1]
["V13"," Butterfly Valve To Be Cleaned In Place. Inspect And Clean Rubber Seats For Samsa Survey 350Nb","No.",1]
["V14","Starboard Main Engine Sea Water Strainer Inlet ","No.",1]
["V15","Butterfly Valve To Be Cleaned In Place. Inspect And Clean Rubber Seats For Samsa Survey 250Nb","No.",1]
["V16","Port Main Engine Sea Water Strainer Inlet ","No.",1]
["V17","Butterfly Valve To Be Cleaned In Place. Inspect And Clean Rubber Seats For Samsa Survey 250Nb","No.",1]
["V18","Main Sea Chest Vent Valves 50Nb","No.",2]
[]
["1.1.4","Overhaul Miscellaneous Valves As Per Request 80Nb","No.",4]
["1.1.5","Fabricate And Supply Gaskets Φ 150Mm Non Metalic ","No.",15]
[]
[]
[1.2,"PIPING "]
["1.2.1","Engine Room Sea Water Piping To Renew Whole Piping System Subject To Condition, (Ф100Mm) ","m",2]
["1.2.2","Engine Room Fresh Water Piping To Renew Subject To Condition (Ф100Mm) ","m",2]
["1.2.3","Engine Room Bilge Piping To Renew Subject To Condition (Ф100Mm) ","m",2]
["1.2.4","Engine Room Hydraulic Piping To Renew Subject To Condition (Ф100Mm)","m",2]
[]
[1.3,"BILGES"]
["1.3.1","Entire Engine Room Bilges To Be Washed And Cleaned","m²",5]
["1.3.2","Bilges To Be Pumped Out After Cleaned","m²",5]
[]
[1.4,"SW STRAINERS"]
["1.4.1","Port And Starboard Main Sea Water Strainers To Be Opened And Cleaned","No.",2]
["1.4.2","Coat Of Antifouling To Be Painted - (TNPA TO SUPPLY PAINT)","No.",2]
[]
[1.5,"COOLERS"]
["1.5.1","Plate Coolers "]
[null,"HT Coolers","No.",2]
[null,"LT Coolers","No.",2]
["1.5.2","Open Coolers For Cleaning","No.",4]
["1.5.3","Clean Plate Coolers","No.",4]
["1.5.4","Refit Plates To Required Measurements","No.",4]
["1.5.5","High Temperature And Low Temperature Header Tanks And Main Engines To Be Flushed Through With Fresh Water","No.",2]
[]
[1.6,"PUMPS "]
["1.6.1","Repack FIFI Pumps ","No.",2]
["1.6.2","Supply New  Gauges ","No.",2]
[]
[null,"Sub-Total"]
["Total carried forward"]
["Total brought forward"]
[2,"ALTERNATOR WORK"]
[]
[2.1,"KEEL COOLERS"]
["2.1.1","Flush Through Keel Coolers And Refill","No.",4]
["2.1.2","Clean Keel Coolers","No.",2]
["2.1.3","Remove Old And Fit New Anodes (ANODES TO BE SUPPLIED BY TNPA)","No.",8]
["2.1.4","Supply Nyloc Nuts ","No.",20]
[null,"Sub-Total"]
[3,"VOITH UNITS"]
[]
[3.1,"PORT & STBD VOITH UNITS"]
["3.1.1","Remove Voith Inspections Covers","No.",2]
["3.1.2","High Pressure Wash Rotor Casings 220Bars","No.",2]
["3.1.3","Paint Rotor Casings (Seaquantum Ultra Dark Red) (2 X Coats) - (TNPA TO SUPPLY PAINT)","No.",2]
["3.1.4","Replace Voith Inspection Covers","No.",2]
["3.1.5","Mechanically Clean Voith Blades Using Small Angle Grinder With Wire Brush","No.",10]
[]
[3.2,"DOCKING PLATFORM STRUTS"]
["3.2.1","Docking Platform Struts","No.",2]
["3.2.2","Crack Detecting Tests To Be Done On All Welds ( Submit Report)","No.",1]
[]
[3.3,"SKEG"]
["3.3.1","Lower Plug On Skeg To Be Removed And Check For Water","No.",1]
[]
[3.4,"DOCKING GUARD"]
["3.4.1","Remove Lower Plug And Check For Water","No.",1]
[null,"Sub-Total"]
[4,"ALTERNATOR WORK"]
[]
[4.1,"EXHAUST LAGGING"]
["4.1.1","Remove, Access,Repair OR place as and when required, including assembling in the ENGINE ROOM","m²",1]
[null,"Sub-Total"]
[5,"CLEANING WORK"]
[]
[5.1,"HULL CLEANING (UNDERWATER)"]
["5.1.1","Barnicles To Be Scraped Off Entire Hull","m²",540]
["5.1.2","Entire Hull To Be Pressure Washed  (220Bar) (150Kg)","No.",540]
["5.1.3","Remove Sea Chest Gratings For Cleaning And Later Replaced (1m²)","m²",2]
["5.1.4","Clean Slipway And Barnicles (50Kg) To Be Disposed Off As Per Legislation","Kg",50]
["5.1.5","Mechanically Descale Affected Areas Using Small Angle Grinder With Wire Brush","m²",10]
["5.1.6","Rinse After Mechanically Descaling","m²",540]
[]
[5.2,"ANODES"]
["5.2.1","Remove Existing Anodes (64 X Hull + 20 Vsp Units + 4 X Sea Strainers . Total 88)","No.",88]
["5.2.2","Replace Anodes With New After Painting Hull","No.",88]
["5.2.3","Supply Nyloc Nuts ","No.",200]
[null,"Sub-Total"]
[null,"Total carried forward"]
[null,"Total brought forward"]
[6,"TANKS"]
[]
[6.1,"PORT AND STARBOARD FRESHWATER TANKS  (1.19m³ EACH)"]
["6.1.1","Fresh Water Tanks To Be Drained (Port And Starboard) ","No.",2]
["6.1.2","Fresh Water Tanks To Be Opened And Vented ","No.",2]
["6.1.3","Fresh Water Tanks To Be High Pressure Washed At 220 Bars","No.",2]
["6.1.4","Fresh Water Tanks To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",2]
["6.1.5","Fresh Water Tanks To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",2]
["6.1.6","New None Metallic Gasket To Be Made Up For Manhole Covers (Φ 250Mm)","No.",2]
[]
[6.2,"BLACKWATER TANK (SEWAGE)  (0.516m³)"]
["6.2.1","Blackwater Tank To Be Drained","No.",1]
["6.2.2","Blackwater Tank To Be Opened And Vented","No.",1]
["6.2.3","Blackwater Tank To Be High Pressure Washed At 220 Bars","No.",1]
["6.2.4","Blackwater Tank To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",1]
["6.2.5","Blackwater Tank To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",1]
["6.2.6","New None Metallic Gasket To Be Made Up For Manhole Cover Φ 250Mm)","No.",1]
[]
[6.3,"GREYWATER TANK (0.733m³) "]
["6.3.1","Greywater Tank To Be Drained"]
["6.3.2","Greywater Tank To Be Opened And Vented","No.",1]
["6.3.3","Greywater Tank To Be High Pressure Washed At 220 Bars","No.",1]
["6.3.4","Greywater Tank To Be Spot Chipped And Primed - (TNPA TO SUPPLY PAINT)","No.",1]
["6.3.5","Greywater Tank To Be Painted As Required - (TNPA TO SUPPLY PAINT)","No.",1]
["6.3.6","New None Metallic Gasket To Be Made Up For Manhole Cover Φ 250Mm)","No.",1]
[]
[6.4,"FUEL DOUBLE BOTTOM TANKS (9.47m³ EACH) "]
["6.4.1","Fuel Double Bottom Tanks (Port And Starboard) To Be Opened And Vented","No.",2]
["6.4.2","Fuel Double Bottom (Port And Starboard) Tanks To Be High Pressure Cleaned","No.",2]
["6.4.3","Gas Free Certificate To Be Issued Before Entry","No.",4]
[]
[6.5,"SERVICE TANKS(2.7m³ EACH)  (X2)"]
["6.5.1","Port And Starboard Service Tanks To Be Opened And Vented","No.",2]
["6.5.2","Port And Starboard Service Tanks To Be High Pressure Cleaned","No.",2]
["6.5.3","Gas Free Certificate To Be Issued Before Entry","No.",4]
[null,"Sub-Total"]
[7,"SUPERSTRUCTURE, MAST AND MAIN DECK"]
[]
[7.1,"MAST, WHEELHOUSE AND SUPERSTRUCTURE  (INC. YARDARMS,  LADDERS AND RAILINGS)"]
["7.1.1","Chemically Clean Using Paint Rollers And Brushes","m²",400]
["7.1.2","Cleaning Agent For Chemically Cleaning To Be Provided By Contractor","ltr",20]
["7.1.3","MDS INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["7.1.4","Mechanically Descale Affected Areas Using Small Angle Grinder With Wire Brush","m²",10]
["7.1.5","High Pressure  Wash To Prepare For Priming(220 Bars)","m²",400]
[]
[7.2," MONKEY ISLAND & BRIDGE DECK (INC. LADDERS,RAILINGS & VENTS)"]
["7.2.1","Chemically Clean Using Paint Rollers And Paint Brushes","m²",200]
["7.2.2","Cleaning Agent For Chemically Cleaning To Be Provided By Contractor","ltr",10]
["7.2.3","SAFETY DATA SHEET INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["7.2.4","Mechanically Descale Affected Areas Using Small Angle Grinder With Wire Brush","m²",10]
["7.2.5","High Pressure Wash To Prepare For Priming","m²",200]
[]
[7.3,"MAIN DECK. (INCLUDING BITS)"]
["7.3.1","Chemically Clean Main Deck With Paint Rollers And Paint Brushes","m²",200]
["7.3.2","Cleaning Agent For Chemically Cleaning To Be Provided By Contractor","ltr",10]
["7.3.3","SAFETY DATA SHEET INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["7.3.4","Mechanically Descale Affected Areas With Small Angle Grinder With Wire Brush","m²",10]
["7.3.5","High Pressure Wash To Prepare For Priming ","m²",200]
[]
[7.4,"WATER LINE TO GUNNNEL COMPL (INCLUDING INSIDE BULWARKS)"]
["7.4.1","Chemically Clean Using  Using Paint Rollers And Paint Brushes","m²",200]
["7.4.2","Cleaning Agent For Chemically Cleaning To Be Provided By Contractor","ltr",10]
["7.4.3","SAFETY DATA SHEET INFORMATION TO BE PROVIDED FOR CHEMICALS"]
["7.4.4","Mechanically Descale Affected Areas Using Small Angle Grinder With Wire Brush","m²",10]
["7.4.5","High Pressure Wash To Prepare For Priming ","m²",200]
[]
[7.5," EXHAUST"]
["7.5.1","Wash Down Exhaust Pipes To Remove Salt ( X2) With Fresh Water","m²",35]
["7.5.2","Mechanically Descale Affected Areas  Using Small Angle Grinder With Wire Brush","m²",10]
["7.5.3","High Pressure Wash To Prepare For Priming","m²",35]
[null,"Sub-Total"]
[8,"PAINTINGS"]
[]
[8.1,"MAST, WHEELHOUSE AND SUPERSTRUCTURE (INC. YARDARMS, LADDERS AND RAILINGS)"]
["8.1.1","Prime Affected Areas First Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.1.2","Prime Affected Areas Second Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.1.3","Apply Top Coat -(TNPA TO SUPPLY PAINT)","m²",400]
[]
[8.2,"MONKEY ISLAND & BRIDGE DECK (INC. LADDERS,RAILINGS & VENTS)"]
["8.2.1","Prime Affected Areas First Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.2.2","Prime Affected Areas Second Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.2.3","Apply Top Coat -(TNPA TO SUPPLY PAINT)","m²",200]
[]
[8.3,"MAIN DECK. (INCLUDING BITS)"]
["8.3.1","Prime Affected Areas First Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.3.2","Prime Affected Areas Second Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.3.3","Apply Top Coat -(TNPA TO SUPPLY PAINT)","m²",200]
["8.3.4","Replace Potholes Seals","m²",6]
["8.3.5","Remove, Supply And Fit New Seals For Hatchcovers ","m²",2]
["Total carried forward"]
["Total brought forward"]
[8.4,"WATER LINE TO GUNNNEL COMPL  (INCLUDING INSIDE BULWARKS)"]
["8.4.1","Prime Affected Areas First Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.4.2","Prime Affected Areas Second Coat - (TNPA TO SUPPLY PAINT)","m²",10]
["8.4.3","Apply Top Coat -(TNPA TO SUPPLY PAINT)","m²",200]
[]
[8.5,"HULL"]
["8.5.1","Apply Primer -  (TNPA TO SUPPLY PAINT)","m²",10]
["8.5.2","Apply Undercoat -  (TNPA TO SUPPLY PAINT)","m²",540]
["8.5.3","Apply Antifouling As Per Paint Specifications (Seaquantum Ultra Red) -  (TNPA TO SUPPLY PAINT)","m²",540]
["8.5.4","Apply Antifouling As Per Paint Specifications (Seaquantum Ultra Dark Red) -  (TNPA TO SUPPLY PAINT)","m²",540]
["8.5.5","Draught And Plimsol Marks To Be Painted -  (TNPA TO SUPPLY PAINT)","m²",2]
[]
[8.6,"EXHAUST"]
["8.6.1","Apply Full Coat As Per Paint Specifications (Jotatemp 1000C Aliminium) -  (TNPA TO SUPPLY PAINT)","m²",35]
["8.6.2","Apply Full Coat As Per Paint Specifications (Solvalitt Black) -  (TNPA TO SUPPLY PAINT)","m²",35]
[]
[8.7,"SUNDRIES"]
["8.7.1","Removal Of Debris","m²",0.5]
[null,"Sub-Total"]
[9,"TANKS"]
[]
[9.1,"PORT AND STARBOARD FRESH WATER TANKS "]
["9.1.1","Open Fresh Water Tanks And Ventilate","No.",2]
["9.1.2","OXYGEN READINGS TO BE TAKEN ON EVERY ENTRY"]
["9.1.3","Fresh Water Tanks To Be Cleaned","m²",43]
["9.1.4","Fresh Water Tanks To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush And Primed","m²",10]
["9.1.5","Fresh Water Tanks To Be Touched Up With Paint As Required - (TNPA TO SUPPLY PAINT)","m²",10]
["9.1.6","New Non-Metallic Gaskets To Be Made Up (Φ1000Mm)","No.",1]
["9.1.7","Fresh Water Manhole Cover To Be Refitted","No.",1]
[]
[9.2,"FOREPEAK TANK "]
["9.2.1","Open Forepeak Tank And Ventilate","No.",1]
["9.2.2","OXYGEN READINGS TO BE TAKEN ON EVERY ENTRY"]
["9.2.3","Forepeak Tank To Be Cleaned","m²",52]
["9.2.4","Forepeak To Be Mechanically Descaled And Primed","m²",10]
["9.2.5","Forepeak To Be Touched Up With Paint As Required - (TNPA TO SUPPLY PAINT)","m²",10]
["9.2.6","New Non-Metallic Gaskets To Be Made Up (Φ1000Mm)","No.",1]
["9.2.7","Forepeak Tank Manhole Cover To Be Refitted","No.",1]
[]
[9.3,"AFTPEAK TANK"]
["9.3.1","Open Aftpeak Tank And Ventilate","No.",1]
["9.3.2","OXYGEN READINGS TO BE TAKEN ON EVERY ENTRY"]
["9.3.3","Aftpeak Tank To Be Cleaned","m²",27]
["9.3.4","Aftpeak Tank To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush And Primed","m²",10]
["9.3.5","Aftpeak Tank To Be Touched Up With Paint As Required","m²",10]
["9.3.6","New Nonmetallic Gaskets To Be Made Up (Φ1000Mm)","No.",1]
["9.3.7","Aftpeak Tank Manhole Cover To Be Refitted","No.",1]
[]
[9.4,"PORT AND STARBOARD FUEL SERVICE TANKS"]
["9.4.1","Open Service Tanks And Ventilate","No.",2]
["9.4.2","GAS FREE CERTIFICATE TO BE ISSUED BEFORE ENTRY"]
["9.4.3","Service Tanks To Be Cleaned (X2) ","m²",10]
["9.4.4","New Non-Metallic Gaskets To Be Made Up (Φ1000Mm)","No.",2]
["9.4.5","Service Tanks Manhole Covers To Be Refitted","No.",2]
[]
[9.5,"PORT & STARBOARD DB FUEL TANKS"]
["9.5.1","Open Double Bottom Fuel Tanks And Ventilate","No.",2]
["9.5.2","GAS FREE CERTIFICATE TO BE ISSUED BEFORE ENTRY"]
["9.5.3","Double Bottom Fuel Tanks To Be Cleaned (X2)","m²",68]
["9.5.4","New Non-Metallic Gaskets To Be Made Up (Φ1000Mm)","No.",2]
["9.5.5","Double Bottom Fuel Tanks Manhole Covers To Be Refitted","No.",2]
["Total carried forward"]
["Total brought forward"]
[9.6,"DIRTY OIL TANK"]
["9.6.1","Open Dirty Oil Tank And Ventilate","No.",1]
["9.6.2","OXYGEN AND GAS READINGS TO BE TAKEN ON EVERY ENTRY"]
["9.6.3","Dirty Oil Tank To Be Cleaned","m²",16]
["9.6.4","Dirty Oil Tank To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush And Primed","m²",4]
["9.6.5","Dirty Oil Tank To Be Touched Up With Paint As Required - (TNPA TO SUPPLY PAINT)","m²",4]
["9.6.6","New Non-Metallic Gasket To Be Made Up (Φ1000Mm)","No.",1]
["9.6.7","Dirty Oil Tank Manhole Cover To Be Refitted","No.",1]
[]
[9.7,"VOID SPACE"]
["9.7.1","Open Void Space Tank And Ventilate","m²",10]
["9.7.2","OXYGEN READINGS TO BE TAKEN ON EVERY ENTRY"]
["9.7.3","Void Space Tank To Be Cleaned","m²",10]
["9.7.4","Void Space Tank To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush And Primed","m²",4]
["9.7.5","Void Space Tank To Be Touched Up With Paint As Required","m²",4]
["9.7.6","New None Metallic Gaskets To Be Made Up Φ1000Mm","No.",2]
["9.7.7","Void Space Tank Manhole Cover To Be Refitted","No.",2]
[null,"Sub-Total"]
[10,"ANCHOR AND CHAIN"]
[]
[10.1,"ANCHOR AND CHAIN"]
["10.1.1","Anchor And Chain To Be Dropped And Ranged (Flake Out On The Ground)","No.",1]
["10.1.2","Anchor And Chain To Be High Pressure Cleaned At 220 Bars","No.",1]
["10.1.3","Chain To Be Coated With Boiled Linseed Oil - 20L","No.",1]
["10.1.4","Anchor To Be Painted Black - (TNPA TO SUPPLY PAINT)","No.",1]
["10.1.5","Chain To Be Remarked  - (TNPA TO SUPPLY PAINT)","No.",1]
["10.1.6","Chain And Anchor To Be Restowed","No.",1]
["10.1.7","Service Hydraulic Control Valve ","No.",1]
["10.1.8","Service Brake And Lining","No.",1]
["10.1.9","Service Clutch ","No.",1]
[null,"Sub-Total"]
[10,"CHAIN LOCKER"]
[]
[10.2,"CHAIN LOCKER"]
["10.2.1","Manhole Cover To Be Removed","No.",1]
["10.2.2","Mud To Be Removed And Disposed Of","Kg",5]
["10.2.3","Chain Locker To Be Washed Out","m²",4]
["10.2.4","Chain Locker To Be Mechanically Descaled Using Small Angle Grinder With Wire Brush","m²",1]
["10.2.5","Chain Locker To Be Painted Complete  (Jotamastic Smartpack Red) - (TNPA TO SUPPLY PAINT)","m²",4]
["10.2.6","Grids To Be Removed Washed And Painted 1,5Mm X 5Mm - (TNPA TO SUPPLY PAINT)","No.",2]
["10.2.7","Manhole Cover To Be Replaced","No.",1]
[null,"Sub-Total"]
[11,"STERN W FENDER"]
[]
[11.1,"STERN W FENDER"]
["11.1.1","Remove Bow Fender","No.",1]
["11.1.2","Remove Damaged Sections Of Stern Fender As Allocated","No.",4]
["11.1.3","Refit New Sections Of Stern Fender","No.",4]
["11.1.4","Refit Missing Sections Of Stern Fender","No.",4]
["11.1.5","Supply New Pins As Per Specifications For Fender","No.",12]
["11.1.6","Refit Bow Fender After Completion Of Work","No.",1]
[null,"Sub-Total"]
[12,"FENDER LUGS"]
[]
[12.1,"STERN FENDER LUGS"]
["12.1.1","Cut Off Damaged Lugs On Stern Holding Stern Fender (X2 Per Lug Set)","No.",12]
["12.1.2","Reweld New Double Lugs For Stern Fender Straps","No.",12]
["12.1.3","Supply Pins To Fit New Lugs Ans Straps","No.",12]
[null,"Sub-Total"]
[13,"METAL WORK"]
[]
[13.1,"METAL WORK "]
["13.1.1","Metal Work ","Ton",0.5]
[null,"Sub-Total"]
["Total carried forward"]
["Total brought forward"]
[14,"BRIDGE "]
[]
[14.1,"FLOOR "]
["14.1.1","Remove Bridge Carpet ","m²",5]
["14.1.2","Supply And Fit Vinyl Foor In Bridge","m²",5]
[]
[14.2,"WINDOWS "]
["14.2.1","Remove, Supply And Fit New Seals In The Bridge ","No.",4]
["14.2.2","Supply And Fit Draining System In The Windows","No.",2]
["14.2.3","Remove, Supply And Fit New Wipers ","No.",8]
[]
[14.3,"MASTER'S CHAIR "]
["14.3.1","Repair And Replace Seat Cover On Master'S Chair","No.",1]
[null,"Sub-Total"]
[15,"MISCELLANEOUS WORK"]
[]
[15.1,"MISCELLANEOUS WORK"]
["15.1.1","Budget R50 000 For Unplanned Work Identified After Inspection","Prov. Sum",1,{"v":50000,"d":"R50,000.00"},{"v":50000,"d":"R50,000.00"}]
["15.1.2","Budget For Skilled Labour 1 X 20 Hours","hrs",20]
["15.1.3","Budget For Semi-Skilled Labour 1 X 20 Hours","hrs",20]
["15.1.4","Budget For Machine Shop Cost 1  X 10 Hours","hrs",10]
["15.1.5","Assist Cmeo And Voith Technician With Voith Heath Check for 4 Hrs a day","Days",4]
["15.1.6","Scaffolding","Days",7]
["15.1.7","Budget For Skilled Labour Overtime For Three Saturdays And Three Sundays (4Hrs Per Day) ","No.",2]
["15.1.8","She File, She Plan And Risk Assessment","Sum",1]
[]
[15.2,"DISBURSEMENTS"]
["15.2.1","Travelling Expenses ","Days",28]
["15.2.2","Accomodation","Days",28]
["15.2.3","Other disbursements","Days",28]
[]
[15.3,"GENERAL CLEANING"]
["15.3.1","Provide Semi Skilled  Labour 8 Hrs For Cleaning And Assisting Tnpa Engine Room Staff","Days",7]
[]
[null,"Sub-Total"]
[null,"Total  for Task 2 excluding VAT"]
[null,"VAT 15%"]
[null,"Total  for Task 2 including VAT - carried forward to final summary"]
[]
[null,"FINAL SUMMARY"]
[null,"Total  for Task 1 including VAT - Brought forward"]
[null,"Total  for Task 2 including VAT - brought forward"]
[null,"Grand Total  Total including VAT Carried to Master Services Agreement"]