{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["ICP-MS BOQ"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"ICP-MS BOQ","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"merged":[[0,2,0,6],[1,2,1,6],[2,2,2,6],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,10,4],[9,5,10,5],[9,6,10,6],[13,0,20,0],[22,0,24,0],[34,1,34,6]]}
[null,"BID NUMBER","RW 10406411/23"]
[null,"BID DESCRIPTION","Supply, delivery, installation, commisioning and training on Inductively Coupled Plasma Mass Spectrometry (ICP-MS) used for the analysis of water treatment chemicals at Process Technology, Scientific Services."]
[null,"BIDDER NAME"]
[null,"DELIVERABLES (DESCRIPTION)","Specification","QTY (A)","UNIT OF MEASURE","RATE (B)","Total (A x B)"]
[null,"ICP-MS equiped with triple quadropole"]
["1.","Complete ICP-MS system for elemental analysis with a triple quadropole. The system should be all inclusive of all components required to allow its full, fluent functioning (Turn Key System)",null,1,"NO",null,{"$f":"D6*F6","v":0}]
["2.","Water recirculator ",null,1,"NO",null,0]
["3.","Autosampler that can handle 120 samples with automatic dilution features for samples and standards ",null,1,"NO"]
["4.","UPS system providing \"Clean power\" with sufficient backup capacity",null,1,"NO",null,0]
["5.","Computer system with instrument controlling software: (Intel i5 Quad Core CPU or faster\n16 GB RAM or more, 1 TB Hard Drive minimum capacity, Gigabit, Windows 10 Operating System, 64 bit Microsoft\nDVD Combo, 17’’ LCD Flat screen or bigger, 1 user license, valid for the full life of the instrument system)",null,1,"NO",null,{"$f":"D10*F11","v":0}]
[]
["6.","Instrument start up standards set/kit","Standards start up kit to test instrument capability to detect and quantify all elements ",1,"NO",null,{"$f":"D12*F12","v":0}]
["7.","On-site Rand Water Site Installation, commissioning and training by factory trained engineers or applications specialists. ",null,1,"NO",null,{"$f":"D13*F13","v":0}]
["8.","Site preparation ",null,1,"NO",null,{"$f":"D14*F14","v":0}]
[null,"Electrical; ensure that electrical meet the supply and power specifications of the instrument; provide socket suitable to power requirements of the instrument  ",null,1,"NO",null,{"$f":"D15*F15","v":0}]
[null,"Cooling water",null,1,"NO"]
[null,"Argon gas supply pipeline installation that can handle specified flow rate and pressure:","with suitable gas regulators ",1,"NO",null,{"$f":"D17*F17","v":0}]
[null,"Cell gas supply pipeline installation:","with suitable gas regulators ",1,"NO",null,0]
[null,"Plasma Exhaust extraction Installation:",null,1,"NO",null,0]
[null,"Installation of Desk for the TQ-ICP-MS instrument ","Based on instrument’s dimensions",1,"NO",null,0]
[null,"Air conditioner installation; suitable for temperature adjustments as required by the instrument ",null,1,"NO",null,0]
[null,"Supply Collision gases with safe cage, ",null,1,"NO"]
["9.","Additional items"]
[null,"Training of 5 personnel on Introductory training / hardware and maintenance training / Fault finding training / Method development and interference elimination training for a minimum of 5 days or until personnel are competent to use instrument and troubleshoot the instrument: 2x Scientists and 2 x Chemists, 1 x Technician ",null,1,"NO"]
[null,"Instrument validation including the validation report with all instrument testing conducted "]
[]
[null,"SUB-TOTAL"]
[]
[]
[null,"Total for all  Deliverables",null,{"$f":"G27","v":0}]
[null,"SUBTOTAL before VAT",null,{"$f":"SUM(D30:D30)","v":0}]
[null,"VAT (if applicable)",null,{"$f":"D31*0.15","v":0}]
[null,"FORM OF OFFER \n(for commercial evaluation purposes)",null,{"$f":"SUM(D31:D32)","v":0}]