{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["1M-36458"],"not_rendered":{"defined_names":31},"read":"whole","date_system":"1900"}

{"sheet":"1M-36458","index":0,"n_rows":497,"n_cols":10,"rows_kept":497,"merged":[[1,1,1,2],[1,3,1,9]]}
[]
[null,"1M-36458",null,"Rates-Based Panel Contract for Roadway Related Construction Works to be used As-and-When-Required, for a period of 36 Months (CIDB Grades 4, 5 and 6)"]
[]
[{"$nulls":6},"BILL of QUANTITIES"]
[]
[]
[null,1,"PRELIMINARY AND GENERAL ITEMS",{"$nulls":6},{"$f":"J47","v":0}]
[null,null,"0102","C1.2 GENERAL REQUIREMENTS AND PROVISIONS",{"$nulls":3},40,{"$f":"J48","v":0}]
[]
[null,null,"0105","C1.5 ACCOMMODATION OF TRAFFIC",{"$nulls":3},20,{"$f":"J157","v":0}]
[null,2,"SITE CLEARANCE",{"$nulls":6},{"$f":"J190","v":0}]
[null,null,"0106","C1.6 CLEARING AND GRUBBING",{"$nulls":3},13,{"$f":"J191","v":0}]
[null,3,"SERVICES"]
[null,null,"0201","C2.1 GEN REQMENTS AND TRENCHING SERVICE",{"$nulls":3},10,{"$f":"J211","v":{"v":1160000,"d":"R1,160,000.00"}}]
[null,4,"DRAINAGE",{"$nulls":6},{"$f":"J240","v":0}]
[null,null,"0302","C3.2 CULVERTS",{"$nulls":3},36,{"$f":"J241","v":0}]
[null,null,"0303","C3.3 CONCRETE KERBING AND CHANNELING",{"$nulls":3},14,{"$f":"J306","v":0}]
[null,5,"EARTHWORKS"]
[null,null,"0402","C4.2 CUT MATERIALS",{"$nulls":3},8,{"$f":"J324","v":{"v":50000,"d":"R50,000.00"}}]
[null,null,"0403","C4.3 EXISTING ROAD MATERIALS",{"$nulls":3},17,{"$f":"J334","v":0}]
[null,null,"0404","C4.4 COMMERCIAL MATERIALS",{"$nulls":3},5,{"$f":"J353","v":0}]
[null,6,"LAYERWORKS",{"$nulls":6},{"$f":"J359","v":0}]
[null,null,"0501","C5.1 ROADBED",{"$nulls":3},9,{"$f":"J360","v":0}]
[null,null,"0502","C5.2 FILL",{"$nulls":3},7,{"$f":"J371","v":0}]
[null,null,"0503","C5.3 ROAD PAVEMENT LAYERS",{"$nulls":3},10,{"$f":"J379","v":0}]
[null,null,"0504","C5.4 STABILISATION",{"$nulls":3},5,{"$f":"J392","v":0}]
[]
[null,null,"0901","C9.1 ASPHALT LAYERS",{"$nulls":3},14,{"$f":"J398","v":0}]
[null,7,"ANCILLARY ROAD WORKS"]
[null,null,"1104","C11.4 ROAD RESTRAINT SYSTEMS",{"$nulls":3},9,{"$f":"J419","v":0}]
[null,null,"1105","C11.5 FENCING",{"$nulls":3},5,{"$f":"J429","v":0}]
[null,null,"1106","C11.6 ROAD SIGNS",{"$nulls":3},10,{"$f":"J436","v":0}]
[null,null,"1107","C11.7 ROAD MARKINGS AND ROAD STUDS",{"$nulls":3},9,{"$f":"J447","v":0}]
[null,null,"1108","C11.8 LANDSCAPING AND PLANTING PLANTS",{"$nulls":3},7,{"$f":"J461","v":0}]
[null,null,"1109","C11.9 FINISHING  ROAD AND ROAD RESERVE",{"$nulls":3},7,{"$f":"J469","v":{"v":250000,"d":"R250,000.00"}}]
[null,null,"1206","C12.6 MECH STABILISED FILL AND GABIONS",{"$nulls":3},16,{"$f":"J479","v":0}]
[]
[{"$nulls":8},"Sub-Total:"]
[]
[{"$nulls":8},"VAT @ 15%:",{"$f":"J38*15/100","v":0}]
[]
[{"$nulls":8},"TOTAL CARRIED TO FORM OF OFFER (C1.1):",{"$f":"J38+J40","v":0}]
[]
[]
[null,"Section","Chapter","Item#","Clause","Unit","Description","Est. Qty.","Rate","Value"]
[]
[null,1,"PRELIMINARY AND GENERAL ITEMS",{"$nulls":5},"SECTION TOTAL:",{"$f":"J48+J157","v":0}]
[null,1,"0102","C1.2 GENERAL REQUIREMENTS AND PROVISIONS",{"$nulls":3},40,"Chapter Total:",{"$f":"SUM(J49:J156)","v":0}]
[{"$nulls":6},"C1.3.1.1:   Fixed Obligations per Work Package Order"]
[null,1,"0102",1,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H50*I50","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0102",2,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H51*I51/100","v":0}]
[null,1,"0102",3,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H52*I52","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0102",4,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H53*I53/100","v":0}]
[null,1,"0102",5,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H54*I54","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",6,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H55*I55/100","v":0}]
[null,1,"0102",7,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H56*I56","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",8,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H57*I57/100","v":0}]
[null,1,"0102",9,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H58*I58","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0102",10,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H59*I59/100","v":0}]
[{"$nulls":6},"C1.3.1.3:   Time-related Obligations per Work Package Order"]
[null,1,"0102",11,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H61*I61","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0102",12,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H62*I62/100","v":0}]
[null,1,"0102",13,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H63*I63","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0102",14,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H64*I64/100","v":0}]
[null,1,"0102",15,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H65*I65","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",16,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H66*I66/100","v":0}]
[null,1,"0102",17,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H67*I67","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",18,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H68*I68/100","v":0}]
[null,1,"0102",19,"PS.C1.3.1.1\nPS.C1.3.1.2","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H69*I69","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0102",20,"PS.C1.3.1.1\nPS.C1.3.1.2","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H70*I70/100","v":0}]
[{"$nulls":6},"PS.9:   Environmental Management: Monitoring of compliance with and reporting on the EMP per Work Package Order"]
[null,1,"0102",21,"C1.2.1.1","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H72*I72","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0102",22,"C1.2.1.1","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H73*I73/100","v":0}]
[null,1,"0102",23,"C1.2.1.1","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H74*I74","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0102",24,"C1.2.1.1","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H75*I75/100","v":0}]
[null,1,"0102",25,"C1.2.1.1","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H76*I76","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",26,"C1.2.1.1","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H77*I77/100","v":0}]
[null,1,"0102",27,"C1.2.1.1","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H78*I78","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",28,"C1.2.1.1","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H79*I79/100","v":0}]
[null,1,"0102",29,"C1.2.1.1","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H80*I80","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0102",30,"C1.2.1.1","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H81*I81/100","v":0}]
[null,1,"0102",31,"C1.2.1.1","months","Dedicated environmental officer per Work Package Order",12,null,{"$f":"H82*I82","v":0}]
[{"$nulls":6},"PS.14:   Liasing, coordinating and mentoring CPG Sub-contractors per Work Package Order"]
[null,1,"0102",32,"C1.3.1.1","sum","Where Work Package Order is <R1m",1,null,{"$f":"H84*I84","v":0}]
[null,1,"0102",33,"C1.3.1.1","sum","Where Work Package Order is >R1m and <R3m",1,null,{"$f":"H85*I85","v":0}]
[null,1,"0102",34,"C1.3.1.1","sum","Where Work Package Order is >R3m and <R6m",1,null,{"$f":"H86*I86","v":0}]
[null,1,"0102",35,"C1.3.1.1","sum","Where Work Package Order is >R6m and <R10m",1,null,{"$f":"H87*I87","v":0}]
[null,1,"0102",36,"C1.3.1.1","sum","Where Work Package Order is >R10m",1,null,{"$f":"H88*I88","v":0}]
[{"$nulls":6},"PS.12.4: Submission of As-Built Data per Work Package Order"]
[null,1,"0102",37,"C1.3.1.1","sum","Where Work Package Order is <R1m",1,null,{"$f":"H90*I90","v":0}]
[null,1,"0102",38,"C1.3.1.1","sum","Where Work Package Order is >R1m and <R3m",1,null,{"$f":"H91*I91","v":0}]
[null,1,"0102",39,"C1.3.1.1","sum","Where Work Package Order is >R3m and <R6m",1,null,{"$f":"H92*I92","v":0}]
[null,1,"0102",40,"C1.3.1.1","sum","Where Work Package Order is >R6m and <R10m",1,null,{"$f":"H93*I93","v":0}]
[null,1,"0102",41,"C1.3.1.1","sum","Where Work Package Order is >R10m",1,null,{"$f":"H94*I94","v":0}]
[{"$nulls":6},"PS.10: Health and Safety Plan and Implementation of Health and Safety Plan per Work Package Order"]
[null,1,"0102",42,"C1.2.5.1","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H96*I96","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0102",43,"C1.2.5.1","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H97*I97/100","v":0}]
[null,1,"0102",44,"C1.2.5.1","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H98*I98","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0102",45,"C1.2.5.1","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H99*I99/100","v":0}]
[null,1,"0102",46,"C1.2.5.1","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H100*I100","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",47,"C1.2.5.1","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H101*I101/100","v":0}]
[null,1,"0102",48,"C1.2.5.1","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H102*I102","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",49,"C1.2.5.1","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H103*I103/100","v":0}]
[null,1,"0102",50,"C1.2.5.1","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H104*I104","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0102",51,"C1.2.5.1","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H105*I105/100","v":0}]
[{"$nulls":6},"Programming and Reporting Per Work Package Order:\nWhere Work Package Order is <R6m"]
[null,1,"0102",52,"C1.2.1.1\nPS.1","Lump sum","Submission of a Scheme 1 Programme",1,null,{"$f":"H107*I107","v":0}]
[null,1,"0102",53,"C1.2.1.1\nPS.1","months","Reviewing and updating a Scheme 1 Programme",12,null,{"$f":"H108*I108","v":0}]
[{"$nulls":6},"Programming and Reporting Per Work Package Order:\nWhere Work Package Order is >R6m"]
[null,1,"0102",54,"C1.2.2.4\nPS.1","Lump sum","Submission of a Scheme 2 Full Programme",1,null,{"$f":"H110*I110","v":0}]
[null,1,"0102",55,"C1.2.2.5\nPS.1","months","Reviewing and updating a Scheme 2 programme every month",12,null,{"$f":"H111*I111","v":0}]
[{"$nulls":6},"PS.14: Stakeholder Management & Liaison per Work Package Order"]
[null,1,"0102",56,"C1.2.4","PC Sum","Where Work Package Order is <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H113*I113","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",57,"C1.2.4","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H114*I114/100","v":0}]
[null,1,"0102",58,"C1.2.4","PC Sum","Where Work Package Order is >R6m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H115*I115","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",59,"C1.2.4","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H116*I116/100","v":0}]
[{"$nulls":6},"Community Liaison Officer"]
[null,1,"0102",60,"PS.11","PC Sum","Allow for CLO to be appointed per Work Package Order",{"v":100000,"d":"100,000"},1,{"$f":"H118*I118","v":{"v":100000,"d":"R100,000.00"}}]
[null,1,"0102",61,"PS.11","%","Handling costs and profit in respect of item above",{"v":100000,"d":"100,000"},null,{"$f":"H119*I119/100","v":0}]
[{"$nulls":6},"Provision of security on site to guard against any disruption of the works throughout the duration of each Work Package Order"]
[null,1,"0102",62,"PS.11.4","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H121*I121","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0102",63,"PS.11.4","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H122*I122/100","v":0}]
[null,1,"0102",64,"PS.11.4","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H123*I123","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0102",65,"PS.11.4","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H124*I124/100","v":0}]
[null,1,"0102",66,"PS.11.4","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H125*I125","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0102",67,"PS.11.4","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H126*I126/100","v":0}]
[null,1,"0102",68,"PS.11.4","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H127*I127","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0102",69,"PS.11.4","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H128*I128/100","v":0}]
[null,1,"0102",70,"PS.11.4","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H129*I129","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0102",71,"PS.11.4","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H130*I130/100","v":0}]
[null,1,"0102",72,"C1.3.2\nPS.C1.3.2","no.","Contract sign boards",1,null,{"$f":"H131*I131","v":0}]
[{"$nulls":6},"Routine road maintenance of existing public roads within the Site of the Works or other public roads outside the Site of the Works which are used as detours"]
[null,1,"0102",73,"C1.2.3.1\nPS.12.1","m2","Grass cutting",{"v":5000,"d":"5,000"},null,{"$f":"H133*I133","v":0}]
[null,1,"0102",74,"C1.2.3.2\nPS.12.1","m","Drain cleaning",250,null,0]
[null,1,"0102",75,"C1.2.3.3\nPS.12.1","m3","Cleaning out culverts",25,null,0]
[null,1,"0102",76,"C1.2.3.7\nPS.12.1","m2","Base and/or surface patching using hot plant mixed asphalt",20,null,0]
[null,1,"0102",77,"C1.2.3.10\nPS.12.1","kl","Watering of temporary gravel deviations and existing roads used as detours",5,null,0]
[null,1,"0102",78,"C1.2.3.11\nPS.12.1","PC Sum","Other road maintenance work ordered by the Engineer",{"v":50000,"d":"50,000"},1,{"v":50000,"d":"R50,000.00"}]
[null,1,"0102",79,"C1.2.3.12\nPS.12.1","%","Handling cost, profit and all other charges in respect of item C1.2.3.11",{"v":50000,"d":"50,000"},null,{"$f":"H139*I139/100","v":0}]
[{"$nulls":6},"Dayworks"]
[null,1,"0102",80,"C1.2.8.1(a)","hour","Personnel:\n(a) Unskilled labourer",30,null,{"$f":"H141*I141","v":0}]
[null,1,"0102",81,"C1.2.8.1(b)","hour","(b) Semi-skilled labourer",10,null,0]
[null,1,"0102",82,"C1.2.8.1 (c )","hour","(c) Skilled labourer",10,null,0]
[null,1,"0102",83,"C1.2.8.1(d)","hour","(d) Gang leader",10,null,0]
[null,1,"0102",84,"C1.2.8.1 (e )","hour","(e) Foreman",10,null,0]
[null,1,"0102",85,"C1.2.8.2(a)","hour","Construction equipment :\n(a) Motor grader",15,null,0]
[null,1,"0102",86,"C1.2.8.2(b)","hour","(b) Vibratory roller",15,null,0]
[null,1,"0102",87,"C1.2.8.2 (c )","hour","(c) Pneumatic roller",15,null,0]
[null,1,"0102",88,"C1.2.8.2€","hour","(e) Tractor loader backhoe",15,null,0]
[null,1,"0102",89,"C1.2.8.2(f)","hour","(f) Excavator",15,null,0]
[null,1,"0102",90,"C1.2.8.3(a)","km","Vehicles :\n(a) Light delivery vehicle",40,null,0]
[null,1,"0102",91,"C1.2.8.3 (c )","km","(c) Dump truck",40,null,0]
[null,1,"0102",92,"C1.2.8.4(a)","PC Sum","Materials - Procurement of materials",{"v":100000,"d":"100,000"},1,{"v":100000,"d":"R100,000.00"}]
[null,1,"0102",93,"C1.2.8.4(b)","%","(b) Contractor's handling costs, profit and all other charges in respect of item C1.2.8.4(a)",{"v":100000,"d":"100,000"},null,{"$f":"H154*I154/100","v":0}]
[{"$nulls":6},"***********                 NOTE                  *************\nThe following item (with a negative value) is to be\nincluded in the summation of item Amounts"]
[null,1,"0102",94,"-","PC Sum","PC Sum reversal",{"v":-216250000,"d":"-216,250,000"},1,{"$f":"H156*I156","v":{"v":-216250000,"d":"-R216,250,000.00"}}]
[null,1,"0105","C1.5 ACCOMMODATION OF TRAFFIC",{"$nulls":3},20,"Chapter Total:",{"$f":"SUM(J158:J189)","v":0}]
[{"$nulls":6},"Accommodation of pedestrian, non-motorised and motorised traffic"]
[null,1,"0105",1,"C1.5.1.1\nPS.1.3","PC Sum","Where Work Package Order is <R1m",{"v":1000000,"d":"1,000,000"},1,{"$f":"H159*I159","v":{"v":1000000,"d":"R1,000,000.00"}}]
[null,1,"0105",2,"C1.5.1.1\nPS.1.3","%","Enter % of Work Package Order",{"v":1000000,"d":"1,000,000"},null,{"$f":"H160*I160/100","v":0}]
[null,1,"0105",3,"C1.5.1.1\nPS.1.3","PC Sum","Where Work Package Order is >R1m and <R3m",{"v":3000000,"d":"3,000,000"},1,{"$f":"H161*I161","v":{"v":3000000,"d":"R3,000,000.00"}}]
[null,1,"0105",4,"C1.5.1.1\nPS.1.3","%","Enter % of Work Package Order",{"v":3000000,"d":"3,000,000"},null,{"$f":"H162*I162/100","v":0}]
[null,1,"0105",5,"C1.5.1.1\nPS.1.3","PC Sum","Where Work Package Order is >R3m and <R6m",{"v":6000000,"d":"6,000,000"},1,{"$f":"H163*I163","v":{"v":6000000,"d":"R6,000,000.00"}}]
[null,1,"0105",6,"C1.5.1.1\nPS.1.3","%","Enter % of Work Package Order",{"v":6000000,"d":"6,000,000"},null,{"$f":"H164*I164/100","v":0}]
[null,1,"0105",7,"C1.5.1.1\nPS.1.3","PC Sum","Where Work Package Order is >R6m and <R10m",{"v":10000000,"d":"10,000,000"},1,{"$f":"H165*I165","v":{"v":10000000,"d":"R10,000,000.00"}}]
[null,1,"0105",8,"C1.5.1.1\nPS.1.3","%","Enter % of Work Package Order",{"v":10000000,"d":"10,000,000"},null,{"$f":"H166*I166/100","v":0}]
[null,1,"0105",9,"C1.5.1.1\nPS.1.3","PC Sum","Where Work Package Order is >R10m",{"v":20000000,"d":"20,000,000"},1,{"$f":"H167*I167","v":{"v":20000000,"d":"R20,000,000.00"}}]
[null,1,"0105",10,"C1.5.1.1\nPS.1.3","%","Enter % of Work Package Order",{"v":20000000,"d":"20,000,000"},null,{"$f":"H168*I168/100","v":0}]
[null,1,"0105",11,"C1.5.1.1\nPS.1.3","man-day","Traffic safety officer",100,null,{"$f":"H169*I169","v":0}]
[{"$nulls":6},"Traffic Safety Officer: Penalties"]
[null,1,"0105",12,"A1.5.3.7\nPS.1.3.7","RateOnly","(a) Fixed Penalty per occurrence, R2000 per day",0]
[null,1,"0105",13,"A1.5.3.7\nPS.1.3.7","RateOnly","(b) Time-Related Penalty, R1000 per hour",0]
[null,1,"0105",14,"C1.5.7.1(b)","no","Delineators including mounting bases and ballast: Double sided, reversible left or right (1200mm x 250mm)",200,null,{"$f":"H173*I173","v":0}]
[null,1,"0105",15,"PS.1.3.6","m","Temporary barriers for accommodation of traffic, concrete New Jersey type, Contractor's own source",30,null,{"$f":"H174*I174","v":0}]
[null,1,"0105",16,"C1.5.7.3","man-day","Flagmen",100,null,{"$f":"H175*I175","v":0}]
[null,1,"0105",17,"C1.5.7.4","man-day","Traffic controllers",100,null,{"$f":"H176*I176","v":0}]
[{"$nulls":6},"Provision of Illuminated Traffic Signs"]
[null,1,"0105",18,"C1.5.7.5(a)(i)","no","Sign mounted flashing amber lights (2 lights with the specified power supply) mounted on a backing board which is:\n(a)(i) 900 mm wide x 150 mm high",6,null,{"$f":"H178*I178","v":0}]
[null,1,"0105",19,"C1.5.7.5(b)","no","(b) Flashing LED illuminated arrow board",6,null,0]
[{"$nulls":6},"Maintenance of Illuminated Traffic Signs",null,null,0]
[null,1,"0105",20,"C1.5.7.6(a)","no","(a) Sign mounted flashing amber lights (i and ii)",2,null,0]
[null,1,"0105",21,"C1.5.7.6(b)","no","(b) Flashing LED illuminated arrow board",2,null,0]
[null,1,"0105",22,"C1.5.7.6 (c )","no","(c) Illuminated road sign – R & TR series (1200mm diameter)",2,null,0]
[null,1,"0105",23,"C1.5.7.6(d)","no","(d) Illuminated road sign – TW series (1200mm sides)",2,null,0]
[null,1,"0105",24,"C1.5.7.9","no","Cleaning of traffic control facilities",2,null,0]
[{"$nulls":6},"Traffic Calming Devices"]
[null,1,"0105",25,"C1.5.7.7(a)","m","(a) 25 mm high x 100 mm wide asphalt rumble strips",50,null,{"$f":"H187*I187","v":0}]
[{"$nulls":6},"************                 NOTE                  *************\nThe following item (with a negative value) is to be\nincluded in the summation of item Amounts"]
[null,1,"0105",26,"-","PC Sum","PC Sum reversal",{"v":-40000000,"d":"-40,000,000"},1,{"$f":"H189*I189","v":{"v":-40000000,"d":"-R40,000,000.00"}}]
[null,2,"SITE CLEARANCE",{"$nulls":5},"SECTION TOTAL:",{"$f":"J191","v":0}]
[null,2,"0106","C1.6 CLEARING AND GRUBBING",{"$nulls":3},13,"Chapter Total:",{"$f":"SUM(J192:J209)","v":0}]
[{"$nulls":6},"Clearing"]
[null,2,"0106",1,"C1.6.1.1","m2","Clearing with machines and some hand labour where necessary",{"v":2000,"d":"2,000"},null,{"$f":"H193*I193","v":0}]
[null,2,"0106",2,"C1.6.1.2","m2","Clearing with hand labour only when labour enhanced work is specified",{"v":2000,"d":"2,000"},null,{"$f":"H194*I194","v":0}]
[{"$nulls":6},"Grubbing"]
[null,2,"0106",3,"C1.6.2.1","m2","Grubbing with machines and some hand labour where necessary",{"v":2000,"d":"2,000"},null,{"$f":"H196*I196","v":0}]
[null,2,"0106",4,"C1.6.2.2","m2","Grubbing with hand labour when labour enhancement work is specified or it is not practical to use a machine",{"v":2000,"d":"2,000"},null,{"$f":"H197*I197","v":0}]
[{"$nulls":6},"Removal and Grubbing of Large Trees and Tree Stumps"]
[null,2,"0106",5,"C1.6.3.1","no","Girth equal to or exceeding 1,0 m up to and including 2,0 m",5,null,{"$f":"H199*I199","v":0}]
[null,2,"0106",6,"C1.6.3.2","no","Girth exceeding 2,0 m up to and including 3,0 m",3,null,{"$f":"H200*I200","v":0}]
[{"$nulls":6},"Stockpile Site"]
[null,2,"0106",7,"C4.1.10","m3","Compacting the floor of the stockpile sites",20,null,{"$f":"H202*I202","v":0}]
[null,2,"0106",8,"C4.1.15.2(c)","m3","Finishing of the stockpile sites",20,null,{"$f":"H203*I203","v":0}]
[null,2,"0106",9,"C1.6.9.1","m3","Conservation of topsoil:\nStockpiling topsoil",200,null,{"$f":"H204*I204","v":0}]
[null,2,"0106",10,"C1.6.9.2","m3","Windrowing topsoil",200,null,{"$f":"H205*I205","v":0}]
[{"$nulls":6},"Hauling Material"]
[null,2,"0106",11,"C1.7.2.1(a)\nPS.C1.7","m3","Hauling material for use in the Works and off-loading it on the site of the Works:\n(a) Soil, gravel, crushed stone and pavement layer material",{"v":5000,"d":"5,000"},null,{"$f":"H207*I207","v":0}]
[null,2,"0106",12,"C1.7.2.2(a)\nPS.C1.7","m3","Hauling material to spoil and off-loading it at a designated spoil area:\n(a) Cleared and grubbed material (organic matter and all other unsuitable or waste material)",{"v":3000,"d":"3,000"},null,{"$f":"H208*I208","v":0}]
[null,2,"0106",13,"C1.7.2.2(b)\nPS.C1.7","m3","(b) Soil and gravel material",{"v":1000,"d":"1,000"},null,{"$f":"H209*I209","v":0}]
[null,3,"SERVICES",{"$nulls":5},"SECTION TOTAL:",{"$f":"J211","v":{"v":1160000,"d":"R1,160,000.00"}}]
[null,3,"0201","C2.1 GEN REQMENTS AND TRENCHING SERVICE",{"$nulls":3},10,"Chapter Total:",{"$f":"SUM(J212:J239)","v":{"v":1160000,"d":"R1,160,000.00"}}]
[{"$nulls":6},"Relocation of Services by Others:\nWater"]
[null,3,"0201",1,"C2.1.1.2\nPS.3","PC Sum","Permanent services relocation or protection work by others",{"v":150000,"d":"150,000"},{"v":1,"d":"R1.00"},{"$f":"H213*I213","v":{"v":150000,"d":"R150,000.00"}}]
[null,3,"0201",2,"C2.1.1.3\nPS.3","%","Handling costs and profit in respect of item above",{"v":150000,"d":"150,000"},null,{"$f":"H214*I214/100","v":0}]
[{"$nulls":6},"Sewer"]
[null,3,"0201",3,"C2.1.1.2\nPS.4","PC Sum","Permanent services relocation or protection work by others",{"v":150000,"d":"150,000"},{"v":1,"d":"R1.00"},{"$f":"H216*I216","v":{"v":150000,"d":"R150,000.00"}}]
[null,3,"0201",4,"C2.1.1.3\nPS.4","%","Handling costs and profit in respect of item above",{"v":150000,"d":"150,000"},null,{"$f":"H217*I217/100","v":0}]
[{"$nulls":6},"Electricity"]
[null,3,"0201",5,"C2.1.1.2\nPS.6","PC Sum","Permanent services relocation or protection work by others",{"v":150000,"d":"150,000"},{"v":1,"d":"R1.00"},{"$f":"H219*I219","v":{"v":150000,"d":"R150,000.00"}}]
[null,3,"0201",6,"C2.1.1.3\nPS.6","%","Handling costs and profit in respect of item above",{"v":150000,"d":"150,000"},null,{"$f":"H220*I220/100","v":0}]
[{"$nulls":6},"Telecommunications"]
[null,3,"0201",7,"C2.1.1.2\nPS.7","PC Sum","Permanent services relocation or protection work by others",{"v":150000,"d":"150,000"},{"v":1,"d":"R1.00"},{"$f":"H222*I222","v":{"v":150000,"d":"R150,000.00"}}]
[null,3,"0201",8,"C2.1.1.3\nPS.7","%","Handling costs and profit in respect of item above",{"v":150000,"d":"150,000"},null,{"$f":"H223*I223/100","v":0}]
[{"$nulls":6},"Relocation of Services by the Contractor:\nWater"]
[null,3,"0201",9,"C2.1.1.4\nPS.3","ProvSum","Permanent services relocation or protection work by the Contractor",1,{"v":150000,"d":"R150,000.00"},{"$f":"H225*I225","v":{"v":150000,"d":"R150,000.00"}}]
[{"$nulls":6},"Sewer"]
[null,3,"0201",10,"C2.1.1.4\nPS.4","ProvSum","Permanent services relocation or protection work by the Contractor",1,{"v":150000,"d":"R150,000.00"},{"$f":"H227*I227","v":{"v":150000,"d":"R150,000.00"}}]
[{"$nulls":6},"Electricity"]
[null,3,"0201",11,"C2.1.1.4\nPS.6","ProvSum","Permanent services relocation or protection work by the Contractor",1,{"v":120000,"d":"R120,000.00"},{"$f":"H229*I229","v":{"v":120000,"d":"R120,000.00"}}]
[{"$nulls":6},"Telecommunications"]
[null,3,"0201",12,"C2.1.1.4\nPS.7","ProvSum","Permanent services relocation or protection work by the Contractor",1,{"v":120000,"d":"R120,000.00"},{"$f":"H231*I231","v":{"v":120000,"d":"R120,000.00"}}]
[{"$nulls":6},"Existing Services Location, Detection and Verification"]
[null,3,"0201",13,"C2.1.2.1\nPS.2","PC Sum","Using specialist detection services (ground penetrating radar, radio detection etc.)",{"v":20000,"d":"20,000"},{"v":1,"d":"R1.00"},{"$f":"H233*I233","v":{"v":20000,"d":"R20,000.00"}}]
[null,3,"0201",14,"C2.1.2.2\nPS.2","%","Handling costs and profit in respect of item above",{"v":20000,"d":"20,000"},null,{"$f":"H234*I234/100","v":0}]
[null,3,"0201",15,"C2.1.2.5\nPS.2","m3","Using hand excavation to locate, expose and verify services",30,null,{"$f":"H235*I235","v":0}]
[null,3,"0201",16,"C2.1.27.1\nPS.C2.1.27.1","m3","Demolition of existing manholes, access chambers and other service structures consisting of: Unreinforced concrete",5,null,{"$f":"H236*I236","v":0}]
[null,3,"0201",17,"C2.1.27.2\nPS.C2.1.27.1","m3","Demolition of existing manholes, access chambers and other service structures consisting of: Reinforced concrete",5,null,{"$f":"H237*I237","v":0}]
[null,3,"0201",18,"C2.1.27.3\nPS.C2.1.27.2","m3","Demolition of existing manholes, access chambers and other service structures consisting of: Masonry",5,null,{"$f":"H238*I238","v":0}]
[null,3,"0201",19,"C2.2.5.2","m3","Concrete encasement of services (class 20/26)",30,null,{"$f":"H239*I239","v":0}]
[null,4,"DRAINAGE",{"$nulls":5},"SECTION TOTAL:",{"$f":"J241+J306","v":0}]
[null,4,"0302","C3.2 CULVERTS",{"$nulls":3},36,"Chapter Total:",{"$f":"SUM(J242:J305)","v":0}]
[{"$nulls":6},"Excavation:\n375mm Pipes"]
[null,4,"0302",1,"C3.2.1.1(a)\nPS.C3.2.3.2\nPS.C2.1","m3","Excavation for culvert structures: in all material situated within the following depth ranges below the surface level:\n(a) 0 m to 1,5 m",30,null,{"$f":"H243*I243","v":0}]
[null,4,"0302",2,"C3.2.1.1(b)\nPS.C3.2.3.2\nPS.C2.1","m3","(b) Exceeding 1,5 m and up to 3,0 m",20,null,{"$f":"H244*I244","v":0}]
[{"$nulls":6},"450mm Pipes"]
[null,4,"0302",3,"C3.2.1.1(a)\nPS.C3.2.3.2\nPS.C2.1","m3","Excavation for culvert structures: in all material situated within the following depth ranges below the surface level:\n(a) 0 m to 1,5 m",30,null,{"$f":"H246*I246","v":0}]
[null,4,"0302",4,"C3.2.1.1(b)\nPS.C3.2.3.2\nPS.C2.1","m3","(b) Exceeding 1,5 m and up to 3,0 m",20,null,{"$f":"H247*I247","v":0}]
[{"$nulls":6},"600mm Pipes"]
[null,4,"0302",5,"C3.2.1.1(a)\nPS.C3.2.3.2\nPS.C2.1","m3","Excavation for culvert structures: in all material situated within the following depth ranges below the surface level:\n(a) 0 m to 1,5 m",30,null,{"$f":"H249*I249","v":0}]
[null,4,"0302",6,"C3.2.1.1(b)\nPS.C3.2.3.2\nPS.C2.1","m3","(b) Exceeding 1,5 m and up to 3,0 m",20,null,{"$f":"H250*I250","v":0}]
[{"$nulls":6},"900mm Pipes"]
[null,4,"0302",7,"C3.2.1.1(a)\nPS.C3.2.3.2\nPS.C2.1","m3","Excavation for culvert structures: in all material situated within the following depth ranges below the surface level: (a) 0 m to 1,5 m",30,null,{"$f":"H252*I252","v":0}]
[null,4,"0302",8,"C3.2.1.1(b)\nPS.C3.2.3.2\nPS.C2.1","m3","(b) Exceeding 1,5 m and up to 3,0 m",20,null,{"$f":"H253*I253","v":0}]
[null,4,"0302",9,"C3.2.1.1(c )\nPS.C3.2.3.2\nPS.C2.1","m3","(c) Exceeding 3,0 m and up to 4,5 m",10,null,{"$f":"H254*I254","v":0}]
[{"$nulls":6},"Culverts (up to 3m x 3m)"]
[null,4,"0302",10,"C3.2.1.1(a)\nPS.C3.2.3.2\nPS.C2.1","m3","Excavation for culvert structures: in all material situated within the following depth ranges below the surface level: (a) 0 m to 1,5 m",30,null,{"$f":"H256*I256","v":0}]
[null,4,"0302",11,"C3.2.1.1(b)\nPS.C3.2.3.2\nPS.C2.1","m3","(b) Exceeding 1,5 m and up to 3,0 m",10,null,{"$f":"H257*I257","v":0}]
[null,4,"0302",12,"C3.2.1.1(c )\nPS.C3.2.3.2\nPS.C2.1","m3","(c) Exceeding 3,0 m and up to 4,5 m",50,null,{"$f":"H258*I258","v":0}]
[null,4,"0302",13,"C3.2.1.4\nPS.C3.2.3.2\nPS.C2.1","m3","Extra over sub-item C3.2.1.1 for excavation in hard or boulder material, irrespective of depth",50,null,{"$f":"H259*I259","v":0}]
[{"$nulls":6},"Backfilling"]
[null,4,"0302",14,"C3.2.2.1\nPS.C3.2.3.2","m3","Backfilling: Using the excavated material",250,null,{"$f":"H261*I261","v":0}]
[null,4,"0302",15,"C3.2.2.2(a)\nPS.C3.2.3.2","m3","Backfilling: Using granular material",100,null,{"$f":"H262*I262","v":0}]
[null,4,"0302",16,"C3.2.8\nPS.C3.2.3.2","m3","Concrete backfill or encasement for culverts (Grade 20/26)",20,null,{"$f":"H263*I263","v":0}]
[null,4,"0302",17,"C3.2.12.1","m","Demolition of concrete members or elements: 0 mm - 450 mm diameter pipes for spoil",30,null,{"$f":"H264*I264","v":0}]
[null,4,"0302",18,"C3.2.12.1","m","Demolition of concrete members or elements: 575 mm - 900 mm diameter pipes for spoil",30,null,{"$f":"H265*I265","v":0}]
[{"$nulls":6},"Concrete Pipes: Spigot and Socket Type"]
[null,4,"0302",19,"C3.2.3.2\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class B bedding (375mm diameter concrete Class 100D)",20,null,{"$f":"H267*I267","v":0}]
[null,4,"0302",20,"C3.2.3.3\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class C bedding (375mm diameter concrete Class 100D)",20,null,0]
[null,4,"0302",21,"C3.2.3.2\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class B bedding (450mm diameter concrete Class 100D)",20,null,0]
[null,4,"0302",22,"C3.2.3.3\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class C bedding (450mm diameter concrete Class 100D)",20,null,0]
[null,4,"0302",23,"C3.2.3.2\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class B bedding (600mm diameter concrete Class 100D)",15,null,0]
[null,4,"0302",24,"C3.2.3.3\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class C bedding (600mm diameter concrete Class 100D)",15,null,0]
[null,4,"0302",25,"C3.2.3.2\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class B bedding (900mm diameter concrete Class 100D)",10,null,0]
[null,4,"0302",26,"C3.2.3.3\nPS.C3.2.3.2","m","Concrete pipe culverts: On Class C bedding (900mm diameter concrete Class 100D)",10,null,0]
[null,4,"0302",27,"C3.2.5.1","m","Prefabricated portal culverts; wall and roof combination (1500 x 1500 culvert)",10,null,0]
[null,4,"0302",28,"C3.2.5.2","m","Prefabricated floor slabs (for 1500 x 1500 culvert)",10,null,0]
[null,4,"0302",29,"C3.2.5.1","m","Prefabricated portal culverts; wall and roof combination (3000 x 3000 culvert)",10,null,0]
[null,4,"0302",30,"C3.2.5.2","m","Prefabricated floor slabs (for 3000 x 3000 culvert)",10,null,0]
[{"$nulls":6},"8KN/m2 HDPE Pipe"]
[null,4,"0302",31,"C2.2.1.1","m","Supply and lay 450mm HDPE (8KN/m2) pipe in restrictive conditions as directed by the Engineer",16,null,{"$f":"H280*I280","v":0}]
[null,4,"0302",32,"C2.2.1.1","no","Supply and install 450mm HDPE connector clamps in restrictive conditions",2,null,{"$f":"H281*I281","v":0}]
[null,4,"0302",33,"C2.2.4.4","m3","Clean coarse sand bedding",4,null,{"$f":"H282*I282","v":0}]
[{"$nulls":6},"Inlets with Heavy Duty Concrete Covers"]
[null,4,"0302",34,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S1; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",2,null,{"$f":"H284*I284","v":0}]
[null,4,"0302",35,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S1; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",2,null,0]
[null,4,"0302",36,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S2; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",5,null,0]
[null,4,"0302",37,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S2; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",5,null,0]
[null,4,"0302",38,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type D3; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",2,null,0]
[null,4,"0302",39,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type D3; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",2,null,0]
[{"$nulls":6},"Inlets with Heavy Duty Polymer Concrete Covers"]
[null,4,"0302",40,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S1; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",2,null,{"$f":"H291*I291","v":0}]
[null,4,"0302",41,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S1; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",2,null,0]
[null,4,"0302",42,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S2; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",5,null,0]
[null,4,"0302",43,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type S2; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",5,null,0]
[null,4,"0302",44,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type D3; Depth: Exceeding 0,0m and up to 1,5m, including brickwork for inlet walls",3,null,0]
[null,4,"0302",45,"C3.2.15.2\nPS.C3.2.15.3","no","Inlet: Type D3; Depth: Exceeding 1,5m and up to 2,0m, including brickwork for inlet walls",3,null,0]
[null,4,"0302",46,"C3.2.15.2\nPS.C3.2.15.2","no","Manhole: Type A (Dwg 38571), including brickwork for inlet walls",3,null,0]
[null,4,"0302",47,"C3.2.15.2\nPS.C3.2.15.2","no","Manhole: Type B (Dwg 38571), including brickwork for inlet walls",3,null,0]
[null,4,"0302",48,"C13.4.11","m3","Additional cast in situ concrete for blinding as directed by the Engineer (Grade 15/19)",5,null,0]
[{"$nulls":6},"Headwalls"]
[null,4,"0302",49,"PS.C3.2.15.2\nPS.C3.2.15.4","no","Headwalls, Type A, for 375mm and 450mm pipes",3,null,{"$f":"H301*I301","v":0}]
[null,4,"0302",50,"PS.C3.2.15.2\nPS.C3.2.15.4","no","Headwalls, Type B, for 375mm and 450mm pipes",1,null,{"$f":"H302*I302","v":0}]
[null,4,"0302",51,"PS.C3.2.15.2\nPS.C3.2.15.4","no","Headwalls, Type A, for 600mm and 900mm pipes",2,null,{"$f":"H303*I303","v":0}]
[null,4,"0302",52,"PS.C3.2.15.2\nPS.C3.2.15.4","no","Headwalls, Type B, for 600mm and 900mm pipes",1,null,{"$f":"H304*I304","v":0}]
[null,4,"0302",53,"C2.1.19.2","sum","Dealing with subsurface water",1,null,{"$f":"H305*I305","v":0}]
[null,4,"0303","C3.3 CONCRETE KERBING AND CHANNELING",{"$nulls":3},14,"Chapter Total:",{"$f":"SUM(J307:J322)","v":0}]
[null,4,"0303",1,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type A Barrier Kerb, with 300mm channel, Drawing 38577)",150,null,{"$f":"H307*I307","v":0}]
[null,4,"0303",2,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type A Barrier Kerb, with 300mm fillet, Drawing 38577)",150,null,0]
[null,4,"0303",3,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type C Mountable Kerb, with 300mm channel, Drawing 38577)",150,null,0]
[null,4,"0303",4,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type C Mountable Kerb, with 300mm fillet, Drawing 38577)",150,null,0]
[null,4,"0303",5,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type D Barrier Kerb, with 300mm channel, Drawing 38577)",150,null,0]
[null,4,"0303",6,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing, cast in-situ channeling (Type D Barrier Kerb, with 300mm fillet, Drawing 38577)",150,null,0]
[null,4,"0303",7,"C3.3.3.1\nPS.C3.3.2.1","m","Extra over item C3.3.1 for concrete kerbing and \nchanneling on curves of radii more than or equal to 2,0 m but less than 25 m",30,null,0]
[null,4,"0303",8,"C3.3.3.2\nPS.C3.3.2.1","m","Extra over items C3.3.1 for concrete kerbing and \nchanneling on curves with radii less than 2,0 m",10,null,0]
[null,4,"0303",9,"C3.3.4\nPS.C3.3.2.1","m","Drop kerbs and channel / Fillet at pedestrian crossings and driveways (Drawing 38579)",20,null,0]
[{"$nulls":6},"Sidewalk Edge Restraint"]
[null,4,"0303",10,"C3.3.2.1\nPS.C3.3.2.1","m","Prefabricated kerbing (edge restraint, Figure 12 kerb including 100mm x 100mm haunching)",500,null,{"$f":"H317*I317","v":0}]
[{"$nulls":6},"Sidewalk Edge Restraint"]
[null,4,"0303",11,"C13.4.11","m3","Cast in situ concrete for Pedestrian / Vehicular Scoop (Grade 20/13)",10,null,{"$f":"H319*I319","v":0}]
[null,4,"0303",12,"C13.4.11","m3","Additional cast in situ concrete for kerbs and channels as directed by the Engineer (Grade 20/13)",10,null,{"$f":"H320*I320","v":0}]
[null,4,"0303",13,"C3.3.8.1","m3","Linings for open drains: 600mm Cast in situ concrete v-drain, inclusive of formwork and reinforcing (class 20/13)",10,null,{"$f":"H321*I321","v":0}]
[null,4,"0303",14,"C2.1.16\nPS.C2.1.16","m","Subsurface drains in trench bottoms (Drawing 38575 - Type A)",100,null,{"$f":"H322*I322","v":0}]
[null,5,"EARTHWORKS",{"$nulls":5},"SECTION TOTAL:",{"$f":"J324+J334+J353","v":{"v":50000,"d":"R50,000.00"}}]
[null,5,"0402","C4.2 CUT MATERIALS",{"$nulls":3},8,"Chapter Total:",{"$f":"SUM(J325:J333)","v":{"v":50000,"d":"R50,000.00"}}]
[null,5,"0402",1,"C4.2.1.1","no","Compiling and implementing M&U plans for the cuttings exceeding 5 000 m3 up to 10 000 m3",1,null,{"$f":"H325*I325","v":0}]
[null,5,"0402",2,"C4.2.2.1","PC Sum","Cost of additional trial pits and/or drilling and laboratory testing",{"v":50000,"d":"50,000"},1,{"$f":"H326*I326","v":{"v":50000,"d":"R50,000.00"}}]
[null,5,"0402",3,"C4.2.2.2","%","Handling costs and profit in respect of item C4.2.2.1",{"v":50000,"d":"50,000"},null,{"$f":"H327*I327/100","v":0}]
[null,5,"0402",4,"C4.2.4.1\nPS.C4.2","m3","Excavating of materials in box cuts for use in the works, material obtained from: \nSoft excavation",500,null,{"$f":"H328*I328","v":0}]
[null,5,"0402",5,"C4.2.9.1\nPS.C4.3","m3","Excavate material to spoil in sites designated by the Contractor, material obtained from:\nSoft excavation, overburden and unsuitable material",500,null,0]
[null,5,"0402",6,"C4.2.9.3","m3","Boulder excavation class B",50,null,0]
[null,5,"0402",7,"C4.2.9.4","m3","Hard excavation (other than by blasting)",50,null,0]
[null,5,"0402",8,"C4.2.12.1(a)","m2","Finishing the side slopes of Cuttings:\n(a) In soft material",{"v":2000,"d":"2,000"},null,0]
[null,5,"0402",9,"C4.2.12.1(c )","m2","(c) In hard material",50,null,0]
[null,5,"0403","C4.3 EXISTING ROAD MATERIALS",{"$nulls":3},17,"Chapter Total:",{"$f":"SUM(J335:J352)","v":0}]
[{"$nulls":6},"Saw-cut"]
[null,5,"0403",1,"C4.3.4.1(a)","m","Saw-cutting existing materials within the following average depth ranges:\nAsphalt:\n(a) Up to 50 mm",20,null,{"$f":"H336*I336","v":0}]
[null,5,"0403",2,"C4.3.4.1(b)","m","(b) Exceeding 50 mm and up to 100 mm",10,null,0]
[null,5,"0403",3,"C4.3.9.2\nPS.C4.3","m3","Excavating material by using conventional road construction equipment to stockpile: Crushed stone and macadam materials",{"v":2000,"d":"2,000"},null,0]
[null,5,"0403",4,"C4.3.9.4\nPS.C4.3","m3","Excavating material by using conventional road construction equipment to stockpile: Natural gravel and sand materials",{"v":2000,"d":"2,000"},null,0]
[null,5,"0403",5,"C4.3.18.1\nPS.C4.4","m3","Excavate non-compliant or excess pavement layer material to spoil in sites designated by the Contractor, material consisting of: Asphalt material",{"v":2000,"d":"2,000"},null,0]
[null,5,"0403",6,"C4.3.18.2\nPS.C4.3","m3","Excavate non-compliant or excess pavement layer material to spoil in sites designated by the Contractor, material consisting of: Crushed stone, macadam, gravel and sand material",{"v":1000,"d":"1,000"},null,0]
[null,5,"0403",7,"C4.3.18.4\nPS.C4.4","m3","Excavate non-compliant or excess pavement layer material to spoil in sites designated by the Contractor, material consisting of: Concrete material",20,null,0]
[null,5,"0403",8,"C4.3.14.1(a)(iii)","m3","Removing of existing road edging using construction equipment:\n(a) Kerbing and edge beams:\n(iii) Precast concrete kerbing and situ concrete channel",30,null,0]
[null,5,"0403",9,"C4.3.14.1(b)","m3","Removing of existing road edging using construction equipment:\n(b) Kerb inlets",10,null,0]
[null,5,"0403",10,"C4.3.15.4","m3","Stockpiling of road layer materials",{"v":4000,"d":"4,000"},null,0]
[null,5,"0403",11,"C4.3.5.2","no","Providing large milling machine with a cutting width exceeding 1,2 m",1,null,0]
[null,5,"0403",12,"C4.3.7.1","m3","Milling and removal of existing asphalt layers with an average milling depth \n(Employer takes ownership): Not exceeding 50mm",175,null,0]
[null,5,"0403",13,"PS.C4.3.5.3","no","Providing a mobile cold asphalt recylcing plant",1,null,0]
[null,5,"0403",14,"C5.4.5.1(a)","t","Addition of stabilisation agents for pavement layers - Cement",10,null,0]
[null,5,"0403",15,"C5.4.5.1(b)","t","Addition of stabilisation agents for pavement layers - lime",10,null,0]
[null,5,"0403",16,"C5.4.8.3","l","Addition of stabilisation agents for pavement layers - Foamed bitumen (70/100)",100,null,0]
[null,5,"0403",17,"PS.C4.3.5.3","m3","Stabilisation of pavement layers using mobile cold asphalt recylcing plant and laid with paver",175,null,0]
[null,5,"0404","C4.4 COMMERCIAL MATERIALS",{"$nulls":3},5,"Chapter Total:",{"$f":"SUM(J354:J358)","v":0}]
[null,5,"0404",1,"C4.4.2.1(d )","m3","Commercial materials identified by the Contractor from commercial, private or other non-commercial suppliers:\nPavement layer material:Type G2",{"v":1050,"d":"1,050"},null,{"$f":"H354*I354","v":0}]
[null,5,"0404",2,"C4.4.2.1(d )","m3","Commercial materials identified by the Contractor from commercial, private or other non-commercial suppliers:\nPavement layer material:Type G4",{"v":1050,"d":"1,050"},null,{"$f":"H355*I355","v":0}]
[null,5,"0404",3,"C4.4.2.1(e )","m3","Commercial materials identified by the Contractor from commercial, private or other non-commercial suppliers: \nPavement layer material:Type G5",{"v":1100,"d":"1,100"},null,{"$f":"H356*I356","v":0}]
[null,5,"0404",4,"C4.4.2.1(g )","m3","Commercial materials identified by the Contractor from commercial, private or other non-commercial suppliers:\nPavement layer material:Type G7",{"v":1150,"d":"1,150"},null,{"$f":"H357*I357","v":0}]
[null,5,"0404",5,"C4.4.4.1\nPS.C4.4.4.1","t","Cementitious stabilising agents: Cement",60,null,{"$f":"H358*I358","v":0}]
[null,6,"LAYERWORKS",{"$nulls":5},"SECTION TOTAL:",{"$f":"J360+J371+J379+J392+J398","v":0}]
[null,6,"0501","C5.1 ROADBED",{"$nulls":3},9,"Chapter Total:",{"$f":"SUM(J361:J370)","v":0}]
[null,6,"0501",1,"C5.1.1.2\nPS.C5.1.1.2","m3","Roadbed construction and compaction to 95 % of MDD",{"v":1050,"d":"1,050"},null,{"$f":"H361*I361","v":0}]
[null,6,"0501",2,"C5.1.3.1(a)\nPS.C4.2","m3","Excavate material to spoil from roadbed construction, material obtained from:\n(a) Soft excavation",35,null,0]
[null,6,"0501",3,"C5.1.3.1(c )\nPS.C4.2","m3","(c) Boulder excavation Class B",10,null,0]
[null,6,"0501",4,"C5.1.3.1(d)\nPS.C4.2","m3","(d) Hard excavation",5,null,0]
[null,6,"0501",5,"C5.1.4.1","m3","In-place treatment of roadbed in hard material: by ripping",30,null,0]
[null,6,"0501",6,"C5.1.5.2","m2","Roller passes compaction: Pad foot vibratory rollers",600,null,0]
[null,6,"0501",7,"C5.1.5.3","m2","Roller passes compaction: Smooth drum vibratory rollers",600,null,0]
[{"$nulls":6},"Subgrade Improvement"]
[null,6,"0501",8,"C12.3.20\nPS.C.12.3.21","m3","Importing dump rock for subgrade improvement, 300mm thick",50,null,{"$f":"H369*I369","v":0}]
[null,6,"0501",9,"PS.C12.3.22","m2","Supply and place general grade geofabric, A5 or similar approved.",200,null,{"$f":"H370*I370","v":0}]
[null,6,"0502","C5.2 FILL",{"$nulls":3},7,"Chapter Total:",{"$f":"SUM(J372:J378)","v":0}]
[null,6,"0502",1,"C5.2.1.1","no","Compiling and implementing M&U plans: For fills more than 5000 m3",1,null,{"$f":"H372*I372","v":0}]
[null,6,"0502",2,"C5.2.2.1(a)","m3","Fill construction: Normal fill material in compacted layer thicknesses of 200 mm and less:\n(a) Compacted to 90 % of MDD",500,null,0]
[null,6,"0502",3,"C5.2.2.1(b)","m3","(b) Compacted to 93 % of MDD",500,null,0]
[null,6,"0502",4,"C5.2.3","m3","Side-cut to fill compacted to 93 % of MDD in compacted layer thicknesses of 200 mm and less",500,null,0]
[null,6,"0502",5,"C5.2.9.1","m2","Finishing-off fill slopes",{"v":6000,"d":"6,000"},null,0]
[null,6,"0502",6,"C5.2.2.1(a)","m3","Fill construction from stockpile: Haul fill material from stockpile and place in compacted layer thicknesses of 200 mm and less:\n(a) Compacted to 90 % of MDD",{"v":4000,"d":"4,000"},null,0]
[null,6,"0502",7,"C5.2.2.1(b)","m3","(b) Compacted to 93 % of MDD",{"v":4000,"d":"4,000"},null,0]
[null,6,"0503","C5.3 ROAD PAVEMENT LAYERS",{"$nulls":3},10,"Chapter Total:",{"$f":"SUM(J380:J391)","v":0}]
[null,6,"0503",1,"C5.3.1","no","Compiling and implementing M&U plans for the construction of all the pavement layers.",1,null,{"$f":"H380*I380","v":0}]
[null,6,"0503",2,"C5.3.2.1(h)","m3","150mm Upper subbase (C3) layer compacted to 95 % of MDD",{"v":1050,"d":"1,050"},null,{"$f":"H381*I381","v":0}]
[null,6,"0503",3,"C5.3.2.1(b)","m3","150mm Selected layer (G2) compacted to 98 % of MDD",{"v":1050,"d":"1,050"},null,{"$f":"H382*I382","v":0}]
[null,6,"0503",4,"C5.3.2.1(b)","m3","150mm Selected layer (G5) compacted to 98 % of MDD",{"v":1100,"d":"1,100"},null,{"$f":"H383*I383","v":0}]
[null,6,"0503",5,"C5.3.2.1(b)","m3","150mm Selected layer (G7) compacted to 95 % of MDD",{"v":1150,"d":"1,150"},null,{"$f":"H384*I384","v":0}]
[{"$nulls":6},"Riding Quality Measurements"]
[null,6,"0503",6,"C5.3.11.1","m","Using a 3,0 m straight edge",50,null,{"$f":"H386*I386","v":0}]
[null,6,"0503",7,"C5.3.11.2","m","Using a rolling straight edge",50,null,{"$f":"H387*I387","v":0}]
[null,6,"0503",8,"C5.3.11.3","m","Using an inertial profilometer",50,null,{"$f":"H388*I388","v":0}]
[{"$nulls":6},"Sidewalk"]
[null,6,"0503",9,"C5.3.2.1(b)","m3","Sidewalk selected layer (G5) compacted to 98 % of MDD",150,null,{"$f":"H390*I390","v":0}]
[null,6,"0503",10,"C5.3.2.1(b)","m3","Selected layer (G2) compacted to 98 % of MDD for driveways and restricted areas",10,null,{"$f":"H391*I391","v":0}]
[null,6,"0504","C5.4 STABILISATION",{"$nulls":3},5,"Chapter Total:",{"$f":"SUM(J393:J397)","v":0}]
[null,6,"0504",1,"C5.4.1.1","m3","Pre-treatment of (G4) gravel layer",{"v":1050,"d":"1,050"},null,{"$f":"H393*I393","v":0}]
[null,6,"0504",2,"C5.4.5.1(a)","t","Addition of cementitious soil stabilisation agents for pavement layers:\n(a) Cement (for pavement layer)",60,null,{"$f":"H394*I394","v":0}]
[null,6,"0504",3,"C5.4.2.1","m3","Cementitious stabilisation (150mm layers) of pavement layers (to C3 quality)",{"v":1050,"d":"1,050"},null,{"$f":"H395*I395","v":0}]
[null,6,"0504",4,"C5.4.10","kl","Provision and application of water for curing",50,null,{"$f":"H396*I396","v":0}]
[null,6,"0504",5,"C5.4.14","m2","Trial section for a cementitiously stabilised layer (3.5m wide)",70,null,{"$f":"H397*I397","v":0}]
[null,6,"0901","C9.1 ASPHALT LAYERS",{"$nulls":3},14,"Chapter Total:",{"$f":"SUM(J399:J417)","v":0}]
[{"$nulls":6},"Asphalt Mix Designs"]
[null,6,"0901",1,"C9.1.1.2(a)\nPS.C9.1","Lump sum","Sand skeletal mixes: Continuously graded base or surfacing (SA-S14).",1,null,{"$f":"H400*I400","v":0}]
[null,6,"0901",2,"C9.1.1.2(a)\nPS.C9.1","Lump sum","Sand skeletal mixes: Continuously graded base or surfacing (SA-S10).",1,null,{"$f":"H401*I401","v":0}]
[{"$nulls":6},"Bond Coat",null,null,{"$f":"H402*I402","v":0}]
[null,6,"0901",3,"C9.1.3.1\nPS.C9.1","m2","Stable–grade 30 % net bitumen emulsion as specified. Applied with a calibrated distributer",{"v":5000,"d":"5,000"},null,{"$f":"H403*I403","v":0}]
[null,6,"0901",4,"C9.1.3.2\nPS.C9.1","m2","Applied in restricted areas using a portable pressure sprayer",{"v":2000,"d":"2,000"},null,{"$f":"H404*I404","v":0}]
[{"$nulls":6},"Asphalt Surface"]
[null,6,"0901",5,"C9.1.5.1(a)\nPS.C9.1\nC3.4.3","m2","New construction (paver laid)\n(a) Stone skeletal mix – continuously graded (SA-S14) as defined (45mm layer)",{"v":3000,"d":"3,000"},null,{"$f":"H406*I406","v":0}]
[null,6,"0901",6,"C9.1.5.1(a)\nPS.C9.1\nC3.4.3","m2","New construction (hand laid)\n(a) Stone skeletal mix – continuously graded (SA-S14) as defined (45mm layer)",{"v":1000,"d":"1,000"},null,{"$f":"H407*I407","v":0}]
[null,6,"0901",7,"C9.1.5.1(a)\nPS.C9.1\nC3.4.3","m2","New construction (paver laid)\n(a) Stone skeletal mix – continuously graded (SA-S10) as defined (30mm layer)",{"v":3000,"d":"3,000"},null,{"$f":"H408*I408","v":0}]
[null,6,"0901",8,"C9.1.5.1(a)\nPS.C9.1\nC3.4.3","m2","New construction (hand laid)\n(a) Stone skeletal mix – continuously graded (SA-S10) as defined (30mm layer)",{"v":1000,"d":"1,000"},null,{"$f":"H409*I409","v":0}]
[null,6,"0901",9,"C9.1.12","m2","Asphalt reinforcing - complete (Glassgrid GG100 or similar)",500,null,{"$f":"H410*I410","v":0}]
[{"$nulls":6},"Coring of Asphalt Layers"]
[null,6,"0901",10,"C9.1.13.1","no","100 mm diameter",20,null,{"$f":"H412*I412","v":0}]
[null,6,"0901",11,"C9.1.13.2","no","150 mm diameter",10,null,{"$f":"H413*I413","v":0}]
[null,6,"0901",12,"C8.1.1.2","m2","Prime coat: MC -30 cut-back bitumen",{"v":5000,"d":"5,000"},null,{"$f":"H414*I414","v":0}]
[null,6,"0901",13,"C8.1.3","m2","Extra over item C8.1.1 for applying the prime coat accessible only to hand-held or light equipment",{"v":2000,"d":"2,000"},null,{"$f":"H415*I415","v":0}]
[{"$nulls":6},"Sidewalk"]
[null,6,"0901",14,"C9.1.2.1\nPS.C9.1\nC3.4.3","m2","Asphalt layers (SA-S10, 30mm layers)",{"v":1500,"d":"1,500"},null,{"$f":"H417*I417","v":0}]
[null,7,"ANCILLARY ROAD WORKS",{"$nulls":5},"SECTION TOTAL:",{"$f":"J419+J429+J436+J447+J461+J469+J479","v":{"v":250000,"d":"R250,000.00"}}]
[null,7,"1104","C11.4 ROAD RESTRAINT SYSTEMS",{"$nulls":3},9,"Chapter Total:",{"$f":"SUM(J420:J428)","v":0}]
[null,7,"1104",1,"C11.4.1.1(b)\nPS.C11.4.5.2","m","Erecting of guardrails at 3,81 m spacing:\nComplete galvanized system compliant to SANS 1350:\n(b) on CONCRETE post(Drawing 38580)",200,null,{"$f":"H420*I420","v":0}]
[null,7,"1104",2,"C11.4.1.1(b)\nPS.C11.4.5.2","no","Supply and install concrete posts (Drawing 38580)",15,null,0]
[null,7,"1104",3,"C11.4.1.2(a)\nPS.C11.4.5.2","no","Terminal sections for 3,81 guardrails comprising of:\n(a) End wings to SANS 1350",5,null,0]
[null,7,"1104",4,"C11.4.6.2\nPS.C11.4.5.2","no","Reflective \nPlastic plates",200,null,0]
[null,7,"1104",5,"C11.4.11.5\nPS.C11.4.5.2","no","Spacer blocks compliant to SANS 1350",15,null,0]
[null,7,"1104",6,"C11.4.11.7\nPS.C11.4.5.2","no","Post bolt complete with nut and washer compliant to SANS 1350",30,null,0]
[null,7,"1104",7,"C11.4.4.1\nPS.C11.4.5.2","m","Extra over C11.4.1 and C11.4.11 for horizontally curved guard rails factory bent to a radius of less than 45m",5,null,0]
[null,7,"1104",8,"C11.4.7","m","Removing existing guardrails, including posts, and backfilling holes",10,null,0]
[null,7,"1104",9,"C11.4.9.1\nPS.C11.4.5.2","m","Re-erection of guardrails with recovered or provided material:\nSingle guardrail",10,null,0]
[null,7,"1105","C11.5 FENCING",{"$nulls":3},5,"Chapter Total:",{"$f":"SUM(J430:J435)","v":0}]
[{"$nulls":6},"Wire Mesh Fence - Drawing 38583"]
[null,7,"1105",1,"C11.5.1.3","m2","Diamond mesh",20,null,{"$f":"H431*I431","v":0}]
[null,7,"1105",2,"C11.5.1.9(a)(i)","no","Straining posts, stays and anchors:\n(a) Vertical (Concrete straining post)",10,null,{"$f":"H432*I432","v":0}]
[null,7,"1105",3,"C11.5.1.9(a)(i)","no","Straining posts, stays and anchors:\n(a) Inclined post (Concrete straining post) (Drawing 38583)",5,null,{"$f":"H433*I433","v":0}]
[null,7,"1105",4,"C11.5.4.1(a)","m","Dismantling existing fences:\n(a) Stock-proof fences",20,null,{"$f":"H434*I434","v":0}]
[null,7,"1105",5,"C11.5.5.1","m","Providing temporary fences and gates:\nStock-proof fence",20,null,{"$f":"H435*I435","v":0}]
[null,7,"1106","C11.6 ROAD SIGNS",{"$nulls":3},10,"Chapter Total:",{"$f":"SUM(J437:J446)","v":0}]
[null,7,"1106",1,"C11.6.1.3(a)","m2","Road signboards with painted or coloured semi-matt background. Symbols, lettering and borders in semi- matt black or in Class I retro-reflective material, where the sign board is constructed from:\nPrepainted galvanized steel plate:\n(a) Area 0 to 0,5 m2",5,null,{"$f":"H437*I437","v":0}]
[null,7,"1106",2,"C11.6.1.3(b)","m2","(b) Area exceeding 0,5 m2 but not 2,0 m2",5,null,0]
[null,7,"1106",3,"C11.6.3.2","m","Road sign supports (overhead road sign structures excluded):Timber (100mm diameter)",5,null,0]
[null,7,"1106",4,"C11.6.5.1","m3","Excavation and backfilling for road sign supports (not applicable to kilometre posts):\nExcavating soft material and backfilling",2,null,0]
[null,7,"1106",5,"C11.6.5.4","m3","Extra over item C11.6.5.1 for hard material excavation",1,null,0]
[null,7,"1106",6,"C13.4.11","m3","Cast in situ concrete for road sign footings as directed by the Engineer (Grade 20/19)",1,null,0]
[null,7,"1106",7,"C11.6.7.1(a)","m2","Dismantling and storing of road signs with a surface area of:\n(a) Area 0 to 0,5 m2",5,null,0]
[null,7,"1106",8,"C11.6.7.1(b)","m2","(b) Area exceeding 0,5 m2 but not 2,0 m2",5,null,0]
[null,7,"1106",9,"C11.6.10.1","m2","Disposing of road signs with a surface area of:\nArea 0 to 0,5 m2",5,null,0]
[null,7,"1106",10,"C11.6.10.2","m2","Area exceeding 0,5 m2 but not 2,0 m2",5,null,0]
[null,7,"1107","C11.7 ROAD MARKINGS AND ROAD STUDS",{"$nulls":3},9,"Chapter Total:",{"$f":"SUM(J448:J460)","v":0}]
[{"$nulls":6},"Lettering and Symbols"]
[null,7,"1107",1,"C11.7.1.4","m2","White lettering and symbols (Thermoplastic)",5,null,{"$f":"H449*I449","v":0}]
[{"$nulls":6},"Transverse Lines and Islands"]
[null,7,"1107",2,"C11.7.1.7","m2","Transverse lines, painted island and arrestor bed markings (White) (Thermoplastic)",50,null,{"$f":"H451*I451","v":0}]
[{"$nulls":6},"Broken and Unbroken Lines"]
[null,7,"1107",3,"C11.7.3.1","m","Thermoplastic road marking, broken or unbroken (White, 100mm wide)",{"v":2000,"d":"2,000"},null,{"$f":"H453*I453","v":0}]
[null,7,"1107",4,"C11.7.3.1","m","Thermoplastic road marking, broken or unbroken (Yellow, 100mm wide)",250,null,{"$f":"H454*I454","v":0}]
[{"$nulls":6},"Road Studs"]
[null,7,"1107",5,"C11.7.7.1","no","Permanent road studs compliant to SANS 1442 (Tempered glass 360 degree, Clear Holophane or similar approved)",20,null,{"$f":"H456*I456","v":0}]
[null,7,"1107",6,"C11.7.7.1","no","Permanent road studs compliant to SANS 1442 (Tempered glass 360 degree, two colour, Clear & Yellow Holophane or similar approved)",10,null,{"$f":"H457*I457","v":0}]
[null,7,"1107",7,"C11.7.7.1","no","Permanent road studs compliant to SANS 1442 (Tempered glass 360 degree, two colour, Clear & Red Holophane or similar approved)",10,null,{"$f":"H458*I458","v":0}]
[null,7,"1107",8,"C11.7.7.3","no","Temporary road studs compliant to SANS 1442 or 1463 (red or yellow)",200,null,{"$f":"H459*I459","v":0}]
[null,7,"1107",9,"C11.7.8","m","Setting out and premarking the lines",100,null,{"$f":"H460*I460","v":0}]
[null,7,"1108","C11.8 LANDSCAPING AND PLANTING PLANTS",{"$nulls":3},7,"Chapter Total:",{"$f":"SUM(J462:J468)","v":0}]
[null,7,"1108",1,"C11.8.1.1","m2","Machine trimming",200,null,{"$f":"H462*I462","v":0}]
[null,7,"1108",2,"C11.8.3.3(a)","m3","(a) Topsoil obtained from within the road reserve or borrow areas",5,null,0]
[null,7,"1108",3,"C11.8.3.3(b)","m3","(b) Topsoil obtained from commercial sources by the Contractor",5,null,0]
[null,7,"1108",4,"C11.8.4.2(a)","m2","Sodding by using the following types of sods:\n(a) Nursery sod",200,null,0]
[null,7,"1108",5,"C11.8.6","kl","Watering the already planted grass, trees and shrubs during the growing season",2,null,0]
[null,7,"1108",6,"C11.8.7","m2","Mowing the grass",200,null,0]
[null,7,"1108",7,"C11.8.10","ProvSum","Unspecified work for landscaping",1,null,0]
[null,7,"1109","C11.9 FINISHING  ROAD AND ROAD RESERVE",{"$nulls":3},7,"Chapter Total:",{"$f":"SUM(J470:J478)","v":{"v":250000,"d":"R250,000.00"}}]
[null,7,"1109",1,"C11.9.1.1","m","Finishing the road and road reserve: Single carriageway road",50,null,{"$f":"H470*I470","v":0}]
[null,7,"1109",2,"C11.9.1.1","m","Finishing the road and road reserve: \nDual carriageway road",50,null,{"$f":"H471*I471","v":0}]
[null,7,"1109",3,null,"PC Sum","Traffic Signals",{"v":200000,"d":"200,000"},1,{"$f":"H472*I472","v":{"v":200000,"d":"R200,000.00"}}]
[null,7,"1109",4,null,"%","Handling costs and profit in respect of item 3",{"v":200000,"d":"200,000"},null,{"$f":"H473*I473/100","v":0}]
[null,7,"1109",5,"PS.6","PC Sum","Street lighting",{"v":50000,"d":"50,000"},1,{"$f":"H474*I474","v":{"v":50000,"d":"R50,000.00"}}]
[null,7,"1109",6,"PS.6","%","Handling costs and profit in respect of item 5",{"v":50000,"d":"50,000"},null,{"$f":"H475*I475/100","v":0}]
[null,7,"1109",7,null,"no","Supply and lay precast concrete steps (1m wide, 40Mpa)",50,null,{"$f":"H476*I476","v":0}]
[null,7,"1109",8,null,"no","Supply and lay polymer concrete stanchions (at least 1m high)",600,null,{"$f":"H477*I477","v":0}]
[null,7,"1109",9,null,"m","Supply and lay polymer concrete handrails (to fit on polymer concrete posts)",50,null,{"$f":"H478*I478","v":0}]
[null,7,"1206","C12.6 MECH STABILISED FILL AND GABIONS",{"$nulls":3},16,"Chapter Total:",{"$f":"SUM(J480:J497)","v":0}]
[{"$nulls":6},"Gabions"]
[null,7,"1206",1,"C12.6.14.1(a)","m3","Foundation trench excavation: Excavating all material situated within the following depth ranges below the surface level\n(a) 0 m to 1,5 m",15,null,{"$f":"H481*I481","v":0}]
[null,7,"1206",2,"C12.6.15","m2","Surface preparation for bedding the gabions",50,null,0]
[null,7,"1206",3,"C12.6.3","m3","Concrete for wall base foundation (Grade 20/26)",15,null,0]
[null,7,"1206",4,"C12.6.4.1","t","Reinforcing steel in wall base foundation: Mild steel",3,null,0]
[null,7,"1206",5,"C12.6.16.1","m3","Gabions and mattresses: Galvanized gabion boxes (0.3m x 1m)",5,null,0]
[null,7,"1206",6,"C12.6.16.1","m3","Gabions and mattresses: Galvanized gabion boxes (1m x 1m)",100,null,0]
[null,7,"1206",7,"C12.6.17","m2","Geotextile (filtration and separation grade)",300,null,0]
[null,7,"1206",8,"C12.6.11","m3","Backfill (using material from excavation)",100,null,0]
[{"$nulls":6},"Dry Stacking Wall"]
[null,7,"1206",9,"C12.6.14.1(a)","m3","Foundation trench excavation: Excavating all material situated within the following depth ranges below the surface level\n(a) 0 m to 1,5 m",25,null,{"$f":"H490*I490","v":0}]
[null,7,"1206",10,"C12.6.3","m3","Concrete for wall base foundation (Grade 20/26)",25,null,0]
[null,7,"1206",11,"C12.6.4.1","m2","Reinforcing steel in wall base foundation: Mesh ref 245",45,null,0]
[null,7,"1206",12,"C12.6.11","m2","Supply and lay L500 or similar approved",50,null,0]
[null,7,"1206",13,"C12.6.11","m3","Backfill (using material from excavation) to 95% MOD AASHTO",25,null,0]
[null,7,"1206",14,"C12.6.11","m3","Stabilised backfill (12:1 Clean Coarse Sand and Cement)",10,null,0]
[null,7,"1206",15,"C12.6.3","m3","Mass concrete for top row of blocks",10,null,0]
[null,7,"1206",16,null,"m","Weepholes 50mm dia at 5m c/c",10,null,0]