{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Machine requirements OHTE "],"read":"whole","date_system":"1900"}

{"sheet":"Machine requirements OHTE ","index":0,"n_rows":229,"n_cols":34,"rows_kept":229,"merged":[[1,3,1,4],[7,3,7,4],[13,3,13,4],[24,3,24,4],[27,3,27,4],[59,3,59,4],[61,3,61,4],[80,3,80,4],[108,3,108,4],[112,3,112,4],[127,3,127,4],[135,3,135,4],[167,3,167,4],[175,3,175,4],[186,3,186,4],[200,3,200,4],[210,3,210,4],[216,3,216,4]]}
["No.","Group",null,"Transnet Item Numbers","Item Description","Estimated QTY","Drawing/Specification","Factory/Machinery/Manufacturing Required",{"$nulls":25},"Machinery available?"]
[null,null,"#","Group A"]
[1,"Group A",1,54033494,"SPLICE, CONDUCTOR; TYPE: TENSION, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3593BBB 3591BBB 3597; EQUIPMENT USED ON OHTE; SUITABLE FOR 800 MM SQ ACSR TO 800 MM SQ AAC WIRE.(CODE NAME LAPWING TO BULL)",3200,"BBB 3593\nBBB 3591\nBBB 3597","1) Press machine\n2) Lathe/CNC machine\n\n"]
[2,"Group A",2,54033469,"SPLICE, CONDUCTOR; TYPE: TENSION SPLICE, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3594BBB 3593BBB 3592; SUITABLE FOR 500 MM SQ ACSR TO 500 MM SQ ACSR WIRE (CODE NAME DEER TO DEER)",3200,"BBB 3594\nBBB 3593\nBBB 3592","1) Press machine\n2) Lathe/CNC machine\n\n"]
[3,"Group A",3,54033470,"SPLICE, CONDUCTOR; TYPE: TENSION, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3593, LA; BBB 3592, LA; BBB 3595, LA; EQUIPMENT USED ON OHTE; SUITABLE FOR 800 MM SQ ACSR TO 800 MM SQ ACSR WIRE (CODE NAME LAPWING TO LAPWING)",3200,"BBB 3593\nBBB 3592\nBBB 3595","1) Press machine\n2) Lathe/CNC machine\n\n"]
[4,"Group A",4,54033445,"ATTACHMENT; TYPE: DEAD END, APPLICATION: FEEDER TERMINATION; DRAWING NO: BBB 3590, LA; BBB 3589, LA; BBB 3596, LA; EQUIPMENT USED ON OHTE SUITABLE FOR 500 MM2 FEEDER WIRE",800,"BBB 3590\nBBB 3589\nBBB 3596","1) Aluminium welder\n2) Lathe\n3) Cutting machine \n4. Stamping/drilling machine"]
[5,"Group A",5,54000944,"SPLICE, CONDUCTOR; TYPE: FEEDER, MATERIAL: ALUMINIUM; DRAWING NO: CEE-TNB-0024; SPECIFICATION: CEE.0038/83; SUITABLE FOR 500MM2 FEEDER WIRE ",3200,"CEE-TNB-0024\nCEE.0038/83","1) Press machine\n2) Lathe/CNC machine\n\n"]
[{"$nulls":3},"Group B"]
[1,"Group B",1,54016913,"SPLICE, CONDUCTOR; EQUIPMENT USED ON OHTE; PREFORMED SPIRAL; FOR JOINING 50 MM SQ ALUMINIUM WIRE ACSR 6/1/3,35 STRANDING RABBIT",800,"As per description","1) Spiral Binding Machine\n2) Cutting machine"]
[2,"Group B",2,54009096,"SPLICE, CONDUCTOR; TYPE: PREFORMED; EQUIPMENT USED ON OHTE; FULL TENSION SPLICE SUITABLE FOR USE ON CONDUCTOR WITH 30/7/2,36 STRANDING ACSR WIRE (TIGER WIRE) DIA 16.52 MM.",9600,"As per description","1) Spiral Binding Machine\n2) Cutting machine"]
[3,"Group B",3,54005531,"SPLICE, CONDUCTOR;  EQUIPMENT USED ON 5405802; PREFORMED SPIRAL; FOR JOINING 160 SQ MM ALUMINIUM WIRE 19/3,25 MM STRANDING (HORNET)",800,"As per description","1) Spiral Binding Machine\n2) Cutting machine"]
[4,"Group B",4,54000207,"GRIP; TYPE: PREFORMED DEAD END, MATERIAL: ALUMINIUM WIRE; DRAWING NO: SSE-208228, LA; 8MM; OVERHEAD TRACK; ITEM USED ON THE SALDANHA LINE",240,"SSE-208228\nH500110-3-133-E-DE-0091","1) Spiral Binding Machine\n2) Cutting machine"]
[5,"Group B",5,54010799,"GRIP; TYPE: PREFORMED DEAD END; SUITABLE FOR USE ON 131,23/30,62/160 SQ MM TIGER 30/7/2,36 STRANDING ACSR WIRE DIA 16,52 MM.",240,"As per description","1) Spiral Binding Machine\n2) Cutting machine"]
[{"$nulls":3},"Group C"]
[1,"Group C",1,54112448,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 100 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[2,"Group C",2,54112449,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 120 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[3,"Group C",3,54112450,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 150 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[4,"Group C",4,54112451,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 160 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[5,"Group C",5,54112445,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 50 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[6,"Group C",6,54112446,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 70 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",3200,"CEE-TU-0136","1) Stamping machine.\n"]
[7,"Group C",7,54005607,"TERMINAL, LUG; TYPE: COMPRESSION, WIRE SIZE ACCOMMODATED: 160 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM, ATTACHMENT METHOD: CRIMPING; DRAWING NO: CEE-TZ1-0121 SHEET 37, LA",3200,"CEE-TZ1-0121 SHEET 37","1) Stamping machine.\n"]
[8,"Group C",8,54017109,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 95 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA",24000,"CEE-TU-0136","1) Stamping machine.\n"]
[9,"Group C",9,54031697,"TERMINAL, LUG; TYPE: CRIMPING, WIRE SIZE ACCOMMODATED: 95 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: TINNED COPPER, SPECIAL FEATURES: M16 STUD; DRAWING NO: BBH 1332 SHEET 1, LA",3200,"BBH 1332 SHEET 1","1) Stamping machine.\n2) Facilities for copper tinning."]
[10,"Group C",10,54017122,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 150 MM2, HOLE QUANTITY: 1; DRAWING NO: CEE-TU-0136, LA; EQUIPMENT USED ON OHTE",3200,"CEE-TU-0136","a) Stamping machine.\n"]
[{"$nulls":3},"Group D"]
[1,"Group D",1,54001076,"INSULATOR ASSEMBLY; TYPE: SUSPENSION, INSULATOR MATERIAL: PORCELAIN; DRAWING NO: CEE-TNC-0018, LA",7200,"CEE-TNC-0018","1)Clay mixer and grinder\n2) Machine to shape insulator\n3) Temperature controle industrial oven\n4) Glasing facilities."]
[2,"Group D",2,54016901,"GREASE; TYPE: ELECTRICAL JOINTING COMPOUND, TRADE NAME: OXIDATION INHIBITION; TO BE SUPPLIED IN 1 KG TINS. BIDDERS ARE REQUIRED TO SUBMIT A TECHNICAL DATASHEET OF THE COMPOUND. ITEM USED ON ALUMINIUM CONDUCTORS FOR OXIDATION INHIBITION.",80,"As per description","1. Chemical composition laboratory"]
[{"$nulls":3},"Group E"]
[1,"Group E",1,54017021,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: 11 TO 13 MM WIRE; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121 DATE 2000 , LA; ITEM USED ON OHTE",16000,"BBH 1889","1. Forging Machine"]
[2,"Group E",2,54001201,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 16 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA",16000,"BBH 1889","1. Forging Machine"]
[3,"Group E",3,54032590,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 22 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA",16000,"BBH 1889","1. Forging Machine"]
[4,"Group E",4,54003859,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 11 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121",16000,"BBH 1889","1. Forging Machine"]
[5,"Group E",5,54003872,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 16 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA; WIRE SIZE ACCOMODATED DIA 19 MM",16000,"BBH 1889","1. Forging Machine"]
[6,"Group E",6,54006363,"SHACKLE; SHACKLE MATERIAL: STAINLESS STEEL, MATERIAL GRADE: 316; DRAWING NO:  H500110-3-133-E-DE-0046,SSE-208 211 ; OHTE CATENARY SYSTEM",480,"H500110-3-133-E-DE-0046,\nSSE-208 211","1. Bending machine\n2. Cutting machine"]
[7,"Group E",7,54009780,"ADAPTOR, INSULATOR; TYPE: STEADY ARM, DIMENSIONS: OD 42 MM, APPLICATION: OVERHEAD TRACK EQUIPMENT;  DRAWING NO: CEE-TZ-9/27, 0; HOLDER, STEADY ARM EYE; TUBE DIAMETER 2 BOLT TYPE",320,"CEE-TZ9-0027","1. Drilling Machine \n2. Cutting Machine"]
[8,"Group E",8,54009844,"ADAPTOR, INSULATOR; TYPE: STEADY ARM EYE CLAMP, DIMENSIONS: OD 50.8/57 MM, APPLICATION: OVERHEAD TRACK EQUIPMENT;  ; DRAWING NO: CEE-TZ-9/35, 0; HOLDER TUBE DIAMETER",160,"CEE-TZ9-0035","1) Drilling Machine \n2) Cutting Machine"]
[9,"Group E",9,54006330,"CLIP; TYPE: ROPE, DIMENSIONS: DIA 3 MM, MATERIAL: WIRE; DRAWING NO: H500110-3-133-E-DE-0109C; TROLLEY WIRE; SALDANHA",3200,"H500110-3-133-E-DE-0109C"]
[10,"Group E",10,54000208,"BOLT ASSEMBLY; NOMINAL DIAMETER: M16, LENGTH: 100 MM, THREAD SERIES: UNC, HEAD: HEXAGON, BOLT GRADE: 8.8, BOLT MATERIAL: STEEL, NUT QUANTITY: 1, THREAD LENGTH: 40 MM; ITEM TO BE SUPPLIED WITH A M16 NUT, M16 SPRING WASHER AND M16 FLAT WASHER. ITEM USED ON THE SISHEN-SALDANHA LINE. H500110-3-133-E-DE-0072",240,"H500110-3-133-E-DE-0072","1. Bolt and Nut forming machine\n"]
[11,"Group E",11,54006329,"ASSEMBLY; TYPE: U-BOLT, APPLICATION: ORE LINE RAIL, DIMENSIONS: DIA 16 MM, MATERIAL: STEEL; DRAWING NO:  H500110-3-133-E-DE-0106, ; TROLLEY WIRE; SALDANHA",0,"H500110-3-133-E-DE-0106,\n SSE-208150","1. Bending/threading machine"]
[12,"Group E",12,54000209,"KIT, MOUNTING, BODY, VEHICULAR; TYPE: BOLT AND NUT, APPLICATION: TROLLEY WIRE; DRAWING NO: H500110-3-133-E-DE-0072, LA; WASHERS; M16; 65MM; OVERHEAD TRACK;  SISHEN SALDANHA RAILWAY LINE (TFR) OHTE CATENARY SYSTEM",160,"H500110-3-133-E-DE-0072011J","1. Bending/threading machine"]
[13,"Group E",13,54006264,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 6 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214,; TROLLEY WIRE; SALDANHA",400,"SSE-208214, \nH500110-3-133-E-DE-0084","1. Bending and cutting machine"]
[14,"Group E",14,54006263,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 13 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214, TROLLEY WIRE; SALDANHA",400,"SSE-208214, \nH500110-3-133-E-DE-0084","1. Bending and cutting machine"]
[15,"Group E",15,54005264,"THIMBLE, ROPE; TYPE: RETAINER, DIMENSIONS: LG 96 MM, MATERIAL: STEEL, ROPE DIAMETER: 100 MM2; DRAWING NO: CEE-TNB-0085; SPECIFICATION: SANS 2262",400,"CEE-TNB-0085\nCEE-TN-0292","1. Bending and cutting machine"]
[16,"Group E",16,54007162,"THIMBLE, ROPE; DRAWING NO: CEE-TZ-7-126 SHEET 36, 0; EQUIPMENT USED ON OHTE; WITH CLEVIS; 25KV; EQUIPMENT USED ON OHTE",400,"CEE-TZ-7-126 SHEET 36","1. Bending and cutting machine"]
[17,"Group E",17,54016291,"THIMBLE, ROPE;  EQUIPMENT USED ON OHTE; SPECIFICATION NUMBER SANS 2262 DATE 1984.; ORDINARY; GALVANISED; TO SPEC SANS 121 DATE 2000; NOMINAL SIZE 17 MM DIA. WIRE.; SABS 811 FIG 1 TABLE 1",400,"As per description and SANS","1. Bending and cutting machine"]
[18,"Group E",18,54015111,"THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 10 X LG 47 MM, MATERIAL: STEEL GALVANIZED, ROPE DIAMETER: 8 MMDRAWING NO: CEE-TZ1-0126 SHEET 6; SPECIFICATION: SANS 2262 DATE 1984",400,"CEE-TZ1-0126 SHEET 6","1. Bending and cutting machine"]
[19,"Group E",19,"54004157","THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 8 X LG 32 MM, MATERIAL: STEEL, FINISH: GALVANIZED, ROPE DIAMETER: 6 MMDRAWING NO: CEE-TNB-0008; SPECIFICATION: CEE.0054BS 4042, 0; EQUIPMENT USED ON OHTE; 6 MM; ALUMINIUM BRONZE DIE CAST; FOR SECTION INSULATOR",80,"CEE-TNB-0008\nCEE.0054 BS 4042","1. Bending and cutting machine"]
[20,"Group E",20,54006261,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 8 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214, TROLLEY WIRE; SALDANHA",400,"SSE-208214,\nH500110-3-133-E-DE-0084","1. Bending and cutting machine"]
[21,"Group E",21,54002498,"THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 27 X LG 150 MM, MATERIAL: STEEL, ROPE DIAMETER: 22 MM, SPECIAL FEATURES: GALVANIZED; DRAWING NO: CEE-TNB-0039; SPECIFICATION: SANS 121 DATE 2000SANS 2262 DATE 1984",400,"CEE-TNB-0039","1. Bending \n2. cutting machine"]
[22,"Group E",22,54011202,"BRACKET; TYPE: CLIMBING ANGLE, APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 1.75 M; DRAWING NO: CEE-TMF-0191; FOR RAIL MAST",240,"CEE-TMF-0191","1. Cutting machine  \n2. welder"]
[23,"Group E",23,54008814,"BRACKET; TYPE: SUPPORT, APPLICATION: STAY WIRE ASSEMBLY, MATERIAL: STEEL; DRAWING NO:  CEE-TMHA-0027",240,"CEE-TMHA-0027 ","1. Cutting machine "]
[24,"Group E",24,54010383,"BRACKET; TYPE: CLIMBING ANGLE , APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 600 MM; DRAWING NO:  CEE-TMF-0152",240,"CEE-TMF-0152 ","1. Cutting machine\n2. welder"]
[25,"Group E",25,54011162,"BRACKET; TYPE: CLIMBING ANGLE , APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 965 MM; DRAWING NO: CEE-TMF-0191; FOR RAIL MAST",320," CEE-TMF-0191","1. Cutting machine \n2. welder"]
[27,"Group E",26,54006272,"BRACKET; TYPE: CLEVIS, MATERIAL: SPHEROIDAL GRAPHITE IRON; SWINGING , H500110-3-133-E-DE-0067,",1120,"H500110-3-133-E-DE-0067,\n SSE-208153","1. Drilling machine\n2. Cutting machine / grinding machine"]
[28,"Group E",27,54011404,"BRACKET; TYPE: VERTICAL ATTACHMENT, MATERIAL: STEEL; DRAWING NO: CEE-TMF-0344; ELECTRICAL EQUIPMENT; EQUIPMENT USED ON OHTE; VERTICAL *A FOR 4725 CONTACT WIRE HEIGHT AUTO TENSION CONSTRUCTION USERS INTEREST 3, 25 AND 50 KV; FOR 25 KV AUTO-TENSION",160," CEE-TMF-0344","1. Drilling machine\n2. Cutting machine / grinding machine"]
[29,"Group E",28,54006343,"ASSEMBLY; TYPE: BRACKET SWIVEL BOLT ON, APPLICATION: ORE LINE RAIL; DRAWING NO:  H500110-3-133-E-DE-0039",320,"H500110-3-133-E-DE-0039","1. Cutting machine\n2. Drilling machine"]
[30,"Group E",29,54002171,"PLATE, METALLIC; TYPE: ADAPTOR, THICKNESS: 6 MM, WIDTH: 50 MM, LENGTH: 120 MM, PLATE MATERIAL: STEEL; DRAWING NO: CEE-TNE-0033, LA; EQUIPMENT USED ON 5405201; EXTENSION AND LINK STRAP GALVANISED FLAT IRON.",120,"CEE-TNE-0033","1. Cutting machine\n2. Drilling machine"]
[31,"Group E",30,54032908,"ASSEMBLY; TYPE: OVERHEAD TRACK EQUIPMENT SUPPORT, APPLICATION: DOME ROOF TUNNEL, DIMENSIONS: LG 65 MM; DRAWING NO: BBB 1673; EQUIPMENT USED ON LINK FOR SUPPORT FITTING AND BRIDGES; 3 KV DC AND 25 KV AC; TO BE SUPPLIED COMPLETE WITH 6 X STEEL FLAT WASHERS GALVANIZED; NORMAL M12. 3 X HEX STEEL BOLTS GALVANIZED WITH NYLOCK NUTS M12",240," BBB 1673","1. Fibreglass mould\n2. Cutting \n3. Drilling machine"]
[32,"Group E",31,54002195,"PLATE, METALLIC; TYPE: ADAPTOR, THICKNESS: 10 MM, WIDTH: 80 MM, LENGTH: 540 MM, MATERIAL GRADE: 304; DRAWING NO: CEE-TNE-0022; EXTENSION AND LINK STRAP GALVANISED MALLEABLE CAST IRON",80," CEE-TNE-0022;","1. Cutting machine\n2. Drilling machine"]
[{"$nulls":3},"Group F"]
[1,"Group F",1,54002805,"ATTACHMENT; TYPE: DROPPER SET, APPLICATION: OVERHEAD TRACK EQUIPMENT; DRAWING NO: CEE-TND-0005, LA; CEE-TND-0022, LA; CEE-TND-0009, LA; COMPLETE SET OF 4 MM. DIAMETER. HARD DRAWN COPPER/STAINLESS DROPPERS FOR A 67 METRE SPAN . TO SUIT ITEM 12 160 MM. SQ. CLIP-ON TYPE CATENARY CLIP. REFER TO (54/16836) AND 161 MM. SQ CONTACT CLIP REFER TO TO BE SUPPLIED WITHOUT CATENARY AND CONTACT CLIP.",8059.200000000001,"CEE-TND-0005, \nCEE-TND-0022, \nCEE-TND-0009","1.Bending machine"]
[{"$nulls":3},"Group G"]
[1,"Group G",1,54032528,"INSULATOR, STANDOFF; TYPE: SQUARE TONGUE/SPADE, INSULATOR MATERIAL: SILICON RUBBER, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBB0429, 4; BBB0430, 3; EQUIPMENT USED ON OHTE",800,"BBB0429, 4; BBB0430","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[2,"Group G",2,54016897,"INSULATOR, STRAIN; TYPE: VANDAL PROOF, POTENTIAL RATING: 3 KVDC; DRAWING NO: CEE-TNC-0004, LA; TONGUE AND CLEVIS TYPE; MUST COMPLY TO QUOTED DRAWING",4000,"CEE-TNC-0004","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[3,"Group G",3,54024239,"INSULATOR, SUSPENSION; TYPE: VANDAL PROOF, INSULATOR MATERIAL: SILICON RUBBER, INSULATOR ATTACHMENT METHOD: ROUND TONGUE/HOOK TONGUE END CAPS, SPECIAL FEATURES: CREEPAGE PATH, 1476 MM; DRAWING NO: BBB3019, LA; BBB 3020, LA; EQUIPMENT USED ON OHTE;25 KV AC",1600,"BBB3019, BBB 3020","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[4,"Group G",4,54032553,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0430, LA; BBB 0429, LA; END CAP CONFIGURATION, CLEVIS/PIPE FITTING",1280,"BBB 0430, BBB 0429","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[5,"Group G",5,54000205,"INSULATOR; TYPE: LONG ROD, VANDAL PROOF, POTENTIAL: 50 KV, MATERIAL: COMPOSITE; DRAWING NO: BBC 1777, LA; ITEM USED ON SISHEN SALDANHA FEEDER LINE TROLLEY WIRE.",240,"BBC 1777","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[6,"Group G",6,54006182,"INSULATOR; TYPE: COMPOSITE COMPRESSION, POTENTIAL: 50 KVAC, MATERIAL: VANDAL PROOF; DRAWING NO: BBF 9766, LA; ITEM USED ON 50KV AC ELECTRIFICATION.",160,"BBF 9766","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[7,"Group G",7,54033393,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 3019, LA; BBB 3020, LA; END CAP CONFIGURATION, ROUND TONGUE: INSULATOR ATTACHMENT METHOD: ROUND TONGUE END CAP",2720," BBB 3019, BBB 3020","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[8,"Group G",8,54033408,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 3019, LA; BBB 3020, LA; END CAP CONFIGURATION: INSULATOR ATTACHMENT METHOD: HOOK/PIPE FITTING END CAPS SPECIAL FEATURES: CREEPAGE PATH, 1476 MM",6080,"BBB 3019, BBB 3020","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[9,"Group G",9,54032541,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB0429, LA; BBB0430, LA; END CAP CONFIGURATION, CLEVIS PIPE FITTING.",5600,"BBB0429, BBB0430","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[10,"Group G",10,54032516,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB0430, LA; BBB0429, LA; VANDAL PROOF, END CAP CONFIGURATION: ROUND TONGUE/PIPE FITTING",1600,"BBB0430, BBB0429","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[11,"Group G",11,54024883,"INSULATOR; TYPE: POST, POTENTIAL: 11 KV, MATERIAL: SILICON RUBBER; DRAWING NO: BBC 8439, LA; SPECIFICATION: SANS 121, LA; VANDAL PROOF POST TRANSMISSION LINE INSULATOR, EQUIPMENT USED ON;  MAST STRUCTURE; F-NECK TYPE; TO INCLUDE M20 X 155 MM LONG FULL THREAD SPINDLE; NUT AND FLAT WASHER",16000,"BBC 8439","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[12,"Group G",12,54033975,"INSULATOR, STANDOFF; TYPE: VANDAL PROOF, INSULATOR MATERIAL: SILICON, POTENTIAL RATING: 50 KVAC, INSULATOR ATTACHMENT METHOD: SQUARE TONGUE AND TUBE END FITTING; USED ON SISHEN-SALDANHA ,H500110-3-133-E-DE-0140, BBC 1684",160,"H500110-3-133-E-DE-0140, \nBBC 1684","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[13,"Group G",13,54032488,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KV, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0281, LA; SPECIFICATION: IEC 1109, 0; CREEPAGE PATH 1476; VANDAL PROOF; (COMPOSITE) SQUARE TONGUE AND ROUND CLEVIS END CAPS",800,"BBB 0281","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[14,"Group G",14,54032476,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO:  BBB0281 , LA; SPECIFICATION: IEC 1109, LA; END CAP CONFIGURATION, ROUND CLEVIS/ROUND TONGUE COMPOSITE",1600,"  BBB0281","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[15,"Group G",15,54032011,"ASSEMBLY; TYPE: INSULATED KNUCKLE, APPLICATION: CATENARY AND CONTACT WIRE; DRAWING NO: CEE-TND-0040; CONSISTING OF ITEMS 1 AND 3 OF QUOTED DRAWING. EQUIPMENT USED ON OHTE ",160,"CEE-TND-0040","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[16,"Group G",16,54032605,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0281, LA; SPECIFICATION: IEC 1109, LA; END CAP CONFIGURATION, SQUARE TONGUE.",800,"BBB 0281","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[17,"Group G",17,54000612,"INSULATOR; TYPE: UNIVERSAL VANDAL PROOF, POTENTIAL: 25 KVAC, DIMENSIONS: AS PER DRAWING; DRAWING NO: BBG 2208",2400,"BBG 2208","1. Crimping / Glueing machine\n2. Silicon injection moulding machine\n"]
[18,"Group G",18,54032868,"ASSEMBLY; TYPE: PIVOT ARM, APPLICATION: DOME ROOF TUNNEL; DRAWING NO: BBB1685 ",120," BBB1685 ","1. Fibreglass mould\n2. Cutting \n3. Drilling machine"]
["CLAMPS ",null,null,"Group H"]
[1,"Group H",1,54002033,"ASSEMBLY; TYPE: CLAMP, APPLICATION: EARTH WIRE; DRAWING NO: CEE-TN-0371, LA; USED ON O.H.T.E",4000,"CEE-TN-0371","1. Drilling machine\n2. Cutting machine"]
[2,"Group H",2,54002753,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 100/80MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE.",4800,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[3,"Group H",3,54002777,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE",24000,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[4,"Group H",4,54000880,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250 TO 160 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA",1280,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[5,"Group H",5,54000907,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250 TO 250 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE",640,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[6,"Group H",6,54000867,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250-100 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE",800,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[7,"Group H",7,54000791,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 80 TO 100 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE",2400,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[8,"Group H",8,54000766,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: 100/80 MM TO 50 MM2, MATERIAL: COPPER AND NICKEL AND SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA",1600,"BBH 2141\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[9,"Group H",9,54001949,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: 100/80 TO 161 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; EQUIPMENT USED ON OHTE",800,"BBH 2142","1. Stamping machine\n2. Machine for serations"]
[10,"Group H",10,54014850,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: 80, 100 TO 107 MM2, MATERIAL: COPPER AND NICKEL AND SILICON; DRAWING NO: BBH 2142, LA; SPECIFICATION: CEE-0063, LA, ITEM: SHEET 1; EQUIPMENT USED ON OHTE",800,"BBH 2142\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[11,"Group H",11,54014862,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: ID 160 TO 107 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; EQUIPMENT USED ON OHTE",10400,"BBH 2142\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[12,"Group H",12,54004930,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: ID 160 TO 161 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; SPECIFICATION: CEE 0063, LA; EQUIPMENT USED ON OHTE",19200,"BBH 2142\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[13,"Group H",13,54006827,"SPLICE, CONDUCTOR; DIMENSIONS: DIA 107 MM2, TYPE: CONTACT WIRE, MATERIAL: COPPER/NICKEL/SILICON; DRAWING NO: BBH 2137, LA",3200,"BBH 2137","1. Stamping machine\n2. Machine for serations"]
[14,"Group H",14,54000754,"SPLICE, CONDUCTOR; DIMENSIONS: 161 MM2, TYPE: CONTACT WIRE, MATERIAL: COPPER/NICKEL/SILICON; DRAWING NO: BBH 2139  , LA; TO BE SUPPLIED 25 EACH PER CARTOON",8000,"BBH 2139 ","1. Stamping machine\n2. Machine for serations"]
[15,"Group H",15,54032504,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA; EQUIPMENT USED ON OHTE",56000,"BBG 7987","1. Stamping machine\n2. Machine for serations"]
[16,"Group H",16,54000560,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 500 TO 160, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA, ITEM: SHEET 2; FEEDER 50 KV; USED ON OHTE FCC CONNECTION 500 MM2 TO 160 MM2 TIGER WIRE",24000,"BBG 7987","1. Stamping machine\n2. Machine for serations"]
[17,"Group H",17,54000603,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 800 TO 160, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA, ITEM: SHEET 3; FEEDER 50 KV; USED ON OHTE FCC 800 MM2 TO 160 MM2 TIGER WIRE",8000,"BBG 7987","1. Stamping machine\n2. Machine for serations"]
[18,"Group H",18,54006787,"ASSEMBLY; TYPE: DROPPER CLIP, APPLICATION: CONTACT WIRE, DIMENSIONS: SQ 107 MM; DRAWING NO; CEE-TND-0022, LA; SPECIFICATION: CEE-0063, LA",16000,"CEE-TND-0022,\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[19,"Group H",19,54017312,"ASSEMBLY; TYPE: DROPPER CLIP, APPLICATION: CONTACT WIRE, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: CEE-TND-0022, LA; SPECIFICATION: CEE.0063, LA; ITEM USED ON CONTACT WIRE SIZE 161MM2.",80000,"CEE-TND-0022,\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[20,"Group H",20,54020848,"KIT; TYPE: MAST CONNECTOR WEDGE, APPLICATION: BONDING; DRAWING NO: BBC 7863, LA; SPECIFICATION: BBB 6017, LA; ITEM USED FOR BONDING ON UNIVERSAL COLUMN AND I-BEAM MAST",40000,"BBC 7863, \nBBB 6017","1. CNC machine"]
[21,"Group H",21,54020824,"KIT; TYPE: RAIL BOND CONNECTOR WEDGE, APPLICATION: BONDING; DRAWING NO: BBC 7864, LA; SPECIFICATION: BBB 6017, LA; EQUIPMENT USED ON OHTE RAIL BONDING",144000,"BBC 7864, \nBBB 6017","1. CNC machine"]
[22,"Group H",22,54011275,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; TYPE: SUSPENSION, CLAMP TYPE: SHACKLE STRAP; DRAWING NO: BBH 2963, LA; SPECIFICATION: SANS 121, LA; EQUIPMENT USED ON OHTE FOR EARTH WIRE; 150 TO 250 MM2; LINER TO BE 2 MM THICK",480,"BBH 2963","1. Stamping machine\n2. Machine for serations"]
[23,"Group H",23,54011643,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 3656 SHEET 1, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 161MM2 CONTACT WIRE FOR LARGE SWIVEL HEADS.",16000,"BBH 3656 SHEET 1\nCEE-0063","1. Stamping machine\n2. Machine for serations"]
[24,"Group H",24,54028819,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLAMP; DRAWING NO: BBH 3656 SHEET 4, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 107MM2 CONTACT WIRE FOR SMALL SWIVEL HEADS.",8000,"BBH 3656 SHEET 4\nCEE-0063","1. Stamping machine\n2. Furnace"]
[25,"Group H",25,54011591,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 3656 SHEET 3, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 107MM2 CONTACT WIRE FOR LARGE SWIVEL HEAD.",8000,"BBH 3656 SHEET 3\nCEE-0063","1. Stamping machine\n2. Furnace"]
[26,"Group H",26,54000690,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON, ATTACHMENT METHOD: WIRE 161 MM2; DRAWING NO: BBH 3656 SHEET 2, LA; CEE-TND-0001 SHEET 1, LA; CEE-TND-0035, LA; SPECIFICATION: CEE-0063, LA; CONTACT WIRE FOR SMALL SWIVEL HEAD FOR GENERAL USE COMPLETE WITH STEADY ARM FITTING.",8000," BBH 3656 SHEET 2\nCEE-0063","1. Stamping machine\n2. Furnace"]
[27,"Group H",27,54033583,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLAMP; DRAWING NO: BBH 3656 SHEET 2, LA; SPECIFICATION: CEE-0063, LA; FULL ASSEMBLY SWIVEL CHEEKS FOR 161 MM2 CONTACT WIRE FOR SMALL SWIVEL HEAD.",8000,"BBH 3656 SHEET 2\nCEE-0063","1. Stamping machine\n2. Furnace"]
[{"$nulls":3},"Group I"]
[1,"Group I",1,54016836,"CLIP; TYPE: DROPPER SADDLE, MATERIAL: NYLON, APPLICATION: SINGLE CATENARY; DRAWING NO: CEE-TND-0005, LA; INSULATOR,ELECTRICAL CONDUCTOR EQUIPMENT USED ON OHTE. SINGLE CATENARY NYLON DROPPER SADDLE. FOR CATENARY WIRE 160 MM SQ",112000,"CEE-TND-0005","1. Plastic injection moulding machine"]
[2,"Group I",2,54006840,"HANGER, WIRE STRAND; TYPE: CLIP ON, MATERIAL: NYLON; DRAWING NO: CEE-TND-0005; INSULATOR ELECTRICAL CONDUCTOR EQUIPMENT USED ON OHTE; SINGLE CATENARY NYLON DROPPER SADDLE; FOR CATENARY WIRE 80 MM SQ",32000," CEE-TND-0005","1. Plastic injection moulding machine"]
[3,"Group I",3,54017070,"SADDLE; TYPE: CATENARY LOOP DROPPER, MATERIAL: NYLON; DRAWING NO: CEE-TND-0011, LA; SLEEVE,PROTECTIVE; EQUIPMENT USED ON OHTE; CLIP-ON-TYPE. ONLY SUITABLE FOR USE WITH 4 MM SOLID WIRE",16000," CEE-TND-0011","1. Plastic injection moulding machine"]
[{"$nulls":3},"Group J"]
[1,"Group J",1,54004020,"PIN, STRAIGHT, HEADED; DIAMETER: 16 MM, LENGTH: 60 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0066CEE-TX-0054; SPECIFICATION: SANS 121 DATE 2000; COMPLETE WITH BRASS SPLIT PIN ACCORDING TO DRAWING",9600," CEE-TX-0066\nCEE-TX-0054","1. Cotter pin forming machine"]
[2,"Group J",2,54006193,"CLAMP ASSEMBLY, RETAINING; TYPE: BALL SWIVEL; DRAWING NO: BBH 1181 , LA; ATTACHMENT TO REGISTER ARM CONSISTING OF BODY, M12 DIA \"U\" BOLT, COMPLETE WITH NUTS & SPRING WASHERS. ATTACHMENT FOR 42.4MM AND 48.3MM PIPE. EQUIPMENT USED ON 25KV OHTE.",240," BBH 1181","1. Drilling machine\n2. Cutting/grinding machine"]
[3,"Group J",3,54006270,"CLAMP ASSEMBLY, RETAINING; TYPE: STRAIN, ATTACHMENT METHOD: CLEVIS;  DRAWING NO: BBH 1179, LA;  ITEM USED ON 25 KV AC OHTE FOR A PIPE OF DIAMETER 42.4 MM2 AND 48.3 MM2",560,"BBH 1179","1. Drilling machine\n2. Cutting/grinding machine"]
[4,"Group J",4,54004019,"PIN, CLEVIS; DIAMETER: 24 MM, LENGTH: 60 MM, MATERIAL: MILD STEEL; DRAWING NO: CEE-TX-0080; COMPLETE WITH SPLIT PIN ",4800,"CEE-TX-0080","1. Cotter pin forming machine"]
[5,"Group J",5,54027321,"PIN, CLEVIS; DIAMETER: 16 MM, LENGTH: 80 MM, MATERIAL: STEEL; DRAWING NO: SSE-208269; CF 222, 50KV AC ",4800," SSE-208269","1. Cotter pin forming machine"]
[6,"Group J",6,54015855,"PIN, CLEVIS; DIAMETER: 20 MM2, LENGTH: 315 MM, MATERIAL: STAINLESS STEEL, HEAD STYLE: FLAT;  DRAWING NO: BBH 1164, LA;  EQUIPMENT USED BETWEEN ERMELO AND VRYHEID ELECTRICFICATION",4800," BBH 1164","1. Cotter pin forming machine"]
[7,"Group J",7,54017753,"PIN, STRAIGHT, HEADED; DIAMETER: M16, LENGTH: 55 MM, MATERIAL: STAINLESS STEEL; SPECIFICATION: SANS 1700 PART 17, LA; PIN FINISH MUST BE SNAPHEAD AND MUST BE SUPPLIED WITH A LOCKING SPLIT PIN. ITEM USED ON THE SISHEN-SALDANHA LINE. H500110-3-133-E-DE-0074, SSE-208269",0,"H500110-3-133-E-DE-0074\nSSE-208269","1. Cotter pin forming machine"]
[8,"Group J",8,54020885,"PIN, CLEVIS; DIAMETER: 12 MM, LENGTH: 33 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0073; FINISH, HOT DIP GALVANISE TO SANS 121. EQUIPMENT USED ON OHTE STORES DESCRIPTION CLEVIS PIN M12 FOR TROLLEY WIRE DESIGN 25 AND 50 KV COMPLETE WITH BRASS SPLIT PIN ",4000,"CEE-TX-0073","1. Cotter pin forming machine"]
[9,"Group J",9,54011793,"PIN, CLEVIS; DIAMETER: 16 MM, LENGTH: 152 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0054; EQUIPMENT USED ON: OHTE; ROUND HEAD, STEEL,ZINC COATED M16 X 160 MM LONG CENTRE LINE OF 7 MM DIA SPLIT PIN HOLE 152 MM DIA FROM HEAD SUPPLIED WITH SPLIT PIN; CLEVIS (54003734) ",4000," CEE-TX-0054","1. Cotter pin forming machine"]
[10,"Group J",10,54004007,"PIN, CLEVIS; DIAMETER: 24 MM2, LENGTH: 76 MM, MATERIAL: MILD STEEL; DRAWING NO: CEE-TX-0059, LA, ITEM: 1 & 2; CEE-TX-0059; EQUIPMENT USED ON TENSION BRIDGE AND ANCHOR MAST;  COMPLETE WITH SPLIT PIN AS PER DRAWING.",4000,"CEE-TX-0059, LA, ITEM: 1 & 2;\n CEE-TX-0059","1. Cotter pin forming machine"]
[11,"Group J",11,54001582,"ATTACHMENT; TYPE: ADAPTOR, APPLICATION: STEADY ARM SOCKET; DRAWING NO: CEE-TNB-0076, LA",1600,"CEE-TNB-0076","1. Drilling machine\n2. Cutting/grinding machine"]
[12,"Group J",12,54002790,"SLEEVE; TYPE: TUBING, APPLICATION: DROPPER SECURING, INSIDE DIAMETER: 8 MM, OUTSIDE DIAMETER: 10 MM, LENGTH: 10 MM, MATERIAL: COPPER; DRAWING NO: CEE-TX-0079, LA",68800,"CEE-TX-0079","1) Tube cutter/ Spring forming machine"]
[13,"Group J",13,54004978,"ASSEMBLY; TYPE: WIRE ENDING CONE, APPLICATION: CONTACT WIRE; DRAWING NO: CEE-TNB-0036, LA; EQUIPMENT USED ON OHTE",480,"CEE-TNB-0036","1. Drilling machine\n2. Cutting/grinding machine"]
[null,null,14,54112457,"BUSHING, SLEEVE; TYPE: SPRING, INSIDE DIAMETER: 9 MM, OUTSIDE DIAMETER: 12.2 MM, OVERALL LENGTH: 10 MM, APPLICATION: DROPPER SECURING; DRAWING NO: CEE-TX-0079 SHEET 1, LA",null,null,"1) Tube cutter/ Spring forming machine"]
[{"$nulls":3},"Group K"]
[1,"Group K",1,54016925,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 800 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 4",9600,"BBD 5138,","1. Stamping machine"]
[2,"Group K",2,54002152,"CLAMP; TYPE: FEEDER CLAMP, DIMENSIONS: AS PER DRAWING, MATERIAL: BI-METALLIC; DRAWING NO: BBH 0306, LA; CLAMP IS USED FOR JOINING 160 MM2 ALUMINIUM(TIGER) AND 107 MM2 COPPER CONTACT WIRE; BI-METAL  FEEDER CLAMP",19200,"BBH 0306","1. Stamping machine"]
[3,"Group K",3,54000401,"CLAMP; TYPE: FEEDER, DIMENSIONS: AS PER DRAWING, MATERIAL: BI-METALLIC; DRAWING NO: BBG 6147, 0; SPECIFICATION: CEE-0063, 0; PARALLEL; CU-NI-SI; COPPER CONTACT WIRE, TIGER TO 161 CONTACT",96000,"BBG 6147","1. Stamping machine"]
[4,"Group K",4,54032387,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA; BI-METAL, WITH A PERMANENT FORGED COPPER INSERT",24000,"BBD 5138","1. Stamping machine"]
[5,"Group K",5,54032375,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 100/80 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 5",4800,"BBD 5138, LA, ITEM: SHEET 5","1. Stamping machine"]
[6,"Group K",6,54016937,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 500 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 3",10400,"BBD 5138, LA, ITEM: SHEET 3","1. Stamping machine"]
[7,"Group K",7,54032363,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 50 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 5",3520," BBD 5138, LA, ITEM: SHEET 5","1. Stamping machine"]
[{"$nulls":3},"Group L"]
[1,"Group L",1,54009274,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 28.8 MM, OUTSIDE DIAMETER: 31.8 MM, LENGTH: 6.1 M, MATERIAL: STEEL; SPECIFICATION: SANS 121 DATE 2000; MATERIAL TO BE GRADE 300 WA HOT DIPPED GALVANISED TO SPECIFICATION ",800,null,"1. Cutting machine"]
[2,"Group L",2,54001962,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 44 MM, OUTSIDE DIAMETER: 48 MM, LENGTH: 3.36 M, MATERIAL: STEEL; DRAWING NO: CEE-TMHH-0002; SPECIFICATION:  SANS 657 PART 1; STORES DESCRIPTION PUSH-PULL-OFF REGISTERING TUBE WITH A CLEVIS AT EACH END. ",800,"CEE-TMHH-0002","1. Cutting machine\n2. Crimping tool"]
[3,"Group L",3,54029813,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 34.9 MM, OUTSIDE DIAMETER: 38.1 MM, LENGTH: 3.02 M, MATERIAL: STEEL; DRAWING NO: BT102; EQUIPMENT USED ON OHTE BRITS-THABAZIMBI STORES DESCRIPTION REGISTERING TUBE 38.1 X 38.1 X 3.2 MM WALL X 3.020 METRE LONG ",800,null,"1. Crimping tool\n2. Cutting Machine"]
[4,"Group L",4,54030162,"TUBE; TYPE: REGISTERING , INSIDE DIAMETER: 22.5 MM, OUTSIDE DIAMETER: 26 MM, LENGTH: 1.65 M, MATERIAL: STEEL; EQUIPMENT USED ON OHTE BRITS-THABAZIMBI STORES DESCRIPTION REGISTERING TUBE 26 MM OD X 3.5 MM THICK ",800,null,"1. Cutting machine"]
[5,"Group L",5,54009302,"TUBE, STRUCTURAL; TYPE: STEADY ARM BRIDGE TYPE, DIMENSIONS: THK 2.03 MM, MATERIAL: STAINLESS STEEL GRADE 304;  DRAWING NO: CEE-TN -0152; OD = 25.4 MM. TOLERANCE+0-O.75 WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE STRESS = 486 N/MM SQ. MINIMUM. MATERIAL = AISI 304 WELDED",800,"CEE-TN -0152","1. Pipe bending Machine"]
[6,"Group L",6,54009314,"TUBE, STRUCTURAL; TYPE: CURVED STEADY ARM, DIMENSIONS: DIA 25.4 MM X LG 1.132 M, MATERIAL: STAINLESS STEEL GRADE 304; DRAWING NO: CEE-TND-0019; TOLERANCE+0-0.75. WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE STRESS = 486 N/MM SQ. MINIMUM. MATERIAL = AISI 304 WELDED",800,"CEE-TND-0019","1. Pipe bending Machine"]
[7,"Group L",7,54027624,"TUBE, STRUCTURAL; TYPE: REGISTRATION TUBE, DIMENSIONS: OD 42.8 MM X LG 3.06 M; DRAWING NO: BBH 1283, LA; ITEM USED FOR PUSH-PULL-OFF APPLICATION",800,"BBH 1283","1. Crimping tool\n2. Cutting Machine"]
[8,"Group L",8,54009338,"TUBE, STRUCTURAL; TYPE: TUNNEL STEADY ARM, DIMENSIONS: DIA 25.4 X LG 990 X THK 2.03 MM, MATERIAL: STAINLESS STEEL GRADE 304; DRAWING NO: CEE-TN -0153, 0; STRESS = 486 N/MM SQ MINIMUM. MATERIAL = AISI 304 WELDED. TUNNEL STEADY ARM. OD = 25.4 MM.TOLERANCE+0-0.75. WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE",800,"CEE-TN -0153","1. Pipe bending Machine"]
[9,"Group L",9,54001735,"TUBE, STRUCTURAL; TYPE: CANTILEVER, DIMENSIONS: DIA 76 MM X LG 2.8 M X THK 5.5 MM; DRAWING NO: CEE-TMC-0042; USED FOR 2.75 M TRACK CENTRES FOR 203 X 203 UC MASTS ",800,"CEE-TMC-0042","1. Cutting machine \n2. welder"]
[10,"Group L",10,54002450,"TUBE, STRUCTURAL; TYPE: REGISTERING ARM, DIMENSIONS: OD 48 X LG 900 X THK 4 MM, MATERIAL: STEEL; DRAWING NO: CEE-TN-0244; SPECIFICATION: SANS 657; EQUIPMENT USED ON 5400000 5405200 5405202 SPECIFICATION NUMBER SANS 657 GALVANISED WITH CLEVIS FITTING EACH END; GRADE 340 ERW ",800," CEE-TN-0244","1. Pipe bending Machine\n2. Crimping tool"]
[11,"Group L",11,54112455,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT, MATERIAL: STAINLESS STEEL; DRAWING NO: BBH 0441, LA, ITEM: 1; ITEM USED FOR TANGENT TRACK BETWEEN BRITS AND THABAZIMBI.",800,"BBH 0441","1. Pipe bending Machine\n2. Crimping tool"]
[12,"Group L",12,54920893,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 2; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI.",800,"BBH 0442","1. Pipe bending Machine\n2. Crimping tool"]
[13,"Group L",13,54112456,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 3; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI.",800,"BBH 0442, LA, ITEM: 3;","1. Pipe bending Machine\n2. Crimping tool"]
[14,"Group L",14,54112452,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 1; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI",800,"BBH 0442, LA, ITEM: 1","1. Pipe bending Machine\n2. Crimping tool"]
[15,"Group L",15,54001658,"PIPE ASSEMBLY; TYPE: REGISTERING , APPLICATION: PUSH PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 X THK 4 X LG 2730, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO:  1CEE-TMHH- 2/LATEST, 0; SPECIFICATION: SANS 657 PART 1; SPECIFICATION GRADE 340 ERW ",800,"CEE-TMHH- 2","1. Crimping tool"]
[16,"Group L",16,54015451,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: OVERHEAD TRACK EQIPMENT, MATERIAL: STEEL, DIMENSIONS: ID 30 MM X LG 1.015 M X THK 2 MM, CONNECTION TYPE: HOOK AND SOCKET; DRAWING NO: CEE-TN-0386, LA; SPECIFICATION: SANS 121, LASANS 657 GRADE 250, LA",800,"CEE TZ4-0068","1. Pipe bending Machine\n2. Crimping tool"]
[17,"Group L",17,54000236,"PIPE ASSEMBLY; TYPE: REGISTERING , APPLICATION: DOUBLE BOOMS, MATERIAL: STEEL, DIMENSIONS: OD 48 X THK 4 X LG 2320 MM, CONNECTION TYPE: WITH CLEVIS; DRAWING NO: CEE-TMF-0444; SPECIFICATION: SANS 121DATE 2000SANS 657 PART 1; 25KV AUTO TENSION   BEAUFORT-WEST DE AAR ,SPECIFICATION HOT DIPPED GALVANISED ",800,"CEE-TMF-0444","1. Crimping tool"]
[18,"Group L",18,54001723,"PIPE ASSEMBLY; TYPE: REGISTERING ARM, APPLICATION: PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 MM X LG 1.9 M X THK 4 MM, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO: CEE-TMHH-0002; CEE-TN-0408",800,"CEE-TMHH-0002;\n CEE-TN-0408","1. Crimping tool"]
[19,"Group L",19,54001747,"PIPE ASSEMBLY; TYPE: REGISTERING ARM, APPLICATION: PUSH PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 MM X THK 4 MM X LG 3.030 M, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO: CEE-TMHH-0002; SPECIFICATION: SANS 657 PART 1; SPECIFICATION GRADE 340 ERW ",800," CEE-TMHH-0002","1. Crimping tool"]
[20,"Group L",20,54000111,"PIPE, METALLIC; TYPE: STEADY ARM, PIPE SIZE: OD 25 MM, LENGTH: 2.3 M, WALL THICKNESS: 2.5 MM, PIPE MATERIAL: STAINLESS STEEL, SPECIAL FEATURES: STRAIGHT ADJUSTABLE STEADY ARM; DRAWING NO: CEE-TZ7-0123 SHEET 49, LA; EQUIPMENT USED ON 25 KV OHTE; WITH EYE CLAMP (ITEM 2)",800,"CEE-TZ7-0123 SHEET 49","1. Crimping tool"]
[21,"Group L",21,54007303,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 44 MM, OUTSIDE DIAMETER: 48 MM, LENGTH: 6 IN, MATERIAL: STEEL; DRAWING NO: CEE-TND-0034; STEEL TUBE FOR STRUCTURAL AND GENERAL ENGINEERING PURPOSES, GALVANISED TO SABS 763.25 KV OHTE ",48,"CEE-TND-0034","1. Crimping tool"]
[22,"Group L",22,54028185,"TUBE; TYPE: REGISTERING , INSIDE DIAMETER: 46 MM, OUTSIDE DIAMETER: 50 MM, LENGTH: 3.1 M, MATERIAL: STEEL; DRAWING NO: SSE-208206 CF 506; 3.81KG/M. EQUIPMENT USED ON THE SISHEN SALDANHA OVERHEAD TRACK EQUIPMENT ",48,"SSE-208206","1. Crimping tool"]
[23,"Group L",23,54009755,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 30.02 MM, OUTSIDE DIAMETER: 33.4 MM, LENGTH: 6 IN, MATERIAL: STAINLESS STEEL GRADE 304",48,null,"1.Cutting tool"]
[24,"Group L",24,54009237,"TUBE; TYPE: REGISTERING INLAND, INSIDE DIAMETER: 38.86 MM, OUTSIDE DIAMETER: 42.86 MM, LENGTH: 6.1 M, MATERIAL: STEEL; DRAWING NO: SANS 121 DATE 2000; MATERIAL TO BE GRADE 300 WA HOT DIPPED GALVANISED TO SPEC ",48,null,"1.Cutting tool"]
[25,"Group L",25,54001812,"TUBE ASSEMBLY, METALLIC; TYPE: CANTILEVER, LENGTH: 3.75 M, TUBE MATERIAL: STEEL; DRAWING NO: CEE-TMC-0042 ; FOR 203 X 203 UNIVERSAL COLUMNS MAST ",48,"CEE-TMC-0042","1. Cutting machine \n2. welder"]
[26,"Group L",26,54001407,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 3 M, OUTSIDE DIAMETER: 50 MM, WALL THICKNESS: 4 MM, TUBE MATERIAL: STEEL;  DRAWING NO: CEE-TND-0038;  SPECIFICATION: SANS 121 DATE 2000;  PUSH-PULL OFF.EQUIPMENT USED ON OHTE",48,"CEE-TND-0038;","1. Crimping tool\n2. Cutting Machine"]
[27,"Group L",27,54112441,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 3600 MM, OUTSIDE DIAMETER: 480 MM, WALL THICKNESS: 4 MM, TUBE MATERIAL: STEEL; DRAWING NO: CEE-TMG-0140, LA, ITEM: 11",48,"CEE-TMG-0140","1. Cutting Machine"]
[28,"Group L",28,54001432,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 2.8 M, OUTSIDE DIAMETER: 76 MM, TUBE MATERIAL: STEEL, SURFACE TREATMENT: GALVANIZED;    DRAWING NO: CEE-TMC-0041;  CANTILEVER, FOR 2,75 M TRACK CENTRES AND 203 X 152 AND 229 X 178 MM I MASTS",48," CEE-TMC-0041","1. Cutting machine \n2. welder"]
[29,"Group L",29,54009351,"TUBE; TYPE: KNUCKLE, INSIDE DIAMETER: 23.4 MM, OUTSIDE DIAMETER: 25.4 MM, LENGTH: 330 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: CE-TN -0155; TOLERANCE+0-0.75; MINIMUM AFTER MANIPULATION; HARDNESS: 180-270 BRINELL; ELONGATION: 6 PCT MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 PCT OFFSET; ULTIMATE TENSILE STRESS: 486 N/MM SQ MINIMUM; MATERIAL: AISI 304 WELDED ",48,"CE-TN -0155","1.Cutting machine"]
[30,"Group L",30,54006259,"ARM; TYPE: STEADY, DIMENSIONS: LG 910 MM, MATERIAL: STAINLESS STEEL; DRAWING NO:  H500110-3-133-E-DE-0051",160,"H500110-3-133-E-DE-0051","1. Pipe bending Machine\n2. Crimping tool\n3. Welder"]
[31,"Group L",31,54009743,"TUBE, STRUCTURAL; TYPE: CANTILEVER, DIMENSIONS: 60,33 MM OD X 3,91 MM WALL X 6 M LONG, MATERIAL: STAINLESS STEEL GRADE 304",48,null,"1.Cutting tool"]
[{"$nulls":3},"Group M"]
[1,"Group M",1,54011441,"INSULATOR;  P/N: 655154665, ARTHUR FLURY;  P/N: UNKNOWN, PFISTERER (PTY)LIMITED; SECTION SPECIFICATION NUMBER CEE.0056.86 25KV AC - 3KV DC CHANGE OVER YARDS. FOR 161 SQ MM CONTACT WIRE. TO QUOTED PARTNUMBER OR EQUAL. ",16,"CEE.0056.86","1.Welding Machine \n2. Bending facilities for runners\n3. Facilities for insulation rods"]
[2,"Group M",2,54005304,"INSULATOR; TYPE: NEUTRAL SECTION, POTENTIAL: 25 KV, DIMENSIONS: DIA 161 MM2;  P/N: 655.236.000, ARTHUR FLURY; MATERIAL NUMBER; 54005304;  EQUIPMENT USED ON OHTE, CONTACT WIRE 3 KVDC; COMPLETE WITH HANGING GEAR ",40,null,"1.Welding Machine \n2. Bending facilities for runners\n3. Facilities for insulation rods"]
[3,"Group M",3,54010840,"INSULATOR; TYPE: DOUBLE ROD SECTION, POTENTIAL: 25 KVAC; SPECIFICATION: CEE-0055, LA; FOR 107 SQ MM CONTACT WIRE",48,"CEE-0055","1.Welding Machine \n2. Bending facilities for runners\n3. Facilities for insulation rods"]
[4,"Group M",4,54010775,"INSULATOR; TYPE: SECTION INSULATOR, POTENTIAL: 3 KVDC; SPECIFICATION: CEE.0054, LA; ITEM USED ON 161 SQ MM CONTACT WIRE ON 3KV DC ELECTRIFICATION.",48,"CEE.0054","1.Welding Machine \n2. Bending facilities for runners\n3. Facilities for insulation rods"]
[5,"Group M",5,54005454,"INSULATOR; TYPE: NEUTRAL SECTION, POTENTIAL: 25 KV, DIMENSIONS: DIA 107 MM2;  P/N: 655.150.720, ARTHUR FLURY; MATERIAL NUMBER 54005454,EQUIPMENT USED ON OHTE, TO QUOTED PART NUMBERS OR EQUAL ",48,"P/N: 655.150.720","1.Welding Machine \n2. Bending facilities for runners\n3. Facilities for insulation rods"]
[6,"Group M",6,48007470,"MAGNET; TYPE: TRACK SIDE; DRAWING NO: CEE-TLE 7, LV; 25KV AC MAGNET TYPE S25000-Q 5697-C5 WITH AN EFFECTIVE FLUX OF 3090: 10 WEBBER AT A VERTICAL HEIGHT OF 150 MM AND AN OFF CENTRE OFF DISTANCE OF 50 MM AT AN AMBIENT TEMP: OF 60 DEG C. TO QUOTED PART NUMBER OR EQUAL FOR BOLTS 48000290 EQUIPMENT USED ON SUBS",57.6,"CEE-TLE 7\n","1. Magnet cutting machine\n2. Magnet Magnitize/charging machine"]
[7,"Group M",7,48008968,"BLOCK; TYPE: MOUTING TRACK MAGNET RUBBER, WIDTH: 380 MM, LENGTH: 1.4 M, HEIGHT: 170 MM, MATERIAL: RUBBER; DRAWING NO: BBC 0694, LV; ITEM 48008968:TRACK MAGNET RUBBER DESIGNED FOR SLEEPER SPACING FROM 630MM TO 725MM 25 KV. LOCOMOTIVE SWITCHING AT NEUTRAL SECTIONS. COMPLETE AS PER DRAWING FOR \"U: BOLTS 54000515 FOR MAGNET 4807470 FOR MAGNET BOLTS 48000290; EQUIPMENT USED ON OHTE / SUBS; MOUNTING",57.6," BBC 0694","1. Rubber moulding/forming machine"]
[{"$nulls":3},"Group N"]
[1,"Group N",1,54016003,"WEIGHT, COUNTERBALANCE; TYPE: ROUND, WEIGHT MATERIAL: CONCRETE, GROSS WEIGHT: 25 KG, SPECIAL FEATURES: WITHOUT EYE;  DRAWING NO: CEE-TZ9-0113 ITEM 15; CEE-TZ9-0107",48,"CEE-TZ9-0113 ITEM 15; \nCEE-TZ9-0107","1) Scale for measurements"]
[2,"Group N",2,54006738,"WEIGHT, COUNTERBALANCE; TYPE: SOLID, WEIGHT MATERIAL: IRON, GROSS WEIGHT: 20 KG;  DRAWING NO: CEE-TMF-0491; LINE TENSIONING EQUIPMENT USED ON CID 5400000 5405202; IRON WEIGHT. 20 KG. CONTACT AND CATENARY WIRES. 25 KV OVERHEAD TRACK EQUIPMENT",48," CEE-TMF-0491","Casting - no special tools required"]
[3,"Group N",3,54016229,"WEIGHT, COUNTERBALANCE; TYPE: ROUND, WEIGHT MATERIAL: CONCRETE, GROSS WEIGHT: 25 KG;  DRAWING NO: CEE-TZ9-0113; CEE-TZ9-0461; CEE-TZ9-0400;  STORES DESCRIPTION CONCRETE WEIGHT 25 KG WITH EYE PIECE.",48,"CEE-TZ9-0113; \nCEE-TZ9-0461;\n CEE-TZ9-0400","1) Scale for measurements"]
[4,"Group N",4,54006726,"WEIGHT, COUNTERBALANCE; TYPE: SOLID, WEIGHT MATERIAL: IRON, GROSS WEIGHT: 40 KG;  DRAWING NO: CEE-TMF-0490; LINE TENSIONING; EQUIPMENT USED ON: CID 5400000 5405202; CAST IRON WEIGHT. 40 KG. CONTACT AND CATENARY WIRES.",48,"CEE-TMF-0490","1) Scale for measurements"]
[5,"Group N",5,54009186,"TENSIONER; TYPE: COMPACT AUTOMATIC SPRING, DIMENSIONS: AS PER SPECIFICATION; SPECIFICATION: BBG 2165, LA; ITEM USED FOR TENSIONING OHTE CONDUCTORS.",48," BBG 2165","1. Spring Forming Machine"]
[6,"Group N",6,54000202,"COUNTERWEIGHT; TYPE: PULLEY WHEEL, DIMENSIONS: AS PER DRAWING, APPLICATION: TROLLEY WIRE; DRAWING NO: SSE TMF 05 , LA; OVERHEAD TRACK; COMPLETE; 50KV OHTE; VICTORY ELECTRICAL CAPE TOWN ; SALDANHA; HOT DIPPED GALVANIZED, H500110-3-133-E-DE-0102",40,"SSE TMF 05\nH500110-3-133-E-DE-0102","1. Lathe/CNC Machine"]
[7,"Group N",7,54006326,"COUNTERWEIGHT; TYPE: PULLEY WIRE, DIMENSIONS: LG 6.3 M X THK 10 MM, MATERIAL: STAINLESS STEEL; DRAWING NO:  H500110-3-133-E-DE-0110; TROLLEY WIRE; SALDANHA",48,"H500110-3-133-E-DE-0110","1. Crimping tool\n2.Cable cutter"]
[8,"Group N",8,54006637,"GUIDE; TYPE: EYE, APPLICATION: BALANCE WEIGHT, MATERIAL: STEEL;  DRAWING NO: CEE-TZ1-0124 SHEET 6",48,"CEE-TZ1-0124 SHEET 6 ","1. Crimping tool\n2. Bending machine/Foam factor machine"]
[9,"Group N",9,54009326,"FAIRLEAD, SHEAVE; TYPE: BALANCE WEIGHT PULLEY, MATERIAL: STEEL; DRAWING NO: CEE-TZ1-0124 SHEET 8; SPECIFICATION: SANS 121 DATE 2000; ELECT RAIL PULLEY SINGLE BALANCE WEIGHT PULLEY WITHOUT BOND ATTACHMENT TO TENSION 25 KV. O.H.T.E.LINE GALVANISED TO SPECIFICATION",160," CEE-TZ1-0124 SHEET 8","1. Lathe/CNC Machine"]
[10,"Group N",10,54010763,"TENSIONER PULLEY ASSEMBLY; TYPE: BALANCE WEIGHT, MATERIAL: STEEL; DRAWING NO: CEE-TMF-0523; SPECIFICATION: CEE-0131-85; STANDARD: SABS ISO 1461 ; CONTACT AND CATENARY 25 KV WIRE DEVICE: CONSISTING OF BASIC BALANCE WEIGHT PULLEY, WIRE ROPE AND CONNECTING DEVICES",48,"CEE-TMF-0523; \nCEE-0131-85;","1. Lathe/CNC Machine\n2. Drilling machine\n3. Cable crimping tool"]
[{"$nulls":3},"Group O"]
[1,"Group O",1,54011934,"SWITCH ASSEMBLY; TYPE: CHANGEOVER TRACK SWITCH; DRAWING NO: BBH 2140, LA; ITEM USED AS  25 KV AC - 3 KV DC SWITCH IN THE CHANGE OVER YARD.",16," BBH 2140","1. Crimping tool\n2. Cutting Machine"]
[2,"Group O",2,54033926,"SWITCH ASSEMBLY; TYPE: TRACK, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBB5971; BBC6441; CEE-TZ9-0236; BBC6440;  EQUIPMENT USED ON OHTE STORES DESCRIPTION TRACK SECTIONING SWITCH 25 KV AC COMPLETE WITH LOCKING DEVICE BUT WITHOUT CLOSING MECHANISM",16," BBB5971; BBC6441;\n CEE-TZ9-0236; BBC6440","1. Crimping tool\n2. Cutting Machine"]
[3,"Group O",3,54017765,"SWITCH ASSEMBLY; TYPE: SIDING, POTENTIAL RATING: 3 KVDC; DRAWING NO: BBB5971 ; CEE-TLB-0038; BBB5970; SPECIFICATION: CEE-0228.96;  STORES DESCRIPTION SIDING SWITCH 3 KV. DC. WITHOUT OPERATING HANDLE, COMPLETE WITH LOCKING DEVICE. INSULATORS MUST BE OF THE SILICON VANDAL PROOF TYPE APPROVED INSULATOR : SILICOSIL-POST INSULATOR TO PARTNUMBER DP167-0178-003 GMC POWERLINE OR EQUAL",16," BBB5971 ; CEE-TLB-0038; \nBBB5970","1. Crimping tool\n2. Cutting Machine"]
[4,"Group O",4,54001331,"SWITCH ASSEMBLY; TYPE: SIDING, SPECIAL FEATURES: NO LOCKING DEVICE; DRAWING NO: CEE-TLB-0038; SPECIFICATION: CEE.0228.96; SIDING 3 KV DC. WITHOUT OPERATING HANDLE.",40,"CEE-TLB-0038\n T-S2F-0002CEE.0228.96","1. Crimping tool\n2. Cutting Machine"]
[5,"Group O",5,54033938,"SWITCH ASSEMBLY; TYPE: SIDING, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBC6441; BBC6440 ; BBB5971; CEE-TZ7-0121 SHEET 189; SPECIFICATION: CEE.0228.96; STORES DESCRIPTION SIDING SWITCH 25 KV AC COMPLETE WITH LOCKING DEVICE",16,"BBC6441; BBC6440 ; \nBBB5971; CEE-TZ7-0121 SHEET 189","1. Crimping tool\n2. Cutting Machine"]
[6,"Group O",6,54005733,"SWITCH, KNIFESPECIFICATION CEE.0228.96; SIDING 25 KV AC. POLLUTED & NON POLLUTED AREAS. TO QUOTED PART NUMBER OR EQUAL",16,"CEE.0228.96","1. Crimping tool\n2. Cutting Machine"]
[7,"Group O",7,54001242,"SWITCH, KNIFE; TYPE: TRACK, CURRENT RATING: 3 KA, POTENTIAL RATING: 3 KV;  SPECIFICATION: CEE 228.96, EQUIPMENT USED ON OHTE MOVING BLADE FOR AEG TYPE; STORES DESCRIPTION BLADE, ELECTRICAL SWITCH",16,"CEE 228.96","1. Crimping tool\n2. Cutting Machine"]
[8,"Group O",8,54017397,"SWITCH, KNIFE; TYPE: TRACK SWITCH, POTENTIAL RATING: 3 KVDC, NUMBER OF POLES: SINGLE, SPECIAL FEATURES: COMPLETE WITH LOCKING DEVICE; DRAWING NO: BBC 8741, LA, ITEM: 1 (with locking device)",16,"BBC 8741,","1. Crimping tool\n2. Cutting Machine"]
[9,"Group O",9,54014938,"SWITCH ASSEMBLY; TYPE: TRACK SWITCH, POTENTIAL RATING: 25 KVAC, SPECIAL FEATURES: SINGLE POLE; DRAWING NO: BBC 8743, LA",32,"BBC 8743","1. Crimping tool\n2. Cutting Machine"]
[10,"Group O",10,54005276,"SWITCH, KNIFE; TYPE: TRACK, POTENTIAL RATING: 3 KVDC, NUMBER OF POLES: SINGLE, SPECIAL FEATURES: WITHOUT LOCKING DEVICE; DRAWING NO: BBC 8741, LA, ITEM: 2 (no locking device)",16,"BBC 8741","1. Crimping tool\n2. Cutting Machine"]
[11,"Group O",11,54015892,"ASSEMBLY; TYPE: BLADE SET, APPLICATION: SWITCH, TRACK, 25 KVAC; DRAWING NO: BBD 7601, LA",16,"BBD 7601","1. Crimping tool\n2. Cutting Machine"]
[12,"Group O",12,54005745,"MECHANISM; TYPE: OPEN/CLOSE OPERATION, APPLICATION: TRACK SWITCH;; DRAWING NO: CEE-TZ1-0121 SHEET 52; EQUIPMENT USED ON 5400000 5405902 TRACK 25 KV AC COMPLETE, WITHOUT OPERATING ROD.",24,"CEE-TZ1-0121 SHEET 52","1. Crimping tool\n2. Cutting Machine"]
[13,"Group O",13,54001392,"SWITCH, KNIFE; TYPE: TRISWITCH 4A, CURRENT RATING: 200 A, POTENTIAL RATING: 11 KVAC; TRISWITCH TYPE 4 A, LINEGEAR 2000; EQUIPMENT USED ON OHTE; DISCONNECT 3 PHASE GANG OPERATED; SWITCHING BY MEANS OF A INSULATED PORTABLE LINK STICK; TO QUOTED PARTNUMBER OR EQUAL; 3 POLE",16,null,"1. Crimping tool\n2. Cutting Machine"]
[{"$nulls":3},"Group P"]
[1,"Group P",1,"54001913","TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: CEE-TNB-0031; SPECIFICATION: BS 4429SANS 121 DATE 2000; EQUIPMENT USED ON: OHTE; DROP-FORGED; 110 MM TAKE-UP; M16 SCREWS.;EYE TO EYE.; COMPLETE WITH LOCKNUT; HOT DIPPED GALVANISED ",80," CEE-TNB-0031","1. Forging machine \n2. Tapping machine"]
[2,"Group P",2,54001937,"TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: CU-NI-SI; DRAWING NO: CEE-TN-0332; EQUIPMENT USED ON OHTE; TAKE-UP: 90 MM; FOR STAINLESS STEEL AND 75 MM; FOR CU-NI-SI.; QUOTED DRAWING FOR CU-NI-SI ONLY. ",80,"CEE-TN-0332","1. Forging machine \n2. Tapping machine"]
[3,"Group P",3,54001925,"TURNBUCKLE; TYPE: ADJUSTABLE, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: BBH 2962; SPECIFICATION: SANS 121 DATE 2000; EQUIPMENT USED ON OHTE; DROP-FORGED; 400 MM - 460 MM TAKE-UP; M24 SCREWS.; HOT DIPPED GALVANISED. ",80," CEE-TNB-0019","1. Forging machine \n2. Tapping machine"]
[4,"Group P",4,"54031523","TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: CEE-TNB-0079; SPECIFICATION: SANS 121 DATE 2000; DROP-FORGED; EYE AND EYE; 130 MM TAKE-UP; COMPLETE WITH ONE LOCKNUT; M20 SCREWS.; HOT DIPPED GALVANISED. ",80,"CEE-TNB-0079","1. Forging machine \n2. Tapping machine"]
[5,"Group P",5,54033659,"SPRING, HELICAL, EXTENSION; TYPE: TENSIONING, OUTSIDE DIAMETER: 120 MM, INSIDE DIAMETER: 80 MM, NUMBER OF TURNS: 17, SPRING MATERIAL: STEEL, MATERIAL SIZE: 20 MM; DRAWING NO: BBB 2902; EQUIPMENT USED ON OHTE; CONTACT AND CATENARY WIRE TENSIONING; FOR 25 KV AC LINES",48,"BBB 2902","1. Spring forming machine"]
[6,"Group P",6,54022544,"SPRING, HELICAL, EXTENSION; TYPE: TENSIONING, OUTSIDE DIAMETER: 285 MM, INSIDE DIAMETER: 225 MM, NUMBER OF TURNS: 9.5, SPRING MATERIAL: STEEL, MATERIAL SIZE: 30 MM; DRAWING NO: CEE-TNB-33; CEE-TNB-30; EQUIPMENT USED ON OHTE; CONTACT WIRE TENSIONING FOR 3 KV.DC. LINES",48,"CEE-TNB-33; \nCEE-TNB-30","1. Spring forming machine"]
[7,"Group P",7,54007226,"BOLT, U; THREAD DIAMETER: M12, THREAD SERIES: UNC, MATERIAL: STEEL, INSIDE DISTANCE BETWEEN SHANKS: 32 MM, THREAD LENGTH: 30 MM; DRAWING NO: CEE-TX-0089; SPECIFICATION: SANS 121 DATE 2000; EQUIPMENT USED ON OHTE; COMPLETE WITH NUTS ",80,"CEE-TX-0089","1. Bolt forming machine\n"]
[8,"Group P",8,54003014,"HOOK, SAFETY; TYPE: TOWER, MATERIAL: STEEL; DRAWING NO: CEE-TNB-0041, LA; EQUIPMENT USED ON OHTE",480,"CEE-TNB-0041","1. Forging machine \n2. Tapping machine"]
[9,"Group P",9,54001521,"FITTING; TYPE: CLEVIS TWISTED H, COMMERCIAL SIZE: AS PER DRAWING, MATERIAL: SPHEROIDAL GRAPHITE IRON; DRAWING NO: CEE-TNB-0060, LA; EQUIPMENT USED ON OHTE.",480,"CEE-TNB-0060","\n1. Cutting\n2. Drilling \n3.Tapping facilities"]
[{"$nulls":3},"Group Q"]
[1,"Group Q",1,54001217,"ARRESTER, ELECTRICAL; TYPE: SURGE, POTENTIAL PROTECTION LEVEL: 12 KVAC; SPECIFICATION: BBH 2339, LA; EQUIPMENT USED ON TRANSMISSION LINE 11 KV; COMPLETE WITH MOUNTING BRACKET POLYMER HOUSED",32,"BBH 2339","1. Fibre glass rod extrusion machine\n2. Polymer injection moulding machine\n"]
[2,"Group Q",2,54031940,"ARRESTER, ELECTRICAL; TYPE: SPARK GAP, POTENTIAL PROTECTION LEVEL: 450 V; DRAWING NO: BBB0906 LATEST; SPECIFICATION: BBB1616LATEST; MATERIAL NUMBER 54031940, COMPLETE ASSEMBLY WITH GAS FILLED ARRESTER. NOTE TO TENDERERS: MUST SUPPLY TEST CERTIFICATES FOR THE GAS ARRESTERS ON INSPECTION DATE",400,"BBB0906 \nBBB1616","1. Press\n2. CNC Machine"]
[3,"Group Q",3,54008798,"ARRESTER, ELECTRICAL; TYPE: SURGE OHTE, POTENTIAL PROTECTION LEVEL: 3 KVDC, CAPACITANCE: 4 UF; SPECIFICATION NUMBER: CEE.0115.86.",32,"CEE.0115.86","1. Fibre glass rod extrusion machine\n2. Polymer injection moulding machine\n"]
[4,"Group Q",4,"54001189","ARRESTER, ELECTRICAL; TYPE: SURGE, POTENTIAL PROTECTION LEVEL: 4.8 KVDC; SPECIFICATION: CEE-0240, LA; METAL OXIDE TYPE. PEDESTAL MOUNTED: WITH ADAPTER PLATE TO QUOTED DRAWING.",32,"CEE-0240","1. Fibre glass rod extrusion machine\n2. Polymer injection moulding machine\n"]
[5,"Group Q",5,54112409,"ASSEMBLY; TYPE: LIGHTNING ARRESTER, APPLICATION: TUBULAR CANTILEVER; DRAWING NO: BBB 2141, LA; STORES DESCRIPTION, ARCING HORNS LIGHTNING ARRESTER FOR 3KV DC ELECTRIFCATION. THE DEPOTS MUST CONFIRM PRIOR IF THEY REQUIRE FOR A TUBULAR OR RAIL MAST CANTILVER. ITEM 7, 8 & 12 CAN BE EXCLUDED BY THE SUPPLIER.",240,"BBB 2141","1. Clay mixer and grinder\n2. Machine to shape insulator\n3. Temperature controle industrial oven\n4. Glasing facilities."]
[{"$nulls":3},"Group R"]
[1,"Group R",1,54005215,"CLAMP; TYPE: SWIVEL CLAMP RETAINER, DIMENSIONS: AS PER DRAWING, MATERIAL: GRAPHITE IRON; DRAWING NO: -TND-025, 0; EQUIPMENT USED ON 5400000 5406100 5406102; CLIP; COMPLETE WITH M12 U-BOLT, NUTS AND WASHERS SUITABLE FOR 107 AND 161 MM SQ CONTACT WIRE SWIVEL CLIPS",1600,"CEE-TN - 360/LATEST, \nCEE-TND-025","1. Stamping machine\n2. Furnace"]
[2,"Group R",2,54033129,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN;  DRAWING NO: BBH1118, EQUIPMENT USED ON OHTE PISTOL GRIP TYPE 5  MM DIA. TO 20.5 MM DIA. USERS INTEREST FOR USE ON ALUMINIUM WIRE;3 U BOLTS",800," BBB1790","1. Drilling machine\n2. Cutting machine"]
[3,"Group R",3,54034095,"CLAMP; TYPE: DOUBLE SUSPENSION, DIMENSIONS: 800 MM2, MATERIAL: GALVANIZED STEEL; DRAWING NO: BBC 7533, 0; FEEDER AND DEER CATENARY",2400,"BBC 7533","1. Drilling machine\n2. Cutting machine"]
[4,"Group R",4,54004764,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; CATENARY WIRE FOR 80 - 160 SQ MM, MIN DIA: 8 MM MAX DIA: 18 MM. STRANDED COPPER AND ALUMINIUM CONDUCTORS; 3 U BOLTS",2400,"As per description","1. Drilling machine\n2. Cutting machine"]
[5,"Group R",5,54009933,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; DRAWING NO: CEE-TZ-9/43, 0; EQUIPMENT USED ON OHTE HOOK CONNECTION. 42 MM TUBE DIAMETER",960," CEE-TZ-9/43,","1. Drilling machine\n2. Cutting machine"]
[6,"Group R",6,54010496,"ASSEMBLY; TYPE: CLAMP, APPLICATION: EARTH WIRE; DRAWING NO: CEE-TN-0371, LA; CLAMP USED ON 160MM2 ALUMINIUM CONDUCTOR",1600,"CEE-TN-0371","1. Drilling machine\n2. Cutting machine"]
[7,"Group R",7,54004917,"CLAMP, CABLE, ELECTRICAL CONNECTOR; TYPE: DOUBLE SUSPENSION, CABLE SIZE: 80 TO 250 MM2; DRAWING NO: CEE-TNB-0074, LA; STORES DESCRIPTION: DOUBLE SUSPENSION CLAMP FROM BOTH 80 TO 250 MM2 AND 500 TO 800 MM2; FEEDER CONDUCTORS",1600,"CEE-TNB-0074","1. Drilling machine\n2. Cutting machine"]
[8,"Group R",8,54021980,"CLAMP, CABLE, ELECTRICAL CONNECTOR; TYPE: SINGLE SUSPENSION, CLAMP MATERIAL: SPHEROIDAL GRAPHITE IRON, CABLE SIZE: 500 TO 800 MM2; DRAWING NO: CEE-TNB-0091 SHEET 1-6, LA; ITEM USED FOR STRANDED ALUMINIUM FEEDER WIRE",1600,"CEE-TNB-0091, Sht 1-6","1. Drilling machine\n2. Cutting machine"]
[9,"Group R",9,54033522,"CLAMP, ELECTRICAL; CLAMP TYPE: PARALLEL, POTENTIAL RATING: 25 KV, CLAMP MATERIAL: ALUMINIUM GRADE 6063, FURNISHED ITEMS: INSERT COPPER; DRAWING NO: BBB4186, 3; BBB4185, 3; USED ON OHTE WITH \"SKUNK\" CATENARY; 100 MM2 ACSR TO 160 MM2 COPPER; WITH A PERMANENT FORGED COPPER INSERT",960,"BBB4186, 3; BBB4185","1. Stamping machine\n2. Machine for serations\n3. Forging Machine"]
[10,"Group R",10,54009893,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; DRAWING NO: CEE-TZ-9/39, 0; EQUIPMENT USED ON OHTE HOOK JOINT FOR 31 TO 34 MM DIAMETER TUBE",960,"CEE-TZ-9/39","1. Drilling machine\n2. Cutting machine"]
[11,"Group R",11,54006299,"CLAMP; TYPE: GUIDE, COUNTERWEIGHT, DIMENSIONS: AS PER DRAWING, MATERIAL: STEEL , SSE-208301, H500110-3-133-E-DE-0099",160,"SSE-208301, \nH500110-3-133-E-DE-0099","1. Stamping machine\n2. Machine for serations\n3. Forging Machine"]
[12,"Group R",12,54000199,"CLAMP, ELECTRICAL; CLAMP TYPE: CLIP SWIVEL, POTENTIAL RATING: 50 KV, OVERALL LENGTH: 107 MM; CONTACT WIRE; OVERHEAD TRACK; VICTORY ELECTRICAL CAPE TOWN SSE TN208200; SALDANHA",480,"SSE TN208200","1. Stamping machine\n2. Furnace"]