{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["SANBI-COMPL"],"read":"whole","date_system":"1900"}

{"sheet":"SANBI-COMPL","index":0,"n_rows":630,"n_cols":17,"rows_kept":630}
[null,null,"SANBI-COMPL","19/11/2025","07:57:42",".","3.5.4.1"]
[null,null,"Completion of Kwelera National Botanical Gardens Phase 1b"]
["COUNTER","ISC","SECTION","BILL","PAGE NO","ITEM NO","DOC REF","PAY REF","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT","LABOUR INTENSIVE","WORDING","EDIT DATE"]
[1,12063,1,1,"1","","1","","BILL No. 1 ","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[2,12064,1,1,"1","","1","","PRELIMINARIES","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[3,12065,1,1,"1","","1","","MEANING OF TERMS \"TENDER/TENDERER\"","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[4,12066,1,1,"1","","1","","Any reference to the words \"Tender\" or \"Tenderer\" herein and/or in any other documentation shall be construed to have the same meaning as the words \"Bid\" or \"Bidder\"","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[5,12067,1,1,"1","","1","","PRELIMINARIES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[6,12068,1,1,"1","","1","","The JBCC Series 2000 Principal Building Agreement (July 2007 edition 5.0 - reprint 1) prepared by the Joint Building Contract Committee shall be the applicable building agreement, amended as hereinafter described.  The JBCC Principal Building Agreement Contract Data EC and the JBCC Principal Building Agreement Contract Data CE form an integral part of this Agreement.  The ASAQS Preliminaries (November 2007 edition) published by the Association of South African Quantity Surveyors for use with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these Bills of Quantities.  Contractors are referred to the above mentioned documents for the full intent and meaning of each clause thereof.  These clauses are referred to by number and heading only. Where standard clauses or options are not entirely applicable to this agreement such modifications, corrections or supplements as will apply are given under each relevant clause and such modifications, corrections or supplements shall take precedence notwithstanding anything contrary contained in the above mentioned documents.  Where an item is not relevant to this specific agreement such item is marked. \"N/A\" signifying \"Not Applicable\".","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[7,12069,1,1,"2","","2","","PREAMBLES FOR TRADES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[8,12070,1,1,"2","","2","","The Model Preambles for Trades (2008 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these Bills of Quantities and no claims arising from brevity of description of items fully described in the Model Preambles will be entertained.  Supplementary preambles are incorporated in these Bills of Quantities to satisfy the requirements of this project.  Such supplementary preambles shall take precedence over the provisions of the said Model Preambles.  The Contractor's prices for all items throughout these Bills of Quantities must take account of and include for all of the obligations, requirements and specifications given in the said Model Preambles and in any supplementary preambles.  Additionally, the Department of Public Works Construction Work Specification (PW371 A-B) is to apply.","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[9,12071,1,1,"2","","2","","PRICING OF PRELIMINARIES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[10,12072,1,1,"2","","2","","Should the Contractor select Option A in terms of sub-clause 3.2.1 in the Contract Data - Contractor to Employer (CE) for the purpose of adjustment of these Preliminaries, the amount entered into the amount column in these Preliminaries is to be divided into one or more of the three categories provided namely Fixed, Value Related or Time Related and the respective amounts entered in the spaces provided under each item","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[11,12073,1,1,"2","","2","","Items not priced in these Preliminaries shall be deemed to be included elsewhere in these Bills of Quantities","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[12,12074,1,1,"2","","2","","SECTION A: JBCC PRINCIPAL BUILDING AGREEMENT","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[13,12075,1,1,"2","","2","","DEFINITIONS","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:56",""]
[14,12076,1,1,"2","1","2.1","","A1\tDEFINITIONS AND INTERPRETATIONClause 1.0                                                                                                   Clause 1.1 Definition of \"Commencement Date\" is added:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[15,12077,1,1,"2","","2","","\"Commencement Date\" means the date that the Agreement, made in terms of the Form of Offer and Acceptance, comes into effect","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[16,12078,1,1,"2","","2","","Clause 1.1 Definition of \"Construction Period\" is amended by replacing it with the following:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[17,12079,1,1,"2","","2","","\"Construction Period\" means the period commencing on the commencement date and ending on the date of Practical Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[18,12080,1,1,"3","","3","","“Interest” means the interest rates applicable on this contract, whether specifically indicated in the relevant clauses or not, will be in terms of the legislation of the Republic of South Africa, and in particular:  (a) in respect of interest owed by the Employer, the interest rate as determined by the Minister of Justice and constitutional Development, from time to time, in terms of section 1 (2) of the Prescribed Rate of Interest Act, 1975 (Act No. 55 of 1975), will apply, and  (b) in respect of interest owed to the Employer, the interest rate as determined by the Minister of Finance, from time to time, in terms of section 80 (1) (b) of the Public Finance Management Act, 1999 (Act No. 1 of 1999), will apply","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[19,12081,1,1,"3","","3","","No clause  Fixed:________ Value related:_________ Time related:_______","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:17:57",""]
[20,12082,1,1,"3","","3","","OBJECTIVE AND PREPARATION","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[21,12083,1,1,"3","2","3.2","","A2\tOFFER, ACCEPTANCE AND PERFORMANCE OBLIGATIONS  Clause 2.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:17:57",""]
[22,12084,1,1,"3","3","3.3","","A3\tDOCUMENTS \tClause 3.0Clause 3.7 is amended by the addition of the following:  The Contractor shall supply and keep a copy of the JBCC Series 2000 Principal Building Agreement and Preliminaries applicable to this contract on the site, to which the Employer, Principal Agent and agents shall have access at all timesFixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:17:57",""]
[23,12085,1,1,"3","4","3.4","","A4\tDESIGN RESPONSIBILITY \tClause 4.0 Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:17:57",""]
[24,12086,1,1,"3","5","3.5","","A5\tEMPLOYER’S AGENTS Clause 5.0 Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:17:57",""]
[25,12087,1,1,"4","6","4.6","","A6\tSITE REPRESENTATIVE Clause 6.0 Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:49:31",""]
[26,12088,1,1,"4","7","4.7","","A7\tCOMPLIANCE WITH LAWS AND REGULATIONS Clause 7.0 Note: Without limiting the generality of the provisions of clause 7.0, the Contractor's attention is drawn to the provisions of the Construction Regulations, 2014 issued in terms of the Occupational Health and Safety Act, 1993.  It is specifically stated that the Employer shall prepare a documented site specific health and safety specification for the works and that the Employer shall ensure that the Contractor has made provision for the cost of health and safety measures during the execution of the works.  The Contractor shall price opposite this item for compliance with the act and the regulations and the reasonable provisions of the aforementioned health and safety specificationsFixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:49:27",""]
[27,12089,1,1,"4","8","4.8","","A8\tWORKS RISK Clause 8.0 Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:49:46",""]
[28,12090,1,1,"4","9","4.9","","A9\tINDEMNITIES Clause 9.0 Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:50:01",""]
[29,12091,1,1,"4","10","4.10","","A10\tGENERAL INSURANCES Clause 10.0 Clause 10.0 is amended by the addition of the following clauses:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:57",""]
[30,12092,1,1,"4","","4","","10.5 Damage to the Works  (a) \tWithout in any way limiting the Contractor’s obligations in terms of the contract, the Contractor shall bear the full risk of damage to and/or destruction of the works by whatever cause during construction of the works and hereby indemnifies and holds harmless the Employer against any such damage. The Contractor shall take such precautions and security measures and other steps for the protection and security of the works as the Contractor may deem necessary","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[31,12093,1,1,"5","","5","","(b)\tThe Contractor shall at all times proceed immediately to remove or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[32,12094,1,1,"5","","5","","(c)\tThe Employer shall carry the risk of damage to or destruction of the works and material paid for by the Employer that is the result of the excepted risks as set out in 10.6","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[33,12095,1,1,"5","","5","","(d)\tWhere the Employer bears the risk in terms of this contract, the Contractor shall, if requested to do so, reinstate any damage or destroyed portions of the works and the costs of such reinstatement shall be measured and valued in terms of 32.0 hereof","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[34,12096,1,1,"5","","5","","10.6 Injury to Persons or loss of or damage to Properties  (a)\tThe Contractor shall be liable for and hereby indemnifies the Employer against any liability, loss, claim or proceeding whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever arising out of or in the course of or caused by the execution of the works unless due to any act or neglect of any person for whose actions the Employer is legally liable","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[35,12097,1,1,"5","","5","","(b)\tThe Contractor shall be liable for and hereby indemnifies the Employer against any liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the Employer or any other body or person, arising out of or in the course of or by reason of the execution of the works unless due to any act or neglect of any person for whose actions the Employer is legally liable","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[36,12098,1,1,"5","","5","","(c)\tThe Contractor shall, upon receiving a contract instruction from the Principal Agent, cause the same to be made good in a perfect and workmanlike manner at his own cost and in default thereof the Employer shall be entitled to cause it to be made good and to recover the cost thereof from the Contractor or to deduct the same from amounts due to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[37,12099,1,1,"5","","5","","(d)\tThe Contractor shall be responsible for the protection and safety of such portions of the premises placed under his control by the Employer for the purpose of executing the works until the issue of the Certificate of Practical Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[38,12100,1,1,"5","","5","","(e)\tWhere the execution of the works involves the risk of removal of or interference with support to adjoining properties including land or structures or any structures to be altered or added to, the Contractor shall obtain adequate insurance and will remain adequately insured or insured to the specific limit stated in the contract against the death of or injury to persons or damage to such property consequent on such removal or interference with the support until such portion of the works has been completed","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[39,12101,1,1,"6","","6","","(f)\tThe Contractor shall at all times proceed immediately at his own cost to remove or dispose of any debris and to rebuild, restore, replace and/or repair such property and to execute the works","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[40,12102,1,1,"6","","6","","10.7 High risk insurance In the event of the project being executed in a geological area classified as a “High Risk Area”, that is an area which is subject to highly unstable subsurface conditions that might result in catastrophic ground movement evident by sinkhole or doline formation the following will apply:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[41,12103,1,1,"6","","6","","10.7.1 Damage to the works  The Contractor shall, from the commencement date of the works until the date of Practical Completion, bear the full risk of and hereby indemnifies and holds harmless the Employer against any damage to and/or destruction of the works consequent upon a catastrophic ground movement as mentioned above. The Contractor shall take such precautions and security measures and other steps for the protection of the works as he may deem necessary","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[42,12104,1,1,"6","","6","","When so instructed to do so by the Principal Agent, the Contractor shall proceed immediately to remove and/or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works, at the Contractor's own costs","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[43,12105,1,1,"6","","6","","10.7.2 Injury to persons or loss of or damage to property  The Contractor shall be liable for and hereby indemnifies and holds harmless the Employer against any liability, loss, claim or proceeding arising at any time during the period of the contract whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever resulting from, arising out of or caused by a catastrophic ground movement as mentioned above","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[44,12106,1,1,"6","","6","","The Contractor shall be liable for and hereby indemnifies the Employer against any and all liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the Employer or any other body or person whomsoever arising out of or caused by a catastrophic ground movement, as mentioned above, which occurred during the period of the contract","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[45,12107,1,1,"6","","6","","10.7.3 It is the responsibility of the Contractor to ensure that he has adequate insurance to cover his risk and liability as mentioned in 10.7.1 and 10.7.2. Without limiting the Contractor’s obligations in terms of the contract, the Contractor shall, within twenty-one (21) calendar days of the commencement date but before commencement of the works, submit to the Employer proof of such insurance policy, if requested to do so","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:58",""]
[46,12108,1,1,"7","","7","","10.7.4 The Employer shall be entitled to recover any and all losses and/or damages of whatever nature suffered or incurred consequent upon the Contractor’s default of his obligations as set out in 10.7.1; 10.7.2 and 10.7.3. Such losses or damages may be recovered from the Contractor or by deducting the same from any amounts still due under this contract or under any other contract presently or hereafter existing between the Employer and the Contractor and for this purpose all these contracts shall be considered one indivisible whole Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:50:39",""]
[47,12109,1,1,"7","11","7.11","","A11\tSPECIAL INSURANCES  Clause 11.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:50:46",""]
[48,12110,1,1,"7","12","7.12","","A12\tEFFECTING INSURANCES  Clause 12.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:50:58",""]
[49,12111,1,1,"7","13","7.13","","A13\tASSIGNMENT  Clause 13.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 02:51:09",""]
[50,12112,1,1,"7","14","7.14","","A14\tSECURITY  Clause 14.0  Clauses 14.1 - 14.9 are amended by replacing them with the following:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[51,12113,1,1,"7","","7","","14.1 In respect of contracts with a contract sum up to R1 million, the security to be submitted by the Contractor to the Employer will be as a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT)","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[52,12114,1,1,"7","","7","","14.1.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[53,12115,1,1,"7","","7","","14.1.2 The Employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0 provided that the Employer complies with the provisions of 33.4 in which event the Employer’s entitlement shall take precedence over his obligations to refund the payment reduction security or portions thereof to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[54,12116,1,1,"8","","8","","14.2 In respect of contracts with a contract sum above R1 million, the Contractor shall have the right to select the security to be provided in terms of 14.3, 14.4, 14.5, 14.6, or 14.7 as stated in the schedule. Such security shall be provided to the Employer within twenty-one (21) calendar days from commencement date. Should the Contractor fail to select the security to be provided or should the Contractor fail to provide the Employer with the selected security within twenty-one (21) calendar days from commencement date, the security in terms of 14.7 shall be deemed to have been selected","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[55,12117,1,1,"8","","8","","14.3 Where security as a cash deposit of ten per cent (10%) of the contract sum (excluding VAT) has been selected:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[56,12118,1,1,"8","","8","","14.3.1 The Contractor shall furnish the Employer with a cash deposit equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[57,12119,1,1,"8","","8","","14.3.2 Within twenty-one (21) calendar days of the date of Practical Completion of the works, the Employer shall reduce the cash deposit to an amount equal to three per cent (3%) of the contract value (excluding VAT), and refund the balance to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[58,12120,1,1,"8","","8","","14.3.3 Within twenty-one (21) calendar days of the date of Final Completion of the works, the Employer shall reduce the cash deposit to an amount equal to one per cent (1%) of the contract value (excluding VAT) and refund the balance to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[59,12121,1,1,"8","","8","","14.3.4 On the date of payment of the amount in the final payment certificate, the Employer shall refund the remainder of the cash deposit to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[60,12122,1,1,"8","","8","","14.3.5 The Employer shall be entitled to recover expense and loss from the cash deposit in terms of 33.0, provided that the Employer complies with the provisions of 33.4 in which event the Employer’s entitlement shall take precedence over his obligations to refund the cash deposit security or portions thereof to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[61,12123,1,1,"8","","8","","14.3.6 The parties expressly agree that neither the Employer nor the Contractor shall be entitled to cede the rights to the deposit to any third party","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[62,12124,1,1,"8","","8","","14.4 Where security as a variable construction guarantee of ten percent (10%) of the contract sum (excluding VAT) has been selected:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[63,12125,1,1,"8","","8","","14.4.1 The Contractor shall furnish the Employer with an acceptable variable construction guarantee equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:17:59",""]
[64,12126,1,1,"8","","8","","14.4.2 The variable construction guarantee shall reduce and expire in terms of the Variable Construction Guarantee form included in the invitation to tender","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[65,12127,1,1,"8","","8","","14.4.3 The Employer shall return the variable construction guarantee to the Contractor within fourteen (14) calendar days of it expiring","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[66,12128,1,1,"9","","9","","14.4.4 Where the Employer has a right of recovery against the Contractor in terms of 33.0, the Employer shall issue a written demand in terms of the variable construction guarantee","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[67,12129,1,1,"9","","9","","14.5 Where security as a fixed construction guarantee of five per cent (5%) of the contract sum (excluding VAT) and a five per cent (5%) payment reduction of the value certified in the payment certificate (excluding VAT) has been selected:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[68,12130,1,1,"9","","9","","14.5.1 The Contractor shall furnish a fixed construction guarantee to the Employer equal in value to five per cent (5%) of the contract sum (excluding VAT)","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[69,12131,1,1,"9","","9","","14.5.2 The fixed construction guarantee shall come into force on the date of issue and shall expire on the date of Practical Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[70,12132,1,1,"9","","9","","14.5.3 The Employer shall return the fixed construction guarantee to the Contractor within fourteen (14) calendar days of it expiring","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[71,12133,1,1,"9","","9","","14.5.4 The payment reduction of the value certified in a payment certificate shall be in terms of 31.8 (A) and 34.8","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[72,12134,1,1,"9","","9","","14.5.5 Where the Employer has a right of recovery against the Contractor in terms of 33.0, the Employer shall be entitled to issue a written demand in terms of the fixed construction guarantee or may recover from the payment reduction or may do both","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[73,12135,1,1,"9","","9","","14.6 Where security as a cash deposit of five per cent (5%) of the contract sum (excluding VAT) and a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT) has been selected:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[74,12136,1,1,"9","","9","","14.6.1 The Contractor shall furnish the Employer with a cash deposit equal in value to five per cent (5%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[75,12137,1,1,"9","","9","","14.6.2 Within twenty-one (21) calendar days of the date of Practical Completion of the works, the Employer shall refund the cash deposit in total to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[76,12138,1,1,"9","","9","","14.6.3 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[77,12139,1,1,"9","","9","","14.6.4 Where the Employer has a right of recovery against the Contractor in terms of 33.0, the Employer may issue a written notice in terms of 33.4 or may recover from the payment reduction or may do both","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[78,12140,1,1,"9","","9","","14.7 Where security as a payment reduction of ten per cent (10%) of the value certified in the payment certificate (excluding VAT) has been selected:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[79,12141,1,1,"9","","9","","14.7.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(B)","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[80,12142,1,1,"10","","10","","14.7.2 The Employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0, provided that the Employer complies with the provisions of 33.4 in which event the Employer’s entitlement shall take precedence over his obligations to refund the payment reduction or portions thereof to the Contractor","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[81,12143,1,1,"10","","10","","14.8 Payments made by the Guarantor to the Employer in terms of the fixed or variable construction guarantee shall not prejudice the rights of the Employer or Contractor in terms of this Agreement","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:00",""]
[82,12144,1,1,"10","","10","","14.9 Should the Contractor fail to furnish the security in terms of 14.2, the Employer, in his sole discretion and without notification to the Contractor, is entitled to change the Contractor’s selected form of security to that of a ten per cent (10%) payment reduction of the value certified in the payment certificate (excluding VAT), where after 14.7 shall be applicable  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:48:10",""]
[83,12145,1,1,"10","","10","","EXECUTION","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[84,12146,1,1,"10","15","10.15","","A15\tPREPARATION FOR AND EXECUTION OF THE WORKS  Clause 15.0","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[85,12147,1,1,"10","","10","","Clause 15.1 is amended by the addition of the following clause:  15.1.4 An acceptable Health and Safety Plan, required in terms of the Occupational Health and Safety Act, 1993 (Act 85 of 1993), within twenty-one (21) calendar days of commencement date","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[86,12148,1,1,"10","","10","","Clause 15.2.1 is amended by replacing it with the following clause:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[87,12149,1,1,"10","","10","","Give the Contractor possession of the site within ten (10) working days of the Contractor complying with the terms of 15.1.2 and 15.1.4  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:48:32",""]
[88,12151,1,1,"10","16","10.16","","A16\tSITE AND ACCESS Clause 16.0Fixed:________ Value related:_________ Time related:_________","N/A",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[89,12152,1,1,"10","17","11.17","","A17\tCONTRACT INSTRUCTIONS  Clause 17.0  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:48:45",""]
[90,12153,1,1,"11","18","11.18","","A18\tSETTING OUT OF THE WORKS  Clause 18.0  The Contractor shall notify the Principal Agent if any encroachments of adjoining foundations, building, structures, pavements, boundaries, etc. exist in order that the necessary arrangements may be made for the rectification of any such encroachments [18.1]  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:48:58",""]
[91,12154,1,1,"11","19","11.19","","A19\tTEMPORARY WORKS AND PLANT  Clause 19.0  \tClause 19.1.1 - Enclosure of the works \tClause 19.1.2 - Office accommodation \tClause 19.2 - Advertising rights and notice boards \t Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 03:07:37",""]
[92,12155,1,1,"11","20","11.20","","A20\tNOMINATED SUB-CONTRACTORS  Refer to the provisions on general attendance hereinafter\t  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:01",""]
[93,12156,1,1,"11","21","11.21","","A21\tSELECTED SUB-CONTRACTORS  General attendance of Selected Sub-contractors for pricing by the Contractor shall be in accordance with the Selected Sub-contractors' agreement. Notwithstanding this provision, general attendance shall be deemed to include for the Contractor to provide free of charge to any Selected Sub-contractor such scaffolding as may reasonably be required by such Selected Sub-contractor for the execution of the relevant sub-contract work  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:01",""]
[94,12157,1,1,"11","22","11.22","","A22\tEMPLOYER’S DIRECT CONTRACTORS  Clause 22.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:01",""]
[95,12158,1,1,"11","23","12.23","","A23\tCONTRACTOR'S DOMESTIC SUB-CONTRACTORS  Clause 23.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:01",""]
[96,12159,1,1,"12","","12","","COMPLETION","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:01",""]
[97,12160,1,1,"12","24","12.24","","A24\tPRACTICAL COMPLETION  Clause 24.0  Clause 24 is hereby amended by the addition of the following clause:  24.11 Should the Contractor, in the opinion of the Principal Agent, not have achieved Practical Completion of any area of the works, the Employer may, not withstanding the Contractor's ongoing responsibilities, take possession of any such area and such possession by the Employer shall not be construed as the achievement of Practical Completion. Should such an instance arise, the Principal Agent will give notice to the Contractor, in writing, that the Employer is taking immediate possession without Practical Completion having been achieved in order to mitigate his exposure to any expenses. The Contractor's responsibilities and liabilities shall remain in full force and effect until, in the opinion of the Principal Agent, Practical Completion has been achieved.  Access by the Contractor to any such area in possession of the Employer, prior to the Contractor's achievement of Practical Completion, shall be at the Employer's convenience, which will not be unreasonably withheld  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:01",""]
[98,12161,1,1,"12","25","12.25","","A25\tWORKS COMPLETION  Clause 25.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:02",""]
[99,12162,1,1,"12","26","12.26","","A26\tFINAL COMPLETION  Clause 26.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:02",""]
[100,12163,1,1,"12","27","12.27","","A27\tLATENT DEFECTS LIABILITY PERIOD  Clause 27.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:02",""]
[101,12165,1,1,"12","28","10.16","","A28\tSECTIONAL COMPLETION  Clause 28.0  Fixed:________ Value related:_________ Time related:_________","N/A",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[102,12166,1,1,"13","29","13.29","","A29\tREVISION OF DATE FOR PRACTICAL COMPLETION  Clause 29.0  The removal and replacement of materials and/or workmanship which do not conform to specification or the contract drawings shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value (Clause 29.3)  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:02",""]
[103,12167,1,1,"13","30","13.30","","A30\tPENALTY FOR LATE OR NON-COMPLETION  Clause 30.0 - Refer to C1.2: Contract Data for penalty details  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:02",""]
[104,12168,1,1,"13","","13","","PAYMENT","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[105,12169,1,1,"13","31","13.31","","A31\tINTERIM PAYMENT TO THE CONTRACTOR  Clause 31.0  The inclusion of materials and goods stored off site in the amount authorised for payment in terms of clause 31.4 shall be at the sole discretion of the Principal Agent and such inclusion shall only be considered upon the provision, by the Contractor, of an approved guarantee issued by a registered commercial bank","CONT",{"v":0,"d":"0.00"},"","","","","20/10/2025 12:18:02",""]
[106,12170,1,1,"13","","13","","Clause 31.8 is amended by replacing it with the following two alternative clauses:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[107,12171,1,1,"13","","13","","Alternative A  31.8(A) Where a security is selected in terms of 14.1; 14.5 or 14.6, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[108,12172,1,1,"13","","13","","31.8(A).1 Ninety-five per cent (95%) of such value in interim payment certificates issued up to the date of Practical Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[109,12173,1,1,"13","","13","","31.8(A).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of Practical Completion and up to but excluding the date of Final Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[110,12174,1,1,"13","","14","","31.8(A).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of Final Completion and up to but excluding the final payment certificate in terms of 34.6","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[111,12175,1,1,"13","","14","","31.8(A).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the Employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[112,12176,1,1,"14","","14","","Alternative B","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:02",""]
[113,12177,1,1,"14","","14","","31.8(B) Where security is a payment reduction in terms of 14.7 the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[114,12178,1,1,"14","","14","","31.8(B).1 Ninety per cent (90%) of such value in interim payment certificates issued up to the date of Practical Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[115,12179,1,1,"14","","14","","31.8(B).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of Practical Completion and up to but excluding the date of Final Completion","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[116,12180,1,1,"14","","14","","31.8(B).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of Final Completion and up to but excluding the final payment certificate in terms of 34.6","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[117,12181,1,1,"14","","14","","31.8(B).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the Employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[118,12182,1,1,"14","","14","","Clause 31.9 is amended by replacing the following:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[119,12183,1,1,"14","","14","","Replace seven (7) calendar days with thirty (30) calendar days  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[120,12184,1,1,"14","32","14.32","","A32\tADJUSTMENT TO THE CONTRACT VALUE  Clause 32.0  Where prices are submitted by the Contractor or Nominated/Selected Sub-contractors during the process of the works, in respect of contract instructions or in regard to a claim under the terms of the contract and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the Principal Agent wish to accept any such prices prior to the issue of the Certificate of Final Completion, it shall be in writing  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[121,12185,1,1,"15","33","15.33","","A33\tRECOVERY OF EXPENSE AND LOSS  Clause 33.0  33.2.9 the Contractor's failure or neglect to commence with the works on the dates prescribed in the contract  33.2.10 the Contractor's failure or neglect to proceed with the works in terms of the contract  33.2.11 the Contractor's failure or neglect for any reason to complete the works in accordance with the contract  33.2.12 the Contractor's refusal or neglect to comply strictly with any of the conditions of contract or any contract instructions and/or orders in writing given in terms of the contract  33.2.13 the Contractor's estate being sequestrated, liquidated or surrendered in terms of the insolvency laws in force within the Republic of South Africa  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[122,12186,1,1,"15","34","15.34","","A34 \tFINAL ACCOUNT AND FINAL PAYMENT  Clause 34.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[123,12187,1,1,"15","35","15.35","","A35\tPAYMENT TO OTHER PARTIES  Clause 35.0  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[124,12188,1,1,"15","","15","","TERMINATION","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[125,12189,1,1,"15","","15","","A36\tTERMINATION BY EMPLOYER - CONTRACTOR’S DEFAULT  Clause 36.0","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[126,12190,1,1,"15","","15","","36.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the Employer or the Contractor; or for any reason whatsoever, the Contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The Contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[127,12191,1,1,"15","36","15.36","","A37\tCANCELLATION BY EMPLOYER - LOSS AND DAMAGE  Clause 37.0","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[128,12192,1,1,"16","","16","","Clause 37.0 is amended by the addition of the following clause:  37.5 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the Employer or the Contractor; or for any reason whatsoever, the Contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The Contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:03",""]
[129,12193,1,1,"16","37","16.37","","A38\tTERMINATION BY CONTRACTOR - EMPLOYER’S DEFAULT  Clause 38.0  Clause 38.0 is amended by the addition of the following clause:","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:03",""]
[130,12194,1,1,"16","","16","","38.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the Employer or the Contractor; or for any reason whatsoever, the Contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The Contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[131,12195,1,1,"16","38","16.38","","A39\tTERMINATION - CESSATION OF THE WORKS  Clause 39.0  Fixed:________ Value related:_________ Time related:_________ ","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[132,12196,1,1,"16","39","16.39","","A40\tSETTLEMENT OF DISPUTESClause 40.0 \tFixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[133,12197,1,1,"16","","16","","CONTRACT VARIABLES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:04",""]
[134,12198,1,1,"16","40","16.40","","A41\tPOST TENDER PROVISIONS  Clause 41.0  The Contractor is to complete before submission of his tender the JBCC Principal Building Agreement Contract Data CE  Tenderers are referred to C1.2: Contract Data for variables pertaining to this contract  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[135,12199,1,1,"17","41","17.41","","A42\tCONTRACTUAL AGREEMENT  Clause 42.0  The required information of the contracting parties and the amount of the accepted contract sum shall be inserted in the agreement for signature of the agreement by the parties  Tenderers are referred to C1.2: Contract Data for variables pertaining to this contract  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[136,12201,1,1,"17","","18","","SECTION B: JBCC PRELIMINARIES","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:04",""]
[137,12202,1,1,"17","","18","","B1.0  DEFINITIONS AND INTERPRETATION","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:04",""]
[138,12203,1,1,"17","42","18.42","","B1.1  Definitions and interpretation  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[139,12204,1,1,"17","","18","","B2.0  DOCUMENTS","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:04",""]
[140,12205,1,1,"17","43","18.43","","B2.1  Checking of documents  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[141,12206,1,1,"17","44","18.44","","B2.2  Bills of Quantities  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[142,12207,1,1,"17","45","18.45","","B2.3  Availability of construction documentation  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[143,12208,1,1,"17","","18","","B3.0  PREVIOUS WORK AND ADJOINING PROPERTIES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:04",""]
[144,12209,1,1,"17","46","18.46","","B3.1  Previous work - dimensional accuracy  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:04",""]
[145,12210,1,1,"17","47","18.47","","B3.2  Previous work - defects  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[146,12211,1,1,"17","48","18.48","","B3.3 Inspection of adjoining property  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[147,12212,1,1,"18","49","18.49","","B2.5  Priced documents  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[148,12213,1,1,"18","50","18.50","","B2.6  Tender submission  Clause 2.6 is amended by replacing “JBCC Form of Tender” with C1.1: Form of Offer & Acceptance  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[149,12214,1,1,"18","","19","","B3.0  THE SITE","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:05",""]
[150,12215,1,1,"18","51","19.51","","B3.1  Defined works area  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[151,12216,1,1,"18","52","19.52","","B3.2  Geotechnical Investigation  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[152,12217,1,1,"18","53","19.53","","B3.3  Inspection of the site  A compulsory site briefing session will take place on site on 9 February 2021 at 10:00 at the Kwelera National Botanical Garden Offices (Farm No. 1505, Road DR02731, Kwelera)  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[153,12218,1,1,"18","","19","","B4.0  SAMPLES, SHOP DRAWINGS AND MANUFACTURERS' INSTRUCTIONS","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:05",""]
[154,12219,1,1,"18","54","19.54","","B4.1  Samples of materials  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[155,12220,1,1,"18","55","19.55","","B4.2  Workmanship samples  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[156,12221,1,1,"18","56","19.56","","B4.3  Shop drawings  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[157,12222,1,1,"18","57","19.57","","B4.4  Compliance with manufacturers' instructions  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[158,12223,1,1,"19","","19","","B5.0  DEPOSITS AND FEES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:05",""]
[159,12224,1,1,"19","58","19.58","","B5.1  Deposits and fees  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:05",""]
[160,12225,1,1,"19","","19","","B6.0  TEMPORARY SERVICES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:05",""]
[161,12226,1,1,"19","59","19.59","","B6.1  Water  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:49:43",""]
[162,12227,1,1,"19","60","19.60","","B6.2  Electricity  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:49:35",""]
[163,12228,1,1,"19","61","20.61","","B6.3  Telecommunication facilities  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:50:10",""]
[164,12229,1,1,"19","62","20.62","","B6.4  Ablution facilities  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:50:26",""]
[165,12230,1,1,"19","63","20.63","","B6.5  Main notice board Note that an additional EPWP type notice board will be required; refer to C3.1: Description of the Works.  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[166,12231,1,1,"19","","20","","B7.0  PRIME COST AMOUNTS","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:06",""]
[167,12232,1,1,"19","64","20.64","","B7.1  Responsibility for prime cost amounts  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[168,12233,1,1,"19","","20","","B8.0  SPECIAL ATTENDANCE ON SELECTED SUB-CONTRACTORS","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:06",""]
[169,12234,1,1,"19","65","20.65","","B8.1  Special attendance  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[170,12235,1,1,"19","","20","","B9.0  GENERAL","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:06",""]
[171,12236,1,1,"19","66","20.66","","B9.1  Protection of the works  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:50:42",""]
[172,12237,1,1,"20","67","20.67","","B9.2  Protection/isolation of existing/sectionally occupied works  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:50:56",""]
[173,12238,1,1,"20","68","20.68","","B9.3  Security of the works  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:51:12",""]
[174,12239,1,1,"20","69","20.69","","B9.4  Notice before covering work  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[175,12240,1,1,"20","70","20.70","","B9.5  Disturbance  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[176,12241,1,1,"20","71","20.71","","B9.6  Environmental disturbance  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:06",""]
[177,12242,1,1,"20","72","21.72","","B9.7  Works cleaning and clearing  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:51:30",""]
[178,12243,1,1,"20","73","21.73","","B9.8  Vermin  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:07",""]
[179,12244,1,1,"20","74","21.74","","B9.9  Overhand work  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:07",""]
[180,12245,1,1,"20","75","21.75","","B9.10  As-built information  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:51:44",""]
[181,12246,1,1,"20","","21","","B10.  SCHEDULE OF VARIABLES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[182,12247,1,1,"20","","21","","Information necessary for completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder. Where no information is given it shall mean that no specific requirements are expected or that the clause is not relevant to this contract.","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[183,12248,1,1,"20","","21","","10.1\tProvisional Bills of Quantities [2.2]\tThe quantities are provisional: No","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[184,12249,1,1,"20","","21","","10.2\tAvailability of construction documentation [2.3]\tConstruction of documentation is complete: Yes","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[185,12250,1,1,"20","","21","","10.3\tPrevious work - dimensional accuracy [3.1]\tDetails: Nil","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[186,12251,1,1,"21","","21","","10.4\tPrevious work - defects [3.2]\tDetails: To be checked on site by Contractor prior to commencing with building operations","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[187,12252,1,1,"21","","21","","10.5\tInspection of adjoining properties[3.3]\tSpecific requirements: The Contractor must inspect adjoining \tproperties and immediately bring to the notice of the Principal \tAgent of any consequences that may arise from the building works","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[188,12253,1,1,"21","","21","","10.6\tWater [7.2]\tOption A (by Contractor) (Yes)  \tOption B (by Employer - free of charge when available)\t(No)  \tOption C (by Employer- metered) (No)","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[189,12254,1,1,"21","","22","","10.7\tElectricity [7.3]\tOption A (by Contractor) (Yes)\t  \tOption B (by Employer - free of charge when available) (No)  \tOption C (by  Employer - metered) (No)","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[190,12255,1,1,"21","","22","","10.8\tTelecommunications [7.4]\tTelephone (by Contractor) (Yes)  \tFacsimile (by Contractor) (Yes)  \teMail (by Contractor) (Yes)","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[191,12256,1,1,"21","","22","","10.9\tAblution facilities [7.5]\tOption A (by Contractor) (Yes)     \t\t  \tOption B (by Employer) (No)","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:07",""]
[192,12257,1,1,"21","","22","","10.10\tProtection of works [9.1]\tSpecific requirements:\t  \tThe Contractor shall protect the works for the duration of the contract","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[193,12258,1,1,"21","","22","","10.11\tProtection of existing/sectionally occupied works [9.2]\tProtection is required No","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[194,12259,1,1,"21","","22","","10.12\tDisturbance [9.5]\tSpecific requirements:  \tThe Contractor shall keep the site, structures, etc. well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust screens all to the satisfaction of the Principal Agent","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[195,12260,1,1,"22","","22","","10.13\tEnvironmental disturbance[9.6]\tSpecific requirements: Protection of existing trees, shrubs and wetland areas is required. Details/Information will be made available at the compulsory site inspection meeting.","",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[196,12262,1,1,"23","","23","","SECTION C: SPECIFIC PRELIMINARIES","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[197,12263,1,1,"23","","23","","Section C contains specific Preliminaries items which apply to this contract except where N/A (Not Applicable) appears against an item","CONT",{"v":0,"d":"0.0"},"","","","","20/10/2025 12:18:08",""]
[198,12264,1,1,"23","76","23.76","","C1\tCONTRACT DRAWINGS  The drawings issued with the tender documents do not comprise the complete set but serve as a guide only for tendering purposes and for indicating the scope of the work to enable the Tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed  Should any part of the drawings not be clearly intelligible to the Tenderer he shall, before submitting his tender, obtain clarification in writing from the Principal Agent  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:08",""]
[199,12265,1,1,"23","77","23.77","","C2\tGENERAL PREAMBLES  The document “Specification of Materials and Methods to be used (PW371)” is obtainable on request from the head office and all regional offices of the Department of Public Works. This document shall be read in conjunction with the Bills of Quantities and be referred to for the full descriptions of work to be done and materials to be used  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:08",""]
[200,12266,1,1,"23","78","23.78","","C3\tTRADE NAMES  Wherever a trade name for any product has been described in the Bills of Quantities, the Tenderers' attention are drawn to the fact that any other product of equal quality may be used subject to the written approval of the Principal Agent being obtained prior to the closing date for submission of tenders  If prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:08",""]
[201,12267,1,1,"23","79","23.79","","C4\tIMPORTED MATERIALS AND EQUIPMENT  Where imported items are listed in the tender documents, the Tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency fluctuations.  Notwithstanding any provisions elsewhere regarding the adjustment of contract prices, the price of any item, material or equipment listed in terms of this clause shall be excluded from the Contract Price Adjustment Provisions  Fixed:________ Value related:_________ Time related:________","Item",{"v":1,"d":"1.00"},"","","","","20/10/2025 12:18:08",""]
[202,12271,1,1,"24","80","","","C5\tCLO ALLOWANCE  Any additional costs, etc. relating to the employment and payment of the CLO (CLO Allowance indicated in PROVISIONAL SUMS section of the Bills of Quantities), should be allowed for in this item (Clause C8).  Fixed:________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 03:08:18",""]
[203,12269,1,1,"24","81","29.14","","C6\tOCCUPATIONAL HEALTH AND SAFETY ACT  The Contractor shall comply with the requirements set out in the Construction Regulations, 2014 issued under the Occupational Health and Safety Act, 19093 (Act No. 85 of 1993), including COVID-19 Requirements as per Government Notice No. 479 dated 29 April 2020.  It is required of the Contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this section of the Bills of Quantities  The Contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.  In the event of partial or total non-compliance, the Principal Agent, notwithstanding the provisions of Clause A31 of the Preliminaries or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the Contractor provides satisfactory proof of compliance.  The Contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment  Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced hereunder and no additional claims in this regard shall be entertained  Fixed: _________ Value related:_________ Time related:_________","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:44:33",""]
[204,12270,1,1,"24","82","","","C7\tREPORTING BY CONTRACTOR  The Contractor is required to complete the CONTRACTOR MONTHLY REPORT, which is to be submitted together with the Contractor's payment claim. Payment of the Contractor is conditional on this information being accurate and timeously provided. Payment shall be subject to the Employer giving the Contractor a tax invoice for the amount due. The Contractor is to take note of the following requirements - At the bottom of the CONTRACTOR MONTHLY REPORT, the Contractor must sign the document as proof that the people indicated have worked the number of days.  Fixed:_______ Value related:_______ Time related:_______","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 01:43:14",""]
[206,11520,1,2,"27","","1","","BILL NO. 2 HEALTH AND SAFETY","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[207,11521,1,2,"27","","26","","MODEL PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[208,11522,1,2,"27","","26","","The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[209,11523,1,2,"27","","26","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[210,11525,1,2,"27","","26","","The contractor's prices for all items throughout these bills of quantities shall take account of and include where applicable for all of the obligations, requirements and specifications given in the General Preambles and in any supplementary preambles and/or specifications.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[211,11526,1,2,"27","","26","","Prior to pricing the principal contractor must familiarize him/herself with the Occupational Health and Safety Act No. 85 Of 1993, Construction Regulations 2014, other relevant Regulations and Standards as well as project specific Health & Safety specifications including any latest amendments.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[212,11527,1,2,"27","","26","","The items in this Bill do not contain quantities hence the Contractor must insert his own quantities based on his individual requirements to comply with the Health and Safety obligations and demands of the Occupational Health and Safety Act No. 85 of 1993, Construction Regulations 2014, other relevant Regulations and Standards as well as project specific Health & Safety Specifications.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[213,11529,1,2,"27","","27","","OCCUPATIONAL HEALTH AND SAFETY","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[214,11530,1,2,"27","","27","","General:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[215,11531,1,2,"27","1","27.1","","One full time Construction Health and Safety Officer or Manager (CHSO/M)  Full time attendance on site of a SACPCMP-registered CHSO/M from the start of construction until the end of project handover and provisions of telecommunications.","Item",{"v":1,"d":"1.00"},"","","","","23/10/2025 11:13:50",""]
[216,11532,1,2,"27","2","","","Provision for Health and Safety Management Plans and Primary Health and Safety file together with 3 times secondary files for each Residential Block","Item",{"v":1,"d":"1.00"},"","","","","22/10/2025 03:25:25",""]
[217,11533,1,2,"27","3","27.2","","Allow for the necessary Workman’s Compensation Fund or approved Insurer contributions for the duration of the project with and including renewals","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[218,11534,1,2,"28","4","27.3","","Medical certificates of fitness.  Medical examination of all employees and certification of fitness for Pre-employment is required.  Medical examination of all employees and certification of fitness for Exit-employment is required.  Allow for annual medicals for employees if the project duration is more than 12 months.","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[219,11535,1,2,"28","5","27.4","","Emergency Equipment based on the risk exposure and emergency rescue. stretchers, neck brace, first aid kits, fire fighting equipment.","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[220,11536,1,2,"28","6","27.5","","Competent inspectors for equipment such as examples scaffolding inspectors and lifting machine inspector.","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[221,11537,1,2,"28","7","","","Mandatory training such as risk assessments, legal liability/OHS Act, awareness, first aid incident investigation.","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[222,11538,1,2,"28","","27","","Provide, supply and maintenance for each worker the following SANS approved personal protective equipment & clothing as per the site-specific risk assessments:","H3",{"v":0,"d":"0.00"},"","","","","14/10/2025 09:26:42",""]
[223,11539,1,2,"28","8","27.10","","Hard hats (High density polyethylene with 6 point lining)","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[224,11540,1,2,"28","9","","","Overall/work suits (100% Cotton)","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[225,11541,1,2,"28","10","","","Reflective vests with visible marking of contractor and proof of induction","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[226,11542,1,2,"28","11","","","Safety boots/shoes (Steel-Toe)","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[227,11543,1,2,"28","12","","","Ear Plugs/Muffs","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[228,11544,1,2,"28","13","","","Dust Mask FFP2","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[229,11545,1,2,"28","14","","","Safety goggles","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[230,11546,1,2,"28","15","","","Safety gloves","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[231,11547,1,2,"28","16","","","Respirators","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[232,11548,1,2,"28","17","","","Safety harness","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[233,11549,1,2,"28","18","","","Permit board","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[234,11550,1,2,"28","19","","","Weight bearing barricading and hoarding","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[235,11551,1,2,"29","20","","","Personal fall arrest and rescue equipment with and including lifelines and associated equipment","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[236,11552,1,2,"29","21","","","Temporary handrails, toe boards other than for access to scaffolding","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[237,11553,1,2,"29","22","","","Construction information, warning signage, posters","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[238,11554,1,2,"29","23","","","Allow for fire extinguishers and fire fighting equipment","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[239,11555,1,2,"29","24","","","Safe lifting equipment for lifting and lowering pipes, lifting tackles and slings","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[240,11556,1,2,"29","25","","","Rubble shoot to be provided for the discarding of rubble from buildings into a rubble skip","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[241,11557,1,2,"29","26","","","Allow for provision of telecommunication facilities for the appointed OHS officer","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[242,11558,1,2,"29","27","","","Provide for appointment of responsible and competent person/s to manage and supervise the works and administer and enforce health and safety on site ","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[243,11559,1,2,"29","28","","","Allow for provision of Basic medical Preparedness and Response equipment & at least Level 2 First Aider/s","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[244,11560,1,2,"29","","28","","Environmental:","H3",{"v":0,"d":"0.00"},"","","","","14/10/2025 09:26:42",""]
[245,11561,1,2,"29","29","","","Dust control measure for the prevention of dust nuisance.  Buildings that are partial decanted.  Hoarding to be provided for dust control. Hoarding to extend into the ceiling of the buildings.","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[246,11562,1,2,"29","30","","","Provision for spill kits, drip trays","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[247,11563,1,2,"29","31","","","Housekeeping – provide for the waste bins, safe collection and disposal of waste material from site by an approved method (a) Air monitoring (b) Analysing Samples (c) Test on Workers","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[248,11564,1,2,"29","","28","","Disease Awareness Education:","H3",{"v":0,"d":"0.00"},"","","","","14/10/2025 09:26:42",""]
[249,11565,1,2,"29","32","","","Principal contractor's time related obligations in respect of the Disease Management","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[251,11612,1,3,"31","","","","BILL No. 3: ALTERATIONS (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:37:12",""]
[252,11617,1,3,"31","","36","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[253,11618,1,3,"31","","37","","General","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[254,11619,1,3,"31","","203","","All work described in this bill is to be to be executed in/on existing buildings and prices shall allow for this","",{"v":0,"d":"0.0"},"","","","","22/10/2025 04:34:06",""]
[255,11620,1,3,"31","","","","All Architectural and Engineering drawings and specifications to be read in conjunction and any discrepancies to be brought to the attention of the Principal Agent.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[256,11621,1,3,"31","","37","","Descriptions that include the text \".... take out/up/off/down and remove ......\" shall indicate that the Tenderer shall allow that these items/materials shall become his property and shall be removed from site, or dumped at a site of disposal that the Tenderer has identified. Descriptions that include the text \"...... make good .....\" shall indicate that the Tenderer shall allow for all associated costs of repairing disturbed finishes, costs of disconnecting/removing the items/materials and preparatory work to receive new items/materials.All costs associated with the above will be deemed to be included in the Tenderer's prices.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[257,11622,1,3,"31","","37","","The Contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants. He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the Principal Agent.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[258,11623,1,3,"31","","37","","Making good of finishes shall include making good of the brick and/or concrete surfaces onto which the new finishes are applied, where necessary","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[259,11624,1,3,"31","","37","","The Contractor will be required to take dimensions when fitting new items/elements to existing structures/frames, etc. as there may be some minor adjustments required and it shall be deemed that all prices shall include such minor adjustment work.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[260,12926,1,3,"32","","37","","Reference in the Bills of Quantities (in square brackets [X]) refer to the associated number on the drawings attached to the Bills of Quantities","",{"v":0,"d":"0.0"},"","","","","22/10/2025 04:37:38",""]
[261,11625,1,3,"32","","36","","Viewing of the site","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[262,11626,1,3,"32","","36","","Before submitting his tender, the Contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished. No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[263,11627,1,3,"32","","29","","Removal and disposal of harmful material","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[264,11629,1,3,"32","","29","","Tenderers are to note that some of the items to be removed, may contain harmful materials/elements:  The items that are measured in this section are described, where applicable, as \"asbestos\". However, it is the Tenderers' responsibility to assess and decide whether the items identified are all harmful asbestos materials/elements.  Should the Tenderers be of the opinion that the items listed are identified as possible harmful materials/elements and disposal thereof, the onus will be on them to assess the latter on site and define/establish and prices the respective items accordingly. It will be deemed that Tenderers' prices received have fully taken the above requirements into consideration and priced accordingly to allow for the correct procedure of removal and disposal thereof to a designated dumping site in terms of the latest legislation applicable.  No extra cost will be entertained should the Contractor establish at a later stage that some materials/elements are harmful and their pricing did not include for the additional cost applicable due to legislative requirements relating to removal and disposal thereof.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[265,11632,1,3,"32","","","","CLEANING OF EXISTING SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[266,11634,1,3,"32","1","","","Clean existing paving by pressure cleaning to remove all algae, discolourations, dirt, etc. [25]","m2",57,"","","","","23/10/2025 10:45:02",""]
[267,11637,1,3,"32","","","","GENERAL ALTERATIONS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[268,11638,1,3,"33","","151","","General repairs:","H3",{"v":0,"d":"0.0"},"","","","","22/10/2025 03:43:48",""]
[269,11972,1,3,"33","2","","","Take off 1000mm section of 110mm PVC pipe, replace with new including fittings to correct fall including holes in walls, etc. [10]","No",1,"","","","","23/10/2025 10:47:17",""]
[270,11973,1,3,"33","3","","","Refasten and service existing Pearl code 7300SC cistern including sealing around flushpipe [10]","No",1,"","","","","23/10/2025 10:47:22",""]
[271,11975,1,3,"33","4","","","Take out two ball bearing butt hinge to door and replace with new (elsewhere) [11]","No",3,"","","","","14/10/2025 03:18:29",""]
[272,11976,1,3,"33","5","","","Fit exiting sink mixer and waste connection, including connecting all services [14]","No",1,"","","","","22/10/2025 03:44:41",""]
[273,11977,1,3,"33","6","","","Take off existing pull handle make good door to receive new pull handle (elsewhere) [15]","No",1,"","","","","14/10/2025 03:25:33",""]
[274,11978,1,3,"33","7","","","Repair existing stone cladding and bond to wall [21]","m2",5,"","","","","14/10/2025 04:12:08",""]
[275,11979,1,3,"33","8","","","Replace cover (lid) on rainwater tank [23]","No",2,"","","","","14/10/2025 04:14:05",""]
[276,11980,1,3,"33","9","","","Fill cores/frogs at ends of projecting facebrick to match facebrick colour [29]","No",82,"","","","","14/10/2025 04:16:03",""]
[277,11981,1,3,"33","10","","","Fill and seal mitred facebrick joints with tinted mortar to match facebrick [58]","m",26,"","","","","14/10/2025 04:25:17",""]
[278,11652,1,3,"33","","153","","Take out and remove existing doors or door frames/linings and fanlights complete with thresholds:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[279,11956,1,3,"33","11","34.27","","Timber door size 600 x 2100mm high from steel lining [35]","No",3,"","","","","22/10/2025 03:48:56",""]
[280,11957,1,3,"33","12","34.28","","Timber door size 1200 x 2100mm high from steel lining [35]","No",2,"","","","","22/10/2025 03:49:25",""]
[281,11701,1,3,"33","","154","","Take down and remove existing roofs, ceilings, fascias, gutters, flashings, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[282,11702,1,3,"33","13","","","Profile sheet metal roof covering and accessories, including timber purlins [44]","m2",30,"","","","","22/10/2025 03:50:43",""]
[283,11708,1,3,"33","14","","","Suspended ceilings complete with grid, cornice, etc. [40]","m2",38,"","","","","14/10/2025 09:38:23",""]
[284,11938,1,3,"33","15","","","Fibre cement fascia including accessories [56]","m",15,"","","","","14/10/2025 09:42:52",""]
[285,11820,1,3,"33","","","","JOINT SEALANTS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[286,11823,1,3,"34","","","","Approved polysulphide sealing compound including backing cord, bond breaker, primer, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[287,11965,1,3,"34","16","78.9","","Polysulphide movement joint between tiles or between tiles and wall (Provisional) [2]","m",145,"","","","","14/10/2025 12:29:52",""]
[288,11967,1,3,"34","17","78.9","","Around windows, Shopfronts, etc[19]","m",371,"","","","","14/10/2025 12:37:37",""]
[289,11982,1,3,"34","","37","","REINSTATE EXISTING PAVING TO BUILDING ENTRANCES AND AROUND EXTERNAL FACADE","H2",{"v":0,"d":"0.0"},"","","","","17/10/2025 10:45:42",""]
[290,11983,1,3,"34","","","","lifting up:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 11:12:31",""]
[291,11984,1,3,"34","18","","","Lift up existing 75mm concrete pavers and set aside for reuse (elsewhere) [25]","m2",138,"","","","","17/10/2025 10:53:17",""]
[292,11990,1,3,"34","","107","LI","Earth filling supplied by the Contractor under walkways, etc.:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 11:00:19",""]
[293,11986,1,3,"34","19","107.58","","G9 Material in accordance with SANS 1200DM in 150mm layers compacted to a minimum of 93% Mod AASHTO dry density [25]","m3",28,"","","","","22/10/2025 04:33:02",""]
[294,11995,1,3,"34","","38","","Coarse river sand filling supplied by the contractor:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 11:09:12",""]
[295,11996,1,3,"34","20","38.16","","Under Paving, etc.[25]","m2",138,"","","","","22/10/2025 04:33:22",""]
[296,11988,1,3,"34","","31","","Soil insecticide in accordance with SANS 5859 (compliance certificate will be required after completion):","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 10:59:18",""]
[297,11989,1,3,"34","21","31.17","","Under surface beds or rafts, etc. including forming and poisoning shallow furrows against foundation walls, etc. filling in and ramming [25]","m2",138,"","","","","22/10/2025 04:33:40",""]
[298,11991,1,3,"34","","107","","203 x 102 x 70mm Thick paving blocks from the stockpile on site:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 11:03:38",""]
[299,11992,1,3,"34","22","107.61","","Paving laid in herringbone pattern to falls and slopes [25]","m2",138,"","","","","17/10/2025 11:22:06",""]
[300,11993,1,3,"34","","107","","Prescribed density tests on filling:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 11:05:42",""]
[301,11994,1,3,"34","23","107.60","","Modified AASHTO density test","No",4,"","","","","17/10/2025 11:19:36",""]
[303,1235,1,4,"36","","45","","BILL No. 4","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:37:59",""]
[304,1236,1,4,"36","","45","","ROOF COVERINGS, ETC.","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[305,5179,1,4,"36","","45","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[306,1237,1,4,"36","","45","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[307,12942,1,4,"36","","82","","Proprietary products in descriptions","H3",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:36:14",""]
[308,12943,1,4,"36","","68","","Reference to any particular trademark, name, patent, design, type, specific origin or producer is purely to establish a standard for requirements.  Products or articles of an equivalent standard may be substituted","",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:36:14",""]
[309,1238,1,4,"36","","45","","Straight cutting","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[310,1239,1,4,"36","","45","","Descriptions of all roof coverings are deemed to include for all straight cutting","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[311,5180,1,4,"36","","45","","PROFILED METAL SHEETING AND ACCESSORIES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[312,5181,1,4,"36","","45","","0,55mm Thick Saflok 410 Colorplus AZ200 or equivalent interlocking aluminium-zinc roof sheeting and accessories, fixed to timber purlins (elsewhere measured) at 1700mm centres with concealed fixing, pierce-fixing through each sheet under the flashings, cappings or along the top of the sheets (for low pitch roofs), all in accordance with the manufacturer's instructions:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[313,5182,1,4,"36","1","45.1","","Roof covering with pitch not exceeding 25 degrees [44]","m2",30,"","","","","22/10/2025 04:38:48",""]
[314,1337,1,4,"36","","46","","ROOF AND WALL INSULATION","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[315,1338,1,4,"36","","46","","Insulation R4 double sided reflective foil based insulation:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[316,1339,1,4,"36","2","46.9","","Laid taut over purlins (at approximately 1700mm centres) and fixed concurrent with roof covering, including taped laps and nylon straining wires [44]","m2",30,"","","","","22/10/2025 04:39:00",""]
[318,1360,1,5,"37","","48","","BILL No. 5","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:38:16",""]
[319,5225,1,5,"37","","48","","CARPENTRY & JOINERY","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[320,5226,1,5,"37","","48","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[321,5227,1,5,"37","","48","","PREFABRICATED ROOF TRUSSES, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[322,5228,1,5,"37","","48","","The prefabricated timber roof trusses shall be designed by a Registered Professional Engineer and shall be in accordance with SANS 0160 and 0163, as well as the additional requirements of PW 371, clause 8.10. The wind loading shall be as determined in terms of Clause 5.5 of SANS 0160. The applicable terrain category shall be taken as Category 2.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[323,5229,1,5,"37","","48","","The prefabricated timber roof trusses shall be fabricated in a factory by a truss fabricator who has been awarded a Certificate of Competence by the Institute of Timber Construction and who is approved by the Principal Agent.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[324,5230,1,5,"37","","48","","All prices shall be deemed to include the cost of the Registered Professional Engineer and the issueing of a certificate on completion, certifying the workmanship, erection and materials meeting the stated requirements.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[325,5231,1,5,"37","","48","","All roof truss dimensions are measured to the external perimeter of the structures/buildings.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[326,5257,1,5,"37","","49","","GENERAL ROOF TIMBERS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[327,5258,1,5,"37","","49","","Sawn softwood:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[328,5259,1,5,"37","1","49.9","","50 x 76mm Purlins. [44]","m",70,"","","","","23/10/2025 10:41:01",""]
[329,5264,1,5,"37","","50","","EAVES, VERGES, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[330,5265,1,5,"37","","50","","Sawn softwood:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[331,5266,1,5,"37","2","50.13","","38 x 38mm Battens fixed to walls. [44]","m",10,"","","","","23/10/2025 10:41:32",""]
[332,5268,1,5,"38","","50","","Pressed fibre cement:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[333,5269,1,5,"38","3","50.15","","12 x 225mm Fascia fixed vertically to timber battens at end of roof trusses (elsewhere measured) with brass screws, including H-profile PVC joint strips, caps, etc. [40]","m",15,"","","","","14/10/2025 09:47:44",""]
[334,10569,1,5,"38","","51","","MEDIUM DENSITY FIBREBOARD","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[335,10570,1,5,"38","","51","","Supawood with plain and smooth surface suitable for painting both sides, hung to timber door linings:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[336,10683,1,5,"38","4","51.24","","22mm Thick door, size 600 x 2100mm high. [35]","No",3,"","","","","23/10/2025 10:42:11",""]
[337,10571,1,5,"38","5","51.25","","22mm Thick double door in two equal leaves, size 1200 x 2100mm high. [35]","No",2,"","","","","23/10/2025 10:42:32",""]
[338,10891,1,5,"38","","51","","GUMPOLE FENCING","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[339,10892,1,5,"38","6","","","60mm Diameter treated round pealed gumpole assembly 1900mm high, fixed vertically side by side, secured with and including two 50 x 50 x 5mm hot dip galvanised steel angle section horizontal bearers along the total length, one vertical bearer at each end and intermediate vertical bearers at approximately 2420mm centres, all securely fixed to gumpoles, etc. with gumpoles' lower ends securely bedded in unreinforced concrete (20MPa/19mm) base size 150 x 200mm high, including excavations, etc. [26]","m",10,"","","","","23/10/2025 10:43:08",""]
[340,10936,1,5,"38","","","","JOINERY FITTINGS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[341,10941,1,5,"38","","","","The references in the descriptions refer to the respective joinery fittings/units and combination units as per the Architects' detail sheets/drawings attached to these Bills of Quantities.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[342,10942,1,5,"38","","","","All components are to be assembled, securely fixed, adjusted, etc. and primed/varnished/painted and/or finished as per the Architects' detail sheets and prices shall include for same.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[343,10944,1,5,"39","","","","All cupboards to have 20mm thick medium density fibreboard faced with high pressure laminate on both faces as backing, secured to walls, etc. and supported with and including 22 x 44mm wrot softwood and/or chipboard bearers where indicated as such on the Architects' drawings and/or details.All cupboard units with medium density fibreboard and/or glass doors (single or double) to be fitted with an intermediate shelf (except if otherwise described) formed of 20mm thick medium density fibreboard faced with high pressure laminate on both faces. All cupboard and/or drawer units shall be fitted with 20mm thick medium density fibreboard faced with high pressure laminate on both faces as base shelving to the units.Where cupboards are fitted with medium density fibreboard on top (closing off the units on top), these are to be formed of 20mm thick medium density fibreboard faced with high pressure laminate on both faces.Where the descriptions refer to medium density fibreboard, it shall be deemed to indicate PG Bison Melawood and/or SupaWhite products with melamine finish to Architects' approval.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[344,10945,1,5,"39","","","","All prices for the descriptions of joinery fittings that may have doors, drawers, etc. are to be inclusive of all specified furniture, etc. as well as the components described above.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[345,10947,1,5,"39","","","","Staff Facility:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[346,10949,1,5,"39","7","","","Slatted seating 500mm wide, consisting of 22 x 44mm wrot Meranti twice angle rounded slats spaced 20mm apart, twice brass screwed from below through support brackets (elsewhere measured) (brackets spaced at 404mm centres)[7]","m",8,"","","","","14/10/2025 02:32:13",""]
[347,10957,1,5,"39","","","","Store:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[348,10958,1,5,"39","8","","","Shelving unit formed of 22mm thick wrot laminated softwood 600mm wide in three tiers, hung on and screwed to a total of six white epoxy coated adjustable shelf brackets, brackets secured to and including 1280mm long white epoxy wall bands, each three times plugged and screwed to wall with top of bands secured with and including 6mm diameter x 50mm long rawlbolts, overall length of unit 2250mm, refer drawing E15-891-7.201B. [16]","No",1,"","","","","23/10/2025 10:43:42",""]
[349,10954,1,5,"40","","","","STEEL LOCKERS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[350,10955,1,5,"40","","","","Ricor or equivalent hammertone paint finished lockers complete, including fixing:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[351,10956,1,5,"40","9","","","Code BPGM02 two tier factory locker, four times bolted to wall with and including 10mm diameter expansion bolts 70mm long, size 300 x 450 x 1800mm high [7]","No",10,"","","","","14/10/2025 02:30:18",""]
[353,1596,1,6,"42","","54","","BILL No. 6","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:38:43",""]
[354,5793,1,6,"42","","54","","CEILINGS, PARTITIONS & ACCESS FLOORING","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[355,5794,1,6,"42","","54","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[356,5795,1,6,"42","","54","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[357,5796,1,6,"42","","54","","Descriptions","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[358,5797,1,6,"42","","54","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[359,5798,1,6,"42","","54","","Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[360,5799,1,6,"42","","54","","NAILED UP CEILINGS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[361,5800,1,6,"42","","54","","6mm Thick Nutec or equivalent fibre cement ceiling boarding, laid in staggered pattern with and including white H-profile uPVC jointing strips, secured to brandering with serrated edge nails at maximum 150mm centres:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[362,5801,1,6,"42","1","54.1","","Ceiling fixed to and including 38 x 38mm sawn softwood brandering at 400mm centres at joints, against walls, etc. [5][30][41][55]","m2",22,"","","","","23/10/2025 10:40:35",""]
[363,10057,1,6,"42","2","54.2","","Extra over for downlighter opening. [41]","No",1,"","","","","23/10/2025 10:38:57",""]
[364,10061,1,6,"42","3","54.3","","Extra over for trapdoor assembly complete. [41]","No",1,"","","","","23/10/2025 10:38:42",""]
[365,5815,1,6,"42","","55","","CORNICES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[366,5816,1,6,"42","","55","","Gypsum cornices plugged to walls:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[367,5819,1,6,"42","4","55.6","","75mm Coved cornice including sealing along both edges with silicone sealer to render airtight. [41]","m",9,"","","","","23/10/2025 10:37:55",""]
[368,5835,1,6,"42","","55","","SUSPENDED CEILINGS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[369,5845,1,6,"43","","55","","12,5mm Thick Gyproc RhinoBoard or equivalent square edged 'Frost White' vinyl clad gypsum ceiling boarding, secured to and including Donnceil T37K grid, with screws to main tees at 1200mm centres and 35 x 32mm high cross tees at 600mm centres, with and including all necessary angles, cleats, hangers, grids, locking type end clips, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[370,5849,1,6,"43","5","55.7","","Suspended ceiling system fixed not exceeding 1m below timber trusses (spaced at approximately 1000mm centres) [40]","m2",38,"","","","","14/10/2025 09:29:32",""]
[371,10050,1,6,"43","6","55.8","","Extra over for downlighter opening. [40]","No",10,"","","","","23/10/2025 10:36:49",""]
[372,5895,1,6,"43","","55","","Shadowline powder coated cornices fixed in accordance with the manufacturer's instructions:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[373,5897,1,6,"43","7","55.11","","Cornice fixed securely along perimeter of suspended ceiling [40]","m",39,"","","","","14/10/2025 09:30:35",""]
[374,5826,1,6,"43","","56","","INSULATION","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[375,1626,1,6,"43","","56","","Aerolite or equivalent insulation:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[376,9973,1,6,"43","8","56.13","","100mm Thick layer closely fitted and laid on top of brandering between roof timbers, etc. [40]","m2",38,"","","","","23/10/2025 10:35:37",""]
[378,1733,1,7,"45","","59","","BILL No. 7","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:38:51",""]
[379,6102,1,7,"45","","59","","IRONMONGERY","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[380,6103,1,7,"45","","59","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[381,6104,1,7,"45","","59","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[382,12944,1,7,"45","","82","","Proprietary products in descriptions","H3",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:37:07",""]
[383,12945,1,7,"45","","68","","Reference to any particular trademark, name, patent, design, type, specific origin or producer is purely to establish a standard for requirements.  Products or articles of an equivalent standard may be substituted","",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:37:08",""]
[384,6105,1,7,"45","","59","","Fixing of ironmongery, etc.","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[385,6106,1,7,"45","","59","","Where applicable fixing of ironmongery are to include for any required fixing stainless steel screws, etc.  All prices should include for assembly, fixing in accordance with the manufacturers' instructions, adjusting, etc.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[386,6107,1,7,"45","","59","","Finishes to ironmongery","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[387,6108,1,7,"45","","59","","Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin Bronze Lacquered; CH Chromium Plated; SC Satin Chromium Plated; SE Silver Enamelled; GE Grey Enamelled; AS Anodised Silver; AB Anodised Bronze; AG Anodised Gold; ABL Anodised Black; PB Polished Brass; PL Polished and Lacquered; PT Epoxy Coated and SD Sanded","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[388,6109,1,7,"45","","59","","HINGES, BOLTS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[389,6110,1,7,"45","","59","","Dormakaba or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[390,6111,1,7,"45","1","59.1","","DBB-SS-009 102 x 75 x 3mm Two ball bearing butt hinge. [11]","No",3,"","","","","23/10/2025 10:32:34",""]
[391,6122,1,7,"45","2","59.2","","PHA3 S DD Three point panic bar set for double door, door leaf size 1000 x 2270mm high, including cutting to fit door width where required. [61]","Sets",2,"","","","","23/10/2025 10:32:07",""]
[392,10740,1,7,"46","","59","","Union or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[393,10738,1,7,"46","3","59.5","","32mm Brass piano hinge 2100mm long. [35]","No",29,"","","","","23/10/2025 10:24:36",""]
[394,10739,1,7,"46","4","60.6","","100 x 25mm SC Brass barrel bolt. [35]","No",1,"","","","","23/10/2025 10:24:21",""]
[395,10741,1,7,"46","5","60.7","","100 x 25mm SC Brass necked bolt. [35]","No",1,"","","","","23/10/2025 10:24:02",""]
[396,6126,1,7,"46","","60","","LOCKS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[397,6127,1,7,"46","","60","","Dormakaba or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[398,6155,1,7,"46","6","60.22","","55mm ISEO 1450.00.55 Backset single long throw two pin profile cylinder gate lock. [57]","No",3,"","","","","23/10/2025 10:22:42",""]
[399,6159,1,7,"46","","61","","HANDLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[400,6160,1,7,"46","","61","","Dormakaba or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[401,6177,1,7,"46","7","61.29","","SH822 SS Cyl lever handle on rose with and including cylinder escutcheon. [15]","Sets",1,"","","","","23/10/2025 10:21:58",""]
[402,10742,1,7,"46","","61","","Union or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[403,10743,1,7,"46","8","61.30","","96mm AL5516AS Centred aluminium cupboard pull handle. [35]","No",7,"","","","","23/10/2025 10:18:49",""]
[404,6223,1,7,"46","","62","","DOOR STOPS, CABIN HOOKS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[405,6224,1,7,"46","","62","","Sundries:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[406,6225,1,7,"46","9","62.36","","10mm Diameter steel dowel 100mm long in and including mortice in timber and concrete","No",10,"","","","","14/10/2025 09:26:42",""]
[407,6226,1,7,"46","","62","","Dormakaba or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[408,6229,1,7,"46","10","62.39","","DDS-SS-021 Floor mounted door stop. [18]","No",1,"","","","","23/10/2025 10:16:05",""]
[409,6241,1,7,"46","","62","","LETTERS, NAMEPLATES, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[410,6242,1,7,"46","","62","","Contractor to provide samples of nameplates for approval of the Architect","H4",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[411,6243,1,7,"46","","63","","Dormakaba or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[412,6248,1,7,"46","11","63.50","","DSS-136 EL Electrical sign. [35]","No",1,"","","","","23/10/2025 10:15:20",""]
[413,6249,1,7,"46","12","63.51","","DSS-137 T Telkom sign. [35]","No",2,"","","","","23/10/2025 10:14:29",""]
[414,6253,1,7,"46","13","63.52","","DSS-145 FHR Fire hose reel sign. [35]","No",1,"","","","","23/10/2025 10:14:17",""]
[415,10758,1,7,"47","","64","","RECESSED MATS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[416,10759,1,7,"47","14","64.67","","1500 x 1000mm Genesis Romat (Code R8900) or equivalent recessed mat assembly in anthracite colour, complete with stainless steel edge trim, forming recess in floor, etc. [34]","No",2,"","","","","23/10/2025 09:59:58",""]
[417,11958,1,7,"47","15","","","Ditto size 2000 x 1000mm. [34]","No",2,"","","","","23/10/2025 09:59:44",""]
[419,1906,1,8,"49","","66","","BILL No. 8","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:38:57",""]
[420,6427,1,8,"49","","66","","METALWORK","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[421,12946,1,8,"49","","82","","Proprietary products in descriptions","H3",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:37:37",""]
[422,12947,1,8,"49","","68","","Reference to any particular trademark, name, patent, design, type, specific origin or producer is purely to establish a standard for requirements.  Products or articles of an equivalent standard may be substituted","",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:37:37",""]
[423,6428,1,8,"49","","66","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[424,6431,1,8,"49","","66","","Hot dip galvanising","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[425,6432,1,8,"49","","66","","Where hot dip galvanising is specified, it should be executed in accordance with SANS 121:2011 (ISO 1461:2009), unless otherwise described.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[426,11959,1,8,"49","","217","","STAINLESS STEEL HANDRAILS, BUMPRAILS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 12:08:23",""]
[427,11960,1,8,"49","","218","","Stainless steel (Grade 316) handrails, including all scribing, welding, setting up in position, adjusting, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 12:08:23",""]
[428,11961,1,8,"49","1","","","60mm Diameter rail fixed to brick wall including all fittings, bolts and closed ends (In 4 No.)[32]","m",30,"","","","","23/10/2025 09:57:20",""]
[429,11962,1,8,"49","","","","Balustrading complete to a minimum of 1000mm high in accordance with SANS10400-B","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 12:08:24",""]
[430,11964,1,8,"49","2","","","Floor mounted balustrading to stairs. [32]","m",3,"","","","","23/10/2025 09:58:02",""]
[431,10706,1,8,"49","","71","","YARD GATES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[432,10707,1,8,"50","","71","","Cochrane or equivalent:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[433,10708,1,8,"50","3","71.29","","Pedestrian gate consisting of 50 x 50 x 2mm hollow section outer framing and one mullion, all mitred and welded at intersections, internal 30 x 4mm flat section welded onto inside of all outer framing, one cut-out size 120 x 200mm high formed of outer framing and flat section as described above, filled in with 3,5mm diameter horizontal and vertical high tensile wires, galvanised with marine fusion bond coating with aperture size 76,2 x 50mm and reinforcing V-section ribs, cut to size and secured tautly around all edges to flat section with 4mm diameter self tapping screws 30mm long at 100mm centres all around, complete with 500 x 800mm high unreinforced concrete (15MPa/19mm) beam, with 5 - 45mm tapering hot dip galvanised (marine fusion bond coating - acid modified) gate posts 2400mm high, sealed with UV stabilized polymer cap, including locking recess mechanism with sealed end caps and 30 x 250mm long angle section base anchors, complete with required vandal resistant bolts and clamping plates, nuts and washers for fixing to gate complete with 300 x 300 x 5mm baseplate cast into concrete base complete with and including all excavations, filling, etc. one heavy duty brass padlock, etc. size 1000 x 2100mm high overall [57]","No",2,"","","","","23/10/2025 09:55:52",""]
[434,10711,1,8,"50","4","72.30","","Ditto size 2000 x 2100mm high overall. [57]","No",1,"","","","","23/10/2025 09:57:09",""]
[435,6697,1,8,"50","","72","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[436,10950,1,8,"50","","","","Hot dip galvanised slatted seating support brackets:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[437,10951,1,8,"50","5","","","Triangular shaped support bracket to timber slatted seating (elsewhere measured), formed of 45 x 45 x 5mm angle sections, all mitred and welded at intersections, vertical leg three times holed for and bolted to wall with and including 8 x 50mm galvanised rawlbolts, support bracket size 460mm wide x 265mm high [7]","No",16,"","","","","22/10/2025 04:50:49",""]
[439,2025,1,9,"52","","74","","BILL No. 9","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:10",""]
[440,6704,1,9,"52","","74","","PLASTERING","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[441,6705,1,9,"52","","74","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[442,6737,1,9,"52","","75","","INTERNAL PLASTER","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[443,6738,1,9,"52","","75","","4:1 Cement plaster (SANS 2001) steel trowelled on brickwork/concrete:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[444,11939,1,9,"52","1","","","On walls in patchings [62]","m2",2,"","","","","14/10/2025 10:12:32",""]
[446,2106,1,10,"53","","77","","BILL No. 10","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:17",""]
[447,6767,1,10,"53","","77","","TILING","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[448,12948,1,10,"53","","82","","Proprietary products in descriptions","H3",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:38:00",""]
[449,12949,1,10,"53","","68","","Reference to any particular trademark, name, patent, design, type, specific origin or producer is purely to establish a standard for requirements.  Products or articles of an equivalent standard may be substituted","",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:38:00",""]
[450,6768,1,10,"53","","77","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[451,6769,1,10,"53","","77","","WALL TILING","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[452,6770,1,10,"53","","77","","600 x 300 x 10mm Thick Titan FIJI or equivalent light grey polished porcelain tiles fixed to plaster with approved tile adhesive, 3mm wide continuous joints in both directions, pointed with light grey anti-fungicidal grout:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[453,6771,1,10,"53","1","77.5","","On walls [62]","m2",2,"","","","","14/10/2025 10:17:48",""]
[455,2590,1,11,"54","","94","","BILL No. 11","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:30",""]
[456,7108,1,11,"54","","94","","GLAZING","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[457,7109,1,11,"54","","94","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[458,2633,1,11,"54","","94","","TOPS, SHELVES, DOORS, MIRRORS, ETC","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[459,2638,1,11,"54","","94","","6mm Thick silvered float glass copper backed mirrors with 10mm bevelled and polished edges, drilled in corners and screw fixed to 16mm Supawood board. Mirror screws to be chromium plated dome capped screws. Supawood board to be screwed onto 32 x 32mm wrot softwood frame, planed all round. Frame to be sanded smooth and painted one coat wood primer and two coats eggshell enamel paint:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[460,2639,1,11,"54","1","94.1","","Mirror size 450 x 900mm high [10]","No",5,"","","","","22/10/2025 04:52:42",""]
[462,2647,1,12,"55","","95","","BILL No. 12","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:35",""]
[463,7160,1,12,"55","","95","","PAINTWORK","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[464,7161,1,12,"55","","95","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 Series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[465,7162,1,12,"55","","95","","PAINTWORK TO NEW AREAS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[466,7163,1,12,"55","","95","","External elements to each block to be painted in a predetermined colour scheme.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[467,7177,1,12,"55","","95","","ON GYPSUM PLASTERBOARD","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[468,7178,1,12,"55","","95","","Prepare, prime all heads of nails and apply one coat plaster primer, one undercoat and two coats interior quality acrylic paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[469,7179,1,12,"55","1","95.6","","Internal ceilings and/or bulkheads with skimmed joints. [41]","m2",3,"","","","","23/10/2025 09:53:42",""]
[470,7180,1,12,"55","","95","","ON FIBRE CEMENT","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[471,7183,1,12,"55","","96","","Prepare and apply one coat undercoat and two coats exterior quality acrylic paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[472,11971,1,12,"55","2","","","Eaves soffits[3]","m2",10,"","","","","14/10/2025 02:17:21",""]
[473,7185,1,12,"55","3","96.10","","Fascias and barge boards. [3]","m2",44,"","","","","23/10/2025 09:52:46",""]
[474,7204,1,12,"55","","96","","ON WOOD","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[475,7216,1,12,"55","","96","","Prepare and apply one coat pink wood primer and two coats eggshell enamel paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[476,7217,1,12,"55","4","96.15","","Timber doors (both sides measured). [35]","m2",18,"","","","","23/10/2025 09:45:18",""]
[477,11013,1,12,"55","","","","Prepare and apply two coats polyurethane wood varnish including sanding between coats on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[478,11014,1,12,"55","5","","","Timber shelving","m2",20,"","","","","23/10/2025 09:52:58",""]
[479,10952,1,12,"56","","","","Prepare, stop and apply three coats Plascon Woodcare Suede Matt varnish, including sanding down between all coats, on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[480,11020,1,12,"56","6","","","Slatted timbers to benches (both sides measured)[7]","m2",14,"","","","","18/10/2025 05:31:02",""]
[481,11940,1,12,"56","","","","PAINTWORK TO PREVIOUSLY PAINTED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 10:56:42",""]
[482,11941,1,12,"56","","","","Wash down soiled surfaces with sugar soap, sand down to remove all flaking paint, fill imperfections with Profill and apply two coats exterior quality acrylic paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 10:56:42",""]
[483,11966,1,12,"56","7","","","Eaves soffits[3]","m2",162,"","","","","14/10/2025 12:34:10",""]
[484,11968,1,12,"56","","","","Sand down, remove all flaking paint/varnish and apply one coat pink wood primer and two coats eggshell enamel paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 12:46:48",""]
[485,11970,1,12,"56","8","","","Exposed roof timbers[20]","m",315,"","","","","18/10/2025 05:25:21",""]
[486,11947,1,12,"56","","","","Wash down soiled surfaces with sugar soap, sand down, fill imperfections with Profill and apply one coat Plascon universal undercoat and two coats Plascon low sheen paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 10:56:43",""]
[487,11948,1,12,"56","9","","","Internal walls [36][37]","m2",50,"","","","","14/10/2025 11:04:29",""]
[488,11951,1,12,"56","","","","Sand down, remove all flaking paint and apply two coats eggshell enamel paint on:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 10:56:43",""]
[489,11952,1,12,"56","10","","","Timber doors (both sides measured) [1]","m2",56,"","","","","14/10/2025 02:08:50",""]
[491,7247,1,13,"58","","98","","BILL No. 13 ","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:42",""]
[492,7246,1,13,"58","","98","SANS 1200","EXTERNAL WORKS (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[493,7248,1,13,"58","","98","","The Tenderer is referred to the relevant Clauses in the separate Supplementary Preambles hereunder and Department of Public Works PW371 document and SANS 2001 series documents","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[494,7249,1,13,"58","","98","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[495,12950,1,13,"58","","82","","Proprietary products in descriptions","H3",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:38:34",""]
[496,12951,1,13,"58","","68","","Reference to any particular trademark, name, patent, design, type, specific origin or producer is purely to establish a standard for requirements.  Products or articles of an equivalent standard may be substituted","",{"v":0,"d":"0.0"},"","","","","07/11/2025 08:38:34",""]
[497,7269,1,13,"58","","98","","Maintenance period","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[498,7270,1,13,"58","","98","","Attention is drawn to the maintenance period of twelve (12) months from Practical Completion.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[499,7271,1,13,"58","","98","","Laying, backfilling, bedding, etc. of pipes","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[500,7272,1,13,"58","","98","","Pipes shall be laid in accordance with the following SANS 2001 Series documents:Part DP1\t\t:  Pipe trenchesPart DP2 Clause 4.3  \t:  Medium-pressure pipelines Part DP4 Clause 4.3\t:  Sewers Part DP5 Clause 4.2.3\t:  Stormwater drainage","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[501,7273,1,13,"59","","99","","Excavations","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[502,7274,1,13,"59","","99","","No claim for rock excavation will be entertained unless the Contractor has timeously notified the Quantity Surveyor thereof prior to backfilling.  Class of excavations will be in accordance with SANS 1200D Clause 3.1.  For the purpose of this project \"Soft Rock\" will have the same meaning as Intermediate excavations as defined in SANS 1200D Clause 3.1.  Boulder excavation definitions as stated in SANS 1200D will not apply.  Classification of soils and gravel is in accordance with SANS 1200M: 1996 Table 3A & 3B or TRH14.  Open face excavation is in accordance with SANS 2001: Part BE1.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[503,11000,1,13,"59","","99","","Shoring to soil drainage piping and manholes","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[504,11001,1,13,"59","","99","","The tenderer must take note that the price for soil drainage piping and manhole installation must include for any temporary support that may be required to prevent the trenches or manhole excavations from collapse during installation.  No additional cost will be entertained.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[505,7275,1,13,"60","","99","","Reinforced concrete work","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[506,7276,1,13,"60","","99","","All aspects of structural concrete work (plain and reinforced) for civil engineering and building construction shall be in accordance with the requirements of SANS 2001: Part CC1 and SANS 0155 (Accuracy in Building). Any discrepancies are to be referred to the Engineer.  1.1 Concrete mixes:  All concrete mixing shall conform to SANS 2001: Part CC1. Specialised concrete applications will be referred to the Engineer. All aggregates used are to be approved by the Engineer. The water is to be clean as for human consumption.  1.2 Concreting:  Concreting shall conform to SANS 2001: Part CC1. All dirt and trash shall be removed from the formwork before concreting. Concrete shall be thoroughly consolidated by means of tamping of vibration.  1.3 Maintaining reinforcement in position: The Contractor shall ensure that the correct concrete cover is maintained during the casting of concrete. In order to do this the Contractor shall provide suitable concrete or plastic cover blocks. All reinforcing is to be inspected and approved by the Engineer prior to casting of concrete. The Engineer shall be given 24 hours notice prior to any inspection required.  1.4 Cure: All new concrete shall be thoroughly cured by means of a resin-based curing compound or as approved by the Engineer.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[507,7277,1,13,"60","","100","","Viewing of the site","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[508,7278,1,13,"60","","100","","Before submitting his tender, the Tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done. No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[509,10930,1,13,"60","","66","","Hot dip galvanising","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[510,10931,1,13,"60","","66","","Where hot dip galvanising is specified, it should be executed in accordance with SANS 121:2011 (ISO 1461:2009), unless otherwise described.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[511,7446,1,13,"61","","102","","PAVED MAIN PARKING BAYS/ROADWORKS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[512,7447,1,13,"61","","103","","All roadworks, unpaved roadworks, paving, walkways, etc. must be maintained throughout the whole contract period, whether or not sections have achieved completion or not. The whole of these elements must, additionally, be maintained for a period of twelve (12) months after Practical Completion.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[513,11997,1,13,"61","","","","Existing paving:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 01:40:16",""]
[514,11998,1,13,"61","1","","","Clean the existing parking area to remove all loose material, remove vegetation growth, apply herbicide and prepare surface to received new road markings (elsewhere measured) [25]","m2",5045,"","","","","23/10/2025 10:51:42",""]
[515,7471,1,13,"61","","104","","White road marking paint to SANS 731 on concrete pavers:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[516,7472,1,13,"61","2","104.39","","Line 100 mm wide for parking bay","m",811,"","","","","14/10/2025 09:26:42",""]
[517,7473,1,13,"61","3","104.40","","Ditto but 500 mm wide to form standard zebra crossing","m",16,"","","","","14/10/2025 09:26:42",""]
[518,10603,1,13,"61","4","105.41","","Four letters arranged to read \"STOP\", size 1000 x 4000mm long overall","No",3,"","","","","14/10/2025 09:26:42",""]
[519,10604,1,13,"61","5","105.42","","Seven letters arranged to read \"NO ENTRY\", size 1000 x 4000mm long overall","No",2,"","","","","14/10/2025 09:26:42",""]
[520,10605,1,13,"61","6","105.43","","Supply and erect statutory \"STOP\" road sign type R1 size 610mm","No",3,"","","","","14/10/2025 09:26:42",""]
[521,10607,1,13,"61","7","105.45","","Supply and erect statutory \"EXIT\" road sign type R3 size 914mm","No",2,"","","","","14/10/2025 09:26:42",""]
[522,10606,1,13,"61","8","105.44","","Supply and erect statutory \"NO ENTRY\" road sign type R3 size 914mm","No",2,"","","","","14/10/2025 09:26:42",""]
[523,7474,1,13,"61","","105","","Yellow road marking paint to SANS 731 on concrete pavers:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[524,10600,1,13,"61","9","105.46","","Traffic arrow 4000mm long and 400mm wide","No",16,"","","","","14/10/2025 09:26:42",""]
[525,10601,1,13,"61","10","105.47","","GM6.3 wheelchair sign size overall 1200 x 1200mm","No",4,"","","","","14/10/2025 09:26:42",""]
[526,10611,1,13,"61","","105","","UNPAVED ROADWORKS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[527,10612,1,13,"62","","106","","Site clearance, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[528,10613,1,13,"62","11","106.51","","Remove topsoil and vegetation to a depth of 100mm and deposit on site in stockpiles where directed by the Engineer. [51]","m2",940,"","","","","23/10/2025 08:49:22",""]
[529,12925,1,13,"62","12","","","Remove growing weed  to existing gravel road and prepare to receive layer of G5 (elsewhere measure). [49]","m2",793,"","","","","23/10/2025 08:50:16",""]
[530,10615,1,13,"62","","106","LI","Earth filling supplied by the Contractor under roads, etc.:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[531,10617,1,13,"62","13","106.52","","G5 Material in accordance with SANS 1200DM with 5% cement as stabilise in 150mm layers compacted to a minimum of 95% Mod AASHTO dry density. [49][51]","m3",560,"","","","","23/10/2025 10:49:48",""]
[532,10619,1,13,"62","","106","LI","Compaction of surfaces:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[533,10620,1,13,"62","14","106.54","","Compaction of in-situ surfaces, etc. including scarifying for a depth of 150mm, breaking down oversized material and compacting to a minimum of 93% Mod AASHTO dry density. [51]","m2",940,"","","","","23/10/2025 08:51:32",""]
[534,10621,1,13,"62","","106","","Prescribed density tests on filling:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[535,10622,1,13,"62","15","106.55","","Modified AASHTO density test. [49][51]","No",12,"","","","","23/10/2025 08:52:07",""]
[536,10623,1,13,"62","16","106.56","","CBR test in accordance with Method A8 of TMH 1. [49][51]","No",2,"","","","","23/10/2025 08:52:21",""]
[537,7611,1,13,"62","","108","","STORMWATER RETICULATION/CHANNELS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[538,7612,1,13,"62","","108","","Precast concrete channels, etc. shall be manufactured in suitable lengths.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[539,12021,1,13,"62","","109","","Stormwater furrow:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 02:16:21",""]
[540,12020,1,13,"62","17","114.32","","Form stormwater channel 1000 x 200mm deep with 1% slope by clearing, levelling, compacting insitu material to 90% Mod AASHTO density. [52]","m",200,"","","","","23/10/2025 08:53:34",""]
[541,7618,1,13,"62","","108","","STORMWATER DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[542,12023,1,13,"62","","","","Catchpits:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 02:51:49",""]
[543,12924,1,13,"62","18","","","Complete existing stormwater catchpit sized 1200 x 1200mm (approximate) by removing all debris inside, construct concrete benching inside, install cementile or similar approved code MS 1201 reinforced concrete Catchpit cover with lid bedded in 1:3 cement mortar.","No",1,"","","","","23/10/2025 09:33:42",""]
[544,7643,1,13,"63","","109","","Stormwater headwall:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[545,7644,1,13,"63","19","109.73","","Stormwater headwall 990mm wide at stormwater outlet to connect to 160mm stormwater pipe (elsewhere measured), projecting for a length of 470mm to extreme width of 11460mm wide, comprising of 150mm thick reinforced concrete (20MPa/19mm) base with Type 245 fabric reinforcement with 230 x 230mm concrete edge to base at extreme side and 230mm brick wing walls on sides for a length of 1220mm, tapering down on two sides from 600mm to 285mm high complete with soldier course brickwork to top of inlet and wing walls with 10mm plaster on visible surfaces including all necessary excavating, compaction to base, carting away, etc.[LI]","No",1,"","","","","17/10/2025 02:49:03",""]
[546,7652,1,13,"63","","109","","Sundries:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[547,12022,1,13,"63","20","102.137","","Reno mattress cage size 2000 x 1000 x 500mm deep using 50mm galvanised diamond mesh stitched closed, lined with \"Bidim A14\" geotextile fabric and filled with 100mm stones including necessary excavating, carting away, etc.","No",2,"","","","","18/10/2025 05:21:28",""]
[548,7650,1,13,"63","","109","","Testing:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[549,7651,1,13,"63","21","109.74","","Allow for testing all external stormwater reticulation piping and components","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 09:26:42",""]
[550,12025,1,13,"63","","112","","PERIMETER FENCING AND GATES","H2",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:08:29",""]
[551,12026,1,13,"63","","","LI","Clearing of site:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:08:29",""]
[552,12027,1,13,"63","22","","","Allow for clearing site for the width of 1m where fencing runs are to be erected including removing trees, shrubs, etc. not exceeding 200mm girth, grubbing up roots and roughly levelling ","m",80,"","","","","17/10/2025 04:36:48",""]
[553,12029,1,13,"63","","","","Betafence or other approved fencing panels and posts complete with all components, setting up, adjusting, etc.:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:30:15",""]
[554,12030,1,13,"63","","","","PVC coated high security fencing and gates. All bolts, nuts and washers to be stainless steel Grade 304.  Fixators to be stainless steel Grade 304 and PVC coated. Fence system to be maintenance free and shall carry a 10 year insurance underwritten anti-corrosion guarantee for material and workmanship issued for original panels, posts and fixators. The supplier/erector to be ISO 9001 compliant.","",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:08:29",""]
[555,12031,1,13,"64","","289","","Allowance shall be made as required to excavate areas that are too high and to fill depressions with approved filling, carted on site where necessary and well compacted prior to erection of fencing","",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:08:29",""]
[556,12032,1,13,"64","23","","","2100mm High density anti climbing and anti-cut pressed mesh panel fencing, formed of 4mm diameter horizontal and 4mm diameter vertical high tensile wires galvanised with marine fusion bond coating with aperture size 76,2 x 12,7mm and reinforcing V-section ribs. Panels with a maximum width of 3305mm (or as determined on site) and laterally strengthened by 4 x 50mm deep V-profiled horizontal stiffener bends to ensure sufficient rigidity, complete with 75mm 70 degree flanges along sides, top and toe and secured to fencing posts (elsewhere measured). [52]","m",80,"","","","","23/10/2025 09:00:32",""]
[557,12048,1,13,"64","24","","","600mm high Anti-burrow underdig mesh panel form of 76,2 x 12,8mm rectangular apertures with horizontal and vertical core wire of 3mm diameter thickness PVC coated Anthracite RAL7021 to a minimum thickness of 200 microns using fluidized bed PVC coating machine, panels to maxim size of 3048 x 600mm high, including excavations, backfilling, etc. [52]","m",80,"","","","","23/10/2025 09:00:58",""]
[558,12035,1,13,"64","25","","","2,5mm Thick x 100mm high hot dip galvanised sawtooth spikes formed of toughened steel, fitted to top of fencing with M8 x 30mm cup square bolts. [52]","m",80,"","","","","23/10/2025 09:01:16",""]
[559,12033,1,13,"64","26","","","2900mm High H-profile secure post formed of 70 x 44 x 2mm thick hollow section, PVC coated Anthracite RAL7021 to a minimum thickness of 200 microns using fluidized bed PVC coating machine, complete with required locking recess mechanism (spider fixators and shear nuts) for fixing to panels (elsewhere measured) and embedded in and including unreinforced concrete (15MPa/19mm) base size 400 x 400 x 600mm deep, including excavations, backfilling, etc. [52]","No",27,"","","","","23/10/2025 09:01:29",""]
[560,12034,1,13,"64","27","","","2900mm High H-profile end post formed of 70 x 70 x 1,6mm thick hollow section, PVC coated Anthracite RAL7021 to a minimum thickness of 200 microns using fluidized bed PVC coating machine, complete with required locking recess mechanism (spider fixators and shear nuts) for fixing to panels (elsewhere measured) and embedded in and including unreinforced concrete (15MPa/19mm) base size 400 x 400 x 600mm deep, including excavations, backfilling, etc. [52]","No",2,"","","","","23/10/2025 09:01:40",""]
[561,12036,1,13,"65","28","114.115","","Hot dip galvanised double gate in two equal leaves hung folding, each leaf consisting of 50 x 50 x 2mm hollow section outer framing and one mullion, all mitred and welded at all intersections, internal 30 x 4mm flat section welded onto inside of all outer framing, two cut-outs each size 120 x 200mm high formed of outer framing and flat section as described above, filled in with 4mm diameter horizontal and 4mm diameter vertical high tensile wires galvanised with marine fusion bond coating with aperture size 76,2 x 12,7mm and reinforcing V-section ribs, cut to size and secured tautly around all edges to flat section with 4mm diameter self tapping screws 30mm long at 100mm centres all around, each leaf fitted with a pair of approved hinges, secured to and including 100 x 100 x 3mm hollow section hot dip galvanised gate post 3m long, lower section of post cast into 450 x 450 x 600mm unreinforced concrete (15MPa/19mm) base, including all excavations, filling, etc., fitting one 100mm horizontal sliding and two 200mm drop bolts (complete with two keeps in concrete), one heavy duty brass padlock, etc. overall size 2500 x 2100mm high. [52]","No",1,"","","","","23/10/2025 09:02:38",""]
[562,12042,1,13,"65","","","LI","Sundries:","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 03:17:21",""]
[563,12044,1,13,"65","29","","","Remove rust to existing fencing panels and paint with approved quality paint to match. [48]","m2",15,"","","","","23/10/2025 09:02:58",""]
[564,12045,1,13,"65","30","","","Clean down cement and concrete spills on weldmesh fencing. [48]","m2",5,"","","","","23/10/2025 09:03:22",""]
[565,12043,1,13,"65","31","","","Replace sliding gate rial with galvanised rail including bedding in concrete. [48]","m",13,"","","","","23/10/2025 09:03:35",""]
[566,12927,1,13,"65","","125","","SEWER POND","H2",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:06:04",""]
[567,12928,1,13,"65","","123","","Brickwork of NFX bricks (14MPa nominal compressive strength) in Class II mortar:","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:11:18",""]
[568,12929,1,13,"65","32","123.248","","One brick wall in two half brick skins, the two skins tied together with and including galvanised wire ties [52]","m2",7,"","","","","23/10/2025 09:19:07",""]
[569,12930,1,13,"65","","75","","4:1 Cement plaster (SANS 2001) steel trowelled on brickwork/concrete:","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:24:03",""]
[570,12932,1,13,"65","33","","","On external walls. [52]","m2",14,"","","","","23/10/2025 09:16:04",""]
[571,12933,1,13,"66","","97","61","Lockable manhole covers","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:41:32",""]
[572,12935,1,13,"66","34","71.4","","600mm diameter lockable circular type M4A product or similar approved manhole SANS 1882 medium duty Dough Moulding compound 4A hinged lid and frame cast into concrete upstand. [52]","No",1,"","","","","23/10/2025 09:40:49",""]
[573,8494,1,13,"66","","126","","Topsoil supplied by the Contractor, including spreading and levelling:","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[574,8495,1,13,"66","35","126.274","","Sewer pond area, grassed areas, etc. [52]","m3",100,"","","","","23/10/2025 09:04:00",""]
[576,2806,1,14,"68","","130","","BILL No. 14","H1",{"v":0,"d":"0.0"},"","","","","20/10/2025 02:39:49",""]
[577,2807,1,14,"68","","130","","PROVISIONAL SUMS, ETC.","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[578,10364,1,14,"68","","130","","The Tenderer is referred to the relevant Clauses in the Supplementary Preambles hereunder and Department of Public Works PW371 document","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[579,10365,1,14,"68","","130","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[580,10366,1,14,"68","","130","","General","H4",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[581,10367,1,14,"68","","130","","Work for which budgetary allowances are provided will be measured and valued in accordance with Clause 32 of the Principal Building Agreement and deducted in whole or in part if not required without any compensation for loss or profit on the said allowances.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[582,10368,1,14,"68","","130","","Prime Cost amounts and Provisional Sums are nett. Prime Cost amounts include for delivery to site of all articles concerned.  Provisional Sums are for material and equipment supplied and installed complete by firms of specialists.","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[583,10384,1,14,"68","","131","","SPECIALIST WORK","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[584,10385,1,14,"68","","131","","ATTENDANCE ","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[585,10386,1,14,"68","","131","","General attendance on Nominated Sub-contractors' work shall be deemed to include the following:","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[586,10387,1,14,"68","","131","","1.  Access to the site and places where the sub-contract work is to be carried out, including the reasonable use of any temporary personnel hoists erected by the Contractor; ","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[587,10388,1,14,"68","","131","","2. The provision of water and lighting and of single phase electric power to a position within 50 metres of the place where sub-contract work is to be carried out but excluding water, fuel and power for commissioning of the installation for which the sub-contractor shall be responsible; ","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[588,10389,1,14,"68","","131","","3. The provision of an area for the sub-contractor to establish office accommodation, temporary workshops and for the storage of plant and material; ","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[589,10390,1,14,"69","","131","","4. The use of erected scaffolding belonging to the Contractor, in common with others having the like right, whilst it so remains erected upon the site;","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[590,10391,1,14,"69","","131","","5. The use of mess rooms, latrine, health and welfare facilities and the like, where provided;","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[591,10392,1,14,"69","","131","","6. The use of site telephone and facsimile machine, where provided, subject to the payment by the sub-contractor for all his outgoing calls. ","",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[592,10401,1,14,"69","","132","","ELECTRICAL INSTALLATION BY NOMINATED/SELECTED SUB-CONTRACTOR ","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[593,10402,1,14,"69","1","132.5","","Provide the sum of R300 000.00 (Three Hundred Thousand Rand) for Electrical Installation complete by a Nominated/Selected Sub-contractor","Item",{"v":1,"d":"1.00"},{"v":300000,"d":"300000.00"},{"v":300000,"d":"300000.00"},"","","23/10/2025 10:02:49",""]
[594,10403,1,14,"69","2","132.6","","Add for profit","Item",{"v":1,"d":"1.00"},"","","","","23/10/2025 10:03:31",""]
[595,10404,1,14,"69","3","132.7","","Allow for attendance","Item",{"v":1,"d":"1.00"},"","","","","23/10/2025 10:03:37",""]
[596,10673,1,14,"69","","132","","GLASS SCREEN AT TURNSTILE INSTALLATION BY NOMINATED/SELECTED SUB-CONTRACTOR","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:40:09",""]
[597,10674,1,14,"69","4","132.17","","Provide the sum of R70 000.00 (Seventy Thousand Rand) for stainless steel and toughened safety glass screens between existing turnstiles","Item",{"v":1,"d":"1.00"},{"v":70000,"d":"70000.00"},{"v":70000,"d":"70000.00"},"","","23/10/2025 10:59:21",""]
[598,10675,1,14,"69","5","133.18","","Add for profit","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 12:58:20",""]
[599,10676,1,14,"69","6","133.19","","Allow for attendance","Item",{"v":1,"d":"1.00"},"","","","","14/10/2025 12:58:29",""]
[600,12936,1,14,"69","","132","","FIRE BOOSTER PUMP, IRRIGATION PUMP INSTALLATION AND ASSOCIATED PIPEWORK AND FITTINGS INSTALLATION BY NOMINATED/SELECTED SUB-CONTRACTOR","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 10:47:52",""]
[601,12937,1,14,"69","7","132.17","","Provide the sum of R1 400 000.00 (One Million Four Hundred Thousand Rand) for The installation of fire booster pumps, housing, pipework and fittings by specialist ","Item",{"v":1,"d":"1.00"},{"v":1400000,"d":"1400000.00"},{"v":1400000,"d":"1400000.00"},"","","23/10/2025 10:18:12",""]
[602,12938,1,14,"69","8","","","Add for profit","%IT","","","","","","23/10/2025 11:12:14",""]
[603,12939,1,14,"69","9","","","Allow for attendance","%IT","","","","","","23/10/2025 11:12:26",""]
[604,10589,1,14,"70","","133","","BOREHOLE, ENCLOSURES & MANUAL PISTON BAILER SYSTEM","H3",{"v":0,"d":"0.0"},"","","","","23/10/2025 09:59:55",""]
[605,10590,1,14,"70","10","133.22","","Provide the sum of R200 000.00 (Two Hundred Thousand Rand) for the a single borehole, Two borehole enclosures (one to a completed borehole) and piston bailer system for sample testing purposes, including water sample testing.","Item",{"v":1,"d":"1.00"},{"v":200000,"d":"200000.00"},{"v":200000,"d":"200000.00"},"","","23/10/2025 10:01:57",""]
[606,12940,1,14,"70","11","","","Add for profit","%IT","","","","","","23/10/2025 10:22:15",""]
[607,12941,1,14,"70","12","","","Allow for attendance","%IT","","","","","","23/10/2025 10:23:10",""]
[608,10421,1,14,"70","","133","","MONETARY PROVISIONS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[609,11010,1,14,"70","","","","CLO ALLOWANCE","H3",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[610,11011,1,14,"70","13","80.1","","Provide the sum of R25,500.00 (Twenty Five Thousand Five Hundred Rand) for the employment of a Community Liaison Officer (R8500.00 per month for duration of contract plus sundries)","Item",{"v":1,"d":"1.00"},{"v":25500,"d":"25500.00"},{"v":25500,"d":"25500.00"},"","","17/10/2025 04:40:38",""]
[611,12049,1,14,"70","","117","","TESTING AND COMPLIANCE OF PREVIOUSLY COMPLETED WORKS","H3",{"v":0,"d":"0.0"},"","","","","17/10/2025 04:00:51",""]
[612,12050,1,14,"70","14","117.5","","Provide the sum of R30 000.00 for testing sewer reticulation from a previous contract including camera surveillance of pipeline and providing footage thereof to be approved by the Engineer.","Item",{"v":1,"d":"1.00"},{"v":30000,"d":"30000.00"},{"v":30000,"d":"30000.00"},"","","17/10/2025 04:06:07",""]
[613,12051,1,14,"70","15","117.6","","Add: Mark-up","%IT","","","","","","17/10/2025 04:00:52",""]
[614,12052,1,14,"70","16","117.7","","Provide the sum of R10 000.00 for pressure testing domestic water pipeline as determined by the Engineer.","Item",{"v":1,"d":"1.00"},{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"","","17/10/2025 04:08:08",""]
[615,12053,1,14,"70","17","117.8","","Add: Mark-up","%IT","","","","","","17/10/2025 04:00:52",""]
[616,12054,1,14,"70","18","117.9","","Provide the sum of R10 000.00 for pressure testing irrigation pipeline as determined by Engineer","Item",{"v":1,"d":"1.00"},{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"","","17/10/2025 04:10:21",""]
[617,12057,1,14,"70","19","","","Add: Mark-up","%IT","","","","","","17/10/2025 04:11:13",""]
[618,12056,1,14,"70","20","","","Provide the sum of R10 000.00 for pressure testing fire main pipeline as determined by Engineer","Item",{"v":1,"d":"1.00"},{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"","","17/10/2025 04:11:03",""]
[619,12055,1,14,"70","21","117.10","","Add: Mark-up","%IT","","","","","","17/10/2025 04:00:52",""]
[621,12058,1,15,"72","1","","","PRELIMINARIES","Page",26,0,"","","","20/10/2025 12:17:54",""]
[622,11518,1,15,"72","2","","","HEALTH AND SAFETY","Page",30,0,"","","","14/10/2025 08:59:37",""]
[623,11610,1,15,"72","3","","","ALTERATIONS (PROVISIONAL)","Page",35,0,"","","","14/10/2025 08:59:41",""]
[624,2821,1,15,"72","4","135.6","","ROOF COVERINGS","Page",36,0,"","","","31/07/2019 12:12:52",""]
[625,2822,1,15,"72","5","135.7","","CARPENTRY AND JOINERY","Page",41,0,"","","","31/07/2019 12:12:52",""]
[626,2823,1,15,"72","6","135.8","","CEILINGS ETC","Page",44,0,"","","","31/07/2019 12:12:52",""]
[627,2825,1,15,"72","7","135.10","","IRONMONGERY","Page",48,0,"","","","31/07/2019 12:12:52",""]
[628,2827,1,15,"72","8","135.11","","METALWORK","Page",51,0,"","","","31/07/2019 12:12:52",""]
[629,2828,1,15,"72","9","135.12","","PLASTERING","Page",52,0,"","","","31/07/2019 12:12:52",""]
[630,2829,1,15,"72","10","135.13","","TILING","Page",53,0,"","","","31/07/2019 12:12:52",""]
[631,2831,1,15,"72","11","135.15","","GLAZING","Page",54,0,"","","","31/07/2019 12:12:52",""]
[632,2832,1,15,"72","12","135.16","","PAINTWORK","Page",57,0,"","","","31/07/2019 12:12:52",""]
[633,7245,1,15,"72","13","135.17","","EXTERNAL WORKS","Page",67,0,"","","","31/07/2019 12:12:52",""]
[634,2833,1,15,"72","14","135.18","","PROVISIONAL AMOUNTS","Page",71,0,"","","","31/07/2019 12:12:52",""]
[635,2834,2,1,"73","1","136.1","","Bills of Quantities","Page",72,0,"","","","27/03/1999 03:29:56",""]
[636,4004,2,1,"73","","136","","Subtotal","ST",{"v":0,"d":"0.00"},"","Sub Total","","","14/10/2025 09:26:42",""]
[637,10719,2,1,"73","","136","","CONTINGENCIES","H1",{"v":0,"d":"0.0"},"","","","","14/10/2025 09:26:42",""]
[638,10720,2,1,"73","","136","","Allow the sum of R200 000.00 (Two Hundred Thousand Rand) for Contingencies to be used or deducted in full at the Principal Agent's discretion","Item",{"v":1,"d":"1.00"},{"v":200000,"d":"200000.00"},{"v":200000,"d":"200000.00"},"","","23/10/2025 11:00:27",""]
[639,10721,2,1,"73","","136","","Sub Total","ST",{"v":0,"d":"0.00"},"","Sub Total","","","14/10/2025 09:26:42",""]
[640,4005,2,1,"73","","136","","ADD: Value added Tax at 15%","TAX",{"v":15,"d":"15.00"},"","","","","14/10/2025 09:26:42",""]
[641,10722,2,1,"73","","136","","TOTAL BUILDING WORKS INCLUDING VAT","ST",{"v":0,"d":"0.00"},"","Sub Total","","","14/10/2025 09:26:42",""]