Annexure A Fibre patch leads and accessories compliance checklist.
Supplier must provide data sheets to support compliance to technical requirements.
	Item
	Description and technical requirements
	Complaint     (Yes/No)
	Comments

	Fiber Optic Cleaning Kit
	1 x Fiber Optic Cleaning Cassette
	 
	 

	
	1 x 1.25mm One Click Cleaning pen (LC)
	 
	 

	
	1 x 2.5mm One Click Cleaning pen (LSH, SC)
	 
	 

	
	1 x Fiber Optic Pump Bottle (200ml)
	 
	 

	
	1 x Fiber Optic Cleaning Swabs (70mm) ,280 sheets
	 
	 

	
	1 x Black Carrying Case
	 
	 

	Attenuators
	Fiber Connector: LC/UPC
	 
	 

	
	Connector : Fixed Male (front) to Female(back)
	 
	 

	
	Ferrule Type : Ceramic
	 
	 

	
	Attenuation Accuracy: ±0.5dB
	 
	 

	
	Polarization Dependent Loss: ≤0.2dB
	 
	 

	
	Relative Humidity: 95%
	 
	 

	
	Storage Temperature Range: -40~85°C
	 
	 

	
	Operating Temperature Range: -40~80°C
	 
	 

	
	Fibre Type: Single mode
	 
	 

	
	Operating Wavelength(nm): 1260~1620(SM)
	 
	 

	
	Select Attenuation: various, 2,5,7,10dB
	 
	 

	
	Relative Humidity :95% 
	 
	 

	Wipes
	Anti-static dispensing and electrostatic discharge
	 
	 

	
	Wiper dimensions: is 210x210mm 
	 
	 

	Alcohol
	99% isopropyl alcohol, pure IPA
	 
	 

	
	Suitable for electronics cleaning & flux thinning
	 
	 

	
	1 Litre
	 
	 

	Alcohol Dispensing Bottle
	Twist-Lock pump can be locked with a simple twist.
	 
	 

	
	Pump action to dispense alcohol
	 
	 

	One Click Cleaner pen (2.5mm)
	Tool for cleaning the end-face of 2.5mm ferrule (SC, ST, FC and LSH)
	 
	 

	
	One-click single action cleaning system
	 
	 

	
	Suitable for cleaning plugs and connectors inside adapters
	 
	 

	
	Dry cleaning with antistatic tape
	 
	 

	
	Over 800 cleanings per unit
	 
	 

	One Click Cleaner pen (1.25mm)
	Tool for cleaning the end-face of 1.25mm ferrule (LC and MU)
	 
	 

	
	One-click single action cleaning system
	 
	 

	
	Suitable for cleaning plugs and connectors inside adapters
	 
	 

	
	Dry cleaning with antistatic tape
	 
	 

	
	Over 800 cleanings per unit
	 
	 

	Cleaning Cassette
	Weight :0.148 kg
	 
	 

	
	Dimensions :8.5 × 3.5 × 12.5 mm
	 
	 

	
	Cleaning times: 550
	 
	 

	
	Connector types :LC, SC, ST, FC
	 
	 

	
	Material Plastic :Casing
	 
	 

	
	Cable type :Single Mode
	 
	 

	
	Cleaning effect : '-20 ~ -50 dB
	 
	 

	
	Connector Qty. Duplex
	 
	 

	
	Insertion loss ≤0.3dB
	 
	 

	SC - SC Midcoupler
	Connector Type : SC-SC
	 
	 

	
	Body Style : Simplex
	 
	 

	
	Polish         : APC
	 
	 

	
	Fiber Type : Single Mode (9/125μm)
	 
	 

	
	Insertion Loss: ≤0.2dB
	 
	 

	
	Durability :1,000 times
	 
	 

	
	Mounting Type :Flanged
	 
	 

	
	Body Material PVC Plastic / Stainless Steel Clip
	 
	 

	
	Sleeve Material :Ceramic
	 
	 

	Splice Protectors
	Inner support stainless steel rod: 1.0mm
	 
	 

	
	Length : 40mm·
	 
	 

	
	Working temperature : -45 ~ 110 ℃
	 
	 

	
	Shrinking temperature range: 120 ℃
	 
	 

	
	Standard colour: Clear
	 
	 

	
	Outer tube material is made of polyolefin
	 
	 

	
	Inner tube material is made by EVA (ethylene-vinyl acetate)
	 
	 

	Item
	Description and technical requirements
	Complaint     (Yes/No)
	Comments

	Cable Stripper
	Dual purpose wire stripper and plastic tube cutting tool 
	 
	 

	
	Cuts and removes insulation from cable– quick and safe
	 
	 

	
	Automatically changes from circular to longitudinal cuts
	 
	 

	
	Adjustable cutting depth
	 
	 

	
	Cuts plastic tubing up to 25mm diameter
	 
	 

	
	Replaceable hardened blade
	 
	 



