{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Bills Of Quantities"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bills Of Quantities","index":0,"n_rows":1124,"n_cols":35,"rows_kept":1124,"flags":["formulas_cached_only"]}
["Page","Item","Description","Uom","Quantity","Rate","Amount","Total","x","Formatted Qty","x","Abstract RecID","x","Lcode","x","x","x","x","x","x","x","x","x","x","x","x","Package","Section","Bill","Trade","Type","ABUm","PayRef"]
[]
[null,null,"SECTION NO. 0 : Single Section",{"$nulls":23},1,0,1,-2,"H"]
[{"$nulls":34},"NOTE:  the column headings a - z must be present for the importer."]
[{"$nulls":34},"These contain an X which is set forecolor = white"]
[null,null,"BILL NO.1 : PRELIMINARIES",{"$nulls":23},1,0,1,-2,"H"]
[]
["1",null,"PRELIMINARY",{"$nulls":8},971,null,0,{"$nulls":12},1,0,1,-2,"H","0"]
[]
["1",null,"In accordance with project specification and SABS 1200A",{"$nulls":8},972,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1",null,"Fixed-Charge and Value-Related Items",{"$nulls":8},973,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1","1","Contractual requirements","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,974,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1",null,"Establishment of Facilities on site",{"$nulls":8},975,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1","2","Facilities for Contractor including offices and storage sheds, workshops, latrine facilities, laboratories, livings, accommodation, tools and  equipment, water and electrical power and plant , etc.","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,976,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1","3","Other fixed-charge obligations","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,977,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1","4","Removal of Site Establishment","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,978,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1","5","Facilities for Engineer","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,979,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1","6","Provide and erect Nameboards","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,980,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","7","Services Detection Equipment","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,981,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["1",null,"Time-Related Items",{"$nulls":8},982,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1","8","Contractual Requirements","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,983,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1",null,"Operation and Maintenance of Facilities on Site",{"$nulls":8},984,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1",null,"Facilities for Contractor including latrine facilities,",{"$nulls":8},985,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1","9","tools and equipment water and electrical power and","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,986,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1",null,"plant etc.",{"$nulls":8},987,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["1","10","Supervision for duration of Construction","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,988,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","11","Company and head offices overhead costs","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,989,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","12","Other time-related obligations","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,990,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","13","Facilities for Engineer","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,991,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","14","Testing ordered by the Engineer","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,992,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","15","Services Detection Equipment","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,993,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["1","16","Dealing with water during construction","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,994,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2",null,"Health and Safety",{"$nulls":8},995,null,0,{"$nulls":12},1,0,1,-2,"S","0"]
[]
["2","17","Submit Health and Safety File","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,996,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["2","18","Health and Safety Officer","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,997,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","19","Compliance with Occupation Health and Safety Act 2014","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,998,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","20","Allow provisions for height access mechanisms in at most two service ducts at a given time of full height of 4.5m for duration not exceeding 12 months","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,999,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","21","Environmental Management Plan","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1000,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["2","22","Maintain Nameboard","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1001,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","23","Security","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1002,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","24","Guarantees","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1003,null,0,{"$nulls":12},1,0,1,-2,"I","N"]
[]
["2","25","Transportation and disposal of removed material to a location nominated by the Engineer","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1004,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
["2","26","Other (Contractor to specify)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1005,null,0,{"$nulls":12},1,0,1,-2,"I","I"]
[]
[]
[null,null,"Bill Total",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[null,null,"BILL NO.2 : BLOCK A",{"$nulls":23},1,0,2,201,"H"]
[]
["4",null,"STEAM RETICULATION PIPING",{"$nulls":8},1029,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["4",null,"DECOMMISIONING",{"$nulls":8},1030,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["4","1","Removal of Existing pipe work for Steam in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the building in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1031,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["4",null,"Installation  of Steam pipes",{"$nulls":8},1032,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Supply, lift into position, install, test, set to work, and commission steam pipe  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as per installaion.",{"$nulls":8},1033,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Piping",{"$nulls":8},1034,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1035,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 80",{"$nulls":8},1036,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4","2","Diameter 20 mm (3/4 Inch)","m",{"v":120,"d":"120.00"},null,{"v":0,"d":"0.00"},null,null,120,null,1037,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["4","3","Diameter 40 mm (1 1/2 Inch)","m",{"v":180,"d":"180.00"},null,{"v":0,"d":"0.00"},null,null,180,null,1038,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["4",null,"Pipe Supports",{"$nulls":8},1039,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1040,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4","4","20mm/ (3/4 Inch) pipe support","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1041,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["4","5","40mm / (1 1/2 inch) pipe support","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1042,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["4",null,"Valves",{"$nulls":8},1043,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1044,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["4","6","Inline Strainer (20mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1045,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["4","7","Inline Strainer (25mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1046,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","8","Inline Strainer (32mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1047,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","9","Non -Return Valve  ( 25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1048,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","10","Gate Valve (20mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1049,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","11","Stainless Steel Ball Valve( 25mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1050,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","12","Stainelss Steel Ball Valve (32mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1051,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","13","Pressure Regulator Pressure Relief Valve ( 25mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1052,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","14","Pressure Regulator ( 25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1053,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","15","Actuator Valve (25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1054,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","16","Seperator ( 25mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1055,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","17","Steam Trap (25mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1056,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","18","Pressure Gauge (25mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1057,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["5","19","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1058,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["5",null,"CHILLER PLANT  RETICULATION PIPING",{"$nulls":8},1059,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["5","20","Removal of Existing pipe work for CHILLER WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1060,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["5",null,"REPLACEMENT   OF CHILLER RETICULATION PIPING",{"$nulls":8},1061,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["5",null,"Supply, lift into position, install, test, set to work, and commission chilled water Pipe Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1062,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["5",null,"Piping",{"$nulls":8},1063,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["5",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1064,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["5",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1065,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["5","21","Diameter 80 mm (3 Inch)","m",{"v":120,"d":"120.00"},null,{"v":0,"d":"0.00"},null,null,120,null,1066,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["5","22","Diameter 100 mm (4 Inch)","m",{"v":180,"d":"180.00"},null,{"v":0,"d":"0.00"},null,null,180,null,1067,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["6","23","Diameter 150 mm (6 Inch)","m",{"v":120,"d":"120.00"},null,{"v":0,"d":"0.00"},null,null,120,null,1068,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["6","24","Diameter 200mm (8 Inch)","m",{"v":140,"d":"140.00"},null,{"v":0,"d":"0.00"},null,null,140,null,1069,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["6",null,"Flanges",{"$nulls":8},1070,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6",null,"Allow for Table 1600  Weld on  Flanges,including gasket of equivalent pressure rating and bolts for coupling of pipe as per pipe sizes supplied",{"$nulls":8},1071,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6","25","80mm ( 3 Inch )","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1072,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","26","100mm( 4 Inch)","No",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1073,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","27","150mm(6 Inch)","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1074,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","28","200mm (8 Inch)","No",{"v":44,"d":"44.00"},null,{"v":0,"d":"0.00"},null,null,44,null,1075,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6",null,"Pipe Supports",{"$nulls":8},1076,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1077,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6","29","80mm","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1078,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","30","100mm","No",{"v":25,"d":"25.00"},null,{"v":0,"d":"0.00"},null,null,25,null,1079,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","31","150mm  bracket Pipe Support, Frabricated with Channel iron  to carry pipe across flange","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1080,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6",null,"Valves",{"$nulls":8},1081,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1082,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["6","32","Ball Valve (25MM)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1083,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","33","Ball Valve (80MM)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1084,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","34","Butterfly Valve (100mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1085,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","35","Wafer Type Valve (80mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1086,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","36","Wafer Type Valve( 150mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1087,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","37","2-Way Pneumatic Valve (40mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1088,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","38","2-Way Pneumatic Valve (80mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1089,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","39","3-Way Pneumatic Valve (80mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1090,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","40","Non-Return  Valve (40mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1091,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["6","41","Non-Return  Valve (80mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1092,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["7",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1093,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7","42","Thermometer (25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1094,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["7","43","Pressure gauge (25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1095,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["7","44","Building Management system Connection","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1096,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["7","45","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1097,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["7",null,"HOT WATER RETICULATION",{"$nulls":8},1098,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["7","46","Removal of Existing pipe work for HOT  WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1099,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["7",null,"REPLACEMENT   OF HOT WATER RETICULATION PIPING",{"$nulls":8},1100,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["7",null,"Supply, lift into position, install, test, set to work, and commission Hot Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1101,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7",null,"Piping",{"$nulls":8},1102,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints,Flanges galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1103,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1104,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7","47","Diameter 100 mm (4 Inch)","m",{"v":70,"d":"70.00"},null,{"v":0,"d":"0.00"},null,null,70,null,1105,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["7","48","Diameter 80 mm (3 Inch)","m",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1106,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["7","49","Diameter 40 mm (1 1/2 Inch)","m",{"v":50,"d":"50.00"},null,{"v":0,"d":"0.00"},null,null,50,null,1107,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["7",null,"Pipe Supports",{"$nulls":8},1108,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1109,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["7","50","80mm/ (3 Inch) pipe support","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1110,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["7","51","100mm / (4 inch) pipe support","No",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1111,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","52","40mm / (1 1/2 inch) pipe support","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1112,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8",null,"Valves",{"$nulls":8},1113,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["8",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1114,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["8","53","Ball Valve (25mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1115,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","54","Gate Valve (32mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1116,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","55","Gate Valve (100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1117,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","56","Strainer (40mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1118,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","57","Wafer Type Valve( 100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1119,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","58","2-Way Pneumatic Valve (40mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1120,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","59","3-Way Pneumatic Valve (80mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1121,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","60","3-Way Pneumatic Valve (100mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1122,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","61","Non-Return  Valve (40mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1123,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","62","Non-Return  Valve (80mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1124,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1125,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["8","63","Thermometer (25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1126,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","64","Pressure gauge (25mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1127,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","65","Building Management system Connection","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1128,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["8","66","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1129,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["8",null,"POTABLE WATER RETICULATION",{"$nulls":8},1130,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["8","67","Removal of Existing pipe work for Potable Water Piping in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1131,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["9",null,"REPLACEMENT   OF POTABLE  WATER RETICULATION PIPING",{"$nulls":8},1132,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["9",null,"Supply, lift into position, install, test, set to work, and commission potable Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1133,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9",null,"Piping",{"$nulls":8},1134,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1135,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1136,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9","68","Diameter 100 mm (4 Inch)","m",{"v":70,"d":"70.00"},null,{"v":0,"d":"0.00"},null,null,70,null,1137,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["9","69","Diameter 80 mm (3 Inch)","m",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1138,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["9","70","Diameter 40 mm (1 1/2 Inch)","m",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1139,null,0,{"$nulls":12},1,0,2,201,"I","1"]
[]
["9",null,"Pipe Supports",{"$nulls":8},1140,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1141,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9","71","80mm/ (3 Inch) pipe support","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1142,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","72","100mm / (4 inch) pipe support","No",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1143,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","73","40mm / (1 1/2 inch) pipe support","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1144,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9",null,"Valves",{"$nulls":8},1145,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1146,null,0,{"$nulls":12},1,0,2,201,"S","0"]
[]
["9","74","Ball Valve (25mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1147,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","75","Gate Valve (32mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1148,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","76","Gate Valve (100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1149,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","77","Strainer (40mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1150,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","78","Wafer Type Valve( 100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1151,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","79","Non-Return  Valve (40mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1152,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["9","80","Non-Return  Valve (80mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1153,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["10","81","Allowance for Pipe Monitoring System","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1154,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10",null,"PROJECT ENGINEERING AND QUALITY MANAGEMENT",{"$nulls":8},1155,null,0,{"$nulls":12},1,0,2,201,"H","0"]
[]
["10","82","Underground Services detection","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1156,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","83","Concealed services Detections (walls, Ceiling e.t.c)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1157,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","84","Testing of equipment in presence of Engineer","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1158,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","85","Commissioning of equipment","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1159,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","86","Certificate of Compliance (Every Installation)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1160,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","87","As-Built Drawings (3 copies every installation type)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1161,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","88","Engineer's tools, tests, & Software","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1162,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","89","Operation & Maintenance Maunuals for all installations (2 hard copies & 1 Digital)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1163,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
["10","90","12 Months Maintenance Period","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1164,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["10","91","6 months Liability Defects period","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1165,null,0,{"$nulls":12},1,0,2,201,"I","N"]
[]
["10","92","Any other omitted item for complete Installation.................................................................................................................................................................","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1166,null,0,{"$nulls":12},1,0,2,201,"I","I"]
[]
[]
[null,null,"Bill Total",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[null,null,"BILL NO.3 : BLOCK C",{"$nulls":23},1,0,3,202,"H"]
[]
["12",null,"STEAM RETICULATION PIPING",{"$nulls":8},1167,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["12",null,"DECOMMISIONING",{"$nulls":8},1168,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["12","1","Removal of Existing pipe work for Steam in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the building in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1169,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["12",null,"Installation  of Steam pipes",{"$nulls":8},1170,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12",null,"Supply, lift into position, install, test, set to work, and commission steam pipe  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as per installaion.",{"$nulls":8},1171,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12",null,"Piping",{"$nulls":8},1172,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1173,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1174,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12","2","Diameter 10 mm (3/8 Inch)","m",{"v":100,"d":"100.00"},null,{"v":0,"d":"0.00"},null,null,100,null,1175,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["12","3","Diameter 20 mm (3/4 Inch)","m",{"v":70,"d":"70.00"},null,{"v":0,"d":"0.00"},null,null,70,null,1176,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["12","4","Daimater 40mm (1 1/4 Inch)","m",{"v":200,"d":"200.00"},null,{"v":0,"d":"0.00"},null,null,200,null,1177,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["12",null,"Pipe Supports",{"$nulls":8},1178,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1179,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["12","5","10mm/ (3/8 Inch) pipe support","No",{"v":25,"d":"25.00"},null,{"v":0,"d":"0.00"},null,null,25,null,1180,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["12","6","20mm / (3/4 inch) pipe support","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1181,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["12","7","Daimater 40mm (1 3/5 inch)","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1182,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13",null,"Valves",{"$nulls":8},1183,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["13",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1184,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["13","8","Ball Valve (20mm)","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1185,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","9","Gate Valve (20mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1186,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","10","Gate Valve Valve (25mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1187,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","11","Ball Valve (25mm)","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1188,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","12","Pressure Regulator Pressure Relief Valve ( 25mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1189,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","13","Pressure Regulator Pressure Relief Valve ( 20mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1190,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","14","Pressure Regulator ( 25mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1191,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","15","Pressure Regulator (20mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1192,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","16","Separator ( 25mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1193,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","17","Separator ( 20mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1194,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","18","Steam Trap (25mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1195,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","19","Steam Trap (20mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1196,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","20","Pressure Gauge (25mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1197,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","21","Pressure Gauge (20mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1198,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","22","Allow for Pipe Lagging for all new installation pipe up to and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1199,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["13","23","2-way Pneumatic Valve (20mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1200,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13","24","2-way pneumatic valve (25mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1201,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["13",null,"CHILLER PLANT  RETICULATION PIPING",{"$nulls":8},1202,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["13","25","Removal of Existing pipe work for CHILLER WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1203,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["14",null,"REPLACEMENT   OF CHILLER RETICULATION PIPING",{"$nulls":8},1204,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["14",null,"Supply, lift into position, install, test, set to work, and commission chilled water Pipe Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1205,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14",null,"Piping",{"$nulls":8},1206,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1207,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1208,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14","26","Diameter 32 mm (1 1/4 Inch)","m",{"v":170,"d":"170.00"},null,{"v":0,"d":"0.00"},null,null,170,null,1209,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["14","27","Diameter 80 mm ( 3 Inch)","m",{"v":350,"d":"350.00"},null,{"v":0,"d":"0.00"},null,null,350,null,1210,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["14","28","Diameter 100 mm (4 Inch)","m",{"v":120,"d":"120.00"},null,{"v":0,"d":"0.00"},null,null,120,null,1211,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["14","29","Diameter 150 mm (6 Inch)","m",{"v":100,"d":"100.00"},null,{"v":0,"d":"0.00"},null,null,100,null,1212,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["14","30","Diameter 300 (12 Inch)","m",{"v":330,"d":"330.00"},null,{"v":0,"d":"0.00"},null,null,330,null,1213,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["14",null,"Flanges",{"$nulls":8},1214,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14",null,"Allow for Table 1600  Weld on  Flanges,including gasket of equivalent pressure rating and bolts for coupling of pipe as per pipe sizes supplied",{"$nulls":8},1215,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14","31","80mm ( 3 Inch )","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1216,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","32","100mm( 4 Inch)","No",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1217,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","33","150mm(6 Inch)","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1218,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","34","300mm (12 Inch)","No",{"v":44,"d":"44.00"},null,{"v":0,"d":"0.00"},null,null,44,null,1219,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14",null,"Pipe Supports",{"$nulls":8},1220,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1221,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["14","35","32mm","No",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1222,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","36","80mm","No",{"v":48,"d":"48.00"},null,{"v":0,"d":"0.00"},null,null,48,null,1223,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","37","100mm","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1224,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["14","38","150mm","No",{"v":66,"d":"66.00"},null,{"v":0,"d":"0.00"},null,null,66,null,1225,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","39","300mm  bracket Pipe Support, Frabricated with angle iron  to carry pipe across flange","No",{"v":66,"d":"66.00"},null,{"v":0,"d":"0.00"},null,null,66,null,1226,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15",null,"Valves",{"$nulls":8},1227,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["15",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1228,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["15","40","Ball Valve (25mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1229,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","41","Ball Valve (32mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1230,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","42","Pressure Gauge (25mm)","No",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1231,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","43","Pressure Gauge (40mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1232,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","44","Pressure Gauge (80mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1233,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","45","Wafer Type Valve (80mm)","No",{"v":36,"d":"36.00"},null,{"v":0,"d":"0.00"},null,null,36,null,1234,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","46","Strainer (80mm)","No",{"v":18,"d":"18.00"},null,{"v":0,"d":"0.00"},null,null,18,null,1235,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","47","2-Way Pneumatic Valve (40mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1236,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","48","2-Way Pneumatic Valve (50mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1237,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","49","2-Way Pneumatic Valve (80mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1238,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","50","2-Way Pneumatic Valve (100mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1239,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","51","3-Way Pneumatic Valve (80mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1240,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","52","3-Way Pneumatic Valve (150mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1241,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","53","3-Way Pneumatic Valve (200mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1242,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","54","Gate  Valve (80mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1243,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","55","Gate  Valve (100mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1244,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","56","Gate  Valve (150mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1245,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","57","Gate  Valve (200mm)","No",{"v":11,"d":"11.00"},null,{"v":0,"d":"0.00"},null,null,11,null,1246,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","58","Gate  Valve (300mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1247,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","59","Non-Return  Valve (80mm)","No",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1248,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1249,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["15","60","Thermometer (25mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1250,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["15","61","Thermometer (32mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1251,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16","62","Thermometer (150mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1252,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16","63","Building Management system Connection","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1253,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16","64","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1254,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16",null,"HOT WATER RETICULATION",{"$nulls":8},1255,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["16","65","Removal of Existing pipe work for HOT  WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1256,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["16",null,"REPLACEMENT   OF HOT WATER RETICULATION PIPING",{"$nulls":8},1257,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["16",null,"Supply, lift into position, install, test, set to work, and commission Hot Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1258,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16",null,"Piping",{"$nulls":8},1259,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints,Flanges galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1260,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1261,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16","66","Diameter 32 mm (1 1/4 Inch)","m",{"v":210,"d":"210.00"},null,{"v":0,"d":"0.00"},null,null,210,null,1262,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["16",null,"Pipe Supports",{"$nulls":8},1263,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1264,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16","67","32mm/ (1 1/4 Inch) pipe support","No",{"v":65,"d":"65.00"},null,{"v":0,"d":"0.00"},null,null,65,null,1265,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16",null,"Valves",{"$nulls":8},1266,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1267,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["16","68","Ball Valve (15mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1268,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16","69","Gate Valve (20mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1269,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["16","70","Gate Valve (25mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1270,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","71","Gate Valve (40mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1271,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","72","Pressure gauge (40mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1272,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","73","2-Way Pneumatic Valve (40mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1273,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","74","3-Way Pneumatic Valve (40mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1274,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","75","3-Way Pneumatic Valve (50mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1275,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1276,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["17","76","Thermometer (40mm)","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1277,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","77","Thermometer (50mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1278,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","78","Building Management system Connection","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1279,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["17","79","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Prov Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1280,null,0,{"$nulls":12},1,0,3,202,"I","PS"]
[]
["17",null,"POTABLE WATER RETICULATION",{"$nulls":8},1281,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["17","80","Removal of Existing pipe work for Potable Water Piping in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1282,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["17",null,"REPLACEMENT   OF POTABLE  WATER RETICULATION PIPING",{"$nulls":8},1283,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["17",null,"Supply, lift into position, install, test, set to work, and commission potable Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1284,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["17",null,"Piping",{"$nulls":8},1285,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["17",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1286,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["17",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1287,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["17","81","Diameter 20 mm","m",{"v":33,"d":"33.00"},null,{"v":0,"d":"0.00"},null,null,33,null,1288,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["17","82","Diameter 25 mm","m",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1289,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","83","Diameter 30 mm","m",{"v":46,"d":"46.00"},null,{"v":0,"d":"0.00"},null,null,46,null,1290,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","84","Diameter 32 mm","m",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1291,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","85","Diameter 35 mm","m",{"v":62,"d":"62.00"},null,{"v":0,"d":"0.00"},null,null,62,null,1292,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","86","Diameter 40 mm","m",{"v":145,"d":"145.00"},null,{"v":0,"d":"0.00"},null,null,145,null,1293,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","87","Diameter 50 mm","m",{"v":35,"d":"35.00"},null,{"v":0,"d":"0.00"},null,null,35,null,1294,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18","88","Diameter 60 mm","m",{"v":35,"d":"35.00"},null,{"v":0,"d":"0.00"},null,null,35,null,1295,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["18",null,"Pipe Supports",{"$nulls":8},1296,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["18",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1297,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["18","89","80mm/ (3 Inch) pipe support","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1298,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","90","100mm / (4 inch) pipe support","No",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1299,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","91","40mm / (1 1/2 inch) pipe support","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1300,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18",null,"Valves",{"$nulls":8},1301,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["18",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1302,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["18","92","Ball Valve (25mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1303,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","93","Gate Valve (32mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1304,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","94","Gate Valve (100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1305,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","95","Strainer (40mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1306,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","96","Wafer Type Valve( 100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1307,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","97","Non-Return  Valve (40mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1308,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["18","98","Non-Return  Valve (80mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1309,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["19",null,"FIRE WATER RETICULATION",{"$nulls":8},1310,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"Removal of Existing pipe work for Fire Water Piping in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .",{"$nulls":8},1311,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"REPLACEMENT   OF FIRE  WATER RETICULATION PIPING",{"$nulls":8},1312,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["19",null,"Supply, lift into position, install, test, set to work, and commission potable Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1313,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"Piping",{"$nulls":8},1314,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1315,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"Galvanised Steel pipe",{"$nulls":8},1316,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19","99","Diameter 80 mm (3 Inch)","m",{"v":60,"d":"60.00"},null,{"v":0,"d":"0.00"},null,null,60,null,1317,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["19","100","Diameter 100 mm (4 Inch)","m",{"v":240,"d":"240.00"},null,{"v":0,"d":"0.00"},null,null,240,null,1318,null,0,{"$nulls":12},1,0,3,202,"I","1"]
[]
["19",null,"Pipe Supports",{"$nulls":8},1319,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1320,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19","101","80mm/ (3 Inch) pipe support","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1321,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["19","102","100mm / (4 inch) pipe support","No",{"v":35,"d":"35.00"},null,{"v":0,"d":"0.00"},null,null,35,null,1322,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["19",null,"Fire Hydrant",{"$nulls":8},1323,null,0,{"$nulls":12},1,0,3,202,"S","0"]
[]
["19","103","Single Fire Hydrant","No",{"v":22,"d":"22.00"},null,{"v":0,"d":"0.00"},null,null,22,null,1324,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["19","104","Fire Hose Reel","No",{"v":22,"d":"22.00"},null,{"v":0,"d":"0.00"},null,null,22,null,1325,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["19",null,"Reticulation",{"$nulls":8},1326,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["19","105","Allowance for Pipe Monitoring System","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1327,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["19",null,"PROJECT ENGINEERING AND QUALITY MANAGEMENT",{"$nulls":8},1328,null,0,{"$nulls":12},1,0,3,202,"H","0"]
[]
["19","106","Underground Services detection","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1329,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","107","Concealed services Detections (walls, Ceiling e.t.c)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1330,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","108","Testing of equipment in presence of Engineer","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1331,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","109","Commissioning of equipment","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1332,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","110","Certificate of Compliance (Every Installation)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1333,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","111","As-Built Drawings (3 copies every installation type)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1334,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","112","Engineer's tools, tests, & Software","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1335,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","113","Operation & Maintenance Maunuals for all installations (2 hard copies & 1 Digital)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1336,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
["20","114","12 Months Maintenance Period","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1337,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["20","115","6 months Liability Defects period","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1338,null,0,{"$nulls":12},1,0,3,202,"I","N"]
[]
["20","116","Any other omitted item for complete Installation.................................................................................................................................................................","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1339,null,0,{"$nulls":12},1,0,3,202,"I","I"]
[]
[]
[null,null,"Bill Total",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[null,null,"BILL NO.4 : BLOCK HG / HL",{"$nulls":23},1,0,4,203,"H"]
[]
["22",null,"STEAM RETICULATION PIPING",{"$nulls":8},1340,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["22",null,"DECOMMISIONING",{"$nulls":8},1341,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["22","1","Removal of Existing pipe work for Steam in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the building in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1342,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["22",null,"Installation  of Steam pipes",{"$nulls":8},1343,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22",null,"Supply, lift into position, install, test, set to work, and commission steam pipe  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as per installaion.",{"$nulls":8},1344,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22",null,"Piping",{"$nulls":8},1345,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1346,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 80",{"$nulls":8},1347,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22","2","Diameter 20 mm (3/4 Inch)","m",{"v":18,"d":"18.00"},null,{"v":0,"d":"0.00"},null,null,18,null,1348,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["22","3","Diameter 40 mm (1 1/2 Inch)","m",{"v":70,"d":"70.00"},null,{"v":0,"d":"0.00"},null,null,70,null,1349,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["22","4","Diameter 80 mm (3 Inch)","m",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1350,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["22",null,"Pipe Supports",{"$nulls":8},1351,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1352,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["22","5","20mm/ (3/4 Inch) pipe support","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1353,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["22","6","40mm / (1 1/2 inch) pipe support","No",{"v":82,"d":"82.00"},null,{"v":0,"d":"0.00"},null,null,82,null,1354,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["22","7","Diameter 80 mm /(3 Inch) pipe support","No",{"v":3,"d":"3.00"},null,{"v":0,"d":"0.00"},null,null,3,null,1355,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23",null,"Valves",{"$nulls":8},1356,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["23",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1357,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["23","8","Ball Valve (40mm)","No",{"v":14,"d":"14.00"},null,{"v":0,"d":"0.00"},null,null,14,null,1358,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","9","Gate Valve (40mm)","No",{"v":18,"d":"18.00"},null,{"v":0,"d":"0.00"},null,null,18,null,1359,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","10","Pressure Regulator Pressure Relief Valve ( 40mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1360,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","11","Separator ( 40mm)","No",{"v":11,"d":"11.00"},null,{"v":0,"d":"0.00"},null,null,11,null,1361,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","12","Steam Trap (40mm)","No",{"v":19,"d":"19.00"},null,{"v":0,"d":"0.00"},null,null,19,null,1362,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","13","Pressure Gauge (20mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1363,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","14","Allow for Pipe Lagging for all new installation pipe up to and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1364,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["23","15","Actuator Valve (25mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1365,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","16","pneumatic valve (40mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1366,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","17","Strainer (50mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1367,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23","18","Non Return Valve (40mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1368,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["23",null,"CHILLER PLANT  RETICULATION PIPING",{"$nulls":8},1369,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["23","19","Removal of Existing pipe work for CHILLER WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1370,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["24",null,"REPLACEMENT   OF CHILLER RETICULATION PIPING",{"$nulls":8},1371,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["24",null,"Supply, lift into position, install, test, set to work, and commission chilled water Pipe Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1372,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Piping",{"$nulls":8},1373,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1374,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1375,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24","20","Diameter 40 mm (1 1/2 Inch)","m",{"v":151,"d":"151.00"},null,{"v":0,"d":"0.00"},null,null,151,null,1376,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["24","21","Diameter 80 mm ( 3 Inch)","m",{"v":104,"d":"104.00"},null,{"v":0,"d":"0.00"},null,null,104,null,1377,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["24",null,"Flanges",{"$nulls":8},1378,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Allow for Table 1600  Weld on  Flanges,including gasket of equivalent pressure rating and bolts for coupling of pipe as per pipe sizes supplied",{"$nulls":8},1379,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24","22","80mm ( 3 Inch )","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1380,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24",null,"Pipe Supports",{"$nulls":8},1381,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1382,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24","23","40mm","No",{"v":38,"d":"38.00"},null,{"v":0,"d":"0.00"},null,null,38,null,1383,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24","24","80mm","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1384,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24",null,"Valves",{"$nulls":8},1385,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1386,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["24","25","Ball Valve (25mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1387,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24","26","Ball Valve (50mm)","No",{"v":27,"d":"27.00"},null,{"v":0,"d":"0.00"},null,null,27,null,1388,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24","27","Ball Valve (80mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1389,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24","28","Pressure Gauge (20mm)","No",{"v":16,"d":"16.00"},null,{"v":0,"d":"0.00"},null,null,16,null,1390,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["24","29","Wafer Type Valve (80mm)","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1391,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","30","Strainer (50mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1392,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","31","Actuator Valve (25mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1393,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","32","Actuator Valve (40mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1394,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","33","Actuator Valve (80mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1395,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","34","Pneumatic Valve (80mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1396,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","35","Non-Return Valve (50mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1397,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","36","Non-Return  Valve (80mm)","No",{"v":24,"d":"24.00"},null,{"v":0,"d":"0.00"},null,null,24,null,1398,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1399,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["25","37","Thermometer (20mm)","No",{"v":14,"d":"14.00"},null,{"v":0,"d":"0.00"},null,null,14,null,1400,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","38","Building Management system Connection","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1401,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["25","39","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1402,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["25",null,"Hot Water Reticulation",{"$nulls":8},1403,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["25","40","Removal of Existing pipe work for HOT  WATER PIPING in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1404,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["25",null,"REPLACEMENT   OF HOT WATER RETICULATION PIPING",{"$nulls":8},1405,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["25",null,"Supply, lift into position, install, test, set to work, and commission Hot Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1406,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["25",null,"Piping",{"$nulls":8},1407,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["25",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints,Flanges galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1408,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["25",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1409,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["25","41","Diameter 40 mm (1 1/2 Inch)","m",{"v":198,"d":"198.00"},null,{"v":0,"d":"0.00"},null,null,198,null,1410,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["25","42","Diameter 80 mm (3 Inch)","m",{"v":89,"d":"89.00"},null,{"v":0,"d":"0.00"},null,null,89,null,1411,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["26",null,"Pipe Supports",{"$nulls":8},1412,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["26",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1413,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["26","43","40mm/ (1 1/2 Inch) pipe support","No",{"v":50,"d":"50.00"},null,{"v":0,"d":"0.00"},null,null,50,null,1414,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","44","Diameter 80 mm (3 Inch) pipe support","No",{"v":25,"d":"25.00"},null,{"v":0,"d":"0.00"},null,null,25,null,1415,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26",null,"Valves",{"$nulls":8},1416,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["26",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1417,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["26","45","Ball Valve (25mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1418,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","46","Ball Valve (32mm)","No",{"v":3,"d":"3.00"},null,{"v":0,"d":"0.00"},null,null,3,null,1419,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","47","Ball Valve (50mm)","No",{"v":19,"d":"19.00"},null,{"v":0,"d":"0.00"},null,null,19,null,1420,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","48","Ball Valve (80mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1421,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","49","Pressure gauge (20mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1422,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","50","Non-Return Valve (50mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1423,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","51","Non-Return Valve (80mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1424,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","52","Temperature gauge (20mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1425,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","53","Actuator Valve (40mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1426,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","54","Actuator Valve (80mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1427,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","55","Gate valve (50mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1428,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","56","Gate valve (80mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1429,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","57","strainer (50mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1430,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","58","strainer (80mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1431,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1432,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["26","59","Thermometer (40mm)","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1433,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","60","Thermometer (50mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1434,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","61","Building Management system Connection","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1435,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["26","62","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1436,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["27",null,"Potable Water Reticulation",{"$nulls":8},1437,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["27","63","Removal of Existing pipe work for Potable Water Piping in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1438,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["27",null,"REPLACEMENT OF POTABLE  WATER RETICULATION PIPING",{"$nulls":8},1439,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["27",null,"Supply, lift into position, install, test, set to work, and commission potable Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1440,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Piping",{"$nulls":8},1441,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1442,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1443,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27","64","Diameter 40 mm (1 1/2 Inch)","m",{"v":198,"d":"198.00"},null,{"v":0,"d":"0.00"},null,null,198,null,1444,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["27","65","Diameter 80 mm (3 Inch)","m",{"v":89,"d":"89.00"},null,{"v":0,"d":"0.00"},null,null,89,null,1445,null,0,{"$nulls":12},1,0,4,203,"I","1"]
[]
["27",null,"Flanges",{"$nulls":8},1446,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Allow for Table 1600  Weld on  Flanges,including gasket of equivalent pressure rating and bolts for coupling of pipe as per pipe sizes supplied",{"$nulls":8},1447,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27","66","80mm ( 3 Inch )","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1448,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["27",null,"Pipe Supports",{"$nulls":8},1449,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1450,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27","67","40mm/ (1 1/2 Inch) pipe support","No",{"v":50,"d":"50.00"},null,{"v":0,"d":"0.00"},null,null,50,null,1451,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["27","68","Diameter 80 mm (3 Inch) pipe support","No",{"v":25,"d":"25.00"},null,{"v":0,"d":"0.00"},null,null,25,null,1452,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["27",null,"Valves",{"$nulls":8},1453,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27",null,"Supply, install, test , set to work, and commission  in service duct, including valve fittings as per current setup  of installation",{"$nulls":8},1454,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["27","69","80mm/ (3 Inch) pipe support","No",{"v":40,"d":"40.00"},null,{"v":0,"d":"0.00"},null,null,40,null,1455,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","70","100mm / (4 inch) pipe support","No",{"v":20,"d":"20.00"},null,{"v":0,"d":"0.00"},null,null,20,null,1456,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","71","40mm / (1 1/2 inch) pipe support","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1457,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","72","Ball Valve (25mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1458,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","73","Gate Valve (32mm)","No",{"v":8,"d":"8.00"},null,{"v":0,"d":"0.00"},null,null,8,null,1459,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","74","Gate Valve (100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1460,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","75","Strainer (40mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1461,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","76","Wafer Type Valve( 100mm)","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1462,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","77","Non-Return  Valve (40mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1463,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","78","Non-Return  Valve (80mm)","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1464,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28",null,"Potable Water Reticulation",{"$nulls":8},1465,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"Removal of Existing pipe work for Potable Water Piping in service duct , through work platform not exceeding 500mm from finish floor level and 500mm through sofit level. Procedure shall ensure no interruption of services in  the other service areas of the builing in exception of the shaft being worked on .",{"$nulls":8},1466,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"REPLACEMENT   OF PORTABLE WATER RETICULATION PIPING",{"$nulls":8},1467,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["28",null,"Supply, lift into position, install, test, set to work, and commission potable Water  Reticulation pipes  and Valves as per schedule below to ensure entire service duct  including provide of lagging of pipe  as existing installation in each service duct.",{"$nulls":8},1468,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"Piping",{"$nulls":8},1469,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"Supply, lift into position, install, test, set to work, and commission  in service duct, including, grooved fittings expansion joints, galvanized hangers and supports and  corrosion painting as per installation  and additional as directed by Engineer",{"$nulls":8},1470,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"Carbon  Steel ASME 16.9 A106 pipe ,Schedule 40",{"$nulls":8},1471,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28","79","Diameter 80 mm (3 Inch)","No",{"v":24,"d":"24.00"},null,{"v":0,"d":"0.00"},null,null,24,null,1472,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28","80","Diameter 100 mm (4 Inch)","No",{"v":140,"d":"140.00"},null,{"v":0,"d":"0.00"},null,null,140,null,1473,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["28",null,"Flanges",{"$nulls":8},1474,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28",null,"Allow for Table 1600  Weld on  Flanges,including gasket of equivalent pressure rating and bolts for coupling of pipe as per pipe sizes supplied",{"$nulls":8},1475,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["28","81","80mm ( 3 Inch )","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"},null,null,30,null,1476,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29",null,"Pipe Supports",{"$nulls":8},1477,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["29",null,"Allow for Pipe support to in installed together with  new piping in service duct, Pipe support should have all wall anchor bolt in  place and thread / steel rod of not more that 300mm",{"$nulls":8},1478,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["29","82","80mm/ (3 Inch) pipe support","No",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"},null,null,4,null,1479,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","83","100mm / (4 inch) pipe support","No",{"v":35,"d":"35.00"},null,{"v":0,"d":"0.00"},null,null,35,null,1480,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","84","Ball Valve (25mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1481,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","85","Ball Valve (32mm)","No",{"v":3,"d":"3.00"},null,{"v":0,"d":"0.00"},null,null,3,null,1482,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","86","Ball Valve (50mm)","No",{"v":19,"d":"19.00"},null,{"v":0,"d":"0.00"},null,null,19,null,1483,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","87","Ball Valve (80mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1484,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","88","Pressure gauge (20mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1485,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","89","Non-Return Valve (50mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1486,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","90","Non-Return Valve (80mm)","No",{"v":7,"d":"7.00"},null,{"v":0,"d":"0.00"},null,null,7,null,1487,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","91","Temperature gauge (20mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1488,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","92","Actuator Valve (40mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1489,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","93","Actuator Valve (80mm)","No",{"v":9,"d":"9.00"},null,{"v":0,"d":"0.00"},null,null,9,null,1490,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","94","Gate valve (50mm)","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1491,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","95","Gate valve (80mm)","No",{"v":10,"d":"10.00"},null,{"v":0,"d":"0.00"},null,null,10,null,1492,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","96","strainer (50mm)","No",{"v":5,"d":"5.00"},null,{"v":0,"d":"0.00"},null,null,5,null,1493,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","97","strainer (80mm)","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1494,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29",null,"Supply , install Instruments for monitoring Devices  to be coupled to devices and to be inline with pipe installation",{"$nulls":8},1495,null,0,{"$nulls":12},1,0,4,203,"S","0"]
[]
["29","98","Thermometer (40mm)","No",{"v":15,"d":"15.00"},null,{"v":0,"d":"0.00"},null,null,15,null,1496,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","99","Thermometer (50mm)","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1497,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","100","Building Management system Connection","No",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"},null,null,2,null,1498,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["29","101","Allow for Pipe Lagging for all new installation pipe upto and including tie in to branch pipe","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1499,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["29","102","Allowance for Pipe Monitoring System","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1500,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30",null,"PROJECT ENGINEERING AND QUALITY MANAGEMENT",{"$nulls":8},1501,null,0,{"$nulls":12},1,0,4,203,"H","0"]
[]
["30","103","Underground Services detection","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1502,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","104","Concealed services Detections (walls, Ceiling e.t.c)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1503,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","105","Testing of equipment in presence of Engineer","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1504,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","106","Commissioning of equipment","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1505,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","107","Certificate of Compliance (Every Installation)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1506,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","108","As-Built Drawings (3 copies every installation type)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1507,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","109","Engineer's tools, tests, & Software","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1508,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","110","Operation & Maintenance Maunuals for all installations (2 hard copies & 1 Digital)","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1509,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
["30","111","12 Months Maintenance Period","No",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"},null,null,12,null,1510,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["30","112","6 months Liability Defects period","No",{"v":6,"d":"6.00"},null,{"v":0,"d":"0.00"},null,null,6,null,1511,null,0,{"$nulls":12},1,0,4,203,"I","N"]
[]
["30","113","Any other omitted item for complete Installation.................................................................................................................................................................","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1512,null,0,{"$nulls":12},1,0,4,203,"I","I"]
[]
[]
[null,null,"Bill Total",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[null,null,"BILL NO.5 : PROVISIONAL SUMS",{"$nulls":23},1,0,5,99,"H"]
[]
["32",null,"SPECIALIST ENGINEERING SERVICES",{"$nulls":8},1006,null,100,{"$nulls":12},1,0,5,99,"H","0"]
[]
["32","1","Provide the amount of R2 250 000.00 (Two Million Two Hundred and Fifty Thousand  Rand) for Specialist Engineering Services (Civil, Structural, Electrical, etc), statutory applications and approvals as required for the successful execution of the contract","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1007,null,77550,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","2","Profit","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1008,null,77560,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","3","Attendance","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1009,null,77570,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32",null,"INSPECTION AND CERTIFICATION OF WORKS",{"$nulls":8},1010,null,77580,{"$nulls":12},1,0,5,99,"S","0"]
[]
["32","4","Provide the amount of R300 000.00 (Three Hundred Thousand Rand) for the inspection and certification of existing work after alterations.","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1011,null,77590,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","5","Profit","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1012,null,77600,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","6","Attendance","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1013,null,77610,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32",null,"COMMUNITY LIAISON OFFICER",{"$nulls":8},1014,null,77620,{"$nulls":12},1,0,5,99,"S","0"]
[]
["32","7","Provide the amount of R 10 000.00 (Ten Thousand Rand) per month for the Community Liaison Officer for a period of Six months.","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1015,null,77630,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","8","Profit","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1016,null,77640,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","9","Attendance","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1017,null,77650,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32",null,"BUILDERS WORKS",{"$nulls":8},1018,null,77660,{"$nulls":12},1,0,5,99,"S","0"]
[]
["32","10","Provide the amount of R1 500 000.00 (One Million and  Five Hundred Thousand  Rand) for Builder works for closing up penetration holes through duct and ensuring fire proof seals","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1019,null,77670,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","11","Profit","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1020,null,77680,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","12","Attendance","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1021,null,77690,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32",null,"AS BUILT DRAWINGS",{"$nulls":8},1022,null,77700,{"$nulls":12},1,0,5,99,"S","0"]
[]
["32","13","Provide the amount of R600 000.00 (Six Hundred Thousand Rand) for the production of as-built drawings","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1023,null,77710,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","14","Profit","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1024,null,77720,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32","15","Attendance","Item",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},null,null,1,null,1025,null,77730,{"$nulls":12},1,0,5,99,"I","I"]
[]
["32",null,"BUDGETARY ALLOWANCES",{"$nulls":8},1026,null,75520,{"$nulls":12},1,0,5,99,"H","0"]
[]
["32",null,"Escalation Allowance",{"$nulls":8},1027,null,75530,{"$nulls":12},1,0,5,99,"S","0"]
[]
["32","16","Provide the amount of R 3 000,000.00 (Three million Rands) for Escalation","Item",null,null,{"v":0,"d":"0.00"},null,null,1,null,1028,null,75540,{"$nulls":12},1,0,5,99,"I","I"]
[]
[]
[null,null,"Bill Total",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[null,null,"Section Total ",{"$nulls":4},{"v":0,"d":"0.00"}]