WATER LEVEL DATALOGGER SPECIFICATIONS

Date compiled: 18 August 2025

Solinst Levelogger 5 is the mostly recommended one
	WATER LEVEL DATALOGGER SPECIFICATIONS

	

	Level Sensor:
	Piezoresistive Silicon with Hastelloy Sensor

	Accuracy:
	± 0.05% FS (Barologger 5: ± 0.05 kPa)

	Stability of Readings:
	Superior, low noise

	Resolution:
	0.002% FS to 0.0006% FS

	Units of Measure:
	m, cm, ft., psi, kPa, bar, ºC. ºF (Barologger 5: psi, kPa, mbar, ºC, ºF)

	Normalization:
	Automatic Temperature Compensation

	Temp. Comp. Range:
	0º to 50ºC (Barologger 5: -10 to +50ºC)

	
	

	Temperature Sensor:
	Platinum Resistance Temperature Detector (RTD)

	Temp. Sensor Accuracy:
	± 0.05ºC

	Temp. Sensor Resolution:
	0.003°C

	Battery Life:
	10 Years - based on 1 reading/minute

	Clock Accuracy:
	± 1 minute/year (-20ºC to 80ºC)

	Operating Temperature:
	-20ºC to 80ºC

	Maximum # Readings:
	150,000 sets of readings

	Memory Mode:
	Slate and Continuous

	Communication:
	Optical high-speed: USB, SDI-12
57,600 bps with USB

	Size:
	22 mm x 160 mm (7/8" x 6.3")

	Weight:
	146 grams (5.2 oz)

	Corrosion Resistance:
	Baked-on coating using polymerization
technology (inside and out)

	Other Wetted Materials:
	Delrin®, Viton®, 316L stainless steel, Hastelloy,
PFAS-free PTFE coating

	Sampling Modes:
	Linear, Event & User-Selectable with Repeat Mode, Future Start, Future Stop, Real-Time View

	Measurement Rates:
	1/8 sec to 99 hrs

	Barometric Compensation:
	Software Wizard and one Barologger 5 in local area (approx. 30 km/20 miles radius)
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