{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["OHTE Small Components Scope"],"read":"whole","date_system":"1900"}

{"sheet":"OHTE Small Components Scope","index":0,"n_rows":230,"n_cols":8,"rows_kept":230,"merged":[[0,0,0,7],[1,5,2,5],[1,6,2,6],[1,7,2,7],[2,0,2,4],[14,0,14,7],[25,0,25,7],[28,0,28,7],[60,0,60,7],[62,0,62,7],[81,0,81,7],[109,0,109,7],[113,0,113,7],[128,0,128,7],[136,0,136,7],[168,0,168,7],[176,0,176,7],[187,0,187,7],[201,0,201,7],[211,0,211,7],[217,0,217,7]]}
["OHTE SMALL COMPONENTS SCOPE"]
["#","Item Numbers","Description","Unit of measure","Drawing/Specification","Bidder/OEM Drawing/Spec/technical datasheet Returned?\nYES/NO","Qauntity ","Unite Price "]
["CATEGORY A"]
[1,54033494,"SPLICE, CONDUCTOR; TYPE: TENSION, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3593BBB 3591BBB 3597; EQUIPMENT USED ON OHTE; SUITABLE FOR 800 MM SQ ACSR TO 800 MM SQ AAC WIRE.(CODE NAME LAPWING TO BULL)","EA","BBB 3593\nBBB 3591\nBBB 3597",null,1]
[2,"\n\n54033469","SPLICE, CONDUCTOR; TYPE: TENSION SPLICE, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3594BBB 3593BBB 3592; SUITABLE FOR 500 MM SQ ACSR TO 500 MM SQ ACSR WIRE (CODE NAME DEER TO DEER)","EA","BBB 3594\nBBB 3593\nBBB 3592",null,1]
[3,54033470,"SPLICE, CONDUCTOR; TYPE: TENSION, MATERIAL: ALUMINIUM; DRAWING NO: BBB 3593, LA; BBB 3592, LA; BBB 3595, LA; EQUIPMENT USED ON OHTE; SUITABLE FOR 800 MM SQ ACSR TO 800 MM SQ ACSR WIRE (CODE NAME LAPWING TO LAPWING)","EA","BBB 3593\nBBB 3592\nBBB 3595",null,1]
[4,54033445,"ATTACHMENT; TYPE: DEAD END, APPLICATION: FEEDER TERMINATION; DRAWING NO: BBB 3590, LA; BBB 3589, LA; BBB 3596, LA; EQUIPMENT USED ON OHTE SUITABLE FOR 500 MM2 FEEDER WIRE","EA","BBB 3590\nBBB 3589\nBBB 3596",null,1]
[5,54000944,"SPLICE, CONDUCTOR; TYPE: FEEDER, MATERIAL: ALUMINIUM; DRAWING NO: CEE-TNB-0024; SPECIFICATION: CEE.0038/83; SUITABLE FOR 500MM2 FEEDER WIRE ","EA","CEE-TNB-0024\nCEE.0038/83",null,1]
["CATEGORY B"]
[1,54016913,"SPLICE, CONDUCTOR; EQUIPMENT USED ON OHTE; PREFORMED SPIRAL; FOR JOINING 50 MM SQ ALUMINIUM WIRE ACSR 6/1/3,35 STRANDING RABBIT","EA","Technical Datasheet",null,1]
[2,54009096,"SPLICE, CONDUCTOR; TYPE: PREFORMED; EQUIPMENT USED ON OHTE; FULL TENSION SPLICE SUITABLE FOR USE ON CONDUCTOR WITH 30/7/2,36 STRANDING ACSR WIRE (TIGER WIRE) DIA 16.52 MM.","EA","Technical Datasheet",null,1]
[3,54005531,"SPLICE, CONDUCTOR;  EQUIPMENT USED ON 5405802; PREFORMED SPIRAL; FOR JOINING 160 SQ MM ALUMINIUM WIRE 19/3,25 MM STRANDING (HORNET) ","EA","Technical Datasheet",null,1]
[4,54000207,"GRIP; TYPE: PREFORMED DEAD END, MATERIAL: ALUMINIUM WIRE; DRAWING NO: SSE-208228, LA; 8MM; OVERHEAD TRACK; VICTORY ELECTRICAL CAPE TOWN; SALDANHA","EA","SSE-208228\nH500110-3-133-E-DE-0091",null,1]
[5,54010799,"GRIP; TYPE: PREFORMED DEAD END; SUITABLE FOR USE ON 131,23/30,62/160 SQ MM TIGER 30/7/2,36 STRANDING ACSR WIRE DIA 16,52 MM. COLOUR CODE BROWN.","EA","Technical Datasheet",null,1]
["CATEGORY C"]
[1,54112448,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 100 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[2,54112449,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 120 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[3,54112450,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 150 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[4,54112451,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 160 MM2, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[5,54112445,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 50 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[6,54112446,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 70 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[7,54005607,"TERMINAL, LUG; TYPE: COMPRESSION, WIRE SIZE ACCOMMODATED: 160 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM, ATTACHMENT METHOD: CRIMPING; DRAWING NO: CEE-TZ1-0121 SHEET 37, LA","EA","CEE-TZ1-0121 SHEET 37",null,1]
[8,54017109,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 95 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: ALUMINIUM; DRAWING NO: CEE-TU-0136, LA","EA","CEE-TU-0136",null,1]
[9,54031697,"TERMINAL, LUG; TYPE: CRIMPING, WIRE SIZE ACCOMMODATED: 95 MM2, HOLE QUANTITY: 1, TERMINAL MATERIAL: TINNED COPPER, SPECIAL FEATURES: M16 STUD; DRAWING NO: BBH 1332 SHEET 1, LA","EA","BBH 1332 SHEET 1",null,1]
[10,54017122,"TERMINAL, LUG; TYPE: BOND FASTENER, WIRE SIZE ACCOMMODATED: 150 MM2, HOLE QUANTITY: 1; DRAWING NO: CEE-TU-0136, LA; EQUIPMENT USED ON OHTE","EA","CEE-TU-0136",null,1]
["CATEGORY D"]
[1,54001076,"INSULATOR ASSEMBLY; TYPE: SUSPENSION, INSULATOR MATERIAL: PORCELAIN; DRAWING NO: CEE-TNC-0018, LA","EA","CEE-TNC-0018",null,1]
[2,54016901,"GREASE; TYPE: ELECTRICAL JOINTING COMPOUND, TRADE NAME: OXIDATION INHIBITION; TO BE SUPPLIED IN 1 KG TINS. BIDDERS ARE REQUIRED TO SUBMIT A TECHNICAL DATASHEET OF THE COMPOUND. ITEM USED ON ALUMINIUM CONDUCTORS FOR OXIDATION INHIBITION.","KG","Technical Datasheet",null,1]
["CATEGORY E"]
[1,54017021,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: 11 TO 13 MM WIRE; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121 DATE 2000 , LA; ITEM USED ON OHTE","EA","BBH 1889",null,1]
[2,54001201,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 16 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA","EA","BBH 1889",null,1]
[3,54032590,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 22 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA","EA","BBH 1889",null,1]
[4,54003859,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 11 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA","EA","BBH 1889",null,1]
[5,54003872,"ASSEMBLY; TYPE: CROSBY CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: DIA 16 MM; DRAWING NO: BBH 1889, LA; SPECIFICATION: SANS 121, LA; WIRE SIZE ACCOMODATED DIA 19 MM","EA","BBH 1889",null,1]
[6,54006363,"SHACKLE; SHACKLE MATERIAL: STAINLESS STEEL, MATERIAL GRADE: 316; DRAWING NO: SSE-208 211 ; OHTE CATENARY SYSTEM ","EA","SSE-208 211",null,1]
[7,54009780,"ADAPTOR, INSULATOR; TYPE: STEADY ARM, DIMENSIONS: OD 42 MM, APPLICATION: OVERHEAD TRACK EQUIPMENT; DRAWING NO: CEE-TZ-9/27, 0; HOLDER, STEADY ARM EYE; TUBE DIAMETER 2 BOLT TYPE ","EA","CEE-TZ9-0027",null,1]
[8,54009844,"ADAPTOR, INSULATOR; TYPE: STEADY ARM EYE CLAMP, DIMENSIONS: OD 50.8/57 MM, APPLICATION: OVERHEAD TRACK EQUIPMENT;  DRAWING NO: CEE-TZ9-0035; HOLDER TUBE DIAMETER ","EA","CEE-TZ9-0035",null,1]
[9,54006330,"CLIP; TYPE: ROPE, DIMENSIONS: DIA 3 MM, MATERIAL: WIRE; DRAWING NO: H500110-3-133-E-DE-0109C; TROLLEY WIRE; SALDANHA ","EA","H500110-3-133-E-DE-0109C",null,1]
[10,54000208,"BOLT ASSEMBLY; NOMINAL DIAMETER: M16, LENGTH: 100 MM, THREAD SERIES: UNC, HEAD: HEXAGON, BOLT GRADE: 8.8, BOLT MATERIAL: STEEL, NUT QUANTITY: 1, THREAD LENGTH: 40 MM; ITEM TO BE SUPPLIED WITH A M16 NUT, M16 SPRING WASHER AND M16 FLAT WASHER. ITEM USED ON THE SISHEN-SALDANHA LINE. H500110-3-133-E-DE-0072","EA","H500110-3-133-E-DE-0072",null,1]
[11,54006329,"ASSEMBLY; TYPE: U-BOLT, APPLICATION: ORE LINE RAIL, DIMENSIONS: DIA 16 MM, MATERIAL: STEEL; DRAWING NO:  H500110-3-133-E-DE-0106; TROLLEY WIRE; SALDANHA ","EA","H500110-3-133-E-DE-0106\n",null,1]
[12,54000209,"KIT, MOUNTING, BODY, VEHICULAR; TYPE: BOLT AND NUT, APPLICATION: TROLLEY WIRE; DRAWING NO: H5001103133EDE0072, LA; WASHERS; M16; 65MM; OVERHEAD TRACK; VICTORY ELECTRICAL CAPE TOWN; SISHEN SALDANHA RAILWAY LINE (TFR) OHTE CATENARY SYSTEM","EA","H5001103133EDE0072",null,1]
[13,54006264,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 6 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214,  TROLLEY WIRE; SALDANHA ","EA","SSE-208214",null,1]
[14,54006263,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 13 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214, TROLLEY WIRE; SALDANHA ","EA","SSE-208214",null,1]
[15,54005264,"THIMBLE, ROPE; TYPE: RETAINER, DIMENSIONS: LG 96 MM, MATERIAL: STEEL, ROPE DIAMETER: 100 MM2; DRAWING NO: CEE-TNB-0085, SPECIFICATION: SANS 2262 ","EA","CEE-TNB-0085",null,1]
[16,54007162,"THIMBLE, ROPE; DRAWING NO: CEE-TZ7-0126 SHEET 36, EQUIPMENT USED ON OHTE; WITH CLEVIS; 25KV.","EA","CEE-TZ7-0126 SHEET 36",null,1]
[17,54016291,"THIMBLE, ROPE; EQUIPMENT USED ON OHTE; SPECIFICATION NUMBER SANS 2262 DATE 1984.; ORDINARY; GALVANISED; TO SPEC SANS 121 DATE 2000; NOMINAL SIZE 17 MM DIA. WIRE.; SABS 811 FIG 1 TABLE 1 ","EA","Technical Datasheet\nSABS 811",null,1]
[18,54015111,"THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 10 X LG 47 MM, MATERIAL: STEEL GALVANIZED, ROPE DIAMETER: 8 MM; DRAWING NO: CEE-TZ1-0126 SHEET 6; SPECIFICATION: SANS 2262 DATE 1984","EA","CEE-TZ1-0126 SHEET 6",null,1]
[19,"54004157","THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 8 X LG 32 MM, MATERIAL: STEEL, FINISH: GALVANIZED, ROPE DIAMETER: 6 MM;  DRAWING NO: CEE-TNB-0008; SPECIFICATION: CEE.0054BS 4042, 0; EQUIPMENT USED ON OHTE; 6 MM; ALUMINIUM BRONZE DIE CAST; FOR SECTION INSULATOR","EA"," CEE-TNB-0008\nCEE.0054",null,1]
[20,54006261,"THIMBLE; TYPE: OPEN, DIMENSIONS: DIA 8 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: SSE-208214; TROLLEY WIRE; SALDANHA ","EA","SSE-208214",null,1]
[21,54002498,"THIMBLE, ROPE; TYPE: WIRE COUPLER RELEASE, DIMENSIONS: WD 27 X LG 150 MM, MATERIAL: STEEL, ROPE DIAMETER: 22 MM, SPECIAL FEATURES: GALVANIZED;  DRAWING NO: CEE-TNB-0039; SPECIFICATION: SANS 121 DATE 2000SANS 2262 DATE 1984","EA","CEE-TNB-0039",null,1]
[22,54011202,"BRACKET; TYPE: CLIMBING ANGLE, APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 1.75 M; DRAWING NO: CEE-TMF-0191; FOR RAIL MAST","EA","CEE-TMF-0191",null,1]
[23,54008814,"BRACKET; TYPE: SUPPORT, APPLICATION: STAY WIRE ASSEMBLY, MATERIAL: STEEL; DRAWING NO:  CEE-TMHA-0027 ","EA","CEE-TMHA-0027 ",null,1]
[24,54010383,"BRACKET; TYPE: CLIMBING ANGLE , APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 600 MM; DRAWING NO:  CEE-TMF-0152 ","EA","CEE-TMF-0152 ",null,1]
[25,54011162,"BRACKET; TYPE: CLIMBING ANGLE , APPLICATION: STEADY ARM/HOCKEY STICKS, MATERIAL: STEEL, DIMENSIONS: LG 965 MM; DRAWING NO: CEE-TMF-0191; FOR RAIL MAST ","EA"," CEE-TMF-0191",null,1]
[26,54006272,"BRACKET; TYPE: CLEVIS, MATERIAL: SPHEROIDAL GRAPHITE IRON; SWINGING , H500110-3-133-E-DE-0067.","EA","H500110-3-133-E-DE-0067,",null,1]
[27,54011404,"BRACKET; TYPE: VERTICAL ATTACHMENT, MATERIAL: STEEL; DRAWING NO: CEE-TMF-0344; ELECTRICAL EQUIPMENT; EQUIPMENT USED ON OHTE; VERTICAL *A FOR 4725 CONTACT WIRE HEIGHT AUTO TENSION CONSTRUCTION USERS INTEREST 3, 25 AND 50 KV; FOR 25 KV AUTO-TENSION","EA"," CEE-TMF-0344",null,1]
[28,54006343,"ASSEMBLY; TYPE: BRACKET SWIVEL BOLT ON, APPLICATION: ORE LINE RAIL; DRAWING NO:  H500110-3-133-E-DE-0039","EA","H500110-3-133-E-DE-0039",null,1]
[29,54002171,"PLATE, METALLIC; TYPE: ADAPTOR, THICKNESS: 6 MM, WIDTH: 50 MM, LENGTH: 120 MM, PLATE MATERIAL: STEEL; DRAWING NO: CEE-TNE-0033, LA; EQUIPMENT USED ON 5405201; EXTENSION AND LINK STRAP GALVANISED FLAT IRON.","EA","CEE-TNE-0033",null,1]
[30,54032908,"ASSEMBLY; TYPE: OVERHEAD TRACK EQUIPMENT SUPPORT, APPLICATION: DOME ROOF TUNNEL, DIMENSIONS: LG 65 MM; DRAWING NO: BBB 1673; EQUIPMENT USED ON LINK FOR SUPPORT FITTING AND BRIDGES; 3 KV DC AND 25 KV AC; TO BE SUPPLIED COMPLETE WITH 6 X STEEL FLAT WASHERS GALVANIZED; NORMAL M12. 3 X HEX STEEL BOLTS GALVANIZED WITH NYLOCK NUTS M12","EA"," BBB 1673",null,1]
[31,54002195,"PLATE, METALLIC; TYPE: ADAPTOR, THICKNESS: 10 MM, WIDTH: 80 MM, LENGTH: 540 MM, MATERIAL GRADE: 304; DRAWING NO: CEE-TNE-0022; EXTENSION AND LINK STRAP GALVANISED MALLEABLE CAST IRON ","EA"," CEE-TNE-0022;",null,1]
["CATEGORY F"]
[1,54002805,"ATTACHMENT; TYPE: DROPPER SET, APPLICATION: OVERHEAD TRACK EQUIPMENT; DRAWING NO: CEE-TND-0005, LA; CEE-TND-0022, LA; CEE-TND-0009, LA; COMPLETE SET OF 4 MM. DIAMETER. HARD DRAWN COPPER/STAINLESS DROPPERS FOR A 67 METRE SPAN . TO SUIT ITEM 12 160 MM. SQ. CLIP-ON TYPE CATENARY CLIP. REFER TO (54/16836) AND 161 MM. SQ CONTACT CLIP REFER TO TO BE SUPPLIED WITHOUT CATENARY AND CONTACT CLIP.","SET","CEE-TND-0005, \nCEE-TND-0022, \nCEE-TND-0009",null,1]
["CATEGORY G"]
[1,54032528,"INSULATOR, STANDOFF; TYPE: SQUARE TONGUE/SPADE, INSULATOR MATERIAL: SILICON RUBBER, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBB0429, 4; BBB0430, 3; EQUIPMENT USED ON OHTE","EA","BBB0429, 4; BBB0430",null,1]
[2,54016897,"INSULATOR, STRAIN; TYPE: VANDAL PROOF, POTENTIAL RATING: 3 KVDC; DRAWING NO: CEE-TNC-0004, LA; TONGUE AND CLEVIS TYPE; MUST COMPLY TO QUOTED DRAWING","EA","CEE-TNC-0004",null,1]
[3,54024239,"INSULATOR, SUSPENSION; TYPE: VANDAL PROOF, INSULATOR MATERIAL: SILICON RUBBER, INSULATOR ATTACHMENT METHOD: ROUND TONGUE/HOOK TONGUE END CAPS, SPECIAL FEATURES: CREEPAGE PATH, 1476 MM; DRAWING NO: BBB3019, LA; BBB 3020, LA; EQUIPMENT USED ON OHTE;25 KV AC","EA","BBB3019, BBB 3020",null,1]
[4,54032553,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0430, LA; BBB 0429, LA; END CAP CONFIGURATION, CLEVIS/PIPE FITTING","EA","BBB 0430, BBB 0429",null,1]
[5,54000205,"INSULATOR; TYPE: LONG ROD, VANDAL PROOF, POTENTIAL: 50 KV, MATERIAL: COMPOSITE; DRAWING NO: BBC 1777, LA; ITEM USED ON SISHEN SALDANHA FEEDER LINE TROLLEY WIRE.","EA","BBC 1777",null,1]
[6,54006182,"INSULATOR; TYPE: COMPOSITE COMPRESSION, POTENTIAL: 50 KVAC, MATERIAL: VANDAL PROOF; DRAWING NO: BBF 9766, LA; ITEM USED ON 50KV AC ELECTRIFICATION.","EA","BBF 9766",null,1]
[7,54033393,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 3019, LA; BBB 3020, LA; END CAP CONFIGURATION, ROUND TONGUE: INSULATOR ATTACHMENT METHOD: ROUND TONGUE END CAP","EA"," BBB 3019, BBB 3020",null,1]
[8,54033408,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 3019, LA; BBB 3020, LA; END CAP CONFIGURATION: INSULATOR ATTACHMENT METHOD: HOOK/PIPE FITTING END CAPS SPECIAL FEATURES: CREEPAGE PATH, 1476 MM","EA","BBB 3019, BBB 3020",null,1]
[9,54032541,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB0429, LA; BBB0430, LA; END CAP CONFIGURATION, CLEVIS PIPE FITTING.","EA","BBB0429, BBB0430",null,1]
[10,54032516,"INSULATOR; TYPE: COMPRESSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB0430, LA; BBB0429, LA; VANDAL PROOF, END CAP CONFIGURATION: ROUND TONGUE/PIPE FITTING","EA","BBB0430, BBB0429",null,1]
[11,54024883,"INSULATOR; TYPE: POST, POTENTIAL: 11 KV, MATERIAL: SILICON RUBBER; DRAWING NO: BBC 8439, LA; SPECIFICATION: SANS 121, LA; VANDAL PROOF POST TRANSMISSION LINE INSULATOR, EQUIPMENT USED ON;  MAST STRUCTURE; F-NECK TYPE; TO INCLUDE M20 X 155 MM LONG FULL THREAD SPINDLE; NUT AND FLAT WASHER","EA","BBC 8439",null,1]
[12,54033975,"INSULATOR, STANDOFF; TYPE: VANDAL PROOF, INSULATOR MATERIAL: SILICON, POTENTIAL RATING: 50 KVAC, INSULATOR ATTACHMENT METHOD: SQUARE TONGUE AND TUBE END FITTING;  P/N: 144 034-015,  USED ON SISHEN-SALDANHA , H500110-3-133-E-DE-0140, BBC 1684","EA","H500110-3-133-E-DE-0140, BBC 1684",null,1]
[13,54032488,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KV, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0281, LA; SPECIFICATION: IEC 1109, 0; CREEPAGE PATH 1476; VANDAL PROOF; (COMPOSITE) SQUARE TONGUE AND ROUND CLEVIS END CAPS","EA","BBB 0281",null,1]
[14,54032476,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO:  BBB0281 , LA; SPECIFICATION: IEC 1109, LA; END CAP CONFIGURATION, ROUND CLEVIS/ROUND TONGUE COMPOSITE","EA","  BBB0281",null,1]
[15,54032011,"ASSEMBLY; TYPE: INSULATED KNUCKLE, APPLICATION: CATENARY AND CONTACT WIRE; DRAWING NO: CEE-TND-0040; CONSISTING OF ITEMS 1 AND 3 OF QUOTED DRAWING. EQUIPMENT USED ON OHTE ","EA","CEE-TND-0040",null,1]
[16,54032605,"INSULATOR; TYPE: TENSION, POTENTIAL: 25 KVAC, MATERIAL: SILICON RUBBER; DRAWING NO: BBB 0281, LA; SPECIFICATION: IEC 1109, LA; END CAP CONFIGURATION, SQUARE TONGUE.","EA","BBB 0281",null,1]
[17,54000612,"INSULATOR; TYPE: UNIVERSAL VANDAL PROOF, POTENTIAL: 25 KVAC, DIMENSIONS: AS PER DRAWING; DRAWING NO: BBG 2208","EA","BBG 2208",null,1]
[18,54032868,"ASSEMBLY; TYPE: PIVOT ARM, APPLICATION: DOME ROOF TUNNEL; DRAWING NO: BBB1685 ","EA"," BBB1685 ",null,1]
["CATEGORY H"]
[1,54002033,"ASSEMBLY; TYPE: CLAMP, APPLICATION: EARTH WIRE; DRAWING NO: CEE-TN-0371, LA; USED ON O.H.T.E","EA","CEE-TN-0371",null,1]
[2,54002753,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 100/80MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE.","EA","BBH 2141\nCEE-0063",null,1]
[3,54002777,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE","EA","BBH 2141\nCEE-0063",null,1]
[4,54000880,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250 TO 160 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA","EA","BBH 2141\nCEE-0063",null,1]
[5,54000907,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250 TO 250 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE","EA","BBH 2141\nCEE-0063",null,1]
[6,54000867,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 250-100 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE","EA","BBH 2141\nCEE-0063",null,1]
[7,54000791,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 80 TO 100 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA; EQUIPMENT USED ON OHTE","EA","BBH 2141\nCEE-0063",null,1]
[8,54000766,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: OVERHEAD TRACK EQUIPMENT, DIMENSIONS: 100/80 MM TO 50 MM2, MATERIAL: COPPER AND NICKEL AND SILICON; DRAWING NO: BBH 2141, LA; SPECIFICATION: CEE-0063, LA","EA","BBH 2141\nCEE-0063",null,1]
[9,54001949,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: 100/80 TO 161 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; EQUIPMENT USED ON OHTE","EA","BBH 2142",null,1]
[10,54014850,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: 80, 100 TO 107 MM2, MATERIAL: COPPER AND NICKEL AND SILICON; DRAWING NO: BBH 2142, LA; SPECIFICATION: CEE-0063, LA, ITEM: SHEET 1; EQUIPMENT USED ON OHTE","EA","BBH 2142\nCEE-0063",null,1]
[11,54014862,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: ID 160 TO 107 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; EQUIPMENT USED ON OHTE","EA","BBH 2142\nCEE-0063",null,1]
[12,54004930,"ASSEMBLY; TYPE: FEEDER CLAMP, APPLICATION: ID 160 TO 161 MM2, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 2142, LA; SPECIFICATION: CEE 0063, LA; EQUIPMENT USED ON OHTE","EA","BBH 2142\nCEE-0063",null,1]
[13,54006827,"SPLICE, CONDUCTOR; DIMENSIONS: DIA 107 MM2, TYPE: CONTACT WIRE, MATERIAL: COPPER/NICKEL/SILICON; DRAWING NO: BBH 2137, LA","EA","BBH 2137",null,1]
[14,54000754,"SPLICE, CONDUCTOR; DIMENSIONS: 161 MM2, TYPE: CONTACT WIRE, MATERIAL: COPPER/NICKEL/SILICON; DRAWING NO: BBH 2139  , LA; TO BE SUPPLIED 25 EACH PER CARTOON","EA","BBH 2139 ",null,1]
[15,54032504,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA; EQUIPMENT USED ON OHTE","EA","BBG 7987",null,1]
[16,54000560,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 500 TO 160, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA, ITEM: SHEET 2; FEEDER 50 KV; USED ON OHTE FCC CONNECTION 500 MM2 TO 160 MM2 TIGER WIRE","EA","BBG 7987",null,1]
[17,54000603,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 800 TO 160, MATERIAL: ALUMINIUM; DRAWING NO: BBG 7987, LA, ITEM: SHEET 3; FEEDER 50 KV; USED ON OHTE FCC 800 MM2 TO 160 MM2 TIGER WIRE","EA","BBG 7987",null,1]
[18,54006787,"ASSEMBLY; TYPE: DROPPER CLIP, APPLICATION: CONTACT WIRE, DIMENSIONS: SQ 107 MM; DRAWING NO; CEE-TND-0022, LA; SPECIFICATION: CEE-0063, LA","EA","CEE-TND-0022,\nCEE-0063",null,1]
[19,54017312,"ASSEMBLY; TYPE: DROPPER CLIP, APPLICATION: CONTACT WIRE, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: CEE-TND-0022, LA; SPECIFICATION: CEE.0063, LA; ITEM USED ON CONTACT WIRE SIZE 161MM2.","EA","CEE-TND-0022,\nCEE-0063",null,1]
[20,54020848,"KIT; TYPE: MAST CONNECTOR WEDGE, APPLICATION: BONDING; DRAWING NO: BBC 7863, LA; SPECIFICATION: BBB 6017, LA; ITEM USED FOR BONDING ON UNIVERSAL COLUMN AND I-BEAM MAST","EA","BBC 7863, \nBBB 6017",null,1]
[21,54020824,"KIT; TYPE: RAIL BOND CONNECTOR WEDGE, APPLICATION: BONDING; DRAWING NO: BBC 7864, LA; SPECIFICATION: BBB 6017, LA; EQUIPMENT USED ON OHTE RAIL BONDING","EA","BBC 7864, \nBBB 6017",null,1]
[22,54011275,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; TYPE: SUSPENSION, CLAMP TYPE: SHACKLE STRAP; DRAWING NO: BBH 2963, LA; SPECIFICATION: SANS 121, LA; EQUIPMENT USED ON OHTE FOR EARTH WIRE; 150 TO 250 MM2; LINER TO BE 2 MM THICK","EA","BBH 2963",null,1]
[23,54011643,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 3656 SHEET 1, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 161MM2 CONTACT WIRE FOR LARGE SWIVEL HEADS.","EA","BBH 3656 SHEET 1\nCEE-0063",null,1]
[24,54028819,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLAMP; DRAWING NO: BBH 3656 SHEET 4, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 107MM2 CONTACT WIRE FOR SMALL SWIVEL HEADS.","EA","BBH 3656 SHEET 4\nCEE-0063",null,1]
[25,54011591,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON; DRAWING NO: BBH 3656 SHEET 3, LA; SPECIFICATION: CEE-0063, LA; ITEM USED ON 107MM2 CONTACT WIRE FOR LARGE SWIVEL HEAD.","EA","BBH 3656 SHEET 3\nCEE-0063",null,1]
[26,54000690,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLIP, MATERIAL: COPPER NICKEL SILICON, ATTACHMENT METHOD: WIRE 161 MM2; DRAWING NO: BBH 3656 SHEET 2, LA; CEE-TND-0001 SHEET 1, LA; CEE-TND-0035, LA; SPECIFICATION: CEE-0063, LA; CONTACT WIRE FOR SMALL SWIVEL HEAD FOR GENERAL USE COMPLETE WITH STEADY ARM FITTING.","EA"," BBH 3656 SHEET 2\nCEE-0063",null,1]
[27,54033583,"CLAMP ASSEMBLY, RETAINING; TYPE: SWIVEL CLAMP; DRAWING NO: BBH 3656 SHEET 2, LA; SPECIFICATION: CEE-0063, LA; FULL ASSEMBLY SWIVEL CHEEKS FOR 161 MM2 CONTACT WIRE FOR SMALL SWIVEL HEAD.","EA","BBH 3656 SHEET 2\nCEE-0063",null,1]
["CATEGORY I"]
[1,54016836,"CLIP; TYPE: DROPPER SADDLE, MATERIAL: NYLON, APPLICATION: SINGLE CATENARY; DRAWING NO: CEE-TND-0005, LA; INSULATOR,ELECTRICAL CONDUCTOR EQUIPMENT USED ON OHTE. SINGLE CATENARY NYLON DROPPER SADDLE. FOR CATENARY WIRE 160 MM SQ","EA","CEE-TND-0005",null,1]
[2,54006840,"HANGER, WIRE STRAND; TYPE: CLIP ON, MATERIAL: NYLON; DRAWING NO: CEE-TND-0005; INSULATOR ELECTRICAL CONDUCTOR EQUIPMENT USED ON OHTE; SINGLE CATENARY NYLON DROPPER SADDLE; FOR CATENARY WIRE 80 MM SQ","EA"," CEE-TND-0005",null,1]
[3,54017070,"SADDLE; TYPE: CATENARY LOOP DROPPER, MATERIAL: NYLON; DRAWING NO: CEE-TND-0011, LA; SLEEVE,PROTECTIVE; EQUIPMENT USED ON OHTE; CLIP-ON-TYPE. ONLY SUITABLE FOR USE WITH 4 MM SOLID WIRE","EA"," CEE-TND-0011",null,1]
["CATEGORY J"]
[1,54004020,"PIN, STRAIGHT, HEADED; DIAMETER: 16 MM, LENGTH: 60 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0066CEE-TX-0054; SPECIFICATION: SANS 121 DATE 2000; COMPLETE WITH BRASS SPLIT PIN ACCORDING TO DRAWING","EA"," CEE-TX-0066\nCEE-TX-0054",null,1]
[2,54006193,"CLAMP ASSEMBLY, RETAINING; TYPE: BALL SWIVEL; DRAWING NO: BBH 1181 , LA; ATTACHMENT TO REGISTER ARM CONSISTING OF BODY, M12 DIA \"U\" BOLT, COMPLETE WITH NUTS & SPRING WASHERS. ATTACHMENT FOR 42.4MM AND 48.3MM PIPE. EQUIPMENT USED ON 25KV OHTE.","EA"," BBH 1181",null,1]
[3,54006270,"CLAMP ASSEMBLY, RETAINING; TYPE: STRAIN, ATTACHMENT METHOD: CLEVIS;  DRAWING NO: BBH 1179, LA;  ITEM USED ON 25 KV AC OHTE FOR A PIPE OF DIAMETER 42.4 MM2 AND 48.3 MM2","EA","BBH 1179",null,1]
[4,54004019,"PIN, CLEVIS; DIAMETER: 24 MM, LENGTH: 60 MM, MATERIAL: MILD STEEL; DRAWING NO: CEE-TX-0080; COMPLETE WITH SPLIT PIN ","EA","CEE-TX-0080",null,1]
[5,54027321,"PIN, CLEVIS; DIAMETER: 16 MM, LENGTH: 80 MM, MATERIAL: STEEL; DRAWING NO: SSE-208269; CF 222, 50KV AC ","EA"," SSE-208269",null,1]
[6,54015855,"PIN, CLEVIS; DIAMETER: 20 MM2, LENGTH: 315 MM, MATERIAL: STAINLESS STEEL, HEAD STYLE: FLAT;  DRAWING NO: BBH 1164, LA;  EQUIPMENT USED BETWEEN ERMELO AND VRYHEID ELECTRICFICATION","EA"," BBH 1164",null,1]
[7,54017753,"PIN, STRAIGHT, HEADED; DIAMETER: M16, LENGTH: 55 MM, MATERIAL: STAINLESS STEEL; SPECIFICATION: SANS 1700 PART 17, LA; PIN FINISH MUST BE SNAPHEAD AND MUST BE SUPPLIED WITH A LOCKING SPLIT PIN. ITEM USED ON THE SISHEN-SALDANHA LINE. H500110-3-133-E-DE-0074, SSE-208269","EA","H500110-3-133-E-DE-0074\nSSE-208269",null,1]
[8,54020885,"PIN, CLEVIS; DIAMETER: 12 MM, LENGTH: 33 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0073; FINISH, HOT DIP GALVANISE TO SANS 121. EQUIPMENT USED ON OHTE STORES DESCRIPTION CLEVIS PIN M12 FOR TROLLEY WIRE DESIGN 25 AND 50 KV COMPLETE WITH BRASS SPLIT PIN ","EA","CEE-TX-0073",null,1]
[9,54011793,"PIN, CLEVIS; DIAMETER: 16 MM, LENGTH: 152 MM, MATERIAL: STEEL; DRAWING NO: CEE-TX-0054; EQUIPMENT USED ON: OHTE; ROUND HEAD, STEEL,ZINC COATED M16 X 160 MM LONG CENTRE LINE OF 7 MM DIA SPLIT PIN HOLE 152 MM DIA FROM HEAD SUPPLIED WITH SPLIT PIN; CLEVIS (54003734) ","EA"," CEE-TX-0054",null,1]
[10,54004007,"PIN, CLEVIS; DIAMETER: 24 MM2, LENGTH: 76 MM, MATERIAL: MILD STEEL; DRAWING NO: CEE-TX-0059, LA, ITEM: 1 & 2; CEE-TX-0059; EQUIPMENT USED ON TENSION BRIDGE AND ANCHOR MAST;  COMPLETE WITH SPLIT PIN AS PER DRAWING.","EA","CEE-TX-0059, LA, ITEM: 1 & 2;\n CEE-TX-0059",null,1]
[11,54001582,"ATTACHMENT; TYPE: ADAPTOR, APPLICATION: STEADY ARM SOCKET; DRAWING NO: CEE-TNB-0076, LA","EA","CEE-TNB-0076",null,1]
[12,54002790,"SLEEVE; TYPE: TUBING, APPLICATION: DROPPER SECURING, INSIDE DIAMETER: 8 MM, OUTSIDE DIAMETER: 10 MM, LENGTH: 10 MM, MATERIAL: COPPER; DRAWING NO: CEE-TX-0079, LA","EA","CEE-TX-0079",null,1]
[13,54112457,"BUSHING, SLEEVE; TYPE: SPRING, INSIDE DIAMETER: 9 MM, OUTSIDE DIAMETER: 12.2 MM, OVERALL LENGTH: 10 MM, APPLICATION: DROPPER SECURING; DRAWING NO: CEE-TX-0079 SHEET 1, LA","EA","CEE-TX-0079",null,1]
[14,54004978,"ASSEMBLY; TYPE: WIRE ENDING CONE, APPLICATION: CONTACT WIRE; DRAWING NO: CEE-TNB-0036, LA; EQUIPMENT USED ON OHTE","EA","CEE-TNB-0036",null,1]
["CATEGORY K"]
[1,54016925,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 800 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 4","EA","BBD 5138,",null,1]
[2,54002152,"CLAMP; TYPE: FEEDER CLAMP, DIMENSIONS: AS PER DRAWING, MATERIAL: BI-METALLIC; DRAWING NO: BBH 0306, LA; CLAMP IS USED FOR JOINING 160 MM2 ALUMINIUM(TIGER) AND 107 MM2 COPPER CONTACT WIRE; BI-METAL  FEEDER CLAMP","EA","BBH 0306",null,1]
[3,54000401,"CLAMP; TYPE: FEEDER, DIMENSIONS: AS PER DRAWING, MATERIAL: BI-METALLIC; DRAWING NO: BBG 6147, 0; SPECIFICATION: CEE-0063, 0; PARALLEL; CU-NI-SI; COPPER CONTACT WIRE, TIGER TO 161 CONTACT","EA","BBG 6147",null,1]
[4,54032387,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA; BI-METAL, WITH A PERMANENT FORGED COPPER INSERT","EA","BBD 5138",null,1]
[5,54032375,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 100/80 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 5","EA","BBD 5138, LA, ITEM: SHEET 5",null,1]
[6,54016937,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 500 TO 160 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 3","EA","BBD 5138, LA, ITEM: SHEET 3",null,1]
[7,54032363,"ASSEMBLY; TYPE: PARALLEL CLAMP, APPLICATION: 160 TO 50 MM2, MATERIAL: BI-METALLIC; DRAWING NO: BBD 5138, LA, ITEM: SHEET 5","EA"," BBD 5138, LA, ITEM: SHEET 5",null,1]
["CATEGORY L"]
[1,54009274,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 28.8 MM, OUTSIDE DIAMETER: 31.8 MM, LENGTH: 6.1 M, MATERIAL: STEEL; SPECIFICATION: SANS 121 DATE 2000; MATERIAL TO BE GRADE 300 WA HOT DIPPED GALVANISED TO SPECIFICATION ","EA","Technical Datasheet",null,1]
[2,54001962,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 44 MM, OUTSIDE DIAMETER: 48 MM, LENGTH: 3.36 M, MATERIAL: STEEL; DRAWING NO: CEE-TMHH-0002; SPECIFICATION:  SANS 657 PART 1; STORES DESCRIPTION PUSH-PULL-OFF REGISTERING TUBE WITH A CLEVIS AT EACH END. ","EA","CEE-TMHH-0002",null,1]
[3,54029813,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 34.9 MM, OUTSIDE DIAMETER: 38.1 MM, LENGTH: 3.02 M, MATERIAL: STEEL; DRAWING NO: BT102; EQUIPMENT USED ON OHTE BRITS-THABAZIMBI STORES DESCRIPTION REGISTERING TUBE 38.1 X 38.1 X 3.2 MM WALL X 3.020 METRE LONG ","EA","Technical Datasheet",null,1]
[4,54030162,"TUBE; TYPE: REGISTERING , INSIDE DIAMETER: 22.5 MM, OUTSIDE DIAMETER: 26 MM, LENGTH: 1.65 M, MATERIAL: STEEL; EQUIPMENT USED ON OHTE BRITS-THABAZIMBI STORES DESCRIPTION REGISTERING TUBE 26 MM OD X 3.5 MM THICK ","EA","Technical Datasheet",null,1]
[5,54009302,"TUBE, STRUCTURAL; TYPE: STEADY ARM BRIDGE TYPE, DIMENSIONS: THK 2.03 MM, MATERIAL: STAINLESS STEEL GRADE 304;  DRAWING NO: CEE-TN -0152; OD = 25.4 MM. TOLERANCE+0-O.75 WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE STRESS = 486 N/MM SQ. MINIMUM. MATERIAL = AISI 304 WELDED","EA","CEE-TN -0152",null,1]
[6,54009314,"TUBE, STRUCTURAL; TYPE: CURVED STEADY ARM, DIMENSIONS: DIA 25.4 MM X LG 1.132 M, MATERIAL: STAINLESS STEEL GRADE 304; DRAWING NO: CEE-TND-0019; TOLERANCE+0-0.75. WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE STRESS = 486 N/MM SQ. MINIMUM. MATERIAL = AISI 304 WELDED","EA","CEE-TND-0019",null,1]
[7,54027624,"TUBE, STRUCTURAL; TYPE: REGISTRATION TUBE, DIMENSIONS: OD 42.8 MM X LG 3.06 M; DRAWING NO: BBH 1283, LA; ITEM USED FOR PUSH-PULL-OFF APPLICATION","EA","BBH 1283",null,1]
[8,54009338,"TUBE, STRUCTURAL; TYPE: TUNNEL STEADY ARM, DIMENSIONS: DIA 25.4 X LG 990 X THK 2.03 MM, MATERIAL: STAINLESS STEEL GRADE 304; DRAWING NO: CEE-TN -0153, 0; STRESS = 486 N/MM SQ MINIMUM. MATERIAL = AISI 304 WELDED. TUNNEL STEADY ARM. OD = 25.4 MM.TOLERANCE+0-0.75. WALL THICKNESS = 2 MM MINIMUM AFTER MANIPULATION. HARDNESS = 180-270 BRINELL. ELONGATION = 6 % MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 % OFFSET. ULTIMATE TENSILE","EA","CEE-TN -0153",null,1]
[9,54001735,"TUBE, STRUCTURAL; TYPE: CANTILEVER, DIMENSIONS: DIA 76 MM X LG 2.8 M X THK 5.5 MM; DRAWING NO: CEE-TMC-0042; USED FOR 2.75 M TRACK CENTRES FOR 203 X 203 UC MASTS ","EA","CEE-TMC-0042",null,1]
[10,54002450,"TUBE, STRUCTURAL; TYPE: REGISTERING ARM, DIMENSIONS: OD 48 X LG 900 X THK 4 MM, MATERIAL: STEEL; DRAWING NO: CEE-TN-0244; SPECIFICATION: SANS 657; EQUIPMENT USED ON 5400000 5405200 5405202 SPECIFICATION NUMBER SANS 657 GALVANISED WITH CLEVIS FITTING EACH END; GRADE 340 ERW ","EA"," CEE-TN-0244",null,1]
[11,54112455,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT, MATERIAL: STAINLESS STEEL; DRAWING NO: BBH 0441, LA, ITEM: 1; ITEM USED FOR TANGENT TRACK BETWEEN BRITS AND THABAZIMBI.","EA","BBH 0441",null,1]
[12,54920893,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 2; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI.","EA","BBH 0442",null,1]
[13,54112456,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 3; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI.","EA","BBH 0442, LA, ITEM: 3;",null,1]
[14,54112452,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: 25 KV OVERHEAD TRACK EQUIPMENT; DRAWING NO: BBH 0442, LA, ITEM: 1; FOR LIGHT AND HEAVY CURVES BETWEEN BRITS AND THABAZIMBI","EA","BBH 0442, LA, ITEM: 1",null,1]
[15,54001658,"PIPE ASSEMBLY; TYPE: REGISTERING , APPLICATION: PUSH PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 X THK 4 X LG 2730, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO:  1CEE-TMHH- 2/LATEST, 0; SPECIFICATION: SANS 657 PART 1; SPECIFICATION GRADE 340 ERW ","EA","CEE-TMHH-0002",null,1]
[16,54015451,"PIPE ASSEMBLY; TYPE: STEADY ARM, APPLICATION: OVERHEAD TRACK EQIPMENT, MATERIAL: STEEL, DIMENSIONS: ID 30 MM X LG 1.015 M X THK 2 MM, CONNECTION TYPE: HOOK AND SOCKET; DRAWING NO: CEE-TN-0386; SPECIFICATION: SANS 657 GRADE 250SANS 121 DATE 2000","EA","CEE-TN-0386",null,1]
[17,54000236,"PIPE ASSEMBLY; TYPE: REGISTERING , APPLICATION: DOUBLE BOOMS, MATERIAL: STEEL, DIMENSIONS: OD 48 X THK 4 X LG 2320 MM, CONNECTION TYPE: WITH CLEVIS; DRAWING NO: CEE-TMF-0444; SPECIFICATION: SANS 121DATE 2000SANS 657 PART 1; 25KV AUTO TENSION   BEAUFORT-WEST DE AAR ,SPECIFICATION HOT DIPPED GALVANISED ","EA","CEE-TMF-0444",null,1]
[18,54001723,"PIPE ASSEMBLY; TYPE: REGISTERING ARM, APPLICATION: PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 MM X LG 1.9 M X THK 4 MM, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO: CEE-TMHH-0002.","EA","CEE-TMHH-0002",null,1]
[19,54001747,"PIPE ASSEMBLY; TYPE: REGISTERING ARM, APPLICATION: PUSH PULL OFF CANTILEVER, MATERIAL: STEEL, DIMENSIONS: OD 48 MM X THK 4 MM X LG 3.030 M, CONNECTION TYPE: CLEVIS EACH END; DRAWING NO: CEE-TMHH-0002; SPECIFICATION: SANS 657 PART 1; SPECIFICATION GRADE 340 ERW ","EA"," CEE-TMHH-0002",null,1]
[20,54000111,"PIPE, METALLIC; TYPE: STEADY ARM, PIPE SIZE: OD 25 MM, LENGTH: 2.3 M, WALL THICKNESS: 2.5 MM, PIPE MATERIAL: STAINLESS STEEL, SPECIAL FEATURES: STRAIGHT ADJUSTABLE STEADY ARM; DRAWING NO: CEE-TZ7-0123 SHEET 49, LA; EQUIPMENT USED ON 25 KV OHTE; WITH EYE CLAMP (ITEM 2)","EA","CEE-TZ7-0123 SHEET 49",null,1]
[21,54007303,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 44 MM, OUTSIDE DIAMETER: 48 MM, LENGTH: 6 IN, MATERIAL: STEEL; DRAWING NO: CEE-TND-0034; STEEL TUBE FOR STRUCTURAL AND GENERAL ENGINEERING PURPOSES, GALVANISED TO SABS 763.25 KV OHTE ","EA","CEE-TND-0034",null,1]
[22,54028185,"TUBE; TYPE: REGISTERING , INSIDE DIAMETER: 46 MM, OUTSIDE DIAMETER: 50 MM, LENGTH: 3.1 M, MATERIAL: STEEL; DRAWING NO: SSE-208206 CF 506; 3.81KG/M. EQUIPMENT USED ON THE SISHEN SALDANHA OVERHEAD TRACK EQUIPMENT ","EA","SSE-208206",null,1]
[23,54009755,"TUBE; TYPE: REGISTERING ARM, INSIDE DIAMETER: 30.02 MM, OUTSIDE DIAMETER: 33.4 MM, LENGTH: 6 IN, MATERIAL: STAINLESS STEEL GRADE 304","EA","Technical Datasheet",null,1]
[24,54009237,"TUBE; TYPE: REGISTERING INLAND, INSIDE DIAMETER: 38.86 MM, OUTSIDE DIAMETER: 42.86 MM, LENGTH: 6.1 M, MATERIAL: STEEL; DRAWING NO: SANS 121 DATE 2000; MATERIAL TO BE GRADE 300 WA HOT DIPPED GALVANISED TO SPEC ","EA","Technical Datasheet",null,1]
[25,54001812,"TUBE ASSEMBLY, METALLIC; TYPE: CANTILEVER, LENGTH: 3.75 M, TUBE MATERIAL: STEEL; DRAWING NO: CEE-TMC-0042 ; FOR 203 X 203 UNIVERSAL COLUMNS MAST ","EA","CEE-TMC-0042",null,1]
[26,54001407,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 3 M, OUTSIDE DIAMETER: 50 MM, WALL THICKNESS: 4 MM, TUBE MATERIAL: STEEL;  DRAWING NO: CEE-TND-0038;  SPECIFICATION: SANS 121 DATE 2000;  PUSH-PULL OFF.EQUIPMENT USED ON OHTE","EA","CEE-TND-0038",null,1]
[27,54112441,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 3600 MM, OUTSIDE DIAMETER: 480 MM, WALL THICKNESS: 4 MM, TUBE MATERIAL: STEEL.","EA","technical Datasheet",null,1]
[28,54001432,"TUBE, METALLIC; SHAPE: ROUND, TUBE LENGTH: 2.8 M, OUTSIDE DIAMETER: 76 MM, TUBE MATERIAL: STEEL, SURFACE TREATMENT: GALVANIZED;   DRAWING NO: CEE-TMC-0041;  CANTILEVER, FOR 2,75 M TRACK CENTRES AND 203 X 152 AND 229 X 178 MM I MASTS","EA"," CEE-TMC-0041",null,1]
[29,54009351,"TUBE; TYPE: KNUCKLE, INSIDE DIAMETER: 23.4 MM, OUTSIDE DIAMETER: 25.4 MM, LENGTH: 330 MM, MATERIAL: STAINLESS STEEL; DRAWING NO: CE-TN -0155; TOLERANCE+0-0.75; MINIMUM AFTER MANIPULATION; HARDNESS: 180-270 BRINELL; ELONGATION: 6 PCT MINIMUM ON 25.4 MM GAUGE LENGTH AT 0.02 PCT OFFSET; ULTIMATE TENSILE STRESS: 486 N/MM SQ MINIMUM; MATERIAL: AISI 304 WELDED ","EA","CEE-TN -0155",null,1]
[30,54006259,"ARM; TYPE: STEADY, DIMENSIONS: LG 910 MM, MATERIAL: STAINLESS STEEL; DRAWING NO:  H500110-3-133-E-DE-0051","EA","H500110-3-133-E-DE-0051",null,1]
[31,54009743,"TUBE, STRUCTURAL; TYPE: CANTILEVER, DIMENSIONS: 60,33 MM OD X 3,91 MM WALL X 6 M LONG, MATERIAL: STAINLESS STEEL GRADE 304","EA","Technical Datasheet",null,1]
["CATEGORY M"]
[1,54011441,"INSULATOR;  P/N: 655154665, ARTHUR FLURY;  P/N: UNKNOWN, PFISTERER (PTY)LIMITED; SECTION SPECIFICATION NUMBER CEE.0056.86 25KV AC - 3KV DC CHANGE OVER YARDS. FOR 161 SQ MM CONTACT WIRE. TO QUOTED PARTNUMBER OR EQUAL. ","EA","CEE.0056.86",null,1]
[2,54005304,"INSULATOR; TYPE: NEUTRAL SECTION, POTENTIAL: 25 KV, DIMENSIONS: DIA 161 MM2;  P/N: 655.236.000, ARTHUR FLURY; MATERIAL NUMBER; 54005304;  EQUIPMENT USED ON OHTE, CONTACT WIRE 3 KVDC; COMPLETE WITH HANGING GEAR ","EA","Technical Datasheet",null,1]
[3,54010840,"INSULATOR; TYPE: SINGLE ROD SECTION, POTENTIAL: 25 KVAC; SPECIFICATION: CEE-0055, LA; FOR 107 SQ MM CONTACT WIRE","EA","CEE-0055",null,1]
[4,54010775,"INSULATOR; TYPE: SECTION INSULATOR, POTENTIAL: 3 KVDC; SPECIFICATION: CEE.0054, LA; ITEM USED ON 161 SQ MM CONTACT WIRE ON 3KV DC ELECTRIFICATION.","EA","CEE.0054",null,1]
[5,54005454,"INSULATOR; TYPE: NEUTRAL SECTION, POTENTIAL: 25 KV, DIMENSIONS: DIA 107 MM2;  P/N: 655.150.720, ARTHUR FLURY; MATERIAL NUMBER 54005454,EQUIPMENT USED ON OHTE, TO QUOTED PART NUMBERS OR EQUAL ","EA","P/N: 655.150.720",null,1]
[6,48007470,"MAGNET; TYPE: TRACK SIDE; DRAWING NO: CEE-TLE 7, LV; 25KV AC MAGNET TYPE S25000-Q 5697-C5 WITH AN EFFECTIVE FLUX OF 3090: 10 WEBBER AT A VERTICAL HEIGHT OF 150 MM AND AN OFF CENTRE OFF DISTANCE OF 50 MM AT AN AMBIENT TEMP: OF 60 DEG C. TO QUOTED PART NUMBER OR EQUAL FOR BOLTS 48000290 EQUIPMENT USED ON SUBS","EA","CEE-TLE-0007\n",null,1]
[7,48008968,"BLOCK; TYPE: MOUTING TRACK MAGNET RUBBER, WIDTH: 380 MM, LENGTH: 1.4 M, HEIGHT: 170 MM, MATERIAL: RUBBER; DRAWING NO: BBC 0694, LV; ITEM 48008968:TRACK MAGNET RUBBER DESIGNED FOR SLEEPER SPACING FROM 630MM TO 725MM 25 KV. LOCOMOTIVE SWITCHING AT NEUTRAL SECTIONS. COMPLETE AS PER DRAWING FOR \"U: BOLTS 54000515 FOR MAGNET 4807470 FOR MAGNET BOLTS 48000290; EQUIPMENT USED ON OHTE / SUBS; MOUNTING","EA"," BBC 0694",null,1]
["CATEGORY N"]
[1,54016003,"WEIGHT, COUNTERBALANCE; TYPE: ROUND, WEIGHT MATERIAL: CONCRETE, GROSS WEIGHT: 25 KG, SPECIAL FEATURES: WITHOUT EYE;  DRAWING NO: CEE-TZ9-0113 ITEM 15; CEE-TZ9-0107","EA","CEE-TZ9-0113 ITEM 15; \nCEE-TZ9-0107",null,1]
[2,54006738,"WEIGHT, COUNTERBALANCE; TYPE: SOLID, WEIGHT MATERIAL: IRON, GROSS WEIGHT: 20 KG; DRAWING NO: CEE-TMF-0491; LINE TENSIONING EQUIPMENT USED ON CID 5400000 5405202; IRON WEIGHT. 20 KG. CONTACT AND CATENARY WIRES. 25 KV OVERHEAD TRACK EQUIPMENT ","EA"," CEE-TMF-0491",null,1]
[3,54016229,"WEIGHT, COUNTERBALANCE; TYPE: ROUND, WEIGHT MATERIAL: CONCRETE, GROSS WEIGHT: 25 KG;  DRAWING NO: CEE-TZ9-0113; CEE-TZ9-0461; CEE-TZ9-0400;  STORES DESCRIPTION CONCRETE WEIGHT 25 KG WITH EYE PIECE.","EA","CEE-TZ9-0113; \nCEE-TZ9-0461;\n CEE-TZ9-0400",null,1]
[4,54006726,"WEIGHT, COUNTERBALANCE; TYPE: SOLID, WEIGHT MATERIAL: IRON, GROSS WEIGHT: 40 KG; DRAWING NO: CEE-TMF-0490; LINE TENSIONING; EQUIPMENT USED ON: CID 5400000 5405202; CAST IRON WEIGHT. 40 KG. CONTACT AND CATENARY WIRES. ","EA","CEE-TMF-0490",null,1]
[5,54009186,"TENSIONER; TYPE: COMPACT AUTOMATIC SPRING, DIMENSIONS: AS PER SPECIFICATION; SPECIFICATION: BBG 2165, LA; ITEM USED FOR TENSIONING OHTE CONDUCTORS.","EA"," BBG 2165",null,1]
[6,54000202,"COUNTERWEIGHT; TYPE: PULLEY WHEEL, DIMENSIONS: AS PER DRAWING, APPLICATION: TROLLEY WIRE; DRAWING NO: SSE TMF 05 , LA; OVERHEAD TRACK; COMPLETE; 50KV OHTE; VICTORY ELECTRICAL CAPE TOWN ; SALDANHA; HOT DIPPED GALVANIZED, H500110-3-133-E-DE-0102","EA","SSE TMF 05\nH500110-3-133-E-DE-0102",null,1]
[7,54006326,"COUNTERWEIGHT; TYPE: PULLEY WIRE, DIMENSIONS: LG 6.3 M X THK 10 MM, MATERIAL: STAINLESS STEEL; DRAWING NO:  H500110-3-133-E-DE-0110; TROLLEY WIRE; SALDANHA ","EA","H500110-3-133-E-DE-0110",null,1]
[8,54006637,"GUIDE; TYPE: EYE, APPLICATION: BALANCE WEIGHT, MATERIAL: STEEL; DRAWING NO: CEE-TZ1-0124 SHEET 6 ","EA","CEE-TZ1-0124 SHEET 6 ",null,1]
[9,54009326,"FAIRLEAD, SHEAVE; TYPE: BALANCE WEIGHT PULLEY, MATERIAL: STEEL; DRAWING NO: CEE-TZ1-0124 SHEET 8; SPECIFICATION: SANS 121 DATE 2000; ELECT RAIL PULLEY SINGLE BALANCE WEIGHT PULLEY WITHOUT BOND ATTACHMENT TO TENSION 25 KV. O.H.T.E.LINE GALVANISED TO SPECIFICATION ","EA"," CEE-TZ1-0124 SHEET 8",null,1]
[10,54010763,"TENSIONER PULLEY ASSEMBLY; TYPE: BALANCE WEIGHT, MATERIAL: STEEL; DRAWING NO: CEE-TMF-0523; SPECIFICATION: CEE-0131-85; STANDARD: SABS ISO 1461 ; CONTACT AND CATENARY 25 KV WIRE DEVICE: CONSISTING OF BASIC BALANCE WEIGHT PULLEY, WIRE ROPE AND CONNECTING DEVICES","EA","CEE-TMF-0523; \nCEE-0131-85;",null,1]
["CATEGORY O"]
[1,54011934,"SWITCH ASSEMBLY; TYPE: CHANGEOVER TRACK SWITCH; DRAWING NO: BBH 2140, LA; ITEM USED AS  25 KV AC - 3 KV DC SWITCH IN THE CHANGE OVER YARD.","EA"," BBH 2140",null,1]
[2,54033926,"SWITCH ASSEMBLY; TYPE: TRACK, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBB5971; BBC6441; BBC 8743; BBC6440;  EQUIPMENT USED ON OHTE STORES DESCRIPTION TRACK SECTIONING SWITCH 25 KV AC COMPLETE WITH LOCKING DEVICE BUT WITHOUT CLOSING MECHANISM","EA"," BBB5971; BBC6441;\nBBC 8743; BBC6440",null,1]
[3,54017765,"SWITCH ASSEMBLY; TYPE: SIDING, POTENTIAL RATING: 3 KVDC; DRAWING NO: BBB5971 ; BBC 8741; BBB5970; SPECIFICATION: CEE-0228.96;  STORES DESCRIPTION SIDING SWITCH 3 KV. DC. WITHOUT OPERATING HANDLE, COMPLETE WITH LOCKING DEVICE. INSULATORS MUST BE OF THE SILICON VANDAL PROOF TYPE APPROVED INSULATOR : SILICOSIL-POST INSULATOR TO PARTNUMBER DP167-0178-003 GMC POWERLINE OR EQUAL","EA"," BBB5971 ; BBC 8741; \nBBB5970",null,1]
[4,54001331,"SWITCH ASSEMBLY; TYPE: SIDING, SPECIAL FEATURES: NO LOCKING DEVICE; DRAWING NO: BBC 8741 ; SPECIFICATION: CEE.0228.96; SIDING 3 KV DC. WITHOUT OPERATING HANDLE.","EA","BBC 8741",null,1]
[5,54033938,"SWITCH ASSEMBLY; TYPE: SIDING, POTENTIAL RATING: 25 KVAC; DRAWING NO: BBC6441; BBC6440 ; BBB5971; CEE-TZ7-0121 SHEET 189; SPECIFICATION: CEE.0228.96; STORES DESCRIPTION SIDING SWITCH 25 KV AC COMPLETE WITH LOCKING DEVICE","EA","BBC6441; BBC6440 ; \nBBB5971; CEE-TZ7-0121 SHEET 189",null,1]
[6,54005733,"SWITCH, KNIFE;  SPECIFICATION CEE.0228.96; SIDING 25 KV AC. POLLUTED & NON POLLUTED AREAS. TO QUOTED PART NUMBER OR EQUAL ","EA","CEE.0228.96",null,1]
[7,54001242,"SWITCH, KNIFE; TYPE: TRACK, CURRENT RATING: 3 KA, POTENTIAL RATING: 3 KV;  SPECIFICATION: CEE 228.96, 0CEE.0117.85; EQUIPMENT USED ON 5400000, 5405900 AND 5405901; MOVING BLADE FOR AEG TYPE; STORES DESCRIPTION BLADE, ELECTRICAL SWITCH ","EA","CEE-0228.96",null,1]
[8,54017397,"SWITCH, KNIFE; TYPE: TRACK SWITCH, POTENTIAL RATING: 3 KVDC, NUMBER OF POLES: SINGLE, SPECIAL FEATURES: COMPLETE WITH LOCKING DEVICE; DRAWING NO: BBC 8741, LA, ITEM: 1 (with locking device)","EA","BBC 8741,",null,1]
[9,54014938,"SWITCH ASSEMBLY; TYPE: TRACK SWITCH, POTENTIAL RATING: 25 KVAC, SPECIAL FEATURES: SINGLE POLE; DRAWING NO: BBC 8743, LA","EA","BBC 8743",null,1]
[10,54005276,"SWITCH, KNIFE; TYPE: TRACK, POTENTIAL RATING: 3 KVDC, NUMBER OF POLES: SINGLE, SPECIAL FEATURES: WITHOUT LOCKING DEVICE; DRAWING NO: BBC 8741, LA, ITEM: 2 (no locking device)","EA","BBC 8741",null,1]
[11,54015892,"ASSEMBLY; TYPE: BLADE SET, APPLICATION: SWITCH, TRACK, 25 KVAC; DRAWING NO: BBD 7601, LA","EA","BBD 7601",null,1]
[12,54005745,"MECHANISM; TYPE: OPEN/CLOSE OPERATION, APPLICATION: TRACK SWITCH; DRAWING NO: CEE-TZ1-0121 SHEET 52; EQUIPMENT USED ON 5400000 5405902 TRACK 25 KV AC COMPLETE, WITHOUT OPERATING ROD.","EA","CEE-TZ1-0121 SHEET 52",null,1]
[13,54001392,"SWITCH, KNIFE; TYPE: TRISWITCH 4A, CURRENT RATING: 200 A, POTENTIAL RATING: 11 KVAC;  TRISWITCH TYPE 4 A, LINEGEAR 2000; EQUIPMENT USED ON OHTE; DISCONNECT 3 PHASE GANG OPERATED; SWITCHING BY MEANS OF A INSULATED PORTABLE LINK STICK; TO QUOTED PARTNUMBER OR EQUAL; 3 POLE","EA","Technical Datasheet",null,1]
["CATEGORY P"]
[1,"54001913","TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: BBH 2962; SPECIFICATION: BS 4429SANS 121 DATE 2000; EQUIPMENT USED ON: OHTE; DROP-FORGED; 110 MM TAKE-UP; M16 SCREWS.;EYE TO EYE.; COMPLETE WITH LOCKNUT; HOT DIPPED GALVANISED ","EA","BBH 2962",null,1]
[2,54001937,"TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: CU-NI-SI; DRAWING NO: BBH 2962; EQUIPMENT USED ON OHTE; TAKE-UP: 90 MM; FOR STAINLESS STEEL AND 75 MM; FOR CU-NI-SI.; QUOTED DRAWING FOR CU-NI-SI ONLY. ","EA","BBH 2962",null,1]
[3,54001925,"TURNBUCKLE; TYPE: ADJUSTABLE, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: BBH 2962; SPECIFICATION: SANS 121 DATE 2000; EQUIPMENT USED ON OHTE; DROP-FORGED; 400 MM - 460 MM TAKE-UP; M24 SCREWS.; HOT DIPPED GALVANISED. ","EA","BBH 2962",null,1]
[4,"54031523","TURNBUCKLE; TYPE: ADJUSTING, THREAD SERIES: UNIFIED NATIONAL COARSE, MATERIAL: STEEL; DRAWING NO: CEE-TNB-0079; SPECIFICATION: SANS 121 DATE 2000; DROP-FORGED; EYE AND EYE; 130 MM TAKE-UP; COMPLETE WITH ONE LOCKNUT; M20 SCREWS.; HOT DIPPED GALVANISED. ","EA","BBH 2962",null,1]
[5,54033659,"SPRING, HELICAL, EXTENSION; TYPE: TENSIONING, OUTSIDE DIAMETER: 120 MM, INSIDE DIAMETER: 80 MM, NUMBER OF TURNS: 17, SPRING MATERIAL: STEEL, MATERIAL SIZE: 20 MM; DRAWING NO: BBB 2902; EQUIPMENT USED ON OHTE; CONTACT AND CATENARY WIRE TENSIONING; FOR 25 KV AC LINES","EA","BBB 2902",null,1]
[6,54022544,"SPRING, HELICAL, EXTENSION; TYPE: TENSIONING, OUTSIDE DIAMETER: 285 MM, INSIDE DIAMETER: 225 MM, NUMBER OF TURNS: 9.5, SPRING MATERIAL: STEEL, MATERIAL SIZE: 30 MM;  DRAWING NO: CEE-TNB-33; CEE-TNB-30; EQUIPMENT USED ON OHTE; CONTACT WIRE TENSIONING FOR 3 KV.DC. LINES","EA","CEE-TNB-0033; \nCEE-TNB-0030",null,1]
[7,54007226,"BOLT, U; THREAD DIAMETER: M12, THREAD SERIES: UNC, MATERIAL: STEEL, INSIDE DISTANCE BETWEEN SHANKS: 32 MM, THREAD LENGTH: 30 MM; DRAWING NO: CEE-TX-0089; SPECIFICATION: SANS 121 DATE 2000; EQUIPMENT USED ON OHTE; COMPLETE WITH NUTS ","EA","CEE-TX-0089",null,1]
[8,54003014,"HOOK, SAFETY; TYPE: TOWER, MATERIAL: STEEL; DRAWING NO: CEE-TNB-0041, LA; EQUIPMENT USED ON OHTE","EA","CEE-TNB-0041",null,1]
[9,54001521,"FITTING; TYPE: CLEVIS TWISTED H, COMMERCIAL SIZE: AS PER DRAWING, MATERIAL: SPHEROIDAL GRAPHITE IRON; DRAWING NO: CEE-TNB-0060, LA; EQUIPMENT USED ON OHTE.","EA","CEE-TNB-0060",null,1]
["CATEGORY Q"]
[1,54001217,"ARRESTER, ELECTRICAL; TYPE: SURGE, POTENTIAL PROTECTION LEVEL: 12 KVAC; SPECIFICATION: BBH 2339, LA; EQUIPMENT USED ON TRANSMISSION LINE 11 KV; COMPLETE WITH MOUNTING BRACKET POLYMER HOUSED","EA","BBH 2339",null,1]
[2,54031940,"ARRESTER, ELECTRICAL; TYPE: SPARK GAP, POTENTIAL PROTECTION LEVEL: 450 V; DRAWING NO: BBB0906 LATEST; SPECIFICATION: BBB1616LATEST; MATERIAL NUMBER 54031940, COMPLETE ASSEMBLY WITH GAS FILLED ARRESTER. NOTE TO TENDERERS: MUST SUPPLY TEST CERTIFICATES FOR THE GAS ARRESTERS ON INSPECTION DATE","EA","BBB0906 \nBBB1616",null,1]
[3,54008798,"ARRESTER, ELECTRICAL; TYPE: SURGE OHTE, POTENTIAL PROTECTION LEVEL: 3 KVDC, CAPACITANCE: 4 UF; SPECIFICATION NUMBER: CEE.0115.86.","EA","CEE.0115.",null,1]
[4,"54001189","ARRESTER, ELECTRICAL; TYPE: SURGE, POTENTIAL PROTECTION LEVEL: 4.8 KVDC; SPECIFICATION: CEE-0240, LA; METAL OXIDE TYPE. PEDESTAL MOUNTED: WITH ADAPTER PLATE TO QUOTED DRAWING.","EA","CEE-0240",null,1]
[5,54112409,"ASSEMBLY; TYPE: LIGHTNING ARRESTER, APPLICATION: TUBULAR CANTILEVER; DRAWING NO: BBB 2141, LA; STORES DESCRIPTION, ARCING HORNS LIGHTNING ARRESTER FOR 3KV DC ELECTRIFCATION. THE DEPOTS MUST CONFIRM PRIOR IF THEY REQUIRE FOR A TUBULAR OR RAIL MAST CANTILVER. ITEM 7, 8 & 12 CAN BE EXCLUDED BY THE SUPPLIER.","EA","BBB 2141,",null,1]
["CATEGORY R"]
[1,54005215,"CLAMP; TYPE: SWIVEL CLAMP RETAINER, DIMENSIONS: AS PER DRAWING, MATERIAL: GRAPHITE IRON; DRAWING NO: LATEST, 0CEE-TND-025, ; COMPLETE WITH M12 U-BOLT, NUTS AND WASHERS SUITABLE FOR 107 AND 161 MM SQ CONTACT WIRE SWIVEL CLIPS ","EA","CEE-TND-025",null,1]
[2,54033129,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN;  DRAWING NO: BBH 1118; SPECIFICATION T-T10A-10 EQUIPMENT USED ON OHTE PISTOL GRIP TYPE 5  MM DIA. TO 20.5 MM DIA. USERS INTEREST FOR USE ON ALUMINIUM WIRE;3 U BOLTS ","EA","BBH 1118",null,1]
[3,54034095,"CLAMP; TYPE: DOUBLE SUSPENSION, DIMENSIONS: 800 MM2, MATERIAL: GALVANIZED STEEL; DRAWING NO: BBC 7533, 0; FEEDER AND DEER CATENARY","EA","BBC 7533",null,1]
[4,54004764,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; SPECIFICATION NUMBER T-T10A-19. CATENARY WIRE FOR 80 - 160 SQ MM, MIN DIA: 8 MM MAX DIA: 18 MM. STRANDED COPPER AND ALUMINIUM CONDUCTORS; 3 U BOLTS","EA","Technical Datasheet",null,1]
[5,54009933,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN;  DRAWING NO: CEE-TZ-9/43, 0; EQUIPMENT USED ON CID 5400000 540 5200 5405202 OHTE HOOK CONNECTION. 42 MM TUBE DIAMETER","EA"," CEE-TZ9-0043",null,1]
[6,54010496,"ASSEMBLY; TYPE: CLAMP, APPLICATION: EARTH WIRE; DRAWING NO: CEE-TN-0371, LA; CLAMP USED ON 160MM2 ALUMINIUM CONDUCTOR","EA","CEE-TN-0371",null,1]
[7,54004917,"CLAMP, CABLE, ELECTRICAL CONNECTOR; TYPE: DOUBLE SUSPENSION, CABLE SIZE: 80 TO 250 MM2; DRAWING NO: CEE-TNB-0074, LA; STORES DESCRIPTION: DOUBLE SUSPENSION CLAMP FROM BOTH 80 TO 250 MM2 AND 500 TO 800 MM2; FEEDER CONDUCTORS","EA","CEE-TNB-0074",null,1]
[8,54021980,"CLAMP, CABLE, ELECTRICAL CONNECTOR; TYPE: SINGLE SUSPENSION, CLAMP MATERIAL: SPHEROIDAL GRAPHITE IRON, CABLE SIZE: 500 TO 800 MM2; DRAWING NO: CEE-TNB-0091 SHEET 1-6, LA; ITEM USED FOR STRANDED ALUMINIUM FEEDER WIRE","EA","CEE-TNB-0091, Sht 1-6",null,1]
[9,54033522,"CLAMP, ELECTRICAL; CLAMP TYPE: PARALLEL, POTENTIAL RATING: 25 KV, CLAMP MATERIAL: ALUMINIUM GRADE 6063, FURNISHED ITEMS: INSERT COPPER; DRAWING NO: BBD 5138, ITEM NUMBER 54033522 ; USED ON OHTE WITH \"SKUNK\" CATENARY; 100 MM2 ACSR TO 160 MM2 COPPER; WITH A PERMANENT FORGED COPPER INSERT","EA","BBD 5138",null,1]
[10,54009893,"CLAMP, ELECTRICAL CONDUCTOR, STRAIN; DRAWING NO: CEE-TZ-9/39, 0; EQUIPMENT USED ON CID 5400000 540 5200 5405202 OHTE HOOK JOINT FOR 31 TO 34 MM DIAMETER TUBE","EA","CEE-TZ9-0039",null,1]
[11,54006299,"CLAMP; TYPE: GUIDE, COUNTERWEIGHT, DIMENSIONS: AS PER DRAWING, MATERIAL: STEEL , SSE-208301, H500110-3-133-E-DE-0099","EA","SSE-208301, \nH500110-3-133-E-DE-0099",null,1]
[12,54000199,"CLAMP, ELECTRICAL; CLAMP TYPE: CLIP SWIVEL, POTENTIAL RATING: 50 KV, OVERALL LENGTH: 107 MM; CONTACT WIRE; OVERHEAD TRACK; VICTORY ELECTRICAL CAPE TOWN BBH 3656; SALDANHA","EA","BBH 3656",null,1]