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Specification For General Build maintenance

· Replace the cracked glass panel in the entrance door.
· Replace bent and broken blinds in tearoom and offices.
· Replace missing/broken ceiling panels in the short passage.
· Replace loose and torn carpets tiles in various areas in the office building
· Paint rusted doors and burglar bars.
· Fix the leaking roof that causes unsightly stains on the ceiling panels.
· Replace broken ceilings on the outside to prevent pigeons from entering the roof.
· Install burglar bars and windows at the chemical store.
· Replace broken padlocks at car ports.
· Replace dilapidated ceiling at oven lab.
· Replace door lock at oven lab.
· Do upholstery of all chairs with thorn material covers.
· Door lock at Room 19
· Door lock between rooms 7 & 8

Compulsory Requirements:
➢ Supplier with at least 2 RECOMMENDATION LETTERS over R 100 000 each
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