{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":456,"n_cols":10,"rows_kept":456,"merged":[[1,0,1,6],[3,0,3,2],[4,0,8,0],[10,0,10,3],[11,0,13,0],[11,1,13,1],[15,0,15,2],[16,0,21,0],[16,1,18,1],[19,1,21,1],[23,0,23,2],[24,0,27,0],[29,0,29,2],[30,0,35,0],[30,2,35,2],[30,3,35,3],[30,4,35,4],[30,5,35,5],[38,0,38,2],[39,0,41,0],[39,2,41,2],[39,3,41,3],[39,4,41,4],[39,5,41,5],[44,0,46,0],[44,2,46,2],[44,3,46,3],[48,0,50,0],[49,2,50,2],[49,3,50,3],[56,0,56,2],[57,0,60,0],[57,2,59,2],[57,3,59,3],[57,4,59,4],[62,0,62,2],[63,0,64,0],[66,0,66,4],[67,0,77,0],[67,1,69,1],[68,2,69,2],[68,4,69,4],[68,5,69,5],[68,6,69,6],[70,1,73,1],[70,2,71,2],[70,4,71,4],[70,5,71,5],[70,6,71,6],[72,2,73,2],[72,4,73,4],[72,5,73,5],[72,6,73,6],[74,1,77,1],[74,2,75,2],[74,4,75,4],[74,5,75,5],[74,6,75,6],[76,2,77,2],[76,4,77,4],[76,5,77,5],[76,6,77,6],[78,0,78,6],[80,0,81,0],[80,1,81,1],[83,0,83,2],[84,0,86,0],[84,2,85,2],[84,3,85,3],[84,4,85,4],[88,0,88,2],[89,0,93,0],[89,2,90,2],[89,3,90,3],[89,4,90,4],[91,2,92,2],[91,3,92,3],[91,4,92,4],[93,3,93,4],[99,0,104,0],[99,1,104,1],[99,2,100,2],[99,4,100,4],[99,5,100,5],[101,2,102,2],[101,4,102,4],[101,5,102,5],[103,2,104,2],[103,4,104,4],[103,5,104,5],[106,0,106,3],[107,0,110,0],[107,1,108,1],[119,0,119,3],[120,0,124,0],[120,1,121,1],[122,1,123,1],[124,1,124,2],[126,0,126,3],[127,0,128,0],[127,1,128,1],[131,0,131,2],[132,0,135,0],[137,0,137,3],[138,0,140,0],[138,1,140,1],[142,0,142,2],[143,0,145,0],[147,0,147,2],[148,0,153,0],[155,0,155,3],[156,0,159,0],[168,0,168,3],[169,0,172,0],[171,3,172,3],[171,4,172,4],[171,5,172,5],[174,0,174,3],[175,0,183,0],[175,1,183,1],[175,3,176,3],[175,4,176,4],[175,5,176,5],[177,3,178,3],[177,4,178,4],[177,5,178,5],[185,0,185,2],[186,0,187,0],[192,0,192,3],[193,0,195,0],[193,2,194,2],[193,3,194,3],[193,4,194,4],[193,5,194,5],[197,0,197,3],[198,0,202,0],[198,1,202,1],[204,0,204,3],[205,0,209,0],[205,1,209,1],[211,0,211,3],[212,0,215,0],[212,1,215,1],[214,3,215,3],[214,4,215,4],[214,5,215,5],[217,0,217,3],[218,0,219,0],[218,1,219,1],[221,0,221,3],[222,0,230,0],[232,0,232,3],[233,0,239,0],[243,0,243,3],[243,4,243,5],[243,6,243,7],[245,0,251,0],[253,0,253,3],[254,0,266,0],[254,1,266,1],[268,0,268,3],[269,0,278,0],[269,1,278,1],[280,0,280,3],[281,0,287,0],[282,2,282,9],[294,0,294,3],[295,0,301,0],[296,2,296,9],[304,0,304,3],[305,0,310,0],[312,0,312,3],[313,0,318,0],[320,0,321,3],[320,4,320,5],[320,6,320,7],[322,0,330,0],[332,0,333,3],[332,4,332,6],[332,7,332,8],[333,6,333,7],[334,0,342,0],[334,6,334,7],[335,6,335,7],[336,6,336,7],[337,6,337,7],[338,6,338,7],[339,6,339,7],[340,6,340,7],[341,6,341,7],[342,6,342,7],[349,0,349,3],[350,0,353,0],[350,1,353,1],[355,0,355,3],[356,0,359,0],[356,1,359,1],[361,0,361,2],[362,0,367,0],[369,0,372,0],[376,0,387,0],[376,1,376,2],[376,3,377,3],[376,4,377,4],[377,1,377,2],[378,2,379,2],[378,3,379,3],[378,4,379,4],[380,2,381,2],[380,3,381,3],[380,4,381,4],[382,2,383,2],[382,3,383,3],[382,4,383,4],[384,2,385,2],[384,3,385,3],[384,4,385,4],[389,0,398,0],[389,1,389,3],[389,4,390,4],[389,5,390,6],[390,1,390,3],[391,5,391,6],[392,5,392,6],[393,5,393,6],[394,5,394,6],[395,4,395,5],[396,4,396,5],[397,4,397,5],[398,4,398,5],[401,0,406,0],[401,1,401,2],[401,3,402,3],[401,4,402,4],[402,1,402,2],[403,2,404,2],[403,3,404,3],[403,4,404,4],[405,2,406,2],[405,3,406,3],[405,4,406,4],[408,0,413,0],[408,1,408,2],[408,3,409,3],[408,4,409,4],[408,5,409,5],[408,6,409,6],[408,7,409,7],[408,8,409,8],[409,1,409,2],[410,2,411,2],[410,3,411,3],[410,4,411,4],[410,5,411,5],[410,6,411,6],[410,7,411,7],[410,8,411,8],[412,2,413,2],[412,3,413,3],[412,4,413,4],[412,5,413,5],[412,6,413,6],[412,7,413,7],[412,8,413,8],[415,0,416,0],[415,2,416,2],[415,3,416,3],[418,0,418,3],[419,0,421,0],[419,2,420,2],[419,3,420,3],[419,4,420,4],[419,5,420,5],[423,0,423,2],[427,0,427,3],[428,0,429,0],[434,0,434,2],[435,0,436,0],[435,2,436,2],[435,3,436,3],[435,4,436,4],[439,0,439,2],[440,0,441,0],[440,2,441,2],[440,3,441,3],[440,4,441,4],[444,0,444,2],[445,0,447,0],[449,0,449,2],[450,0,451,0],[450,2,451,2],[455,1,456,2]]}
[]
["FOR THE PROVISION OF MINOR CONSTRUCTION, MAINTENANCE, AND REPAIR WORK AT THE PREMISES OF FOSKOR (PTY) LIMITED IN PHALABORWA AND NAMAKGALE, INCLUDING SERVICES AT THE CAFETERIA WITHIN THE PLANT AND MINING DEPARTMENTS.\nFOR THE PERIOD OF THREE YEARS"]
[]
[{"$nulls":3},"Earth","Shale","Soft rock"]
[1.1,"Excavations","m³","R","R","R"]
[null,"Backfill levelled not compacted","m³","R","R","R"]
[null,"Backfill compacted in 300mm layers","m³","R","R","R"]
[null,"Backfill compacted in 150mm layers","m³","R","R","R"]
[null,"Load, transport and unload","m³/km","R","R","R"]
[]
[{"$nulls":4},"Earth or shale","Crushed rock","Sand or Ash"]
[1.2,"Spreading & levelling of material","50 mm layers","m³","R","R","R"]
[null,null,"100 mm layers","m³","R","R","R"]
[null,null,"300 mm layers","m³","R","R","R"]
[]
[{"$nulls":3},"Slabs","Columns","Foundations"]
[1.3,"Demolition of reinforced concrete","m³","R","R","R"]
[null,null,"m³","R","R","R"]
[null,null,"m³","R","R","R"]
[null,"Demolition of non-reinforced concrete","m³","R","R","R"]
[null,null,"m³","R","R","R"]
[null,null,"m³","R","R","R"]
[]
[{"$nulls":3},"1 brick wall (Double)","½ brick wall (Single)"]
[1.4,"Erecting of brick walls – FACE BRICK","m²","R","R"]
[null,"Erecting of brick walls – STOCK BRICK","m²","R","R"]
[null,"Demolition of brick walls – FACE BRICK","m²","R","R"]
[null,"Demolition of brick walls –STOCK BRICK","m²","R","R"]
[]
[{"$nulls":3},"Slabs","Columns","Foundations"]
[1.5,"General purpose REINFORCED concrete structures","m3","R","R","R"]
[null,"·   Minimum reinforcing to be as per MR Reference 245"]
[null,"·   25MPa"]
[null,"·   Only HT deformed rounds"]
[null,"·   Cement surface 50mm from reinforcing"]
[null,"·   Including Shuttering"]
[]
[]
[{"$nulls":3},"Slabs","Columns","Foundations"]
[1.6,"General purpose concrete structures","m3","R","R","R"]
[null,"·   25Mpa"]
[null,"·   Including Shuttering"]
[]
[]
[1.7,"Cement screed on Concrete floor 38 – 40 mm Thick ","m²","R"]
[null,"25Mpa cement screed on concrete floor"]
[null,"(70% of surface chipped)"]
[]
[1.8,"Plastering of NEW brick walls (Cement 3:1 Sand)","m²","R"]
[null,"Re-Plastering of OLD brick walls (Cement 3:1 Sand)","m²","R"]
[null,"(Including remove OLD plaster and 70% surface chipped)"]
[]
[]
["PRICING SCHEDULE #1 (Cont)"]
["MASONRY"]
[]
[{"$nulls":3},"Floor","Wall"]
[1.9,"Laying of ceramic tiles  (Floor & wall)","m²","R","R"]
[null,"Cost to include -Tile cement/adhesive and 70% area chipped."]
[null,"Cost to exclude:  Tiles and grout to be quoted on minor works request at cost plus 10% handling fee"]
[null,"Removal of ceramic tiles","m²","R","R"]
[]
[{"$nulls":3},"Soap dish","Toilet paper holders"]
[1.1,"Replace / install NEW White Ceramic fixture","each","R","R"]
[null,"Replace / install NEW Stainless steel fixture","each","R","R"]
[]
[{"$nulls":5},"Single","Double"]
[1.11,"Steel door Frame","REPLACE","Remove OLD and Install NEW door Frame. (Including Supply of NEW Frame)","each","R","R"]
[null,null,"NEW","Supply and Install NEW door Frame.","each","R","R"]
[{"$nulls":3},"(Including Supply of NEW Frame)"]
[null,"Steel door only","REPLACE","Remove OLD and Install NEW door","each","R","R"]
[{"$nulls":3},"(Including Supply of NEW door)"]
[null,null,"NEW","Supply and Install NEW door","each","R","R"]
[{"$nulls":3},"(Including Supply of NEW door)"]
[null,"Steel door and frame complete Unit","REPLACE","Remove OLD and Install NEW Frame and Door","each","R","R"]
[{"$nulls":3},"(Including Supply NEW Frame and door)"]
[null,null,"NEW","Install NEW Steel door and Frame","each","R","R"]
[{"$nulls":3},"(Including Supply NEW Frame and door)"]
["Excluding door locks,  hinges and paint"]
[]
[1.12,"Steel Window Frame","REPLACE","Remove OLD and Install NEW  Window Frame (Excluding supply of NEW frame, include repaint)? ","window circumference in m","R"]
[null,null,"NEW","Install Window Frame. (Excluding supply of NEW frame include repaint)? ","window circumference in m","R"]
[]
[{"$nulls":3},"REPLACE","NEW"]
[1.13,"Placing of glass in window pane","m²","R","R"]
[null,"(Including window putty and repaint to original colour)"]
[null,"Window Putty, including paint to original colour ","p/m","R","R"]
[]
[{"$nulls":3},"NEW","Re-lay OLD"]
[1.14,"80 mm Interlocking paving stones ","m²","R","R"]
[null,"(Including levelling and sand base)"]
[null,"50 X 100 X 200 mm paving stones","m²","R","R"]
[null,"(Including levelling and of sand base)"]
[null,"Removal and disposal of paving bricks, including re-levelling of area","m²","R"]
[]
[]
["PRICING SCHEDULE #1 (Cont)"]
["MASONRY"]
[]
[1.15,"Install wall mounted air conditioner box","REPLACE","Replace existing wall mounted air conditioner / box","each","R"]
[{"$nulls":3},"(Remove OLD, install NEW and repaint walls to original colour) "]
[null,null,"NEW","Install NEW wall mounted air conditioner / box ","each","R"]
[{"$nulls":3},"(Make hole, install and repaint walls to original colour)"]
[null,null,"REMOVE","Remove OLD wall mounted air conditioner / box"]
[{"$nulls":3},"(Remove, brick up, finish/repaint to original wall colour and texture)"]
[]
[{"$nulls":4},"25mm dia","50mm dia","100mm dia"]
[1.16,"Core drilling – walls and non-reinforced concrete structures","Vertical","p/m","R","R","R"]
[null,null,"Horizontal","p/m","R","R","R"]
[null,"Core drilling –reinforced concrete ","Vertical","p/m","R","R","R"]
[null,"Structures","Horizontal","p/m","R","R","R"]
[]
[1.17,"Seal 210 litre drum containing waste with 100mm thick 25Mpa cement topping ","each","R"]
[]
[]
[]
[]
["PRICING SCHEDULE #2"]
["CARPENTRY"]
[{"$nulls":4},"Roofing","Side cladding"]
[2.1,"Remove OLD & replace with NEW galvanised sheeting","IBR 0.8mm","m²","R","R"]
[null,null,"Corrugated 0.8mm","m²","R","R"]
[null,"Install NEW galvanised sheeting","IBR 0.8mm","m²","R","R"]
[null,null,"Corrugated 0.8mm","m²","R","R"]
[null,"Re-fix OLD galvanised sheeting to original specification",null,"m²","R","R"]
[]
[{"$nulls":4},"Roofing","Side cladding"]
[2.2,"Waterproof galvanised sheeting ","With bitumen membrane according to OEM (Including application and paint)","m²","R","R"]
[null,null,"With Rain Seal and Membrane according to OEM (Including application and paint)","m²","R","R"]
[]
[]
[{"$nulls":3},"Replace OLD with NEW","Fit NEW"]
[2.3,"50mm X75mm  wooden roof PURLINS","m","R","R"]
[null,"38mm X 114mm wooden roof TRUSSES","m","R","R"]
[null,"38mm X 38mm wooden roof TILE BATTENS","m","R","R"]
[null,"38mm X 50mm wooden roof CEILING BRANDING","m","R","R"]
[]
[{"$nulls":4},"Replace OLD with NEW","Fit NEW"]
[2.4,"Ceiling ","Fibre cement board ","m²","R","R"]
[null,null,"Rhino board ","m²","R","R"]
[null,null,"Suspended  With GYPREX FROST WHITE 12.5 x 1200 x 600mm","m²","R","R"]
[]
[{"$nulls":3},"Replace OLD with NEW","Fit NEW"]
[2.5,"CORNICE 70mm","m",null,"R"]
[null,"SKIRTING 75mm","m",null,"R"]
[null,"QUARTERING 19mm","m",null,"R"]
[]
[{"$nulls":3},"Replace OLD with NEW","Fit NEW"]
[2.6,"Fibre FACIA Board 150 mm","m","R","R"]
[null,"Fibre FACIA Board 228 mm","m","R","R"]
[null,"uPVC FACIA Board","m","R","R"]
[null,"Fibre BARGE Board 150 mm","m","R","R"]
[null,"Fibre BARGE Board 228 mm","m","R","R"]
[null,"uPVC BARGE Board","m","R","R"]
[]
[{"$nulls":4},"Replace OLD with NEW","Fit NEW"]
[2.7,"Single doors","Flush panel Masonite (Brown Hard board) Flat","Each","R","R"]
[null,"Include Labour for hanging of door.","Sapele Mahogany Veneer (Flat )","Each","R","R"]
[null,"Exclude Union Lock and 100mm But Hinges.","Frame/Ledge & Z-Brace B (Pine)","Each","R","R"]
[null,null,"Frame/Ledge & Z-Brace B (Meranti)","Each","R","R"]
[]
[]
[]
[]
["PRICING SCHEDULE #2 (Cont)"]
["CARPENTRY"]
[]
[]
[{"$nulls":4},"Replace OLD with NEW","Fit NEW"]
[2.8,"Double doors","Flush panel Masonite (Brown Hard board) Flat","Each","R","R"]
[null,"Include: Rebate Kit, 2 barrel bolts and Labour For installation.","Flush panel Sapele Mahogany Veneer (Flat )","Each","R","R"]
[null,"Exclude  Union Lock and 100mm Butt Hinges.","Frame/Ledge & With Z-Brace","Each","R","R"]
[null,null,"(Meranti)"]
[]
[{"$nulls":4},"Replace OLD with NEW*","Fit NEW"]
[2.9,"Door Fixtures and Fittings","Mortice 2 lever lock with keys – UNION  (Exl handles)","Each","R","R"]
[null,null,"NO Alternative allowed"]
[null,null,"Mortice 2 lever lock with keys – UNION  (Incl handles)","Each","R","R"]
[null,null,"NO Alternative allowed"]
[null,null,"Night Latch lock – UNION","Each","R","R"]
[null,null,"Door Handle only - UNION (Exl lock)*","Each","R","R"]
[null,null,"Bathroom/Toilet indicator lock – UNION","Each","R","R"]
[null,null,"100mm stainless steel Butt Hinges ","Each","R","R"]
[null,null,"Heavy Duty Ryobi Door Closer .80 kg ","Each","R","R"]
["*ALL Locks and Handles Replaced MUST be Returned to Civil w/s"]
[{"$nulls":3},"Replace OLD with NEW","Fit NEW"]
[2.1,"Window stay fastener","Each",null,"R"]
[null,"Window fastener","Each",null,"R"]
[]
[]
["PRICING SCHEDULE #3"]
["PLUMBING"]
[{"$nulls":4},"Replace OLD","Install NEW"]
[3.1,"Hot water geyser complete and installed ","100 litre","Each","R","R"]
[null,"ONLY Franke or Kwikot"]
[null,"(Including brackets & fixtures)","150 litre","Each","R","R"]
[]
[{"$nulls":4},"Replace OLD","Install NEW"]
[3.2,"WASH BASIN: Glazed white ceramic mounted on wall. ","Bain minimum width 560mm","Each","R","R"]
[null,null,"Chromed Waste trap (Standard)"]
[null,null,"P-trap","Each","R","R"]
[null,null,"S-Trap","Each","R","R"]
[null,null,"Connector Braided 300 mm FxF (Flexi Hose )","Each","R","R"]
[]
[{"$nulls":4},"Replace OLD","Install NEW"]
[3.3,"TOILET: glazed white ceramic mounted on wall / floor","Bowl (Complete)","Each","R","R"]
[null,null,"Cistern (Tank)","Each","R","R"]
[null,null,"Cistern (Kit)","Each","R","R"]
[null,null,"Flush master chromed Complete","Each","R","R"]
[null,null,"Seat (White Heavy duty)","Each","R","R"]
[]
[{"$nulls":4},"Replace OLD","Install NEW"]
[3.4,"URINAL: glazed white ceramic mounted on wall","Bowl","Each","R","R"]
[null,null,"Chromed Waste trap","Each","R","R"]
[null,null,"Urinal Flush master Junior Slim line","Each","R","R"]
[null,null,"(Complete kit)"]
[]
[{"$nulls":4},"Replace OLD","Install NEW"]
[3.5,"BATH: Glazed white ceramic 1.7m Installed","Bath tub 1.7m","Each","R","R"]
[null,null,"Waste","Each","R","R"]
[]
[{"$nulls":4},"15mm","20mm","25mm","32mm","40mm","50mm"]
[3.6,"REPLACE OLD galvanised water piping","Length m","Meter","R","R","R","R","R","R"]
[null,"(Chasing, plastering, painting, etc. addressed under MASONRY & PAINTING)","Elbow 90°","Each","R","R","R","R","R","R"]
[null,null,"T-Piece","Each","R","R","R","R","R","R"]
[null,null,"Union","Each","R","R","R","R","R","R"]
[null,null,"Socket","Each","R","R","R","R","R","R"]
[null,null,"Nipple","Each","R","R","R","R","R","R"]
[null,null,"Gate valve","Each","R","R","R","R","R","R"]
[null,null,"Ball valve","Each","R","R","R","R","R","R"]
[null,null,"Johnson Coup","Each","R","R","R","R","R","R"]
[]
[{"$nulls":4},"15mm","20mm","25mm","32mm","40mm","50mm"]
[3.7,"INSTALL NEW galvanised water piping","Length m","Meter","R","R","R","R","R","R"]
[null,"(Chasing, plastering, painting, etc. addressed under MASONRY & PAINTING)","Elbow 90°","Each","R","R","R","R","R","R"]
[null,null,"T-Piece","Each","R","R","R","R","R","R"]
[null,null,"Union","Each","R","R","R","R","R","R"]
[null,null,"Socket","Each","R","R","R","R","R","R"]
[null,null,"Nipple","Each","R","R","R","R","R","R"]
[null,null,"Johnson Coup","Each","R","R","R","R","R","R"]
[]
["PRICING SCHEDULE #3 (Continued)"]
["PLUMBING"]
[{"$nulls":4},"REPLACE OLD",null,"INSTALL NEW"]
[{"$nulls":4},"15mm","22mm","15mm","22mm"]
[3.8,"Chromed bathroom & kitchen fittings","Bib tap – wall mount","Each","R","R","R","R"]
[null,"(COBRA ONLY)","Pillar tap – basin mount","Each","R","R","R","R"]
[null,null,"Mixer pillar tap swivel head – basin mount","Each","R","R","R","R"]
[null,null,"Mixer tap swivel head – wall mount","Each","R","R","R","R"]
[null,null,"Under tile tap – shower","Each","R","R","R","R"]
[null,null,"Single function shower rose","Each","R","R","R","R"]
[null,null,"Shower arm","Each","R","R","R","R"]
[]
[{"$nulls":4},"REPLACE OLD","INSTALL NEW"]
[3.9,"110mm Sewer and Drainage uPVC piping","Length","meter","R","R"]
[null,null,"Straight couplings","Each","R","R"]
[null,null,"Tee  ","Each","R","R"]
[null,null,"Bend 90°","Each","R","R"]
[null,null,"Bend 90° Inspection Eye","Each","R","R"]
[null,null,"Bend 90° Inspection Eye/ Vent horn","Each","R","R"]
[null,null,"Bend Offset","Each","R","R"]
[null,null,"Bend 45°","Each","R","R"]
[null,null,"Rodding Eye","Each","R","R"]
[null,null,"Gully Head","Each","R","R"]
[null,null,"Gully P- Trap","Each","R","R"]
[null,null,"Offset Pan Connector","Each","R","R"]
[null,null,"Y-Junction (Tee 45°)","Each","R","R"]
[]
[{"$nulls":4},"REPLACE OLD","INSTALL NEW"]
[3.1,"50mm Waist uPVC piping","Length p/m","Each","R","R"]
[null,null,"Straight couplings","Each","R","R"]
[null,null,"Bend 90°","Each","R","R"]
[null,null,"Bend 90° Inspection Eye","Each","R","R"]
[null,null,"Bend 45° ","Each","R","R"]
[null,null,"Tee  ","Each","R","R"]
[null,null,"Tee  Inspection Eye","Each","R","R"]
[null,null,"Y-Junction (Tee 45°)","Each","R","R"]
[null,null,"Socket reducer","Each","R","R"]
[null,null,"Adapter (to Iron)","Each","R","R"]
[]
[{"$nulls":4},"16mm","22mm","25mm","32mm","40mm","50mm"]
[3.11,"REPLACE OLD","Length p/m","Meter","R","R","R","R","R","R"]
[null,"HDPE Class 10 water piping (SABS Specifications/Standards SANS 4427)","Compression Fittings        (Plasson/Marley)"]
[null,null,"Coupling","Each","R","R","R","R","R","R"]
[null,null,"Adaptor","Each","R","R","R","R","R","R"]
[null,null,"Elbow","Each","R","R","R","R","R","R"]
[null,null,"Tee","Each","R","R","R","R","R","R"]
[null,null,"Plug","Each","R","R","R","R","R","R"]
["Reducers priced cost plus 10%"]
[]
[]
["PRICING SCHEDULE #3 (Continued)"]
["PLUMBING"]
[]
[{"$nulls":4},"16mm","22mm","25mm","32mm","40mm","50mm"]
[3.12,"INSTALL NEW","Length p/m","Meter","R","R","R","R","R","R"]
[null,"HDPE Class 10 water piping (SABS Specifications/Standards SANS 4427)","Compression Fittings        (Plasson/Marley)"]
[null,null,"Coupling","Each","R","R","R","R","R","R"]
[null,null,"Adaptor","Each","R","R","R","R","R","R"]
[null,null,"Elbow","Each","R","R","R","R","R","R"]
[null,null,"Tee","Each","R","R","R","R","R","R"]
[null,null,"Plug","Each","R","R","R","R","R","R"]
["Reducers priced cost plus 10%"]
[]
[{"$nulls":4},"16mm","22mm","25mm","32mm","40mm","50mm"]
[3.13,"REPLACE OLD","Length p/m","Meter","R","R","R","R","R","R"]
[null,"HDPE Class 3 water piping (SABS Specifications/Standards SANS 4427)","Coupling","Each","R","R","R","R","R","R"]
[null,null,"Adaptor","Each","R","R","R","R","R","R"]
[null,null,"Elbow","Each","R","R","R","R","R","R"]
[null,null,"Tee","Each","R","R","R","R","R","R"]
[null,null,"Plug","Each","R","R","R","R","R","R"]
["Reducers priced cost plus 10%"]
[{"$nulls":4},"16mm","22mm","25mm","32mm","40mm","50mm"]
[3.14,"INSTALL NEW","Length p/m","Meter","R","R","R","R","R","R"]
[null,"HDPE Class 3 water piping (SABS Specifications/Standards SANS 4427)","Coupling","Each","R","R","R","R","R","R"]
[null,null,"Adaptor","Each","R","R","R","R","R","R"]
[null,null,"Elbow","Each","R","R","R","R","R","R"]
[null,null,"Tee","Each","R","R","R","R","R","R"]
[null,null,"Plug","Each","R","R","R","R","R","R"]
["Reducers priced cost plus 10%"]
[{"$nulls":4},"REPLACE OLD",null,"INSTALL NEW"]
[{"$nulls":4},"15mm","22mm","15mm","22mm"]
[3.15,"Copper water piping","Length p/m","Meter","R","R","R","R"]
[null,"(LEAD SOLDER)","Elbow 90°","Each","R","R","R","R"]
[null,null,"Elbow 45°","Each","R","R","R","R"]
[null,null,"Tee","Each","R","R","R","R"]
[null,null,"Straight Coupler","Each","R","R","R","R"]
[null,null,"Union Coupler","Each","R","R","R","R"]
[null,null,"Tube End Cap.","Each","R","R","R","R"]
[null,null,"Wall Plate Elbow 90°","Each","R","R","R","R"]
[null,null,"Full Crossover","Each","R","R","R","R"]
["Reducers priced cost plus 10%"]
[{"$nulls":4},"REPLACE OLD",null,null,"INSTALL NEW"]
[{"$nulls":4},"15mm","22mm","15mm",null,"22mm"]
[3.16,"Copper water piping","Length m","Meter","R","R","R",null,"R"]
[null,"(Compression Fittings CONEX)","Elbow 90°","Each","R","R","R",null,"R"]
[null,null,"Elbow 45°","Each","R","R","R",null,"R"]
[null,null,"Tee","Each","R","R","R",null,"R"]
[null,null,"Straight Coupler","Each","R","R","R",null,"R"]
[null,null,"Union Coupler","Each","R","R","R",null,"R"]
[null,null,"Tube End Cap.","Each","R","R","R",null,"R"]
[null,null,"Wall Plate Elbow 90°","Each","R","R","R",null,"R"]
[null,null,"Full Crossover","Each","R","R","R",null,"R"]
[]
["Reducers priced cost plus 10%"]
[]
["PRICING SCHEDULE #3 (Continued)"]
["PLUMBING"]
[]
[{"$nulls":4},"15mm","22mm","25mm","32mm","40mm","50mm"]
[3.17,"REPLACE OLD Valves","Gate Valve Brass","Each","R","R","R","R","R","R"]
[null,null,"Ball Valve Galvanise ","Each","R","R","R","R","R","R"]
[null,null,"Ball valve C/P","Each","R","R","R","R","R","R"]
[null,null,"Ball Valve Brass","Each","R","R","R","R","R","R"]
[]
[{"$nulls":4},"15mm","22mm","25mm","32mm","40mm","50mm"]
[3.18,"INSTALL NEW Valves","Gate Valve Brass","Each","R","R","R","R","R","R"]
[null,null,"Ball Valve Galvanise ","Each","R","R","R","R","R","R"]
[null,null,"Ball valve C/P","Each","R","R","R","R","R","R"]
[null,null,"Ball Valve Brass","Each","R","R","R","R","R","R"]
[]
[{"$nulls":3},"Replace OLD","Install NEW"]
[3.19,"Flashings Fibrocement","m","R","R"]
[null,"Flashings uPVC","m","R","R"]
[null,"Galvanised Iron gutters (Complete with all fittings)","m","R","R"]
[null,"Galvanised Iron down pipes (Complete standard single story)","Each","R","R"]
[null,"uPVC gutters  (Complete with all fittings)","m","R","R"]
[null,"uPVC down pipes  (Complete standard single story)","Each","R","R"]
[]
[3.2,"Unblock sewerage drain – At toilet","Each","R"]
[null,"Unblock sewerage drain – Main line","Each","R"]
[null,"Unblock wash basin drain","Each","R"]
[null,"Unblock shower drain","Each","R"]
[]
["PRICING SCHEDULE #4"]
["PAINTWORK"]
[4.1,"CONCRETE / MASONRY",null,"Interior","Exterior"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent"]
[null,"Clean (NEW) cement / plastered walls","m²","R","R"]
[null,"(Primer & two colour over coats)"]
[null,"Previously painted cement / plastered walls","m²","R","R"]
[null,"(Primer & two colour over coats)"]
[null,"Clean (NEW) face brick walls","m²","R","R"]
[null,"(Primer and two colour over coats)– "]
[null,"Previously painted face brick walls","m²","R","R"]
[null,"(Primer and two colour over coats)"]
[null,"Apply one colour over coat – plastered walls","m²","R","R"]
[null,"Apply one colour over coat – Face brick walls","m²","R","R"]
[]
[4.2,"GALVANISED METAL SHEETING",null,null,"Interior","Exterior"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent"]
[null,"Clean (NEW) galvanized sheet metal – CLADDING","IBR","m²","R","R"]
[null,"(Apply primer and two colour over coats)","Corrugated","m²","R","R"]
[null,"Previously painted galvanized sheet metal – CLADDING","IBR","m²","R","R"]
[null,"(Clean and apply primer and two colour over coats)","Corrugated","m²","R","R"]
[null,"Clean (NEW) galvanized sheet metal – ROOF TOP","IBR","m²","R",null,"R"]
[null,"(Apply primer and two colour over coats)","Corrugated","m²","R",null,"R"]
[null,"Previously painted galvanized sheet metal – ROOF TOP","IBR","m²","R",null,"R"]
[null,"(Clean and apply primer and two colour over coats)","Corrugated","m²","R",null,"R"]
[]
[]
[4.3,"METAL STRUCTURES",null,"Structures > 50 mm","Structures < 50 mm"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent"]
[null,"Clean (NEW)","m²","R","R"]
[null,"(Sand clean, apply primer and two colour over coats)"]
[null,"Previously painted","m²","R","R"]
[null,"(Sand clean and apply primer and two colour over coats)"]
[]
[4.4,"METAL PIPING",null,"15-32mm","40-80mm","100mm","150mm","200mm","300mm"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent"]
[null,"Clean (NEW)","m","R","R","R","R","R","R"]
[null,"(Sand clean, apply primer and two colour over coats)"]
[null,"Previously painted","m","R","R","R","R","R","R"]
[null,"(Sand clean and apply primer and two colour over coats)"]
[]
[4.5,"Ceilings (Acrylic PVA – white)","m²","R"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent"]
[]
[{"$nulls":4},"Single","Double"]
[4.6,"Doors","FL & B ","Each","R","R"]
[null,"(Primer and two colour overcoats –enamel)"]
[null,"ONLY Plascon, O’Grady, Sigma, Dulux or Prominent","Flash panel door","Each","R","R"]
[]
[{"$nulls":3},"Single","Double"]
[4.7,"Doors wooden (Water resistant varnish – Apply minimum of 3 coats) ","Each","R","R"]
[]
[]
[{"$nulls":4},"Single","Double"]
[4.8,"Door frames","Steele ","Each","R","R"]
[null,"(Primer and two colour overcoats –enamel)","Timber","Each","R","R"]
[]
["PRICING SCHEDULE #4 (Continued)"]
["PAINTWORK"]
[]
[{"$nulls":3},"OLD","NEW"]
[4.9,"Steele window frames ","m","R","R"]
[null,"(Clean, repair putty, primer and two colour overcoats – enamel)"]
[]
[]
[{"$nulls":3},"Paint NEW","Repaint OLD"]
[4.1,"Hand railings (Railing yellow and upright black)","Running meter","R","R"]
[null,"(Sand clean, apply primer and two colour over coats)"]
[]
[]
[{"$nulls":3},"Paint NEW","Repaint OLD"]
[4.11,"Flashings","m"]
[null,"Galvanised Iron gutters","m"]
[null,"Galvanised Iron down pipes (Standard single story)","Each"]
[]
[{"$nulls":3},"Structures > 50 mm","Structures < 50 mm","Flat surfaces"]
[4.12,"Sandblast clean metal surfaces","m²","R","R","R"]
[null,"Sandblast rusted/painted surfaces",null,"R","R","R"]
[]
[]
[null,"TOTAL ESTIMATE PER MONTH"]
[null,"Assuming that the repairs for each task are carried out once a month."]