{"text_format":"3","workbook":"xlsx","n_sheets":40,"sheets":["PV1","PV2","PV3","PV4","T1A DC","T1A ","T1B","T1C","T2","T3","T4AD","T4AS","T4AD DC","T4BD","T4BS","T5AD","T5AS","T5BD","T5BS","T6","T7","T8T","T8","T9","T10","T11","T12","T13D","T13S","T14S AUTOMATIC","Permitted Ancillaries","25 Seater Bus","30 Seater Bus","Bus 45 Seater","60 Seater Bus","65 Seater Bus","Sheet10","Sheet11","Sheet12","Sheet13"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"PV1","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and 2 passengers up to a GVM of 4100 kg on all types of road surfaces with up to 20% off road usage"]
["PV1","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Panel Van 4x2 Standard roof >3500<=4100kg GVM (Single wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and pasengers","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"Tool Boxes"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Fog Lights"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["POWER STEERING","To be Standard",{"$nulls":4},"Driving lights"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Reverse alarm / beeper"]
["PARK DISTANCE CONTROLL WITH CAMERA OR BEEPER","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["Engine Protection Device Manufactures approved (Factory Warranty)","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["TOWBAR PRICE FULLY INSTALLED","To be Standard"]
["VEHICLE CONFIGURATION :","Panel Van 4x2 Standard roof up to 4100kg GVM"]
["TRACTION: ","4x2"]
["Loading Volume ","8cm³-10,8cm³"]
["Load Area  Height","1533mm – 1912mm"]
["Load Area  Width","1736mm  - 1800mm"]
["Load Area  Length","3000mm - 3265mm"]
["Approximate body/ payload Kg","1500 kg"]
["POWER RATING - kW","100Kw"]
["TORQUE RATING - NM","350Nm"]
["Permissible Front axle rating “ Max.”","1600kg – 1850kg"]
["Permissible Rear axle rating “ Max.”","1060kg – 2240kg"]
["Wheel base “ Max.”","3000mm – 3578mm"]
["Fuel (Diesel)","YES"]
["Fully synchromesh 6 speed gearbox","YES"]
["Tyres (Size)  (Single wheel application)","Specify"]
["Seat Belts: SABS approved","YES"]
["Seats to be cloth","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"PV2","index":1,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and 2 passengers up to a GVM of 5400 kg on all types of road surfaces with up to 20% off road usage"]
["PV2","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Panel Van 4x2 High roof >3600<=4100kg GVM (Dual wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"Tool Boxes"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Fog Lights"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["POWER STEERING","To be Standard",{"$nulls":4},"Driving lights"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Reverse alarm / beeper"]
["PARK DISTANCE CONTROL WITH CAMERA OR BEEPER","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["Engine Protection Device Manufactures approved (Factory Warranty)","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["TOWBAR PRICE FULLY INSTALLED","To be Standard"]
["VEHICLE CONFIGURATION :","Panel Van 4x2 high roof up to 4100kg GVM"]
["TRACTION: ","4x2"]
["Loading Volume ","11.5 cm³ – 13.9 cm³"]
["Load Area  Height","1900cmm – 2146cmm"]
["Load Area  Width","1730cmm  - 1800cmm"]
["Load Area  Length","3210cmm -  3720cmm "]
["Approximate body/ payload Kg","1500 kg"]
["POWER RATING - kW","100 Kw"]
["TORQUE RATING - NM","350 Nm"]
["Permissible Front axle rating “ Max.”","1600kg – 1850kg"]
["Permissible Rear axle rating “ Max.”","2060kg – 2240kg"]
["Wheel base “ Max.”","3550mm – 3578mm"]
["Fuel (Diesel)","YES"]
["Fully synchromesh 6 speed gearbox","YES"]
["Tyres (Size)  (Dual wheel application)","Specify"]
["Seat Belts: SABS approved","YES"]
["Seats to be cloth","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"PV3","index":2,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and 2 passengers up to a GVM of 5350 kg on all types of road surfaces with up to 20% off road usage"]
["PV3","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Panel Van 4x2 Standard roof > 4100 < 5350 GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"Tool Boxes"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Fog Lights"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["POWER STEERING","To be Standard",{"$nulls":4},"Driving lights"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Reverse alarm / beeper"]
["PARK DISTANCE CONTROL WITH CAMERA OR BEEPER","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["Engine Protection Device Manufactures approved (Factory Warranty)","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["TOWBAR PRICE FULLY INSTALLED","To be Standard"]
["VEHICLE CONFIGURATION :","Panel Van 4x2 Standard roof up to 5350kg GVM"]
["TRACTION: ","4x2"]
["Loading Volume ","15,2m3"]
["Load Area  Height","1940mm"]
["Load Area  Width","1820 mm"]
["Load Area  Length","4560 mm"]
["Approximate body/ payload Kg","2800 kg"]
["POWER RATING - kW","150Kw"]
["TORQUE RATING - NM","400Nm"]
["Permissible Front axle rating “ Max.”","1800kg "]
["Permissible Rear axle rating “ Max.”","3700 kg"]
["Wheel base “ Max.”","4100 mm"]
["Fuel (Diesel)","YES"]
["Fully synchromesh 6 speed gearbox","YES"]
["Tyres (Size)  ( dual wheel application)","Specify"]
["Seat Belts: SABS approved","YES"]
["Seats to be cloth","YES"]
["Mud-flaps: Factory fitted","Specify"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"PV4","index":3,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and 2 passengers up to a GVM of 5400 kg on all types of road surfaces with up to 20% off road usage"]
["PV4","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Panel Van 4x2 High roof 4100 kg < 5400 kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"Tool Boxes"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Fog Lights"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["POWER STEERING","To be Standard",{"$nulls":4},"Driving lights"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Reverse alarm / beeper"]
["PARK DISTANCE CONTROL WITH CAMERA OR BEEPER","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["Engine Protection Device Manufactures approved (Factory Warranty)","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["TOWBAR PRICE FULLY INSTALLED","To be Standard"]
["VEHICLE CONFIGURATION :","Panel Van 4x2 High  roof up to 5400kg GVM"]
["TRACTION: ","4x2"]
["Loading Volume ","15,2m3"]
["Load Area  Height","1940mm"]
["Load Area  Width","1820 mm"]
["Load Area  Length","4560 mm"]
["Approximate body/ payload Kg","2800 kg"]
["POWER RATING - kW","150Kw"]
["TORQUE RATING - NM","400Nm"]
["Permissible Front axle rating “ Max.”","1800kg "]
["Permissible Rear axle rating “ Max.”","3700 kg"]
["Wheel base “ Max.”","4100 mm"]
["Fuel (Diesel)","YES"]
["Fully synchromesh 6 speed gearbox","YES"]
["Tyres (Size) ( dual wheel application)","Specify"]
["Seat Belts: SABS approved","YES"]
["Seats to be cloth","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T1A DC","index":4,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and 4 passengers up to a GVM of 5300kg –  on all types of road surfaces with up to 40% off road usage"]
["T1A D/C","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4x2 >3500 <5300kg GVM Double Cab","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Cargo van body"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Tool cab"]
["POWER STEERING","To be Standard",{"$nulls":4},"Ladder Rack"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"“H” Frame"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Tool Boxes"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Fog Lights"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Working Lights"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["PARK DISTANCE CONTROL WITH CAMERA OR REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["TOWBAR PRICE FULLY INSTALLED","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["VEHICLE CONFIGURATION :","Light Truck 4x2 D/C >3500 <5300kg GVM",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","80Kw"]
["Torque Rating - NM","270Nm"]
["Permissible Front axle rating ","1600 to 2300"]
["Permissible Rear axle rating ","2300 to 3500"]
["Approximate body/ payload Kg","1800 kg"]
["D/T Rating “Min.”","4505 Kg"]
["Wheel base “ Max.”","2520mm"]
["Chassis to facilitate the fitting of hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) ","Specify"]
["Number of gears, manual","YES"]
["Seats to be cloth","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T1A ","index":5,"n_rows":52,"n_cols":7,"rows_kept":52,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 5500 kg on all types of road surfaces with up to 40% off road usage"]
["T1A ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4x2 >3500 <5500kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"PTO"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Cargo van body"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Tool cab"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Ladder Rack"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"“H” Frame"]
["PTO(PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Tool Boxes"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Fog Lights"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Working Lights"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["PARK DISTANCE CONTROL WITH CAMERA OR REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["VEHICLE CONFIGURATION :","Light Truck 4x2 >3500 <5500 GVM",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["TRACTION: ","4x2",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Power Rating - Kw","80Kw"]
["Torque Rating - NM","270Nm"]
["Permissible Front axle rating “ Max.”","1600 to 2300 kg"]
["Permissible Rear axle rating “ Max.”","2300 to 3500 kg"]
["Approximate body / payload  ","1912 to 3400 kg"]
["D/T Rating “Min.”","5900 to 8800 Kg"]
["Wheel base “ Max.”","2545 mm"]
["Chassis to facilitate the fitting of hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size)","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T1B","index":6,"n_rows":52,"n_cols":7,"rows_kept":52,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 5500 – 6500kg on all types of road surfaces with up to 40% off road usage"]
["T1B","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4x2 >5500 <6500kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"PTO"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Cargo van body"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Ladder Rack"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"“H” Frame"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Tool Boxes"]
["PTO(PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Fog Lights"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Working Lights"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["PARK DISTANCE CONTROL WITH CAMERA OR REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Reverse alarm / beeper"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["VEHICLE CONFIGURATION :","Light Truck 4x2 >5500 <6500kg GVM",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["TRACTION: ","4x2",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Power Rating - Kw","100Kw"]
["Torque Rating - NM","370Nm"]
["Permissible Front axle rating “ Max.”","2400 - 3400kg"]
["Permissible Rear axle rating “ Max.”","4400 - 5100kg"]
["Approximate body / payload  ","3400 to 4500"]
["D/T Rating “Min.”","7100 to 8300 Kg"]
["Wheel base “ Max.”","3400mm"]
["Chassis to facilitate the fitting of hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) ","SPECIFY"]
["Number of gears, manual","SPECIFY"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T1C","index":7,"n_rows":52,"n_cols":7,"rows_kept":52,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 7000 kg on all types of road surfaces with up to 40% off road usage"]
["T1C","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4x2 >6500 <7500kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard",{"$nulls":4},"PTO"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Cargo van body"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Tool cab"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Ladder Rack"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"“H” Frame"]
["PTO(PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Tool Boxes"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Fog Lights"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Working Lights"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Amber Revolving Light"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["VEHICLE CONFIGURATION :","Light Truck 4x2 >6500 <7500 GVM",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["TRACTION: ","4x2",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Power Rating - Kw","100Kw"]
["Torque Rating - NM","370Nm"]
["Permissible Front axle rating “ Max.”","3100kg"]
["Permissible Rear axle rating “ Max.”","5000 - 5500kg"]
["Approximate body / payload  ","4600 to 5067 kg"]
["D/T Rating “Min.”","9300 to 10300 Kg"]
["Wheel base “ Max.”","3800mm"]
["Chassis to facilitate the fitting of hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 750R16 12PR","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T2","index":8,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 12000 kg on all types of road surfaces with up to 40% off road usage"]
["T2","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Medium Truck 4x2 > 7500 < 12000 kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"PTO"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M"]
["ABS BRAKES","To be Standard",{"$nulls":4},"13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M"]
["POWER STEERING","To be Standard",{"$nulls":4},"14 Ton Crane 14M Horizontal, 17.5 Vertical Reach and 530Kg & 14.2M"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Hour meter"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Cargo van body"]
["PTO(PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Tool cab"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Ladder Rack"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"“H” Frame"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Tool Boxes"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Fog Lights"]
["VEHICLE CONFIGURATION :","Medium Truck 4x2 >7500 <12000 GVM",{"$nulls":4},"Working Lights"]
["TRACTION: ","4x2",{"$nulls":4},"Amber Revolving Light"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Power Rating - Kw","125Kw",{"$nulls":4},"Winch type spare wheel carrier "]
["Torque Rating - NM","450Nm",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Front axle rating “ Max.”","4100 to 5500kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","7000kg to 9000kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","17000kg to 21000Kg"]
["Wheel base “ Max.”","4500mm and 4850mm "]
["Chassis to facilitate the fitting of hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 10.00R20 / 11.00X20 / 8.25R20 14PR","Specify"]
["Number of gears, manual","Specify"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T3","index":9,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 17000 kg on all types of road surfaces with up to 40% off road usage"]
["T3","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Heavy Truck 4x2 >15000 <17000kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"14 Ton Crane 14M Horizontal, 17.5 Vertical Reach and 530Kg & 14.2M"]
["ABS BRAKES","To be Standard",{"$nulls":4},"15 Ton Crane 14.35M Horizontal, 16 Vertical Reach and 650Kg & 14.35M"]
["POWER STEERING","To be Standard",{"$nulls":4},"15 Ton Crane 12M Horizontal, 16 Vertical Reach and 650Kg & 14.35M"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Hour meter"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tail lift 2 ton capacity"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["PTO(PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Cargo van body"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Crew cab"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Ladder Rack"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," “H” Frame"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Tool Boxes"]
["VEHICLE CONFIGURATION :","Heavy Truck 4x2 >15000 <17000 GVM",{"$nulls":4},"Stainless steel Water Tank"]
["TRACTION: ","4x2",{"$nulls":4},"Working Lights"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Amber Revolving Light"]
["Power Rating - Kw","150Kw",{"$nulls":4},"Tow bar"]
["Torque Rating - NM","600Nm",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Permissible Front axle rating “ Max.”","6300kg",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Rear axle rating “ Max.”","9000kg",{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["D/T Rating “Min.”","20000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","5650mm",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Chassis to facilitate the fitting of 15Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00X20 or equivalent","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T4AD","index":10,"n_rows":47,"n_cols":7,"rows_kept":47,"merged":[[3,1,3,4],[4,2,4,3],[46,0,46,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 7000 kg on all types of road surfaces with up to 80% off road usage."]
["T4A Dual wheel","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4X4 >4500<=7000KG GVM (Dual wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["DRIVER AND PASSENGER AIRBAGS","Specify"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["POWER STEERING","To be Standard",{"$nulls":4},"PTO"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Cargo van body"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Ladder Rack"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4}," “H” Frame"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Tool Boxes"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Working Lights"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"9.2m live line Aerial platform"]
["VEHICLE CONFIGURATION :","Light Truck 4X4 >4500<=7000KG GVM (Dual wheel application)",{"$nulls":4},"11m Non insulated Aerial platform"]
["TRACTION: ","4x4",{"$nulls":4},"Tow bar"]
["ATTACHED TECHNICAL SPECS BROCHURES FOR VERIFICATION","Specify"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Power Rating - Kw","100 Kw",{"$nulls":4},"Winch type spare wheel carrier "]
["Torque Rating - NM","350 Nm",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Front axle rating “ Max.”","2600 kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","4300 kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","7000 kg"]
["Wheel base “ Max.”","3400 mm to 4000 mm "]
["Chassis to facilitate the fitting of 6Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 7.50R16-10 PR (up to 80% off road usage) Compatible diff ratio","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
[null,"Speicy"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"T4AS","index":11,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 7000 kg on all types of road surfaces with up to 80% off road usage."]
["T4A Single Wheel","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4X4 >4500<=7000KG GVM (Single wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["POWER STEERING","To be Standard",{"$nulls":4},"PTO"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Cargo van body"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Ladder Rack"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4}," “H” Frame"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Tool Boxes"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Working Lights"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"9.2m live line Aerial platform"]
["VEHICLE CONFIGURATION :","Light Truck 4X4 >4500<=7000KG GVM (Single wheel application)",{"$nulls":4},"11m Non insulated Aerial platform"]
["TRACTION: ","4x4",{"$nulls":4},"Tow bar"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Power Rating - Kw","100 Kw",{"$nulls":4},"Winch type spare wheel carrier "]
["Torque Rating - NM","350 Nm",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Front axle rating “ Max.”","2600 kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","4300 kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","7000 kg"]
["Wheel base “ Max.”","3400 mm to 4000 mm "]
["Chassis to facilitate the fitting of 6Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 7.50R16-10 PR (up to 80% off road usage) Compatible diff ratio","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T4AD DC","index":12,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 7000 kg on all types of road surfaces with up to 80% off road usage."]
["T4A Dual wheel D/Cab","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4X4 D/cab >4500<=7000KG GVM (Duel wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["POWER STEERING","To be Standard",{"$nulls":4},"PTO"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Cargo van body"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Ladder Rack"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4}," “H” Frame"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Tool Boxes"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Working Lights"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"9.2m live line Aerial platform"]
["VEHICLE CONFIGURATION :","Light Truck 4X4 D/Cab >4500<=7000KG GVM (Dual wheel application)",{"$nulls":4},"11m Live line Aerial platform"]
["TRACTION: ","4x4",{"$nulls":4},"11m Non insulated Aerial platform"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Tow bar"]
["Power Rating - Kw","100 Kw",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Torque Rating - NM","350 Nm",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Front axle rating “ Max.”","2600 kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Rear axle rating “ Max.”","4300 kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","7000 kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","3400 mm to 4000 mm "]
["Chassis to facilitate the fitting of 6Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 7.50R16-10 PR (up to 80% off road usage) Compatible diff ratio","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T4BD","index":13,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 13000 kg on all types of road surfaces with up to 80% off road usage."]
["T4 B Dual wheel","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4X4 >7000<=13000KG GVM (Dual wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"PTO"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Cargo van body"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Ladder Rack"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4}," “H” Frame"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Tool Boxes"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Working Lights"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["VEHICLE CONFIGURATION :","Light Truck 4X4 >7000<=13000KG GVM (Dual wheel application)",{"$nulls":4},"11m Live line Aerial platform"]
["TRACTION: ","4x4",{"$nulls":4},"16.5m Non insulated Aerial platform"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"18m Non insulated Aerial platform"]
["Power Rating - Kw","150Kw",{"$nulls":4},"Tow bar"]
["Torque Rating - NM","600Nm",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Permissible Front axle rating “ Max.”","4500kg",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Rear axle rating “ Max.”","9000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["D/T Rating “Min.”","20000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4600mm and 4800mm ",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Chassis to facilitate the fitting of 10Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 10.00 R 20 (up to 80% off road usage) Compatible diff ratio","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T4BS","index":14,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 13000 kg on all types of road surfaces with up to 80% off road usage."]
["T4 B Single Wheel","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Light Truck 4X4 >7000<=13000KG GVM (Single wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"11m Live line Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"16.5m Non insulated Aerial platform"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"18m Non insulated Aerial platform"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Cargo van body"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Crew cab"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Ladder Rack"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," “H” Frame"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Tool Boxes"]
["VEHICLE CONFIGURATION :","Light Truck 4X4 >7000<=13000KG GVM (Single wheel application)",{"$nulls":4},"Stainless steel Water Tank"]
["TRACTION: ","4x4",{"$nulls":4},"Working Lights"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4}," Amber Revolving Light"]
["Power Rating - Kw","150Kw",{"$nulls":4},"Tow bar"]
["Torque Rating - NM","600Nm",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Permissible Front axle rating “ Max.”","4500kg",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Rear axle rating “ Max.”","9000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["D/T Rating “Min.”","20000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4600mm and 4800mm ",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Chassis to facilitate the fitting of 10Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 10.00 R 20(up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T5AD","index":15,"n_rows":46,"n_cols":7,"rows_kept":46,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 16000 kg on all types of road surfaces with up to 80% off road usage."]
["T5AD \nDual wheel\n ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Medium Truck 4x4 >13000 <16000 GVM (Dual wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"16 Tm & 14.3m Horisontal &  735kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["DRIVER AND PASSENGER AIRBAGS","Specify"]
["ABS BRAKES","To be Standard",{"$nulls":4},"11 m Live line Aerial platform"]
["POWER STEERING","To be Standard",{"$nulls":4},"16.5 m Non insulated Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Auger drill"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["PTO Suitable for a 15Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Cargo van body"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Crew cab"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Ladder Rack"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4}," “H” Frame"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Tool Boxes"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["VEHICLE CONFIGURATION :","Medium Truck 4x4 >13000 <16000 GVM (Dual wheel application)",{"$nulls":4},"Working Lights"]
["TRACTION: ","4x4",{"$nulls":4}," Amber Revolving Light"]
["ATTACHED TECHNICAL SPECS BROCHURES FOR VERIFICATION","Specify"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Tow bar"]
["Power Rating - Kw","125Kw",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Torque Rating - NM","660Nm",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Front axle rating “ Max.”","6000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Rear axle rating “ Max.”","9000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","15000 to 21000kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4500mm and 4800mm "]
["Chassis to facilitate the fitting of 13Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11 R 22.5. (up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"T5AS","index":16,"n_rows":46,"n_cols":7,"rows_kept":46,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 16000 kg on all types of road surfaces with up to 80% off road usage."]
["T5AS \nSingle wheel\n ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Medium Truck 4x4 >13000 <16000 GVM (Single wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"16 Tm & 14.3m Horisontal &  735kg"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER AIRBAGS","Specify"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"11 m Live line Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"16.5 m Non insulated Aerial platform"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Auger drill"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["PTO Suitable for a 15Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Cargo van body"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Crew cab"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Ladder Rack"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4}," “H” Frame"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Tool Boxes"]
["VEHICLE CONFIGURATION :","Medium Truck 4x4 >13000 <16000 GVM (Single wheel application)",{"$nulls":4},"Stainless steel Water Tank"]
["TRACTION: ","4x4",{"$nulls":4},"Working Lights"]
["ATTACHED TECHNICAL SPECS BROCHURES FOR VERIFICATION","Specify"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4}," Amber Revolving Light"]
["Power Rating - Kw","125Kw",{"$nulls":4},"Tow bar"]
["Torque Rating - NM","660Nm",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Permissible Front axle rating “ Max.”","6000kg",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Rear axle rating “ Max.”","8000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["D/T Rating “Min.”","15000 to 21000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4500mm and 4800mm ",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Chassis to facilitate the fitting of 10Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 12R20.00 (up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"T5BD","index":17,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[3,1,3,4],[4,2,4,3],[50,0,50,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 19000 kg on all types of road surfaces with up to 80% off road usage.."]
["T5BD \nDual wheel\n ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Medium Truck 4x4 >16000 <19000GVM (Duel wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"18 Tm & 21m Horisontal & 500Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"17 Tm & 14.3m Horisontal &  735kg"]
["DRIVER AND PASSENGER AIRBAGS","Specify"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Hour meter"]
["POWER STEERING","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"16.5m Live line Aerial platform"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"18m Non insulated Aerial platform"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"900 CFM compressor"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Auger drill"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"PTO"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Cargo van body"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Crew cab"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Ladder Rack"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4}," “H” Frame"]
["VEHICLE CONFIGURATION :","Medium Truck 4x4 >16000 <19000GVM (Duel wheel application)",{"$nulls":4},"Tool Boxes"]
["TRACTION: ","4x4",{"$nulls":4},"Stainless steel Water Tank"]
["ATTACHED TECHNICAL SPECS BROCHURES FOR VERIFICATION","Specify"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Working Lights"]
["Power Rating - Kw","160Kw","176kW MAN",{"$nulls":3}," Amber Revolving Light"]
["Torque Rating - NM","850Nm","925Nm MAN",{"$nulls":3},"Tow bar"]
["Permissible Front axle rating “ Max.”","7500kg",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Permissible Rear axle rating “ Max.”","9000kg",{"$nulls":4},"Winch type spare wheel carrier "]
["D/T Rating “Min.”","21000Kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Wheel base “ Max.”","4500mm and 4800mm ",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Chassis to facilitate the fitting of 13Tm hydraulic crane ","YES",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Fully synchromesh Gearbox","YES"]
["Independent transfer box (4x4)","YES"]
["Gear ratio: Top gear 1:1 ","YES"]
["Gear ratio: Lowest gear higher than 8:1","YES"]
["Top speed of  vehicle max 100kmph (determine by gear ratio, no electronic speed limiters allowed)","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11 R 22.5. (up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"T5BS","index":18,"n_rows":55,"n_cols":7,"rows_kept":55,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[48,0,48,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 19000 kg on all types of road surfaces with up to 80% off road usage.."]
["T5BS \nSingle Wheel\n ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Medium Truck 4x4 >16000 <19000GVM (Single Wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"17 Tm & 14.3m Horisontal &  735kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["ABS BRAKES","To be Standard",{"$nulls":4},"16.5m Live line Aerial platform"]
["POWER STEERING","To be Standard",{"$nulls":4},"900 CFM compressor"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Auger drill"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Tail lift 1.5 Ton capacity"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Cargo van body"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Crew cab"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Ladder Rack"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," “H” Frame"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Tool Boxes"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Working Lights"]
["VEHICLE CONFIGURATION :","Medium Truck 4x4 >16000 <19000GVM (Single Wheel application)",{"$nulls":4}," Amber Revolving Light"]
["TRACTION: ","4x4",{"$nulls":4},"Tow bar"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Power Rating - Kw","160Kw",{"$nulls":4},"Winch type spare wheel carrier "]
["Torque Rating - NM","850Nm",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Front axle rating “ Max.”","7500kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","8000kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","21000Kg"]
["Wheel base “Min and Max.”","4500mm and 4800mm "]
["Chassis to facilitate the fitting of 15Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Independent transfer box (4x4)","YES"]
["Gear ratio: Top gear 1:1 ","YES"]
["Gear ratio: Lowest gear higher than 8:1","YES"]
["Top speed of  vehicle max 100kmph (determine by gear ratio, no electronic speed limiters allowed)","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 1400R20 Steel radial Tyres (Michelin XZL)  (up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T6","index":19,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Goods, equipment and passengers up to a GVM of 26000 kg on all types of road surfaces with up to 40% off road usage"]
["T6","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Heavy Truck 6x4 >17000 <26000 GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horisontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horisontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Tail lift 3 Ton capacity"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"PTO"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Cargo van body"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Ladder Rack"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4}," “H” Frame"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Tool Boxes"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Working Lights"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["VEHICLE CONFIGURATION :","Heavy Truck 6x4 >17000 <26000 GVM",{"$nulls":4},"Tow bar"]
["TRACTION: ","6x4",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Winch type spare wheel carrier "]
["Power Rating - Kw","190Kw",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Torque Rating - NM","1000Nm",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Front axle rating “ Max.”","6300kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","30000kg to 60000Kg"]
["Wheel base (Center front axle to center of rear axle unit) (Min)","5000mm"]
["Chassis to facilitate the fitting of 18Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00X20 or equivalent","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T7","index":20,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","Required tocarrying Goods, equipment and passengers of 26000 kg GVM and above on all types of road surfaces with up to 40% off road usage"]
["T7","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Heavy Truck 6x4 >26000 GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horisontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horisontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER AIRBAGS","To be Standard"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Tail lift 3 Ton capacity"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"PTO"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Cargo van body"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Crew cab"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Ladder Rack"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4}," “H” Frame"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Tool Boxes"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Working Lights"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["VEHICLE CONFIGURATION :","Heavy Truck 6x4 > 26000 GVM",{"$nulls":4},"Tow bar"]
["TRACTION: ","6x4",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Winch type spare wheel carrier "]
["Power Rating - Kw","220Kw",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Torque Rating - NM","1000Nm",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Permissible Front axle rating “ Max.”","7500kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","65000Kg"]
["Wheel base (Center front axle to center of rear axle unit) (Min)","5100mm"]
["Chassis to facilitate the fitting of 22Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00X20 or equivalent","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T8T","index":21,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to carrying Tipper body and passengers up to a GVM of 15000 kg on all types of road surfaces with up to 60% off road usage. "]
["T8T\n ","Annexure A3","Tendering Service Provider to compleate",null,"Eskom technical team to compleate"]
["Vehicle Type Required:","Tipper Truck 4x2 15000Kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Hour meter"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"PTO"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Tipper load body"]
["POWER STEERING","To be Standard",{"$nulls":4},"Tool Boxes"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Working Lights"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Tow bar"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["VEHICLE CONFIGURATION :","Tipper Truck 4x2 15000Kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","280 Kw"]
["Torque Rating - NM","1400Nm"]
["Permissible Front axle rating “ Max.”","6000kg"]
["Permissible Rear axle rating “ Max.”","9000kg"]
["D/T Rating “Min.”","18000Kg"]
["Wheel base “ Max.”","3800mm"]
["Chassis to facilitate the Tipper body  ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00 X 20","specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T8","index":22,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to draw a trailer up to 41000kg and passengers on all types of road surfaces with up to 60% off road usage. "]
["T8\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Truck Tractor 4x2 >17000Kg <41000Kg GCM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"16 Tm and 14.3 Metre horizontal reach"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["ABS BRAKES","To be Standard",{"$nulls":4},"PTO"]
["POWER STEERING","To be Standard",{"$nulls":4},"Fifth wheel "]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Tool Boxes"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Working Lights"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Tow bar"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["VEHICLE CONFIGURATION :","Truck Tractor 4x2 >17000Kg <41000Kg GCM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","250Kw"]
["Torque Rating - NM","1400Nm"]
["Permissible Front axle rating “ Max.”","7000kg"]
["Permissible Rear axle rating “ Max.”","9000kg"]
["D/T Rating “Min.”","41000Kg"]
["Wheel base “ Max.”","3800mm"]
["Chassis to facilitate the fitting of 14Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00 X 20","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T9","index":23,"n_rows":50,"n_cols":7,"rows_kept":50,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[43,0,43,4]]}
[]
[]
[]
["Vehicle Job Description:","Required to for carrying Goods & equipment of up to 75000 kg GCM on all types of road surfaces short & long distance "]
["T9\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Truck Tractor 6x4 >28000 <75000 GCM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"17 Tm & 14.3m Horizontal &  735kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["ABS BRAKES","To be Standard",{"$nulls":4},"PTO"]
["POWER STEERING","To be Standard",{"$nulls":4},"Fifth wheel "]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Tool Boxes"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Working Lights"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Tow bar"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["VEHICLE CONFIGURATION :","Track tractor"]
["TRACTION: ","6x4"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","330Kw"]
["Torque Rating - NM","2200Nm"]
["Permissible Front axle rating “ Max.”","7500kg"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","75000Kg"]
["Wheel base “ Max.”","4800mm"]
["Chassis to facilitate the fitting of 17Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 11.00 X 20","specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T10","index":24,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","ABNORMAL Truck Tractor To handle a Trailer of >85000Kg <100000Kg (Mobile Substation)"]
["T10\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Abnormal Truck Tractor 6x4 >85000 GCM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"Hour meter"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"PTO"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Fifth wheel "]
["POWER STEERING","To be Standard",{"$nulls":4},"Tool Boxes"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Working Lights"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Tow bar"]
["PTO (PRICE FITTED IF NOT STD)","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["VEHICLE CONFIGURATION :","Track tractor"]
["TRACTION: ","6x4"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","350 Kw"]
["Torque Rating - NM","2300 Nm"]
["Permissible Front axle rating “ Max.”","7700 kg"]
["Permissible Rear axle rating “ Max.”","18000 kg"]
["D/T Rating “Min.”","90000 Kg"]
["Wheel base “ Max.”","3875 mm"]
["Chassis to facilitate the fitting of 18Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Vehicle to be able to pull a trailer of at least 85000 tons to 100000 tons","YES"]
["Tyres (Size) 11.00 X 20","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T11","index":25,"n_rows":47,"n_cols":7,"rows_kept":47,"merged":[[3,1,3,4],[4,2,4,3],[46,0,46,4]]}
[]
[]
[]
["Vehicle Job Description:","Required for carrying Goods, equipment and passengers of 42000 kg GVM and above on all types of road surfaces with up to 40% off road usage"]
["T11\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Heavy Truck 6x6 42000 GCM (Single Wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horisontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horisontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["DRIVER AND PASSENGER AIRBAGS","Specify"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"28m Live line Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"30m Non insulated Telescopic Aerial platform"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tail lift 3 Ton capacity"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)FROM 4525mm 6000MM","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Cargo van body"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Crew cab"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Ladder Rack"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4}," “H” Frame"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Tool Boxes"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["VEHICLE CONFIGURATION :","Heavy Truck 6x6 42000 GCM (Single Wheel application)",{"$nulls":4},"Working Lights"]
["TRACTION: ","6x6",{"$nulls":4}," Amber Revolving Light"]
["ATTACHED TECHNICAL SPECS BROCHURES FOR VERIFICATION","Specify"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Tow bar"]
["Power Rating - Kw","300Kw",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Torque Rating - NM","1500Nm",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Front axle rating “ Max.”","8000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Rear axle rating “ Max.”","26000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","42000Kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4525mm"]
["Chassis to facilitate the fitting of 22Tm hydraulic crane ","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 1400R20 Steel radial Tyres  (up to 80% off road usage) Compatible diff ratio","Specify"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"T12","index":26,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","Required for carrying equipment of up to 36000 kg GCM on all types of road surfaces short & long distance with an 80% off road (Tipper chassis or concrete mixer chassis)"]
["T12\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Heavy Truck 6x4 36000 GCM (Single Wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horisontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horisontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"HHH DTH Drill"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"HHH DTH Drill and 900 CFM compressor"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"Waste removal compactor"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tipper load body"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"Tool Boxes"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Working Lights"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Tow bar"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["REVERSE LIGHTS","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["VEHICLE CONFIGURATION :","Truck 6x4 >36000 kg GVM Construction vehicle (Tipper chassis or concrete mixer chassis) long wheel base",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["TRACTION: ","6x4",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","350Kw"]
["Torque Rating - NM","1700Nm"]
["Permissible Front axle rating “ Max.”","7100kg"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","33000Kg"]
["Wheel base Centre of front acsle to centre of front rear tyre  “ Max.”","4600 mm"]
["Chassis to facilitate the fitting of 10 cubik tipper body","YES"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 315/80R22.5 with an 80% off road","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T13D","index":27,"n_rows":52,"n_cols":7,"rows_kept":52,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[45,0,45,4]]}
[]
[]
[]
["Vehicle Job Description:","Required for carrying Goods & equipment of up to 28000 kg GVM on all types of road surfaces short & long distance with an 80% off road (Tipper / Concrete Chassis) "]
["T13D","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Truck 8x8 Construction vehicle >28000 kg GVM (Tipper chassis or concrete mixer chassis)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horizontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horizontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Up to 60m Live line Telescopic Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Wheel base extension"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Working Lights"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)FROM 4600mm 6000MM","To be Standard",{"$nulls":4},"Tow bar"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["REVERSE LIGHTS","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["VEHICLE CONFIGURATION :","Truck 8x8 >28000 kg GVM Construction vehicle (Tipper chassis or concrete mixer chassis)"]
["TRACTION: ","8x8"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","360Kw"]
["Torque Rating - NM","1700Nm"]
["Permissible Front axle rating “ Max.”","7100kg"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","33000Kg"]
["Wheel base “ Max.”","4600 mm"]
["Chassis to facilitate the fitting of a hydraulic Truck mounted crane ","up to a 32Tm crane"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 315/80R22.5 with an 80% off road","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T13S","index":28,"n_rows":53,"n_cols":7,"rows_kept":53,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[46,0,46,4]]}
[]
[]
[]
["Vehicle Job Description:","Required for carrying Goods & equipment of up to 28000 kg GVM on all types of road surfaces short & long distance with an 80% off road (Tipper / Concrete Chassis) "]
["T13S\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Truck 8x8 Construction vehicle >28000 kg GVM (Tipper chassis or concrete mixer chassis) Single wheel application","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horizontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horizontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"Up to 60m Live line Telescopic Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"Wheel base extension"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Working Lights"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4}," Amber Revolving Light"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)FROM 4600mm 6000MM","To be Standard",{"$nulls":4},"Tow bar"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Winch type spare wheel carrier "]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["REVERSE LIGHTS","To be Standard"]
["Chassis to facilitate the fitting of 22Tm hydraulic crane ","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["VEHICLE CONFIGURATION :","Truck 8x8 Construction vehicle >28000 kg GVM (Tipper chassis or concrete mixer chassis) Single wheel application"]
["TRACTION: ","8x8"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","360Kw"]
["Torque Rating - NM","1700Nm"]
["Permissible Front axle rating “ Max.”","7100kg"]
["Permissible Rear axle rating “ Max.”","18000kg"]
["D/T Rating “Min.”","33000Kg"]
["Wheel base “ Max.”","4600 mm"]
["Chassis to facilitate the fitting of a hydraulic Truck mounted crane ","up to a 32Tm crane"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 315/80R22.5 with an 80% off road","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"T14S AUTOMATIC","index":29,"n_rows":51,"n_cols":7,"rows_kept":51,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[44,0,44,4]]}
[]
[]
[]
["Vehicle Job Description:","Required for carrying Goods, equipment and passengers of 26000 kg GVM and above on all types of road surfaces with up to 40% off road usage"]
["T14S AUTOMATIC\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Heavy Truck 6x6 26000 GCM (Single Wheel application) AUTOMATIC","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD)","To be Standard",{"$nulls":4},"23 Tm & 21m Horisontal & 650Kg"]
["Seat Belts: SABS APPROVED","To be Standard",{"$nulls":4},"32 Tm & 20m Horisontal & 880Kg "]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Hour meter"]
["ABS BRAKES","To be Standard",{"$nulls":4},"Inter lock hand brake system"]
["POWER STEERING","To be Standard",{"$nulls":4},"28m Live line Aerial platform"]
["DAY RUN LIGHTS INSTALLED","To be Standard",{"$nulls":4},"30m Non insulated Telescopic Aerial platform"]
["TWO EMMERGENCY TRIANGLES","To be Standard",{"$nulls":4},"HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)"]
["IMMOBILISER (Factory Warranty)","To be Standard",{"$nulls":4},"Tail lift 3 Ton capacity"]
["ALARM (Factory Warranty)","To be Standard",{"$nulls":4},"PTO"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)FROM 4525mm 6000MM","To be Standard",{"$nulls":4},"Flat Bed Drop side"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ","To be Standard",{"$nulls":4},"Cargo van body"]
["ENGINE PROTECTION DEVICE ","To be Standard",{"$nulls":4},"Crew cab"]
["TRAILER BRAKE CONTROL","To be Standard",{"$nulls":4},"Ladder Rack"]
["AIR CHARGE LINE TO THE FRONT","To be Standard",{"$nulls":4}," “H” Frame"]
["REVERSE ALARM/BEEPER","To be Standard",{"$nulls":4},"Tool Boxes"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard",{"$nulls":4},"Stainless steel Water Tank"]
["VEHICLE CONFIGURATION :","Heavy Truck 6x6 42000 GCM (Single Wheel application)",{"$nulls":4},"Working Lights"]
["TRACTION: ","6x6",{"$nulls":4}," Amber Revolving Light"]
["Diesel Powered (Normally aspirated or Turbo)","YES",{"$nulls":4},"Tow bar"]
["Power Rating - Kw","309 Kw",{"$nulls":4},"Under run bumper fixed or energy absorbing type "]
["Torque Rating - NM","1900Nm",{"$nulls":4},"Winch type spare wheel carrier "]
["Permissible Front axle rating “ Max.”","8000kg",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Permissible Rear axle rating “ Max.”","26000kg",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["D/T Rating “Min.”","42000Kg",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["Wheel base “ Max.”","4525mm"]
["Chassis to facilitate the fitting of 22Tm hydraulic crane ","YES"]
["Automatic transmition, 'Triptronic transmition'","YES"]
["Power assisted Steering","YES"]
["Seat Belts: SABS approved","YES"]
["Tyres (Size) 1400R20 Steel radial Tyres (Michelin XZL)  (up to 80% off road usage) Compatible diff ratio","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"Permitted Ancillaries","index":30,"n_rows":26,"n_cols":32,"rows_kept":26,"hidden":true}
["PV1","PV2","PV3","PV4","T1A DC","T1A ","T1B","T1C","T2","T3","T4AD","T4AS","T4AD DC","T4BD","T4BS","T5AD","T5AS","T5BD","T5BS","T6","T7","T8T","T9","T10","T11","T12","T13D","T13S","25 Seater Bus"]
["Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries","Permitted Ancillaries"]
["Tow bar","Tow bar","Tow bar","Tow bar","Tow bar","Tow bar","Tow bar","Tow bar","Tow bar","11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M","6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M","6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M","6 Ton Crane 7.5M Horizontal, 10.5M Vertical Reach and 720Kg & 7.5M","11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M","11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M","16 Tm & 14.3m Horisontal &  735kg","16 Tm & 14.3m Horisontal &  735kg","18 Tm & 21m Horisontal & 500Kg ","17 Tm & 14.3m Horisontal &  735kg","23 Tm & 21m Horisontal & 650Kg","23 Tm & 21m Horisontal & 650Kg","16 Tm and 14.3 Metre horizontal reach","17 Tm & 14.3m Horizontal &  735kg","Hour meter","23 Tm & 21m Horisontal & 650Kg","23 Tm & 21m Horisontal & 650Kg","23 Tm & 21m Horizontal & 650Kg","23 Tm & 21m Horizontal & 650Kg","Wheel chair compatible","Wheel chair compatible","Wheel chair compatible","Wheel chair compatible"]
["Tool Boxes","Tool Boxes","Tool Boxes","Tool Boxes","Flat Bed Drop side","PTO","PTO","PTO","PTO","13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M","Hour meter","Hour meter","Hour meter","13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M","13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M","Hour meter","Hour meter","17 Tm & 14.3m Horizontal &  735kg","Hour meter","32 Tm & 20m Horizontal & 880Kg ","32 Tm & 20m Horizontal & 880Kg ","Hour meter","Hour meter","Inter lock hand brake system","32 Tm & 20m Horisontal & 880Kg ","32 Tm & 20m Horisontal & 880Kg ","32 Tm & 20m Horizontal & 880Kg ","32 Tm & 20m Horizontal & 880Kg ","Wheel chair access","Wheel chair access","Wheel chair access","Wheel chair access"]
["Fog Lights","Fog Lights","Fog Lights","Fog Lights","Cargo van body","Hour meter","Hour meter","Hour meter","11 Ton Crane 8.1M Horizontal, 11.5M Vertical Reach and 1350Kg & 8M","14 Ton Crane 14M Horizontal, 17.5 Vertical Reach and 530Kg & 14.2M","Inter lock hand brake system","Inter lock hand brake system","Inter lock hand brake system","Hour meter","Hour meter","Inter lock hand brake system","Inter lock hand brake system","Hour meter","Inter lock hand brake system","Hour meter","Hour meter","Inter lock hand brake system","Inter lock hand brake system","PTO","Hour meter","Hour meter","Hour meter","Hour meter","Spill kit","Spill kit","Spill kit","Spill kit"]
["Amber Revolving Light","Amber Revolving Light","Amber Revolving Light","Amber Revolving Light","Tool cab","Inter lock hand brake system","Inter lock hand brake system","Inter lock hand brake system","13 Ton Crane 10.2M Horizontal, 13.5 Vertical Reach and 950Kg & 10.2M","15 Ton Crane 14.35M Horizontal, 16 Vertical Reach and 650Kg & 14.35M","Tail lift 1.5 Ton capacity","Tail lift 1.5 Ton capacity","Tail lift 1.5 Ton capacity","Inter lock hand brake system","Inter lock hand brake system","11 m Live line Aerial platform","11 m Live line Aerial platform","Inter lock hand brake system","16.5m Live line Aerial platform","Inter lock hand brake system","Inter lock hand brake system","PTO","PTO","Fifth wheel ","Inter lock hand brake system","Inter lock hand brake system","Inter lock hand brake system","Inter lock hand brake system"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["Driving lights","Driving lights","Driving lights","Driving lights","Ladder Rack","Flat Bed Drop side","Flat Bed Drop side","Flat Bed Drop side","14 Ton Crane 14M Horizontal, 17.5 Vertical Reach and 530Kg & 14.2M","15 Ton Crane 12M Horizontal, 16 Vertical Reach and 650Kg & 14.35M","PTO","PTO","PTO","Tail lift 1.5 Ton capacity","11m Live line Aerial platform","16.5 m Non insulated Aerial platform","16.5 m Non insulated Aerial platform","16.5m Live line Aerial platform","900 CFM compressor","Tail lift 3 Ton capacity","Tail lift 3 Ton capacity","Fifth wheel ","Fifth wheel ","Tool Boxes","28m Live line Aerial platform","HHH DTH Drill","Up to 60m Live line Telescopic Aerial platform","Up to 60m Live line Telescopic Aerial platform","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["Reverse alarm / beeper","Reverse alarm / beeper","Reverse alarm / beeper","Reverse alarm / beeper","“H” Frame","Cargo van body","Cargo van body","Cargo van body","Hour meter","Inter lock hand brake system","Flat Bed Drop side","Flat Bed Drop side","Flat Bed Drop side","PTO","16.5m Live line Aerial platform","Auger drill","Auger drill","18m Non insulated Aerial platform","Auger drill","PTO","PTO","Tool Boxes","Tool Boxes","Stainless steel Water Tank","30m Non insulated Telescopic Aerial platform","Waste removal compactor","Wheel base extension","Wheel base extension","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":4},"Tool Boxes","Tool cab","Ladder Rack","Tool cab","Inter lock hand brake system","Hour meter","Cargo van body","Cargo van body","Cargo van body","Flat Bed Drop side","18m Non insulated Aerial platform","Tail lift 1.5 Ton capacity","Tail lift 1.5 Ton capacity","900 CFM compressor","Tail lift 1.5 Ton capacity","Flat Bed Drop side","Flat Bed Drop side","Stainless steel Water Tank","Stainless steel Water Tank","Working Lights","HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)","Tool Boxes","HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)","HHH DTH Drill and 900 CFM compressor (HHH DTH OBC)"]
[{"$nulls":4},"Stainless steel Water Tank","Ladder Rack","“H” Frame","Ladder Rack","Flat Bed Drop side","Tail lift 2 ton capacity","Crew cab","Crew cab","Crew cab","Cargo van body","Tail lift 1.5 Ton capacity","PTO","PTO","Auger drill","PTO","Cargo van body","Cargo van body","Working Lights","Working Lights"," Amber Revolving Light","Tail lift 3 Ton capacity","Stainless steel Water Tank","Working Lights","Working Lights"]
[{"$nulls":4},"Fog Lights","“H” Frame","Tool Boxes","“H” Frame","Cargo van body","PTO","Ladder Rack","Ladder Rack","Ladder Rack","Crew cab","PTO","Flat Bed Drop side","Flat Bed Drop side","Tail lift 1.5 Ton capacity","Flat Bed Drop side","Crew cab","Crew cab"," Amber Revolving Light"," Amber Revolving Light","Tow bar","PTO","Working Lights"," Amber Revolving Light"," Amber Revolving Light"]
[{"$nulls":4},"Working Lights","Tool Boxes","Stainless steel Water Tank","Tool Boxes","Tool cab","Flat Bed Drop side"," “H” Frame"," “H” Frame"," “H” Frame","Ladder Rack","Flat Bed Drop side","Cargo van body","Cargo van body","PTO","Cargo van body","Ladder Rack","Ladder Rack","Tow bar","Tow bar","Under run bumper fixed or energy absorbing type ","Flat Bed Drop side"," Amber Revolving Light","Tow bar","Tow bar"]
[{"$nulls":4},"Amber Revolving Light","Stainless steel Water Tank","Fog Lights","Stainless steel Water Tank","Ladder Rack","Cargo van body","Tool Boxes","Tool Boxes","Tool Boxes"," “H” Frame","Cargo van body","Crew cab","Crew cab","Flat Bed Drop side","Crew cab"," “H” Frame"," “H” Frame","Under run bumper fixed or energy absorbing type ","Under run bumper fixed or energy absorbing type "," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Cargo van body","Tow bar","Under run bumper fixed or energy absorbing type ","Under run bumper fixed or energy absorbing type "]
[{"$nulls":4},"Under run bumper fixed or energy absorbing type ","Fog Lights","Working Lights","Fog Lights","“H” Frame","Crew cab","Stainless steel Water Tank","Stainless steel Water Tank","Stainless steel Water Tank","Tool Boxes","Crew cab","Ladder Rack","Ladder Rack","Cargo van body","Ladder Rack","Tool Boxes","Tool Boxes"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Crew cab","Under run bumper fixed or energy absorbing type "," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
[{"$nulls":4},"Wheel Flaps:  SABS 1496 specification (Jan 1999)","Working Lights","Amber Revolving Light","Working Lights","Tool Boxes","Ladder Rack","Working Lights","Working Lights","Working Lights","Stainless steel Water Tank","Ladder Rack"," “H” Frame"," “H” Frame","Crew cab"," “H” Frame","Stainless steel Water Tank","Stainless steel Water Tank","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Ladder Rack"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Amber Revolving Light","Under run bumper fixed or energy absorbing type ","Amber Revolving Light","Stainless steel Water Tank"," “H” Frame"," Amber Revolving Light"," Amber Revolving Light"," Amber Revolving Light","Working Lights"," “H” Frame","Tool Boxes","Tool Boxes","Ladder Rack","Tool Boxes","Working Lights","Working Lights","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)",null," “H” Frame","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Under run bumper fixed or energy absorbing type ","Reverse alarm / beeper","Under run bumper fixed or energy absorbing type ","Fog Lights","Tool Boxes","9.2m live line Aerial platform","9.2m live line Aerial platform","9.2m live line Aerial platform"," Amber Revolving Light","Tool Boxes","Stainless steel Water Tank","Stainless steel Water Tank"," “H” Frame","Stainless steel Water Tank"," Amber Revolving Light"," Amber Revolving Light",{"$nulls":3},"Tool Boxes","Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":5},"Wheel Flaps:  SABS 1496 specification (Jan 1999)","Wheel Flaps:  SABS 1496 specification (Jan 1999)","Wheel Flaps:  SABS 1496 specification (Jan 1999)","Working Lights","Stainless steel Water Tank","11m Live line Aerial platform","11m Non insulated Aerial platform","11m Live line Aerial platform","11m Live line Aerial platform","Stainless steel Water Tank","Working Lights","Working Lights","Tool Boxes","Working Lights","Tow bar","Tow bar",{"$nulls":3},"Stainless steel Water Tank"]
[{"$nulls":5},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Amber Revolving Light","Working Lights","11m Non insulated Aerial platform","Tow bar","11m Non insulated Aerial platform","16.5m Live line Aerial platform","Working Lights"," Amber Revolving Light"," Amber Revolving Light","Stainless steel Water Tank"," Amber Revolving Light","Under run bumper fixed or energy absorbing type ","Under run bumper fixed or energy absorbing type ",{"$nulls":3},"Working Lights"]
[{"$nulls":5},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Under run bumper fixed or energy absorbing type ","Amber Revolving Light","Tow bar","Under run bumper fixed or energy absorbing type ","Tow bar","18m Non insulated Aerial platform"," Amber Revolving Light","Tow bar","Tow bar","Working Lights","Tow bar"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)",{"$nulls":3}," Amber Revolving Light"]
[{"$nulls":8},"Wheel Flaps:  SABS 1496 specification (Jan 1999)","Tow bar","Under run bumper fixed or energy absorbing type "," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Under run bumper fixed or energy absorbing type ","Tow bar","Tow bar","Under run bumper fixed or energy absorbing type ","Under run bumper fixed or energy absorbing type "," Amber Revolving Light","Under run bumper fixed or energy absorbing type ","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)",{"$nulls":3},"Tow bar"]
[{"$nulls":8},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Under run bumper fixed or energy absorbing type "," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Under run bumper fixed or energy absorbing type ","Under run bumper fixed or energy absorbing type "," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Tow bar"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)",{"$nulls":3},"Under run bumper fixed or energy absorbing type "]
[{"$nulls":8},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Wheel Flaps:  SABS 1496 specification (Jan 1999)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Under run bumper fixed or energy absorbing type ","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)",{"$nulls":5}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
[{"$nulls":9},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)",null,"Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)"," Wheel Flaps:  SABS 1496 specification (Jan 1999)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)",{"$nulls":5},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":9},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)",{"$nulls":3},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)","Homologation of load body according to (Road traffic Act and Regulations No. 192A)",null,null,"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)",{"$nulls":6},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
[{"$nulls":17},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]

{"sheet":"25 Seater Bus","index":31,"n_rows":56,"n_cols":7,"rows_kept":56,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[49,0,49,4]]}
[]
[]
[]
["Vehicle Job Description:","Semi luxury bus required to carrying 25 passengers and Goods up to a GVM of 7000 kg on all types of road surfaces with up to 40% off road usage"]
["B25S","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Bus 25 Seater 4x2 >6500 <7500kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and passengers","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD) With additional speakers for bus","To be Standard",{"$nulls":4},"Wheel chair compatible"]
["DRIVER AIRBAGS","To be Standard",{"$nulls":4},"Wheel chair access"]
["DRIVER SEAT TO BE ADJUSTABLE ","To be Standard",{"$nulls":4},"Spill kit"]
["A PARTITION IMMEDIATELY BEHIND THE DRIVER SEAT","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["DRIVER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["All SEATS MUST BE COVERES IN SOFT CLOTH AND NOT VINYL MATERIAL","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["3 POINT SEAT BELTS ON ALL SEATS","To be Standard"]
["EMERGENCY EXITS (REGULATION 252)","To be Standard"]
["FIRE EXTINGUISHERS (REGULATION 260)","To be Standard"]
["ABS BRAKES","To be Standard"]
["POWER STEERING","To be Standard"]
["DAY RUN LIGHTS INSTALLED","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["ENGINE PROTECTION DEVICE ","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["THE BUS MUST COMPLY TO ALL ROAD TRAFFIC & ROAD TRANSPORT LEGISLATION","To be Standard"]
["STEPS MUST HAVE ANTI-SLIP TREADS","To be Standard"]
["VEHICLE MUST BE FITTED WITH A REVERSE ALARM BEEPER","To be Standard"]
["NON-SMOKING AND SAFETY BELT STICKERS MUST BE DISPLAYED IN BUS","To be Standard"]
["VEHICLE CONFIGURATION :","Bus 25 Seater 4x2 >6500 <7500kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","90Kw"]
["Torque Rating - NM","304Nm"]
["Permissible Front axle rating “ Max.”","3100kg"]
["Permissible Rear axle rating “ Max.”","5000 - 5500kg"]
["Approximate body / payload  ","4600 to 5067 kg"]
["D/T Rating “Min.”","9300 to 10300 Kg"]
["Wheel base “ Max.”","3800mm"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) 750R16 12PR","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"30 Seater Bus","index":32,"n_rows":57,"n_cols":7,"rows_kept":57,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[50,0,50,4]]}
[]
[]
[]
["Vehicle Job Description:","Semi luxury bus required to carrying required to carrying 30 passengers and Goods up to a GVM of 7000 kg on all types of road surfaces with up to 40% off road usage"]
["B30S","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Bus 30 Seater 4x2 >6500 <7500kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and passengers","To be Standard",{"$nulls":4},"Permitted Ancillaries"]
["RADIO/CD PRICE FITTED (IF NOT STD) With additional speakers for bus","To be Standard",{"$nulls":4},"Wheel chair compatible"]
["DRIVER AIRBAGS","To be Standard",{"$nulls":4},"Wheel chair access"]
["DRIVER SEAT TO BE ADJUSTABLE ","To be Standard",{"$nulls":4},"Spill kit"]
["A PARTITION IMMEDIATELY BEHIND THE DRIVER SEAT","To be Standard",{"$nulls":4}," Wheel Flaps:  SABS 1496 specification (Jan 1999)"]
["DRIVER SEATBELT REMINDER INDICATOR/ALARM","To be Standard",{"$nulls":4},"Yellow reflective tape that must be fitted (Road traffic Act and Regulations No. 192A)"]
["All SEATS MUST BE COVERES IN SOFT CLOTH AND NOT VINYL MATERIAL","To be Standard"]
["3 POINT SEAT BELTS ON ALL SEATS","To be Standard",{"$nulls":4},"Homologation of load body according to (Road traffic Act and Regulations No. 192A)"]
["EMERGENCY EXITS (REGULATION 252)","To be Standard"]
["FIRE EXTINGUISHERS (REGULATION 260)","To be Standard"]
["ABS BRAKES","To be Standard"]
["POWER STEERING","To be Standard"]
["DAY RUN LIGHTS INSTALLED","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["ENGINE PROTECTION DEVICE ","To be Standard"]
["Seat Belts: SABS APPROVED","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["STEPS MUST HAVE ANTI-SLIP TREADS","To be Standard"]
["VEHICLE MUST BE FITTED WITH A REVERSE ALARM BEEPER","To be Standard"]
["NON-SMOKING AND SAFETY BELT STICKERS MUST BE DISPLAYED IN BUS","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["THE BUS MUST COMPLY TO ALL ROAD TRAFFIC & ROAD TRANSPORT LEGISLATION","To be Standard"]
["VEHICLE CONFIGURATION :","Bus 30 Seater 4x2 >6500 <7500kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","90Kw"]
["Torque Rating - NM","304Nm"]
["Permissible Front axle rating “ Max.”","3100kg"]
["Permissible Rear axle rating “ Max.”","5000 - 5500kg"]
["Approximate body / payload  ","4600 to 5067 kg"]
["D/T Rating “Min.”","9300 to 10300 Kg"]
["Wheel base “ Max.”","3800mm"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) 750R16 12PR","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"Bus 45 Seater","index":33,"n_rows":55,"n_cols":5,"rows_kept":55,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[48,0,48,4]]}
[]
[]
[]
["Vehicle Job Description:","Semi luxury bus required to carrying required to carrying 45 passengers and Goods up to a GVM of 12000 kg on all types of road surfaces with up to 40% off road usage"]
["B30S","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Bus 45 Seater  4x2 > 7500 < 12000 kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and passengers","To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD) With additional speakers for bus","To be Standard"]
["DRIVER AIRBAGS","To be Standard"]
["DRIVER SEAT TO BE ADJUSTABLE ","To be Standard"]
["A PARTITION IMMEDIATELY BEHIND THE DRIVER SEAT","To be Standard"]
["DRIVER SEATBELT REMINDER INDICATOR/ALARM","To be Standard"]
["All SEATS MUST BE COVERES IN SOFT CLOTH AND NOT VINYL MATERIAL","To be Standard"]
["3 POINT SEAT BELTS ON ALL SEATS","To be Standard"]
["EMERGENCY EXITS (REGULATION 252)","To be Standard"]
["FIRE EXTINGUISHERS (REGULATION 260)","To be Standard"]
["ABS BRAKES","To be Standard"]
["POWER STEERING","To be Standard"]
["DAY RUN LIGHTS INSTALLED","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["ENGINE PROTECTION DEVICE ","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["STEPS MUST HAVE ANTI-SLIP TREADS","To be Standard"]
["VEHICLE MUST BE FITTED WITH A REVERSE ALARM BEEPER","To be Standard"]
["NON-SMOKING AND SAFETY BELT STICKERS MUST BE DISPLAYED IN BUS","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["THE BUS MUST COMPLY TO ALL ROAD TRAFFIC & ROAD TRANSPORT LEGISLATION","To be Standard"]
["VEHICLE CONFIGURATION :","Bus 45 Seater  4x2 > 7500 < 12000 kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","125Kw"]
["Torque Rating - NM","450Nm"]
["Permissible Front axle rating “ Max.”","4100 to 5500kg"]
["Permissible Rear axle rating “ Max.”","7000kg to 9000kg"]
["D/T Rating “Min.”","17000kg to 21000Kg"]
["Wheel base “ Max.”","4500mm and 4850mm "]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) 10.00R20 / 11.00X20 / 8.25R20 14PR","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"60 Seater Bus","index":34,"n_rows":55,"n_cols":5,"rows_kept":55,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[48,0,48,4]]}
[]
[]
[]
["Vehicle Job Description:","Semi luxury bus required to carrying required to carrying 60 passengers and Goods up to a GVM of 17000 kg on all types of road surfaces with up to 40% off road usage"]
["B30S","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Bus 60 Seater   4x2 >15000 <17000kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and passengers","To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD) With additional speakers for bus","To be Standard"]
["DRIVER AIRBAGS","To be Standard"]
["DRIVER SEAT TO BE ADJUSTABLE ","To be Standard"]
["A PARTITION IMMEDIATELY BEHIND THE DRIVER SEAT","To be Standard"]
["DRIVER SEATBELT REMINDER INDICATOR/ALARM","To be Standard"]
["All SEATS MUST BE COVERES IN SOFT CLOTH AND NOT VINYL MATERIAL","To be Standard"]
["3 POINT SEAT BELTS ON ALL SEATS","To be Standard"]
["EMERGENCY EXITS (REGULATION 252)","To be Standard"]
["FIRE EXTINGUISHERS (REGULATION 260)","To be Standard"]
["ABS BRAKES","To be Standard"]
["POWER STEERING","To be Standard"]
["DAY RUN LIGHTS INSTALLED","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["ENGINE PROTECTION DEVICE ","To be Standard"]
["REVERSE ALARM/BEEPER","To be Standard"]
["STEPS MUST HAVE ANTI-SLIP TREADS","To be Standard"]
["VEHICLE MUST BE FITTED WITH A REVERSE ALARM BEEPER","To be Standard"]
["NON-SMOKING AND SAFETY BELT STICKERS MUST BE DISPLAYED IN BUS","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["THE BUS MUST COMPLY TO ALL ROAD TRAFFIC & ROAD TRANSPORT LEGISLATION","To be Standard"]
["VEHICLE CONFIGURATION :","Bus 60 Seater   4x2 >15000 <17000kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","150Kw"]
["Torque Rating - NM","600Nm"]
["Permissible Front axle rating “ Max.”","6300kg"]
["Permissible Rear axle rating “ Max.”","9000kg"]
["D/T Rating “Min.”","20000kg"]
["Wheel base “ Max.”","5650mm"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) 11.00X20 or equivalent","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"65 Seater Bus","index":35,"n_rows":54,"n_cols":5,"rows_kept":54,"hidden":true,"merged":[[3,1,3,4],[4,2,4,3],[47,0,47,4]]}
[]
[]
[]
["Vehicle Job Description:","Semi luxury bus required to carrying required to carrying 65 passengers and Goods up to a GVM of 17000 kg on all types of road surfaces with up to 40% off road usage"]
["B30S","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Bus 65 Seater   4x2 >15000 <17000kg GVM","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty) for the bus and passengers","To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD) With additional speakers for bus","To be Standard"]
["DRIVER AIRBAGS","To be Standard"]
["DRIVER SEAT TO BE ADJUSTABLE ","To be Standard"]
["A PARTITION IMMEDIATELY BEHIND THE DRIVER SEAT","To be Standard"]
["DRIVER SEATBELT REMINDER INDICATOR/ALARM","To be Standard"]
["All SEATS MUST BE COVERES IN SOFT CLOTH AND NOT VINYL MATERIAL","To be Standard"]
["3 POINT SEAT BELTS ON ALL SEATS","To be Standard"]
["EMERGENCY EXITS (REGULATION 252)","To be Standard"]
["FIRE EXTINGUISHERS (REGULATION 260)","To be Standard"]
["ABS BRAKES","To be Standard"]
["POWER STEERING","To be Standard"]
["DAY RUN LIGHTS INSTALLED","To be Standard"]
["TWO EMMERGENCY TRIANGLES","To be Standard"]
["IMMOBILISER (Factory Warranty)","To be Standard"]
["ALARM (Factory Warranty)","To be Standard"]
["ENGINE PROTECTION DEVICE ","To be Standard"]
["STEPS MUST HAVE ANTI-SLIP TREADS","To be Standard"]
["VEHICLE MUST BE FITTED WITH A REVERSE ALARM BEEPER","To be Standard"]
["NON-SMOKING AND SAFETY BELT STICKERS MUST BE DISPLAYED IN BUS","To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard"]
["THE BUS MUST COMPLY TO ALL ROAD TRAFFIC & ROAD TRANSPORT LEGISLATION","To be Standard"]
["VEHICLE CONFIGURATION :","Bus 65 Seater   4x2 >15000 <17000kg GVM"]
["TRACTION: ","4x2"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Power Rating - Kw","150Kw"]
["Torque Rating - NM","600Nm"]
["Permissible Front axle rating “ Max.”","6300kg"]
["Permissible Rear axle rating “ Max.”","9000kg"]
["D/T Rating “Min.”","20000kg"]
["Wheel base “ Max.”","5650mm"]
["Fully synchromesh Gearbox","YES"]
["Power assisted Steering","YES"]
["Tyres (Size) 11.00X20 or equivalent","YES"]
["Number of gears, manual","YES"]
["Mud-flaps: Factory fitted","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","Specify"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or register dealer",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sails service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"Sheet10","index":36,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet11","index":37,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet12","index":38,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet13","index":39,"n_rows":0,"n_cols":0,"rows_kept":0}