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Annexure D
Technical Specification & Response Form
For
Display Technologies

















NOTE: The minimum specifications below are to be complied with in terms of hardware supply. The supply portion in the scope of works is related to the FIDS Display specification below. All other specifications below will be required as and when needed in terms of replacement of current display failures, or by ACSA’s discretion.


FIDS (Flight Information Display System) Specification
	Components
	Screen Type
	Comply\ Non-Comply
	Reference in Document

	Screen size
	40” 42” 46” 50” 55” 65” (2-inch tolerance accepted)
	
	

	Resolution
	1,920 x 1,080
	
	

	Type
	LED / LCD
	
	

	Mounting method
	Flush wall mount
	
	

	Additional Features
	
	
	

	Operation
	24 Hour Industrial Operation
	
	

	Clock On/Off Timer
	Yes
	
	

	HDMI
	Yes - 2 ports
	
	

	USB
	Yes - 2 ports
	
	

	Built in PC
	Yes
	
	

	Ethernet (LAN)
	Yes, network bootable (boot from LAN)
	
	

	Bezel Type
	Slim, maximum 10mm
	
	

	Front Colour
	Black
	
	

	Power Supply
	AC 220 - 240 V (50 / 60 Hz)
	
	

	Power Consumption (Stand-by)
	< 0.3 W
	
	

	Wall Mount Support
	Yes
	
	

	
Universal internal pc (slots into display, not bolt on) 

	Intel i5 processor
120 gig SSD
1 gig Ethernet adaptor (RJ45)
DDR 2 gig 
Video RAM 256MB
Video outputs DVI\VGA\HDMI
USB2 x 3
Wi-Fi enabled
Windows 10, 11 and Lynix capable
	
	

	Warranty
	
	
	

	Minimum
	3 YEARS ONSITE COMPREHENSIVE
	
	

	Minimum
	1 YEAR DEFECTS LIABILITY PERIOD
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