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TAD MAJOR SERVICE OF THE TRAIN CHILLER PLANT SERIAL NUMBER: U94L04757, MODEL NUMBER: RTHB380RLB00NW00TOUNN4LF2LF0000, WATER TREATMENT AND COOLING TOWERS.
	Numbering
	Description
	AMOUNT
	TOTAL

	1.
	Cleaning of condenser tubes
	
	

	2.
	Replacement of compressor discharge pipe gasket
	
	

	3.
	Check gas leaks
	
	

	4.
	Vacuum and recharging of R22 refrigerant 

	
	

	5.
	Replacement of oil with lip-seal

	
	

	6.
	 Replacement of refrigerant filters with lip-seal

	
	

	7.
	Test flow switch for both condenser and chilled line.
	
	

	8.
	Supply three circuit breakers (3-phase;80A)
	
	

	9.
	Supply three contactors (80A)
	
	

	10.
	Supply three overload protection (38A-50A) 
	
	

	11.
	Supply and install temperature control sensor
	
	

	12.
	Repair of water treatment dosing supply tank and automatic pump dosing
	
	

	13.
	Water treatment on both chilled and condenser pipes
	
	

	14.
	Cleaning of strainers on the condenser line and chilled line
	
	

	15.
	Install the standby pumps for chiller line and condenser line
	
	

	16.
	Cleaning of cooling towers and tower perks
	
	

	17.
	Repair, installation and commissioning of the cooling tower motor (7.5kW) X2
	
	

	18.
	Commissioning of the chiller after repairs
	
	

	19.
	Provide Test and Service report for water treatment
	
	

	20.
	Issue COC upon completion
	
	

	21.
	Provide proof of Qualified technician registered with SAQCC
	
	

	22.
	Total price EXCL.VAT
	
	

	23.
	VAT (15%) IF APPLICABLE
	
	

	24.
	Final grand total inclusive of VAT
	
	



NB: Site Visit Compulsory
Complete visitor’s forms for site access to be submitted on 13 June 2025 at 12h00PM
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