{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Building BOQ","Sheet1","Sheet2","Building BOQ (2)"],"not_rendered":{"external_links":1,"defined_names":18},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Building BOQ","index":0,"n_rows":4233,"n_cols":8,"rows_kept":4233,"merged":[[4,1,4,2],[6,1,6,2],[8,1,8,2],[10,1,10,2],[12,1,12,2],[14,1,14,2],[15,1,15,2],[18,1,18,2],[20,1,20,2],[22,1,22,2],[39,1,39,2],[43,1,43,2],[45,1,45,2],[51,1,51,2],[55,1,55,2],[57,1,57,2],[61,1,61,2],[63,1,63,2],[65,1,65,2],[69,1,69,2],[73,1,73,2],[76,1,76,2],[78,1,78,2],[80,1,80,2],[82,1,82,2],[95,1,95,2],[97,1,97,2],[99,1,99,2],[101,1,101,2],[105,1,105,2],[109,1,109,2],[113,1,113,2],[117,1,117,2],[121,1,121,2],[125,1,125,2],[129,1,129,2],[143,1,143,2],[145,1,145,2],[149,1,149,2],[153,1,153,2],[157,1,157,2],[161,1,161,2],[165,1,165,2],[169,1,169,2],[173,1,173,2],[177,1,177,2],[179,1,179,2],[181,1,181,2],[187,1,187,2],[191,1,191,2],[195,1,195,2],[199,1,199,2],[214,1,214,2],[216,1,216,2],[218,1,218,2],[220,1,220,2],[222,1,222,2],[224,1,224,2],[228,1,228,2],[230,1,230,2],[234,1,234,2],[236,1,236,2],[238,1,238,2],[240,1,240,2],[242,1,242,2],[244,1,244,2],[246,1,246,2],[248,1,248,2],[250,1,250,2],[254,1,254,2],[265,1,265,2],[267,1,267,2],[269,1,269,2],[271,1,271,2],[273,1,273,2],[275,1,275,2],[277,1,277,2],[279,1,279,2],[283,1,283,2],[285,1,285,2],[293,1,293,2],[305,1,305,2],[307,1,307,2],[309,1,309,2],[313,1,313,2],[334,1,334,2],[336,1,336,2],[340,1,340,2],[342,1,342,2],[344,1,344,2],[348,1,348,2],[350,1,350,2],[352,1,352,2],[354,1,354,2],[356,1,356,2],[358,1,358,2],[360,1,360,2],[362,1,362,2],[368,1,368,2],[370,1,370,2],[372,1,372,2],[383,1,383,2],[385,1,385,2],[387,1,387,2],[389,1,389,2],[391,1,391,2],[399,1,399,2],[405,1,405,2],[409,1,409,2],[411,1,411,2],[413,1,413,2],[415,1,415,2],[417,1,417,2],[419,1,419,2],[421,1,421,2],[423,1,423,2],[427,1,427,2],[429,1,429,2],[431,1,431,2],[443,1,443,2],[447,1,447,2],[451,1,451,2],[455,1,455,2],[457,1,457,2],[459,1,459,2],[465,1,465,2],[471,1,471,2],[475,1,475,2],[479,1,479,2],[483,1,483,2],[487,1,487,2],[489,1,489,2],[514,1,514,2],[518,1,518,2],[524,1,524,2],[526,1,526,2],[528,1,528,2],[532,1,532,2],[536,1,536,2],[540,1,540,2],[544,1,544,2],[548,1,548,2],[552,1,552,2],[556,1,556,2],[560,1,560,2],[562,1,562,2],[564,1,564,2],[568,1,568,2],[572,1,572,2],[588,1,588,2],[590,1,590,2],[592,1,592,2],[594,1,594,2],[596,1,596,2],[598,1,598,2],[624,1,624,2],[628,1,628,2],[629,1,629,2],[644,1,644,2],[645,1,645,2],[646,1,646,2],[647,1,647,2],[648,1,648,2],[654,1,654,2],[656,1,656,2],[660,1,660,2],[662,1,662,2],[666,1,666,2],[668,1,668,2],[672,1,672,2],[674,1,674,2],[689,1,689,2],[691,1,691,2],[693,1,693,2],[697,1,697,2],[699,1,699,2],[703,1,703,2],[705,1,705,2],[709,1,709,2],[711,1,711,2],[715,1,715,2],[717,1,717,2],[728,1,728,2],[730,1,730,2],[732,1,732,2],[736,1,736,2],[738,1,738,2],[742,1,742,2],[744,1,744,2],[748,1,748,2],[750,1,750,2],[764,1,764,2],[767,1,767,2],[769,1,769,2],[771,1,771,2],[773,1,773,2],[775,1,775,2],[777,1,777,2],[779,1,779,2],[786,1,786,2],[789,1,789,2],[817,4,817,5],[822,1,822,2],[890,1,890,2],[892,1,892,2],[896,1,896,2],[898,1,898,3],[900,1,900,2],[902,1,902,2],[903,1,903,2],[904,1,904,2],[906,1,906,2],[917,1,917,2],[921,1,921,2],[923,1,923,2],[925,1,925,2],[926,1,926,2],[929,1,929,2],[973,4,973,5],[978,1,978,2],[1046,1,1046,2],[1048,1,1048,2],[1052,1,1052,2],[1056,1,1056,2],[1060,1,1060,2],[1062,1,1062,2],[1064,1,1064,2],[1078,1,1078,2],[1080,1,1080,2],[1082,1,1082,2],[1084,1,1084,2],[1086,1,1086,2],[1090,1,1090,2],[1092,1,1092,2],[1095,1,1095,2],[1099,1,1099,2],[1107,1,1107,2],[1131,4,1131,5],[1136,1,1136,2],[1204,1,1204,2],[1206,1,1206,2],[1210,1,1210,2],[1212,1,1212,3],[1214,1,1214,2],[1216,1,1216,2],[1217,1,1217,2],[1218,1,1218,2],[1220,1,1220,2],[1221,1,1221,2],[1222,1,1222,2],[1235,1,1235,2],[1239,1,1239,2],[1241,1,1241,2],[1243,1,1243,2],[1245,1,1245,2],[1247,1,1247,2],[1251,1,1251,2],[1255,1,1255,2],[1259,1,1259,2],[1279,1,1279,2],[1285,1,1285,2],[1287,1,1287,2],[1340,4,1340,5],[1345,1,1345,2],[1406,1,1406,2],[1410,1,1410,2],[1412,1,1412,2],[1416,1,1416,2],[1420,1,1420,2],[1422,1,1422,2],[1424,1,1424,2],[1426,1,1426,2],[1428,1,1428,2],[1444,1,1444,2],[1450,1,1450,2],[1452,1,1452,2],[1508,4,1508,5],[1513,1,1513,2],[1575,1,1575,2],[1575,8,1575,9],[1577,8,1577,9],[1579,1,1579,2],[1581,1,1581,2],[1587,1,1587,2],[1591,1,1591,2],[1595,1,1595,2],[1599,1,1599,2],[1605,1,1605,2],[1626,1,1626,2],[1630,1,1630,2],[1632,1,1632,2],[1636,1,1636,2],[1642,1,1642,2],[1676,4,1676,5],[1745,1,1745,2],[1749,1,1749,2],[1751,1,1751,2],[1755,1,1755,2],[1757,1,1757,2],[1761,1,1761,2],[1770,1,1770,2],[1798,4,1798,5],[1867,1,1867,2],[1871,1,1871,2],[1873,1,1873,2],[1877,1,1877,2],[1881,1,1881,2],[1885,1,1885,2],[1889,1,1889,2],[1905,1,1905,2],[1910,1,1910,2],[1914,1,1914,2],[1916,1,1916,2],[1917,1,1917,2],[1918,1,1918,2],[1919,1,1919,2],[1920,1,1920,2],[1921,1,1921,2],[1922,1,1922,2],[1926,1,1926,2],[1928,1,1928,2],[1950,1,1950,2],[1952,1,1952,2],[1958,1,1958,2],[1962,1,1962,2],[1968,1,1968,2],[1999,4,1999,5],[2072,1,2072,2],[2076,1,2076,2],[2078,1,2078,2],[2080,1,2080,2],[2082,1,2082,2],[2083,1,2083,2],[2085,1,2085,2],[2086,1,2086,2],[2089,1,2089,2],[2090,1,2090,2],[2091,1,2091,2],[2092,1,2092,2],[2093,1,2093,2],[2096,1,2096,2],[2097,1,2097,2],[2101,1,2101,2],[2103,1,2103,2],[2115,1,2115,2],[2117,1,2117,2],[2123,1,2123,2],[2129,1,2129,2],[2141,1,2141,2],[2147,1,2147,2],[2155,1,2155,2],[2172,1,2172,2],[2174,1,2174,2],[2176,1,2176,2],[2182,1,2182,2],[2184,1,2184,2],[2188,1,2188,2],[2192,1,2192,2],[2226,4,2226,5],[2299,1,2299,2],[2303,1,2303,2],[2305,1,2305,2],[2309,1,2309,2],[2311,1,2311,2],[2315,1,2315,2],[2319,1,2319,2],[2323,1,2323,2],[2331,1,2331,2],[2346,1,2346,2],[2357,1,2357,2],[2365,1,2365,2],[2367,1,2367,2],[2369,1,2369,2],[2371,1,2371,2],[2373,1,2373,2],[2375,1,2375,2],[2388,1,2388,2],[2390,1,2390,2],[2394,1,2394,2],[2396,1,2396,2],[2398,1,2398,2],[2400,1,2400,2],[2402,1,2402,2],[2404,1,2404,2],[2408,1,2408,2],[2410,1,2410,2],[2414,1,2414,2],[2425,1,2425,2],[2426,1,2426,2],[2428,1,2428,2],[2430,1,2430,2],[2432,1,2432,2],[2434,1,2434,2],[2435,1,2435,2],[2436,1,2436,2],[2438,1,2438,2],[2440,1,2440,2],[2441,1,2441,2],[2444,1,2444,2],[2447,1,2447,2],[2457,4,2457,5],[2462,1,2462,2],[2530,1,2530,2],[2534,1,2534,2],[2536,1,2536,2],[2540,1,2540,2],[2546,1,2546,2],[2552,1,2552,2],[2557,1,2557,2],[2566,1,2566,2],[2576,4,2576,5],[2649,1,2649,2],[2653,1,2653,2],[2655,1,2655,2],[2661,1,2661,2],[2662,1,2662,2],[2676,1,2676,2],[2681,1,2681,2],[2706,1,2706,2],[2708,1,2708,2],[2727,1,2727,2],[2731,1,2731,2],[2736,1,2736,2],[2738,1,2738,2],[2755,1,2755,2],[2761,1,2761,2],[2763,1,2763,2],[2765,1,2765,2],[2767,1,2767,2],[2769,1,2769,2],[2819,1,2819,2],[2820,4,2820,5],[2894,1,2894,2],[2898,1,2898,2],[2900,1,2900,2],[2904,1,2904,2],[2906,1,2906,2],[2908,1,2908,2],[2910,1,2910,2],[2914,1,2914,2],[2929,1,2929,2],[2931,1,2931,2],[2933,1,2933,2],[2935,1,2935,2],[2941,1,2941,2],[2943,1,2943,2],[2944,1,2944,2],[2945,1,2945,2],[2946,1,2946,2],[2948,1,2948,2],[2954,1,2954,2],[2956,1,2956,2],[2963,1,2963,2],[2964,4,2964,5],[3033,1,3033,2],[3037,1,3037,2],[3039,1,3039,2],[3044,1,3044,2],[3047,1,3047,2],[3050,1,3050,2],[3053,1,3053,2],[3055,1,3055,2],[3068,1,3068,2],[3070,1,3070,2],[3072,1,3072,2],[3076,1,3076,2],[3080,1,3080,2],[3117,4,3117,5],[3190,1,3190,2],[3194,1,3194,2],[3196,1,3196,2],[3200,1,3200,2],[3204,1,3204,2],[3206,1,3206,2],[3208,1,3208,2],[3212,1,3212,2],[3233,4,3233,5],[3306,1,3306,2],[3310,1,3310,2],[3312,1,3312,2],[3316,1,3316,2],[3320,1,3320,2],[3324,1,3324,2],[3328,1,3328,2],[3332,1,3332,2],[3345,1,3345,2],[3349,1,3349,2],[3353,1,3353,2],[3355,1,3355,2],[3357,1,3357,2],[3361,1,3361,2],[3365,1,3365,2],[3367,1,3367,2],[3381,1,3381,2],[3385,1,3385,2],[3389,1,3389,2],[3393,1,3393,2],[3395,1,3395,2],[3399,1,3399,2],[3401,1,3401,2],[3403,1,3403,2],[3405,1,3405,2],[3409,1,3409,2],[3421,1,3421,2],[3425,1,3425,2],[3484,4,3484,5],[3557,1,3557,2],[3561,1,3561,2],[3563,1,3563,2],[3567,1,3567,2],[3571,1,3571,2],[3573,1,3573,2],[3575,1,3575,2],[3577,1,3577,2],[3581,1,3581,2],[3585,1,3585,2],[3589,1,3589,2],[3593,1,3593,2],[3595,1,3595,2],[3605,4,3605,5],[3678,1,3678,2],[3682,1,3682,2],[3684,1,3684,2],[3690,1,3690,2],[3694,1,3694,2],[3697,1,3697,2],[3700,1,3700,2],[3703,1,3703,2],[3706,1,3706,2],[3721,1,3721,2],[3725,1,3725,2],[3729,1,3729,2],[3732,1,3732,2],[3736,1,3736,2],[3739,1,3739,2],[3743,1,3743,2],[3770,1,3770,2],[3822,4,3822,5],[3895,1,3895,2],[3899,1,3899,2],[3901,1,3901,2],[3905,1,3905,2],[3909,1,3909,2],[3913,1,3913,2],[3921,1,3921,2],[3945,4,3945,5],[4018,1,4018,2],[4022,1,4022,2],[4024,1,4024,2],[4031,1,4031,2],[4034,1,4034,2],[4037,1,4037,2],[4041,1,4041,2],[4044,1,4044,2],[4048,1,4048,2],[4050,1,4050,2],[4062,1,4062,2],[4072,1,4072,2],[4076,1,4076,2],[4080,1,4080,2],[4088,1,4088,2],[4096,1,4096,2],[4117,4,4117,5],[4185,0,4185,7],[4229,1,4229,2]],"flags":["formulas_cached_only"]}
["Item","SECTION  1 ",null,"Unit","Qty","Rate ",null,"Amount"]
[]
[null,"BILL  NO. 1 "]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES "]
[]
[null,"The JBCC Series 2000 Minor Works Agreement (March 2014  edition 5.1) prepared by the Joint Building Contract Committee  shall be the applicable building agreement, amended as  hereinafter described "]
[]
[null,"The ASAQS Preliminaries (November 2007 edition) published  by the Association of South African Quantity Surveyors for use  with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these bills of quantities  "]
[]
[null,"Contractors are referred to the abovementioned documents for  the full intent and meaning of each clause thereof"]
[]
[null,"These clauses are hereinafter referred to by clause number  and heading only. Where standard clauses or alternatives are  not entirely applicable to this contract such modifications,  corrections or supplements as will apply are given under each  relevant clause heading and such modifications, corrections or  supplements shall take precedence notwithstanding anything  contrary contained in the abovementioned documents "]
[]
[null,"Where any item is not relevant to this specific contract such item is marked N/A, signifying not applicable "]
[]
[null,"PREAMBLES FOR TRADES  "]
[]
[null,"The Model Preambles for Trades (2008 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of  items fully described in the said Model Preambles will be entertained"]
[]
[null,"Supplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles shall take precedence over the provisions of the said Model preambles"]
[]
[null,"The contractor's prices for all items throughout these bills of quantities must take account of and include for all of the  obligations, requirements and specifications given in the said Model Preambles and in any supplementary preambles  "]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"PRICING OF PRELIMINARIES  "]
[]
[null,"Should the contractor select Option A in terms of sub clause 3.2.1 in the Contract Data - Contractor to Employer (CE) for the purpose of adjustment of these preliminaries, the amount entered into the amount column in these preliminaries is to be divided into one or more of the three categories provided namely Fixed (F), Value Related (V) and Time Related (T) "]
[]
[null,"GENERAL "]
[]
[null,"The contractor's prices for all items thought-out these bills of quantities must take into account SANS 10400-F: 2010 Edition 3 part F site operations available of SABS."]
[]
[null,"SECTION A - PRINCIPAL BUILDING  AGREEMENT "]
[]
[null,"Definitions "]
[]
[1,"Clause 1.0 - Definitions and interpretation "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Objective and preparations   "]
[]
[2,"Clause 2.0 - Offer acceptance and performance obligations  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3,"Clause 3.0 - Documents  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Clause 3 is deemed to be amended by the following: "]
[]
[null,"3.2.1 The construction guarantee shall be in the JBCC  Variable Construction Guarantee Format"]
[]
[4,"Clause 4.0 - Design responsibility  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[5,"Clause 5.0 - Employer's agents "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[6,"Clause 6.0 - Contractor's site representative  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7,"Clause 7.0 - Compliance with laws and regulations  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Clause 7 is deemed to be amended by the addition of the following clause:"]
[]
[7.1,"Without limiting the generality of the provisions of  clause 7.0 of the agreement, the contractor's  attention is drawn to the provisions of the Construction  Regulations, 2003 issued in terms of the Occupational  Health and Safety Act, 1993 in which it is specifically  stated that the employer shall prepare a documented  health and safety specification for the works and that  the employer shall ensure that the contractor has  made provision for the cost of health and safety  measures during the execution of the works.  The  contractor shall price opposite this item for compliance  with the act and the regulations and the provisions of  the aforementioned health and safety specification"]
[]
[7.2,"Without limiting the generality of the provisions of Clause 7.0 of the agreement the Contractors attention is drawn to the provisions of the SSA Emergency Plan and Risk Management requirements, e.g. Risk Assessments, Environmental Awareness Plan and on- and off-site Emergency Evacuation Plans may be required. The Contractor shall price opposite this item for compliance with requirements."]
[]
[7.3,"Without limiting the generality of the provisions of Clause 7.0 of the agreement the Contractors attention is drawn to the provisions of the Rehabilitation Plan requirements. The Contractor shall   price opposite this item for compliance with requirements."]
[]
[8,"Clause 8.0 - Works risk "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9,"Clause 9.0 - Indemnities  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[10,"Clause 10.0 - General insurances "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11,"Clause 11.0 - Special insurances  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[12,"Clause 12.0 - Effecting insurances  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[13,"Clause 13.0 - Assignment "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14,"Clause 14.0 - Security "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Execution  "]
[]
[15,"Clause 15.0 - Preparation for and execution of the works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[16,"Clause 16.0 - Site and access"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[17,"Clause 17.0 - Contract instructions "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[18,"Clause 18.0 - Setting out of the works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[19,"Clause 19.0 - Temporary works and plant"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[20,"Clause 19.2 - Notice boards"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[21,"Clause 20.0 - Nominated subcontractors  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[22,"Clause 21.0 - Selected subcontractors  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[23,"Clause 22.0 - Employer's direct contractors"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[24,"Clause 23.0 - Contractor's domestic subcontractors "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Completion  "]
[]
[25,"Clause 24.0 - Practical completion"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[26,"Clause 25.0 - Works completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[27,"Clause 26.0 - Final completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[28,"Clause 27.0 - Latent defects liability period  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[29,"Clause 28.0 - Sectional completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[30,"Clause 29.0 - Revision of date for practical completion  "]
[]
[null,"The removal and replacement of materials and/or workmanship which do not conform to specification or drawing shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value (Clause 29.3) "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[31,"Clause 30.0 - Penalty for late or non-completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Payment   "]
[]
[32,"Clause 31.0 is deemed to be amended to read as follows:"]
[]
[" ","The employer shall pay the contractor the amount certified in an interim payment certificate within Thirty (30) calendar days following the date of the interim payment certificate. Payment shall be subject to the contractor giving the Project Manager a  valid tax invoice for the amount due "]
[]
[33,"Clause 31.0 - Interim payment ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"The inclusion of materials and goods stored off site in the amount authorised for payment shall be at the sole discretion of the managers and such inclusion shall only be considered upon the provision, by the contractor, of an approved bank. "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[34,"Clause 32.0 - Adjustment to the contract value "]
[]
[null,"All fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor Where prices are submitted by the contractor or n/s subcontractor during the progress of the works in respect of contract instructions or in regard to a  claim under the terms of the contract and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the project manager wish to accept any such prices prior to the certificate, it shall be in writing issue of the final payment"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[35,"Clause 33.0 - Recovery of expense and loss  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[36,"Clause 34.0 - Final account and final payment "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[37,"Clause 35.0 - Payment to other parties "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Termination "]
[]
[38,"Clause 36.0 - Termination by employer - contractor's default  ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[39,"Clause 37.0 - Termination by employer - loss and damage  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[40,"Clause 38.0 - Termination by contractor - employer's default  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[41,"Clause 39.0 - Termination - cessation of the works  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Dispute   "]
[]
[42,"Clause 40.0 - Settlement of disputes "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Contract agreement "]
[]
[43,"Clause 41.0 - Post tender provisions  ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[44,"Clause 42.0 - Contractual agreement ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"The required information of the contracting parties and the amount of the accepted contract sum shall be inserted in the contractual agreement for signature of the agreement by the contracting parties  "]
[]
[1,"CONTRACTING AND OTHER PARTIES"]
[]
[1.1,"Employer: SSA"]
[]
[null,"Physical address:"]
[null,"Erf. 1024, "]
[null,"22 Protea Street, "]
[null,"Doringkloof, Centurion "]
[null,"Pretoria "]
[]
[1.2,"Interest of project team in the project "]
[]
[null,"The team have no interest in this project apart from their professional interest."]
[]
[2,"CONTRACT DATA - CONTRACT AND SITE INFORMATION "]
[]
[2.1,"Works Description"]
[]
[null,"The scope of work shall include (but is not limited to) the following: REFURBISHMENT OF KIEPERSOL BUILDING "]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[2.2,"Site Description"]
[null,"Erf. 1024, "]
[null,"22 Protea Street, "]
[null,"Doringkloof, Centurion "]
[null,"Pretoria "]
[]
[2.3,"Date on which possession of the site is intended to  be given: on 60 days from submission of tender"]
[]
[2.4,"Period for the commencement of the works after the contractor takes possession of the site: 1 Day "]
[]
[2.5,"Completion in sections is required"]
[]
[2.6,"Waiver of the contractor's lien or right of continuing  possession is required but SSA does not provide a Payment Guarantee. YES"]
[]
[2.7,"Defined restrictions to the site area - Public toilets may be used as long as premises are left clean, no washing or changing allowed. No sleeping on site"]
[]
[2.8,"Geotechnical investigation of the site has been undertaken N/A"]
[]
[2.9,"Existing premises occupied. NO"]
[]
[3,"CONTRACT DATE - INSURANCES AND SECURITIES"]
[]
[3.1,"Contract works insurance to be effected by the Contractor: For the amount of: Contract Sum + 25 % With deductibles payable by the Contractor to the amount N/A"]
[]
[null,"SASRIA insurance required:                 By Contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.2,"Supplementary/ special insurance to be effected by Contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.3,"Public liability insurance to be effected by - Contractor (As per signed Service Level Agreement)"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.4,"Support insurance to be effected N/A"]
[]
[3.5,"Special insurance to be effected N/A"]
[]
[4,"CONTRACT DATA - PRACTICAL COMPLETION DATES AND PENALTIES "]
[]
[4.1,"Intended date of practical completion is: 60 days from issue of order."]
[]
[4.2,"Intended date of practical completion where sectional completion is required and the penalty per calendar day for the works in sections: N/A and the penalty per calendar day for the works as a whole is: N/A"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[5,"CONTRACT DATA - DOCUMENTS AND GENERAL "]
[]
[5.1,"Construction document copies to be supplied to the  contractor free of charge"]
[]
[5.2,"The priced document may be used as a specification of materials and goods"]
[]
[5.3,"The contractor shall provide a schedule of rates where applicable "]
[]
[5.4,"On acceptance of the tender the priced document  is to be submitted within 1 Working days",null,"No"]
[]
[null,"SECTION B -  PRELIMINARIES  "]
[]
[6,"DEFINITIONS AND INTERPRETATION "]
[]
[6.1,"Clause 1.0 - Definitions and interpretation  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7,"DOCUMENTS"]
[]
[7.1,"Clause 2.1 - Checking of documents  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7.2,"Clause 2.2* - Provisional bills of quantities"]
[]
[null,"These bills of quantities are re-measurable in its totality. no claim or adjustment of rates will be considered to increase or  decrease in quantities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7.3,"Clause 2.3 - Availability of construction documentation "]
[]
[null,"The budgetary allowances and selected/nominated subcontract amounts allocated for subsequent trades included in this document will be separately procured, based on multiple procurement of selected/nominated subcontractors during the construction period"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8,"PREVIOUS WORK AND ADJOINING PROPERTIES"]
[]
[8.1,"Clause 3.1 - Previous work - dimensional accuracy  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8.2,"Clause 3.2 - Previous work - defects  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8.3,"Clause 3.3 - Inspection of adjoining properties "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[9,"SAMPLES, SHOP DRAWINGS AND MANUFACTURER'S INSTRUCTIONS"]
[]
[9.1,"Clause 4.1 - Samples of materials  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.2,"Clause 4.2 - Workmanship samples  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.3,"Clause 4.3 - Shop drawings "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.4,"Clause 4.4 - Compliance with manufacturer's instructions "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[10,"DEPOSIT AND FEES"]
[]
[10.1,"Clause 5.1 - Deposits and fees  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item"]
[{"$nulls":4},{"v":1,"d":"1.00"},null,null,0]
[11,"TEMPORARY SERVICES"]
[]
[11.1,"Clause 6.1 - Water "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.2,"Clause 6.2 - Electricity "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.3,"Clause 6.3 - Telecommunication facilities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.4,"Clause 6.4 - Ablution facilities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[12,"PRIME COST AMOUNTS"]
[]
[12.1,"Clause 7.1 - Responsibility for prime cost amounts "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":11}
[null,"Total Carried to Collection",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[13,"SPECIAL ATTENDANCE ON N/S SUBCONTRACTORS"]
[]
[13.1,"Clause 8.1 - Special attendance "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14,"GENERAL"]
[]
[14.1,"Clause 9.1 - Protection of the works"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.2,"Clause 9.2 - Protection/isolation of existing/section ally occupied works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.3,"Clause 9.3 - Security of the works"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.4,"Clause 9.4 - Notice before covering work  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.5,"Clause 9.5 - Disturbance  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.6,"Clause 9.6 - Environmental disturbance "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.7,"Clause 9.7 - Works cleaning and clearing"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.8,"Clause 9.8 - Vermin "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.9,"Clause 9.9 - Rubbish removals "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
["14.10","Clause 9.9 - Overhand work "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.11,"Clause 9.10 - Instruction manuals and guarantees"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.12,"Clause 9.11 - As built information"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.13,"Clause 9.12 - Tenant installations"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[15,"SCHEDULE OF VARIABLES "]
[]
[null,"Information necessary for elections and completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder Where no information is given it shall mean that no specific requirements are expected or that the clause is not relevant to this specific contract  "]
[]
[15.1,"Provisional bills of quantities [clause 2.2] The quantities are provisional YES"]
[]
[15.2,"Availability of construction documentation [clause 2.3] Construction documentation is complete"]
[]
[15.3,"Previous work - dimensional [clause 3.1] accuracy N/A "]
[]
[15.4,"Previous work - defects [clause 3.2] N/A "]
[]
[15.5,"Inspection of adjoining properties [clause 3.3] N/A"]
[]
[15.6,"Water [clause 7.2]"]
[null,"Option A (by contractor)                                        ","No"]
[null,"Option B (by employer - free of charge)    ","Yes"]
[null,"Option C (by employer - metered)    ","No"]
[]
[15.7,"Electricity [clause 7.3]"]
[null,"Option A (by contractor)     ","Yes"]
[null,"Option B (by employer - free of charge)    ","No"]
[null,"Option C (by employer - metered)    ","No"]
[]
[15.8,"Telecommunications [clause 7.4]"]
[null,"Telephone "]
[null,"Contractor"]
[null,"Facsimile"]
[null,"Contractor"]
[null,"E-mail"]
[null,"Contractor"]
[]
[15.9,"Ablution facilities [clause 7.5]"]
[null,"Option A (by contractor)  ","No"]
[null,"Option B (by employer)    ","Yes"]
[]
["15.10","Protection of the works [clause 9.1]"]
[]
[15.11,"Protection/isolation of existing/section ally  occupied works  [clause 9.2] Protection/isolation is  required YES "]
[]
[15.12,"Disturbance [clause 9.5]"]
[]
[null,"The following paragraphs shall be added to this sub-clause:"]
[null,"The contractor shall take all necessary measures to minimise noise. Such measures shall include inter alia, the use of 'silent' compressors and the like."]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"All work shall be executed without unacceptable and unreasonable dust, noise, vibrations, nuisance, inconvenience, annoyance and the like to the public, others other property. Any delays, stoppages and the like arising from or in order to comply with the above will not constitute grounds for an adjustment to the construction period or contract value 'whatsoever'"]
[]
[null,"The contractor indemnifies the employer against and accepts entire responsibilities for any claims, costs, damages and all other loss of whatsoever nature or delays which may arise on the above grounds."]
[]
[null,"The contractor shall take every precaution to protect buildings, etc. on adjoining sites against damage and shall be held solely responsible for any damage to persons or property caused by inadequate precautions."]
[]
[null,"SECTION  C - SPECIFIC PRELIMINARIES "]
[]
[16,"SITE INSTRUCTIONS"]
[]
[null,"Instructions issued on site are to be recorded in triplicate in a site instruction book which is to be maintained on site by the contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[17,"PROPRIETARY BRANDED PRODUCTS"]
[]
[null,"The contractor shall take delivery of, handle, store, use apply and/or fix all proprietary branded products in  strict accordance with the manufacturers instruction after consultation with the manufacturers authorised representative."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[18,"OVERTIME"]
[]
[null,"Should overtime be required to be worked for any reason whatsoever, the costs of such overtime are to be borne by the contractor unless the project manager has specifically authorised in writing, prior to the execution thereof, that costs for such overtime are to be borne by the employer."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[19,"AS BUILT DRAWINGS"]
[]
[null,"The position of construction breaks and the extent of individual concrete pours are to be recorded by the contractor on the structural engineer's drawings and are to be submitted to the project manager and the structural engineer for their records"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[20,"SITE INSTRUCTIONS"]
[]
[null,"Site instructions issued on site are to be recorded in a Site Instruction Book which is to be maintained on site by the contractor. This shall be a carbon triplicate book numbered consecutively which may be used only for the issue of site instructions"]
[]
[null,"Site instructions directed at the contractor and various sub-contractors may be issued only by the project manager or any of the professional consultants so authorised by the project manager and must be addressed firstly for the attention of the contractor, for further distribution. Copies of all site instructions issued are to be submitted to the project manager and the quantity surveyor at the following site meeting or not later than 21days after issue."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[21,"LABOUR RECORD"]
[]
[null,"At the end of each week the contractor shall provide the project manager with a written record, in schedule form, reflecting the number and description of tradesmen and labourers employed by him and all sub-contractors on the works each day."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[22,"PLANT RECORD"]
[]
[null,"At the end of each week the contractor shall provide the project manager with a written record, in schedule form, reflecting the number, type and capacity of all plant, excluding hand tools, currently used on the works."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[23,"NON CESSION OF MONIES"]
[]
[null,"The contractor shall not cede nor assign his rights or claims to any monies due or to become due under this contract"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[24,"CONTRACTOR TO BE RESPONSIBLE"]
[]
[null,"The contractor acknowledges that the principal objective of his appointment is his expert knowledge in the execution of the scope of work of this Contract. The Contractor shall therefore be solely responsible for all aspects of the construction of the Works including but not limited to management, resourcing, programming, co-ordination, etc. all as required for the type of project described within the time limits and quality standards specified."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[25,"INSTALLATION OF FURNITURE, EQUIPMENT, ETC"]
[]
[null,"During the progress of the contract the employer reserves the right to send onto, install, commission and test in the works any furniture, furnishings, fitments, machinery, equipment and installation, etc., not allowed for in this contract. The contractor shall permit the employer and his representatives and contractors entry to the works for this purpose. No financial allowance shall be made to the contractor (except as specifically allowed for in these bills of quantities) on account of the presence of any of the abovementioned workmen and their materials other than reasonable costs actually incurred and approved by the Project Manager "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[26,"PRICING OF BILLS"]
[]
[null,"Tenderers are to allow opposite each item for all costs associated therewith. All prices are to include, unless otherwise stated, for all materials, fabrication, conveyance and delivery, unloading, storing, unpacking, hoisting, labour, setting, fitting and fixing in position, cutting and waste (except where measured in accordance with the Standard System Of Measurement), patterns, models and templates, plant, temporary works, returning of packings, duties, taxes, imports, establishment charges, overheads, profit and all other obligation arising out of the contract. "]
[]
[null,"Items left unpriced will be deemed to be covered in prices against other items throughout these bills of quantities and no claim for any extras arising out of the tenderer's omission to price any item will be entertained."]
[]
[27,"UNAUTHORISED PERSONS ON SITE"]
[]
[null,"The contractor shall at all times strictly exclude all unauthorised persons from the site. No workmen are to be allowed to sleep on the premises. "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[28,"DAYWORKS"]
[]
[null,"Where in the opinion of the quantity surveyor any extra work cannot  properly be measured or valued at contract rates, the contractor will be allowed day work prices calculated at the rates and principles stated elsewhere in these bills of quantities. Failure by the contractor to properly complete the day work schedule will be deemed to be  acceptance of the quantity surveyor's discretion as to what applicable day work rates to be used.  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[29,"OCCUPATIONAL HEALTH AND SAFETY"]
[]
[null,"It is a requirement of this contract that the works are to be executed in strict accordance with the requirements of the Occupation Health And Safety Act. The successful contractor will therefor have to comply with all aspect related thereto and all costs associated therewith are deemed to be included in the contract price. No claims of any kind whatsoever will be entertained due to the contractor's non-compliance with the requirements of the act, the same being enforced onto the contractor. The successful contractor will be issued with a safety specification from the employer in terms of the act. "]
[]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Personal Protective Equipment (PPE)"]
[]
[null,"The contractor shall provide and maintain the appropriate personal protective equipment to all employees (maximum of 20 people) for the duration of the contract "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Medicals"]
[]
[null,"The contractor shall carried out medical check-up on employees (maximum of 20 people) for those involved in the following operations"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"SUMMARY OF CATEGORIES "]
[]
[null,"Category : Fixed   R.........................................................",{"$nulls":5},0]
[]
[]
[null,"Category : Value   R.........................................................",{"$nulls":5},0]
[]
[]
[]
[null,"Category : Time    R........................................................."]
{"$rows_empty":11}
[null,"Total Carried to Collection",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION  1 "]
[]
[null,"BILL  NO. 1 "]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES "]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,1,null,null,0]
[{"$nulls":4},2,null,null,0]
[{"$nulls":4},3,null,null,0]
[{"$nulls":4},4,null,null,0]
[{"$nulls":4},5,null,null,0]
[{"$nulls":4},6,null,null,0]
[{"$nulls":4},7,null,null,0]
[{"$nulls":4},8,null,null,0]
[{"$nulls":4},9,null,null,0]
[{"$nulls":4},10,null,null,0]
[{"$nulls":4},11,null,null,0]
[{"$nulls":4},12,null,null,0]
[{"$nulls":4},13,null,null,0]
[{"$nulls":4},14,null,null,0]
[{"$nulls":4},15,null,null,0]
{"$rows_empty":26}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 1"]
[]
[null,"DEMOLITIONS"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"View site"]
[]
[null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"Explosives"]
[]
[null,"No explosives whatsoever may be used for demolition purposes unless otherwise stated"]
[]
[null,"General"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the project manager. All undue noise is to be prevented and should the use of jack hammers, vibrators or similar plant be considered necessary by the Contractor, then prior permission must be obtained from the project manager.  Except where necessary for building operations, workmen must not enter the existing occupied buildings."]
[]
[null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the project manager"]
[]
[]
[null,"Total Carried to Collection"]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Demolitions"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Note: The following items are to remain the property of the employer and are to be carefully taken out, temporarily stored, transported over a distance of approximately 100km and handed over"]
[]
[]
[]
[null,"Deduct: \tAllowance of credit for materials salvaged from the demolitions"]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
[]
[null,"Taking down and removing"]
[]
[1,"Allow the sum of R 200 000.00 for the removal of shed at the courtyard",null,"Item",1,{"v":200000,"d":"200,000.00"},null,{"v":200000,"d":"R200,000.00"}]
{"$rows_empty":34}
[null,"Total Carried to Collection",{"$nulls":5},{"v":200000,"d":"R200,000.00"}]
[]
[]
[]
[]
[null,"SECTION 2 "]
[null,"Bill No. 1"]
[null,"Demolitions"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 1"]
[]
[null,"DEMOLITIONS"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,17,null,null,0]
[]
[{"$nulls":4},18,null,null,0]
{"$rows_empty":38}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"SECTION 2 "]
[null,"Bill No. 1"]
[null,"Demolitions"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 2"]
[]
[null,"ALTERATIONS PROVISIONAL"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"View site"]
[]
[null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"Explosives"]
[]
[null,"No explosives whatsoever may be used for alteration purposes unless otherwise stated"]
[]
[null,"General"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc. which are to remain the property of the employer shall be carefully taken out, temporarily stored, transported over a distance of approximately 100km to store and handed over to the employer"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc. which are to be re-used shall be thoroughly overhauled before refaxing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc., and oiling, adjusting and repairing ironmongery as necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described. Re-painting or re-varnishing is given separately"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 2 "]
[null,"Bill No. 2"]
[null,"Alterations "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Prices for taking out of doors, windows, etc. shall include for removal of all beads, architraves, ironmongery, etc."]
[]
[null,"Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc."]
[]
[null,"With regard to building up of openings in existing walls, cement screeds and paving's, granolithic, tops of walls, etc., shall be levelled and prepared for raising of brickwork"]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc."]
[]
[1,"Remove corrugated roof sheet from soffit of slab",null,"m²",1800,null,null,0]
[]
[]
[null,"Hacking up/off and removing ceramic tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc."]
[]
[2,"Floors and Landings ",null,"m²",178,null,null,0]
[]
[null,"Hacking up/off and removing wallpaper and glue from concrete or brickwork and preparing surfaces for new, plaster, paint finish, etc."]
[]
[3,"Walls ",null,"Item ",1,{"v":68000,"d":"68,000.00"},null,{"v":68000,"d":"R68,000.00"}]
[]
[null,"CUTTING THROUGH FLOORS AND CEILINGS"]
[]
[null,"Cutting through:"]
[]
[3,"1500mm core drilled opening  (making good floor finishes elsewhere)",null,"No",8,null,null,0]
{"$rows_empty":12}
[null,"Total Carried to Collection",{"$nulls":5},{"v":68000,"d":"R68,000.00"}]
[]
[]
[]
[]
[]
[]
[null,"SECTION 2 "]
[null,"Bill No. 2"]
[null,"Alterations "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 2"]
[]
[null,"ALTERATIONS PROVISIONAL"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,20,null,null,0]
[]
[{"$nulls":4},21,null,null,0]
{"$rows_empty":38}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"SECTION 2 "]
[null,"Bill No. 2"]
[null,"Alterations "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 3"]
[]
[null,"EARTHWORKS (PROVISIONAL)"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"View site"]
[]
[null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"Explosives"]
[]
[null,"No explosives whatsoever may be used for demolition purposes unless otherwise stated"]
[]
[null,"General"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the project manager. All undue noise is to be prevented and should the use of jack hammers, vibrators or similar plant be considered necessary by the Contractor, then prior permission must be obtained from the project manager.  Except where necessary for building operations, workmen must not enter the existing occupied buildings."]
[]
[null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the project manager"]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 3"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
[]
[null,"Nature of ground"]
[]
[null,"The nature of the ground is assumed to be loose sandy material, therefore \"earth\", but possibly interspersed with \"soft rock\" or \"hard rock\""]
[]
[null,"The nature of the ground is assumed to be gravel, therefore \"earth\", but possibly interspersed with \"soft rock\" or \"hard rock\""]
[]
[null,"The nature of the ground is assumed to be silty clay with loose river boulders varying in size up to approximately 450mm diameter, all of which will be deemed as \"earth\", but possibly interspersed with \"hard rock\""]
[]
[null,"Trial holes indicate that the nature of the ground is silty clay to a depth of approximately 500mm with fine to medium loose sandy material below, therefore \"earth\""]
[]
[null,"A soils investigation has been carried out on the site by the engineer and the report is annexed to these bills of quantities.  The soils report indicates that the ground varies between silty sand, reworked soil of mixed origin and residual shale, all of which will be deemed as \"earth\". All very hard unweathered shale, ironstone, etc., the removal of which necessitates the use of explosives or heavy duty hydraulic percussion hammers (peckers), will be classified as \"hard rock\""]
[]
[null,"Carting away of excavated material"]
[]
[null,"Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site"]
[]
[null,"Filling and layer work materials"]
[]
[null,"References such as \"G1\", \"G2\", etc. and \"C1\", \"C2\", etc. in descriptions of filling and layer work materials refer to corresponding references in the document \"Guidelines for Road Construction Materials.  TRH 14 : 1985\" compiled by the Committee of State Road Authorities and the properties set out therein for each kind shall be applicable to the respective materials described hereinafter"]
[]
[null,"Testing"]
[]
[null,"Prices for filling are to include for all necessary density and other tests"]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 3"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SITE CLEARANCE"]
[]
[null,"Site clearance"]
[]
[1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc. and trees not exceeding 200mm girth",null,"m²",20,null,null,0]
[]
[null,"EXCAVATIONS ETC"]
[]
[null,"Digging up topsoil"]
[]
[2,"Digging up topsoil to an average depth of 150mm and preserving for use as filling",null,"m²",3,null,null,0]
[]
[null,"Open face excavation in earth over sloping site"]
[]
[3,"Open face excavation",null,"m³",1,null,null,0]
[]
[null,"Excavation in earth for basement"]
[]
[4,"Not exceeding 2m deep",null,"m³",3,null,null,0]
{"$rows_empty":37}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 3"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 3"]
[]
[null,"EARTHWORKS (PROVISIONAL)"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,23,null,null,0]
[]
[{"$nulls":4},24,null,null,0]
[]
[{"$nulls":4},24,null,null,0]
{"$rows_empty":33}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 3"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 4"]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Lightweight concrete"]
[]
[null,"Lightweight concrete shall have a density of 600kg/m3 for the top 50mm and 400kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc. shall be 50mm"]
[]
[null,"Formwork"]
[]
[null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[null,"The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself"]
[]
[null,"Formwork to soffits of solid slabs etc. shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described"]
[]
[null,"Formwork to soffits of slabs, beams, etc. shall be deemed to be propped up exceeding 1,5m and not exceeding 3,5m high unless otherwise described"]
[]
[null,"Formwork to sides of bases, pile caps, ground beams, etc. will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 4"]
[null,"Concrete, Formwork and reinforcement "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[1,"Thicking under brick wall",null,"m³",10,null,null,0]
[]
[null,"REINFORCED CONCRETE CAST ON/IN FORMWORK"]
[]
[null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES"]
[]
[null,"25MPa/20mm concrete"]
[]
[2,"Strip footings",null,"m³",10,null,null,0]
{"$rows_empty":40}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 4"]
[null,"Concrete, Formwork and reinforcement "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 4"]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"Total Brought forward from page no.",null,null,27,null,null,0]
[]
[{"$nulls":4},28,null,null,0]
{"$rows_empty":40}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 4"]
[null,"Concrete, Formwork and reinforcement "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 5"]
[]
[null,"MASONRY"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"BRICKWORK"]
[]
[null,"Sizes in descriptions"]
[]
[null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[null,"Bagged and sealed walls"]
[]
[null,"Walls in two skins described as \"bagged and sealed\" shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats bitumen emulsion waterproofing coating"]
[]
[null,"Face bricks"]
[]
[null,"Bricks shall be ordered timeously to obtain uniformity in size and colour"]
[]
[null,"Pointing"]
[]
[null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc."]
[]
[null,"BLOCKWORK"]
[]
[null,"Concrete masonry units"]
[]
[null,"Blocks are to be either solid or hollow modular dense concrete masonry units having a compressive strength of 7MPa"]
[]
[null,"Wall ties for blockwork"]
{"$rows_empty":10}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 5"]
[null,"Masonry "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Wall ties shall be polypropylene ties complying with BS 76377.  Ties for hollow walls shall be of sufficient length to allow not less than 75mm of each end to be built into the blockwork.  Ties are to be spaced at intervals of not more than 1m in the horizontal direction and not more than 400mm staggered in the vertical direction except at openings, vertical joints or ends of walls where they are to be placed vertically above each other"]
[]
[null,"Blockwork"]
[]
[null,"Blockwork shall comply with SANS 10145 \"Concrete Masonry Construction\""]
[]
[null,"Surfaces to be plastered shall have joints raked out to a depth of at least 10mm to provide a key. Cavities of hollow walls shall be kept free of mortar droppings or other undesirable matter. Every second perpend of the bottom course of the external skin of hollow walls shall be left open as a weep hole"]
[]
[null,"Standard complementary blocks"]
[]
[null,"Descriptions of blockwork shall be deemed to include standard complementary blocks such as corner, three-quarter, half and quarter blocks required in the construction of corners, reveals, jambs, ends, etc. to solid and hollow walls and for bonding as necessary"]
[]
[null,"BRICKWORK"]
[]
[null,"SUPERSTRUCTURE"]
[]
[null,"Block walls"]
[]
[1,"One brick walls face to match the existing (External) ",null,"m²",18,null,null,0]
[]
[2,"Half brick walls to match the existing",null,"m²",14,null,null,0]
{"$rows_empty":20}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 5"]
[null,"Masonry "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 5"]
[]
[null,"MASONRY"]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,30,null,null,0]
[]
[{"$nulls":4},31,null,null,0]
{"$rows_empty":39}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 5"]
[null,"Masonry "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 6"]
[]
[null,"WATERPROOFING"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Waterproofing"]
[]
[null,"Waterproofing of roofs, basements, etc. shall be laid under a ten year guarantee.  Waterproofing to roofs shall be laid to even falls to outlets etc. with necessary ridges, hips and valleys. Descriptions of sheet or membrane waterproofing shall be deemed to include additional labour to turn-ups and turn-downs"]
[]
[null,"DAMPPROOFING OF WALLS AND FLOORS"]
[]
[null,"One layer type FV damp-proof course"]
[]
[null,"One layer 375 micron embossed polyethylene damp-proof course (SANS 952-1985 type B)"]
[]
[1,"Walls and Window Sills ",null,"m²",5,null,null,0]
[]
[]
[null,"DAMPPROOFING OF FLAT ROOFS, ETC"]
[]
[null,"Waterproofing, drainage, etc."]
[]
[2,"DPC under walls and  window sill",null,"m²",10,null,null,0]
[]
[3,"Waterproofing to roof ",null,"m²",1700,null,null,0]
{"$rows_empty":16}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 6"]
[null,"Waterproofing"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 6"]
[]
[null,"WATERPROOFING"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,33,null,null,0]
{"$rows_empty":42}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 6"]
[null,"Waterproofing"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 7"]
[]
[null,"ROOF COVERINGS, CLADDINGS, ETC"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Roof Covering"]
[]
[null,"The roof coverings shall be interlocking concealed-fix profile roll-formed in continuous lengths and cut to length by a pneumatic cut-off process from certified Z275 commercial quality galvanized steel. The profile shall be roll-formed with three ribs at centres not exceeding 203mm and a cover width not exceeding 406mm. These will include a male and female rib. When interlocked, the minimum sheet depth shall be 48mm. Each trough shall incorporate two stiffener ribs."]
[]
[null,"Finish for roof sheeting"]
[]
[null,"The paint finish shall be a full top coat Silicone Polyester and a half coat Grey to the reverse side"]
[]
[null,"Fixing of roof sheeting"]
[]
[null,"The sheets shall be fixed to every purlin by means of patented fixing method which will securely hold the sheets in position and lock-in both the side lap and centre ribs. The clips shall be manufactured from Galvanised steel and shall be fixed to the steel purlins with two cadmium plated teak 3 no 10,24 x 16mm long self-drilling/tapping screws, or with NA2 annular nails to timber purlins"]
[]
[null,"Safety"]
[]
[null,"The contractor shall exercise special care when handling long length sheeting, particularly in windy conditions. Should work be interrupted for any reason, all loose sheeting and incomplete sections must be adequately secured against possible movement by wind and gravity."]
{"$rows_empty":8}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 7"]
[null,"Roof Coverings, Claddings etc."]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Handling and storage"]
[]
[null,"The contractor shall ensure that all materials used on site for cladding, etc. are transported, handled and stored in accordance with the manufacturer's recommendations. Material damaged shall be rejected and replaced with undamaged material at the contractor's expense. Repair of damaged material will not generally be permitted. Rates are to include for preventing damage and protecting sheets through all stages of construction."]
[]
[null,"Inspection prior to installation or erection"]
[]
[null,"Before commencing installation, the contractor shall verify that the following items have been checked and accepted:"]
[]
[null,"a. The entire structure or the portion thereof to be sheeted has been correctly aligned, levelled and grouted"]
[null,"b. Purlins and sheeting rails are at the correct spacing and are within the specified tolerances."]
[null,"c. The corners of the roof are square and the wall framework is perpendicular or as specified"]
[null,"d. No protrusions such as bolt heads, splice plates, cleats, etc. appear on the face of the framework"]
[null,"e. All members to which roofing and cladding are to be fixed in aesthetically sensitive areas are true and square."]
[null,"f. Paint and any other materials that may be incompatible with the sheeting, have been painted over or so dealt with that direct contact with the sheeting is avoided."]
[null,"g. The contact faces between the purlins or the girts and the cladding are in the same plane. Should the alignment be inadequate, the contractor shall request instructions from the Engineer before proceeding with the fixing of the cladding."]
[]
[null,"Cleaning of roofs, etc."]
[]
[null,"All debris, etc. arising from the fixing of the cladding shall be removed from the sheeting as the fixing progresses. In addition, off-cuts of insulation, surplus fasteners and sealants, mandrels from pop rivets, off-cuts of flashings and sheeting, surplus flashing, food packaging, cartons, bottles, cans, etc. shall not be left on the roof or in the gutters."]
[]
[null,"Care shall be taken to ensure that no such material enters, blocks or partially impedes the flow of water into the outlets, down pipes, etc."]
[]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 7"]
[null,"Roof Coverings, Claddings etc."]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"ROOF COVERINGS"]
[]
[null,"PROFILED METAL SHEETING AND ACCESSORIES"]
[]
[null,"0.6mm Thick concealed fix \"Klip-Lok 700\" or similar approved light industrial Z275 spelter galvanised steel sheeting with \"Globalcoat\"or similar approved finish and colour to one side, \"Global coat Grey\" or similar approved finish to other side with and including accessories fixed to timber purlins at 2000mm centres"]
[]
[1,"Roof covering with pitch not exceeding 25 degrees",null,"m²",120,null,null,0]
[]
[null,"ROOF VENTILATORS"]
[]
[2,"Fibre-cement plain wing continuous ridge ventilators to 30 degrees angle and with base wing 230mm wide fixed through fibre-cement roof sheeting to steel purlins including watertight heading joints, necessary sealing strips, fixing accessories, etc.",null,"m",12,null,null,0]
[]
[3,"Extra over for closed end piece",null,"No",10,null,null,0]
[]
[4,"Galvanised sheet steel multi-purpose ventilator 1,83m long fixed through troughed roof sheeting to steel purlins including flashings, closers, sealing strips, etc.",null,"No",10,null,null,0]
[]
[null,"ROOF AND WALL INSULATION"]
[]
[null,"Aerolite insulation"]
[]
[5,"50mm Insulation closely fitted and laid on top of rendering between roof timbers concurrent with roof covering, all in accordance with manufacturer's instructions",null,"m²",100,null,null,0]
{"$rows_empty":21}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 7"]
[null,"Roof Coverings, Claddings etc."]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 7"]
[]
[null,"ROOF COVERINGS, CLADDINGS, ETC"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,35,null,null,0]
[]
[{"$nulls":4},36,null,null,0]
[]
[{"$nulls":4},37,null,null,0]
{"$rows_empty":42}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 7"]
[null,"Roof Coverings, Claddings etc."]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 8"]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Particle board"]
[null,"Particle board shall comply with the following specifications:"]
[]
[null,"a) SABS 1300 Particle board: exterior and flooring type"]
[null,"b) SABS 1301 Particle board: interior type"]
[]
[null,"Descriptions"]
[null,"The term \"planted on\" shall mean the nailing of timber to timber"]
[null,"The term \"screwed on\" shall mean the countersunk screwing of timber to timber"]
[null,"The term \"screwed and pelleted on\" shall mean the screwing of timber to timber with the heads of screws sunk and pelleted"]
[null,"The term \"plugged\" shall mean the countersunk screwing of timber to brickwork or concrete including plastic plugs"]
[null,"The term \"plugged and pelleted\" shall mean the screwing of timber to brickwork or concrete including plugs with heads of screws sunk and pelleted"]
[]
[null,"Joinery"]
[null,"Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc."]
[null,"Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes"]
[]
[null,"Fixing"]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 8"]
[null,"Carpentry and Joinery "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Decorative thermosetting plastic laminate covering"]
[]
[null,"Laminate covering shall be glued under pressure and edge strips of same shall be butt jointed at junctions with adjacent similar finish"]
[]
[null,"The sizes listed are Nominal sizes for solid SA pine member"]
[]
[null,"STRUCTURAL TIMBERWORK ETC"]
[]
[null,"ROOF CONSTRUCTION"]
[]
[null,"Prefabricated plate nailed timber roof truss construction"]
[]
[null,"Sawn softwood trusses, bracing, etc."]
[]
[null,"Typical Truss A"]
[]
[null,"Mono pitched truss construction to 12 degrees pitch comprising of 38 x 152mm SAP grade 7 rafter, 38 x 114mm SAP grade 7 tie beam, 38 x 114 SAP grade 7 webs and struts including all sprockets, bracing, gangnails, nails, nuts, washers, joints etc., approximate size 8100mm long x 1800mm high with entire truss containing 500mm eaves overhang projection on one side and 595mm overhang projection on the other side"]
[]
[null,"Sawn softwood grade 7"]
[]
[1,"38 x 114mm Wall plates",null,"m",20,null,null,0]
[]
[2,"52 x 76mm Purlins",null,"m",30,null,null,0]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Pressed-fibre cement"]
[]
[3,"12 x 250mm Barge boards including galvanised steel H-profile jointing strips",null,"m",200,null,null,0]
[]
[null,"SKIRTINGS"]
[]
[null,"Wrought meranti"]
[]
[4,"19 x 76mm Skirting nailed to walls with heads of nails punched and filled including 19mm quadrant bead planted on at junction with floor",null,"m",3400,null,null,0]
[]
[5,"Ditto to treads and risers",null,"m",10,null,null,0]
[]
[null,"TIMBER DOORS, WINDOWS, ETC"]
[]
[null,"Fire doors"]
[]
[null,"Fire doors are to be in accordance with SANS 1253"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 8"]
[null,"Carpentry and Joinery "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"DOORS ETC"]
[]
[null,"Solid Flush panel door "]
[]
[null,"44mm Thick semi-solid flush doors with commercial veneer both sides suitable for painting and hung to steel, aluminium, timber frames"]
[]
[6,"Door, size 813 x 1880mm high",null,"No",4,null,null,0]
[]
[null,"40mm Thick semi-solid flush panel doors with commercial veneer both sides suitable for painting and hung to steel, aluminium, timber frames"]
[]
[7,"Door, size 813 x 2032mm high",null,"No",56,null,null,0]
[]
[8,"Door, size 915 x 2300mm high",null,"No",20,null,null,0]
[]
[9,"Double door in two equal leaves with rebated meeting stiles, size 1510 x 2032mm high",null,"No",8,null,null,0]
[]
[null,"PROVISIONAL SUMS LOW VOLTAGE SERVICES"]
[]
[null,"CUPBOARDS"]
[]
[null,"Allow amount of R 8 000,00 (Eight Thousand Only) for the construction of built in cupboards "]
[]
[10,"Built-in Cupboards ",null,"Item ",1,{"v":8000,"d":"8,000.00"},null,{"v":8000,"d":"R8,000.00"}]
[]
[11,"Allow amount of R 80 000,00 (Eighty Thousand Only) for the construction of kitchen floors and wall cupboards ",null,"Item ",1,{"v":80000,"d":"80,000.00"},null,{"v":80000,"d":"R80,000.00"}]
{"$rows_empty":22}
[null,"Total Carried to Collection",{"$nulls":5},{"v":88000,"d":"R88,000.00"}]
[]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 8"]
[null,"Carpentry and Joinery "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,39,null,null,0]
[]
[{"$nulls":4},40,null,null,0]
[]
[{"$nulls":4},41,null,null,{"v":88000,"d":"R88,000.00"}]
{"$rows_empty":44}
[null,"Total Carried to Summary ",{"$nulls":5},{"v":88000,"d":"R88,000.00"}]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 8"]
[null,"Carpentry and Joinery "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 9"]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Fixing"]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[null,"Ceilings"]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal"]
[]
[null,"Bulkheads"]
[]
[null,"Unless otherwise described bulkheads shall be deemed to be horizontal along the length"]
[]
[null,"Steel components"]
[]
[null,"All steel components for ceilings, partitions, etc. are to be galvanised in accordance with SANS 121"]
[]
[null,"CEILING TIMBERS, BEADS, INSULATION, ETC"]
[]
[null,"NAILED-UP CEILINGS"]
[]
[null,"Openings"]
[]
[null,"Prices for openings for light fittings, ventilation grilles, air conditioning diffusers, etc. are to include for any necessary additional support, trimming around, etc."]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 9"]
[null,"Ceilings, Partitions and Access Flooring"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Gypsum plasterboard ceilings"]
[]
[null,"6,4mm Gypsum plasterboard ceilings including 38 x 38mm sawn softwood rendering at 450mm centres in one direction in 900mm board widths with metal joints and fixed as recommended by the manufacturer"]
[]
[1,"Horizontal ceilings to timber trusses",null,"m²",1800,null,null,0]
[]
[]
[null,"Gypsum coved cornice"]
[]
[2,"75mm Fixed to ceilings",null,"m",100,null,null,0]
[]
[null,"Trapdoors"]
[]
[3,"Extra over ceiling for 600 X 600mm trap door with framing, one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around",null,"No",10,null,null,0]
[]
[null,"SUSPENDED CEILINGS"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Proprietary suspended ceilings"]
[]
[null,"Hangers, suspension grids, \"lay-in\" panels, etc. are to be in accordance with the manufacturers' recommendations"]
[]
[null,"Flush plastered gypsum plasterboard suspended ceilings"]
[]
[null,"Ceilings shall comprise 9,5mm gypsum plasterboard boards screwed to and including screw-up suspension grid consisting of main tees at 1 200mm centres and galvanised steel capped cross tees at 400mm centres and with tape fixed over joints and the whole finished with gypsum plaster trowelled to a smooth polished surface"]
[]
[null,"The grid shall be suspended by means of galvanised steel L-section hangers at suitable centres, securely shot-pinned or screwed to concrete, steel or wood"]
[]
[null,"Flush plastered gypsum plasterboard suspended bulkheads"]
[]
[null,"Bulkheads shall comprise galvanised steel studding of 63,5mm top and bottom tracks with vertical studs at maximum 400mm centres, pop-riveted to the top and bottom tracks with similar additional vertical studs as necessary at abutments, ends, etc. and covered as described with plasterboard screwed to studding with drywall screws at maximum 300mm centres. Boards shall be butt jointed and finished with tape and jointing compound and the whole finished with gypsum plaster trowelled to a smooth polished surface to the thickness recommended by the manufacturer"]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 9"]
[null,"Ceilings, Partitions and Access Flooring"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Descriptions shall be deemed to include any additional studs at ends and intersections, corner beads, cornices at junctions with ceilings, jointing compound, tape, etc."]
[]
[null,"Brandering will not be allowed with each ceiling replacement; where possible existing Brandering must be used"]
[]
[null,"Ceilings Supply and Install"]
[]
[null,"Fire Barriers: The type and thickness of boards, the number of layers and the insulation (if necessary) is to be such as to produce the specified fire rating all in accordance with the manufacturer's recommendation and will be a PC item."]
[]
[null,"Proprietary suspended ceilings’ hangers, suspension grids, \"lay-in\" panels, etc. are to be in accordance with the manufacturers' recommendations"]
[]
[null,"All steel components for ceilings, partitions, etc. are to be galvanized in accordance with SANS 121"]
[]
[null,"Costs for openings for light fittings, ventilation grilles, air-conditioning diffusers, etc. are to include for any necessary additional support, trimming around, etc."]
[]
[null,"Suspended ceiling panels: 600mm x 600mm x 12,7mm, Acoustic Constellation/ Sternbuild 3 - NRC 0.70 OWAcoustic Constellation/Sternbuild 3 biologically absorbable mineral wool ceiling tiles, NRC - 0.70, size 1200 x 600 x 15mm with square-edge and white painted finish, laid on fire rated OWA construct S3 exposed demountable T24 suspension system, comprising galvanised main tees and cross tees with main tees suspended by means of galvanised hangers at centres not exceeding 1200mm, and all installed to manufacturer's instructions."]
[]
[4,"Ceilings suspended not exceeding 1m below timber trusses",null,"m²",1500,null,null,0]
[]
[null,"BULKHEADS"]
[]
[null,"Bulkhead formed of 9.5mm thick plasterboard comprising of one vertical face including all framework, jointing, etc.. with and including 6mm composite layer of Rhinolite plaster applied in two layers all in accordance with Architects specifications"]
[]
[5,"Plasterboard to form vertical face of bulkhead 80mm high",null,"m",50,null,null,0]
[]
[null,"Sundries"]
[]
[6,"Allow for light fitting openings, cutting, etc. in suspended ceilings",null,"no",10,null,null,0]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 9"]
[null,"Ceilings, Partitions and Access Flooring"]
[null,"Renovation of Kiepersol Building "]
["Item","PARTITIONS ETC",null,"Unit","Qty","Rate ",null,"Amount"]
[null,"\"Rhino-Drywall\" or other approved partitioning shall comprise steel studding formed of 89mm top and bottom tracks with vertical studs at maximum 600mm centres, friction fitted or pop-riveted to the top and bottom tracks with similar additional vertical studs ass necessary at abutments, ends, etc. and covered as described with \"Drywall\" screws at  maximum 220mm centres. boards ate to be built jointed and finished with \"rhino\" tape and \"ready mix D\" jointing compound all in accordance with the manufacturer's instructions. Intersections and abutments ate measured separately and descriptions shall be deemed to include any additional studs, corner beads, jointing compound, tape etc."]
[null,"Note: Paint and vanish finishes are measured elsewhere"]
[]
[null,"Partitioning 2800mm high with bottom track plugged and top track fixed to suspended ceiling tees, partitions to be equipped with sound Proofing,"]
[]
[null,"Rhino-Drywall or equivalent partitioning shall comprise of steel studding formed of 63,5mm top and bottom tracks with vertical studs at maximum 600mm centres, friction fitted or pop riveted to the top and bottom tracks with similar additional vertical studs as necessary at abutments, ends, etc. and covered as described with wallboard screwed to studding with \"Drywall\" screws at maximum 220mm centres. Boards are to butt jointed and finished with \"Rhino tape\" and \"Ready-mix D\" jointing compound all in accordance with the manufacturer's instructions. intersections and abutments are measured separately and descriptions shall be deemed to include any additional studs, corner beads, jointing compound, tape, etc."]
[]
[7,"Partitioning 3000mm high with bottom and top tracks plugged",null,"m",100]
[]
[null,"Extra over partitions for 40mm semi-solid flush doors with veneer on both sides and hardwood edge strips to vertical edges, hung to and including standard pressed steel door frame with one pair of 100mm steel hinges to each hanging stile, including additional studding, trimming, etc. to partitions"]
[]
[8,"Extra over partition for for door opening 813 x 2032mm high including natural anodised aluminium door frame with one pair of 100mm nylon washered aluminium hinges for timber door (elsewhere)",null,"No",10,null,null,0]
[]
[9,"Ditto for double door opening 1610 x 2032mm high, ditto",null,"No",2,null,null,0]
[]
[null,"GYPWALL FIRESTOP 51/F60S42 PARTITIONING SYSTEMS"]
[10,"Partitioning 3000mm high with bottom and top tracks plugged",null,"m",10,null,null,0]
[]
[null,"SKIRTINGS, ETC"]
[11,"4 x 100mm High aluminium skirting's",null,"m",100,null,null,0]
[]
[null,"INSULATION "]
[12,"install 100mmisotherm insulation (insulation included)",null,"m²",1500,null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 9"]
[null,"Ceilings, Partitions and Access Flooring"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 9"]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,43,null,null,0]
[]
[{"$nulls":4},44,null,null,0]
[]
[{"$nulls":4},45,null,null,0]
[]
[{"$nulls":4},46,null,null,0]
{"$rows_empty":40}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 9"]
[null,"Ceilings, Partitions and Access Flooring"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 10"]
[]
[null,"FLOOR COVERINGS, WALL LININGS, ETC"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Fixing"]
[]
[null,"Floor coverings, wall linings, etc. shall, where applicable, be fixed with adhesive as recommended by the manufacturers of the flooring, linings, etc."]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"SKIRTINGS, NOSINGS, ETC"]
[]
[null,"600 x 600mm \"Porcelain floor tiles\" or similar approved laid complete as per manufacturer's instructions including brass trimmings, edging, beads, etc."]
[]
[1,"On floors",null,"m²",325,null,null,0]
[]
[2,"On treads and risers of stairs",null,"m²",50,null,null,0]
[]
[null,"300 x 600mm \"Porcelain wall tiles\" or similar approved laid complete as per manufacturer's instructions including brass trimmings, edging, beads, etc."]
[]
[3,"On floors",null,"m²",498,null,null,0]
[]
[null,"WALL LININGS"]
[null,"5mm fully flexible vinyl sheeting with welded joints"]
[]
[4,"On walls",null,"m²",10,null,null,0]
[]
[null,"CORNER PROTECTORS, DIVIDING STRIPS, ETC"]
[]
[5,"4 x 50mm Aluminium cover strip",null,"m",100,null,null,0]
[]
[null,"ENTRANCE MAT"]
[null,"Matco Trio Scraper entrance mat colour Grey (Code: 2402), overall size 1800 x 1600 x 13mm gauge, consisting of polypropylene coarse fibre needle punch alternated with polyamide brush and drying strips, fixed in sunken aluminium mat surround formed of pre-formed matwell frame, complete with mitred edges and corner connectors, bedded into screed (by others), all in accordance with the manufacturers recommendations."]
[]
[6,"On floors",null,"No",2,null,null,0]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 10"]
[null,"Floor Coverings, Wall Linings, Etc."]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 10"]
[]
[null,"FLOOR COVERINGS, WALL LININGS, ETC"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,48,null,null,0]
{"$rows_empty":46}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 10"]
[null,"Floor Coverings, Wall Linings, Etc."]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 11"]
[]
[null,"IRONMONGERY"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"SUPPLEMENTARY PREAMBLE"]
[]
[null,"Finishes to ironmongery"]
[]
[null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list:"]
[null,"BS Satin bronze lacquered CH Chromium plated"]
[null,"SC Satin chromium plated"]
[null,"SE Silver enamelled"]
[null,"GE Grey enamelled"]
[null,"AS Anodised silver"]
[null,"AB Anodised bronze"]
[null,"AG Anodised gold"]
[null,"ABL Anodised black"]
[null,"PB Polished brass"]
[null,"PL Polished and lacquered"]
[null,"PT Epoxy coated"]
[null,"SD Sanded"]
[]
[null,"Proprietary items"]
[null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc. clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[null,"HINGES, BOLTS, ETC"]
[]
[null,"Union or similar"]
[1,"Chromium plated (brass plated) piano hinges",null,"m",10,null,null,0]
[2,"37651LH Indicator bolt",null,"No",2,null,null,0]
[3,"Paraplegic type ditto",null,"No",2,null,null,0]
[4,"Brass piano hinges",null,"m",2,null,null,0]
[5,"ART 208C91 Flush bolt 150mm",null,"No",2,null,null,0]
[6,"Steel rising hinge",null,"No",2,null,null,0]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 11"]
[null,"Ironmongery"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"CATCHES, CABIN HOOKS, ETC"]
[]
[null,"Union or similar"]
[7,"AL8721AS Union aluminium hat & coat hook",null,"No",10,null,null,0]
[]
[null,"LOCKS"]
[]
[8,"5 Lever Lockset ",null,"No",100,null,null,0]
[]
[null,"EN-SUITE LOCKS"]
[]
[null,"The following locks are to be suitable for master key operation"]
[]
[null,"The following locks are to be suitable for master and grand master key operation"]
[]
[null,"Union or similar approved"]
[]
[9,"Latchset",null,"No",1,null,null,0]
[10,"Rim night latch",null,"No",10,null,null,0]
[11,"Bathroom lockset with striking plate fixed to metal",null,"No",10,null,null,0]
[12,"Cylinder profile lock",null,"No",80,null,null,0]
[13,"Four-lever rebated deadlock",null,"No",80,null,null,0]
[14,"Two-lever lockset",null,"No",1,null,null,0]
[]
[null,"HANDLES"]
[]
[null,"Union or similar"]
[]
[15,"Flush handle",null,"No",1,null,null,0]
[16,"Anodised aluminium knob",null,"No",1,null,null,0]
[17,"Pull handle",null,"No",1,null,null,0]
[18,"Aluminium pull handle with roses",null,"No",1,null,null,0]
[19,"200mm anodised aluminium pull handle with back plates",null,"No",1,null,null,0]
[]
[null,"PUSH PLATES AND KICK PLATES"]
[]
[null,"Anodised aluminium plates countersunk screwed along edges at not exceeding 200mm centres"]
[]
[20,"Push plate",null,"No",1,null,null,0]
[21,"Kick plate",null,"No",1,null,null,0]
[22,"1 mm Steel plate",null,"No",1,null,null,0]
[23,"Circular pull handle on 150 x 150 x 3mm thick back plate",null,"No",1,null,null,0]
[24,"Handle on back plate",null,"No",1,null,null,0]
[25,"800 x 200mm high Natural Anodised aluminium kick/push plate plate",null,null,1,null,null,0]
[]
[null,"DOOR CLOSERS"]
[]
[26,"Interior single door closer",null,"No",50,null,null,0]
[27,"DC500 Cam action closer EN1-4SIL",null,"No",2,null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 11"]
[null,"Ironmongery"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"LETTERS, NAMEPLATES, ETC"]
[]
[null,"Assa Abloy' or other similar approved"]
[]
[28,"150 x 150mm engraved aluminium \"Electrical\" indicator plate",null,"No",10,null,null,0]
[]
[null,"Standard statutory signage set in bronze anodised aluminium frame with red fields on white field fixed to plastered or face brick wall with tamper proof screws"]
[]
[29,"Anodised aluminium plate with fire exit, fire extinguisher, fire hose reel or fire hydrant symbol",null,"No",5,null,null,0]
[]
[null,"1.6mm thick Natural anodised plates with and including 65mm high black Swiss 721 engraved letters fixed to wall above doors with tamper proof screws"]
[]
[30,"Nameplate 80 x 300mm with five and not exceeding ten numerals or letters",null,"No",10,null,null,0]
{"$rows_empty":40}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 11"]
[null,"Ironmongery"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 11"]
[]
[null,"IRONMONGERY"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,50,null,null,0]
[]
[{"$nulls":4},51,null,null,0]
[]
[{"$nulls":4},52,null,null,0]
{"$rows_empty":42}
[null,"Total Carried to Summary ",{"$nulls":5},0]
[]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 11"]
[null,"Ironmongery"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 12"]
[]
[null,"METALWORK"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Descriptions of bolts, anchors, etc."]
[]
[null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[]
[null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described"]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres"]
[]
[null,"Aluminium doors, windows, etc."]
[]
[null,"Doors and windows shall comply with AAAMSA design criteria  Glazing shall comply with SAGGA regulations.  Glass shall be  laminated performance glass as shown on the window schedules/drawings appended to these bills of quantities (as described in the headings to window descriptions?.  Glass thickness shall comply with SAGGA regulations irrespective of thicknesses shown on the schedules/drawings  Doors and windows shall be supplied with protective tape and plastic and shall be removed only once surrounding trades have been completed  For purpose made windows and doors, refer to drawings annexed to (issued separately with bills of quantities"]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 12"]
[null,"Metalwork"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"The following certificates shall be provided prior to commencement of site work:1\tA copy of the relevant AAAMSA Performance \tTest Certificate from the manufacturer/contractor \tsupplying the architectural aluminium product 2\tA Certificate of Conformance confirming that \tanodising or powder coating has been processed in \taccordance with SANS 999 and SANS 1796 \trespectively"]
[]
[null,"3\tA powder guarantee of not less than 15 years \tissued by the powder manufacturer.  The \t\tspecific\tconditions contained in this guarantee \tshall form part of the powder coating process 4\tA Certificate of Conformance confirming that \tglazing has been installed in accordance with \tSANS 0137, ensuring that safety glazing \tmaterials have been installed in the mandatory \tareas and that each individual pane of safety \tglazing materials has been permanently marked5\tA warranty from the manufacturer of the\tlaminated safety glass and/or hermetically \tsealed glazing units guaranteeing the products \tagainst delamination and colour degredation for a \tperiod of not less than five years"]
[]
[null,"WELDED STEEL FRAMEWORK, COLUMNS, ETC"]
[]
[null,"METALWORK"]
[]
[null,"ALUMINIUM WINDOWS, DOORS, ETC"]
[]
[null,"Aluminium windows of aluminium extrusion alloy 6063 or 6261 in temper T5 or T6 to comply with BS1474"]
[]
[null,"Finish to be epoxy powder coated aluminium to SABS standards and approved approved standard colour range"]
[null,"Prices to include for glazing as specified, fitting in position and sealing watertight all round (Refer to window schedules attached to these bills of quantities)"]
[null,"Aluminium work to be manufactured and installed in accordance with the standards and norms as prescribed by the accosiation of architectural aluminium manufacturers of South Africa. Contractors to issue a certification on completion that these standards has been complied to."]
[null,"Epoxy powder coated aluminium purpose made window complete with frames, subframes, ironmongery including glazing as per window schedule and fixed to brickwork or concrete and sealed water tight all round"]
[]
[null,"Allow R 20 000,00 for fixing Aluminium windows to comply with BS1474"]
[]
[1,"On Windows ",null,"Item ",1,{"v":20000,"d":"20,000.00"},null,{"v":20000,"d":"R20,000.00"}]
[]
[null,"ALUMINIUM SHOPFRONTS"]
[]
[null,"Powder coated shopfronts, system complete with subframes, ironmongery, glass, sealing, etc. and fixing to brickwork or concrete"]
[]
[2,"Purpose made shopfront, 1900 X 3000mm high ",null,"No",1,null,null,0]
[]
[null,"Total Carried to Collection",{"$nulls":5},{"v":20000,"d":"R20,000.00"}]
[]
[null,"Section 2"]
[null,"Bill No. 12"]
[null,"Metalwork"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 12"]
[]
[null,"METALWORK"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,54,null,null,0]
[]
[{"$nulls":4},55,null,null,{"v":20000,"d":"R20,000.00"}]
{"$rows_empty":40}
[null,"Total Carried to Summary ",{"$nulls":5},{"v":20000,"d":"R20,000.00"}]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 12"]
[null,"Metalwork"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 13"]
[]
[null,"PLASTERING"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"GRANOLITHIC"]
[]
[null,"Method"]
[null,"The method to be used shall be either the monolithic method or the bonded method"]
[]
[null,"Preparation"]
[null,"For granolithic applied monolithically, the concrete floor shall be swept clean after bleeding of the concrete has ceased and the slab has begun to stiffen; any remaining bleed water shall be removed and the granolithic applied immediately thereafter. For granolithic to be bonded to the floor slab after it has hardened, the slab surface shall be hacked (preferably by mechanical means) until all laitance, dirt, oil, etc. is dislodged and swept clean of all loose matter. The slab shall then be wetted and kept damp for at least six hours before applying the granolithic"]
[]
[null,"Mix"]
[null,"Granolithic shall attain a compressive strength of at least 41MPa. The coarse aggregate shall comply with SANS 1083 and shall generally be capable of passing a 10mm mesh sieve. Where the thickness of the granolithic exceeds 25mm, the size of the coarse aggregate shall be increased to the maximum size compatible with the thickness of the granolithic"]
[]
[null,"Panels"]
[null,"Granolithic shall be laid in panels not exceeding 14m² for monolithic finishes, not exceeding 9,5m² for bonded finishes and not exceeding 6m² for all external granolithic. Wherever possible, panels shall be square but at no time should the length of the panel exceed 1,5 times its width"]
[]
[null,"Where possible joints between panels shall be positioned over joints in the floor slab and shall be at least 3mm wide through the full thickness of the finish, separated by strips of wood or fibreboard and finished with V-joints"]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 13"]
[null,"Plastering "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Laying"]
[]
[null,"Monolithic granolithic shall be applied to the partially set slab and thoroughly compacted and lightly wood floated to the required levels"]
[]
[null,"Bonded granolithic shall be applied to the slab after applying a 1:1 sand-and-cement slurry brushed over the surface and allowed to partially set before applying the granolithic. The granolithic shall be thoroughly compacted and lightly wood floated to the required levels"]
[]
[null,"After wood floating, the monolithic and bonded granolithic shall remain undisturbed until bleeding has ceased and the surface has stiffened. Any remaining bleed water and laitance shall then be removed and the surface steel trowelled or power floated"]
[]
[null,"Curing, seasoning and protection"]
[]
[null,"Granolithic shall be covered with clean hessian with waterproof building foil over and kept wet for at least seven days after laying"]
[]
[null,"Colour"]
[]
[null,"Coloured granolithic shall be tinted with an approved colouring pigment mixed into the granolithic in the proportion of ? kg pigment per pocket of cement, of uniform appearance and consistent colour throughout"]
[]
[null,"SCREEDS"]
[]
[null,"Screeds wood floated, on concrete"]
[]
[1,"On Floors ",null,"m²",30,null,null,0]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Compo plaster steel trowelled, on brickwork"]
[]
[2,"On Walls ",null,"m²",50,null,null,0]
{"$rows_empty":15}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 13"]
[null,"Plastering "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 13"]
[]
[null,"PLASTERING"]
[]
[null,"PREAMBLES"]
[]
[]
[]
[null,"Total Brought forward from page no.",null,null,57,null,null,0]
[]
[{"$nulls":4},58,null,null,0]
{"$rows_empty":42}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 13"]
[null,"Plastering "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 14"]
[]
[null,"TILING"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Patterns"]
[]
[null,"Unless otherwise described, tiles shall be laid with continuous joints in both directions"]
[]
[null,"Fixing"]
[]
[null,"Unless described as \"fixed with adhesive to plaster (plaster elsewhere)\" descriptions of tiling on brick or concrete walls, columns, etc. shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc. shall be deemed to include 1:3 plaster bedding"]
[]
[null,"Tiling described as \"fixed with adhesive on power floated concrete\" shall be deemed to include for approved tiling key-coat"]
[]
[null,"Ceramic, porcelain, marble and granite tiles are to be fixed and grouted with suitable adhesives and grouts as recommended by the manufacturer of the tiles"]
[]
[null,"WALL TILING"]
[]
[null,"300 X 600mm Porcelain tiles (PC R 2/m²) fixed with adhesive to plaster (plaster elsewhere) and flush pointed with tinted grout"]
[]
[1,"On walls",null,"m²",498,null,null,0]
{"$rows_empty":9}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"SECTION 2 "]
[null,"Bill No. 14"]
[null,"Tilling "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 14"]
[]
[null,"TILING"]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,60,null,null,0]
{"$rows_empty":48}
[null,"Total Carried to Summary ",{"$nulls":5},0]
[]
[]
[]
[]
[null,"SECTION 2 "]
[null,"Bill No. 14"]
[null,"Tilling "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 15"]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Wire gratings"]
[]
[null,"Descriptions of gutter outlets etc. shall be deemed to include wire balloon gratings"]
[]
[null,"Storm water channels"]
[]
[null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc., and disposal of surplus material on site"]
[]
[null,"French drains"]
[]
[null,"Descriptions of French drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, \"?\" geofabric filter blanket over stone, 300mm earth filling over and disposal of surplus material on site"]
[]
[null,"Septic tanks"]
[]
[null,"Descriptions of proprietary type septic tanks shall be deemed to include excavation, bedding and jointing, concrete base slabs, jointing to drains and backfilling, compaction, etc. all in accordance with the manufacturer's instructions and disposal of surplus material on site"]
[]
[null,"Stainless steel basins, sinks, wash troughs, urinals, etc."]
[]
[null,"Stainless steel for economy basins, domestic sinks and worktops shall be Type 430 (17/0)  Stainless steel for urinals, basins, quality sinks, wash troughs, institutional equipment, etc. shall be Type 304 (18/8)  Stainless steel for laboratory sinks, photographic equipment, etc. shall be Type 316 (18/8)  Units shall have standard aprons on all exposed edges and tiling keys against walls where applicable"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 15"]
[null,"Plumbing And Drainage (Provisional)"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Sealing of edges"]
[]
[null,"Outer edges of sinks, basins, baths, urinals, etc. are to be sealed against adjacent surfaces with approved silicone"]
[]
[null,"PVC-U pipes and fittings"]
[]
[null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[null,"PVC-U pressure pipes and fittings"]
[]
[null,"Pipes of 50mm diameter and smaller shall be plain ended with solvent welded PVC-U loose sockets and fittings  Pipes of 63mm diameter and greater shall have sockets and spigots with push-in type integral rubber ring joints.  Bends shall be PVC-U and all other fittings shall be cast iron, all with similar push-in type joints"]
[]
[null,"High density polyethylene (HDPe) pipes and fittings"]
[]
[null,"Pipes shall be type IV and of the class specified with compression fittings"]
[]
[null,"Polypropylene pipes"]
[]
[null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc. with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[null,"Copper pipes"]
[]
[null,"Pipes shall be hard drawn and half-hard pipes of the class described.  Class 0 (thin walled hard drawn) pipes shall not be bent.  Class 1 (thin walled half-hard), Class 2 (half-hard) and Class 3 (heavy walled half-hard) pipes shall only be bent with benders with inner and outer formers.  Fittings to copper waste, vent and anti-syphon pipes, capillary solder fittings and compression fittings shall be \"?\" type.  Capillary solder fittings shall comply with ISO 2016"]
[]
[null,"Copper pipes are to be installed in accordance with the latest revision of the Code of Practice for Copper Plumbing soldering techniques.  Flux, solder, etc. to be strictly in accordance with the manufacturer's requirements with special attention to copper flux composition"]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 15"]
[null,"Plumbing And Drainage (Provisional)"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Reducing fittings"]
[]
[null,"Where fittings have reducing ends or branches they are described as \"reducing\" and only the largest end or branch size is given. Should the contractor wish to use other fittings and bushes or reducers he may do so on the understanding that no claim in this regard will be entertained"]
[]
[null,"Fixing of pipes"]
[]
[null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc., casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[null,"Paper wrapping to pipes"]
[]
[null,"Pipes chased into brickwork must be wrapped with two layers of stout brown paper tied with wire.  Rates are to include for wrapping around joints and fittings"]
[]
[null,"Disinfection of water pipework"]
[]
[null,"Water pipework is to be disinfected at completion"]
[]
[null,"Prices for wrapping of pipes shall include for all work as described to couplings in the length"]
[]
[null,"General"]
[]
[null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc. are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc. shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of ?% Mod AASHTO density and disposal of surplus material on site"]
[]
[null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc. and to steel pipes (adaptors for connections to copper pipes, etc. are given separately)"]
[]
[null,"Descriptions of WC pans, slop hoppers, etc. shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[null,"As-built drawings"]
[]
[null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 15"]
[null,"Plumbing And Drainage (Provisional)"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"RAINWATER DISPOSAL"]
[]
[1,"Allow the sums of R 500 000,00 for the plumbing works (sanitary fittings, sundries, water tanks etc. ",null,"Item ",1,{"v":500000,"d":"500,000"},null,{"v":500000,"d":"R500,000.00"}]
[]
[null,"WATER SUPPLIES AND FIRE APPLIANCES"]
[]
[2,"Allow the sums of R 500 000,00 for water suppliers and installation of fire detection and alarm systems including testing ",null,"Item ",1,{"v":500000,"d":"500,000"},null,{"v":500000,"d":"R500,000.00"}]
[]
[null,"AS-BUILT DRAWINGS"]
[]
[3,"Provision of as-built drawings",null,"Item",1,null,null,0]
{"$rows_empty":45}
[null,"Total Carried to Collection",{"$nulls":5},{"v":1000000,"d":"R1,000,000.00"}]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 15"]
[null,"Plumbing And Drainage (Provisional)"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 15"]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,62,null,null,0]
[]
[{"$nulls":4},63,null,null,0]
[]
[{"$nulls":4},64,null,null,0]
[]
[{"$nulls":4},65,null,null,{"v":1000000,"d":"R1,000,000.00"}]
{"$rows_empty":40}
[null,"Total Carried to Summary ",{"$nulls":5},{"v":1000000,"d":"R1,000,000.00"}]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 15"]
[null,"Plumbing And Drainage (Provisional)"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 16"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Specifications, drawings, etc."]
[]
[null,"Tenderers will be referred to the specification by Engineers for the electrical work, for the full descriptions of  items are to be read and priced in conjunction with the specification and drawings"]
[]
[null,"Contract price adjustment provisions"]
[]
[null,"With reference to clause ? of the Preliminaries all items in this bill will be subject to fluctuations in the cost of labour and material on the following basis:"]
[]
[null,"(a) Ring main units, miniature substations, transformers, main low tension boards, distribution boards and busbars between transformer and low tension boards calculated on the indices published by the Steel and Engineering Industries Federation of South Africa"]
[]
[null,"(b) Cables in excess of 16mm² calculated on the basis of proven cost  "]
[]
[null,"(c) All other work calculated on the index for work group"]
[]
[null,"Distribution boards etc."]
[]
[null,"Rates for distribution boards etc. are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[null,"Switches, socket outlets, etc."]
[]
[null,"Rates for switches, socket outlets, etc. are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[null,"Light fittings"]
[]
[null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[null,"LOW TENSION DISTRIBUTION"]
[]
[null,"MAIN LOW TENSION BOARD and RETICULATIONS"]
[]
[1,"Allow the sum of 120 000.00 for the power factor correction and lighting and ground protection ",null,"Item ",1,{"v":120000,"d":"120,000"},null,{"v":120000,"d":"R120,000.00"}]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},{"v":120000,"d":"R120,000.00"}]
[]
[]
[null,"Section  2"]
[null,"Bill No. 16"]
[null,"Electrical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 16"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,67,null,null,0]
{"$rows_empty":46}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section  2"]
[null,"Bill No. 16"]
[null,"Electrical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 17"]
[]
[null,"MECHANICAL WORK"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Specifications, drawings, etc."]
[]
[null,"Specification and drawings for the mechanical work to be developed by engineer, with full descriptions of which are to be read and priced in conjunction with the said specification and drawings to be provided by the mechanical engineer "]
[]
[null,"Ductwork"]
[]
[null,"Descriptions of ducts shall be deemed to include stiffeners, jointing materials, sealants, couplers in the running length and access/inspection panels in accordance with the specification"]
[]
[null,"Dampers"]
[null,"Descriptions of smoke and fire dampers shall be deemed to include fusible links, sleeves, frames, supports and access openings in ducts"]
[]
[null,"Air diffusion"]
[null,"Descriptions of air terminals, grilles, louvres and the like shall be deemed to include necks, frames, supports and flexible connections"]
[]
[null,"Fans"]
[null,"Descriptions of fan assemblies shall be deemed to include supports from the structure, flexible or other connections to ductwork, vibration isolation mountings and airtight inspection doors"]
[]
[null,"Sound attenuators"]
[null,"Descriptions of sound attenuators shall be deemed to include flanged or flexible connections to ducts and supports from the structure"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 17"]
[null,"Mechanical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"Fan coil units, fan air terminals and fan heaters"]
[]
[null,"Descriptions of fan coil units, fan air terminals and fan heaters shall be deemed to include connection points for water, air and electrical supply, for air grilles, dust trays, condensate trays and vibration isolation mountings.  Flexible ducts, flexible hose and connecting cables for connecting these units to each other or to water pipe, and electrical supply are separately measured"]
[]
[null,"Major equipment"]
[]
[null,"Descriptions of major equipment such as chillers, air handling units and the like shall be deemed to include connections to water, air and electrical supply and/or discharge points, supports, bearers, vibration insulation mountings, filters, insulation, inspection ladders and gangways, access doors and panels and painting etc. as specified"]
[]
[null,"Piping"]
[]
[null,"Pipe diameters are nominal internal unless otherwise stated  Where fittings have reducing ends or branches they are described as \"reducing\". In the case of pipes with diameters not exceeding 60mm only the largest end or branch diameter is given.  Should the contractor wish to use other fittings and bushes or reducers he may do so on the understanding that no claim in this regard will be entertained.  In the case of pipes with diameters exceeding 60mm all diameters are given and no claim for extra bushes, reducers, etc. will be entertained"]
[null,"Fixing of pipes"]
[]
[null,"Unless otherwise stated, descriptions of pipes shall be deemed to include fixing to walls etc., casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[null,"Pump sets"]
[]
[null,"Descriptions of pumps shall be deemed to include connections to water and electrical supply and/or discharge points, vibration insulation mountings, insulation, drip trays with outlets, pressure gauges, etc."]
[null,"Valves"]
[]
[null,"Descriptions of valves shall be deemed to include flanged or screwed connections to pipes, reducers, supports, etc."]
[]
[null,"Insulation"]
[]
[null,"Descriptions of insulation shall be deemed to include priming the pipes with zinc chromate primer before the insulation is applied, painting the insulation when completed and applying vapour barrier where specified"]
{"$rows_empty":8}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 17"]
[null,"Mechanical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"AIR CONDITIONING INSTALLATION"]
[]
[null,"SPLIT TYPE UNITS"]
[]
[1,"Supply and install 3.5kW MidWall split unit, 12000 BTU, including divider plates",null,"No",30,null,null,0]
[]
[2,"Apply and install 5.2kW MidWall split unit, 18000 BTU, including divider plates",null,"No",50,null,null,0]
[]
[null,"LIFT INSTALLATION"]
[]
[3,"Allow the sums of R 800 000,00 for the installation of Passenger lift car including frame, guides, enclosure, base, car door, inspection door, sill, internal finishes, handrails, lighting and ventilation",null,"Item ",1,{"v":800000,"d":"800,000"},null,{"v":800000,"d":"R800,000.00"}]
{"$rows_empty":44}
[null,"Total Carried to Collection",{"$nulls":5},{"v":800000,"d":"R800,000.00"}]
[]
[]
[null,"Section 2"]
[null,"Bill No. 17"]
[null,"Mechanical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 17"]
[]
[null,"MECHANICAL WORK"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,69,null,null,0]
[]
[{"$nulls":4},70,null,null,0]
[]
[{"$nulls":4},71,null,null,{"v":800000,"d":"R800,000.00"}]
{"$rows_empty":43}
[null,"Total Carried to Summary ",{"$nulls":5},{"v":800000,"d":"R800,000.00"}]
[]
[]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 17"]
[null,"Mechanical Works "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2 "]
[]
[null,"BILL 18"]
[]
[null,"GLAZING"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"Float glass"]
[]
[null,"The term \"float glass\" is used for monolithic annealed glass"]
[]
[null,"Laminated glass"]
[]
[null,"Laminated glass to have polyvinyl butyral (PVB) interlayer(s)"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"GLAZING TO STEEL WITH SCREWED-ON BEADS (BEADS ELSEWHERE)"]
[]
[null,"6mm Clear float glass"]
[]
[1,"500 X 700mm thick mirror coated float glass",null,"No",16,null,null,0]
[]
[null,"Sun Control "]
[]
[2,"Allow the sum of R 90 000,00 for  the installation of corten sun control panels ",null,"Item",1,90000,null,{"v":90000,"d":"R90,000.00"}]
{"$rows_empty":16}
[null,"Total Carried to Collection",{"$nulls":5},{"v":90000,"d":"R90,000.00"}]
[]
[]
[null,"Section 2 "]
[null,"Bill No. 18"]
[null,"Glazing "]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 18"]
[]
[null,"GLAZING"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,73,null,null,{"v":90000,"d":"R90,000.00"}]
{"$rows_empty":46}
[null,"Total Carried to Summary ",{"$nulls":5},{"v":90000,"d":"R90,000.00"}]
{"$rows_empty":7}
[null,"Section 2 "]
[null,"Bill No. 18"]
[null,"Glazing "]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"SECTION 2"]
[]
[null,"BILL 19"]
[]
[null,"PAINTWORK"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"PREPARATORY WORK TO EXISTING WORK"]
[]
[null,"Previously painted plastered surfaces"]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces"]
[null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces"]
[null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[null,"PAINT SPECIFICATIONS"]
[]
[null,"All painting shall be done in accordance with \"?\" specifications unless otherwise described"]
[]
[null,"COLOURS"]
[null,"Colours for all paintwork shall be standard colours with a value exceeding 7 on the Munsell system"]
[]
[null,"PAINTWORK ETC TO NEW WORK"]
[]
[null,"PAINTWORK, ETC TO NEW WORK ON PLASTER BOARD SURFACES"]
[]
[null,"One (1) coat \"Dulux Duraseal\" alkali resistant primer and two coats \"Dulux Dura 100\" interior double velvet paint ",null,""]
[]
[1,"On Plastered wall",null,"m²",25,null,null,0]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[null,"Section 2"]
[null,"Bill No. 19"]
[null,"Paintwork"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Qty","Rate ",null,"Amount"]
[null,"One (1) coat \"Acrylunder primer and two coat  ''Dulux Acrylic PVA Brilliant White \"paint on plastered wall, ceilings"]
[]
[2,"On Ceilings ",null,"m²",50,null,null,0]
[]
[3,"Cornice ",null,"m",10,null,null,0]
[]
[null,"PAINTWORK, ETC ON FLOATED PLASTER"]
[]
[null,"\"DULUX HICHEM\" EPOXY ENAMEL PAINT",null,""]
[]
[null,"Prepare and apply One (1) coats \"Dulux Dura 100\" interior double velvet paint ",null,""]
[]
[4,"On plastered wall",null,"m²",7200,null,null,0]
[]
[null,"Prepare and apply One (1) coats \"Dulux Dura 100\" interior Low sheen Acrylic "]
[]
[5,"On Plastered wall",null,"m²",35,null,null,0]
[]
[null,"Prepare and apply One (1) coat Dulux Acrylic PVA Brilliant White \"paint on plastered wall, ceilings"]
[]
[6,"On Ceilings ",null,"m²",200,null,null,0]
[]
[7,"Cornice ",null,"m",100,null,null,0]
[]
[null,"WOOD",null,""]
[]
[null,"Prepare and apply One (1) coat wood primer, one undercoat polyurethane varnish thinned with 10% mineral turpentine  and Two (2) full woodluv Gloss (External surface)"]
[]
[8,"On Exterior wooden double door ",null,"m²",280,null,null,0]
[]
[9,"On Exterior wooden Frames ",null,"m²",50,null,null,0]
[]
[null,"METAL",null,""]
[]
[null,"Prepare and apply spot prime bare patches in pre-primed surfaces with zinc chromate primer, One (1) coat \"Dulux Duragrip\" universal undercoat and Two (2) finishing coats of \"Dulux\" high gloss enamel paint on;",null,""]
[]
[10,"Angle Iron, Burglar Bars, Bracket",null,"m",50,null,null,0]
[]
[11,"On steel windows (internal and external with a size not exceeding 1m²",null,"No",20,null,null,0]
{"$rows_empty":9}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 19"]
[null,"Paintwork"]
[null,"Renovation of Kiepersol Building "]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 2"]
[]
[null,"BILL 19"]
[]
[null,"PAINTWORK"]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,75,null,null,0]
[]
[{"$nulls":4},76,null,null,0]
{"$rows_empty":43}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 2"]
[null,"Bill No. 19"]
[null,"Paintwork"]
[null,"Renovation of Kiepersol Building "]
["SUMMARY"]
[null,"SECTION 1"]
[]
[null,"Preliminaries",null,"Page"]
[]
[null,"SECTION 2"]
[]
[1,"Demolitions",null,"Page"]
[2,"Alterations",null,"Page"]
[3,"Earthworks (provisional)",null,"Page"]
[4,"Concrete, formwork and reinforcement",null,"Page"]
[5,"Masonry",null,"Page"]
[6,"Waterproofing",null,"Page"]
[7,"Roof coverings, claddings, etc.",null,"Page"]
[8,"Carpentry and joinery",null,"Page"]
[9,"Ceilings, partitions and access flooring",null,"Page"]
[10,"Floor coverings, wall linings, etc.",null,"Page"]
[11,"Ironmongery",null,"Page"]
[12,"Metalwork",null,"Page"]
[13,"Plastering",null,"Page"]
[14,"Tiling",null,"Page"]
[15,"Plumbing and drainage",null,"Page"]
[16,"Electrical work",null,"Page"]
[17,"Mechanical work",null,"Page"]
[18,"Glazing",null,"Page"]
[19,"Paintwork",null,"Page"]
[]
[]
[]
[]
[]
[null,"Sub-total",{"$nulls":3},"Cur"]
[]
[null,"Less: Credit for old materials salvaged from demolitions etc.",null,"Item"]
[]
[null,"Sub-total",{"$nulls":3},"Cur"]
[]
[null,"Add: Contingency",null,{"v":0.05,"d":"5%"}]
[]
[]
[null,"Sub-total",{"$nulls":3},"Cur"]
[]
[null,"Value Added Tax at 15%"]
[]
[null,"Allow Fifteen per cent (15%) of the above sub-total for Value Added  Tax",null,"Item"]
[]
[]
[null,"Carried to form of tender",{"$nulls":3},"Cur"]

{"sheet":"Sheet1","index":1,"n_rows":535,"n_cols":8,"rows_kept":535,"merged":[[3,1,3,2],[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,1,11,2],[14,1,14,2],[16,1,16,2],[20,1,20,2],[28,1,28,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[132,1,132,2],[133,1,133,2],[435,1,435,2],[436,1,436,2],[437,1,437,2],[438,1,438,2],[439,1,439,2],[440,1,440,2],[441,1,441,2],[442,1,442,2],[443,1,443,2],[444,1,444,2],[446,1,446,2],[447,1,447,2],[448,1,448,2],[449,1,449,2],[450,1,450,2],[451,1,451,2],[452,1,452,2],[453,1,453,2]],"flags":["formulas_cached_only"]}
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 2 "]
[null,"BILL 3"]
[null,"EARTHWORKS (PROVISIONAL)"]
[]
[null,"Note: All alterations and removal of existing work should be approved by the Architect before any work can be carried out by the appointed contractor or sub-contractor"]
[]
[null,"OLD MATERIAL TO BECOME PROPERTY OF THE CONTRACTOR"]
[null,"Old materials from alterations, accept where described to be re-used or handed over, become  the property of the contractor who must allow credit for some in the final Summary"]
[]
[null,"OLD MATERIAL TO CARTED  AWAY"]
[null,"Old materials from alterations, accept where described as to be re-used or handed over, as well as all rubbish, etc. must be regularly carted from the site and not allowed to accumulate on or around the site"]
[]
[null,"OLD MATERIAL NOT TO BE RE-USED"]
[null,"None of the old materials are to used for new work except where specifically described as being set aside for  re-use"]
[]
[null,"Provide all necessary protection, hoarding, etc. to ensure stability of all structures during alteration works. Any damage to the structures as well as the remaining portions of the building and the rectification there of will be for the contractor's account."]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[1,"Removing of items such as doors, partitioning, ceilings  etc. and make good or replace as per direction "]
[]
[1.1,"Remove rubble from site  exceeding 1m³-hand loaded",null,"m³",1]
[]
[1.2,"Removal of rubble exceeding 1m³ in skip waste bins",null,"Per Bin",6]
[]
[null,"Rates For Work / Services: Plumbing "]
[]
[null,"(Note: Alterations refer to the removal of existing fittings/materials etc. and the replacement of such with same.) Where it implies removal/decommissioning or new installation this will be stated as a separate item). "]
[]
[2,"General Maintenance and Repairs"]
[]
[2.1,"Clean storm water channels and pipes",null,"m",1,null,null,"Rate only"]
[]
[2.2,"Clean Manholes",null,"Each",1,null,null,"Rate only"]
[]
[2.3,"Clean gutter and down pipes",null,"m",1,null,null,"Rate only"]
[]
[3,"Replace Cistern"]
[]
[3.1,"Remove Cistern All Tipes ( Low, High Level and Closed Couple)",null,"ea",1,null,null,"Rate only"]
[]
[4," Geysers"]
[4.1,"Remove under counter Geyser 10 / 15 Lt (Kwikot)",null,"ea",1,null,null,"Rate only"]
[]
["4..2","Remove 100Lt/150 Lt/200 LTGeyser (Kwikot) complete",null,"ea",1,null,null,"Rate only"]
[]
[4.3,"Remove  Kwikot  boilers with drain cock 10 L/15L",null,"ea",1,null,null,"Rate only"]
[]
[5,"Plumbing "]
[5.1,"Remove  hand wash basin complete: (Vaal Hibiscus Basin or similar)",null,"ea",1,null,null,"Rate only"]
[5.2,"Remove toilet complete (IQWA Beta Toilet Suite or similar)",null,"ea",1,null,null,"Rate only"]
[5.3,"Remove toilet pan ",null,"ea",1,null,null,"Rate only"]
[5.4,"Remove toilet water tank",null,"ea",1,null,null,"Rate only"]
[5.5,"Remove toilet water Pan",null,"ea",1,null,null,"Rate only"]
[5.6,"Remove Stainless Steel Urinal",null,"ea",1,null,null,"Rate only"]
[5.7,"Remove Toilet Seats Standard Wooden/White",null,"ea",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 3"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[]
[6,"Bathroom"]
[6.1,"Remove existing taps",null,"ea",1,null,null,"Rate only"]
[6.2,"Remove stainless steel sink within cabinet 1.8 (hinge door)",null,"ea",1,null,null,"Rate only"]
[6.3,"Remove Shower Head",null,"ea",1,null,null,"Rate only"]
[6.4,"Remove Shower Door/Unit",null,"ea",1,null,null,"Rate only"]
[]
[7," Repairs -Burst pipes and leaks"]
[7.1,"Burst Pipes Excavation of Trenches ( By hand)",null,"m²",1,null,null,"Rate only"]
[7.2,"Burst Pipes (Mechanical)",null,"Daily","Plant hire Rates"]
[8]
[8.1,"Remove uPVC Pipe 90,110,150 and 200mm",null,"ea",1,null,null,"Rate only"]
[8.2,"Remove Stainless Steel Clamp 90, 110, 150 and 200mm",null,"ea",1,null,null,"Rate only"]
[8.3,"Remove Conversion Clamp 90, 110 150 and 200mm",null,"ea",1,null,null,"Rate only"]
[]
[9," Rates for Work / Services: Paving"]
[9.1,"Uplift, remove and clean paving bricks",null,"ea",1,null,null,"Rate only"]
[9.2,"Uplift, Remove Concrete Curb/Kerb 900mm",null,"ea",1,null,null,"Rate only"]
[null,"Road Repairs"]
[9.3,"Remove existing Tar Road",null,"ea",1,null,null,"Rate only"]
[]
[10,"Rates for Work / Services: Building Works"]
[null,"• These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal must be used or the amount exceeding 1m³."]
[null,"• Prices for taking out of doors, windows, etc. shall include for removal of all beads, architraves, ironmongery, etc"]
[null,"• Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc. and making good floor and wall finishes to match existing"]
[null,"• Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied as maybe required"]
[null,"• Temporary barriers and screens are inclusive of the costs"]
[null,"• The demolition costs for reinforced concrete includes cutting off and removing reinforcement"]
[10.1,"a. Demolition Work"]
[null,"Concrete and brick work"]
["10.1.1","Demolish 230mm brick wall",null,"m²",1,null,null,"Rate only"]
["10.1.2","Demolish 115mm brick wall",null,"m²",1,null,null,"Rate only"]
["10.1.3","Demolish concrete wall",null,"m³",1,null,null,"Rate only"]
["10.1.4","Demolish reinforced concrete slab",null,"m³",1,null,null,"Rate only"]
["10.1.5","Demolish Strong room walls ",null,"m³",1,null,null,"Rate only"]
["10.1.6","Remove dry wall and make good",null,"m",1,null,null,"Rate only"]
["10.1.7","Demolish unreinforced concrete surface bed",null,"M3",1,null,null,"Rate only"]
[null,"Concrete work"]
["10.1.8","Remove existing plaster to brick/concrete surface",null,"m²",1,null,null,"Rate only"]
["10.1.9","Remove Air bricks : 215 x 140mm Terra cotta air brick replacing or installing new therefore breaking out",null,"each",1,null,null,"Rate only"]
[10.2,"b. Brick walls"]
["10.2.1","Remove window in brick wall",null,"m²",1,null,null,"Rate only"]
["10.2.2","Remove single steel door frame in brick wall",null,"each",1,null,null,"Rate only"]
["10.2.3","Remove Double steel door frame in brick wall",null,"each",1,null,null,"Rate only"]
[]
[11,"Rates for Work / Services: for Blinds"]
[null,"Horizontal wooden blinds  50mm Venetian Type:  Wooden Blinds:  Colour:  Mahogany/Cherry"]
[null,"a. Blinds"]
[11.1,"Remove Horizontal Wooden Blinds",null,"ea",1,null,null,"Rate only"]
[11.2,"Remove Vertical perforated aluminum blinds",null,"ea",1,null,null,"Rate only"]
[11.3,"Remove Vertical metallic blinds",null,"ea",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[12,"Rates for Work / Services: Flooring"]
[null,"• The labor, grout and sundries including cleaning must be allowed for in the commissioning amount as indicated "]
[null,"These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal may be used"]
[12.1,"a. Carpets"]
["12.1.1","Remove existing carpet tiles and prepare surface (see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.2","Remove existing stretch carpet and prepare surface (see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.3","Remove existing wood laminate flooring(see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.4","Floor strips aluminum 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.5","Floor strips wooden 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.6","Remove and Install skirting 75mm wooden",null,"m ",1,null,null,"Rate only"]
["12.1.7","Remove and Install quarter round",null,"m ",1,null,null,"Rate only"]
[12.2,"b. Tiling"]
["12.2.1","Break up and remove ceramic wall and floor tiles and make good (Prepare surface for tiling if required)",null,"m²",1,null,null,"Rate only"]
["12.2.2","Remove Screed +/- 10mm  Marley screed (Self Leveling)",null,"m²",1,null,null,"Rate only"]
["12.2.3","Remove Tile skirting",null,"m ",1,null,null,"Rate only"]
[]
[13," Rates for Work / Services: Fencing and Walling"]
[13.1,"a. Timber"]
["13.1.1","Remove 1.2m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.2","Remove 1.5m, High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.3","Remove 1.8m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.4","Remove 2.4m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
[13.2,"b. Galvinized Fencing"]
["13.2.1","Remove, 2.5 x 50mm diamond mesh fence",null,"m ",1,null,null,"Rate only"]
["13.2.2","Remove 2mm x 75mm x  3m x 600mm poles, Galvanized",null,"each",1,null,null,"Rate only"]
["13.2.3","Remove 2.5mm  x 50mm x 3 m High diamond mesh fence, ",null,"m ",1,null,null,"Rate only"]
["13.2.4","Remove 1.2m High Fence ",null,"m ",1,null,null,"Rate only"]
["13.2.5","Remove 1.5m High Fence",null,"m ",1,null,null,"Rate only"]
["13.2.6","Remove 1.8m High Fence",null,"m ",1,null,null,"Rate only"]
["13.2.7","Remove 2.4m High Fence",null,"m ",1,null,null,"Rate only"]
[13.3,"c.  Steel Palisade Fence Devils Fork and Other "]
["13.3.1","Remove 1.2m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.2","Remove 1.5m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.3","Remove 1.8m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.4","Remove 2.4m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.5","Remove 1.2m x 1800 mm double gate ",null,"each",1,null,null,"Rate only"]
["13.3.6","Remove 1.5m x 1 800 mm double gate",null,"each",1,null,null,"Rate only"]
["13.3.7","Remove 1.8m x 1 800 mm double gate ",null,"each",1,null,null,"Rate only"]
["13.3.8","Remove 2.4m x 1 800 mm double gate",null,"each",1,null,null,"Rate only"]
["13.3.9","Remove 1.5m x 3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.10","Remove 1.8m x  3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.11","Remove 2.4m x 3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.12","Remove Electric Fencing 11 Strings 100mm spacing",null,"p/m",1,null,null,"Rate only"]
["13.3.13","Razor Wire Flat wrap",null,"p/m",1,null,null,"Rate only"]
["13.3.14","Razor Wire Coils",null,"p/m",1,null,null,"Rate only"]
["13.3.15","Razor wire diamond mesh 1800mm height",null,"p/m",1,null,null,"Rate only"]
["13.3.16","Razor wire diamond mesh 2400mm height",null,"p/m",1,null,null,"Rate only"]
["13.3.17","Remove Clear VU fence panels 1.8/ 2.4/ 3m x 3m",null,"Unit",1,null,null,"Rate only"]
["13.3.18","Remove Clear VU poles 1.8m/2.4/3m",null,"Unit",1,null,null,"Rate only"]
[13.4,"d. Precast Walls Plain"]
["13.4.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.4.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.4.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.4.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[13.5,"e. Precast Brickwork Panels Single Sided"]
["13.5.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.5.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.5.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.5.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[13.6,"f. Precast Brickwork Panels Double Sided"]
["13.6.1","Remove 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.6.2","Remove 1.5m High",null,"m",1,null,null,"Rate only"]
["13.6.3","Remove 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.6.4","Remove 2.4m High",null,"m",1,null,null,"Rate only"]
[14," Rates for Work / Services: Iron Mongery"]
[null,"d. Carports"]
[14.1,"Remove Double Carports ",null,"Ea",1,null,null,"Rate only"]
[14.2,"Remove Single Carports ",null,"Ea",1,null,null,"Rate only"]
[14.3,"Remove Double Shade ports ",null,"Ea",1,null,null,"Rate only"]
[14.4,"Remove Single Shade Ports ",null,"Ea",1,null,null,"Rate only"]
[]
[15,"Rates for Work / Services: Carpentry and Joinery"]
[15.1,"a. Doors"]
["15.1.1","Remove Cat 2 safe door fitted with 3Way Combination Lock with two x 7 Lever locks",null,"Ea",1,null,null,"Rate only"]
["15.1.2","Remove Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Brick wall",null,"Ea",1,null,null,"Rate only"]
["15.1.3","Remove Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Strengthened Drywall",null,"Ea",1,null,null,"Rate only"]
["15.1.4","Remove Rocklike Class B Fire Double Door fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock",null,"Ea",1,null,null,"Rate only"]
["15.1.5","Remove Rocklike Class B Fire Door Single fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock",null,"Ea",1,null,null,"Rate only"]
["15.1.6","Remove Solid wooden door Single 815 x 2030 High ",null,"Ea",1,null,null,"Rate only"]
["15.1.7","Remove Solid wooden door Double 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.8","Remove Flash back V Joint Meranti Double door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.9","Remove Flash back V Joint Meranti Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.10","Remove Sol-core Masonite door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.11","Remove Sol-core Masonite Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.12","Remove Hollow Core Masonite door 815 x 2030",null,"Ea",1,null,null,"Rate only"]
["15.1.13","Remove Hollow Core Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.14","Remove Hollow Core Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.15","Remove  Roller Shutter Doors ",null,"Ea",1,null,null,"Rate only"]
["15.1.16","Remove sliding gates",null,"Ea",1,null,null,"Rate only"]
["15.1.17","Remove Steel sliding doors",null,"Ea",1,null,null,"Rate only"]
["15.1.18","Remove Wooden Panel Garage Door Single",null,"Ea",1,null,null,"Rate only"]
["15.1.19","Remove Wooden Panel Garage Door Double",null,"Ea",1,null,null,"Rate only"]
["15.1.20","Remove Roller Garage Doors Single",null,"Ea",1,null,null,"Rate only"]
["15.1.21","Remove Roller Garage Doors Double",null,"Ea",1,null,null,"Rate only"]
[15.2,"b. Door Lock and Handles"]
["15.2.1","Toilet Door lock Thumb Turn",null,"ea",1,null,null,"Rate only"]
["15.2.2","Remove door handles",null,"set",1,null,null,"Rate only"]
["15.2.3","Remove Heavy Duty 4 Lever Union Lock and Handles",null,"set",1,null,null,"Rate only"]
["15.2.4","Remove Aluminum Door handle with Square Back plate",null,"set",1,null,null,"Rate only"]
["15.2.5","Remove door handle on build- in Cupboard Push Button Lock",null,"ea",1,null,null,"Rate only"]
["15.2.6","Remove door handle on build- in Cupboard Plain",null,"ea",1,null,null,"Rate only"]
["15.2.7","Remove 4 lever lock Union,",null,"ea",1,null,null,"Rate only"]
["15.2.8","Remove 5 lever lock with Handles: Chub 3K70",null,"ea",1,null,null,"Rate only"]
["15.2.9","Remove 5 lever lock with Handles: Union Lock",null,"ea",1,null,null,"Rate only"]
["15.2.10","Remove 5 lever lock with Handles: Status Lock",null,"ea",1,null,null,"Rate only"]
["15.2.11","Remove 5 lever lock with Handles: Cisa Lock",null,"ea",1,null,null,"Rate only"]
["15.2.12","Remove Small Oval Cylinder Lock",null,"ea",1,null,null,"Rate only"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[]
["15.2.13","Remove Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.14","RemoveLarge Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.15","RemoveMechanical Code Lock, 14 pin type",null,"each",1,null,null,"Rate only"]
["15.2.16","Remove indoor Yale latch door lock",null,"each",1,null,null,"Rate only"]
["15.2.17","Remove indoor Deadbolt security lock Chub 3G110",null,"each",1,null,null,"Rate only"]
["15.2.18","Remove mild steel sliding door lock , hook type latch",null,"each",1,null,null,"Rate only"]
["15.2.19","Remove steel patio door lock, slim line design, 4 lever",null,"each",1,null,null,"Rate only"]
["15.2.20","Remove Double action 7L Security gate Lock",null,"each",1,null,null,"Rate only"]
[]
[15.3,"c.  Door accessories and spares"]
["15.3.1","Remove Hinges Brass heavy duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.2","Remove Hinges Brass light duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.3","Remove Hinges steel heavy duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.4","Remove Hinges steel light duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.5","Remove Hinges Brass light duty with recessed mounting holes, for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.6","Remove Hinges steel light duty with recessed mounting holes , for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.7","Remove Sliding bolts, brass, heavy duty, approx. 150 mm long",null,"each",1,null,null,"Rate only"]
["15.3.8","Remove Sliding bolts, brass, heavy duty, approx. 75 mm long",null,"each",1,null,null,"Rate only"]
["15.3.9","Remove Galvanized steel sliding bolt, approx. 150mm long",null,"each",1,null,null,"Rate only"]
[]
[15.4,"d. Ceilings"]
["15.4.1","Remove  76mm Cornish",null,"m²",1,null,null,"Rate only"]
["15.4.2","Remove suspended ceiling panels: 1200mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.3","Remove suspended ceiling panels: 600mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.4","Remove suspended ceiling panels: 500mm x 500mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.5","Remove  6,4mm gypsum plaster ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.6","Remove  6mm Nutec Ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.7","Remove Trapdoor 600 mm x600 mm",null,"m²",1,null,null,"Rate only"]
["15.4.8","Remove Build Bulk Head Ceiling",null,"m²",1,null,null,"Rate only"]
["15.4.9","Openings (to be made in ceilings)",null,"m²",1,null,null,"Rate only"]
[]
[15.5,"d. Built in Cupboards "]
["15.5.1","Remove Formica Top work surfaces 32mm",null,"m",1,null,null,"Rate only"]
["15.5.2","Remove cabinet locks: union",null,"ea",1,null,null,"Rate only"]
["15.5.3","Remove top section of kitchen unit",null,"m²",1,null,null,"Rate only"]
["15.5.4","Remove bottom section of kitchen unit",null,"m²",1,null,null,"Rate only"]
[]
[15.6,"e. Hangings"]
["15.6.1","Remove picture frame hooks and hang frame (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.2","Remove picture frame hooks (dry wall)",null,"each",1,null,null,"Rate only"]
["15.6.3","Remove notice / white board (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.4","Remove notice / white board (dry wall)",null,"each",1,null,null,"Rate only"]
{"$rows_empty":10}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[16]
[16.1,"a.  Glass",{"$nulls":5},"Rate only"]
["16.1.1","Remove Clear Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.2","Remove Clear Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.3","Remove Clear Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.4","Remove Clear Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.5","Remove Thick deep grey laminated safety glass 6.5mm",null,"m²",1,null,null,"Rate only"]
["16.1.6","Remove Bathroom Frosted Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.7","Remove Bathroom Frosted Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.8","Remove Bathroom Frosted Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.9","Remove Clear Safety Glass 6mm",null,"m²",1,null,null,"Rate only"]
["16.1.10","Remove Clear Safety Glass10mm",null,"m²",1,null,null,"Rate only"]
["16.1.11","Remove Georgian Wire Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.12","Remove Georgian Wire Glass   5mm             ",null,"m²",1,null,null,"Rate only"]
["16.1.13","Remove Shatterproof Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.14","Remove Shatterproof Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.15","Remove Bullet proof glass",null,"m²",1,null,null,"Rate only"]
["16.1.16","Remove Window laminate – frosted /decorative",null,"m²",1,null,null,"Rate only"]
["16.1.17","Remove Window laminate – solar reflective 75%",null,"m²",1,null,null,"Rate only"]
["16.1.18","Polishing of louver glass , all edges polished per louver glass panel",null,"Each",1,null,null,"Rate only"]
[16.2,"b.  Putty Replacement "]
["16.2.1","Remove and / or replace window putty",null,"m",1,null,null,"Rate only"]
[16.3,"c.  Mirrors"]
["16.3.1","Remove mirror non - salvage",null,"m²",1,null,null,"Rate only"]
["16.3.2","Remove mirror salvage",null,"m²",1,null,null,"Rate only"]
["16.3.3","4mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.4","5mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.5","6mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
[16.4,"d.  Aluminum Doors and Windows"]
["16.4.1","Remove Single door (frame mounted and cubicle mounted)",null,"Each",1,null,null,"Rate only"]
["16.4.2","Remove Double door",null,"Each",1,null,null,"Rate only"]
["16.4.3","Remove Floor spring",null,"Each",1,null,null,"Rate only"]
["16.4.4","Remove Top Spring",null,"Each",1,null,null,"Rate only"]
["16.4.5","Remove  sliding door (single)",null,"Each",1,null,null,"Rate only"]
["16.4.6","Remove sliding door (double)",null,"Each",1,null,null,"Rate only"]
["16.4.7","Remove  emergency exit door (single, push bar mechanism, 3point type or similar)",null,"Each",1,null,null,"Rate only"]
["16.4.8","Remove emergency exit door (double, dual push bar mechanism)",null,"Each",1,null,null,"Rate only"]
[16.5,"e.  Spares for Aluminum Doors and windows"]
["16.5.1","Remove Hinges Aluminium Heavy Duty with recessed mounting holes complete with heavy duty rivets",null,"Per Set",1,null,null,"Rate only"]
["16.5.2","Remove Continuous Aluminium hinge, heavy duty type with recessed mounting holes complete with heavy duty mounting kits / rivets 2.1m Long",null,"Per door",1,null,null,"Rate only"]
["16.5.3","Remove Piano Hinges -cubicles",null,"Per hinge",1,null,null,"Rate only"]
["16.5.4","Remove Belt driven hinges - sliding doors",null,"Per",1,null,null,"Rate only"]
["16.5.5","Remove Small Oval Cylinder Lock",null,"belt",1,null,null,"Rate only"]
["16.5.6","Remove Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.7","Remove Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.8","Remove 5 Cylinder Lever Lock Casing",null,"each",1,null,null,"Rate only"]
["16.5.9","Remove Mechanical Code Lock (14 pin type, for Aluminium door)",null,"each",1,null,null,"Rate only"]
["16.5.10","Remove Hydraulic/ pneumatic Door Closer standard",null,"each",1,null,null,"Rate only"]
["16.5.11","Remove Flush bolt",null,"each",1,null,null,"Rate only"]
["16.5.12","Remove Floor Springs Geze TS 500N",null,"each",1,null,null,"Rate only"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations",{"$nulls":5},"Rate only"]
["16.5.13","Remove 75mm x 2 mm Aluminium Skirting",null,"m",1,null,null,"Rate only"]
["16.5.14","Remove 75mm x 50mm x 2 mm Aluminium Profile",null,"m",1,null,null,"Rate only"]
["16.5.15","Remove 30mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.16","Remove 50mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.17","Remove Aluminium Door Handles",null,"ea",1,null,null,"Rate only"]
["16.5.18","Remove Aluminium Window Handles",null,"ea",1,null,null,"Rate only"]
["16.5.19","Remove Hinges for top hung Aluminium windows",null,"set",1,null,null,"Rate only"]
["16.5.20","Remove Hinges for offset mounted Aluminium windows, vertical swing",null,"set",1,null,null,"Rate only"]
["16.5.21","Remove Hinges for offset mounted Aluminium windows, horizontal swing",null,"set",1,null,null,"Rate only"]
[16.6,"f.  Aluminum Doors Manufacture, Supply and Fit (Standard)"]
["16.6.1","Remove 813mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.2","Remove 1200mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.3","Remove 1500mm x 2.1m high natural Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.4","Remove 1800mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.5","Remove 1800mm x 3.0m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.6","Remove 2400mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.7","Remove 3000mm x 2.1m high natural  Aluminium 4 section dual sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.8","Remove 6000 x 2.1m high natural Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)",null,"ea",1,null,null,"Rate only"]
["16.6.9","Remove 6000 x 2.1m high polished Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)",null,"ea",1,null,null,"Rate only"]
[16.7,"g.  Aluminum Doors Manufacture, Supply and Fit (SSA Specifications) "]
["16.7.1","Remove Single cubicle door 950mm x 2200mm Frame size:2100mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.2","Remove Single door 950mm x 2200mm Frame size:1161mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.3","Remove Single door 954mm x 2200mm Frame size:1152mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.4","Remove Double Door 1600mm x 2200mm Frame size:1900mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.5","Remove Automatic Double Sliding Door: Door size 1825mm x 2200mmFrame size 3944mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.6","Remove Automatic Double Sliding Door, Door size 2010mm x 2200mm Frame size 4071mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.7","Remove Double Door 1800mm x 2200mm Frame size:2100mm x 2350m",null,"ea",1,null,null,"Rate only"]
["16.7.8","Remove Double Door 1600mm x 2200mmFrame size:1901mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.9","Remove Automatic Double Sliding Door size 1350mm x 2200mm Frame size 2940mm x 2350mm",null,"ea",1,null,null,"Rate only"]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[16.8,"h.  Aluminum Windows Manufacture, Supply and Fit"]
["16.8.1","Remove 300 mm x 600 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.2","Remove 600 mm x 600mm mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.3","Remove 600 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.4","Remove 900 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.5","Remove 1200mm x 1200 mm high natural Aluminium window with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.6","Remove 300 mm x 600 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.7","Remove 600 mm x 600mm mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.8","Remove 600 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.9","Remove 900 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.10","Remove 1200mm x 1200 mm high polished Aluminium window with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
[16.9,"i.  Custom Aluminum products, Manufacture, Supply and Fit"]
["16.9.1","Custom window panel fitted in 30mm profile natural Aluminium  frame (Fixed Not Opening)",null,"ea",1,null,null,"Rate only"]
["16.9.2","Custom window panel fitted in 30mm profile polished Aluminium frame (Fixed Not Opening)",null,"ea",1,null,null,"Rate only"]
["16.9.3","Custom natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.4","Custom polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.5","Custom natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.6","Custom polished Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.7","Custom natural Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.8","Custom polished Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
[]
[17,"Table 16:  Rates for Work / Services Paintwork"]
[null,"No Alterations "]
[]
[18,"Table 17:  Rates for Work / Services – Waterproofing"]
[18.1,"a.  Waterproofing Tiled Roofs",null,"m² ",1,null,null,"Rate only"]
["18.1.1","Remove and repack tiles ",null,"m ",1,null,null,"Rate only"]
["18.1.2","Remove and repack valley tiles ",null,"m² ",1,null,null,"Rate only"]
["18.1.3","Remove tiles, replace underlay and repack "]
[18.2,"b.  Waterproofing Concrete Roof"]
["18.2.1","Strip and remove existing malthoid type membrane ",null,"m² ",1,null,null,"Rate only"]
[18.3,"c.  Waterproofing IBR or Corrugated Iron Roofs"]
[null,"No Alterations"]
[18.4,"d.  Waterproofing / insulation of surfaces with polymer products"]
[null,"No Alterations"]
{"$rows_empty":10}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Earthworks"]
[null,"Renovation of Kiepersol Building "]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[19,"Rates for Work / Services – Roofing"]
[19.1,"a.  Repairs and Installations Roof Materials"]
["19.1.1","Remove broken concrete roof tiles ",null,"each",1,null,null,"Rate only"]
["19.1.2","Remove  broken ridge tiles ",null,"each",1,null,null,"Rate only"]
["19.1.3","Remove loose concrete roof tiles ",null,"m²",1,null,null,"Rate only"]
["19.1.4","Remove  polyethylene underlay ",null,"m²",1,null,null,"Rate only"]
["19.1.5","Remove  Harvey tiles ",null,"each",1,null,null,"Rate only"]
["19.1.6","Remove  broken slate tiles ",null,"each",1,null,null,"Rate only"]
["19.1.7","Remove corrugated iron roof sheeting (Minimum 0.5 mm)",null,"m²",1,null,null,"Rate only"]
["19.1.8","Remove  corrugated iron roof ridging ",null,"m",1,null,null,"Rate only"]
["19.1.9","Remove  IBR roof sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.10","Remove  IBR ridging ",null,"m",1,null,null,"Rate only"]
["19.1.11","Remove  fiberglass sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.12","Remove polycarbonate sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.13","Remove galvanized valley gutters ",null,"m",1,null,null,"Rate only"]
["19.1.14","Remove fiber cement (Big Six) roof sheeting ",null,"m²",1,null,null,"Rate only"]
["19.1.15","Remove fiber cement (Big Six) ridging ",null,"m",1,null,null,"Rate only"]
["19.1.16","Remove 50mm x 76 mm purlins ",null,"m",1,null,null,"Rate only"]
["19.1.17","Remove 38mm x 38 mm battens ",null,"m",1,null,null,"Rate only"]
["19.1.18","Remove 150mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.19","Remove 225mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.20","Remove 300mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.21","Remove SA pine facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.22","Remove 200mm Nutec barge boards ",null,"m",1,null,null,"Rate only"]
[]
[20,"Table 19:  Rates for Work / Services: Thatching"]
[null,"All thatching must be calculated on the floor area including the overhangs"]
[20.1,"Remove existing thatch and cart away ",null,"m²",1,null,null,"Rate only"]
[20.2,"Remove existing thatch and structure and cart away ",null,"m²",1,null,null,"Rate only"]
[20.3,"Remove laths and battens only ",null,"m²",1,null,null,"Rate only"]
[20.4,"New Thatch covering complete ",null,"No Alt"]
[20.5,"Comb, Brush and minor repairs ",null,"No Alt"]
[20.6,"New timber structure (including laths and battens) ",null,"No Alt"]
[20.7,"Re-thatch 75 mm thick ",null,"No Alt"]
[20.8,"Remove grass ridging ",null,"m",1,null,null,"Rate only"]
[20.9,"Repairs to grass ridging ",null,"No Alt"]
[20.1,"Replace Fiberglas ridge ",null,"m",1,null,null,"Rate only"]
[20.11,"Repairs to fiberglass ridge ",null,"No Alt"]
[20.12,"Remove concrete ridging ",null,"m",1,null,null,"Rate only"]
[20.13,"Repairs to concrete ridging ",null,"No Alt"]
[20.14,"External treatment of thatch cover ",null,"No Alt"]
[20.15,"Internal treatment of thatch cover ",null,"No Alt"]
[20.16,"External and internal treatment of thatch cover ",null,"No Alt"]
[20.17,"New Internal treatment of thatch cover ",null,"No Alt"]
[20.18,"Bi annual inspection on all roof trusses"]

{"sheet":"Sheet2","index":2,"n_rows":18,"n_cols":8,"rows_kept":18,"flags":["formulas_cached_only"]}
[]
[]
[]
[13.4,"d. Precast Walls Plain"]
["13.4.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.4.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.4.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.4.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[13.5,"e. Precast Brickwork Panels Single Sided"]
["13.5.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.5.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.5.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.5.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[13.6,"f. Precast Brickwork Panels Double Sided"]
["13.6.1","Remove 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.6.2","Remove 1.5m High",null,"m",1,null,null,"Rate only"]
["13.6.3","Remove 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.6.4","Remove 2.4m High",null,"m",1,null,null,"Rate only"]

{"sheet":"Building BOQ (2)","index":3,"n_rows":3216,"n_cols":9,"rows_kept":3216,"merged":[[4,1,4,2],[6,1,6,2],[8,1,8,2],[10,1,10,2],[12,1,12,2],[14,1,14,2],[15,1,15,2],[18,1,18,2],[20,1,20,2],[22,1,22,2],[40,1,40,2],[44,1,44,2],[46,1,46,2],[52,1,52,2],[56,1,56,2],[58,1,58,2],[62,1,62,2],[64,1,64,2],[66,1,66,2],[70,1,70,2],[74,1,74,2],[77,1,77,2],[79,1,79,2],[81,1,81,2],[83,1,83,2],[95,1,95,2],[97,1,97,2],[99,1,99,2],[101,1,101,2],[105,1,105,2],[109,1,109,2],[113,1,113,2],[117,1,117,2],[121,1,121,2],[125,1,125,2],[129,1,129,2],[150,1,150,2],[152,1,152,2],[156,1,156,2],[160,1,160,2],[164,1,164,2],[168,1,168,2],[172,1,172,2],[176,1,176,2],[180,1,180,2],[184,1,184,2],[186,1,186,2],[188,1,188,2],[194,1,194,2],[198,1,198,2],[202,1,202,2],[206,1,206,2],[225,1,225,2],[227,1,227,2],[229,1,229,2],[231,1,231,2],[233,1,233,2],[235,1,235,2],[239,1,239,2],[241,1,241,2],[245,1,245,2],[247,1,247,2],[249,1,249,2],[251,1,251,2],[253,1,253,2],[255,1,255,2],[257,1,257,2],[259,1,259,2],[261,1,261,2],[265,1,265,2],[283,1,283,2],[285,1,285,2],[287,1,287,2],[289,1,289,2],[291,1,291,2],[293,1,293,2],[295,1,295,2],[297,1,297,2],[301,1,301,2],[303,1,303,2],[311,1,311,2],[323,1,323,2],[325,1,325,2],[327,1,327,2],[331,1,331,2],[353,1,353,2],[355,1,355,2],[359,1,359,2],[361,1,361,2],[363,1,363,2],[367,1,367,2],[369,1,369,2],[371,1,371,2],[373,1,373,2],[375,1,375,2],[377,1,377,2],[379,1,379,2],[381,1,381,2],[387,1,387,2],[389,1,389,2],[391,1,391,2],[409,1,409,2],[411,1,411,2],[413,1,413,2],[415,1,415,2],[417,1,417,2],[425,1,425,2],[431,1,431,2],[435,1,435,2],[437,1,437,2],[439,1,439,2],[441,1,441,2],[443,1,443,2],[445,1,445,2],[447,1,447,2],[449,1,449,2],[453,1,453,2],[455,1,455,2],[457,1,457,2],[474,1,474,2],[478,1,478,2],[482,1,482,2],[486,1,486,2],[488,1,488,2],[490,1,490,2],[496,1,496,2],[502,1,502,2],[506,1,506,2],[510,1,510,2],[514,1,514,2],[518,1,518,2],[520,1,520,2],[548,1,548,2],[552,1,552,2],[558,1,558,2],[560,1,560,2],[562,1,562,2],[566,1,566,2],[570,1,570,2],[574,1,574,2],[578,1,578,2],[582,1,582,2],[586,1,586,2],[590,1,590,2],[594,1,594,2],[596,1,596,2],[598,1,598,2],[602,1,602,2],[606,1,606,2],[626,1,626,2],[628,1,628,2],[630,1,630,2],[632,1,632,2],[634,1,634,2],[636,1,636,2],[662,1,662,2],[691,1,691,2],[693,1,693,2],[695,1,695,2],[697,1,697,2],[699,1,699,2],[705,1,705,2],[707,1,707,2],[711,1,711,2],[713,1,713,2],[717,1,717,2],[719,1,719,2],[723,1,723,2],[725,1,725,2],[739,1,739,2],[741,1,741,2],[743,1,743,2],[747,1,747,2],[749,1,749,2],[753,1,753,2],[755,1,755,2],[759,1,759,2],[761,1,761,2],[765,1,765,2],[767,1,767,2],[786,1,786,2],[788,1,788,2],[790,1,790,2],[794,1,794,2],[796,1,796,2],[800,1,800,2],[802,1,802,2],[806,1,806,2],[808,1,808,2],[831,1,831,2],[834,1,834,2],[836,1,836,2],[838,1,838,2],[840,1,840,2],[842,1,842,2],[844,1,844,2],[846,1,846,2],[853,1,853,2],[856,1,856,2],[890,4,890,5],[895,1,895,2],[972,1,972,2],[974,1,974,2],[978,1,978,2],[980,1,980,3],[982,1,982,2],[984,1,984,2],[985,1,985,2],[986,1,986,2],[988,1,988,2],[989,1,989,2],[990,1,990,2],[992,1,992,2],[1007,1,1007,2],[1009,1,1009,2],[1011,1,1011,2],[1012,1,1012,2],[1015,1,1015,2],[1018,1,1018,2],[1020,1,1020,2],[1024,1,1024,2],[1032,1,1032,2],[1095,1,1095,2],[1096,1,1096,2],[1097,1,1097,2],[1098,1,1098,2],[1099,1,1099,2],[1100,1,1100,2],[1136,1,1136,2],[1137,1,1137,2],[1439,1,1439,2],[1440,1,1440,2],[1441,1,1441,2],[1442,1,1442,2],[1443,1,1443,2],[1444,1,1444,2],[1445,1,1445,2],[1446,1,1446,2],[1447,1,1447,2],[1448,1,1448,2],[1450,1,1450,2],[1451,1,1451,2],[1452,1,1452,2],[1453,1,1453,2],[1454,1,1454,2],[1455,1,1455,2],[1456,1,1456,2],[1457,1,1457,2],[1566,4,1566,5],[1571,1,1571,2],[1634,1,1634,2],[1640,1,1640,2],[1642,1,1642,2],[1646,1,1646,2],[1662,1,1662,2],[1663,1,1663,2],[1664,1,1664,2],[1666,1,1666,2],[1692,1,1692,2],[1695,1,1695,2],[1798,1,1798,2],[1799,1,1799,2],[1800,1,1800,2],[1801,1,1801,2],[1802,1,1802,2],[1803,1,1803,2],[2801,4,2801,5],[2806,1,2806,2],[2905,1,2905,2],[2909,1,2909,2],[2915,1,2915,2],[2916,1,2916,2],[2917,1,2917,2],[2918,1,2918,2],[2919,1,2919,2],[2920,1,2920,2],[2921,1,2921,2],[2922,1,2922,2],[2923,1,2923,2],[2924,1,2924,2],[2925,1,2925,2],[2926,1,2926,2],[2927,1,2927,2],[2928,1,2928,2],[2929,1,2929,2],[2931,1,2931,2],[2934,1,2934,2],[2935,1,2935,2],[2936,1,2936,2],[2973,4,2973,5],[3120,4,3120,5],[3168,0,3168,7],[3169,0,3169,7],[3170,0,3170,7]],"flags":["formulas_cached_only"]}
["Item No.","SECTION  1 ",null,"Unit","Qty","Rate ",null,"Amount"]
[]
[null,"BILL  NO. 1 "]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES "]
[]
[null,"The JBCC Series 2000 Minor Works Agreement (March 2014  edition 5.1) prepared by the Joint Building Contract Committee  shall be the applicable building agreement, amended as  hereinafter described "]
[]
[null,"The ASAQS Preliminaries (November 2007 edition) published  by the Association of South African Quantity Surveyors for use  with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these bills of quantities  "]
[]
[null,"Contractors are referred to the abovementioned documents for  the full intent and meaning of each clause thereof"]
[]
[null,"These clauses are hereinafter referred to by clause number  and heading only. Where standard clauses or alternatives are  not entirely applicable to this contract such modifications,  corrections or supplements as will apply are given under each  relevant clause heading and such modifications, corrections or  supplements shall take precedence notwithstanding anything  contrary contained in the abovementioned documents "]
[]
[null,"Where any item is not relevant to this specific contract such item is marked N/A, signifying not applicable "]
[]
[null,"PREAMBLES FOR TRADES  "]
[]
[null,"The Model Preambles for Trades (2008 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of  items fully described in the said Model Preambles will be entertained"]
[]
[null,"Supplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles shall take precedence over the provisions of the said Model preambles"]
[]
[null,"The contractor's prices for all items throughout these bills of quantities must take account of and include for all of the  obligations, requirements and specifications given in the said Model Preambles and in any supplementary preambles  "]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[null,"PRICING OF PRELIMINARIES  "]
[]
[null,"Should the contractor select Option A in terms of sub clause 3.2.1 in the Contract Data - Contractor to Employer (CE) for the purpose of adjustment of these preliminaries, the amount entered into the amount column in these preliminaries is to be divided into one or more of the three categories provided namely Fixed (F), Value Related (V) and Time Related (T) "]
[]
[null,"GENERAL "]
[]
[null,"The contractor's prices for all items thought-out these bills of quantities must take into account SANS 10400-F: 2010 Edition 3 part F site operations available of SABS."]
[]
[null,"SECTION A - PRINCIPAL BUILDING  AGREEMENT "]
[]
[null,"Definitions "]
[]
[1,"Clause 1.0 - Definitions and interpretation "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Objective and preparations   "]
[]
[2,"Clause 2.0 - Offer acceptance and performance obligations  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3,"Clause 3.0 - Documents  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Clause 3 is deemed to be amended by the following: "]
[]
[null,"3.2.1 The construction guarantee shall be in the JBCC  Variable Construction Guarantee Format"]
[]
[4,"Clause 4.0 - Design responsibility  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[5,"Clause 5.0 - Employer's agents "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[6,"Clause 6.0 - Contractor's site representative  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7,"Clause 7.0 - Compliance with laws and regulations  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Qty",null,null,"Amount"]
[null,"Clause 7 is deemed to be amended by the addition of the following clause:"]
[]
[7.1,"Without limiting the generality of the provisions of  clause 7.0 of the agreement, the contractor's  attention is drawn to the provisions of the Construction  Regulations, 2003 issued in terms of the Occupational  Health and Safety Act, 1993 in which it is specifically  stated that the employer shall prepare a documented  health and safety specification for the works and that  the employer shall ensure that the contractor has  made provision for the cost of health and safety  measures during the execution of the works.  The  contractor shall price opposite this item for compliance  with the act and the regulations and the provisions of  the aforementioned health and safety specification"]
[]
[7.2,"Without limiting the generality of the provisions of Clause 7.0 of the agreement the Contractors attention is drawn to the provisions of the SSA Emergency Plan and Risk Management requirements, e.g. Risk Assessments, Environmental Awareness Plan and on- and off-site Emergency Evacuation Plans may be required. The Contractor shall price opposite this item for compliance with requirements."]
[]
[7.3,"Without limiting the generality of the provisions of Clause 7.0 of the agreement the Contractors attention is drawn to the provisions of the Rehabilitation Plan requirements. The Contractor shall   price opposite this item for compliance with requirements."]
[]
[8,"Clause 8.0 - Works risk "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9,"Clause 9.0 - Indemnities  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[10,"Clause 10.0 - General insurances "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11,"Clause 11.0 - Special insurances  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[12,"Clause 12.0 - Effecting insurances  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[13,"Clause 13.0 - Assignment "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14,"Clause 14.0 - Security "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[null,"Execution  "]
[]
[15,"Clause 15.0 - Preparation for and execution of the works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[16,"Clause 16.0 - Site and access"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[17,"Clause 17.0 - Contract instructions "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[18,"Clause 18.0 - Setting out of the works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[19,"Clause 19.0 - Temporary works and plant"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[20,"Clause 19.2 - Notice boards"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[21,"Clause 20.0 - Nominated subcontractors  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[22,"Clause 21.0 - Selected subcontractors  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[23,"Clause 22.0 - Employer's direct contractors"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[24,"Clause 23.0 - Contractor's domestic subcontractors "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Completion  "]
[]
[25,"Clause 24.0 - Practical completion"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[26,"Clause 25.0 - Works completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[27,"Clause 26.0 - Final completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[28,"Clause 27.0 - Latent defects liability period  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[29,"Clause 28.0 - Sectional completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[30,"Clause 29.0 - Revision of date for practical completion  "]
[]
[null,"The removal and replacement of materials and/or workmanship which do not conform to specification or drawing shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value (Clause 29.3) "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[31,"Clause 30.0 - Penalty for late or non-completion  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Payment   "]
[]
[32,"Clause 31.0 is deemed to be amended to read as follows:"]
[]
[" ","The employer shall pay the contractor the amount certified in an interim payment certificate within Thirty (30) calendar days following the date of the interim payment certificate. Payment shall be subject to the contractor giving the Project Manager a  valid tax invoice for the amount due "]
[]
[33,"Clause 31.0 - Interim payment ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"The inclusion of materials and goods stored off site in the amount authorised for payment shall be at the sole discretion of the managers and such inclusion shall only be considered upon the provision, by the contractor, of an approved bank. "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[34,"Clause 32.0 - Adjustment to the contract value "]
[]
[null,"All fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor Where prices are submitted by the contractor or n/s subcontractor during the progress of the works in respect of contract instructions or in regard to a  claim under the terms of the contract and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the project manager wish to accept any such prices prior to the certificate, it shall be in writing issue of the final payment"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[35,"Clause 33.0 - Recovery of expense and loss  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[36,"Clause 34.0 - Final account and final payment "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[37,"Clause 35.0 - Payment to other parties "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[]
[null,"Termination "]
[]
[38,"Clause 36.0 - Termination by employer - contractor's default  ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[39,"Clause 37.0 - Termination by employer - loss and damage  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[40,"Clause 38.0 - Termination by contractor - employer's default  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[41,"Clause 39.0 - Termination - cessation of the works  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Dispute   "]
[]
[42,"Clause 40.0 - Settlement of disputes "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Contract agreement "]
[]
[43,"Clause 41.0 - Post tender provisions  ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[44,"Clause 42.0 - Contractual agreement ",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"The required information of the contracting parties and the amount of the accepted contract sum shall be inserted in the contractual agreement for signature of the agreement by the contracting parties  "]
[]
[1,"CONTRACTING AND OTHER PARTIES"]
[]
[1.1,"Employer: SSA"]
[]
[null,"Physical address:"]
[null,"Corner of Joe Nthlantla Road and old Delmas Road"]
[null,"Rietvalei"]
[null,"Pretoria"]
[]
[]
[1.2,"Interest of project team in the project "]
[]
[null,"The team have no interest in this project apart from their professional interest."]
[]
[2,"CONTRACT DATA - CONTRACT AND SITE INFORMATION "]
[]
[2.1,"Works Description"]
[]
[null,"The scope of work shall include (but is not limited to) the following: Appointment of a Contractor for General Building Maintenance "]
[]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[2.2,"Site Description"]
[null,"01 Delmas road "]
[null,"Rietvalei "]
[null,"Pretoria East "]
[]
[2.3,"Date on which possession of the site is intended to  be given: on 60 days from submission of tender"]
[]
[2.4,"Period for the commencement of the works after the contractor takes possession of the site: 1 Day "]
[]
[2.5,"Completion in sections is required"]
[]
[2.6,"Waiver of the contractor's lien or right of continuing  possession is required but SSA does not provide a Payment Guarantee. YES"]
[]
[2.7,"Defined restrictions to the site area - Public toilets may be used as long as premises are left clean, no washing or changing allowed. No sleeping on site"]
[]
[2.8,"Geotechnical investigation of the site has been undertaken N/A"]
[]
[2.9,"Existing premises occupied. NO"]
[]
[3,"CONTRACT DATE - INSURANCES AND SECURITIES"]
[]
[3.1,"Contract works insurance to be effected by the Contractor: For the amount of: Contract Sum + 25 % With deductibles payable by the Contractor to the amount N/A"]
[]
[null,"SASRIA insurance required:                 By Contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.2,"Supplementary/ special insurance to be effected by Contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.3,"Public liability insurance to be effected by - Contractor (As per signed Service Level Agreement)"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[3.4,"Support insurance to be effected N/A"]
[]
[3.5,"Special insurance to be effected N/A"]
[]
[4,"CONTRACT DATA - PRACTICAL COMPLETION DATES AND PENALTIES "]
[]
[4.1,"Intended date of practical completion is: 60 days from issue of order."]
[]
[4.2,"Intended date of practical completion where sectional completion is required and the penalty per calendar day for the works in sections: N/A and the penalty per calendar day for the works as a whole is: N/A"]
[]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[5,"CONTRACT DATA - DOCUMENTS AND GENERAL "]
[]
[5.1,"Construction document copies to be supplied to the  contractor free of charge"]
[]
[5.2,"The priced document may be used as a specification of materials and goods"]
[]
[5.3,"The contractor shall provide a schedule of rates where applicable "]
[]
[5.4,"On acceptance of the tender the priced document  is to be submitted within 1 Working days",null,"No"]
[]
[null,"SECTION B -  PRELIMINARIES  "]
[]
[6,"DEFINITIONS AND INTERPRETATION "]
[]
[6.1,"Clause 1.0 - Definitions and interpretation  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7,"DOCUMENTS"]
[]
[7.1,"Clause 2.1 - Checking of documents  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7.2,"Clause 2.2* - Provisional bills of quantities"]
[]
[null,"These bills of quantities are re-measurable in its totality. no claim or adjustment of rates will be considered to increase or  decrease in quantities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[7.3,"Clause 2.3 - Availability of construction documentation "]
[]
[null,"The budgetary allowances and selected/nominated subcontract amounts allocated for subsequent trades included in this document will be separately procured, based on multiple procurement of selected/nominated subcontractors during the construction period"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8,"PREVIOUS WORK AND ADJOINING PROPERTIES"]
[]
[8.1,"Clause 3.1 - Previous work - dimensional accuracy  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8.2,"Clause 3.2 - Previous work - defects  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[8.3,"Clause 3.3 - Inspection of adjoining properties "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[9,"SAMPLES, SHOP DRAWINGS AND MANUFACTURER'S INSTRUCTIONS"]
[]
[9.1,"Clause 4.1 - Samples of materials  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.2,"Clause 4.2 - Workmanship samples  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.3,"Clause 4.3 - Shop drawings "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[9.4,"Clause 4.4 - Compliance with manufacturer's instructions "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[10,"DEPOSIT AND FEES"]
[]
[10.1,"Clause 5.1 - Deposits and fees  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item"]
[{"$nulls":4},{"v":1,"d":"1.00"},null,null,0]
[11,"TEMPORARY SERVICES"]
[]
[11.1,"Clause 6.1 - Water "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.2,"Clause 6.2 - Electricity "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.3,"Clause 6.3 - Telecommunication facilities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[11.4,"Clause 6.4 - Ablution facilities"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[12,"PRIME COST AMOUNTS"]
[]
[12.1,"Clause 7.1 - Responsibility for prime cost amounts "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":14}
[null,"Total Carried to Collection",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity",null,null,"Amounts"]
[13,"SPECIAL ATTENDANCE ON N/S SUBCONTRACTORS"]
[]
[13.1,"Clause 8.1 - Special attendance "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14,"GENERAL"]
[]
[14.1,"Clause 9.1 - Protection of the works"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.2,"Clause 9.2 - Protection/isolation of existing/section ally occupied works "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.3,"Clause 9.3 - Security of the works"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.4,"Clause 9.4 - Notice before covering work  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.5,"Clause 9.5 - Disturbance  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.6,"Clause 9.6 - Environmental disturbance "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.7,"Clause 9.7 - Works cleaning and clearing"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.8,"Clause 9.8 - Vermin "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.9,"Clause 9.9 - Rubbish removals "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
["14.10","Clause 9.9 - Overhand work "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.11,"Clause 9.10 - Instruction manuals and guarantees"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.12,"Clause 9.11 - As built information"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[14.13,"Clause 9.12 - Tenant installations"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[15,"SCHEDULE OF VARIABLES "]
[]
[null,"Information necessary for elections and completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder Where no information is given it shall mean that no specific requirements are expected or that the clause is not relevant to this specific contract  "]
[]
[15.1,"Provisional bills of quantities [clause 2.2] The quantities are provisional YES"]
[]
[15.2,"Availability of construction documentation [clause 2.3] Construction documentation is complete"]
[]
[15.3,"Previous work - dimensional [clause 3.1] accuracy N/A "]
[]
[15.4,"Previous work - defects [clause 3.2] N/A "]
[]
[15.5,"Inspection of adjoining properties [clause 3.3] N/A"]
[]
[15.6,"Water [clause 7.2]"]
[null,"Option A (by contractor)                                        ","No"]
[null,"Option B (by employer - free of charge)    ","Yes"]
[null,"Option C (by employer - metered)    ","No"]
[]
[15.7,"Electricity [clause 7.3]"]
[null,"Option A (by contractor)     ","Yes"]
[null,"Option B (by employer - free of charge)    ","No"]
[null,"Option C (by employer - metered)    ","No"]
[]
[15.8,"Telecommunications [clause 7.4]"]
[null,"Telephone "]
[null,"Contractor"]
[null,"Facsimile"]
[null,"Contractor"]
[null,"E-mail"]
[null,"Contractor"]
[]
[15.9,"Ablution facilities [clause 7.5]"]
[null,"Option A (by contractor)  ","No"]
[null,"Option B (by employer)    ","Yes"]
[]
["15.10","Protection of the works [clause 9.1]"]
[]
[15.11,"Protection/isolation of existing/section ally  occupied works  [clause 9.2] Protection/isolation is  required YES "]
[]
[15.12,"Disturbance [clause 9.5]"]
{"$rows_empty":14}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[null,"The following paragraphs shall be added to this sub-clause:"]
[]
[null,"The contractor shall take all necessary measures to minimise noise. Such measures shall include inter alia, the use of 'silent' compressors and the like."]
[]
[null,"All work shall be executed without unacceptable and unreasonable dust, noise, vibrations, nuisance, inconvenience, annoyance and the like to the public, others other property. Any delays, stoppages and the like arising from or in order to comply with the above will not constitute grounds for an adjustment to the construction period or contract value 'whatsoever'"]
[]
[null,"The contractor indemnifies the employer against and accepts entire responsibilities for any claims, costs, damages and all other loss of whatsoever nature or delays which may arise on the above grounds."]
[]
[null,"The contractor shall take every precaution to protect buildings, etc. on adjoining sites against damage and shall be held solely responsible for any damage to persons or property caused by inadequate precautions."]
[]
[null,"SECTION  C - SPECIFIC PRELIMINARIES "]
[]
[16,"SITE INSTRUCTIONS"]
[]
[null,"Instructions issued on site are to be recorded in triplicate in a site instruction book which is to be maintained on site by the contractor"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[17,"PROPRIETARY BRANDED PRODUCTS"]
[]
[null,"The contractor shall take delivery of, handle, store, use apply and/or fix all proprietary branded products in  strict accordance with the manufacturers instruction after consultation with the manufacturers authorised representative."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[18,"OVERTIME"]
[]
[null,"Should overtime be required to be worked for any reason whatsoever, the costs of such overtime are to be borne by the contractor unless the project manager has specifically authorised in writing, prior to the execution thereof, that costs for such overtime are to be borne by the employer."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[19,"AS BUILT DRAWINGS"]
[]
[null,"The position of construction breaks and the extent of individual concrete pours are to be recorded by the contractor on the structural engineer's drawings and are to be submitted to the project manager and the structural engineer for their records"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[20,"SITE INSTRUCTIONS"]
[]
[null,"Site instructions issued on site are to be recorded in a Site Instruction Book which is to be maintained on site by the contractor. This shall be a carbon triplicate book numbered consecutively which may be used only for the issue of site instructions"]
[]
[null,"Site instructions directed at the contractor and various sub-contractors may be issued only by the project manager or any of the professional consultants so authorised by the project manager and must be addressed firstly for the attention of the contractor, for further distribution. Copies of all site instructions issued are to be submitted to the project manager and the quantity surveyor at the following site meeting or not later than 21days after issue."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[21,"LABOUR RECORD"]
[]
[null,"At the end of each week the contractor shall provide the project manager with a written record, in schedule form, reflecting the number and description of tradesmen and labourers employed by him and all sub-contractors on the works each day."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[22,"PLANT RECORD"]
[]
[null,"At the end of each week the contractor shall provide the project manager with a written record, in schedule form, reflecting the number, type and capacity of all plant, excluding hand tools, currently used on the works."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[23,"NON CESSION OF MONIES"]
[]
[null,"The contractor shall not cede nor assign his rights or claims to any monies due or to become due under this contract"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[24,"CONTRACTOR TO BE RESPONSIBLE"]
[]
[null,"The contractor acknowledges that the principal objective of his appointment is his expert knowledge in the execution of the scope of work of this Contract. The Contractor shall therefore be solely responsible for all aspects of the construction of the Works including but not limited to management, resourcing, programming, co-ordination, etc. all as required for the type of project described within the time limits and quality standards specified."]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[25,"INSTALLATION OF FURNITURE, EQUIPMENT, ETC"]
[]
[null,"During the progress of the contract the employer reserves the right to send onto, install, commission and test in the works any furniture, furnishings, fitments, machinery, equipment and installation, etc., not allowed for in this contract. The contractor shall permit the employer and his representatives and contractors entry to the works for this purpose. No financial allowance shall be made to the contractor (except as specifically allowed for in these bills of quantities) on account of the presence of any of the abovementioned workmen and their materials other than reasonable costs actually incurred and approved by the Project Manager "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[26,"PRICING OF BILLS"]
[]
[null,"Tenderers are to allow opposite each item for all costs associated therewith. All prices are to include, unless otherwise stated, for all materials, fabrication, conveyance and delivery, unloading, storing, unpacking, hoisting, labour, setting, fitting and fixing in position, cutting and waste (except where measured in accordance with the Standard System Of Measurement), patterns, models and templates, plant, temporary works, returning of packings, duties, taxes, imports, establishment charges, overheads, profit and all other obligation arising out of the contract. "]
[]
[null,"Items left unpriced will be deemed to be covered in prices against other items throughout these bills of quantities and no claim for any extras arising out of the tenderer's omission to price any item will be entertained."]
[]
[27,"UNAUTHORISED PERSONS ON SITE"]
[]
[null,"The contractor shall at all times strictly exclude all unauthorised persons from the site. No workmen are to be allowed to sleep on the premises. "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[28,"DAYWORKS"]
[]
[null,"Where in the opinion of the quantity surveyor any extra work cannot  properly be measured or valued at contract rates, the contractor will be allowed day work prices calculated at the rates and principles stated elsewhere in these bills of quantities. Failure by the contractor to properly complete the day work schedule will be deemed to be  acceptance of the quantity surveyor's discretion as to what applicable day work rates to be used.  "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
{"$rows_empty":12}
[null,"Total Carried to Collection",{"$nulls":5},0]
[]
[]
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[29,"OCCUPATIONAL HEALTH AND SAFETY"]
[]
[null,"It is a requirement of this contract that the works are to be executed in strict accordance with the requirements of the Occupation Health And Safety Act. The successful contractor will therefor have to comply with all aspect related thereto and all costs associated therewith are deemed to be included in the contract price. No claims of any kind whatsoever will be entertained due to the contractor's non-compliance with the requirements of the act, the same being enforced onto the contractor. The successful contractor will be issued with a safety specification from the employer in terms of the act. "]
[null,"Yearley Cost"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Personal Protective Equipment (PPE)"]
[]
[null,"The contractor shall provide and maintain the appropriate personal protective equipment to all employees (maximum of 15 people) for the duration of the contract "]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[null,"Medicals"]
[]
[null,"The contractor shall carried out medical check-up on employees (maximum of 15 people) for those involved in the following operations"]
[]
[null,"F:………......... V:............................T:...........................",null,"Item",{"v":1,"d":"1.00"},null,null,0]
[]
[]
[]
[]
[null,"SUMMARY OF CATEGORIES "]
[]
[null,"Category : Fixed   R.........................................................",{"$nulls":5},0]
[]
[]
[null,"Category : Value   R.........................................................",{"$nulls":5},0]
[]
[]
[]
[null,"Category : Time    R........................................................."]
{"$rows_empty":16}
[null,"Total Carried to Collection",{"$nulls":5},0]
{"$rows_empty":8}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION  1 "]
[]
[null,"BILL  NO. 1 "]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES "]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,1,null,null,0]
[{"$nulls":4},2,null,null,0]
[{"$nulls":4},3,null,null,0]
[{"$nulls":4},4,null,null,0]
[{"$nulls":4},5,null,null,0]
[{"$nulls":4},6,null,null,0]
[{"$nulls":4},7,null,null,0]
[{"$nulls":4},8,null,null,0]
[{"$nulls":4},9,null,null,0]
[{"$nulls":4},10,null,null,0]
[{"$nulls":4},11,null,null,0]
[{"$nulls":4},12,null,null,0]
[{"$nulls":4},13,null,null,0]
[{"$nulls":4},14,null,null,0]
[{"$nulls":4},15,null,null,0]
{"$rows_empty":33}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 1 "]
[null,"Bill No. 1"]
[null,"Building Agreement and Preliminaries "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Quantity","Rate",null,"Amounts"]
[null,"SECTION 2 "]
[]
[null,"BILL 1"]
[]
[null,"ALTERATIONS"]
[]
[null,"ALTERATIONS PROVISIONAL"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles refers \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. "]
[]
[null,"Contractors are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard"]
[]
[null,"View site"]
[]
[null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[null,"Explosives"]
[]
[null,"No explosives whatsoever may be used for demolition purposes unless otherwise stated"]
[]
[null,"General"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the project manager. All undue noise is to be prevented and should the use of jack hammers, vibrators or similar plant be considered necessary by the Contractor, then prior permission must be obtained from the project manager.  Except where necessary for building operations, workmen must not enter the existing occupied buildings."]
[]
[null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the project manager"]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 2 "]
[null,"BILL 1"]
[null,"ALTERATIONS"]
[]
[null,"Note: All alterations and removal of existing work should be approved by the Architect before any work can be carried out by the appointed contractor or sub-contractor"]
[]
[null,"OLD MATERIAL TO BECOME PROPERTY OF THE CONTRACTOR"]
[null,"Old materials from alterations, accept where described to be re-used or handed over, become  the property of the contractor who must allow credit for some in the final Summary"]
[]
[null,"OLD MATERIAL TO CARTED  AWAY"]
[null,"Old materials from alterations, accept where described as to be re-used or handed over, as well as all rubbish, etc. must be regularly carted from the site and not allowed to accumulate on or around the site"]
[]
[null,"OLD MATERIAL NOT TO BE RE-USED"]
[null,"None of the old materials are to used for new work except where specifically described as being set aside for  re-use"]
[]
[null,"Provide all necessary protection, hoarding, etc. to ensure stability of all structures during alteration works. Any damage to the structures as well as the remaining portions of the building and the rectification there of will be for the contractor's account."]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[1,"Removing of items such as doors, partitioning, ceilings  etc. and make good or replace as per direction "]
[]
[1.1,"Remove rubble from site  exceeding 1m³-hand loaded",null,"m³",1]
[]
[1.2,"Removal of rubble exceeding 1m³ in skip waste bins",null,"Per Bin",6]
[]
[null,"Rates For Work / Services: Plumbing "]
[]
[null,"(Note: Alterations refer to the removal of existing fittings/materials etc. and the replacement of such with same.) Where it implies removal/decommissioning or new installation this will be stated as a separate item). "]
[]
[2,"General Maintenance and Repairs"]
[]
[2.1,"Clean storm water channels and pipes",null,"m",1,null,null,"Rate only"]
[]
[2.2,"Clean Manholes",null,"Each",1,null,null,"Rate only"]
[]
[2.3,"Clean gutter and down pipes",null,"m",1,null,null,"Rate only"]
[]
[3,"Replace Cistern"]
[]
[3.1,"Remove Cistern All Tipes ( Low, High Level and Closed Couple)",null,"ea",1,null,null,"Rate only"]
[]
[4," Geysers"]
[4.1,"Remove under counter Geyser 10 / 15 Lt (Kwikot)",null,"ea",1,null,null,"Rate only"]
[]
["4..2","Remove 100Lt/150 Lt/200 LTGeyser (Kwikot) complete",null,"ea",1,null,null,"Rate only"]
[]
[4.3,"Remove  Kwikot  boilers with drain cock 10 L/15L",null,"ea",1,null,null,"Rate only"]
[]
[5,"Plumbing "]
[5.1,"Remove  hand wash basin complete: (Vaal Hibiscus Basin or similar)",null,"ea",1,null,null,"Rate only"]
[5.2,"Remove toilet complete (IQWA Beta Toilet Suite or similar)",null,"ea",1,null,null,"Rate only"]
[5.3,"Remove toilet pan ",null,"ea",1,null,null,"Rate only"]
[5.4,"Remove toilet water tank",null,"ea",1,null,null,"Rate only"]
[5.5,"Remove toilet water Pan",null,"ea",1,null,null,"Rate only"]
[5.6,"Remove Stainless Steel Urinal",null,"ea",1,null,null,"Rate only"]
[5.7,"Remove Toilet Seats Standard Wooden/White",null,"ea",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[]
[6,"Bathroom"]
[6.1,"Remove existing taps",null,"ea",1,null,null,"Rate only"]
[6.2,"Remove stainless steel sink within cabinet 1.8 (hinge door)",null,"ea",1,null,null,"Rate only"]
[6.3,"Remove Shower Head",null,"ea",1,null,null,"Rate only"]
[6.4,"Remove Shower Door/Unit",null,"ea",1,null,null,"Rate only"]
[]
[7," Repairs -Burst pipes and leaks"]
[7.1,"Burst Pipes Excavation of Trenches ( By hand)",null,"m²",1,null,null,"Rate only","Provincial Sums "]
[7.2,"Burst Pipes (Mechanical)",null,"Daily","Plant hire Rates"]
[8]
[8.1,"Remove uPVC Pipe 90,110,150 and 200mm",null,"ea",1,null,null,"Rate only"]
[8.2,"Remove Stainless Steel Clamp 90, 110, 150 and 200mm",null,"ea",1,null,null,"Rate only"]
[8.3,"Remove Conversion Clamp 90, 110 150 and 200mm",null,"ea",1,null,null,"Rate only"]
[]
[9," Rates for Work / Services: Paving"]
[9.1,"Uplift, remove and clean paving bricks",null,"ea",1,null,null,"Rate only"]
[9.2,"Uplift, Remove Concrete Curb/Kerb 900mm",null,"ea",1,null,null,"Rate only"]
[null,"Road Repairs"]
[9.3,"Remove existing Tar Road",null,"ea",1,null,null,"Rate only"]
[]
[10,"Rates for Work / Services: Building Works"]
[null,"• These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal must be used or the amount exceeding 1m³."]
[null,"• Prices for taking out of doors, windows, etc. shall include for removal of all beads, architraves, ironmongery, etc"]
[null,"• Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc. and making good floor and wall finishes to match existing"]
[null,"• Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied as maybe required"]
[null,"• Temporary barriers and screens are inclusive of the costs"]
[null,"• The demolition costs for reinforced concrete includes cutting off and removing reinforcement"]
[10.1,"a. Demolition Work"]
[null,"Concrete and brick work"]
["10.1.1","Demolish 230mm brick wall",null,"m²",1,null,null,"Rate only"]
["10.1.2","Demolish 115mm brick wall",null,"m²",1,null,null,"Rate only"]
["10.1.3","Demolish concrete wall",null,"m³",1,null,null,"Rate only"]
["10.1.4","Demolish reinforced concrete slab",null,"m³",1,null,null,"Rate only"]
["10.1.5","Demolish Strong room walls ",null,"m³",1,null,null,"Rate only"]
["10.1.6","Remove dry wall and make good",null,"m",1,null,null,"Rate only"]
["10.1.7","Demolish unreinforced concrete surface bed",null,"M3",1,null,null,"Rate only"]
[null,"Concrete work"]
["10.1.8","Remove existing plaster to brick/concrete surface",null,"m²",1,null,null,"Rate only"]
["10.1.9","Remove Air bricks : 215 x 140mm Terra cotta air brick replacing or installing new therefore breaking out",null,"each",1,null,null,"Rate only"]
[10.2,"b. Brick walls"]
["10.2.1","Remove window in brick wall",null,"m²",1,null,null,"Rate only"]
["10.2.2","Remove single steel door frame in brick wall",null,"each",1,null,null,"Rate only"]
["10.2.3","Remove Double steel door frame in brick wall",null,"each",1,null,null,"Rate only"]
[]
[11,"Rates for Work / Services: for Blinds"]
[null,"Horizontal wooden blinds  50mm Venetian Type:  Wooden Blinds:  Colour:  Mahogany/Cherry"]
[null,"a. Blinds"]
[11.1,"Remove Horizontal Wooden Blinds",null,"ea",1,null,null,"Rate only"]
[11.2,"Remove Vertical perforated aluminum blinds",null,"ea",1,null,null,"Rate only"]
[11.3,"Remove Vertical metallic blinds",null,"ea",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[12,"Rates for Work / Services: Flooring"]
[null,"• The labor, grout and sundries including cleaning must be allowed for in the commissioning amount as indicated "]
[null,"These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal may be used"]
[12.1,"a. Carpets"]
["12.1.1","Remove existing carpet tiles and prepare surface (see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.2","Remove existing stretch carpet and prepare surface (see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.3","Remove existing wood laminate flooring(see*** note)",null,"m²",1,null,null,"Rate only"]
["12.1.4","Floor strips aluminum 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.5","Floor strips wooden 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.6","Remove and Install skirting 75mm wooden",null,"m ",1,null,null,"Rate only"]
["12.1.7","Remove and Install quarter round",null,"m ",1,null,null,"Rate only"]
[12.2,"b. Tiling"]
["12.2.1","Break up and remove ceramic wall and floor tiles and make good (Prepare surface for tiling if required)",null,"m²",1,null,null,"Rate only"]
["12.2.2","Remove Screed +/- 10mm  Marley screed (Self Leveling)",null,"m²",1,null,null,"Rate only"]
["12.2.3","Remove Tile skirting",null,"m ",1,null,null,"Rate only"]
[]
[13," Rates for Work / Services: Fencing and Walling"]
[13.1,"a. Timber"]
["13.1.1","Remove 1.2m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.2","Remove 1.5m, High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.3","Remove 1.8m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
["13.1.4","Remove 2.4m High Split pole fencing",null,"m ",1,null,null,"Rate only"]
[13.2,"b. Galvinized Fencing"]
["13.2.1","Remove, 2.5 x 50mm diamond mesh fence",null,"m ",1,null,null,"Rate only"]
["13.2.2","Remove 2mm x 75mm x  3m x 600mm poles, Galvanized",null,"each",1,null,null,"Rate only"]
["13.2.3","Remove 2.5mm  x 50mm x 3 m High diamond mesh fence, ",null,"m ",1,null,null,"Rate only"]
["13.2.4","Remove 1.2m High Fence ",null,"m ",1,null,null,"Rate only"]
["13.2.5","Remove 1.5m High Fence",null,"m ",1,null,null,"Rate only"]
["13.2.6","Remove 1.8m High Fence",null,"m ",1,null,null,"Rate only"]
["13.2.7","Remove 2.4m High Fence",null,"m ",1,null,null,"Rate only"]
[13.3,"c.  Steel Palisade Fence Devils Fork and Other "]
["13.3.1","Remove 1.2m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.2","Remove 1.5m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.3","Remove 1.8m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.4","Remove 2.4m x 900 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.5","Remove 1.2m x 1800 mm double gate ",null,"each",1,null,null,"Rate only"]
["13.3.6","Remove 1.5m x 1 800 mm double gate",null,"each",1,null,null,"Rate only"]
["13.3.7","Remove 1.8m x 1 800 mm double gate ",null,"each",1,null,null,"Rate only"]
["13.3.8","Remove 2.4m x 1 800 mm double gate",null,"each",1,null,null,"Rate only"]
["13.3.9","Remove 1.5m x 3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.10","Remove 1.8m x  3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.11","Remove 2.4m x 3000 mm single gate ",null,"each",1,null,null,"Rate only"]
["13.3.12","Remove Electric Fencing 11 Strings 100mm spacing",null,"p/m",1,null,null,"Rate only"]
["13.3.13","Razor Wire Flat wrap",null,"p/m",1,null,null,"Rate only"]
["13.3.14","Razor Wire Coils",null,"p/m",1,null,null,"Rate only"]
["13.3.15","Razor wire diamond mesh 1800mm height",null,"p/m",1,null,null,"Rate only"]
["13.3.16","Razor wire diamond mesh 2400mm height",null,"p/m",1,null,null,"Rate only"]
["13.3.17","Remove Clear VU fence panels 1.8/ 2.4/ 3m x 3m",null,"Unit",1,null,null,"Rate only"]
["13.3.18","Remove Clear VU poles 1.8m/2.4/3m",null,"Unit",1,null,null,"Rate only"]
[13.4,"d. Precast Walls Plain"]
["13.4.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.4.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.4.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.4.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[13.5,"e. Precast Brickwork Panels Single Sided"]
["13.5.1","Remove Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.5.2","Remove Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.5.3","Remove Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.5.4","Remove Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[13.6,"f. Precast Brickwork Panels Double Sided"]
["13.6.1","Remove 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.6.2","Remove 1.5m High",null,"m",1,null,null,"Rate only"]
["13.6.3","Remove 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.6.4","Remove 2.4m High",null,"m",1,null,null,"Rate only"]
[14," Rates for Work / Services: Iron Mongery"]
[null,"d. Carports"]
[14.1,"Remove Double Carports ",null,"Ea",1,null,null,"Rate only"]
[14.2,"Remove Single Carports ",null,"Ea",1,null,null,"Rate only"]
[14.3,"Remove Double Shade ports ",null,"Ea",1,null,null,"Rate only"]
[14.4,"Remove Single Shade Ports ",null,"Ea",1,null,null,"Rate only"]
[]
[15,"Rates for Work / Services: Carpentry and Joinery"]
[15.1,"a. Doors"]
["15.1.1","Remove Cat 2 safe door fitted with 3Way Combination Lock with two x 7 Lever locks",null,"Ea",1,null,null,"Rate only"]
["15.1.2","Remove Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Brick wall",null,"Ea",1,null,null,"Rate only"]
["15.1.3","Remove Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Strengthened Drywall",null,"Ea",1,null,null,"Rate only"]
["15.1.4","Remove Rocklike Class B Fire Double Door fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock",null,"Ea",1,null,null,"Rate only"]
["15.1.5","Remove Rocklike Class B Fire Door Single fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock",null,"Ea",1,null,null,"Rate only"]
["15.1.6","Remove Solid wooden door Single 815 x 2030 High ",null,"Ea",1,null,null,"Rate only"]
["15.1.7","Remove Solid wooden door Double 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.8","Remove Flash back V Joint Meranti Double door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.9","Remove Flash back V Joint Meranti Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.10","Remove Sol-core Masonite door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.11","Remove Sol-core Masonite Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.12","Remove Hollow Core Masonite door 815 x 2030",null,"Ea",1,null,null,"Rate only"]
["15.1.13","Remove Hollow Core Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.14","Remove Hollow Core Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.15","Remove  Roller Shutter Doors ",null,"Ea",1,null,null,"Rate only"]
["15.1.16","Remove sliding gates",null,"Ea",1,null,null,"Rate only"]
["15.1.17","Remove Steel sliding doors",null,"Ea",1,null,null,"Rate only"]
["15.1.18","Remove Wooden Panel Garage Door Single",null,"Ea",1,null,null,"Rate only"]
["15.1.19","Remove Wooden Panel Garage Door Double",null,"Ea",1,null,null,"Rate only"]
["15.1.20","Remove Roller Garage Doors Single",null,"Ea",1,null,null,"Rate only"]
["15.1.21","Remove Roller Garage Doors Double",null,"Ea",1,null,null,"Rate only"]
[15.2,"b. Door Lock and Handles"]
["15.2.1","Toilet Door lock Thumb Turn",null,"ea",1,null,null,"Rate only"]
["15.2.2","Remove door handles",null,"set",1,null,null,"Rate only"]
["15.2.3","Remove Heavy Duty 4 Lever Union Lock and Handles",null,"set",1,null,null,"Rate only"]
["15.2.4","Remove Aluminum Door handle with Square Back plate",null,"set",1,null,null,"Rate only"]
["15.2.5","Remove door handle on build- in Cupboard Push Button Lock",null,"ea",1,null,null,"Rate only"]
["15.2.6","Remove door handle on build- in Cupboard Plain",null,"ea",1,null,null,"Rate only"]
["15.2.7","Remove 4 lever lock Union,",null,"ea",1,null,null,"Rate only"]
["15.2.8","Remove 5 lever lock with Handles: Chub 3K70",null,"ea",1,null,null,"Rate only"]
["15.2.9","Remove 5 lever lock with Handles: Union Lock",null,"ea",1,null,null,"Rate only"]
["15.2.10","Remove 5 lever lock with Handles: Status Lock",null,"ea",1,null,null,"Rate only"]
["15.2.11","Remove 5 lever lock with Handles: Cisa Lock",null,"ea",1,null,null,"Rate only"]
["15.2.12","Remove Small Oval Cylinder Lock",null,"ea",1,null,null,"Rate only"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[]
["15.2.13","Remove Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.14","RemoveLarge Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.15","RemoveMechanical Code Lock, 14 pin type",null,"each",1,null,null,"Rate only"]
["15.2.16","Remove indoor Yale latch door lock",null,"each",1,null,null,"Rate only"]
["15.2.17","Remove indoor Deadbolt security lock Chub 3G110",null,"each",1,null,null,"Rate only"]
["15.2.18","Remove mild steel sliding door lock , hook type latch",null,"each",1,null,null,"Rate only"]
["15.2.19","Remove steel patio door lock, slim line design, 4 lever",null,"each",1,null,null,"Rate only"]
["15.2.20","Remove Double action 7L Security gate Lock",null,"each",1,null,null,"Rate only"]
[]
[15.3,"c.  Door accessories and spares"]
["15.3.1","Remove Hinges Brass heavy duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.2","Remove Hinges Brass light duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.3","Remove Hinges steel heavy duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.4","Remove Hinges steel light duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.5","Remove Hinges Brass light duty with recessed mounting holes, for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.6","Remove Hinges steel light duty with recessed mounting holes , for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.7","Remove Sliding bolts, brass, heavy duty, approx. 150 mm long",null,"each",1,null,null,"Rate only"]
["15.3.8","Remove Sliding bolts, brass, heavy duty, approx. 75 mm long",null,"each",1,null,null,"Rate only"]
["15.3.9","Remove Galvanized steel sliding bolt, approx. 150mm long",null,"each",1,null,null,"Rate only"]
[]
[15.4,"d. Ceilings"]
["15.4.1","Remove  76mm Cornish",null,"m²",1,null,null,"Rate only"]
["15.4.2","Remove suspended ceiling panels: 1200mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.3","Remove suspended ceiling panels: 600mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.4","Remove suspended ceiling panels: 500mm x 500mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.5","Remove  6,4mm gypsum plaster ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.6","Remove  6mm Nutec Ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.7","Remove Trapdoor 600 mm x600 mm",null,"m²",1,null,null,"Rate only"]
["15.4.8","Remove Build Bulk Head Ceiling",null,"m²",1,null,null,"Rate only"]
["15.4.9","Openings (to be made in ceilings)",null,"m²",1,null,null,"Rate only"]
[]
[15.5,"d. Built in Cupboards "]
["15.5.1","Remove Formica Top work surfaces 32mm",null,"m",1,null,null,"Rate only"]
["15.5.2","Remove cabinet locks: union",null,"ea",1,null,null,"Rate only"]
["15.5.3","Remove top section of kitchen unit",null,"m²",1,null,null,"Rate only"]
["15.5.4","Remove bottom section of kitchen unit",null,"m²",1,null,null,"Rate only"]
[]
[15.6,"e. Hangings"]
["15.6.1","Remove picture frame hooks and hang frame (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.2","Remove picture frame hooks (dry wall)",null,"each",1,null,null,"Rate only"]
["15.6.3","Remove notice / white board (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.4","Remove notice / white board (dry wall)",null,"each",1,null,null,"Rate only"]
{"$rows_empty":10}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[16]
[16.1,"a.  Glass",{"$nulls":5},"Rate only"]
["16.1.1","Remove Clear Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.2","Remove Clear Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.3","Remove Clear Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.4","Remove Clear Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.5","Remove Thick deep grey laminated safety glass 6.5mm",null,"m²",1,null,null,"Rate only"]
["16.1.6","Remove Bathroom Frosted Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.7","Remove Bathroom Frosted Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.8","Remove Bathroom Frosted Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.9","Remove Clear Safety Glass 6mm",null,"m²",1,null,null,"Rate only"]
["16.1.10","Remove Clear Safety Glass10mm",null,"m²",1,null,null,"Rate only"]
["16.1.11","Remove Georgian Wire Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.12","Remove Georgian Wire Glass   5mm             ",null,"m²",1,null,null,"Rate only"]
["16.1.13","Remove Shatterproof Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.14","Remove Shatterproof Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.15","Remove Bullet proof glass",null,"m²",1,null,null,"Rate only"]
["16.1.16","Remove Window laminate – frosted /decorative",null,"m²",1,null,null,"Rate only"]
["16.1.17","Remove Window laminate – solar reflective 75%",null,"m²",1,null,null,"Rate only"]
["16.1.18","Polishing of louver glass , all edges polished per louver glass panel",null,"Each",1,null,null,"Rate only"]
[16.2,"b.  Putty Replacement "]
["16.2.1","Remove and / or replace window putty",null,"m",1,null,null,"Rate only"]
[16.3,"c.  Mirrors"]
["16.3.1","Remove mirror non - salvage",null,"m²",1,null,null,"Rate only"]
["16.3.2","Remove mirror salvage",null,"m²",1,null,null,"Rate only"]
["16.3.3","4mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.4","5mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.5","6mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
[16.4,"d.  Aluminum Doors and Windows"]
["16.4.1","Remove Single door (frame mounted and cubicle mounted)",null,"Each",1,null,null,"Rate only"]
["16.4.2","Remove Double door",null,"Each",1,null,null,"Rate only"]
["16.4.3","Remove Floor spring",null,"Each",1,null,null,"Rate only"]
["16.4.4","Remove Top Spring",null,"Each",1,null,null,"Rate only"]
["16.4.5","Remove  sliding door (single)",null,"Each",1,null,null,"Rate only"]
["16.4.6","Remove sliding door (double)",null,"Each",1,null,null,"Rate only"]
["16.4.7","Remove  emergency exit door (single, push bar mechanism, 3point type or similar)",null,"Each",1,null,null,"Rate only"]
["16.4.8","Remove emergency exit door (double, dual push bar mechanism)",null,"Each",1,null,null,"Rate only"]
[16.5,"e.  Spares for Aluminum Doors and windows"]
["16.5.1","Remove Hinges Aluminium Heavy Duty with recessed mounting holes complete with heavy duty rivets",null,"Per Set",1,null,null,"Rate only"]
["16.5.2","Remove Continuous Aluminium hinge, heavy duty type with recessed mounting holes complete with heavy duty mounting kits / rivets 2.1m Long",null,"Per door",1,null,null,"Rate only"]
["16.5.3","Remove Piano Hinges -cubicles",null,"Per hinge",1,null,null,"Rate only"]
["16.5.4","Remove Belt driven hinges - sliding doors",null,"Per",1,null,null,"Rate only"]
["16.5.5","Remove Small Oval Cylinder Lock",null,"belt",1,null,null,"Rate only"]
["16.5.6","Remove Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.7","Remove Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.8","Remove 5 Cylinder Lever Lock Casing",null,"each",1,null,null,"Rate only"]
["16.5.9","Remove Mechanical Code Lock (14 pin type, for Aluminium door)",null,"each",1,null,null,"Rate only"]
["16.5.10","Remove Hydraulic/ pneumatic Door Closer standard",null,"each",1,null,null,"Rate only"]
["16.5.11","Remove Flush bolt",null,"each",1,null,null,"Rate only"]
["16.5.12","Remove Floor Springs Geze TS 500N",null,"each",1,null,null,"Rate only"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations",{"$nulls":5},"Rate only"]
["16.5.13","Remove 75mm x 2 mm Aluminium Skirting",null,"m",1,null,null,"Rate only"]
["16.5.14","Remove 75mm x 50mm x 2 mm Aluminium Profile",null,"m",1,null,null,"Rate only"]
["16.5.15","Remove 30mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.16","Remove 50mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.17","Remove Aluminium Door Handles",null,"ea",1,null,null,"Rate only"]
["16.5.18","Remove Aluminium Window Handles",null,"ea",1,null,null,"Rate only"]
["16.5.19","Remove Hinges for top hung Aluminium windows",null,"set",1,null,null,"Rate only"]
["16.5.20","Remove Hinges for offset mounted Aluminium windows, vertical swing",null,"set",1,null,null,"Rate only"]
["16.5.21","Remove Hinges for offset mounted Aluminium windows, horizontal swing",null,"set",1,null,null,"Rate only"]
[16.6,"f.  Aluminum Doors Manufacture, Supply and Fit (Standard)"]
["16.6.1","Remove 813mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.2","Remove 1200mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.3","Remove 1500mm x 2.1m high natural Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.4","Remove 1800mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.5","Remove 1800mm x 3.0m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.6","Remove 2400mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.7","Remove 3000mm x 2.1m high natural  Aluminium 4 section dual sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.8","Remove 6000 x 2.1m high natural Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)",null,"ea",1,null,null,"Rate only"]
["16.6.9","Remove 6000 x 2.1m high polished Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)",null,"ea",1,null,null,"Rate only"]
[16.7,"g.  Aluminum Doors Manufacture, Supply and Fit (SSA Specifications) "]
["16.7.1","Remove Single cubicle door 950mm x 2200mm Frame size:2100mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.2","Remove Single door 950mm x 2200mm Frame size:1161mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.3","Remove Single door 954mm x 2200mm Frame size:1152mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.4","Remove Double Door 1600mm x 2200mm Frame size:1900mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.5","Remove Automatic Double Sliding Door: Door size 1825mm x 2200mmFrame size 3944mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.6","Remove Automatic Double Sliding Door, Door size 2010mm x 2200mm Frame size 4071mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.7","Remove Double Door 1800mm x 2200mm Frame size:2100mm x 2350m",null,"ea",1,null,null,"Rate only"]
["16.7.8","Remove Double Door 1600mm x 2200mmFrame size:1901mm x 2350mm",null,"ea",1,null,null,"Rate only"]
["16.7.9","Remove Automatic Double Sliding Door size 1350mm x 2200mm Frame size 2940mm x 2350mm",null,"ea",1,null,null,"Rate only"]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[16.8,"h.  Aluminum Windows Manufacture, Supply and Fit"]
["16.8.1","Remove 300 mm x 600 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.2","Remove 600 mm x 600mm mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.3","Remove 600 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.4","Remove 900 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.5","Remove 1200mm x 1200 mm high natural Aluminium window with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.6","Remove 300 mm x 600 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.7","Remove 600 mm x 600mm mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.8","Remove 600 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.9","Remove 900 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.8.10","Remove 1200mm x 1200 mm high polished Aluminium window with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
[16.9,"i.  Custom Aluminum products, Manufacture, Supply and Fit"]
["16.9.1","Custom window panel fitted in 30mm profile natural Aluminium  frame (Fixed Not Opening)",null,"ea",1,null,null,"Rate only"]
["16.9.2","Custom window panel fitted in 30mm profile polished Aluminium frame (Fixed Not Opening)",null,"ea",1,null,null,"Rate only"]
["16.9.3","Custom natural Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.4","Custom polished Aluminium window with 30mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.5","Custom natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.6","Custom polished Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.7","Custom natural Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.9.8","Custom polished Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
[]
[17,"Table 16:  Rates for Work / Services Paintwork"]
[null,"No Alterations "]
[]
[18,"Table 17:  Rates for Work / Services – Waterproofing"]
[18.1,"a.  Waterproofing Tiled Roofs",null,"m² ",1,null,null,"Rate only"]
["18.1.1","Remove and repack tiles ",null,"m ",1,null,null,"Rate only"]
["18.1.2","Remove and repack valley tiles ",null,"m² ",1,null,null,"Rate only"]
["18.1.3","Remove tiles, replace underlay and repack "]
[18.2,"b.  Waterproofing Concrete Roof"]
["18.2.1","Strip and remove existing malthoid type membrane ",null,"m² ",1,null,null,"Rate only"]
[18.3,"c.  Waterproofing IBR or Corrugated Iron Roofs"]
[null,"No Alterations"]
[18.4,"d.  Waterproofing / insulation of surfaces with polymer products"]
[null,"No Alterations"]
{"$rows_empty":10}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 1"]
[null,"Alterations"]
[19,"Rates for Work / Services – Roofing"]
[19.1,"a.  Repairs and Installations Roof Materials"]
["19.1.1","Remove broken concrete roof tiles ",null,"each",1,null,null,"Rate only"]
["19.1.2","Remove  broken ridge tiles ",null,"each",1,null,null,"Rate only"]
["19.1.3","Remove loose concrete roof tiles ",null,"m²",1,null,null,"Rate only"]
["19.1.4","Remove  polyethylene underlay ",null,"m²",1,null,null,"Rate only"]
["19.1.5","Remove  Harvey tiles ",null,"each",1,null,null,"Rate only"]
["19.1.6","Remove  broken slate tiles ",null,"each",1,null,null,"Rate only"]
["19.1.7","Remove corrugated iron roof sheeting (Minimum 0.5 mm)",null,"m²",1,null,null,"Rate only"]
["19.1.8","Remove  corrugated iron roof ridging ",null,"m",1,null,null,"Rate only"]
["19.1.9","Remove  IBR roof sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.10","Remove  IBR ridging ",null,"m",1,null,null,"Rate only"]
["19.1.11","Remove  fiberglass sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.12","Remove polycarbonate sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.13","Remove galvanized valley gutters ",null,"m",1,null,null,"Rate only"]
["19.1.14","Remove fiber cement (Big Six) roof sheeting ",null,"m²",1,null,null,"Rate only"]
["19.1.15","Remove fiber cement (Big Six) ridging ",null,"m",1,null,null,"Rate only"]
["19.1.16","Remove 50mm x 76 mm purlins ",null,"m",1,null,null,"Rate only"]
["19.1.17","Remove 38mm x 38 mm battens ",null,"m",1,null,null,"Rate only"]
["19.1.18","Remove 150mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.19","Remove 225mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.20","Remove 300mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.21","Remove SA pine facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.22","Remove 200mm Nutec barge boards ",null,"m",1,null,null,"Rate only"]
[]
[20,"Table 19:  Rates for Work / Services: Thatching"]
[null,"All thatching must be calculated on the floor area including the overhangs"]
[20.1,"Remove existing thatch and cart away ",null,"m²",1,null,null,"Rate only"]
[20.2,"Remove existing thatch and structure and cart away ",null,"m²",1,null,null,"Rate only"]
[20.3,"Remove laths and battens only ",null,"m²",1,null,null,"Rate only"]
[20.4,"New Thatch covering complete ",null,"No Alt"]
[20.5,"Comb, Brush and minor repairs ",null,"No Alt"]
[20.6,"New timber structure (including laths and battens) ",null,"No Alt"]
[20.7,"Re-thatch 75 mm thick ",null,"No Alt"]
[20.8,"Remove grass ridging ",null,"m",1,null,null,"Rate only"]
[20.9,"Repairs to grass ridging ",null,"No Alt"]
[20.1,"Replace Fiberglas ridge ",null,"m",1,null,null,"Rate only"]
[20.11,"Repairs to fiberglass ridge ",null,"No Alt"]
[20.12,"Remove concrete ridging ",null,"m",1,null,null,"Rate only"]
[20.13,"Repairs to concrete ridging ",null,"No Alt"]
[20.14,"External treatment of thatch cover ",null,"No Alt"]
[20.15,"Internal treatment of thatch cover ",null,"No Alt"]
[20.16,"External and internal treatment of thatch cover ",null,"No Alt"]
[20.17,"New Internal treatment of thatch cover ",null,"No Alt"]
[20.18,"Bi annual inspection on all roof trusses"]
{"$rows_empty":21}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"Section 2"]
[]
[null,"Bill 1"]
[]
[null,"Alterations"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,17,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},18,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},19,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},20,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},21,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},22,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},23,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},24,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},25,{"v":0,"d":"0.00"},null,0]
[{"$nulls":4},26,{"v":0,"d":"0.00"},null,0]
{"$rows_empty":36}
[null,"Total Carried to Summary ",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 1"]
[null,"Alterations"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 2"]
[]
[null,"BILL NO 2"]
[]
[null,"GENERAL Building Maintennce"]
[]
[" ","MATERIAL SCHEDULE SUPPLY AND INSTALL"]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles see \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. Tenderers are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard."]
[]
[null,"All costs must be inclusive of material supply, delivery, installation, profit, and attendance"]
[]
[null,"CPAP ADJUSTMENT "]
[]
[null,"Unless otherwise stated, items shall be deemed to fall into Lump Sum Work Group 180 for Contract Price Adjustment Provisions "]
[]
[null,"SUPPLEMENTARY PREABLES "]
[]
[null,"General "]
[]
[null,"All supplied materials must be SABS approved"]
[]
[]
[null,"MATERIAL SCHEDULE "]
[]
[]
[null,"General Maintenance and Repairs"]
[]
[null,"Rates For Work / Services:  "]
[]
[null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the project manager"]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)"]
{"$rows_empty":13}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 2"]
[null,"BILL NO 2"]
[null,"GENERAL Building Maintennce"]
[null,"MATERIAL SUPPLY AND INSTALL"]
[]
[1,"Removing of items such as doors, partitioning, ceilings  etc. and make good or replace as per direction "]
[null,"Rates part with Alterations"]
[]
[2,"Rates For Work / Services: Plumbing "]
[]
[2.1,"General Maintenance and Repairs"]
["2.1.1","Clean storm water channels and pipes",null,"Alterations"]
["2.1.2","Clean Manholes",null,"Alterations"]
["2.1.3","Build new manhole (1m x 1m x 1m) including cast iron cover.m",null,"ea",1,null,null,"Rate only"]
["2.1.4","Clean gutter and down pipes",null,"Alterations"]
[]
[3,"Replace Cistern (Marterial PC Items Price Labour only)"]
[3.1,"Low level",null,"ea",1,null,null,"Rate only"]
[3.2,"High Level",null,"ea",1,null,null,"Rate only"]
[3.3,"Closed Couple",null,"ea",1,null,null,"Rate only"]
[3.4,"Replace seal kit for flush master",null,"ea",1,null,null,"Rate only"]
[3.5,"Replace  Junior flush master valve",null,"ea",1,null,null,"Rate only"]
[3.6,"Replace toilet flush master",null,"ea",1,null,null,"Rate only"]
[3.7,"Replace 50mm PVC Waste Pipe",null,"ea",1,null,null,"Rate only"]
[3.8,"Replace 50mm PVC Junction",null,"ea",1,null,null,"Rate only"]
[3.9,"Replace 50mm PVC Elbow/ bend",null,"ea",1,null,null,"Rate only"]
[3.1,"Replace 50mm PVC Straight Connector",null,"ea",1,null,null,"Rate only"]
[3.11,"Replace 32mm chrome Urinal bottle with PVC P-Trap",null,"ea",1,null,null,"Rate only"]
[3.12,"Replace 40mm chrome Urinal bottle with PVC P-Trap",null,"ea",1,null,null,"Rate only"]
[]
[4," Geysers"]
[4.1,"Replace under counter Geyser 10 / 15 Lt (Kwikot)","Material PC","ea",1,null,null,"Rate only"]
[4.2,"Install under counter Geyser 10 / 15 Lt (Kwikot)","Material PC","ea",1,null,null,"Rate only"]
[4.3,"Replace 100Lt/150 Lt/200 LT Geyser (Kwikot) complete","Material PC","ea",1,null,null,"Rate only"]
[4.4,"Install 100Lt/150 Lt/200 LT Geyser (Kwikot) complete","Material PC","ea",1,null,null,"Rate only"]
[4.5,"Supply and Install geyser insulation blanket",null,"ea",1,null,null,"Rate only"]
[4.6,"Supply and Install heat return pump (SABS Approved)","Material PC","ea",1]
[4.7,"Replace  Kwikot  boilers with drain cock 10 L/15L","Material PC","ea",1]
[4.8,"Supply and install Kwikot  boilers with drain cock 10 L/15L","Material PC","ea",1]
["4..2","Repair Kwikot boiler ( general)","Material PC","ea",1,null,null,"Rate only"]
[]
[5,"Installations and Replacements"]
[5.1,"Install new hand wash basin complete: (Vaal Hibiscus Basin or similar)","Material PC","ea",1,null,null,"Rate only"]
[5.2,"Replace  hand wash basin complete: (Vaal Hibiscus Basin or similar)","Material PC","ea",1,null,null,"Rate only"]
[5.3,"Install toilet complete (IQWA Beta Toilet Suite or similar)","Material PC","ea",1,null,null,"Rate only"]
[5.4,"Replace toilet complete (IQWA Beta Toilet Suite or similar)","Material PC","ea",1,null,null,"Rate only"]
[5.5,"Replace toilet pan","Material PC","ea",1,null,null,"Rate only"]
[5.6,"Replace toilet water tank to match the existing","Material PC","ea",1,null,null,"Rate only"]
[5.7,"Install Stainless Steel Urinal","Material PC","ea",1,null,null,"Rate only"]
[5.8,"Replace Stainless Steel Urinal","Material PC","ea",1,null,null,"Rate only"]
[5.9,"Replace Toilet Seats Standard Wooden/White","Material PC","ea",1,null,null,"Rate only"]
[]
[6,"Bathroom"]
[6.1,"Install Sink mixer pillar type","Material PC","ea",1,null,null,"Rate only"]
[6.2,"Install Sink mixer wall type","Material PC","ea",1,null,null,"Rate only"]
[6.3,"Replace to match the existing taps","Material PC","ea",1,null,null,"Rate only"]
[6.4,"Supply and Install stainless steel sink within cabinet 1.8 (hinge door)",null,"ea",1,null,null,"Rate only"]
[6.5,"Install Shower Head","Material PC","ea",1,null,null,"Rate only"]
[6.6,"Install Shower Door/Unit","Material PC","ea",1,null,null,"Rate only"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 2"]
[null,"BILL NO 2"]
[null,"MATERIAL SUPPLY AND INSTALL"]
[]
[7," Repairs -Burst pipes and leaks"]
[7.1,"Burst Pipes Excavation of Trenches ( By hand)",null,"m²",1,null,null,"Rate only"]
[7.2,"Burst Pipes (Mechanical)",null,"Daily","Plant hire Rates"]
[8,"Supply and Commission"]
[8.1,"uPVC Pipe 90mm",null,"m",1,null,null,"Rate only"]
[8.2,"uPVC Pipe 110mm",null,"m",1,null,null,"Rate only"]
[8.3,"uPVC Pipe 150mm",null,"m",1,null,null,"Rate only"]
[8.4,"uPVC Pipe 200mm",null,"m",1,null,null,"Rate only"]
[8.5,"Stainless Steel Clamp 90mm",null,"each",1,null,null,"Rate only"]
[8.6,"Stainless Steel Clamp 110mm",null,"each",1,null,null,"Rate only"]
[8.7,"Stainless Steel Clamp 150mm",null,"each",1,null,null,"Rate only"]
[8.8,"Stainless Steel Clamp 200mm",null,"each",1,null,null,"Rate only"]
[8.9,"Conversion Clamp 90mm",null,"each",1,null,null,"Rate only"]
[9,"Conversion Clamp 110mm",null,"each",1,null,null,"Rate only"]
[9.1,"Conversion Clamp 150mm",null,"each",1,null,null,"Rate only"]
[9.2,"Conversion Clamp 200mm",null,"each",1,null,null,"Rate only"]
[9.3,"Honeysuckle sewage service",null,"Daily rate","Plant hire Rates"]
[9.4,"Specialized services – Sweeping Sewerage Pipes","PC Item","m"]
[]
[9," Rates for Work / Services: Paving"]
[9.1,"Uplift, remove and clean paving bricks",null,"Alterations",1,null,null,"Rate only"]
[9.2,"Relay paving (incl. compacting & sundries)",null,"m²",1,null,null,"Rate only"]
[9.3,"Prepare and install new paving (incl. compacting and sundries bedded in 30mm river sand)","Material PC","m²",1,null,null,"Rate only"]
[9.4,"Sump and Grid ","Material PC","m",1,null,null,"Rate only"]
[9.5,"Trench and Grid ","Material PC","m",1,null,null,"Rate only"]
[9.6,"Pool Coping ","Material PC","m",1,null,null,"Rate only"]
[9.7,"Supply and install Concrete Curb/Kerb 900mm",null,"ea",1,null,null,"Rate only"]
[null,"Road Repairs"]
[9.8,"Remove existing Tar Road",null,"Alterations"]
[9.9,"Resurface Tar Road incl material",null,"m²",1,null,null,"Rate only"]
[9.1,"Painting of road marks incl Material",null,"m ",1,null,null,"Rate only"]
[9.11,"Supply and Install Studs on road surface",null,"ea",1,null,null,"Rate only"]
[]
[10,"Rates for Work / Services: Building Works"]
[null,"• These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal must be used or the amount exceeding 1m³."]
[null,"• Prices for taking out of doors, windows, etc. shall include for removal of all beads, architraves, ironmongery, etc"]
[null,"• Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc. and making good floor and wall finishes to match existing"]
[null,"• Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied as maybe required"]
[null,"• Temporary barriers and screens are inclusive of the costs"]
[null,"• The demolition costs for reinforced concrete includes cutting off and removing reinforcement"]
[10.1,"a. Demolition Work"]
[null,"Concrete and brick work"]
["10.1.1","Demolish 230mm brick wall",null,"Alterations"]
["10.1.2","Demolish 115mm brick wall",null,"Alterations"]
["10.1.3","Demolish concrete wall",null,"Alterations"]
["10.1.4","Demolish reinforced concrete slab",null,"Alterations"]
["10.1.5","Demolish Strong room walls ",null,"Alterations"]
["10.1.6","Remove dry wall and make good",null,"m²",1,null,null,"Rate only"]
["10.1.7","Demolish unreinforced concrete surface bed",null,"Alterations"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[]
[null,"Concrete Work"]
["10.1.7","Supply and Casting Concrete 20Mpa",null,"m³",1,null,null,"Rate only"]
["10.1.8","Supply and Casting Concrete 30Mpa",null,"m³",1,null,null,"Rate only"]
["10.1.9","Plaster existing walls, 12mm to smooth finish ",null,"m²",1,null,null,"Rate only"]
["10.1.10","Remove existing plaster to brick/concrete surface",null,"Alterations"]
["10.1.11","Supply and install Air bricks : 215 x 140mm Terra cotta air brick replacing or installing new therefore breaking out",null,"each",1,null,null,"Rate only"]
["10.1.12","Supply, Replace and Install door with frame in brick wall",null,"each",1,null,null,"Rate only"]
["10.1.13","Supply, Replace and Install window in brick wall",null,"m²",1,null,null,"Rate only"]
["10.1.14","Supply and Install 110 x 75mm Lintels in lengths not exceeding 3m",null,"m",1,null,null,"Rate only"]
["10.1.15","Brick force 75mm Wide Provide and Install ",null,"m",1,null,null,"Rate only"]
["10.1.16","Brick force 150mm Wide Provide and Install ",null,"m",1,null,null,"Rate only"]
[]
[10.2,"b. Brick walls"]
["10.2.1","Building of 115mm wall (plastered on both sides)",null,"m²",1,null,null,"Rate only"]
["10.2.2","Building of 230mm wall (plastered on both sides)",null,"m²",1,null,null,"Rate only"]
["10.2.3","Bagging to brickwork / concrete",null,"m²",1,null,null,"Rate only"]
["10.2.4","Building of 115mm wall (face brick)",null,"m²",1,null,null,"Rate only"]
["10.2.5","Building of 230mm wall (Face brick)",null,"m²",1,null,null,"Rate only"]
["10.2.6","Replace/Install door with frame in brick wall",null,"each",1,null,null,"Rate only"]
["10.2.7","Replace/Install window in brick wall",null,"m²",1,null,null,"Rate only"]
["10.2.8","Install 110 x 75mm Lintels in lengths not exceeding 3m",null,"m",1,null,null,"Rate only"]
["10.2.9","Brick force 75mm Wide Provide and Install",null,"m",1,null,null,"Rate only"]
["10.2.10","Brick force 150mm Wide Provide and Install",null,"m",1,null,null,"Rate only"]
["10.2.11","Install single steel door frame in brick wall",null,"each"]
["10.2.12","Install double steel door frame in brick wall",null,"each"]
["10.2.13","Install window in brick wall",null,"m²",{"$nulls":3},"Rate only"]
["10.2.14","Install 110 x 75mm Lintels in lengths not exceeding 3m",null,"m",{"$nulls":3},"Rate only"]
["10.2.15","Brick force 75mm Wide Provide and Install",null,"m",1,null,null,"Rate only"]
["10.2.16","Brick force 150mm Wide Provide and Install",null,"m"]
[]
[11,"Rates for Work / Services: for Blinds"]
[null,"a. Blinds"]
[null,"Installation of vertical cloth blinds 90mm (Metallic Blue)"]
[11.1,"Supply and Install Vertical Cloths Blinds",null,"m²",1,null,null,"Rate only"]
[11.2,"Supply Rail only",null,"m",1,null,null,"Rate only"]
[11.3,"Repair vertical cloth blinds.",null,"hourly",1,null,null,"Rate only"]
[11.4,"Replace and or remove existing cloth vertical blinds including rail Labour only",null,"each",1,null,null,"Rate only"]
[11.5,"Replace existing vertical Cloth blinds excluding rail Labour only",null,"m²",1,null,null,"Rate only"]
[]
[null,"Installation of Horizontal wooden blinds  50mm Venetian Type:  Wooden Blinds:  Colour:  Mahogany / Cherry"]
[11.6,"Supply and install Horizontal Wooden blinds",null,"ea",1,null,null,"Rate only"]
[11.7,"Remove Horizontal Wooden Blinds",null,"Alterations"]
[11.8,"Supply and install vertical perforated aluminum blinds","Material PC","ea",1,null,null,"Rate only"]
[11.9,"Supply and install vertical metallic blinds","Material PC","ea",1,null,null,"Rate only"]
{"$rows_empty":14}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill no 2"]
[null,"Material supply and Install"]
[]
[12,"Rates for Work / Services: Flooring"]
[null,"· Tiling rates are inclusive of both floor and wall"]
[null,"· All carpet glue/binder must be non – toxic, non – fume material costs must include such."]
[null,"· All costs must be inclusive finishing strips at doors and entrances"]
[null,"· Due to the various types of tiles available, no rate will be supplied on the type of tile. The service provider will be allowed a mark-up on the tiles. "]
[null,"• The labor, grout and sundries including cleaning must be allowed for in the commissioning amount as indicated ***"]
[null,"These rates include the removal of rubble up to 1m³. If the rubble exceeds 1m³ then the normal rate for rubble removal may be used"]
[]
[12.1,"a. Carpets"]
["12.1.1","Remove existing carpet tiles and prepare surface (see*** note)",null,"Alterations"]
["12.1.2","Remove existing vinyl and prepare surface (see*** note)",null,"Alterations"]
["12.1.3","Remove existing stretch carpet and prepare surface (see*** note)",null,"Alterations"]
["12.1.4","Remove existing wood laminate flooring(see*** note)",null,"Alterations"]
["12.1.5","Supply and Install Berber Point 920 (Charcoal) 600mm x 600mm",null,"m²",1,null,null,"Rate only"]
["12.1.6","Supply and Install Berber Point 920 (Charcoal) 500mm x 500mm",null,"m²",1,null,null,"Rate only"]
["12.1.7","Supply and Install Vinyl Seneca 4mm",null,"m²",1,null,null,"Rate only"]
["12.1.8","Supply and Install PVC Vinyl Tile 250mm x 250 mm @ 2mm",null,"m²",1,null,null,"Rate only"]
["12.1.9","Supply and Install Wooden Laminate Flooring >6mm",null,"m²",1,null,null,"Rate only"]
["12.1.10","Supply and Install Stretch carpet",null,"m²",1,null,null,"Rate only"]
["12.1.11","Floor strips aluminum 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.12","Floor strips wooden 30-40mm",null,"m ",1,null,null,"Rate only"]
["12.1.13","Remove and Install skirting 75mm wooden",null,"m ",1,null,null,"Rate only"]
["12.1.14","Remove and Install quarter round",null,"m ",1,null,null,"Rate only"]
[]
[12.2,"b. Tiling"]
["12.2.1","Break up and remove ceramic wall and floor tiles and make good (Prepare surface for tiling if required)",null,"Alterations"]
["12.2.2","Install ceramic tiles (wall and floor) Commission rate to include labor, glue and grout for laying floor and wall tiles)"," Material PC ","m²",1,null,null,"Rate only"]
["12.2.3","Clean and re – grout tiles ",null,"m²",1,null,null,"Rate only"]
["12.2.4","Sealing of Terra-cotta tiles",null,"m²",1,null,null,"Rate only"]
["12.2.5","Topping +/- 30mm Thick",null,"m²",1,null,null,"Rate only"]
["12.2.6","Screed +/- 10mm  Marley screed (Self Leveling)",null,"m²",1,null,null,"Rate only"]
["12.2.7","Tile skirting 100mm high",null,"Alterations"]
{"$rows_empty":22}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill no 2"]
[null,"Material supply and Install"]
[]
[13," Rates for Work / Services: Fencing and Walling"]
[null,"· Split pole fencing and pole fences must be treated with Wax All"]
[null,"All steel palisade fencing material cost must include painting"]
[13.1,"a. Timber"]
["13.1.1","Supply and Install1.2m High Split pole fencing"," Material PC ","m ",1,null,null,"Rate only"]
["13.1.2","Supply and Install1.5m High Split pole fencing"," Material PC ","m ",1,null,null,"Rate only"]
["13.1.3","Supply and Install1.8m High Split pole fencing"," Material PC ","m ",1,null,null,"Rate only"]
["13.1.4","Supply and Install2.4m High Split pole fencing"," Material PC ","m ",1,null,null,"Rate only"]
[]
[13.2,"b. Galvinized Fencing"]
["13.2.1","Repair 2.5 x 50mm diamond mesh fence"," Material PC ","m ",1,null,null,"Rate only"]
["13.2.2","Replace 2mm x 75mm x  3m x 600mm poles, Galvanized"," Material PC ","each",1,null,null,"Rate only"]
["13.2.3","Install 2.5mm  x 50mm x 3 m High diamond mesh fence, Galvanized "," Material PC ","m ",1,null,null,"Rate only"]
[]
[13.3,"c.  Steel Palisade Fence Devils Fork and Other "," Material PC ","m ",1,null,null,"Rate only"]
["13.3.1","Install 1.2m High Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.2","Install 1.5m High Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.3","Install 1.8m High Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.4","Install 2.4m High Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.5","Install 1.2m x 900 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.6","Install 1.5m x 900 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.7","Install 1.8m x 900 mm single Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.8","Install 2.4m x 900 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.9","Install 1.2m x 1800 mm double gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","m ",1,null,null,"Rate only"]
["13.3.10","Install 1.5m x 1 800 mm double gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.11","Install 1.8m x 1 800 mm double gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.12","Install 2.4m x 1 800 mm double gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.13","Install 1.5m x 3000 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.14","Install 1.8m x  3000 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.15","Install 2.4m x 3000 mm single gate Max 100mm space between 32mm x 3mm Uprights"," Material PC ","each",1,null,null,"Rate only"]
["13.3.16","Install Electric Fencing 11 Strings 100mm spacing"," Material PC ","each",1,null,null,"Rate only"]
["13.3.17","Install Razor Wire Flat wrap"," Material PC ","each",1,null,null,"Rate only"]
["13.3.18","Install Razor Wire Coils"," Material PC ","each",1,null,null,"Rate only"]
["13.3.19","Install Razor wire diamond mesh 1800mm height"," Material PC ","each",1,null,null,"Rate only"]
["13.3.20","Install Razor wire diamond mesh 2400mm height"," Material PC ","each",1,null,null,"Rate only"]
["13.3.17","Install/Replace Clear VU fence panels 1.8/ 2.4/ 3m x 3m"," Material PC ","Unit",1,null,null,"Rate only"]
["13.3.18","Install/Replace Clear VU poles 1.8m/2.4/3m"," Material PC ","Unit",1,null,null,"Rate only"]
[]
[13.4,"d. Precast Walls Plain"]
["13.4.1","Install Wall 1.2m High "," Material PC ","m",1,null,null,"Rate only"]
["13.4.2","Install Wall 1.5m High"," Material PC ","m",1,null,null,"Rate only"]
["13.4.3","Install Wall 1.8m High "," Material PC ","m",1,null,null,"Rate only"]
["13.4.4","Install Wall 2.4m High"," Material PC ","m",1,null,null,"Rate only"]
[13.5,"e. Precast Brickwork Panels Single Sided"]
["13.5.1","Install Wall 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.5.2","Install Wall 1.5m High",null,"m",1,null,null,"Rate only"]
["13.5.3","Install Wall 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.5.4","Install Wall 2.4m High",null,"m",1,null,null,"Rate only"]
[13.6,"f. Precast Brickwork Panels Double Sided"]
["13.6.1","Remove 1.2m High ",null,"m",1,null,null,"Rate only"]
["13.6.2","Remove 1.5m High",null,"m",1,null,null,"Rate only"]
["13.6.3","Remove 1.8m High ",null,"m",1,null,null,"Rate only"]
["13.6.4","Remove 2.4m High",null,"m",1,null,null,"Rate only"]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[14," Rates for Work / Services: Iron Mongery"]
[]
[14.1,"a.  Burglar Bars at Windows"]
[null,"16mm round bars welded into a 25mm square tubing frame with 2mm wall thickness, rawl bolted to the walls with 10mm rawl bolts welded to frame)"]
[]
[null,"Repllace Broken Window sizes:"]
["14.1.1","Supply and Install (1,26 x 1,51) m",null,"Item",1,null,null,"Rate only"]
["14.1.2","Supply and Install (1,26 x 1,84) m",null,"Item",1,null,null,"Rate only"]
["14.1.3","Supply and Install (1,26 x 0.96) m",null,"Item",1,null,null,"Rate only"]
["14.1.4","Supply and Install (1,63 x 0.96) m",null,"Item",1,null,null,"Rate only"]
[]
[14.2,"b.  Burglar Gates single  -  Built to specification Supply and install"]
["14.2.1","(i)    16mm Round bar welded in a 38mm tubing frame fitted with a  5 Lever STATUS lock",null,"Item",1,null,null,"Rate only"]
[null,"(ii)   Gate to be fitted in a 38mm tubing frame rawl bolted to the wall"]
[null,"(iii)  Rawl bolts to be at least 10mm diameter and welded to frame after installation"]
[null,"(iv)  Space separating Round bars to be 100mm"]
[]
["14.2.2","(i)      Velmatex on 38mm tubing frame fitted with a 5 Lever STATUS lock",null,"Item",1,null,null,"Rate only"]
[null,"(ii)     Gate to be fitted in a 38mm tubing frame rawl bolted to the wall Interlocking closing pin on “fixed panel” of gate"]
[null,"(iii)    20mm x 100mm Bullet hinges or similar heavy duty hinges with interlocking frame pins"]
[null,"(iv)   Two eyelet sets for padlocks for additional security"]
[null,"(v) Rawl bolts to be at least 10mm diameter welded to frame after installation"]
[]
[14.3,"c.  Burglar Gates Double  -  Built to specification Supply and install"]
["14.3.1","(i)    16mm Round bar welded in a 38mm tubing frame with 2mm wall thickness fitted with a 5 Lever STATUS locks)",null,"Item",1,null,null,"Rate only"]
[null,"(ii)   Gate to be fitted in a 38mm tubing frame rawl bolted to the wall "]
[null,"(iii)  Rawl bolts to be at least 10mm and welded to frame after installation"]
[null,"(iv) Spacing for round bars to be 100mm apart "]
[]
["14.3.2","(i)    Velmatex on 38mm tubing frame fitted with a 5 Lever STATUS lock. Gate to be fitted in a 38mmTubing frame rawl bolted to the wall",null,"Item",1,null,null,"Rate only"]
[null,"(ii)   Interlocking closing pin on “fixed panel” of gate"]
[null,"(iii)  Bullet hinges 20mm x 100mm or similar heavy Duty hinges with interlocking frame pins on both panels"]
[null,"(iv)  Two eyelet sets for padlocks for additional security"]
[null,"      (v)  Rawl bolts to be at least 10mm diameter and           bolt head welded after installation"]
[]
["14.3.3","Supply and installation of Trelli / Xpanda doors","PC Item"]
{"$rows_empty":7}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[14.4,"d.  Supply and Install Flat Steel Double Carports"]
[]
[null,"(i)    Supply and install Flat Steel Double carports:   5 m wide x 5, 5 m with 0, 5 mm IBR Chroma-deck sheeting fastened with tech screws to structure. ",null,"Item",1,null,null,"Rate only"]
[null,"(ii)   Poles to be 76 mm x 3mm planted at least 500mm deep. Front poles to move inwards by 1,2m outside and support frame to be 150mm x 50mm Lip Channel."]
[null,"(iii)  Inside Lip Channel to be 75mm x 50mm. "]
[null,"(iv)  Minimum Height to be 2,2m from paved level. "]
[null,"(v)   Gutters and down pipes to be installed at the lowest side."]
[null,"(vi)  Carport to be painted with coast coat self-etching primer and finished with at least two coats of High gloss Enamel  paint Dulux/Plascon"]
[]
[14.5,"e.  Supply and Install  Flat Steel Single Carports"]
[]
[null,"(i)    Supply and Install Flat Steel Single carports:  2,5 m wide x 5,5 m with 0,5 mm IBR Chroma-deck sheeting fastened with tech screws to structure. ",null,"Item",1,null,null,"Rate only"]
[null,"(ii)   Poles to be 76 mm x 3mm planted at least 500mm deep. Front poles to move inwards by 1,2m outside and support frame to be 150mm x 50mm Lip Channel. "]
[null,"(iii)  Inside Lip Channel to be 75mm x 50mm. "]
[null,"(iv)  Minimum Height to be 2,2m from paved level. "]
[null,"(v)   Gutters and down pipes to be installed at the lowest side. "]
[null,"(vi)  Carport to be painted with coast coat self-etching and finished with at least two coats of High Gloss Enamel paint."]
[]
[14.6,"f. Shade port Carports"]
[null,"1) Poles to be at least 100mm x 2mm x2.2 High"]
[null,"2) Frame  to be at least 50mm x 2mm "]
[null,"3) Netting to be 80% UV resistand"]
[null,"4) Poles to be planted at Least 600mm deap fastend with Concrete."]
[]
["14.6.1","Supply and Install  Shade port Single Carports",null,"Item",1,null,null,"Rate only"]
[]
["14.6.2","Replace Netting on Existing Single Shade port",null,"Item",1,null,null,"Rate only"]
[]
["14.6.3","Supply and Install  Shade port Double Carports",null,"Item",1,null,null,"Rate only"]
[]
["14.6.4","Replace Netting on Existing Double Shade port",null,"Item",1,null,null,"Rate only"]
[]
["14.6.5","Supply and Install  Shade port Triple Carports",null,"Item",1,null,null,"Rate only"]
[]
["14.6.6","Replace Netting on Existing Triple Shade port",null,"Item",1,null,null,"Rate only"]
{"$rows_empty":21}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[15,"Rates for Work / Services: Carpentry and Joinery"]
[15.1,"a. Doors Supply and Install"]
["15.1.1","Cat 2 safe door fitted with 3Way Combination Lock with two x 7 Lever locks",null,"Ea",1,null,null,"Rate only"]
["15.1.2","Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Brick wall",null,"Ea",1,null,null,"Rate only"]
["15.1.3","Record Room Door fitted with 7 Lever Lock with a 3 Way Combination Lock in Strengthened Drywall",null,"Ea",1,null,null,"Rate only"]
["15.1.4","Rocklike Class B Fire Double Door fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock. Door to be rapped in 1mm Galv Sheet on all six sides",null,"Ea",1,null,null,"Rate only"]
["15.1.5","Rocklike Class B Fire Door Single fitted with a 5 L Knob Cylinder Lock with an additional Redlim Break Glass Lock. Door to be rapped in 1mm Galv Sheet on all six sides",null,"Ea",1,null,null,"Rate only"]
["15.1.6","Solid wooden door Single 815 x 2030 High ",null,"Ea",1,null,null,"Rate only"]
["15.1.7","Solid wooden door Double 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.8","Flash back V Joint Meranti Double door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.9","Flash back V Joint Meranti Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.10","Sol-core Masonite door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.11","Sol-core Masonite Double door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.12","Semi Solid Masonite door 815 x 2030",null,"Ea",1,null,null,"Rate only"]
["15.1.13","Semi Solid Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.14","Hollow Core Masonite Door 815 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.15","Hollow Core Masonite double Door 1500 x 2030 High",null,"Ea",1,null,null,"Rate only"]
["15.1.16","Roller Shutter Doors "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.17","Service and Repair Roller Shutter Doors "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.18","Sliding gates"," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.19","Steel sliding doors 815x2030mm",null,"Ea",1,null,null,"Rate only"]
["15.1.20","Wooden Panel Garage Door Single. Motorized Complete",null,"Ea",1,null,null,"Rate only"]
["15.1.21","Service / repair Wooden Panel Garage Door Single. "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.22","Wooden Panel Garage Door Double Motorized Complete",null,"Ea",1,null,null,"Rate only"]
["15.1.23","Service / Repair Panel Garage Door Double "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.24","Chromadeck Panel Garage Door Single Motorized Complete"]
["15.1.25","Service / Repair Chromadeck Panel Garage Door Single "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.26","Chromadeck Panel Garage Door Double Motorized Complete"]
["15.1.27","Service / Repair Chromadeck Panel Garage Door Double "," Material PC ","Ea",1,null,null,"Rate only"]
["15.1.28","Roller Shuter Doors Single Motorized Complete",null,"Ea",1,null,null,"Rate only"]
["15.1.29","Roller Shuter Doors Double Motorized Complete",null,"Ea",1,null,null,"Rate only"]
[]
[15.2,"b. Door Lock and Handles Supply and Install"]
["15.2.1","Toilet Door lock Thumb Turn",null,"ea",1,null,null,"Rate only"]
["15.2.2","Door handles Union",null,"set",1,null,null,"Rate only"]
["15.2.3","Heavy Duty 4 Lever Union Lock and Handles",null,"set",1,null,null,"Rate only"]
["15.2.4","Aluminum Door handle with Square Back plate",null,"set",1,null,null,"Rate only"]
["15.2.5","Door handle on build- in Cupboard Push Button Lock",null,"ea",1,null,null,"Rate only"]
["15.2.6","Door handle on build- in Cupboard Plain",null,"ea",1,null,null,"Rate only"]
["15.2.7","4 lever lock Union,",null,"ea",1,null,null,"Rate only"]
["15.2.8","5 lever lock with Handles: Chub 3K70",null,"ea",1,null,null,"Rate only"]
["15.2.9","5 lever lock with Handles: Union Lock",null,"ea",1,null,null,"Rate only"]
["15.2.10","5 lever lock with Handles: Status Lock",null,"ea",1,null,null,"Rate only"]
["15.2.11","5 lever lock with Handles: Cisa Lock",null,"ea",1,null,null,"Rate only"]
["15.2.12","Small Oval Cylinder Lock",null,"ea",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
["15.2.13","Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.14","Large Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["15.2.15","Mechanical Code Lock, 14 pin type",null,"each",1,null,null,"Rate only"]
["15.2.16","Indoor Yale latch door lock",null,"each",1,null,null,"Rate only"]
["15.2.17","indoor Deadbolt security lock Chub 3G110",null,"each",1,null,null,"Rate only"]
["15.2.18","Mild steel sliding door lock , hook type latch",null,"each",1,null,null,"Rate only"]
["15.2.19","Steel patio door lock, slim line design, 4 lever",null,"each",1,null,null,"Rate only"]
["15.2.20","Double action 7L Security gate Lock",null,"each",1,null,null,"Rate only"]
[]
[15.3,"c.  Door accessories and spares Supply and Install"]
["15.3.1","Hinges Brass heavy duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.2","Hinges Brass light duty with recessed mounting holes, for doors",null,"each",1,null,null,"Rate only"]
["15.3.3","Hinges steel heavy duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.4","Hinges steel light duty with recessed mounting holes , for doors",null,"each",1,null,null,"Rate only"]
["15.3.5","Hinges Brass light duty with recessed mounting holes, for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.6","Hinges steel light duty with recessed mounting holes , for cabinet doors , small, approx. 50mm",null,"each",1,null,null,"Rate only"]
["15.3.7","Sliding bolts, brass, heavy duty, approx. 150 mm long",null,"each",1,null,null,"Rate only"]
["15.3.8","Sliding bolts, brass, heavy duty, approx. 75 mm long",null,"each",1,null,null,"Rate only"]
["15.3.9","Galvanized steel sliding bolt, approx. 150mm long",null,"each",1,null,null,"Rate only"]
[]
[15.4,"d. Ceilings Supply and Install"]
[null,"Brandering will not be allowed with each ceiling replacement; where possible existing Brandering must be used"]
[null,"Fire Barriers: The type and thickness of boards, the number of layers and the insulation (if necessary) is to be such as to produce the specified fire rating all in accordance with the manufacturer's recommendation and will be a PC item."]
[null,"Proprietary suspended ceilings’ hangers, suspension grids, \"lay-in\" panels, etc. are to be in accordance with the manufacturers' recommendations"]
[null,"All steel components for ceilings, partitions, etc. are to be galvanized in accordance with SANS 121"]
[null,"Costs for openings for light fittings, ventilation grilles, air-conditioning diffusers, etc. are to include for any necessary additional support, trimming around, etc."]
[]
["15.4.1","Install 76mm Cornish",null,"m²",1,null,null,"Rate only"]
["15.4.2","Suspended ceiling panels: 1200mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.3","Suspended ceiling panels: 600mm x 600mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.4","Suspended ceiling panels: 500mm x 500mm x 12,7mm",null,"m²",1,null,null,"Rate only"]
["15.4.5","6,4mm gypsum plaster ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.6","6mm Nutec Ceilings",null,"m²",1,null,null,"Rate only"]
["15.4.7","Trapdoor 600 mm x600 mm",null,"m²",1,null,null,"Rate only"]
["15.4.8","Build Bulk Head Ceiling",null,"m²",1,null,null,"Rate only"]
["15.4.9","Openings (to be made in ceilings)",null,"Alterations"]
[]
[15.5,"d. Built in Cupboards Supply and Install"]
["15.5.1","Formica Top work surfaces 32mm",null,"m",1,null,null,"Rate only"]
["15.5.2","Cabinet locks: union",null,"ea",1,null,null,"Rate only"]
["15.5.3","Top section of kitchen unit"," Material PC ","m²",1,null,null,"Rate only"]
["15.5.4","Bottom section of kitchen unit"," Material PC ","m²",1,null,null,"Rate only"]
[]
[15.6,"e. Hangings"]
[null,"·  Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[null,".  Items described as \"plugged\" shall be deemed to include screwing to fiber, plastic or metal plugs at not exceeding 500 mm centers, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
["15.6.1","Install picture frame hooks and hang frame (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.2","Install Picture frame hooks (dry wall)",null,"each",1,null,null,"Rate only"]
["15.6.3","Install notice / white board (brick wall)",null,"each",1,null,null,"Rate only"]
["15.6.4","Install notice / white board (dry wall)",null,"each",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[16,"Table 15 : Rates for Work / Services:  Glass and Aluminium"]
[16.1,"a.  Glass Supply and Install including Patty, strips and fittings",{"$nulls":5},"Rate only"]
["16.1.1","Clear Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.2","Clear Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.3","Clear Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.4","Clear Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.5","Thick deep grey laminated safety glass 6.5mm",null,"m²",1,null,null,"Rate only"]
["16.1.6","Bathroom Frosted Glass 3mm",null,"m²",1,null,null,"Rate only"]
["16.1.7","Bathroom Frosted Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.8","Bathroom Frosted Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.9","Clear Safety Glass 6mm",null,"m²",1,null,null,"Rate only"]
["16.1.10","Clear Safety Glass10mm",null,"m²",1,null,null,"Rate only"]
["16.1.11","Georgian Wire Glass 4mm",null,"m²",1,null,null,"Rate only"]
["16.1.12","Georgian Wire Glass   5mm             ",null,"m²",1,null,null,"Rate only"]
["16.1.13","Shatterproof Glass 5mm",null,"m²",1,null,null,"Rate only"]
["16.1.14","Shatterproof Glass  6mm",null,"m²",1,null,null,"Rate only"]
["16.1.15","Bullet proof glass "," Material PC ","m²",1,null,null,"Rate only"]
["16.1.16","Window laminate – frosted /decorative",null,"m²",1,null,null,"Rate only"]
["16.1.17","Window laminate – solar reflective 75%",null,"m²",1,null,null,"Rate only"]
["16.1.18","Polishing of louver glass , all edges polished per louver glass panel",null,"Each",1,null,null,"Rate only"]
[16.2,"b.  Putty Replacement "]
["16.2.1","Remove and / or replace window putty",null,"Alterations"]
[16.3,"c.  Mirrors"]
["16.3.1","Remove Mirror non - salvage",null,"Alterations"]
["16.3.2","Remove mirror salvage",null,"Alterations"]
["16.3.3","4mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.4","5mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
["16.3.5","6mm Drilled at Corners",null,"m²",1,null,null,"Rate only"]
[16.4,"d.  Aluminum Doors and Windows"]
["16.4.1","Adjust & Service Single door (frame mounted and cubicle mounted)",null,"Each",1,null,null,"Rate only"]
["16.4.2","Adjust & Service Double door",null,"Each",1,null,null,"Rate only"]
["16.4.3","Adjust & Service Floor spring",null,"Each",1,null,null,"Rate only"]
["16.4.4","Adjust & Service Top Spring",null,"Each",1,null,null,"Rate only"]
["16.4.5","Adjust & Service sliding door (single)",null,"Each",1,null,null,"Rate only"]
["16.4.6","Adjust & Service sliding door (double)",null,"Each",1,null,null,"Rate only"]
["16.4.7","Adjust & Service emergency exit door (single, push bar mechanism, 3point type or similar)",null,"Each",1,null,null,"Rate only"]
["16.4.8","Adjust & Service emergency exit door (double, dual push bar mechanism)",null,"Each",1,null,null,"Rate only"]
[]
[16.5,"e.  Spares for Aluminum Doors and windows Supply and Install"]
["16.5.1","Hinges Aluminium Heavy Duty with recessed mounting holes complete with heavy duty rivets",null,"Per Set",1,null,null,"Rate only"]
["16.5.2","Continuous Aluminium hinge, heavy duty type with recessed mounting holes complete with heavy duty mounting kits / rivets 2.1m Long",null,"Per door",1,null,null,"Rate only"]
["16.5.3","Install Piano Hinges -cubicles",null,"Per hinge",1,null,null,"Rate only"]
["16.5.4","Belt driven hinges - sliding doors",null,"Per",1,null,null,"Rate only"]
["16.5.5","Small Oval Cylinder Lock",null,"belt",1,null,null,"Rate only"]
["16.5.6","Large Oval Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.7","Profile Cylinder Lock",null,"each",1,null,null,"Rate only"]
["16.5.8","5 Cylinder Lever Lock Casing",null,"each",1,null,null,"Rate only"]
["16.5.9","Mechanical Code Lock (14 pin type, for Aluminium door)",null,"each",1,null,null,"Rate only"]
["16.5.10","Hydraulic/ pneumatic Door Closer standard",null,"each",1,null,null,"Rate only"]
["16.5.11","Flush bolt",null,"each",1,null,null,"Rate only"]
["16.5.12","Floor Springs Geze TS 500N",null,"each",1,null,null,"Rate only"]
["16.5.13","75mm x 2 mm Aluminium Skirting",null,"m",1,null,null,"Rate only"]
["16.5.14","75mm x 50mm x 2 mm Aluminium Profile",null,"m",1,null,null,"Rate only"]
["16.5.15","30mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.17","50mm Aluminium Angle (3 mm thick)",null,"m",1,null,null,"Rate only"]
["16.5.19","Aluminium Door Handles",null,"each",1,null,null,"Rate only"]
["16.5.20","Aluminium Window Handles",null,"each",1,null,null,"Rate only"]
["16.5.21","Hinges for top hung Aluminium windows",null,"set",1,null,null,"Rate only"]
["16.5.22","Hinges for offset mounted Aluminium windows, vertical swing",null,"set",1,null,null,"Rate only"]
["16.5.23","Hinges for offset mounted Aluminium windows, horizontal swing",null,"set",1,null,null,"Rate only"]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[null,"Note : Shop drawings to be approved prior to manufacturing"]
[16.6,"f.  Aluminum Doors Manufacture, Supply and Fit (Standard)"]
["16.6.1","813mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.2","1200mm x 2.1m high natural Aluminium single door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.3","1500mm x 2.1m high natural Aluminium double door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.4","1800mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.5","1800mm x 3.0m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame",null,"ea",1,null,null,"Rate only"]
["16.6.6","2400mm x 2.1m high natural  Aluminium double section single sliding door with 50mm profile fitted in Aluminium frame","PC Item"]
["16.6.7","3000mm x 2.1m high natural  Aluminium 4 section dual sliding door with 50mm profile fitted in Aluminium frame","PC Item"]
["16.6.8","6000 x 2.1m high natural Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)","PC Item"]
["16.6.9","6000 x 2.1m high polished Aluminium 4 section dual sliding door with 100mm profile fitted in Aluminium frame(2400mm wide access when open)","PC Item"]
[]
[16.7,"g.  Aluminum Doors Manufacture, Supply and Fit (SSA Specifications) "]
["16.7.1","Single cubicle door 950mm x 2200mm Frame size:2100mm x 2350mm","PC Item"]
["16.7.2","Single door 950mm x 2200mm Frame size:1161mm x 2350mm","PC Item"]
["16.7.3","Single door 954mm x 2200mm Frame size:1152mm x 2350mm","PC Item"]
["16.7.4","Double Door 1600mm x 2200mm Frame size:1900mm x 2350mm","PC Item"]
["16.7.5","Automatic Double Sliding Door: Door size 1825mm x 2200mmFrame size 3944mm x 2350mm","PC Item"]
["16.7.6","Automatic Double Sliding Door, Door size 2010mm x 2200mm Frame size 4071mm x 2350mm","PC Item"]
["16.7.7","Double Door 1800mm x 2200mm Frame size:2100mm x 2350m","PC Item"]
["16.7.8","Double Door 1600mm x 2200mmFrame size:1901mm x 2350mm","PC Item"]
["16.7.9","Automatic Double Sliding Door size 1350mm x 2200mm Frame size 2940mm x 2350mm","PC Item"]
[]
[16.8,"h.  Aluminum Windows Manufacture, Supply and Fit"]
[]
["16.8.1","300 mm x 600 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.2","600 mm x 600mm mm high natural Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.3","600 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.4","900 mm x 1200 mm high natural Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.5","1200mm x 1200 mm high natural Aluminium window with 50mm profile fitted in Aluminium frame","PC Item"]
["16.8.6","300 mm x 600 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.7","600 mm x 600mm mm high polished Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.8","600 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.9","900 mm x 1200 mm high polished Aluminium window with 30mm profile fitted in Aluminium frame","PC Item"]
["16.8.10","1200mm x 1200 mm high polished Aluminium window with 50mm profile fitted in Aluminium frame","PC Item"]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[16.9,"i.  Custom Aluminum products, Manufacture, Supply and Fit"]
["16.9.1","Custom window panel fitted in 30mm profile natural Aluminium  frame (Fixed Not Opening)"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.2","Custom window panel fitted in 30mm profile polished Aluminium frame (Fixed Not Opening)"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.3","Custom natural Aluminium window with 30mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.4","Custom polished Aluminium window with 30mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.5","Custom natural Aluminium single door with 50mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.6","Custom polished Aluminium single door with 50mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.7","Custom natural Aluminium double door with 50mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
["16.9.8","Custom polished Aluminium double door with 50mm profile fitted in Aluminium frame"," Material PC ","ea",1,null,null,"Rate only"]
{"$rows_empty":58}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[17,"Table 16:  Rates for Work / Services Paintwork"]
[null,"·         Painting (Includes preparation, sanding, poly fill, sugar soap wash etc.)"]
[null,".         Under coating of wall must only be used in areas where the walls are newly plastered / Rhino lite or the paint color is different"]
[null,"·         The rate allows for two coats paint and/or varnish and half the rate for one coat or as an additional paint  "]
[null,"·         The rate for metal surfaces includes anti – rust treatment"]
[null,"·         All paint must be SABS approved and be UV resident, Water resistant, Alkali resistant and Lead Free, Plascon / Dulux"]
[null,"·         All roof paint must be heat reflective and contain a 12 year guarantee, Plascon / Dulux"]
[null,".         Application must be as per supplier specification certification must be provided"]
[]
[17.1,"a.  Repaint Walls"]
["17.1.1","Interior Acrylic PVA",null,"m²",1,null,null,"Rate only"]
["17.1.2","Interior Double  Velvet",null,"m²",1,null,null,"Rate only"]
["17.1.3","Interior low-sheen Acrylic",null,"m²",1,null,null,"Rate only"]
["17.1.4","Exterior PVA (Same or similar to  Dulux Weather Guard quality)",null,"m²",1,null,null,"Rate only"]
["17.1.5","Applying of Bonding liquid on new plastered or damaged walls",null,"m²",1,null,null,"Rate only"]
["17.1.6","Universal Undercoat ",null,"m²",1,null,null,"Rate only"]
["17.1.7","Interior non drip enamel",null,"m²",1,null,null,"Rate only"]
["17.1.8","Exterior non drip enamel",null,"m²",1,null,null,"Rate only"]
["17.1.9","Wood surfaces",null,"m²",1,null,null,"Rate only"]
["17.1.10","Ferrous metal surfaces",null,"m²",1,null,null,"Rate only"]
["17.1.11","Zinc-coated or galvanized surfaces",null,"m²",1,null,null,"Rate only"]
["17.1.12","Masonry, concrete and fiber cement surfaces",null,"m²",1,null,null,"Rate only"]
["17.1.13","Sugar soap wash ",null,"m²",1,null,null,"Rate only"]
["17.1.14","Paint tiled roof ",null,"m²",1,null,null,"Rate only"]
["17.1.15","Technique paint - Supply specialist quotation "," Material PC ","Item"]
[]
[17.2,"b.  Skirting / Quarter rounds / Cornish"]
["17.2.1","Interior Paint PVA",null,"m²",1,null,null,"Rate only"]
["17.2.2","Interior Paint Enamel",null,"m²",1,null,null,"Rate only"]
["17.2.3","Interior Varnish",null,"m²",1,null,null,"Rate only"]
["17.2.4","Exterior Paint",null,"m²",1,null,null,"Rate only"]
["17.2.5","Exterior Varnish",null,"m²",1,null,null,"Rate only"]
[]
[17.3,"c. Repaint Ceilings (PVA)"]
["17.3.1"," Interior Gypsum",null,"m²",1,null,null,"Rate only"]
["17.3.2","Interior Fiber Cement",null,"m²",1,null,null,"Rate only"]
["17.3.3","Interior Mineral Board",null,"m²",1,null,null,"Rate only"]
["17.3.4","Interior Wood",null,"m²",1,null,null,"Rate only"]
["17.3.5","Exterior Gypsum",null,"m²",1,null,null,"Rate only"]
["17.3.6","Exterior Fiber Cement",null,"m²",1,null,null,"Rate only"]
["17.3.7","Exterior Mineral Board",null,"m²",1,null,null,"Rate only"]
["17.3.8","Exterior Wood",null,"m²",1,null,null,"Rate only"]
["17.3.9","Poured concrete and concrete blocks",null,"m²",1,null,null,"Rate only"]
[]
[17.4,"d.  Repaint Roof Coverings (Heat reflection & Tint) = HR"]
[null,"HR = Heat reflective Roof Paint Dulux / Plascon 12 Year"]
["17.4.1","a. IBR Sheeting – HR White ","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. IBR Sheeting – HR White ","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.2","a. IBR Sheeting – HR Tint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. IBR Sheeting – HR Tint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.3","a. IBR Sheeting – Roof paint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. IBR Sheeting – Roof paint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.4","a. Corrugated Sheeting– HR White","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b.Corrugated Sheeting– HR White","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.8","a. Corrugated Sheeting– HR Tint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Corrugated Sheeting– HR Tint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.9","a. Corrugated Sheeting– Roof paint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Corrugated Sheeting– Roof paint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.10","a. Chromadech Sheeting","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Chromadech Sheeting","Airless Spray","m²",1,null,null,"Rate only"]
[]
[]
[]
[]
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
["17.4.10","a. Mineral Fiber Profiled Sheeting – HR White","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Mineral Fiber Profiled Sheeting – HR White","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.11","a. Mineral Fiber Profiled Sheeting – HR Tint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Mineral Fiber Profiled Sheeting – HR Tint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.12","a. Mineral Fiber Profiled Sheeting – Roof Paint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Mineral Fiber Profiled Sheeting – Roof Paint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.13","a. Paint fascia and barges","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint fascia and barges","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.14","a. Paint roof tiles – HR White","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint roof tiles – HR White","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.15","a. Paint roof tiles – HR White","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint roof tiles – HR White","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.16","a. Paint roof tiles – HR Tint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint roof tiles – HR Tint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.17","a. Paint roof tiles – Roof Paint","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint roof tiles – Roof Paint","Airless Spray","m²",1,null,null,"Rate only"]
["17.4.18","a. Paint Torch-on Roofs with Bitumen Silver Paint x2 couts","Hand Apply","m²",1,null,null,"Rate only"]
[null,"b. Paint Torch-on Roofs with Bitumen Silver Paint x2 couts","Airless Spray","m²",1,null,null,"Rate only"]
[]
[17.5,"e. Repaint Window Frames"]
["17.5.1","Exterior Window Frame including Window sill less than 1 m²",null,"ea",1,null,null,"Rate only"]
["17.5.2","Exterior Window Frame including Window sill less than 2 m²",null,"ea",1,null,null,"Rate only"]
["17.5.3","Interior Window Frame including window sill less than 1 m²",null,"ea",1,null,null,"Rate only"]
["17.5.4","Interior Window Frame including window sill less than 2 m²",null,"ea",1,null,null,"Rate only"]
[]
[17.6,"f. Repaint Doors & Frames"]
["17.6.1","Varnish Double door",null,"ea",1,null,null,"Rate only"]
["17.6.2","Varnish Double Frame",null,"ea",1,null,null,"Rate only"]
["17.6.3","Varnish Single door",null,"ea",1,null,null,"Rate only"]
["17.6.4","Varnish Single Frame",null,"ea",1,null,null,"Rate only"]
["17.6.5","Varnish Window Frame",null,"ea",1,null,null,"Rate only"]
["17.6.6","Paint Double Door Frame (Enamel)",null,"ea",1,null,null,"Rate only"]
["17.6.7","Paint Single Door Frame (Enamel)",null,"ea",1,null,null,"Rate only"]
["17.6.8","Paint Single Door (Enamel)",null,"ea",1,null,null,"Rate only"]
["17.6.9","Paint Double Door (Enamel)",null,"ea",1,null,null,"Rate only"]
[]
[]
[17.7,"g. Repaint Metal Surfaces",null,null,1,null,null,"Rate only"]
["17.7.1","Gutters",null,"m",1,null,null,"Rate only"]
["17.7.2","Down pipes / Steel Pipes",null,"m",1,null,null,"Rate only"]
["17.7.3","Louvre’s / Balustrades",null,"m",1,null,null,"Rate only"]
["17.7.4","Gates & Burglar Bars",null,"m² ",1,null,null,"Rate only"]
["17.7.5","Infill Panels & Boxes",null,"m² ",1,null,null,"Rate only"]
[]
[17.8,"h. Spray Paint work for steel works"]
["17.8.1","Interior",null,"m² ",1,null,null,"Rate only"]
["17.8.2","Exterior",null,"m² ",1,null,null,"Rate only"]
{"$rows_empty":18}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[18,"Table 17:  Rates for Work / Services – Waterproofing"]
[18.1,"a.  Waterproofing Tiled Roofs"]
["18.1.1","Replace cracked mortar between ridge tiles ",null,"m ",1,null,null,"Rate only"]
["18.1.2","Waterproof ridge over laps with 100mm membrane ",null,"m ",1,null,null,"Rate only"]
["18.1.3","Waterproof ridge over laps with 200mm membrane ",null,"m ",1,null,null,"Rate only"]
["18.1.4","Remove and repack tiles ",null,"m² ",1,null,null,"Rate only"]
["18.1.5","Remove and repack valley tiles ",null,"m ",1,null,null,"Rate only"]
["18.1.6","Remove tiles, replace underlay and repack ",null,"m² ",1,null,null,"Rate only"]
["18.1.7","Place plaster bond fillet in valley gutter ",null,"m ",1,null,null,"Rate only"]
["18.1.8","Waterproofing to Valley / Noks 500mm membrane",null,"m ",1,null,null,"Rate only"]
["18.1.9","Plaster bond flashing ",null,"m ",1,null,null,"Rate only"]
["18.1.10","Waterproof flashing ",null,"m ",1,null,null,"Rate only"]
[]
[18.2,"b.  Waterproofing Concrete Roof"]
["18.2.1","Strip existing malthoid type membrane ",null,"m² ",1,null,null,"Rate only"]
["18.2.2","Repair and prepare screed surface with plaster bond mixture ",null,"m² ",1,null,null,"Rate only"]
["18.2.3","Prime surface ",null,"m² ",1,null,null,"Rate only"]
["18.2.4","Install torch-on system ",null,"m² ",1,null,null,"Rate only"]
[]
[18.3,"c.  Waterproofing IBR or Corrugated Iron Roofs"]
["18.3.1","Fasten roof screws and replace with new where needed ",null,"m² ",1,null,null,"Rate only"]
[null,"Fasten sheets using rivets ",null,"m² ",1,null,null,"Rate only"]
[null,"Waterproof overlaps with acrylic membrane ",null,"m² ",1,null,null,"Rate only"]
[null,"Waterproof roof screws with acrylic membrane ",null,"m² ",1,null,null,"Rate only"]
[null,"Install torch-on system ",null,"m² ",1,null,null,"Rate only"]
[]
[18.4,"d.  Waterproofing / insulation of surfaces with polymer products"]
["18.4.1","Apply coating of spray-foam (polyurethane type) for insulation / waterproofing "," Material PC ","m² ",1,null,null,"Rate only"]
["18.4.2","Apply coating of spray-epoxy (resin + catalyst, polyuria type)  for insulation / waterproofing / floor covering"," Material PC ","m² ",1,null,null,"Rate only"]
[]
[19,"Table 18:  Rates for Work / Services – Roofing"]
[]
[19.1,"a.  Repairs and Installations Roof Materials Supply and install"]
[]
["19.1.1","Replace broken concrete roof tiles ",null,"each",1,null,null,"Rate only"]
["19.1.2","Replace broken ridge tiles ",null,"each",1,null,null,"Rate only"]
["19.1.3","Refit loose concrete roof tiles ",null,"m²",1,null,null,"Rate only"]
["19.1.4","Replace polyethylene underlay ",null,"m²",1,null,null,"Rate only"]
["19.1.5","Replace Harvey tiles ",null,"each",1,null,null,"Rate only"]
["19.1.6","Replace broken slate tiles ",null,"each",1,null,null,"Rate only"]
["19.1.7","Replace corrugated iron roof sheeting (Minimum 0.5 mm)",null,"m²",1,null,null,"Rate only"]
["19.1.8","Replace corrugated iron roof ridging ",null,"m",1,null,null,"Rate only"]
["19.1.9","Replace IBR roof sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.10","Replace IBR ridging ",null,"m",1,null,null,"Rate only"]
["19.1.11","Replace fiberglass sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.12","Replace polycarbonate sheets ",null,"m²",1,null,null,"Rate only"]
["19.1.13","Replace galvanized valley gutters ",null,"m",1,null,null,"Rate only"]
["19.1.14","Replace fiber cement (Big Six) roof sheeting ",null,"m²",1,null,null,"Rate only"]
["19.1.15","Replace fiber cement (Big Six) ridging ",null,"m",1,null,null,"Rate only"]
["19.1.16","Replace 50mm x 76 mm purlins ",null,"m",1,null,null,"Rate only"]
["19.1.17","Replace 38mm x 38 mm battens ",null,"m",1,null,null,"Rate only"]
["19.1.18","Replace 150mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.19","Replace 225mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.20","Replace 300mm Nutec facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.21","Replace SA pine facia boards ",null,"m",1,null,null,"Rate only"]
["19.1.22","Replace 200mm Nutec barge boards ",null,"m",1,null,null,"Rate only"]
{"$rows_empty":19}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"Section 2"]
[null,"Bill 2"]
[null,"Material supply and Install"]
[]
[]
[20,"Table 19:  Rates for Work / Services: Thatching"]
[null,"All thatching must be calculated on the floor area including the overhangs"]
[20.1,"Remove existing thatch and cart away ","PC item"]
[20.2,"Remove existing thatch and structure and cart away ","PC item"]
[20.3,"Remove laths and battens only ","PC item"]
[20.4,"New Thatch covering complete ","PC item"]
[20.5,"Comb, Brush and minor repairs ","PC item"]
[20.6,"New timber structure (including laths and battens) ","PC item"]
[20.7,"Re-thatch 75 mm thick ","PC item"]
[20.8,"Remove grass ridging ","PC item"]
[20.9,"Repairs to grass ridging ","PC item"]
[20.1,"Replace Fiberglas ridge ","PC item"]
[20.11,"Repairs to fiberglass ridge ","PC item"]
[20.12,"Remove concrete ridging ","PC item"]
[20.13,"Repairs to concrete ridging ","PC item"]
[20.14,"External treatment of thatch cover ","PC item"]
[20.15,"Internal treatment of thatch cover ","PC item"]
[20.16,"External and internal treatment of thatch cover ","PC item"]
[20.17,"New Internal treatment of thatch cover ","PC item"]
[20.18,"Bi annual inspection on all roof trusses","PC item"]
{"$rows_empty":59}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material supply and Install"]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"Section 2"]
[]
[null,"Bill 2"]
[]
[null,"Material supply and Install"]
[]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,28,null,null,0]
[{"$nulls":4},29,null,null,0]
[{"$nulls":4},30,null,null,0]
[{"$nulls":4},31,null,null,0]
[{"$nulls":4},32,null,null,0]
[{"$nulls":4},33,null,null,0]
[{"$nulls":4},34,null,null,0]
[{"$nulls":4},35,null,null,0]
[{"$nulls":4},36,null,null,0]
[{"$nulls":4},37,null,null,0]
[{"$nulls":4},38,null,null,0]
[{"$nulls":4},39,null,null,0]
[{"$nulls":4},40,null,null,0]
[{"$nulls":4},41,null,null,0]
[{"$nulls":4},42,null,null,0]
[{"$nulls":4},43,null,null,0]
[{"$nulls":4},44,null,null,0]
{"$rows_empty":59}
[null,"Total Carried to Collection",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[null,"Section 2"]
[null,"Bill No. 2"]
[null,"Material Schedule Supply and install"]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 3"]
[]
[null,"BILL NO. 1"]
[]
[null,"LABOUR RATES "]
[]
[]
[null,"PREAMBLES"]
[]
[null,"For preambles see \"Model Preambles for Trades (2008 Edition)\" and applicable supplementary preambles as specified in the Trades. The said Model and Supplementary Preambles apply to all work described in this document. Tenderers are therefor referred to these documents for the full meaning and intention of all descriptions as no claims of any kind whatsoever will be entertained in this regard."]
[]
[null,"Rates for Call Outs and Emergency Works"]
[]
[null,"Call outs are for unquoted emergency works either during normal or after hours not applicable to planned services. Fees will be calculated in line with Board Notice 138 of 2015, guideline for Services and Processes for Estimating fees for fees for persons registered in terms of the Engineering Professional Act (ECSA)"]
[]
[null,"Fixed Rates - Artisans and Labours to attend to Emergency Works (shutdown and or any electrical reticulations "]
[]
[null,"Labour Rates Fixed "]
[]
[null,"Normal Hours"]
[1,"Accredited Artisan",null,"p/h",1,null,null,"Rate only "]
[2,"Artisan assistant",null,"p/h",1,null,null,"Rate only "]
[3,"Labour",null,"p/h",1,null,null,"Rate only "]
[]
[null,"Sundays and Public Holidays"]
[4,"Accredited Artisan",null,"p/h",1,null,null,"Rate only "]
[5,"Artisan assistant",null,"p/h",1,null,null,"Rate only "]
[6,"Labour",null,"p/h",1,null,null,"Rate only "]
[]
[null,"After Hours and Saturdays"]
[7,"Accredited Artisan",null,"p/h",1,null,null,"Rate only "]
[8,"Artisan assistant",null,"p/h",1,null,null,"Rate only "]
[9,"Labour",null,"p/h",1,null,null,"Rate only "]
[]
[null,"Fixed Rates"]
[null,"Call out Rates for Emergency`s"]
[null,"Note: Callouts are for unquoted emergency works either during normal or after hours. These rates are not relevant for quotations and planned works"]
[]
[10,"Accredited Artisan",null,"p/h",1,null,null,"Rate only "]
[11,"Artisan assistant",null,"p/h",1,null,null,"Rate only "]
[12,"Labour",null,"p/h",1,null,null,"Rate only "]
[13,"Transport Kilometers will be as per AA rate","PC Item"]
[]
[null,"Material"]
[]
[null,"Mark up on PC Items ","Not Exeeding 12 %"]
[]
[null,"P&G on works above R250 000.00 per item","Total Cost "]
[null,null,"(Excluding % Mark upitems)"]
[]
[null,"Annual Escalation is determined by CPI rate per annum as determined by SSA","Cleint will advice as per Treasury","%"]
{"$rows_empty":15}
[null,"Total Carried to Summary ",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[]
[]
[]
[]
[null,"Section 3"]
[null,"Bill No. 1"]
[null,"Labour Rates "]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 3"]
[]
[null,"BILL NO. 1"]
[]
[null,"RATE ONLY TYPE OF CONTRACT "]
[]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",{"$nulls":3},{"v":46,"d":"46.00"},null,0]
{"$rows_empty":58}
[null,"Total Carried to Summary ",{"$nulls":5},0]
{"$rows_empty":7}
[null,"Section 3"]
[null,"Bill No. 1"]
[null,"Labour Rates "]
[null,"General Building Maintenance"]
["Item",null,null,"Unit","Quantity","Rate",null,"Amounts"]
[null,"SECTION 4"]
[]
[null,"BILL NO. 1"]
[]
[null,"RENTALS OF EQUIPMENT"]
[]
[1,":  Rates for Additional Works – Provision of Specialised Plant and Equipment"]
[null,"(Refer:  The rates of all equipment mention in the table hired must be complete with skilled / qualified / certified operator as required by legislation and inclusive of fuel and transportation costs )"]
[1.1,"TLB ",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.2,"Front loader (1- 2 cubic m scoop capacity)",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.3,"Cherry picker (Up to 15m height capacity, 3m reach from base)",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.4,"Tipper truck (> 5 cub meter)",null,"per km",1,null,null,"Rate only "]
[]
[1.5,"Jack hammer, light duty",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.6,"Jack hammer heavy duty",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.7,"Compacter, light duty",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.8,"Mechanical orga",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.9,"Concrete mixer, fuel driven",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.1,"Portable generator > 5kVA",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.11,"High pressure washer, complete with attachments",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[1.12,"Honeysuckle sewage service",null,"Call out /per liter rate",1,null,null,"Rate only "]
[]
[1.13,"Industrial vacuum cleaner",null,"Daily 8 hrs uninterrupted",1,null,null,"Rate only "]
[]
[]
[null,":  Rates for Additional Works - Provision of Scaffolding"]
[]
[null,"Scaffolding less than 3m forms part of tools inclusive of certification"]
[]
[1.14,"Provision for Scaffolding; for all works, regardless of extent and inclusive of certification will be quotation based.",null,"PC Project Based"]
{"$rows_empty":16}
[null,"Total Carried to Summary ",{"$nulls":3},{"v":0,"d":"0.00"},null,0]
[]
[]
[]
[]
[null,"Section 4"]
[null,"Bill no 1"]
[null,"Rentals of Equipment"]
[null,"General Building Maintenance"]
["Item",{"$nulls":3},"Page No.",null,null,"Amounts"]
[null,"SECTION 4"]
[]
[null,"BILL NO. 1"]
[]
[null,"RENTALS OF EQUIPMENT"]
[]
[null,"COLLECTION"]
[]
[null,"Total Brought forward from page no.",null,null,48,null,null,0]
{"$rows_empty":31}
[null,"Total Carried to Summary ",{"$nulls":5},0]
[]
[]
[null,"Section 4"]
[null,"Bill no 1"]
[null,"Rentals of Equipment"]
[null,"General Building Maintenance"]
[]
["Appointment of a Contractor for the Supply & Maintenance Of General Building Maintenanc  "]
[]
["Bill No.","SUMMARY BUILDING WORK",null,"Page No","Frequency ","Carried to Summary ",null,"Amounts "]
[]
[null,"SECTION 1"]
[]
["Bill no 1","BUILDING AGREEMENT AND PRELIMINARIES  ",null,16,1,{"v":0,"d":"0.00"},null,0]
[]
[null,"SECTION 2"]
[]
["Bill no 1","ALTERATIONS",null,27,1,{"v":0,"d":"0.00"},null,0]
[]
["Bill no 2","MATERIAL SCHEDULE SUPPLY AND INSTALL",null,45,1,{"v":0,"d":"0.00"},null,0]
[]
[null,"SECTION 3"]
[]
["Bill no 1","LABOUR RATES ",null,47,1,{"v":0,"d":"0.00"},null,0]
[]
[null,"SECTION 4"]
[]
["Bill no 1","RENTALS OF EQUIPMENT",null,49,1,{"v":0,"d":"0.00"},null,0]
{"$rows_empty":13}
[null,"Sub-Total ",{"$nulls":5},0]
[]
[]
[null,"Add Contingency @  5%",null,null,"@ 5%",null,null,0]
[]
[null,"Total "]
[]
[null,"Add VAT @ 15%",null,null,"@ 15%"]
[]
[]
[]
[]
[null,"TOTAL ESTIMATED PROJECT COST "]