{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["PRICING"],"not_rendered":{"external_links":1,"defined_names":1,"comments":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PRICING","index":0,"n_rows":318,"n_cols":8,"rows_kept":318,"merged":[[4,2,4,3],[5,2,5,3],[6,2,6,3],[91,0,91,1],[108,0,108,1],[127,0,127,1],[128,0,128,1],[132,0,132,1],[133,0,133,1],[221,0,221,1],[271,1,271,7],[275,1,275,7],[278,1,278,7],[284,0,284,6],[285,0,285,6],[286,0,286,6],[294,0,294,6],[300,0,300,6],[301,0,301,6],[315,0,315,6]],"flags":["formulas_cached_only"]}
["BID RLM - MV & LV CABLES + CONDUCTORS"]
[]
["MV & LV CABLES AND CONDUCTORS"]
[]
["ITEM","DESCRIPTION","PRICE PER",null,null,"TENDER","DELIVERY IN"]
["NO","AS SPECIFIED","UNIT ",null,{"v":0.15,"d":"15%"},"PRICE","RUSTENBURG","STORE "]
[null,null,"FOR RUSTENBURG",null,"V A T","( V A T )","(PERIOD IN","ITEM "]
[null,null,"UNIT","PRICE",null,null,"WEEKS)","NUMBER"]
["11 kV - MV CABLES: TYPE B - UNARMOURED"]
["3 CORE 6,35/11 kV XLPE TYPE B UNARMOURED CABLE ,"]
["INDIVIDUALY SCREENED WITH STRANDED Al CONDUCTORS"]
[]
[1,"35 mm Al ","M",{"$nulls":4},"370006"]
[]
[2,"50 mm Al ","M",{"$nulls":4},"370055"]
[]
[3,"70 mm Al ","M",{"$nulls":4},"370016"]
[]
[4,"95 mm Al ","M",{"$nulls":4},"370026"]
[]
[5,"120 mm Al ","M",{"$nulls":4},"370005"]
[]
[6,"150 mm Al ","M",{"$nulls":4},"3700467"]
[]
[7,"185 mm Al ","M",{"$nulls":4},"370015"]
[]
[8,"240 mm Al ","M",{"$nulls":4},"370050"]
[]
[9,"300 mm Al ","M",{"$nulls":4},"NONE"]
[]
[10,"400 mm Al ","M",{"$nulls":4},"370040"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
["3 CORE 6,35/11 kV XLPE TYPE B UNARMOURED CABLE ,"]
["INDIVIDUALY SCREENED WITH STRANDED Cu CONDUCTORS"]
[]
[11,"300 mm Cu","M",{"$nulls":4},"374020"]
[]
["3 CORE 6,35/11 kV XLPE TYPE A ARMOURED CABLE ,"]
[]
[]
[12,"240 mm Cu","M",{"$nulls":4},"370075"]
[]
["11 kV - MV CABLES: TYPE A (SWA) - ARMOURED"]
["3 CORE 6,35/11 kV XLPE TYPE A ARMOURED CABLE (SWA)"]
["INDIVIDUALY SCREENED WITH STRANDED Al CONDUCTORS"]
[]
[13,"35 mm Al ","M",{"$nulls":4},"NONE"]
[]
[14,"50 mm Al ","M",{"$nulls":4},"NONE"]
[]
[15,"70 mm Al ","M",{"$nulls":4},"NONE"]
[]
[16,"95 mm Al ","M",{"$nulls":4},"NONE"]
[]
[17,"120 mm Al ","M",{"$nulls":4},"NONE"]
[]
[18,"150 mm Al ","M",{"$nulls":4},"NONE"]
[]
[19,"185 mm Al ","M",{"$nulls":4},"NONE"]
[]
[20,"240 mm Al ","M",{"$nulls":4},"NONE"]
[]
[21,"300 mm Al ","M",{"$nulls":4},"NONE"]
[]
[22,"400 mm Al ","M",{"$nulls":4},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["LV CABLES"]
["4 CORE 600/1000 V PVC ; PVC : SWA ;"]
["PVC CABLE WITH SOLID Al CONDUCTOR"]
[]
[23,"50 mm           do","M",{"$nulls":4},"368030"]
[]
[24,"70 mm           do","M",{"$nulls":4},"368035"]
[]
[25,"95 mm           do","M",{"$nulls":4},"368040"]
[]
[26,"120 mm          do","M",{"$nulls":4},"368005"]
[]
[27,"150 mm          do","M",{"$nulls":4},"368010"]
[]
[28,"185 mm          do","M",{"$nulls":4},"368015"]
[]
[29,"240 mm          do","M",{"$nulls":4},"368020"]
[]
[30,"300 mm          do","M",{"$nulls":4},"368025"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["4 CORE 600/1000 V PVC ; PVC : SWA ;"]
["PVC CABLE WITH Cu STRANDED CONDUCTOR"]
[]
[31," 2.5 mm           do","M",{"$nulls":4},"372035"]
[]
[32," 4 mm           do","M",{"$nulls":4},"372060"]
[]
[33," 6 mm           do","M",{"$nulls":4},"372075"]
[]
[34,"10 mm           do","M",{"$nulls":4},"372011"]
[]
[35,"16 mm           do","M",{"$nulls":4},"372025"]
[]
[36,"25 mm           do","M",{"$nulls":4},"372050"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["2 CORE 600/1000 V Cu STRANDED"]
["CONDUCTOR CABLE PVC ; PVC : SWA"]
[]
[37," 2.5 mm           do","M",{"$nulls":4},"372030"]
[]
[38," 4 mm           do","M",{"$nulls":4},"372055"]
[]
[39," 6 mm           do","M",{"$nulls":4},"372070"]
[]
[40,"10 mm           do","M",{"$nulls":4},"372010"]
[]
[41,"16 mm           do","M",{"$nulls":4},"372015"]
[]
[42,"25 mm           do","M",{"$nulls":4},"372045"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
[]
["7 CORE 600/1000 V Cu STRANDED"]
["CONDUCTOR CABLE PVC ; PVC : SWA ; PVC"]
[]
[43,"2,5  mm           do","M",{"$nulls":4},"372040"]
[]
["19 CORE 600/1000 V Cu STRANDED"]
["CONDUCTOR CABLE PVC ; PVC : SWA ; PVC"]
[]
[44,"2,5  mm           do","M",{"$nulls":4},"372001"]
[]
["AIRDAC SNE without pilot cables (Manufactured to SANS 1507 and NRS 063.."]
[]
[45,"10 mm","M",{"$nulls":4},"NONE"]
[]
[46,"16 mm","M",{"$nulls":4},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
[]
[]
["CONDUCTORS"]
[]
["SINGLE CORE PVC INSULATED STRANDED COPPER CONDUCTOR"]
[]
[47,"2.5 mm","M",{"$nulls":4},"408020"]
[]
[48,"4 mm","M",{"$nulls":4},"408050"]
[]
[49,"6 mm","M",{"$nulls":4},"408060"]
[]
[50,"10 mm","M",{"$nulls":4},"NONE"]
[]
["51A","16 mm BLACK","M",{"$nulls":4},"408010"]
[]
["51B","16 mm RED","M",{"$nulls":4},"408012"]
[]
["51C","16 mm WHITE","M",{"$nulls":4},"408013"]
[]
["51D","16 mm BLUE","M",{"$nulls":4},"408014"]
[]
[52,"25 mm","M",{"$nulls":4},"408025"]
[]
[53,"35 mm","M",{"$nulls":4},"408040"]
[]
[54,"50 mm","M",{"$nulls":4},"408055"]
[]
[55,"70 mm","M",{"$nulls":4},"408065"]
[]
[56,"95 mm","M",{"$nulls":4},"408070"]
[]
[57,"120 mm","M",{"$nulls":4},"NONE"]
[]
[58,"150 mm","M",{"$nulls":4},"408005"]
[]
[59,"185 mm","M",{"$nulls":4},"408015"]
[]
[60,"240 mm","M",{"$nulls":4},"NONE"]
[]
[61,"300 mm","M",{"$nulls":4},"408030"]
[]
[62,"35 mm 11kV (HT-tailing)/M ","M",{"$nulls":4},"408035"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
[]
["BARE ANNEALED STRANDED COPPER CONDUCTOR"]
[]
[63,"All Seizes","Kg",{"$nulls":4},"SEE BELOW"]
[null,"4mm EARTHWIRE","Kg",{"$nulls":4},"406035"]
[null,"16mm EARTHWIRE","Kg",{"$nulls":4},"406005"]
[null,"10mm EARTHWIRE","Kg",{"$nulls":4},"405020"]
[null,"25mm EARTHWIRE","Kg",{"$nulls":4},"406025"]
[null,"35mm EARTHWIRE","Kg",{"$nulls":4},"406015"]
[null,"50mm EARTHWIRE","Kg",{"$nulls":4},"406030"]
[null,"150mm EARTHWIRE","Kg",{"$nulls":4},"406031"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["STRANDED ALUMINIUM CONDUCTOR"]
[]
[64,"7/2,06 AAC MIDGE","M",{"$nulls":4},"404020"]
[]
[65,"7/2,79  AAC  LADYBIRD (40)","M",{"$nulls":4},"404045"]
[]
[66,"7/3,40  AAC FLY (63)","M",{"$nulls":4},"404050"]
[]
[67,"7/4,39   AAC WASP (100)","M",{"$nulls":4},"404055"]
[]
[68,"19/3,25  AAC HORNET","M",{"$nulls":4},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["STRANDED Al CONDUCTOR - STEEL RE-INFORCED"]
[]
[69,"6/1/2,36  A.C.S.R.  GOPHER (25)","M",{"$nulls":4},"404040"]
[]
[70,"6/1/3,35  A.C.S.R. RABBIT (50)","M",{"$nulls":4},"404025"]
[]
[71,"6/1/3,66 A.C.S.R. MINK (63)","M",{"$nulls":4},"404030"]
[]
[72,"6/1/4,72  A.C.S.R. HARE (100)","M",{"$nulls":4},"404035"]
[]
[73,"30/7/3.35  A.C.S.R. (Bear) (264)","M",{"$nulls":4},"NONE"]
[]
[74,"54/7/3.18  A.C.S.R. (Zebra) (428)","M",{"$nulls":4},"NONE"]
[]
[75,"Kingbird","M",{"$nulls":4},"NONE"]
[]
[76,"Bersford (687.4)","M",{"$nulls":4},"NONE"]
[]
[77,"Tsikdoo","M",{"$nulls":4},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["ABC BUNDLE CONDUCTOR WITH BARE NEUTRAL  (To conform to SCSSCAAD5) and SANS 1418 Part 1 and 2"]
[]
[78,"3 X 70 + 54.6","M",{"$nulls":4},"368045"]
[]
[79,"3 X 95 + 54.6","M",{"$nulls":4},"368050"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
["ABC BUNDLE CONDUCTOR WITH ISOLATED NEUTRAL  (To conform to SCSSCAAD5) and SANS 1418 Part 1 and 2"]
[]
[80,"3 X 70 + 54.6","M",{"$nulls":4},"NONE"]
[]
[81,"3 X 95 + 54.6","M","add",{"$nulls":3},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
["ABC BUNDLE CONDUCTOR WITH BARE NEUTRAL  (To conform to SCSSCAAD5) and SANS 1418 Part 1 and 2"]
[]
[82,"3 X 35 + 35 Bare Neutral","M",{"$nulls":4},"368055"]
[]
[83,"1 X 35 + 35 Bare Neutral","M",{"$nulls":4},"NONE"]
[]
[84,"3 X 70 + 70 Bare Neutral","M",{"$nulls":4},"NONE"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[85,"3 x 70 + 54.6 Insulated Neutral with Streetlight conductor (70x3+55IN + 25SL)"]
[85,null,"M",{"$nulls":4},"363072"]
[]
[]
[86,"3 x 95 + 54.6 Insulated  Neutral with Streetlight conductor (95x3+55IN + 25SL)"]
[86,null,"M",{"$nulls":4},"363071"]
[]
[87,"3 x 120 + 54.6 Insulated  Neutral with Streetlight conductor (120x3+55IN + 25SL)"]
[87,null,"M",{"$nulls":4},"363070"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
["33kV HV CABLES"]
["Three (3) Core Stranded Copper conductor, semi conductive screen, XLPE Insulated, semi conductive layer over insulation, "]
["semi conductive layer tape, Cu Wire Screen, Waterblocked, Medium Density Polyethelene sheathed semicon "]
["coated – (earthed) type “A2” “B”, 19 - 33 kV to SANS 1339 (swellable tapes under and over the Cu Wire Screen)” or Simmilar.   COMPULSORY - TO SUBMIT DATA SHEET FOR TECHNICAL EVALUATION."]
["Type Cu 240mm2 3C XLPE WB CWS (50) WB MDPE MINEX"]
[]
[88,"240 mm CU X 3 CORE XLPE MDPE","M",{"$nulls":4},"374025"]
[]
["Single Core Stranded Copper conductor, semi conductive screen, XLPE Insulated, semi conductive "]
["layer over insulation, semi conductive layer tape, Cu Wire Screen, Waterblocked, Medium Density"]
[" Polyethelene sheathed semicon coated – typeB”, 19 - 33 kV to SANS 1339 (swellable tapes"]
["under and over the Cu Wire Screen)” COMPULSORY TO SUBMIT DATA SHEET FOR TECHNICAL EVALUATION."]
[]
[89,"500 mm CU X 1 CORE XLPE","M",{"$nulls":4},"374030"]
[]
["Single Core Aluminium conductor, semi conductive screen, XLPE Insulated, semi conductive"]
[" layer over insulation, semi conductive layer tape, semi conducting bedding tape, 0.2 mm Cu Tape"]
[" Screen, Waterblocked, Medium Density Polyethelene  sheathed semicon coated – type \"B”,"]
[" 19 - 33 kV to SANS 1339 (swellable tapes under and over the Cu Tape Screen)” COMPULSORY TO SUBMIT DATA SHEET FOR TECHNICAL EVALUATION."]
[]
[90,"300 mm AL X 1 CORE XLPE MDPE","M",{"$nulls":4},"370030"]
[]
[91,"500 mm AL X 1 CORE XLPE MDPE","M",{"$nulls":4},"370050"]
[]
[92,"800 mm ALX 1 CORE XLPE MDPE","M",{"$nulls":4},"370065"]
[]
[{"$nulls":5},"TOTAL FOR BATCH"]
[]
[]
[]
["88kV HV CABLES"]
[]
["Single (1) Core 500mm2 compacted class 2 aluminium conductor to IEC 60228, Triple layer, simultaneously extruded, cross linked semi conductive conductor screen, Cross linked Polyethylene Insulation, non strippable cross-linked semi conducting core screen insulation. \nCorrugated Seamless Aluminium (CSA) screen and black MPDE sheath, resistant and protected against radial and longitudinal water penetration and meets the requirements of EC 60840 and Embossed. \nThe cable shall also be tested in accordance with IEC 60840 \"COMPULSORY TO SUBMIT DATA SHEET FOR TECHNICAL EVALUATION\".                   "]
[]
[93,"500 mm AL X 1 CORE XLPE MDPE","M"]