{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Summary","BOQ"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Summary","index":0,"n_rows":28,"n_cols":3,"rows_kept":28,"merged":[[0,0,0,2],[15,0,15,1],[17,0,17,1],[19,0,19,1],[21,0,21,1],[23,0,23,1],[25,0,25,1],[27,0,27,1]],"flags":["formulas_cached_only"]}
["Summary of Sections"]
[]
["ITEM","DESCRIPTION","AMOUNT"]
[]
[]
["Section A","Preliminary and General "]
[]
["Section B","Earthworks"]
[]
["Section C","Pipework"]
[]
["Section D","Sundries"]
[]
["Section E","Dayworks"]
[]
["Sub Total 1"]
[]
["Contingencies @ 10%"]
[]
["Sub Total 2"]
[]
["Escalation @ 12%"]
[]
["Sub Total 3"]
[]
["VAT @ 15%"]
[]
["Contract Amount to the Form of Offer"]

{"sheet":"BOQ","index":1,"n_rows":323,"n_cols":9,"rows_kept":323,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[32,0,32,2],[33,0,33,2],[73,0,73,2],[119,0,119,2],[120,0,120,2],[145,0,145,2],[198,0,198,2],[199,0,199,2],[241,0,241,2],[242,0,242,2],[272,0,272,2],[309,0,309,2],[322,0,322,2]],"flags":["formulas_cached_only"]}
[]
["RUSTENBURG MUNICPALITY"]
["TLHABANE BULK AC WATER REPLACEMENT AND INTERNAL RETICULATION:PHASE 2B"]
["BOQ "]
[" "]
["ITEM","PAYMENT REF","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["Section A","SABS 1200 A PSA","Preliminary and General "]
[]
["A1",8.3,"FIXED-CHARGE ITEMS"]
["A1,1","8.3.1","Contractual Requirements","Sum ",1,null,0]
[]
["A1,2","8.3.2","Facilities for the Engineer (Site Office, Site Board and Survey Equipment)"]
["A1,2,1",null,"Engineer's Site Office","Sum ",1,null,0]
["A,1,2,2",null,"Name Board","Sum ",1,null,0]
["A,1,2,3",null,"Survey Equipment","Sum ",1,null,0]
["A,1,2,4",null,"Engineer's Laptop/Printer for the duration of the Contract","Sum ",1,null,0]
[]
["A1,3",null,"Facilities for the Contractor (Offices, Storage sheds, workshops, Water on site, Establishment, Compliance with EMP & OHS and Training of Labour)",{"$nulls":3},0]
["A1,3,1",null,"Offices, storage sheds, workshops and living accommodation.","Sum ",1,null,0]
["A1,3,2",null,"Ablution and latrine facilities","Sum ",1,null,0]
["A1,3,3",null,"Tools, equipment and plant","Sum ",1,null,0]
["A1,3,4",null,"Water supplies, electric power, communications and access","Sum ",1,null,0]
["A1,3,5",null,"Dealing with water:",{"$nulls":3},0]
[null,null,"a) Generally on site","Sum ",1,null,0]
["A1,3,6","8.3.3","Other fixed-charge obligations","Sum ",1,null,0]
["A1,3,7","8.3.4","Remove Contractor's site establishment on completion","Sum ",1,null,0]
["A1,3,8",null,"Accommodation of traffic including road signage as necessary","Sum ",1,null,0]
["A1,3,9",null,"Preparation of risk assessments, safe work procedures, the project H&S File, the H&S plan, the provision of PPE .The sum shall include all fixed costs necessary in complying with the OHS Act (1993 as amended) and the Construction Regulations (2003)  and the Health and Safety Specifications.  ","Sum ",1,null,0]
["A1,3,10",null,"Completing and checking the Project H&S File and handing over the Client on completion of the works","Sum ",1,null,0]
["A1,3,11",null,"Compliance with requirements of the project Environmental Management Plan","Sum ",1,null,0]
[]
["SUBTOTAL CARRIED FORWARD",{"$nulls":5},0]
["SUBTOTAL BROUGHT FORWARD",{"$nulls":5},0]
[]
["A,2",8.4,"Time Related Items"]
["A.2,1","8.4.1","Contractual requirements","Month",15,null,0]
["A2,2","8.4.2","Operate and maintain facilities on the site for the duration of construction:","Month",15,null,0]
["A2,3",null,"Facilities for the Engineer-",{"$nulls":3},0]
["A,2,3,1",null,"Nameboard ","Month",15,null,0]
["A,2,3,2",null,"Survey equipment (Including the use of a trained survey assistant)","Month",15,null,0]
["A,2,3,3",null,"Engineer's site offices including consumables for laptop printer ","Month",15,null,0]
["A,2,3,4",null,"Engineer's Accomodation Cost","Month",15,null,0]
["A,2,3,5",null,"Other time related obligations including Engineer's cellular telephone calls and rental cost","Month",15,null,0]
["A2,4","8.4.2.1","Facilities for the Contractor-",{"$nulls":3},0]
["A2,4,1",null,"Contractor's establishment as per Item A.1,3,1","Month",15,null,0]
["A2,4,2",null,"Dealing with water:",{"$nulls":3},0]
[null,null,"a) Generally on the site","Month",15,null,0]
["A2,4,3",null,"Management and Supervision of Sub Contractors on the Contract","Month",15,null,0]
["A2,4,4","8.4.3","Supervision for duration of construction","Month",15,null,0]
["A2,4,5",null,"Appointment of a full time  construction health and safety officer for the duration of construction works","Month",15,null,0]
["A2,4,6",null,"Accommodation of traffic and maintance of vehicular access to properties","Month",15,null,0]
["A2,4,7","8.4.4","Company and head office overhead costs for the duration of the contract","Month",15,null,0]
["A2,4,8","8.4.5","Other time-related obligations","Month",15,null,0]
["A2,4,9",null,"Updating and amending the risk assessments, safe work procedures, the project H&S File, the H&S plan, the provision of PPE and protective clothing and any other H&S matters that the contractor deems necessary. Rate to include for COVID-19 Virus as detailed in the specifications","Month",15,null,0]
["A2,4,10",null,"Full compliance with all H&S matters during the construction of the works under the contract including all COVID-19 Protocols and procedures","Month",15,null,0]
["A2,4,10",null,"Compliance with requirements of the project Environmental Management Plan","Month",15,null,0]
["A2,4,11",null,"Other time related obligations","Month",15,null,0]
[]
["A3",null,"Provisional Sums",{"$nulls":3},0]
["A,3,1",null,"Locate existing services where ordered","Sum",1,120000,{"v":120000,"d":"120,000.00"}]
["A,3,2",null,"Inspection by Surveyor appointed by the Engineer ","Sum",1,300000,{"v":300000,"d":"300,000.00"}]
[null,null,"Inspection of Materials by Inspectors appointed by the Engineer ","Sum",1,150000,{"v":150000,"d":"150,000.00"}]
["A,3,3",null,"Water for testing pipelines and structures (1 filling)","Sum",1,150000,{"v":150000,"d":"150,000.00"}]
["A,3,4",null,"Allowance for Engineer's technical Assistant for duration of construction works","Sum",1,105000,{"v":105000,"d":"105,000.00"}]
["A,3,5",null,"Engineer's Representative cell phone calls","Sum",1,90000,{"v":90000,"d":"90,000.00"}]
["A,3,6",null,"Engineer's Representative accomodation costs","Sum",1,360000,{"v":360000,"d":"360,000.00"}]
["A,3,7","PC11","Allowance for CLO","Sum",1,270000,{"v":270000,"d":"270,000.00"}]
["A,3,8",null,"Allowance for Engineer appointed ISD/Social Facilitator","Sum",1,900000,{"v":900000,"d":"900,000.00"}]
["A,3,9","PS 12","Inspections by appointed Health and Safety Auditors","Sum",1,350000,{"v":350000,"d":"350,000.00"}]
["A,3,10","PD","Inspections by appointed Environmental Auditors","Sum",1,350000,{"v":350000,"d":"350,000.00"}]
["A,3,11",null,"Contractor's mark up on items A.3,1 to A,3,8","Sum",{"v":3145000,"d":"3,145,000.00"},null,0]
[]
["Sub-Total Carried to Summary - Section A",{"$nulls":5},{"v":3145000,"d":"3,145,000.00"}]
[]
["Section B","SABS 1200 DB","Earthworks"]
["B1",null,"Site Clearance"]
["B1,1","PSDB 7","a) Site Clearance (Clear Vegetation, Remove and reinstate fences, removal and stockpile topsoil)","m",5880,null,0]
[null,null,"(b) Lifting up existing paving blocks including neatly, stacking on site designated by the Engineer (to be re-used, and re-use measured elsewhere)"]
[null,null,"i) 60mm paving","m²",15470,null,0,{"v":16500,"d":"16,500.00"}]
[null,null,"ii) 80mm paving","m²",12780,null,0,{"v":28250,"d":"28,250.00"}]
[{"$nulls":6},0]
[null,null,"(c) Demolish and spoil material for paving, structures, buildings, etc at a spoil site established by the Contractor"]
[null,null,"i) 150mm Thick concrete paving ","m²",9235,null,0]
[]
["B1,2",null,"Setting out of the works as per site plan issued by Engineer ","Sum'",1,null,0]
[]
["B2","PSDB ","Excavations"]
[null,null,"Rates to include for compaction tests of backfill materials as directed by the Engineer "]
[null,null,"Excavate in all materials for trenches, backfill, compact or dispose of surplus / unsuitable material, for:"]
["B,2,1",null,"Excavation for minor Structures ","m³",1950,null,0]
[null,null,"Pipe Trenching (Excavate in all material for tenches, backfill, compact or dispose surplus for pipes with a diameter of 201mm to 500mm at a depth of :"]
["B2,2",null,"Excavation by Machine"]
["B.2,2,1",null,"0,0 m            1,0m","m",11650,null,0]
["B.2,2,2",null,"1,0m             2,0m","m",3350,null,0]
["B.2,2,3",null,"2,0m             3,0m","m",150,null,0]
["B.2,2,4",null,"3,0m             4,0m","m",200,null,0]
[]
[null,null,"Pipe Trenching (Excavate in all material for tenches, backfill, compact or dispose surplus for pipes with a diameter of 201mm to 500mm at a depth of :"]
["B2,3",null,"Excavation by Hand"]
["B.2,3,1",null,"0,0 m            1,0m","m",16500,null,0]
["B.2,3,2",null,"1,0m             2,0m","m",5000,null,0]
["B.2,3,3",null,"2,0m             3,0m","m",550,null,0]
["B.2,3,4",null,"3,0m             4,0m","m",150,null,0]
[{"$nulls":6},0]
["B,3",null,"E.O item B2,2",{"$nulls":3},0]
["B,3,1",null,"Intermediate excavation","m³",2448,null,0,{"v":15000,"d":"15,000.00"},{"v":2250,"d":"2,250.00"}]
["B,3,2",null,"Hard rock excavation","m³",1120,null,0]
[{"$nulls":6},0]
["B,4",null,"Restricted Excavation",{"$nulls":3},0]
[null,null,"Excavate in all materials for trenches, backfill, compact or dispose of surplus / unsuitable material, for: Widths of less than 1000m ",{"$nulls":3},0]
[null,null,"Excavation by Hand",{"$nulls":3},0]
[null,null,"0,0 m            1,0m","m",1950,null,0]
[null,null,"1,0m             2,0m","m",988,null,0]
[{"$nulls":6},0]
["B5",null,"Backfill Material",{"$nulls":3},0]
["B5,1",null,"Imported backfill material from commercial sources","m³",4050,null,0,{"v":8250,"d":"8,250.00"}]
["B5,2",null,"Imported backfill material from designated borrow pit","m³",3375,null,0]
[]
["SUBTOTAL CARRIED FORWARD",{"$nulls":5},0]
["SUBTOTAL BROUGHT FORWARD",{"$nulls":5},0]
[]
["B6",null,"Services that Intersect a Trench:",{"$nulls":3},0]
["B6,1",null,"Stormwater pipes up to 600mm dia","No",265,null,0]
["B6,2",null,"Water mains 20mm to 150mm dia","No",1250,null,0]
["B6,3",null,"Sewer lines up to 350mm dia","No",50,null,0]
[]
["B7",null,"Services that adjoin a Trench"]
["B7,1",null,"Stormwater pipes up to 600mm dia","m",350,null,0]
["B,7,2",null,"Water mains 20mm to 150mm dia","m",8750,null,0]
["B,7,3",null,"Sewer lines up to 350mm dia","m",8750,null,0]
[]
["B8",null,"Roads Crossing"]
["B,8,1",null,"Excavation across tarred roads","m",1850,null,0]
["B,8,2",null,"Compaction under road crossings","m",1850,null,0]
["B,8.3",null,"Reinstating of Tar roads complete with hot mix asphalt","m",1850,null,0]
[{"$nulls":6},0]
["B9","SABS 1200LG","Horizontal Direct Drilling",{"$nulls":3},0]
["B,9,1",null,"Horizontal directional drilling 200mm HDPE Pipe including GPRS scanning","m",325,null,0,{"v":13,"d":"13.00"}]
["B,9,2",null,"Horizontal directional drilling 160mm HDPE Pipe including GPRS scanning","m",300,null,0]
[]
["B,10",null,"Stone Bedding"]
["B,10,1",null,"Supply and place stone bedding","m³",50,null,0]
["B,10,2",null,"Supply and lay geotextile fabric (as Kaymat U14)","m²",125,null,0]
[]
["Sub-Total Carried to Summary - Section B",{"$nulls":5},0]
[]
["ITEM",null,"DESCRIPTION",null,"QTY","RATE","AMOUNT"]
[]
["Section C","SABS 1200L ","Pipework"]
["C1,1","SABS 1200 LB","Bedding & Blanket Material"]
["C1,1",null,"Provision of Bedding (Selected from trenches)","m3",8050,null,0,{"v":1810.8999999999999,"d":"1,810.90"},{"v":905.4499999999999,"d":"905.45"}]
["C1,2",null,"Provision of Bedding (from Commercial Sources)","m3",2810,null,0]
["C1,3",null,"Concrete bedding cradle","m3",115,null,0]
["C1,4",null,"Concrete encasing of pipes in trenches in 20/19 concrete","m3",50,null,0]
[]
["C2","8.2.2","Pressure Pipes (Class 16)"]
[null,null,"Supply, handle, lay,test & disinfect SABS approved PVC pipes and fittings. Flanges to SABS 1123 table 1600. Rate to include for cutting pipes to lengths to suit on site, pressure testing and disinfection "]
["C2,1",null,"200mm Dia uPVC Class 16","m",3850,null,0,{"v":13150,"d":"13,150.00"}]
["C2,2",null,"160mm Dia uPVC Class 16","m",2765,null,0]
["C2,3",null,"110mm Dia uPVC Class 16","m",2950,null,0]
["C2,4",null,"75mm Dia uPVC Class 16","m",3585,null,0,null,"customercare@iwyze.co.za"]
[]
["C3",null,"Pressure bends (Class 16)"]
[null,null,"200mm uPVC bends"]
["C3,1.1",null,"200mm dia x 90 deg Z Lok PVC bend","No.",1,null,0]
["C3,1,2",null,"200mm dia x 45 deg Z Lok PVC bend","No.",4,null,0]
["C3,1,3",null,"200mm dia x 22,5 deg Z Lok PVC bend","No.",4,null,0]
["C3,1,4",null,"200mm dia x 11,25 deg Z Lok PVC bend","No.",2,null,0]
[]
[null,null,"160mm uPVC bends"]
["C3,2,1",null,"160mm dia x 90 deg Z Lok PVC bend","No.",1,null,0]
["C3,2,2",null,"160mm dia x 45 deg Z Lok PVC bend","No.",3,null,0]
["C3,2,3",null,"160mm dia x 22,5 deg Z Lok PVC bend","No.",3,null,0]
["C3,2,4",null,"160mm dia x 11,25 deg Z Lok PVC bend","No.",1,null,0]
[]
[null,null,"110mm uPVC bends"]
["C3,3,1",null,"110mm dia x 90 deg Z Lok PVC bend","No.",6,null,0]
["C3,3,2",null,"110mm dia x 45 deg Z Lok PVC bend","No.",7,null,0]
["C3,3,3",null,"110mm dia x 22,5 deg Z Lok PVC bend","No.",3,null,0]
["C3,3,4",null,"110mm dia x 11,25 deg Z Lok PVC bend","No.",2,null,0]
[]
[null,null,"75mm uPVC bends"]
["C3,5,1",null,"75mm dia x 90 deg Z Lok PVC bend","No.",6,null,0]
["C3,5,2",null,"75mm dia x 45 deg Z Lok PVC bend","No.",14,null,0]
["C3,5,3",null,"75mm dia x 22,5 deg Z Lok PVC bend","No.",10,null,0]
["C3,5,4",null,"75mm dia x 11,25 deg Z Lok PVC bend","No.",10,null,0]
[{"$nulls":6},0]
["C3,6",null,"Cast iron Tees (Class 16)",{"$nulls":3},0]
["C3,6,1",null,"200 x 200","No",6,null,0]
["C3,6,2",null,"160 x 160","No",4,null,0]
["C3,6,3",null,"110 x 110","No",12,null,0]
["C3,6,4",null,"75 x 75","No",12,null,0]
[{"$nulls":6},0]
["C3,7",null,"Reducers (Class 16)",{"$nulls":3},0]
["C3,7,1",null,"200mm x 110mm","No",6,null,0]
["C3,7,2",null,"110mm x 75mm","No",8,null,0]
[]
["SUBTOTAL CARRIED FORWARD",{"$nulls":5},0]
["SUBTOTAL BROUGHT FORWARD",{"$nulls":5},0]
[{"$nulls":6},0]
["C3,8",null,"Flanger Adapters",{"$nulls":3},0]
["C3,8,1",null,"200mm","No",8,null,0]
["C3,8,2",null,"160mm","No",14,null,0]
["C3,8,3",null,"110mm","No",10,null,0]
["C3,8,4",null,"75mm","No",12,null,0]
[{"$nulls":6},0]
["C3,9",null,"End caps (Class 16)",{"$nulls":3},0]
["C3,9,1",null,"200mm","No",2,null,0]
["C3,9,2",null,"160mm","No",2,null,0]
["C3,9,3",null,"110mm","No",2,null,0]
["C3,9,4",null,"75mm","No",2,null,0]
[{"$nulls":6},0]
["C3,10",null,"Pipes and Fittings for Bulk Meter Chamber ",{"$nulls":3},0]
["C3,10,1",null,"150mm diameter x 600mm long D/FL pipe","No",3,null,0]
["C3,10,2",null,"150mm diameter water meter","No",3,null,0]
["C3,10,3",null,"150mm diameter Elter Kent Water Meter","No",3,null,0]
["C3,10,2",null,"150mm diameter Y-Strainer Strainer","No",3,null,0]
["C3,10,3",null,"150mm diameter x 300mm long FL/PE pipe","No",3,null,0]
["C3,10,4",null,"150mm diameter VJ adaptor ","No",3,null,0]
["C3,10,5",null,"250mm dia x 150mm dia flanged eccentric reducer","No",3,null,0]
["C3,10,6",null,"450mm dia x 150mm dia flanged eccentric reducer",null,1,null,0]
["C3,10,7",null,"150mm dia wedge gate valve with square cap ","No",3,null,0]
[{"$nulls":6},0]
["C3,11","PSL 5","Valves",{"$nulls":3},0]
[null,"8.2.3","Supply, handle, lay, joint, test and disinfect RSV valves. All valves to be SABS approved, (flanged to SABS 1123, table 2500). Rate to include for all bolts, nuts, gaskets and jointing material",{"$nulls":3},0]
["C3,11,1",null,"75mm dia wedge gate valve with square cap","No",12,null,0]
["C3,11,2",null,"110mm dia wedge gate valve with square cap","No",15,null,0]
["C3,11,3",null,"160mm dia wedge gate valve with square cap ","No",8,null,0]
["C3,11,4",null,"200mm dia wedge gate valve with square cap ","No",5,null,0]
[]
["C3,12",null,"HDPE pipes SABS 533"]
[null,null,"Supply, handle, lay and test  HDPE pipes and fittings (Plasson compression fittings or similar approved)"]
[null,null,"Pipes "]
["C3,12,1",null,"25mm dia, Class 16","m",16500,null,0]
["C3,12,2",null,"32mm dia, Class 16","m",5500,null,0]
["C3,12,3",null,"40mm dia, Class 16","m",100,null,0]
["C3,12,4",null,"50mm dia, Class 16","m",5000,null,0]
["C3,12,5",null,"160mm dia, Class 16","m",300,null,0]
["C3,12,5",null,"200mm dia, Class 16","m",325,null,0]
[]
["SUBTOTAL CARRIED FORWARD",{"$nulls":5},0]
["SUBTOTAL BROUGHT FORWARD",{"$nulls":5},0]
[]
["C3,13",null,"Male Adaptors (Class 16)"]
["C3,13,1",null,"25mm x 1\" Male Adaptor","No",1100,null,0]
["C3,13,2",null,"32mm x 1½\",\",N°\"","No",550,null,0]
[{"$nulls":6},0]
["C3,14",null,"Compression Tees (Class 16)",{"$nulls":3},0]
["C3,14,1",null,"32mm x 1\" ","No",275,null,0]
["C3,14,2",null,"25mm x 1\"","No",275,null,0]
["C3,14,3",null,"32mm x 1½\"","No",275,null,0]
[]
["C3,15",null,"Saddles (Class 16)"]
["C3,15,1",null,"50 mm x 1½\"","No",80,null,0]
["C3,15,2",null,"75 mm x 1½\"","No",175,null,0]
["C3,15,3",null,"110 mm x 1½\"","No",175,null,0]
[]
[]
["C3,13",null,"Pipes and Fittings for PRV and Meter Chamber ",{"$nulls":3},0]
["C3,13,1",null,"150mm diameter Bermad PRV ","No",2,null,0]
["C3,13,2",null,"150mm diameter Copper to Female Coupling","No",2,null,0]
["C3,13,3",null,"150mm diameter Stainless Spool Piece","No",2,null,0]
["C3,13,4",null,"150mm diameter Gate Valve (MF)","No",2,null,0]
["C3,13,5",null,"150mm diameter Copper to Male Coupling","No",2,null,0]
["C3,13,6",null,"150mm diameter Threaded Loose Flange","No",2,null,0]
["C3,13,7",null,"150mm diameter Bulk Water Meter","No",2,null,0]
["C3,13,8",null,"150mm diameter Male Adaptor to suit","No",2,null,0]
["C3,13,9",null,"150mm diameter Stainless Steel Pipe ","No",2,null,0]
[]
["C.14",null,"Supply and install EZ3 Elster Kent domestic water meter, rate to include for valves and fittings onto 25mm HDPE pipe ","No",580,null,0]
[]
["Sub-Total Carried to Summary - Section C",{"$nulls":5},0,{"$error":"#REF!"},{"$error":"#REF!"}]
[]
["Section D",null,"Sundries"]
[]
["D1",null,"Valve Chambers"]
["D1,1",null,"Supply all materials and construct complete chambers. Pipes and fittings scheduled elsewhere","No.",29,null,0]
[]
["D2",null,"Concrete "]
["D2,1",null,"Anchor blocks in Grade 20/19 concrete as per Drawing N° WN14-D03 (incl. rough shuttering)","m3",25,null,0]
[]
["D3",null,"Marker Posts"]
["D3,1",null,"Supply and install LV, SV and AV marker posts as per Drawing N° DXX (painted with yellow marking paint) including for concrete surround","No.",29,null,0]
[]
["D4",null,"Supply and apply Denso protection to SCJ's, flanges, VJ couplings and VJ adaptor joints :","No.",60,null,0]
[]
["D5",null,"Supply and install M-T-L MC 10 Discus 0370 padlock as supplied by Multi Locking Systems only one security key needed","No.",29,null,0]
[]
["D6",null,"Provisional Sums","Sum",1,750000,{"v":750000,"d":"750,000.00"}]
["A,3,11",null,"Contractor's mark up on items A.3,1 to A,3,8","Sum",750000,{"v":0.1,"d":"10%"},{"v":75000,"d":"75,000.00"}]
[]
["D7",null,"Air Valves",{"$nulls":3},0]
["D7,1",null,"200mm dia. flanged double orifice air valves,class 16, (Vent-O-Mat RBX 2501 or similar approved)","No.",5,null,0]
["D7,2",null,"160mm dia. flanged double orifice air valves,class 16, (Vent-O-Mat RBX 2501 or similar approved)","No.",2,null,0]
["D7,3",null,"110mm dia. flanged double orifice air valves,class 16, (Vent-O-Mat RBX 2501 or similar approved)","No.",5,null,0]
["D7,4",null,"75mm dia. flanged double orifice air valves,class 16, (Vent-O-Mat RBX 2501 or similar approved)","No.",5,null,0]
[{"$nulls":6},0]
["D8",null,"Reinstatement of roads, driveways and private properties",{"$nulls":3},0]
[null,null,"Supply & construct 150mm gravel wearing course  for paved areas in Tlhabane using G5 quality gravel compacted to 98% Mod Aashto","m²",12988,null,0,{"v":12988,"d":"12,988.00"}]
["D8,1",null,"Brick paved driveways","m²",9850,null,0]
["D8,2",null,"Concrete surfaced driveways and pavements","m²",7750,null,0]
["D8,3",null,"Kerbing and channelling in driveways and roadways","m",8500,null,0]
["D8,4",null,"Bitumeninous surfaced roads 30-50mm thick asphalt layer on tar tack coat.","m²",500,null,0]
[]
["D9",null,"Fire Hydrants","No.",18,null,0]
[]
["D10",null,"Disconnect, dewater and decommision in place all existing AC Reticulation Pipes (16km)","Sum",1,null,0]
[]
["Sub-Total Carried to Summary - Section D",{"$nulls":5},{"v":825000,"d":"825,000.00"}]
[]
["ITEM",null,"DESCRIPTION",null,"QTY","RATE","AMOUNT"]
[]
["Section E",null,"Dayworks"]
[]
["E1",null,"Labour","Sum",1,null,0]
[{"$nulls":6},0]
["E2",null,"Plant","Sum",1,null,0]
[{"$nulls":6},0]
["E3",null,"Materials","Sum",1,null,0]
[{"$nulls":6},0]
[]
["Sub-Total Carried to Summary - Section E",{"$nulls":5},0]