Compulsory requirements 
· Bidders must be registered with the Construction Industry Development Board (CIDB) and should have an active CIDB Contractor grading of 1GB or higher (Provide CRS number for verification)
· Gant chart project plan should be submitted - Maximum of 30 days for the project to be completed upon purchase order receipt
· [bookmark: _Hlk199835467]Bidder must attend the compulsory site briefing (Briefing session attendance register must be signed at briefing meeting)
Failure to submit all the above compulsory requirements will lead to disqualification


	

	

	Service description
	UoM
	QTY
	Unit Price VAT Exclusive R
	Total cost Vat Excusive R

	Painting walls with external weatherguard paint, natural hessian in color -two coats (outside of the structure) - External walls
	7.1m(L)x6.1m(W)X3M(H)
	          1                
	 R
	R

	Removal of tiles from interior walls
Painting  walls with matt/medium sheet paint, gentle green-two coats - internal walls
	7.1m(L)x6.1m(W)X3M(H)
	                            1
	 R
	R

	Demolition of walls, and brick bins in second room, and plaster affected walls area for ease of painting
	 
	1
	 R
	R

	Demolition of building (Next door) and clear the rubble from site
	7.4m(L)x7.4m(W)X2.8M(H)
	                             1
	 R
	R

	Remove old aircon, and fill space with bricks and plaster
	0.9m(L)x0.8m(W)
	1
	R
	R

	Supply and install powder coated security window burglar gates similar to Trellis one.
	1. 2mx1m(2 windows)                                 2. 1mx1m(3 windows)
	5
	R
	R

	Supply and install alluminium windows: top hung
	1. 2mx1m(2 windows)                                 2. 1mx1m(3 windows)
	5
	 R
	R

	Painting of window sills (outside)
	According to measurement above
	5
	 R
	R

	Supply and install powder coated security doors/burglar gates similar to Trellis one, covering the entire outside door.
	1. 2.1mx1.2m(1 door)                                 2.  2.1 mx 0.9m(1 door)
	2
	 R
	R

	Supply and install alluminium full frosted glass doors together  with a frame and  complete lockset
	1. 2.1mx1.2m(1 door)                                 2.  2.1 mx 0.9m(1 door)
	2
	 R
	R

	Cutting the tree stump low to the ground and paint the stump with a herbicide such as 9% Triclopyr , Kaput 100 gel or 20% Glyphosate
	 
	3
	 R
	R

	Supply and install 5ft LED light with double tubes
	 
	2
	 R
	R

	Supply and install complete electrical single phase DB unit to its full operation, and issue electrical C.O.C
	 
	1
	 R
	R

	Supply and install electric double plugs
	 
	4
	 R
	R

	Supply and install electric single light switches
	 
	1
	 R
	R

	Supply and install outdoor lights and,  day and night switches
	 
	4
	 R
	R

	Supply and fitting of blinds: roller blinds (block out)
	1. 2mx1m(2 windows)                                 2. 1mx1m(3 windows)
	5
	 R
	R

	Supply and fitting of insect nets protector on aluminium frame
	1. 2mx1m(2 windows)                                 2. 1mx1m(3 windows)
	5
	 R
	R

	Supply and fitting of Upper Edge Classic decorated polystyrene cornice (100x100)
	7.1m(L)x6.1m(W)
	 
	 R
	R

	Replacement of ceiling and paint with white ceiling paints-two coats
	7.1m(L)x6.1m(W)
	 
	 R
	R

	Painting roof with rubber paint, maroon in color - specific paint for IBR metal roofing, two coats- the roof must be prepared and waterproofed before painting
	7.1m(L)x6.1m(W)
	 
	 R
	R

	Build concrete apron of 100mm thickness and 1m wide around the building
	7.1m(L)x6.1m(W)
	 
	 R
	R

	Building floor rehabilitation: fix all the cracks and apply non-slip epoxy - two coats
	7.1m(L)x6.1m(W)
	 
	 R
	R

	Repainting of fascia boards - check fastening of boards
	7.1mx6.1m
	1
	 R
	R

	Supply and installation of gutters and paint
	7.1mx6.1m
	1
	 R
	R

	Supply and installation of downpipes and paint
	3m
	2
	 R
	R

	Check roof trusses and repair where needed
	 
	                             1
	 R
	R

	Plastering outside where needed and at roofline
	 
	                             1
	 R
	R

	Install basin (provided) and taps
	 
	                             1
	 R
	R

	Drain - 
	 
	                             1
	 R
	R

	OHS file
	 
	1
	 R
	R

	Sub Total cost
 
	R

	Contingency cost (10% of sub total cost)
	R

	
Total amount (Excluding of VAT)
	R

	 
 Vat amount (15%)
 
	R

	Total cost (Including of VAT)
	R





Condition 
1.   Any default against the project plan will attract R500.00 per day.
2.    Full payment will be action upon project completion there will be no partial payment
3.    Contractor to clean up all the rubbles from the site

