{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":14},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":647,"n_cols":8,"rows_kept":647,"merged":[[11,1,11,2],[15,1,70,1],[15,3,70,3],[15,4,70,4],[15,5,70,5],[15,6,70,6],[15,7,70,7],[71,1,87,1],[71,3,87,3],[71,4,87,4],[71,5,87,5],[71,6,87,6],[71,7,87,7],[88,1,103,1],[88,3,103,3],[88,4,103,4],[88,5,103,5],[88,6,103,6],[88,7,103,7],[104,1,125,1],[104,3,125,3],[104,4,125,4],[104,5,125,5],[104,6,125,6],[104,7,125,7],[126,1,143,1],[126,3,143,3],[126,4,143,4],[126,5,143,5],[126,6,143,6],[126,7,143,7],[144,1,161,1],[144,3,161,3],[144,4,161,4],[144,5,161,5],[144,6,161,6],[144,7,161,7],[162,1,189,1],[162,3,189,3],[162,4,189,4],[162,5,189,5],[162,6,189,6],[162,7,189,7],[190,1,250,1],[190,3,250,3],[190,4,250,4],[190,5,250,5],[190,6,250,6],[190,7,250,7],[251,1,289,1],[251,3,289,3],[251,4,289,4],[251,5,289,5],[251,6,289,6],[251,7,289,7],[290,1,313,1],[290,3,313,3],[290,4,313,4],[290,5,313,5],[290,6,313,6],[290,7,313,7],[314,1,416,1],[314,3,416,3],[314,4,416,4],[314,5,416,5],[314,6,416,6],[314,7,416,7],[417,1,516,1],[417,3,516,3],[417,4,516,4],[417,5,516,5],[417,6,516,6],[417,7,516,7],[517,1,624,1],[517,3,624,3],[517,4,624,4],[517,5,624,5],[517,6,624,6],[517,7,624,7],[623,2,624,2],[628,2,628,6],[641,1,641,2],[647,2,647,3],[648,2,648,3],[649,2,649,6],[650,2,650,4],[651,2,651,6]]}
[]
[{"$nulls":3},"ANNEXURE B - PRICING SCHEDULE "]
[]
[{"$nulls":3},"Procurement of Multimedia Operational Equipment"]
[]
[]
[null,"NAME OF BIDDER:                     ",null,null,"BID NO.: RFQ/SASSETA/262107104"]
[]
[]
[]
[]
[null,"CLOSING TIME: 11:00    ",null,null,"CLOSING DATE: 25 June 2026"]
[]
[]
[null,"No.","Details","Quantity","PICTURE ","PRICE (incl. of VAT where applicable)","BUY BACK AFTER 4  YEARS (incl. of VAT where applicable)","REPAIR AND MAINTENANCE (HOURLY RATE) (incl. of VAT where applicable)"]
[null,"1.      ","Canon Camera EOS R7:",3]
[]
[null,null,"Ø  Sensor: APS-C CMOS (approx. 22.3 x 14.9 mm)"]
[]
[null,null,"Ø  Effective Resolution: 24.2 megapixels (6000 x 4000) detail for both photos and video. "]
[]
[null,null,"Processor & Performance"]
[]
[null,null,"Ø  Processor: DIGIC X (fast performance and reliable autofocus). "]
[]
[null,null,"Ø  Continuous Shooting: Up to ~15 fps with electronic shutter useful for events and action photography. "]
[]
[null,null,"Autofocus"]
[]
[null,null,"Ø  AF: Dual Pixel CMOS AF II with extensive coverage and subject tracking good for moving subjects and video focus. "]
[]
[null,null,"Video Capabilities"]
[]
[null,null,"Ø  4K UHD Video: Up to 30 fps (oversampled from 6K for improved quality). "]
[]
[null,null,"Ø  Full HD: Up to 120 fps for slow motion. "]
[]
[null,null,"Stabilisation"]
[]
[null,null,"Ø  Image Stabilisation: Digital and lens-based (no in-body stabilization). "]
[]
[null,null,"Display & Viewfinder"]
[]
[null,null,"Ø  Screen: 3.0″ fully articulating touchscreen LCD ideal for vlogging and flexible shooting angles. "]
[]
[null,null,"Connectivity & Ports"]
[]
[null,null,"Ø  Ports: Micro HDMI, USB-C, 3.5 mm mic input. "]
[]
[null,null,"Ø  Wireless: Wi-Fi 4 and Bluetooth 4.2 for easy transfer and remote control. "]
[]
[null,null,"Memory & Power"]
[]
[null,null,"Ø  Card Slot: Single SD/SDHC/SDXC slot. "]
[]
[null,null,"Ø  Battery: LP-E17 rechargeable (included). "]
[]
[null,null,"Size & Weight"]
[]
[null,null,"Ø  Dimensions: Approx. 116.3 × 85.5 × 68.8 mm. "]
[]
[null,null,"Ø  Weight: Approx. 375 g with battery and card. "]
[]
[null,null,"The EOS R50 is a good fit Hybrid Shooter: "]
[null,null,"Good for both high-quality stills and 4K video content, which is needed for events and interviews. "]
[]
[null,null,"·       Articulating Screen: Great for on-camera interviews and vlogging formats. "]
[]
[null,null,"·       Autofocus: Fast and reliable, easier to use in dynamic environments like events. "]
[]
[null,null,"Ø  Wireless Connectivity: Makes it easier to transfer content to devices for editing and posting quickly"]
[null,"2.      ","Wide-angle lenses:",3]
[null,null,"For Canon R50 (APS-C)"]
[]
[null,null,"Ø  Canon RF-S 10-18mm f/4.5-6.3 IS STM"]
[]
[null,null,"Ø  Focal Length: 10–18mm (wide-angle) perfect for group photos"]
[]
[null,null,"Ø  Format: APS-C"]
[]
[null,null,"Ø  Stabilisation: Optical Image Stabilizer"]
[]
[null,null,"Ø  Autofocus: STM (quiet & smooth good for video)"]
[]
[null,null,"Ø  Best For: Events, halls, boardrooms, crowded coverage"]
[]
[null,null,"Ø  Why this Lense is important:"]
[null,null,"Wide enough to not cut people when taking pictures."]
[null,"3.      ","Portrait Lenses:",3]
[null,null,"Key Specifications"]
[]
[null,null,"Ø  Focal Length: 50 mm"]
[]
[null,null,"Ø  Maximum Aperture: f/1.8 (excellent low-light performance & background blur)"]
[]
[null,null,"Ø  Lens Mount: RF (Canon mirrorless)"]
[]
[null,null,"Ø  Autofocus: STM (Stepping Motor quiet & smooth for video)"]
[]
[null,null,"Ø  Minimum Focus Distance: ~0.35 m"]
[]
[null,null,"Ø  Filter Size: 43 mm"]
[]
[null,null,"Ø  Weight: ~160 g"]
[null,4,"Standard Zoom Lenses: ",3]
[]
[]
[null,null,"Ø  Focal Length: 24–70 mm versatile range from wide-angle to short telephoto, ideal for general shooting."]
[]
[null,null,"Ø  Maximum Aperture: Constant f/2.8 throughout zoom range for better low-light performance and shallow depth of field control."]
[]
[null,null,"Ø  Minimum Aperture: f/22 allows for greater depth of field when stopped down."]
[]
[null,null,"Ø  Lens Mount: Canon EF (full-frame and APS-C compatible with crop factor)."]
[]
[null,null,"Ø  Autofocus: Ring-type Ultrasonic Motor (USM) with fast, quiet AF and full-time manual focus override."]
[]
[null,null,"Ø  Minimum Focus Distance: ~0.38 m (1.25 ft) — good for close-up work within this range."]
[]
[null,null,"Ø  Magnification: Around 0.21–0.29×, depending on model version."]
[]
[null,null,"Ø  Diaphragm Blades: Typically, 8–9 rounded blades for smooth bokeh."]
[]
[null,null,"Ø  Filter Size: 77 mm or 82 mm (varies by version)."]
[]
[null,null,"Build Quality: Canon L-series professional build with weather-resistant sealing and high-quality optical glass elements to reduce aberrations and ghosting."]
[null,5,"LED Lights:",3]
[]
[null,null,"Ø  LED Panel Light – Adjustable Bi-Color (e.g., 2-Pack Kit)"]
[null,null," Key Specifications"]
[]
[null,null,"Ø  Type: LED Panel"]
[]
[null,null,"Ø  Color Temperature: 3200 K – 5600 K (adjustable warm to cool)"]
[]
[null,null,"Ø  Brightness: 2000 – 8000 lux "]
[]
[null,null,"Ø  CRI / TLCI:  95 (high color accuracy for skin tones)"]
[]
[null,null,"Ø  Power: AC adapter + optional battery-powered"]
[]
[null,null,"Ø  Size: Approximately 10” × 8” panels"]
[]
[null,null,"Mount: Included light stands + barn doors"]
[null,6,"Phone Tripod:",1]
[]
[null,null,"Key specifications:"]
[]
[null,null,"Ø Maximum Height: Approx 150 cm / 59 inches"]
[null,null,"Tall enough for standing shots and interview setups without bending or awkward angles."]
[]
[null,null,"Ø  Minimum Height: Approx 20 – 30 cm / tabletop mode Useful for seated interviews, desk shots, and creative angles."]
[]
[null,null,"Stability & Build"]
[]
[null,null,"Ø  Aluminium alloy or reinforced ABS"]
[null,null,"Sturdy, doesn’t wobble with a heavy phone + mic mount."]
[]
[null,null,"Phone Mount Compatibility"]
[]
[null,null,"Ø  Fits iPhone 16 Pro Max size (with or without a case)"]
[null,null,"Extendable grip with rubber pads to prevent slips."]
[null,7,"High Speed SD Card:",4]
[]
[]
[null,null,"SDXC 256 GB V90 UHS-II U3"]
[]
[null,null,"Ø  Best for sustained 4K video"]
[]
[null,null,"Ø  Excellent for extended events without swapping cards"]
[]
[null,null,"Ø  Faster transfer speeds"]
[]
[null,null,"Why this recommendation "]
[]
[null,null,"When recording 4K video on cameras like the Canon EOS R50 or R7, the camera generates large amounts of data per second."]
[]
[null,null," Only high-speed cards can write fast enough to your card without interruptions, crucial for:"]
[]
[null,null,"Ø  Interviews"]
[]
[null,null,"Ø  YouTube production"]
[]
[null,null,"Ø  Long event coverage"]
[]
[null,null,"Ø  Fast shooting in burst"]
[]
[null,null,"Ø  Backup redundancy"]
[]
[]
[null,8,"Sony HXR-NX800 4K NXCAM Camcorder",1]
[]
[null,null,"Key specifications"]
[]
[null,null,"Sensor & Imaging"]
[]
[null,null,"Ø  Sensor: 1.0-inch Exmor RS CMOS (13.2 × 8.8 mm) larger sensor for good low light and depth-of-field control. "]
[]
[null,null,"Ø  Effective Resolution: ~14 MP (20.9 MP total) "]
[]
[null,null,"Ø  Lens: Built-in lens with 20× optical zoom (24–480 mm 35 mm eq.) "]
[]
[null,null,"Ø  Aperture Range: f/2.8 (wide) to f/4.5 (telephoto) "]
[]
[null,null,"Ø  Minimum Focus Distance: ~1 cm (wide) "]
[]
[null,null,"Ø  Image Stabilisation: Optical stabilisation in the lens. "]
[]
[null,null,"Video Recording"]
[]
[null,null,"Ø  UHD 4K (3840 × 2160): Up to 120 fps excellent for slow-motion and smooth motion capture. "]
[]
[null,null,"Ø  Full HD (1920 × 1080): Up to 240 fps for high-speed video. "]
[]
[null,null,"Ø  Recording Formats: XAVC HS, XAVC S-I, XAVC S-L, H.264, H.265 gives flexible quality and file size options. "]
[]
[null,null,"Ø  Built-in ND Filter: 2 to 7-stop electronic ND filter to control exposure in bright conditions. "]
[]
[null,null,"Ø  Colour Profiles: Support for S-Cinetone, Rec.709, HLG HDR good for cinematic/grading work. "]
[]
[null,null,"Audio & Inputs"]
[]
[null,null,"Ø  4-Channel Audio: (via detachable handle) with XLR inputs essential for professional microphones. "]
[]
[null,null,"Ø  External Audio: Compatible with industry-standard pro-audio gear. "]
[]
[null,null,"Autofocus & Intelligent Features"]
[]
[null,null,"Ø  Fast Hybrid Autofocus: Phase-detect AF with up to ~475 points and subject tracking. "]
[]
[null,null,"Ø  AI-Powered Features: AI assist and auto-framing features help keep subjects in focus useful for solo shooters. "]
[]
[null,null,"Ø  Streaming & Connectivity: Built-in dual-band Wi-Fi and optional streaming (RTMP/RTMPS/SRT), remote control via app. "]
[]
[null,null,"Storage & Outputs"]
[]
[null,null,"Ø  Media: Dual card slots: CFexpress Type-A and SD (UHS-II), great for recording backups or relay recording. "]
[]
[null,null,"Ø  Video Output: HDMI for monitoring and external recording. "]
[]
[null,null,"Ø  Mobile App Compatibility: Android & iOS remote control and monitoring. "]
[]
[null,null," General Specs"]
[]
[null,null,"Ø  Weight: ~1.9 kg (body only), ~2.38 kg with battery/accessories. "]
[]
[null,null,"Ø  Battery: Sony BP-U series professional batteries (BP-U35/U70/U100). "]
[]
[null,null,"Ø  Dimensions: ~175.6 × 201.3 × 371.1 mm. "]
[]
[]
[null,9,"Canon RF 70-200mm lense ",2]
[]
[null,null,"Key Specification"]
[]
[null,null,"Optical & Performance"]
[]
[null,null,"Ø  Focal Length: 70–200 mm (telephoto zoom)"]
[]
[null,null,"Ø  Maximum Aperture: Constant f/2.8 across the zoom range (great for low light & subject isolation) "]
[]
[null,null,"Ø  Minimum Aperture: f/32 "]
[]
[null,null,"Ø  Lens Construction: 17 elements in 13 groups with Super UD and aspherical elements for sharpness & aberration control "]
[]
[null,null,"Ø  Diaphragm: 9-blade circular aperture for smooth bokeh "]
[]
[null,null,"Ø  Filter Thread: 77 mm "]
[]
[null,null,"Ø  Image Stabilization: Up to ~5 stops (CIPA standard) "]
[]
[null,null,"Focus & Handling"]
[]
[null,null,"Ø  Autofocus: Dual Nano USM — fast, quiet, precise for photos & video "]
[]
[null,null,"Ø  Minimum Focus Distance: ~0.7 m (~2.3 ft) "]
[]
[null,null,"Ø  Max Magnification: ~0.23× "]
[]
[null,null,"Size & Build"]
[]
[null,null,"·       Weather Sealing: Dust & moisture-resistant L-series build "]
[]
[null,null,"·       Dimensions: ~Ø 89.9 × 146 mm "]
[]
[null,null,"·       Weight: ~1,070 g without tripod collar "]
[]
[null,null,"Excellent for sports, wildlife, events, portraits, and low-light shooting."]
[]
[]
[null,10,"Headphones",2]
[]
[null,null,"Driver Size & Type"]
[]
[null,null,"Ø  Driver Size (mm): Larger drivers (e.g., 40–50 mm) usually deliver fuller sound and better bass response."]
[]
[null,null,"Ø  Driver Type:"]
[]
[null,null,"Ø  Dynamic drivers – common, good overall sound."]
[]
[null,null,"Ø  Planar magnetic / Balanced Armature "]
[]
[null,null,"Frequency Response"]
[]
[null,null,"Ø  Range: Typical good monitoring range is 20 Hz – 20 kHz."]
[]
[null,null,"Ø  A flat/neutral response is best for monitoring because it reproduces audio without exaggerated bass or treble"]
[]
[null,null,"Impedance"]
[]
[null,null,"Ø  Low Impedance (~16–32 Ω): Easy to drive with portable camcorders or mixer outputs."]
[]
[null,null,"High Impedance (>80 Ω): Better detail, but often needs an amp to reach comfortable volume."]
[]
[null,11,"Soft boxes/ diffusers",2]
[]
[null,null,"Size & Shape"]
[]
[null,null,"Ø  Common Sizes:"]
[]
[null,null,"o   Medium: 80 × 80 cm, 90 × 120 cm – Versatile for portraits & products"]
[]
[null,null,"o   Large: 120 × 180 cm, 120 × 240 cm – Soft, broad fill light"]
[]
[null,null,"Shapes:"]
[]
[null,null,"Ø  Square/Rectangular: Classic, good for broad even light"]
[]
[null,null,"Ø  Octagonal (Octabox): More natural circular catchlights"]
[]
[null,null,"Ø  Strip: Narrow light, great for rim/edge lighting"]
[]
[]
[null,null,"Diffusion Material"]
[]
[null,null,"Ø  Outer Diffuser (Soft Panel):"]
[]
[null,null,"o   Thick, multi-layered material spreads light evenly"]
[]
[null,null,"o   Should be heat-resistant (for continuous lights)"]
[]
[null,null,"Ø  Inner Diffuser (Baffle):"]
[]
[null,null,"o   Reduces hotspots and ensures even spread across the panel"]
[]
[]
[null,null,"Mount / Bowens Compatibility"]
[]
[null,null,"Ø  Mount Type: Defines what lights you can attach:"]
[]
[null,null,"o   Bowens S-Mount: Most popular universal mount"]
[]
[null,null,"o   Profoto, Elinchrom, Godox, etc: Brand-specific"]
[]
[null,null,"Ø  Adapter Rings: Allow fitting softboxes to different light brands"]
[]
[]
[null,null,"Light Output & Transmission"]
[]
[null,null,"Ø  Transmission %: Amount of light passing through the diffuser (typically 60%–90%)"]
[]
[null,null,"o   Higher transmission = brighter output"]
[]
[null,null,"o   Lower transmission = softer, more diffused light"]
[]
[null,null,"Ø  Loss vs Gain: Larger softboxes often reduce output, so you may need more power"]
[]
[]
[null,null,"Build Quality & Portability"]
[]
[null,null,"Ø  Frame:"]
[]
[null,null,"o   Steel rods (classic): Strong, durable"]
[]
[null,null,"o   Fiberglass rods: Lighter, more flexible"]
[]
[null,null,"Ø  Carrying Case: Handy for location shoots"]
[]
[null,null,"Ø  Speed/Rapid-Fold Design: Quicker to set up and break down"]
[]
[null,null,"Grids & Accessories"]
[]
[null,null,"Ø  Grids (Egg-Crates):"]
[]
[null,null,"o   Narrow light spread, better control"]
[]
[null,null,"o   Available in different densities (e.g., 10°, 20°, etc.)"]
[]
[null,null,"Ø  Inner Baffles:"]
[]
[null,null,"o   Helps soften light further"]
[]
[null,null,"Ø  Snoots/Reflectors:"]
[]
[null,null,"o   For shaping and controlling light"]
[]
[null,null,"Depth & Aspect Ratio"]
[]
[null,null,"Ø  Deeper Softboxes: More directionality and smoother fall-off of light"]
[]
[null,null,"Ø  Shallow Softboxes: Wider spread, less directional control"]
[]
[]
[null,null,"Weight & Handling"]
[]
[null,null,"Ø  Weight: Affects portability, especially for on-location work"]
[]
[null,null,"Ø  Mount Stability: Must securely hold the light"]
[]
[]
[null,null,"Heat Resistance (for Continuous Lights)"]
[]
[null,null,"Ø  Rated for High Temps: Essential if using hot bulbs (tungsten) or high-output LEDs"]
[]
[null,null,"Ø  Material Safety: Should withstand prolonged use without warping"]
[]
[]
[null,12,"Portable LED lights",3]
[]
[null,null," Light Output / Brightness"]
[]
[null,null,"Ø  Lumen / Lux / Power (W):"]
[]
[null,null,"o   Lumen -total light output "]
[]
[null,null,"o   Lux @ 1 m -brightness measured at a distance of 1 meter (common spec for video lights)."]
[]
[null,null,"o   Watt-equivalent / Power draw — how much electrical power the light uses."]
[]
[null,null," Colour Temperature"]
[]
[null,null,"Ø  CCT (Correlated Colour Temperature): Measured in Kelvin (K) tells how warm or cool the light is."]
[]
[null,null,"o   Warm (Tungsten): ~2800–3200 K"]
[]
[null,null,"o   Daylight: ~5500–6500 K"]
[]
[null,null,"o   Variable / Bi-colour: Adjustable range (e.g., 2800–6500 K)"]
[]
[null,null," Colour Accuracy"]
[]
[null,null,"Ø  CRI (Colour Rendering Index):"]
[]
[null,null,"o   Scale up to 100"]
[]
[null,null,"o   CRI ≥ 90+ = accurate colours on skin tones and objects"]
[]
[null,null,"Ø  TLCI (Television Lighting Consistency Index):"]
[]
[null,null,"o   Used in broadcast/video; TLCI ≥ 90+ means reliable colour for video work"]
[]
[null,null,"Power & Battery"]
[]
[null,null,"Ø  Battery Type:"]
[]
[null,null,"o   Built-in rechargeable (USB-C or proprietary)"]
[]
[null,null,"o   Removable batteries (Sony NP-F, V-mount, etc.)"]
[]
[null,null,"Ø  Runtime:"]
[]
[null,null,"o   Rated at full power (e.g., 60 min at 100%)"]
[]
[null,null,"Ø  DC Input / USB-C: Allows power via wall adapter or power bank"]
[]
[null,null,"Dimming & Control"]
[]
[null,null,"Ø  Control Range:"]
[]
[null,null,"o   e.g., 0–100% dimming"]
[]
[null,null,"Ø  Dimming Steps:"]
[]
[null,null,"o   Smooth / stepless vs fixed steps"]
[]
[null,null,"Ø  Control Method:"]
[]
[null,null,"o   On-board dial, app/Bluetooth, remote"]
[]
[null,null,"Size & Mounting"]
[]
[null,null,"Ø  Physical Size: Panel area (e.g., large panel vs small pocket light)"]
[]
[null,null,"Ø  Mounting Options:"]
[]
[null,null,"o   Cold shoe, ¼″ thread, magnetic mounts"]
[]
[null,null,"Beam & Light Spread"]
[]
[null,null,"Ø  Beam Angle:"]
[]
[null,null,"o   Wide (soft spread) ~100°+"]
[]
[null,null,"o   Narrower for more directional throw."]
[]
[null,null,"Build & Accessories"]
[]
[null,null,"Ø  Weather Resistance / Durability: Useful outdoors"]
[]
[null,null,"Ø  Diffusers / Filters:"]
[]
[null,null,"o   Soft diffuser included or built-in"]
[]
[null,null,"o   Filters: gels or magnetic modifiers"]
[]
[null,null,"Ø  Grids / Barndoors: Control spill light"]
[]
[null,null," Additional Features"]
[]
[null,null,"Ø  RGB Capability: Full colour control (hue, saturation, effects)"]
[]
[null,null,"Ø  Effects Modes: Flicker, strobe, paparazzi, etc."]
[]
[null,null,"Ø  Cooling System: Passive (quiet) vs active (fan)"]
[]
[null,null,"Display: LED screen showing values (CCT, % dim, battery)"]
[]
[null,13,"XLR cables",2]
[]
[null,null,"Connector Type"]
[]
[null,null,"Ø  XLR 3-Pin (Standard)"]
[]
[null,null,"o   Male (XLR-M) → usually connects to camera input"]
[]
[null,null,"o   Female (XLR-F) → usually connects to microphone"]
[]
[null,null,"Ø  Most professional camcorders use 3-pin XLR balanced inputs"]
[]
[]
[null,null," Cable Type (Balanced Audio)"]
[]
[null,null,"Ø  Balanced cable (Required for professional audio)"]
[]
[null,null,"o   3 conductors:"]
[]
[null,null,"§  Pin 1: Ground"]
[]
[null,null,"§  Pin 2: Hot (+)"]
[]
[null,null,"§  Pin 3: Cold (−)"]
[]
[null,null,"Ø  Balanced cables reduce:"]
[]
[null,null,"·       Electrical interference"]
[]
[null,null,"·       Hum and noise"]
[]
[null,null,"·       Signal loss over long distances"]
[]
[]
[null,null," Cable Length"]
[]
[null,null,"Ø  Common lengths:"]
[]
[null,null,"·       1–3 meters → On-camera shotgun mic"]
[]
[null,null,"·       5–10 meters → Interviews, small setups"]
[]
[null,null,"·       15–30 meters → Events, stage, conferences"]
[]
[]
[null,null,"Conductor & Gauge"]
[]
[null,null,"Ø  Wire Gauge (AWG):"]
[]
[null,null,"o   22 AWG – 24 AWG is common for mic cables"]
[]
[null,null,"Ø  Oxygen-Free Copper (OFC) preferred for better conductivity"]
[]
[null,null,"Ø  Multi-strand conductors improve flexibility"]
[]
[]
[null,null,"Shielding"]
[]
[null,null,"Good shielding protects from RF interference and hum."]
[]
[null,null,"Ø  Common shielding types:"]
[]
[null,null,"·       Braided Shield (best durability)"]
[]
[null,null,"·       Spiral Shield (flexible)"]
[]
[null,null,"·       Foil Shield (good RF protection)"]
[]
[null,null,"Phantom Power Compatibility"]
[]
[null,null,"Ø  Must support 48V Phantom Power"]
[]
[null,null,"Ø  Required for:"]
[]
[null,null,"o   Condenser microphones"]
[]
[null,null,"o   Shotgun microphones"]
[]
[null,null,"o   Some lav systems"]
[]
[]
[null,null,"Connector Build Quality"]
[]
[null,null,"Ø  Metal connectors (Zinc or Nickel plated)"]
[]
[null,null,"Ø  Gold-plated pins (better corrosion resistance)"]
[]
[null,null,"Ø  Strong strain relief"]
[]
[null,null,"Ø  Locking latch mechanism"]
[]
[null,null,"Reliable brands often use:"]
[]
[null,null,"Ø  Neutrik connectors"]
[]
[null,null,"Ø  Switchcraft connectors"]
[]
[]
[null,null,"Flexibility & Jacket Material"]
[]
[null,null,"Ø  PVC jacket (standard)"]
[]
[null,null,"Ø  Rubberized jacket (more flexible)"]
[]
[null,null,"Ø  Soft-touch jacket for easier coiling"]
[]
[null,null,"Temperature resistant for outdoor use"]
[]
[null,"TOTAL ",{"$nulls":3},{"$f":"SUM(F16:F625)","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(G16:G625)","v":{"v":0,"d":"R0.00"}},{"v":0,"d":"R0.00"}]
[]
[]
[]
[null,"i. Bidders are to submit Annexure B. Non-submission of Annexure B will lead to automatic disqualification. "]
[null,"ii. Bidders are to ensure that all items indicated on (Annexure B) are quoted for. Incomplete Annexure B will lead to automatic disqualification."]
[null,"iii. The template will sum up the total."]
[null,"iv. Bidders are requested to input their costs only and sign off."]
[null,"v. Bidders are requested to submit Annexure B without changing any of the details on this document. Altered Annexure B will lead to automatic disqualification."]
[null,"vi. Bidders are required to submit this excel spreadsheet in Excel format for evaluation purposes and also a signed PDF version for audit trail purposes."]
[null,"Note 1:  Total cost including delivery cost as specified in Annexure B will be considered for evaluation purposes. "]
[null,"Note 2:  Unit price refers to unit descriptions as per Annexure B."]
[null,"Note 3: Prices will escalate with CPIX on the anniversary of the contract. "]
[]
[]
[]
[null,"Signature                                                              ",null,null,"Date"]
[]
[]
[]
[null,"                             "]
[null,"Position                                                                 ",null,null,"Name of bidder     "]