{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["MAIN SHEET"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"MAIN SHEET","index":0,"n_rows":96,"n_cols":10,"rows_kept":96,"merged":[[1,1,1,8],[4,1,4,5],[4,6,4,8],[10,1,10,5],[10,6,10,8],[15,1,15,5],[15,6,15,8],[26,1,26,5],[26,6,26,8],[32,1,32,5],[32,6,32,8],[40,1,40,5],[40,6,40,8],[50,1,50,5],[50,6,50,8],[55,1,55,5],[55,6,55,8],[62,1,62,5],[62,6,62,8],[66,1,66,5],[66,6,66,8],[70,1,70,5],[70,6,70,8],[76,1,76,5],[76,6,76,8],[82,1,82,5],[82,6,82,8],[85,1,85,5],[85,6,85,8],[89,1,89,5],[89,6,89,8],[94,1,94,5],[95,1,95,5]]}
[]
[null,"ANNEXURE A - COMPLIANCE TO STATEMENT OF WORK MATRIX"]
[]
[null,"Ref","Requirement","Compliance criteria","Compliance YES /NO","Reference to Artefacts","Mandatory","Necessary","Desirable"]
[null,"General Requirements ",{"$nulls":4},"Points"]
[null,"GEN-001","The system shall be suitable for military field use.","Mandatory (M)",null,null,1]
[null,"GEN-002","The system shall be operated by one person.","Mandatory (M)",null,null,1]
[null,"GEN-003","The system shall clean a complete 155 mm artillery barrel,  Progressive Rifling (Gain Twist Rifling) and Uniform Rifling (Constant Twist Rifling)","Mandatory (M)",null,null,1]
[null,"GEN-004","The system shall minimise operator exposure to cleaning chemicals.","Necessary",{"$nulls":3},1]
[null,"GEN-005","The system shall require minimal routine maintenance.","Desirable (D)",{"$nulls":4},1]
[null,"Mechanical Requirements",{"$nulls":4},"Points"]
[null,"MEC-001","Combination Steel and Nylon bristles shall be incorporated.","Mandatory (M)",null,null,1]
[null,"MEC-002","Combined brush( Bristles alone) length shall be at least 200 mm.","Mandatory (M)",null,null,1]
[null,"MEC-003","Brushes shall maintain continuous circumferential contact.","Mandatory (M)",null,null,1]
[null,"MEC-004","The brush assembly shall automatically retract from the barrel.(dual direction)","Mandatory (M)",null,null,1]
[null,"Cleaning Fluid System",{"$nulls":4},"Points"]
[null,"FLD-001","Cleaning fluid shall be dispensed automatically.","Mandatory (M)",null,null,1]
[null,"FLD-002","Cleaning fluid shall be delivered directly to the brushes.","Necessary",{"$nulls":3},1]
[null,"FLD-003","The reservoir shall be refillable during operation.","Mandatory (M)",null,null,1]
[null,"FLD-004","The cleaning cycle shall continue uninterrupted while replenishing fluid.","Necessary",{"$nulls":3},1]
[null,"FLD-005","Unlimited cleaning fluid supply shall be possible through replenishment.","Mandatory (M)",null,null,1]
[null,"FLD-006","Used cleaning fluid shall be recovered.","Necessary",{"$nulls":3},1]
[null,"FLD-007","The recovery system shall prevent contamination of the weapon platform.","Desirable (D)",{"$nulls":4},1]
[null,"FLD-008","The recovery system shall prevent contamination of the surrounding area.","Desirable (D)",{"$nulls":4},1]
[null,"FLD-009","The system should be compatible with recognised  types of barrel cleaning fluid ","Necessary",{"$nulls":3},1]
[null,"FLD-010","Used fluid shall be collected in an external container, from the system via a pipe into the external container","Necessary",{"$nulls":3},1]
[null,"Automation",{"$nulls":4},"Points"]
[null,"AUT-001","Cleaning fluid application shall be automatic.","Mandatory (M)",null,null,1]
[null,"AUT-002","Cleaning shall be automatic.","Mandatory (M)",null,null,1]
[null,"AUT-003","Fluid recovery shall be automatic.","Necessary",{"$nulls":3},1]
[null,"AUT-004","Brush extraction shall be automatic. (dual direction)","Mandatory (M)",null,null,1]
[null,"AUT-005","No operator intervention shall be required once the cycle has commenced.","Necessary",{"$nulls":3},1]
[null,"Human Machine Interface",{"$nulls":4},"Points"]
[null,"HMI-001","The system shall incorporate an onboard LCD display.","Mandatory (M)",null,null,1]
[null,"HMI-002","The display shall be colour.","Necessary",{"$nulls":3},1]
[null,"HMI-003","The display shall be touchscreen operated.","Mandatory (M)",null,null,1]
[null,"HMI-004","Cleaning modes shall be selectable.","Necessary",{"$nulls":3},1]
[null,"HMI-005","Cleaning progress shall be displayed.","Necessary",{"$nulls":3},1]
[null,"HMI-006","System Faults shall be displayed.","Mandatory (M)",null,null,1]
[null,"HMI-007","System status shall be displayed.","Necessary",{"$nulls":3},1]
[null,"Inspection System",{"$nulls":4},"Points"]
[null,"CAM-001","The system shall include an integrated inspection camera.","Mandatory (M)",null,null,1]
[null,"CAM-002","High resolution camera shall be onboard the system.","Mandatory (M)",null,null,1]
[null,"CAM-003","Live video shall be available.","Mandatory (M)",null,null,1]
[null,"CAM-004","Images shall be recorded.","Mandatory (M)",null,null,1]
[null,"CAM-005","Video shall be recorded.","Mandatory (M)",null,null,1]
[null,"CAM-006","Images shall be stored automatically.","Mandatory (M)",null,null,1]
[null,"CAM-007","Video shall be stored automatically.","Mandatory (M)",null,null,1]
[null,"CAM-008","Inspection during cleaning shall be possible on the system","Mandatory (M)",null,null,1]
[null,"CAM-09","Inspection after cleaning shall be possible on the system display","Mandatory (M)",null,null,1]
[null,"Cleaning Modes",{"$nulls":4},"Points"]
[null,"MOD-001","Normal Cleaning Mode shall be provided.","Necessary",{"$nulls":3},1]
[null,"MOD-002","Intensive Cleaning Mode shall be provided.","Necessary",{"$nulls":3},1]
[null,"MOD-003","Preservation Mode shall be provided.","Necessary",{"$nulls":3},1]
[null,"MOD-004","De-preservation Mode shall be provided.","Necessary",{"$nulls":3},1]
[null,"Electrical Requirements",{"$nulls":4},"Points"]
[null,"ELE-001","System shall operate from 24 VDC.","Mandatory (M)",null,null,1]
[null,"ELE-002","System shall operate from 220V AC via a power supply","Mandatory (M)",null,null,1]
[null,"ELE-004","Battery status indication shall be provided.","Necessary",{"$nulls":3},1]
[null,"ELE-005","Reverse polarity protection shall be provided.","Necessary",{"$nulls":3},1]
[null,"ELE-006","Electrical overload protection shall be provided.","Necessary",{"$nulls":3},1]
[null,"ELE-007","Motor overload protection shall be provided.","Necessary",{"$nulls":3},1]
[null,"Connectivity",{"$nulls":4},"Points"]
[null,"COM-001","Wi-Fi connectivity shall be provided. To transfer data(video`s, photos)","Mandatory (M)",null,null,1]
[null,"COM-002","Bluetooth connectivity shall be provided.","Desirable (D)",{"$nulls":4},1]
[null,"COM-003","USB interface shall be provided.","Desirable (D)",{"$nulls":4},1]
[null,"Physical Requirements",{"$nulls":4},"Points"]
[null,"PHY-001","System length shall not exceed 800 mm in stored position.","Mandatory (M)",null,null,1]
[null,"PHY-002","One operator shall be able to transport the system.","Mandatory (M)",null,null,1]
[null,"PHY-003","The system shall be suitable for transport in military vehicles.","Mandatory (M)",null,null,1]
[null,"Transport Container",{"$nulls":4},"Points"]
[null,"CAS-001","All components shall fit into one transport container.","Mandatory (M)",null,null,1]
[null,"CAS-002","Maximum case length shall not excced 1100 mm.","Mandatory (M)",null,null,1]
[null,"CAS-003","Maximum case width shall not exceed 350 mm.","Mandatory (M)",null,null,1]
[null,"CAS-004","Maximum case height shall not exceed 250 mm.","Mandatory (M)",null,null,1]
[null,"CAS-005","The container shall protect equipment during transport.","Mandatory (M)",null,null,1]
[null,"Performance Requirements",{"$nulls":4},"Points"]
[null,"PER-001","Normal cleaning cycle shall not exceed 20 minutes.","Necessary",{"$nulls":3},1]
[null,"PER-002","System setup shall not exceed ten minutes.","Necessary",{"$nulls":3},1]
[null,"PER-003","Repacking shall not exceed ten minutes.","Necessary",{"$nulls":3},1]
[null,"PER-004","No cleaning fluid shall contaminate the surrounding area.","Necessary",{"$nulls":3},1]
[null,"PER-005","The cleaning fluid reservoir shall be refillable during operation.","Mandatory (M)",null,null,1]
[null,"Reliability",{"$nulls":4},"Points"]
[null,"REL-001","No scheduled maintenance shall be required before 500 cleaning cycles (excluding routine cleaning and lubrication).","Necessary",{"$nulls":3},1]
[null,"REL-004","Wear components shall be replaceable.","Mandatory (M)",null,null,1]
[null,"Safety",{"$nulls":4},"Points"]
[null,"SAF-001","Brush jam protection shall be provided.","Mandatory (M)",null,null,1]
[null,"SAF-002","Motor overload protection shall be provided.","Necessary",{"$nulls":3},1]
[null,"SAF-003","Automatic fault shutdown shall be provided.","Necessary",{"$nulls":3},1]
[null,"Documentation and Support",{"$nulls":4},"Points"]
[null,"DOC-001","Operator Manual shall be supplied.","Necessary",{"$nulls":3},1]
[null,"DOC-002","Maintenance Manual shall be supplied.","Necessary",{"$nulls":3},1]
[null,"DOC-003","A minimum 24-month warranty shall be provided.","Necessary",{"$nulls":3},1]
[null,"DOC-004","Spare parts and technical support shall be available for a minimum of 10 years","Necessary",{"$nulls":3},1]
[null,"Total Points",{"$nulls":4},{"$f":"SUBTOTAL(9,G6:G87)","v":39},{"$f":"SUBTOTAL(9,H9:H94)","v":31},{"$f":"SUBTOTAL(9,I9:I94)","v":5},{"$f":"SUM(G95:I95)","v":75}]
[null,"The bidder must must achieve",{"$nulls":4},39,25,3,{"$f":"SUM(G96:I96)","v":67}]