
	DEPARTMENT/ INSITUTION
	BID NUMBER & PROJECT DESCRIPTION 
	CONTACT PERSON

	DEPT OF TRANSPORT
	ADDENDUM No.2

DOT-HO-2425- [SCMU10–2425–0008]-(A-F)
APPOINTMENT OF A PANEL OF SERVICE PROVIDERS TO PROVIDE PLANT HIRE SERVICES AND MAINTENANCE OF GRAVEL ROADS IN THE EASTERN CAPE PROVINCE FOR THIRTY-SIX [36] MONTHS.

REASONS FOR ADDENDUM

This addendum serves to extend the closing date, provide clarities on queries raised by several bidders and to provided corrected documents where applicable. 

CLOSING DATE IS EXTENDED TO MONDAY 19 AUGUST 2024 AT 11:00 AM IN RESPECTIVE DISTRICTS
	TECHNICAL / PROJECT ENQUIRIES

Mrs. Z. Zuzile
Cell no: 082 576 3984
Email address: zezethu.zuzile@ectransport.gov.za  

SCM SPECIFIC ENQUIRIES

Mr. Nqikashe
Cell no: 067 419 8001
Email address: philasande.Nqikashe@ectransport.gov.za  



	NO
	QUERY DESCRIPTION
	RESPONSE / AMENDMENT

	1
	TENDER SUBMISSION – 
Do bidders need to submit in each districts if bidding for multiple districts?
	
Bidders may submit at a stipulated addresses at a district closest to them.  Bidders need not submit multiple documents if bidding for multiple districts. Bidders must indicate on page T2.8 the district(s) for which they wish to be considered.

If bidding for multiple districts, bidders must ensure to provide different key personnel and minimum required plant items for each district.

	2
	TENDER BRIEFING - 
I would like to enquire about the briefing attendance and choice of tender district. 
Can we attend any of the briefings dates and still tender at any district?

Will an unsigned certificate of tender briefing certificate render my bid non-responsive.
	
Bidders are required to attend only one briefing and may attend any of the briefings and may tender for any of the districts.

NO – Bidder’s signature in the attendance register will suffice as proof of attendance of a briefing.

The briefings sessions are non-compulsory

	3
	KEY PERSONNEL - 
On page T1.6, it stipulates that the Contract Manager should only have a NQF Level 7 Civil Engineering qualification.

Then on page T1.9 is states that the Contract Manager should be registered as a Professional Engineer or Engineering Technologist.
	
The Contracts Manager, who will be the single point accountable and responsible person for the oversight management of the construction works on site, shall:

•	have a minimum NQF level 7 Civil Engineering qualification and be suitably and verifiably experienced with a minimum of 5 years’ experience in road maintenance and / or construction.

	4
	PREFERRED ADDRESS FOR LOCALITY POINTS – 
Document currently stipulates that:
Preferred Address and satellite offices not edited within on and after date of publishing this tender on latest CSD report of the Bidder company.
	

Amended to:
Preferred Address and satellite offices not edited in the last 12 months on latest CSD report of the Bidder company.

	5
	PROVISION OF PLANT – 
Can I use the same plant for tendering in multiple districts?
	
Minimum plant required for eligibility can only be used for one district. If a bidder wishes to bid for multiple districts, different plant items stipulated as minimum requirements must be used for tendering in different districts. 

Additionally, functionality points can only be awarded to eligible bidders for a single plant item once, therefore if a bidder uses same plant items, stipulated in the full complement list, in different districts they will only be awarded points in the district of their preferred office as indicated on CSD.




	6
	PROVISION OF PLANT – 
Consideration will be given for plant and equipment Owned or hired (with letter of intent from plant hire company within the district for which the Tenderer is bidding)
	
The restriction to only source plant within the district for which a bidder wishes to be considered is revoked. Bidders may source plant anywhere and provide a letter of intent signed by a commissioner of oath stipulating that the plant item will be leased to the bidder and availed for the duration of the contract. 

	7
	PANEL AWARD
How many districts will a tenderer be awarded.
	
A tenderer may be awarded into all panels for which they have scored a minimum 70 functionality points. 

	8
	SIMILAR PROJECTS VERIFICATION
For each similar project listed by the tenderer in TABLE A, the tenderer must attach:
a)		the COMPLETION CERTIFICATE of the project; and
b)	a completed and signed returnable schedule C(A) and returnable schedule C(B): SIMILAR PROJECT COMPLETED VERIFICATION FORM.
	
For each similar project listed by the tenderer in TABLE A, the tenderer must attach:
a)		the COMPLETION CERTIFICATE of the project clearly indicating the value of the project completed. If the completion certificate does not reflect the value, then an appointment letter which indicates the award value must be attached as well.


	9
	ALLOCATION METHOD

Allocation preference in the implementation of the project will be based on the functionality points.  The highest point scoring bidder per district will be the first preferred bidder for allocation and allocations will be awarded rotationally from the highest point scoring to the lowest point scoring bidder.

The department reserves the right not to award any bidder in more than one district.
	AMENDED TO:

Allocation will be made according to the Guidelines for Framework Agreements for Infrastructure and Non-Infrastructure goods works and services.



	10
	RATES
Are Provisional sums on the bid document are they monthly or package (task) based.
	
All rates are package based.

	11
	BILL OF QUANTITIIES is amended in Annexure A Below.
















ANNEXURE 1
BILL OF QUANTIES HEREBY REPLACED
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SUMMARY OF THE SCHEDULE OF QUANTITIES.

	SECTION
	DESCRIPTION

	1200
	GENERAL REQUIREMENTS AND PROVISIONS

	1300
	CONTRACTOR’S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS

	1500
	ACCOMMODATION OF TRAFFIC

	1700
	CLEARING & GRUBBING

	1900
	DAYWORKS (PROVISIONAL)

	2100
	DRAINS

	2200
	PREFABRICATED CULVERTS

	3200
	SELECTIONS, STOCKPILING & BREAKING-DOWN THE MATERIAL FROM BORROW PITS,

	
	CUTTING & EXISTING PAVEMENT LAYERS, AND PLACING & COMPACTING THE

	
	GRAVEL LAYERS

	3300
	MASS EARTHWORKS

	3400
	PAVEMENT LAYERS OF GRAVEL MATERIAL

	3500
	STABILIZATION

	5100
	PITCHING, STONEWORK AND PROTECTION AGAINST EROSION

	5200
	GABIONS

	5400
	GUARDRAILS

	5500
	FENCING

	5600
	ROADSIGNS

	8100
	TESTING WORKMANSHIP AND MATERIALS

	SUB TOTAL

	ADD CONTINGENCIES AT 10%

	SUB TOTAL

	VALUE ADDED TAX (15%)

	TENDER SUM CARRIED TO FORM OF TENDER

















SIGNATURE OF TENDERER: .....................................................................


ON BEHALF OF: .........................................................................................


DATE: ...........................................................................................................




image1.emf
TENDER NO.: SCMU10-24/25-0008 A-F

ITEM

NO.

UNIT RATE

SSPS 1200 GENERAL REQUIREMENTS AND PROVISIONS

B12.01 Community Liaison Officers

(a) Monthly 4 000,00 R            

(b) Monthly 1 000,00 R            

(c) Meeting 350,00 R               

(d) Handling costs and charges for Contractor on items B12.01 (a) to (c) % 10,00%

B12.02 (a)  Monthly 30 000,00 R          

(b) % 10,0%

B12.03 (a) Monthly 35 000,00 R          

(b) % 10%

B12.04 (a) Provision for Occupational Health and Safety Officer Monthly 20 000,00 R          

(b)   Handling costs and charges for Contractor on items B12.02 (a) % 10%

B12.07     (a)      Protection or Relocate of Existing Services Prov Sum 10 000,00 R          

B12.08     (a)      Working adjacent/parallel to existing services  Prov Sum 15 000,00 R          

               (electrical and telecommunication services)

B12.09 Provision for works to be sub-contracted to local SMME's including 

Preliminary and General items Prov Sum 150 000,00 R        

B12.10 Handling cost on item B12.10 (including managing of SMME contractors

for the duration of the contract - 10 months) % 10,00%

DESCRIPTION

Remuneration of PSC members to attend official meetings

Provision for Environmental Management Plan And Audits

TOTAL CARRIED TO SUMMARY

Handling costs and charges for Contractor on items B12.04 (a)

Community Liaison Officer cost

Provision of Engineer's Requirements

Handling costs and charges for Contractor on items B12.02 (a)

Monthly transport allowance for CLO for duration of Contract
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ITEM

NO.

UNIT RATE

SSPS 1300 CONTRACTOR’S ESTABLISHMENT

ON SITE AND GENERAL OBLIGATIONS

B13.01 The Contractor's general obligations: 

(a)   Fixed obligations

Monthly 300 000,00 R        

          Act and Construction regulations

             Assessment (HIRA) CR 7 (1) Monthly 10 000,00 R          

Sum 700,00 R               

(b)   Value Related obligations Lump Sum 50 000,00 R          

(c)   Time-related obligations Months 20 000,00 R          

          -  Facilities  for Contractor including offices,  storagesheds,  

TOTAL CARRIED TO SUMMARY

          -  Provision for Emergency Preparedness &

             Response Plan

DESCRIPTION

             power, communications, setting out of Works, security and 

              living, accommodation, ablution and 

             latrine facilities, tools and equipment, water supplies,  electric, 

             dealing with water, traffic and  access.

          -  Provision for Personal Protective Equipment &

             Protective Clothing

     (i)  Other fixed-charge obligations including

          -  Provision for the Development of a Documented

           - Method Statements and/or Safe Work

          -  Provision for the Preparation of a Project

          -  Provision for the Preparation of a Hazard

          -  Provision for fulfilling the OH&S Functions
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ITEM

NO.

UNIT RATE

SSPS 1500 ACCOMMODATION OF TRAFFIC

B15.01

B15.02 Temporary traffic control facilities

(a)  Flagmen (including equipment) man-day 220,00 R              

(b) Portable STOP and GO-RY signs No. 880,00 R              

(c) Amber flicker lights No. 880,00 R              

(d)  Road signs, R- and TR-series, (1200 mm) No. 880,00 R              

(e )  Road signs, TW-series, (1200 mm) No. 890,00 R              

(f)  Delineators (TW401.TW402) 

(i)  Single sided blade (200mm x 800mm) No. 275,00 R              

(ii)  Double sided blade (200mm x 800mm) No. 450,00 R              

(g) No. 750,00 R              

TOTAL CARRIED TO SUMMARY

km  R         11 500,00 

 Moveable barricade/road sign combination TW 411 (2400mm x 

400mm) 

Accommodation of traffic and maintaining temporary deviations

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 1700 CLEARING & GRUBBING

B17.01 Clearing and grubbing ha 15 800,00 R          

17.02

(a)   Girth exceeding 1m up to and including 2m No 800,00 R               

17.04 Clearing and grubbing at inlets and outlets of m² 15,00 R                 

hydraulic structures

B17.05 Clearing of hydraulic structures

m³ 100,00 R               

m³ 120,00 R               

m³ 170,00 R               

B17.07

and portal culverts hr 120,00 R               

B17.08 Removal of undesired vegetation m² 20,00 R                 

B17.09 Shredding of vegetation cuttings in situ m³ 35,00 R                 

17/120.02 m³-km 18,00 R                 

B17.10 Clearing and grubbing narrow strips m² 35,00 R                 

TOTAL CARRIED FORWARD

Mechanical cleaning of hydraulic structures, pipes 

(d)   Box culverts exceeding 1.5 m vertical

Overhaul on material hauled in excess of 1.0km (ordinary overhaul)

Removal and grubbing of large trees and tree stumps:

(a)   Pipes with an internal diameter up to and including 900mm

(c)   Box culverts up to and including 1.5 m vertical

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 1900 DAYWORKS (PROVISIONAL)

B19.01 Personnel during normal working hours

(a)   Unskilled hr 55,00 R                 

(b)   Semi-skilled hr 75,00 R                 

(c)   Skilled hr 120,00 R               

(d)   Ganger hr 130,00 R               

(e)   Flagmen hr 80,00 R                 

B19.02 Plant

(a)   Flat bed truck (7t) hr 500,00 R               

(b)   Tipper Trucks - 10mᵌ hr 450,00 R               

(c)   Tipper Trucks - 12mᵌ hr 500,00 R               

(d)   Dumper Trucks - 10mᵌ hr 450,00 R               

(e)   Tipper Trucks - 15mᵌ hr 800,00 R               

(f)   Loader  (2.5 ton) 950 hr 230,00 R               

(g)   TLB (digger loader) hr 500,00 R               

(h)    Excavator (20 ton) hr 1 200,00 R            

(i)    Excavator (25 ton) hr 1 300,00 R            

(j)    Excavator (30 ton) hr 1 400,00 R            

(k)    Excavator (Hummer only) HB1700 hr 1 500,00 R            

(l)   Grader (AT 140 G or similar) hr 750,00 R               

(m)   Roller (Smooth 12 ton) hr 500,00 R               

(n)   Roller pneumatic hr 400,00 R               

(o)   Roller Tow Tractor and Grid hr 600,00 R               

(p)   Roller (pad foot 12 ton) hr 600,00 R               

(q)    Water truck (11000 l) hr 500,00 R               

(r)    Water truck (12000 l - 14000 l) hr 600,00 R               

(s)    Water truck (15000 l - 18000 l) hr 700,00 R               

(t)    Jumping Jack hr 126,50 R               

(u)    Dozer (D7 or similar) hr 1 300,00 R            

(v)    Concrete Mixer 400L hr 35,00 R                 

(w)    Steel Drum Hand held Roller hr 500,00 R               

(x)    Sit On 1.5 ton hr 450,00 R               

(y)  Mobile Crusher 600 X 900 hr 2 800,00 R            

(z)  1000 Milling Machine (Skidsteer incl broom, forklift & bucket) hr 800,00 R               

(aa)  Crane Truck 8 ton hr 1 000,00 R            

(ab)  Roll back Truck 8 ton hr 1 200,00 R            

km 15,00 R                 

(ad)   Safety vehicle for pre-marking purposes hr 330,00 R               

(ae)   Compressor (air) including hose and tools (specify) hr 320,00 R               

hr 300,00 R               

hr 231,00 R               

hr 500,00 R               

(ai)   Mobile concrete mixers (specify size) 400kl capacity hr 1 000,00 R            

(aj)    Light delivery vehicle (LDV) km 7,50 R                  

(ak)   Centre-mount crane (specify size) hr 20 000,00 R          

(al)    Low bed truck (35t) km 130,00 R               

(w)   Other Specify  hr

19/120.02 m³-km 18,00 R                 

TOTAL CARRIED TO SUMMARY

Overhaul on material hauled in excess of 1.0km (ordinary overhaul)

(ah)    Cutting torch with mobile electric & oxy aceylene

(ag)   Mobile electric welding sets and accessories



(ac)  Suitable truck/but for transporting labourers



DESCRIPTION

(af)   Dewatering pump including generators and
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ITEM

NO.

UNIT RATE

SSPS 2100 :DRAINS -  ADDITIONAL AS REQUIRED

B21.01 Excavate for open drains

       (i)0m up to 1.5m m³ 120,00 R               

       (ii)Exceeding 1.5m and up to 3m m³ 200,00 R               

B21.02 Clearing and Shaping existing open drains m³ 125,00 R               

21.05 Banks and dykes m³ 300,00 R               

21.15 Overhaul for material hauled in excess of 1,0km  m³-km 18,00 R                 

free-haul (normal overhaul)

21.12 Backfilling existing eroded side drains m³ 50,00 R                 

B21.18 Clearing concrete drainage channels

(a)   Side drains, median drains and the like m² 75,00 R                 

       (i)   less than 1.0m m² 65,00 R                 

       (ii)  1.0m to 2.0m m² 85,00 R                 

21.19 Selected backfill material under concrete-lined side 

m³ 250,00 R               

B21.20 m 70,00 R                 

 grader

B21.03 Excavation in all material for subsurface drains

(i)  0 m up to 1.5m m³ 25,00 R                 

B21.04 Impermeable backfill to subsoil drainage system m³ 65,00 R                 

B21.20 Natural permable backfill (19mm Crushed stone) from  m³ 115,50 R               

approval sources on site

B21.07 Coarse sand from approved sources on site m³ 379,00 R               

B21.08 (i)  Perforated pitch fibre pipe (110mm) m 150,00 R               

(ii)  Non perforated pitch fibre pipe (110mm) m 200,00 R               

B21.10 Grade 2 Geotextile m² 50,00 R                 

TOTAL CARRIED TO SUMMARY

DESCRIPTION

(c)   Other drains and channels within the following invert

drains compacted to 93% of modified AASHTO

(a)   Excavating soft material situated within the following

TOTAL CARRIED BROUGHT FORWARD

Clearing and shaping side and mitre drains by
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ITEM

NO.

UNIT RATE

SSPS 2200 PREFABRICATED CULVERTS

22.01 Excavation

       (i)   0m up to 1.5m m³ 120,00 R               

(ii)Exceding 1.5m up to 3m m³ 140,00 R               

m³ 250,00 R               

220,00 R               

22.02 Backfilling:

(a)  Using the excavated material m³ 90,00 R                 

(b)  Using imported selected material m³ 120,00 R               

m³ 350,00 R               

22.03 Concrete pipe culverts:

(c)  On class B bedding

      (i)   600mm dia class 100D m 1 200,00 R            

      (ii)   900mm dia class 100D m 1 500,00 R            

      (iii)  750mm x 750mm box culvert Class 100D m 1 750,00 R            

250,00 R               

22.07 Cast in-situ concrete and formwork 4 500,00 R            

m³ 3 100,00 R            

m³ 3 500,00 R            

     surface finish (concrete class 25/19)

(d)   Formwork of concrete under sub item 22.07(c) above m² 530,00 R               

22.08 Concrete Backfill for Culverts m³ 3 000,00 R            

22.10 Steel reinforcement

(a)  Welded steel fabric (Ref 888) m² 30,00 R                 

(b)  Welded steel fabric (Ref 617) m² 45,00 R                 

(c)  Welded steel fabric (Ref 395) m² 120,00 R               

(d) Y16 Dowels No 40,00 R                 

(e) High Tensile steel t 22 000,00 R          

22.13 Removing and disposing of existing pipe culverts (600 up to 1200mm) m

15,00 R                 

Overhaul on excavated materials as described, in  m³- km 18,00 R                 

excess of  free haul distance of 1km

22.22 m³ 250,00 R               

Precast Concrete Headwalls - Supply and 

Install complete, to manufacturer's specifications

(i) 600 mm dia  No 1 100,00 R            

(ii) 900 mm dia  No 1 400,00 R            

Access and drainage

(a)  Amount to deal with water during construction of

 bridge and access, including re-routing of water and 

Lump sum 1 500,00 R            

temporary damming

TOTAL CARRIED TO SUMMARY

22.25

(b)  Extra over sub item 22.01(a) for excavating in hard

     material, irrespective of depth

(c)  Extra over sub item 22.02(a) and (b) for soil cement 

      backfilling

22.100

(a) In Class A bedding, screeds and encasing of pipes,

(c)   Inlet & outlet structures, skewed ends, catchpits,

(a)   Excavating soft material situated within the following

DESCRIPTION



Hand excavation to determine the position of existing  services
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ITEM

NO.

UNIT RATE

SSPS 3200 SELECTIONS, STOCKPILING AND BREAKING-DOWN THE

MATERIAL FROM BORROW PITS, CUTTINGS AND EXISTING

PAVEMENT LAYERS, AND PLACING AND COMPACTING

THE GRAVEL LAYERS

32.01 Provision of crushing and/or screening plant:

(a)  Single stage crusher No 80 000,00 R          

32.02 Re-erecting the crusher and/or screening plant:

(a)  Single stage crusher No 100,00 R               

32.03 Crushing and screening:

(a)  Single stage crusher m³ 35,00 R                 

32.05 Additional normal grid rolling m³ 15,00                    

32.06 Stockpiling of material m³ 10,00 R                 

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 3300 MASS EARTHWORKS

33.01 Cut & borrow to fill, including free-haul up to 0.5km:

(a)  Material in compacted layer thickness of 200mm and less:

      (ii)  Compacted to 93% Mod AASHTO m³ 220

33.03 Extra over item 33.01 for excavating and breaking down 

material in:

(a)  Intermediate excavation m³ 250

(b)  Hard Excavation m³ 350

33.04 Cut to spoil, including free-haul up to 1.0km.  Material obtained 

from:

(a)  Soft excavation m³ 100

(b)  Intermediate excavation m³ 250

(b)  Hard excavation m³ 350

33.08 Widening of Cuts (extra over item 33.01, 33.02 and 33.03)

(a) In hard materials m³ 350

33.12 In situ treatment of roadbed 

(b)  insitu treatment by ripping m³ 45

33/16.02 Overhaul on material hauled in excess of 1,0km m³-km 18

(ordinary overhaul)

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 3400 PAVEMENT LAYERS OF GRAVEL MATERIAL

B34.01 Pavement layers constructed from gravel taken from cut or 

borrow including free haul up to 1.0km

(a) Gravel Subbase layer compacted to:

(i) 93% modified AASHTO density (150mm) m³ 280,00 R               

(b)  Gravel wearing course compacted to

      (ii)   95% Mod AASHTO density:

            200mm layer thickness m³ 372,40 R               

34.07 Extra over for temporarily blading the material to  m³ 30,00 R                 

windrow

B34.14 Wet blading

(a)  7m road width (riding surface) km 3 600,00 R            

B34.15 Dry blading

(a)  7m road width (riding surface) km 3 050,00 R            

B34.18 Reshaping

(a) 7m road width (riding surface) km 20 000,00 R          

B34.19 Heavy maintenance

(a)   7m road width (riding surface) km 40 000,00 R          

B34.20 Patch Gravelling (regravelling in short sections) m³ 364,00 R               

B34.21 Light roadbed preparation

(c)   6m road width (riding surface) km 10 000,00 R          

B34.22 Heavy roadbed preparation

(c)   6m road width (riding surface) km 20 000,00 R          

B34/33.03Extra over Items 34.01 (h) (ii) for excavation in

(a)  Intermediate excavation m³ 250,00 R               

(b)  Hard excavation m³ 350,00 R               

34/120.02 Overhaul on material hauled in excess of 1,0km (ordinary overhaul) m³-km 18,00 R                 

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 5100 PITCHING, STONEWORK AND PROTECTION AGAINST 

EROSION

51.01 Stone pitching

(b)  Grouted stone pitching m² 280

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 5200 GABIONS

52.01 Foundation trench excavation and backfilling:

(b)  In all other classes of materials m³ 220

52.02 Surface preparation for bedding the gabions m² 50

52.03 Gabions

(a)  Galvanised gabion boxes m³ 1650

      (i)  1,0m wide x 1,0m wide boxes,  4mm mesh wire x 80mm mesh sides

(c)  Galvanised gabion mattresses m³ 1500

      (i)  0,20m diaphragm spacing, 5,0m long by 2,0m wide

           by 0,3m deep mesh 80mm

52.04 Filter fabric

(a)  Bidim U14 or similar approved m² 65

B52.05 Dismantle and remove gabion structures m³ 300

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 5400 GUARDRAILS

54.01 Guardrails on timber posts:

(a)  Galvanised m 950

54.03 Extra over 54.01 for horizontally curved guardrails factory

bent to a radius less than 45m m 180

End treatments: 

(d)  End treatments in accordance with the drawings 

7000

     where single guardrail sections are used

54.05 Additional guardrail posts:

(a)  Timber No 300

54.06 Reflective Plates No 35

54.15 Adjusting spacer blocks and tightening bolts No 10

B54.16 Remove existing guardrails and replace m 150

TOTAL CARRIED TO SUMMARY

No

DESCRIPTION

54.04
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ITEM 

NO.

UNIT RATE

5500 FENCING (emergency repairs)

55,01 Clearing the fence line, 2m wide strip km

B55.02 Supply and erect new fencing material for new fences and for

supplementing material in existing fences which are being repaired or 

removed:

(a) Zinc-coated barbed wire (Mild steel grade ,double stranded, uni-directional twist  km

wire, 2.5mm diameter)

(b) Zinc-coated smooth wire (High-tensile-grade steel 2.24mm diameter) km

(g) Standards (2.5kg/m "y" sections, 1850mm, steel) No

(h) Droppers (1400mm x 0.56kg/m steel) No

(i) Straining posts, stays and anchors:

(i) Vertical:

- Steel straining posts (2130mm x 100 mm dia. x 2mm mild steel 

tubing with 

   steel cap and 230 x 230 x 2 base plate fully galvanised.) No

- Timber straining posts (150mm diameter) No

(ii) Inclined:

- Steel straining posts (2130mm x 50 mm dia. x 2mm mild steel tubing 

) 

No

(iii) Horizontal:

- Timber stays as anchors (125mm diameter) No

(j) Dipping of wire in yellow paint km

B55.03 New gates

(a) Farm gates as per drawings No

(b) Pedestrian gates as per drawings No

B55.05 Dismantelling existing fences:

(a) Fences:

(i) Stock Proof Fences km

(b) Gates No

55,07 Ringbolts for anchoring fencing to structures No

B55.10 Trimming the fence line, 2m wide strip km

CARRIED FORWARD TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 5600 ROAD SIGNS

56.01 Road sign boards complete with supports with Class 1

retro-reflective background.  Symbols and lettering in semi matt

black. Boarders in Class 1 retro-reflective material, where the

signboard is constructed from: 

(c)  Pre-painted galvinised steel plate (1.2mm chromadek or

      approved equivalent)

(i) 900mm diameter Round or Stop signs:

R 1 No. 800,00 R               

R 201 (40) No. 750,00 R               

(iii) 900mm Triangular Combination signs

WCE. 2 (W208 + for 5km) No.

(iv) 150mm x 600mm Hazard Marker Signs

W401 No. 200,00 R               

W402 No. 204,00 R               

(v) 450mm x 450mm Hazard Marker Signs

W405 No. 350,00 R               

W402 No.

56.03 Road Sign Supports

(a)  Steel tubing t

(b)  Timber (treated 85mm - 100mm diameter) m 80,00 R                 

      

56.05 Excavating and backfilling for road signs supports  m³ 75,00 R                 

56.06 Extra over item 56.05 for cement-treated backfilling m³ 130,00 R               

TOTAL CARRIED TO SUMMARY

DESCRIPTION
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ITEM

NO.

UNIT RATE

SSPS 8100 :TESTING WORKMANSHIP AND MATERIALS

81.02 Other special tests requested by the Engineer Prov Sum 10 000,00             

(a)  Handling costs and charges for the Contractor  % 10%

on item 81.02

TOTAL CARRIED TO SUMMARY

DESCRIPTION


