	[image: image1.jpg]Cskom






	Interior Specifications for Eskom
	Ref: 

Policy  ESK PB AAQ 3

	
	
	Rev 2


The following specifications for interiors.  

1. Material (upholstery and screens)

Upholstery (chairs and couches):  See attachment for material specifications
	Fabric
	Colour
	Code

	Weavers World
	See specifications on the other attachment
	


Screens 
	Fabric
	Colour
	Code

	Weavers World
	See specifications on the other attachment
	


(All fabrics are available from Weavers Warehouse. 
 Contact Steve at 011- 464 1781)  

2. Paint

Old references:

Plascon colour Expressions   
E14 – 2 (Hudson) or 

E14 – 3 (Papyrus)
E14 – 4  (Mayan Stone) or

E14 – 5 (Sombrero)

New references:


Plascon colour Inspired  

Y1-C2-3 (Pale Linen) or

Y2-D2-3 (Veldrift) or

Y2-D2-2 (Stone Wash)

Y2-D2-1 (Waxen Tint)

Blue paint as an accent colour (any paint that matches Eskom’s blue – Pantone 287).  Only to be used as an accent colour in very small amounts.  (Plascon has also matched a blue colour: S3560-R80B).
You may choose any of the four colours above.  (You may apply one colour only, or two or three or all four, but only from the range above).  No other paint colour may be used inside Eskom’s buildings.
3.
Wallpaper:  

Majestic range:  Fiberglass  (paint it with any of the suggested paint colours) or
Majestic range:  Caro-Line No CRA 201 (warm, beige colour) or
Décor:  Capri No 5543 (same colour as paint)
4.        Blinds and curtains

*  Blinds: 

Only blinds in front of windows:  Blinds must be in the same colour as the wallpaper or the wall paint or it must be the same blue as the upholstery material.  

People must use their discretion whether it should be the same colour as the walls or as the blue of the upholstery.  (Small venues look bigger when there is no contrast on the walls).

Blinds and curtains in front of windows:  Blinds must be in a blue that match the curtains and the upholstery material or in the same colour as the wallpaper or the wall paint. 

*  Curtains:  

Curtains must match the upholstery material.  (Blue or the Eskom gold or a 
combination of the two, but it must match the upholstery material)

5.         Carpets  
Nexus:  Berber Point - colour Jute or Raffia with a bitumen backing 

 OR
  Any commercial or industrial duty carpet in the same colour as this Jute or 
  Raffia  colour

                                      
             OR

Nexus:  Berber Point – a plain blue colour that will complement the upholstery 
material (with a bitumen backing) 

 OR

Any commercial or industrial duty carpet in a plain blue colour  or a plain gold 
colour that will complement the upholstery material.  (Carpet must not show marks 
easily).

6.
Tiles
Must be something between gray and beige, but not gray only and also not beige only

Supplier:       Any tile supplier

Criteria:  
Must be a commercial tile (if possible) or a tile that will carry heavy 




traffic



Not slippery




Should not show dirt easily




No varnish finishes on tiles

Must complement the rest of the colour palette for Eskom interiors (something between gray and beige, but not gray only and also not beige only)

Always buy extra tiles to be able to replace broken tiles at a later stage.

7.
Furniture  (See standards for upholstery) 

Furniture finishes to be light maple.  (No black edges on desks, but edges (beading) must match light maple colour)  

Filing cabinet may have a black door.
Surface of reception desk:  light maple or Formica – Sierra Granite (top Face) 534 -  or granite.

Specifications for powder coating of desk/table legs, cabinet and credenza handles, etc.:     

Akzo Nobel.  Range:  Interpon 600 Matt,  ANP 9054,  Cowrie Gold
Chairs must be upholstered in Eskom material and it must have black arm rests or light maple arm rests.   The legs of the chairs must be in light maple or in black.
8.        Desk accessories, pot plant holders, dust bins, frames for office screen,   

           door frames and frames for posters/awards, wall clocks
Desk accessories, dust bins, frames for office screens/doors: Cowrie Gold (see point 7 for details) or maple colour finishes.

Pot plant holders:  the Eskom metallic gold (Pantone 8004C)
Frames for posters/awards/paintings, wall clocks, etc: Refrain from using very heavy and wide frames.  Rather opt for lighter and narrower frames.  Ensure that the colour of the frame matches the Eskom Pantone swatch 8004 (Eskom gold) as closely as possible.  Note that this pantone is not yellow gold and neither is it an aluminum colour.  Frames and wall clocks may also be in a light maple colour.
Frames can be ordered from any supplier.

Specifications for powder-coating:     Akzo Nobel.  Range:  Interpon 600 Matt, ANP 9054,   Cowrie Gold

9.
Exterior finishes

No colour specifications have been set for the outside of buildings, but it is recommended that the buildings be painted one of the following colours:  white/light cream/light gray/ Plascon E14-2/Plascon E14-3.  (New references: (Plascon) Inspired Y2-D2-2 (Stone Wash), Y2-D2-1 (Waxen Tint). 
The roofs should be painted in a dark charcoal or brown and the fascias should be the same colour as the outside walls.

If unsure about any interior applications (excluding the furniture ordering or specifications), please call your communication manager/practitioner or the Corporate Identity (CI) representative for your division or Hanlie Smit at Head Office.

