{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["BoQ","Ps & Gs","Transport"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"BoQ","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"merged":[[1,4,1,7],[2,4,2,7],[3,4,3,7]]}
[]
[null,null,"System Parameter"]
[null,null,"Minimum PV (Wp)"]
[null,null,"Minimum BESS (kWh)"]
[{"$nulls":3},"Unit of measure","Unit","QTY","Supply rate","Labor rate"]
[null,"Line Item","Notes / Description"]
["A","Pre-Construction Activities"]
[1,"Site Assessment","Initial site visit: roof structural capacity, shading analysis, rooftop layout, safety assessment. ","Sum"]
[2,"Feasibility Study and Report","Evaluate if the system is viable: generation estimates, ROI, structural modifications, grid export potential, interconnection constraints.","Sum"]
[3,"System Detailed Engineering & Design","Electrical single-line diagrams, string design, mounting layout, earthing, switchgear design, protection. Comply with NRS / SANS standards. ","Sum"]
[4,"SSEG Application / Registration","Prepare and submit the SSEG application to Eskom or municipal utility. Required parts include SLD, CoC, inverter spec, EGI report, etc.","Sum"]
[]
["B","Construction"]
[1,"PV Modules","Supply of PV solar modules (panels) - number and power depending on system size.(miniumum 550W)","Each",null,null,"Cost plus fee"]
[2,"PV Mount System_Roof","Roof-mounted racking, rails, brackets, supports; structural components for mounting.","Each",null,null,"Cost plus fee"]
[3,"PV Mount System_ Parking Structure",null,"Each",null,null,"Cost plus fee"]
[4,"PV Mount System_ Hollow Container",null,"Each",null,null,"Cost plus fee"]
[5,"Hybrid Inverters","Inverters capable of handling multiple energy sources(PV, Battery, Grid or generator). Must comply with NRS-097-2-1 ","Each",null,null,"Cost plus fee"]
[8,"Batteries (LFP, installed)","Supply & installation of lithium-iron phosphate (LFP) batteries.","Each",null,null,"Cost plus fee"]
[6,"Battery BoS (Cabinets, Cables, Protection)","Battery enclosures, interconnect cabling, safety disconnects, fuses, battery management system wiring.","Each",null,null,"Cost plus fee"]
[7,"PV BoS (AC/DC, cables, DBs, protection, combiner box)","DC cabling, AC cabling, combiner / junction boxes, protection devices (fuses, surge arrestors), distribution boards. Appropriate sizes and standards upto 20m from customer DB","Each",null,null,"Cost plus fee"]
[]
[null,"Post Construction Activities"]
[1,"Testing, Commissioning & CoC","Functional tests, safety checks, inverter commissioning, Certificate of Compliance (CoC) by a registered electrician per SANS 10142-1 / SANS 10142-1-2. (SAPVIA PV GreenCard compliance or equivalent.","per project"]
[2,"Add on service: Training","Training for installers / maintenance staff; could be via PV GreenCard course or equivalent. The SAPVIA PV GreenCard installer course (5-day) gives both theoretical and practical training. \nAssessment: PV GreenCard assessment or quivalent as required","per/person"]
[3,"Add on service: Internet Access / Connectivity for Inverter/Remote monitoring - Where no internet available.","Required minimum for remote inverter / system monitoring in sites where no fixed-line broadband is available. Could include 4G router, SIM-slot, external antenna (if needed), installation and configuration. Could also include a data-subscription option.","Cost plus fee"]

{"sheet":"Ps & Gs","index":1,"n_rows":17,"n_cols":9,"rows_kept":17,"merged":[[1,2,1,5],[16,2,16,6]]}
[]
[null,null,"Preliminaries & General"]
[null,null,"Item","Reference Drawing","Description","Unit","Rate","QTY","Amount"]
[{"$nulls":4},"Every Invoice to be signed and verified by Quantity Surveyor for payment."]
[null,null,1,null,"Site Establishment"]
[null,null,1.1,null,"Overheads for project (This includes Site Establishment Overhead Costs, Office Overheads, Administration Costs etc.) Total Labour Value","%"]
[null,null,1.2,null,"Health and Safety Management, OHSA appointments, PPE etc. Total Labour Value","%"]
[null,null,1.3,null,"Quality & Contract Management. Total Labour Value","%"]
[null,null,1.4,null,"Environmental Management & Site maintenance. Total Labour Value","%"]
[null,null,1.5,null,"De-establishment & Rehabilitation of Site","Sum"]
[null,null,1.6,null,"Security","Cost plus fee"]
[null,null,1.7,null,"Facilities for security (Guard house, toilet etc.)","Month"]
[null,null,1.8,null,"CLO (If required) (Max Value)","Month"]
[null,null,1.9,null,"Registered SACPCMP Construction Manager (Proof of registration required)","Weekly"]
[null,null,{"v":1.1,"d":"1.10"},null,"Safety Officer","Day"]
[null,null,1.11,null,"Responsible person","Day"]
[null,null,"TOTAL"]

{"sheet":"Transport","index":2,"n_rows":14,"n_cols":8,"rows_kept":14}
[]
[]
[{"$nulls":3},1,"TRANSPORT","Unit","Quantity","Rates"]
[{"$nulls":3},1.1,"LDV","km"]
[{"$nulls":3},1.2,"Personnel Transport for Staff","km"]
[{"$nulls":3},1.3,"10 m³ Tipper Truck","km"]
[{"$nulls":3},1.4,"6 m³ Tipper Truck","km"]
[{"$nulls":3},1.5,"Transport Truck 2-4 ton","km"]
[{"$nulls":3},1.6,"Transport Truck 5-8 ton","km"]
[{"$nulls":3},1.7,"Transport Truck 5-8 ton with crane","km"]
[{"$nulls":3},1.8,"Transport Truck 9-14 ton","km"]
[{"$nulls":3},1.9,"Transport Truck 9-14 ton with crane","km"]
[{"$nulls":3},{"v":1.1,"d":"1.10"},"Lowbed","km"]
[{"$nulls":4},"Total carried forward to summary"]