{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"merged":[[0,0,0,4],[24,0,24,3]]}
["Building renovation: Hydroponics Store rooms"]
["Service description","UoM","Quantity/size","Area","Unit Price","Total Cost"]
["Paint (maroon) the zinc store  all sides and the roof(Roof must be patched where necessary and be rubberised with water proof paint)","614.1 m2 metal paint",1,"Storeroom 1"]
["4 zinc sheets to be replaced ","3.1 m",4,"Storeroom 1"]
["Supply and install master pad locks ","7.8 x 5.2 x 3.1 cm alloy steel",5,"Storeroom 1"]
["Repairing zink store lower belt with a sloping 20 cm slab and water-resistant paint","25mx12.5m",1,"Storeroom 1"]
["Painting the zinc store floor (epoxy with resins grey in colour)","25mx12.5m",1,"Storeroom 1"]
["In store compartments made with ganvanised steel and mesh sieve with a lockable doors ","2.4m x 3.6mx2m one will be L-shaped and two will be U-shaped",3,"Storeroom 1"]
["Repatch the windows where cracked or worn off putties ","900mmx9.5 mm",6,"Storeroom 1"]
["Repairing of ventilation openings with a mesh sieve, replace with a similar sieve ","1mx1m",2,"Storeroom 1"]
["Paint the zink store  all sides and the roof(Roof must be patched where necessary and be rubberised with water proof paint)","614.1 metal paint",1,"Soreroom  2"]
["Supply and install 12 window gl with handles and hinges ","45 x30 cm",12,"Soreroom  2"]
["Supply and install 6 window glass","95x30 cm",6,"Soreroom  2"]
["Seal and repair were putty is missing or weared",null,6,"Soreroom  2"]
["Repairing zinc store lower belt with a sloping 20 cm slab and water-resistant paint","25x12.5m",1,"Soreroom  2"]
["Supply and install master pad lock ","x4",4,"Soreroom  2"]
["Door replacements ","Door size",2,"Soreroom  2"]
["New zinc sheet to cover holes and repair where the rust has damaged the window ","1.1x10 m at the back and 1.1 x 16 m at the front","2 sides ","Soreroom  2"]
["Supply of Rubber matt","2mx2m",2]
["5. Contractor to adhere to OHS contract management compliance e.g. Complete contractor SHE file"]
[null,null,"Total cost"]
[null,null,"VAT"]
[null,null,"Grand Total "]
[]
["Compulsory Conditions attached to the projectFailure to submit all the above compulsory requirements will lead to disqualification"]
["1. CIBD Grade:  1GB and above"]
["2. Gant chart project plan should be submitted"]
["3. Compulsory Site Briefing"]
[]
["Conditions attached to the project"]
["1. Any default against the project plan will attract R500.00 per day."]
["2.Full payment will be action upon project completion, there will be no partial payment"]
["3.Contractor to clean up all the rubbles from the site"]
[" 4. Contractor must ensure personell have full PPE regalia relevant to the project, failure to comply with this might result in the termination of the project"]

{"sheet":"Sheet2","index":1,"n_rows":10,"n_cols":5,"rows_kept":10}
[]
[]
[]
[]
[]
[{"$nulls":4},36.6]
[{"$nulls":4},345]
[{"$nulls":4},155]
[{"$nulls":4},77.5]
[{"$nulls":4},{"$f":"SUM(E6:E9)","v":614.1}]