{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Unpriced BOQ"],"not_rendered":{"external_links":14,"defined_names":573},"read":"whole","date_system":"1900"}

{"sheet":"Unpriced BOQ","index":0,"n_rows":35,"n_cols":5,"rows_kept":35}
["Item No.","Description","UOM","Quantity ","RATE"]
[null,"Aux Boiler C&I Spares"]
[1,"MODULE: TYPE: ETHERNET SWITCH; POWER SOURCE: 12-30 V DC; APPLICATION: AUX BOILER; DIMENSIONS: 114X45X99 MM; MANUF P/N:\nMD741-1; SINUAT; RJ45 PLUG; SPEED: 10/100MBS","Each",4]
[{"$f":"A3+1","v":2},"SCANNER: TYPE: FLAME; POTENTIAL: 220 V; CURRENT: 4-20 MA; SUPPL P/N: 7-7955-1064273; MODEL NO: FLS 09 UV5","Each",6]
[{"$f":"A4+1","v":3},"UNIT: TYPE: FLAME MONITOR UNIT; APPLICATION: AUX BOILER; SUPPL P/N: FLUS O6 UV; REFERENCE NO: 7-8385-602164; MATERIAL OF THE FRONT PANEL ALUMINIUM; 2 LED DISPLAYS; AMBIENT TEMPERATURE -10 TO 60 DEG; TYPE OF MOUNTING PLATE FASTENING; HOUSING MATERIAL POLYCARBONATE; DEGREE OF PROTECTION IP20; DIMENSIONS: WD 100\nX HT 75 X DP 110 MM","Each",20]
[4,"SCANNER: TYPE: FLAME; POTENTIAL: 42 VDC; CURRENT: 15 MA; POWER:\n0.63 W; SUPPL P/N: FLS 09-UV-5; REFERENCE NO: 7-7955-602167; AMBIENT TEMPERATURE -10 TO 60 DEG C; HOUSING MATERIAL BRASS, NICKEL PLATED; DEGREE OF PROTECTION IP 65; WITH 3 M CONNECTING LINE","Each",20]
[5,"SWITCH, LIMIT: ENCLOSURE: IP67; DIMENSIONS: WD 40.5 X LG 103.5 X HT 38 MM; SUPPL P/N: ZS-335-11Z-1637","Each",20]
[6,"CONTACT MCB-01G / 1SFA611610R1110, ELEMENT HOLDER MCBH5-00 /1 SFA611601R1100 ROTARY UNLOCKING MPMT3-10R / 1SFA611510R1001, \"EMERGENCY STOP\" LABEL NAS-USE90 / GJD9432256R1592","Each",3]
[7,"INDICATOR, SIGHT FLOW: SUPPL P/N: VZO25S","Each",3]
[8,"THERMOMETER, TYPE: PE 02.40.00","Each",4]
[9,"PRESSURE SWITCH, TYPE: DG 50 B","Each",8]
[10,"SWITCH, PRESSURE: TYPE: AIR; RANGE: 0-150 MBAR; ACTION: DPST; ENCLOSURE RATING: IP54; MANUF P/N: DL150A-31; CONNECTION: BOTTOM 1/2 IN-NPT; POTENTIAL: 250 VOLT ALTERNATING CURRENT; CURRENT: 5\nAMPERE; POWER: 250 VOLT ALTERNATING CURRENT; CONTACT ARRANGEMENT: 1NO 1NC","Each",8]
[11,"ELECTRONIC TEMPERATURE CONTROLLER TYPE ELTC/1-4/05. SUPPLY VOLTAGE:\n230V, +/- 10%, 50HZ, SWITCHING CAPACITY 16A; MEASURING INPUT: PT100 DIN 2- WIRE; ADJUSTMENT RANGES:\n+150…+400°","Each",3]
[12,"CAPILLARY THERMOSTAT, TYPE: ELTH/3 /\n1 POLE","Each",10]
[13,"FLOW MEASURING, TYPE: PROLINE\nPROWIRL 72 F1H / 72F1H-SE1AARAAA4AA","Each",2]
[14,"FLOW MEASURING, TYPE: PROLINE\nPROWIRL 72 F80 / 72F80-SE1AARAAA4AA","Each",5]
[15,"EPHY MESS MOTOR PROTECTION THERMISTOR, TYPE DPTC-SH","Each",10]
[16,"SWITCH BOX, TYPE: WDB0101201","Each",3]
[17,"GESTRA- SENSOR TYPE NRG 16-11, G3/4\", L=1000MM, TRANSMITTER TYPE NRS 1-7 B","Each",8]
[18,"GESTRA- SENSOR TYPE NRG 16-12, G3/4\", L=1000MM, TRANSMITTER TYPE NRS 1-8 B","Each",8]
[19,"CONDUCTIVITY TRANSDUCER / REGULATOR, TYPE: LRGT 16-1 - KS90 /\nPN40 - G1\" / L=615MM","Each",5]
[20,"LEVEL TRANSMITTER, TYPE: NRGT 26-1 / 230V - 50HZ / G3/4\" / EN10204-3.1 / L=794MM / WATER","Each",5]
[21,"IER EBERHARD HENKEL-MAGNETIC FLAP INDICATOR MAGTOP V4 F3C M4 EXH / ME=2000MM WITH LIMIT SWITCH MAGTOP SNAP 201","Each",4]
[22,"FILL LEVEL PROBE, TYPE: NIVOMAT FSG\n1CA / ME=2000MM","Each",2]
[23,"REFLEX LEVEL GAUGE TYPE: LG 40-X2, KOM.-NO.\n2009-202167; SIZE 10 / A=500MM / E=350MM / H=75MM / J=75MM / G=130MM,\nSTOP VALVETYPE A130; DRAIN VALVE TYPE AV 500","Each",5]
[24,"DOUBLE TWO POINT TEMPERATURE MONITOR, TYPE: AMV 2-2","Each",8]
[25,"SURFACE-MOUNTING THERMOSTAT, TYPE: ATHF-70","Each",5]
[26,"SAFETY SWITCH, TYPE: AZ 15 ZVK","Each",8]
[27,"MAGNETIC FLOAT SWITCH, TYPE: 200 L /\nSERIAL 160002303 /\n37603455","Each",5]
[28,"SWITCH, TYPE: 4-EVSA 10NH4.P.02.32.64","Each",3]
[29,"PRESSURE GAUGE, TYPE:\n111.12 /NS=63 / 0 - 6 BAR / G1/4\" B","Each",8]
[30,"PRESSURE GAUGE, TYPE:\n213.53 /\nNS=100 / 0 - 6 BAR / R 1/2\" / LM","Each",3]
[31,"GAUGE, PRESSURE: DIAL SIZE: 160 MM; CONNECTION SIZE: G1/2 IN; CASE MATERIAL: STAINLESS STEEL; CONNECTION MATERIAL: STAINLESS STEEL; CONNECTION LOCATION: BACK LOWER; MOUNT: SCREW; FILLED: GLYCERINE 99.7 PCT;\nSPECIFICATION: 233.50;\nRANGE: 0-2.5 MEGAPASCALS; TUBE MATERIAL: STAINLESS STEEL; CONNECTION TYPE: THD","Each",10]
[32,"PRESSURE GAUGE, TYPE: 612.20 / NS=100 / 0 – 600 KPA / R 1/2\" / LM","Each",3]
[33,"THERMOMETER, TYPE: S73.160 /\nNS=160 / 0 - 400 °C / CONN. NO. 3 /\nUNION NUT M24X1,5 / L1=355MM","Each",8]