{"text_format":"3","workbook":"xlsx","n_sheets":14,"sheets":["Profile","Category 1","Category 2","Category 3","Category 4","Category 5","Category 6","Category 7","Category 8","Category 9","Category 10","Category 11","Category 12","Category 13"],"not_rendered":{"defined_names":40},"read":"whole","date_system":"1900"}

{"sheet":"Profile","index":0,"n_rows":192,"n_cols":4,"rows_kept":192,"merged":[[1,0,1,3],[3,0,3,3],[20,0,20,3],[49,0,49,3],[60,0,60,3],[71,0,71,3],[80,0,80,3],[92,0,92,3],[106,0,106,3],[125,0,125,3],[131,0,131,3],[145,0,145,3],[161,0,161,3],[187,0,187,3]]}
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[]
["1. MEDICAL BOWLS, KIDNEY DISHES, MEASURING JUGS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-01-01","Medical Bowl, type A"]
[2,"RT24-01-02","Medical Bowl, type B, 100mm"]
[3,"RT24-01-03","Medical Bowl, type B, 150mm"]
[4,"RT24-01-04","Medical Bowl, type B, 200mm"]
[5,"RT24-01-05","Bowl Stand, type A"]
[6,"RT24-01-06","Kidney Dish, 150mm"]
[7,"RT24-01-07","Kidney Dish, 195mm"]
[8,"RT24-01-08","Kidney Dish, 260mm"]
[9,"RT24-01-09","Measuring Jug, Plastic, 500ml"]
[10,"RT24-01-10","Measuring Jug, Plastic, 1000ml"]
[11,"RT24-01-11","Measuring Jug, Plastic, 2000ml"]
[12,"RT24-01-12","Measuring Jug, Stainless steel, 500ml"]
[13,"RT24-01-13","Measuring Jug, Stainless steel, 1000ml"]
[14,"RT24-01-14","Measuring Jug, Stainless steel, 2000ml"]
[]
["2. HOSPITAL BEDS, MATTRESSES"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-02-01","Bassinet, hospital, type A, on stand complete with mattress "]
[2,"RT24-02-02","Bassinet, Height-adjustable"]
[3,"RT24-02-03","Infant Cot, Rising backrest"]
[4,"RT24-02-04","Infant Cot, Height-adjustable"]
[5,"RT24-02-05","Adolecent Bed, Electric"]
[6,"RT24-02-06","Gynaecology Examination Chair, Electric"]
[7,"RT24-02-07","Gynaecology Examination Chair, Hydraulic"]
[8,"RT24-02-08","Delivery Bed, Electric"]
[9,"RT24-02-09","Delivery Bed, Hydraulic"]
[10,"RT24-02-10","Chemo-Dialysis Chair"]
[11,"RT24-02-11","Examination couch, with Tilting Backrest"]
[12,"RT24-02-12","Examination Couch, Height Adjustable"]
[13,"RT24-02-13","Trolley/Stretcher, Transport"]
[14,"RT24-02-14","Trolley/Stretcher, emergency, Basic "]
[15,"RT24-02-15","Trolley/Stretcher, emergency, patient, Electric"]
[16,"RT24-02-16","Bed, Hospital, Hydraulic"]
[17,"RT24-02-17","Bed, High Low, Electric, 3-Section"]
[18,"RT24-02-18","ICU Bed, 4-Section, Electric"]
[19,"RT24-02-19","ICU Bed, Multi-function, Electric"]
[20,"RT24-02-20","ICU Bariatric Bed, 4-Section, Electric"]
[21,"RT24-02-21","Bariatric Bed, ICU, Electric"]
[22,"RT24-02-22","MRI Stretcher"]
[23,"RT24-02-23","Mortuary Stretcher"]
[24,"RT24-02-24","Mortuary Hydraulic Elevation Trolley"]
[25,"RT24-02-25","Patient Hoist, Electric, Mobile"]
[26,"RT24-02-26","Bariatric Patient Hoist, Electric"]
[]
["3.  BED PAN AND URINALS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-03-01","Bedpan Slip-in, with handle (Re-usable)"]
[2,"RT24-03-02","Bedpan and urinal stand"]
[3,"RT24-03-03","Bedpan Slip-in, with handle and Lid (Re-usable)"]
[4,"RT24-03-04","Bedpan, with Lid"]
[5,"RT24-03-05","Bedpan Slip-in, (Disposable)"]
[6,"RT24-03-06","Urinal, Male, Plastic"]
[7,"RT24-03-07","Urinal, Male, Stainless Steel"]
[8,"RT24-03-08","Urinal Rack, Wallmount"]
[]
["4.  CABINET UNITS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-04-01","Hospital Food Trolley, stainless steel, Large"]
[2,"RT24-04-02","Hospital Food Trolley, ABS Polymer, Large"]
[3,"RT24-04-03","Hospital Food Trolley, stainless steel, Medium"]
[4,"RT24-04-04","Hospital Food Trolley, ABS Polymer, Medium"]
[5,"RT24-04-05","Drug Cabinet, wall-Mount, Small"]
[6,"RT24-04-06","Drug Cabinet, wall-Mount, Large"]
[7,"RT24-04-07","First-Aid Cabinet, Metal"]
[8,"RT24-04-08","First-Aid Cabinet, Plastic"]
[]
["5.  THEATER TABLES"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-05-01","Theater Table, Standard"]
[1,"RT24-05-02","Theater Table, Bariatric","Appenidix F"]
[2,"RT24-05-03","Universal Orthopaedic Accessories Set"]
[3,"RT24-05-04","Universal Neurosurgery Accessories Set"]
[4,"RT24-05-05","Universal Spinal Accessories"]
[5,"RT24-05-06","Theater Table Replacements Accessories"]
[]
["6.  RESTRAINT SYSTEMS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-06-01","Restraint system (Pair), wrist bands, Small"]
[4,"RT24-06-02","Restraint system (Pair), wrist bands, Medium  "]
[5,"RT24-06-03","Restraint system (Pair), wrist bands, Large  "]
[2,"RT24-06-04","Restraint system (Pair), ankle bands, Small"]
[6,"RT24-06-05","Restraint system (Pair), ankle bands, Medium"]
[7,"RT24-06-06","Restraint system (Pair), ankle bands, Large"]
[3,"RT24-06-07","Restraint system, waist belt, Small"]
[8,"RT24-06-08","Restraint system, waist belt, Medium"]
[9,"RT24-06-09","Restraint system, waist belt, Large"]
[]
["7.  LOCKER , TABLE UNITS AND OVERBED"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-07-01","Bedside Locker, Mild Steel"]
[2,"RT24-07-02","Bedside Locker, ABS Plastic"]
[3,"RT24-07-03","Bedside Locker, HPL"]
[4,"RT24-07-04","Overbed Table, Wood"]
[5,"RT24-07-05","Overbed Table, ABS Plastic"]
[6,"RT24-07-06","Overbed Table, HPL"]
[7,"RT24-07-07","Overbed Table, HPL with Tilting Top"]
[5,"RT24-07-08","Table, utility, 810 mm ","Appendix P"]
[6,"RT24-07-09","Table, utility, 1 720 mm ","Appendix P"]
[7,"RT24-07-10","Table, utility, 1 720 mm with castors","Appendix P"]
[8,"RT24-07-11","Table, Mayo"]
[]
["8.  SCALES"]
[]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-08-01","Scale, Electronic, Infant","Appendix H"]
[2,"RT24-08-02","Scale, Electronic, Neonatal","Appendix H"]
[3,"RT24-08-03","Scale, Analog, Neonatal","Appendix H"]
[4,"RT24-08-04","Scale, Analog, bathroom type","Appendix H"]
[5,"RT24-08-05","Scale, electronic, bathroom type","Appendix H"]
[6,"RT24-08-06","Scale, Analog, with Height rod","Appendix H"]
[7,"RT24-08-07","Scale, Adult, Electronic, Height & Weight","Appendix H"]
[8,"RT24-08-08","Scale,Electronic, Multifunctional Use"]
[9,"RT24-08-09","Chair Scale, Electronic"]
[10,"RT24-08-10","Scale, Pharmacy"]
[11,"RT24-08-11","Mid Upper Arm Circumference (MUAC) Tape, Child (Pack of 100("]
[12,"RT24-08-12","Weight Estimation Tape"]
[13,"RT24-08-13","Weight Estimation Tape, Single-/use (Pack of 10)"]
[14,"RT24-08-14","Stadiometer (Height Board)"]
[15,"RT24-08-15","Infantometer (Length Board)"]
[]
["9.  PATIENT TRANSFER"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-09-01","Transfer Board, 80 cm "]
[2,"RT24-09-02","Transfer Board, 180 cm"]
[3,"RT24-09-03","Transfer Sheet/System, 180 cm x 70 cm"]
[]
["10.  KICK-ABOUT AND DRIP STANDS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-10-01 ","Drip stand, mobile, Type B, Mild steel, 2 IV hooks"]
[7,"RT24-10-02","Dripstand, mobile, Type C, Mild steel, 2 IV hooks"]
[9,"RT24-10-03","Drip stand, mobile, Type B, Mild steel, 4 IV hooks"]
[10,"RT24-10-04","Dripstand, mobile, Type C, Mild steel, 4 IV hooks"]
[8,"RT24-10-05","Dripstand, mobile, Type B, Stainless steel, 2 IV hooks"]
[2,"RT24-10-06","Dripstand, mobile, Type C, Stainless steel, 2 IV hooks"]
[3,"RT24-10-07","Kick-about, for bucket","Appendix G"]
[4,"RT24-10-08","Bucket for kick-about"]
[5,"RT24-10-09","Kick-about, for basin","Appendix G"]
[6,"RT24-10-10","Kick about basin"]
[1,"RT24-10-11","Mobile Medical Screen"]
[]
["11.  STOOLS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-11-01","Anaesthetist stool, with backrest"]
[2,"RT24-11-02","Foot stool, Double, Aluminium top"]
[3,"RT24-11-03","Foot stool, Double, Rubber top"]
[4,"RT24-11-04","Foot stool, Single, Aluminium top"]
[5,"RT24-11-05","Foot stool, Double, Rubber top"]
[6,"RT24-11-06","Visitor chair, hospital, Sleigh base"]
[7,"RT24-11-07","Bathroom stool, hospital"]
[null,"RT24-11-08","Visitor chair, 3-seater, Stainless steel"]
[null,"RT24-11-09","Visitor chair, 4-seater, Stainless steel"]
[7,"RT24-11-10","Visitor chair, 5-seater, Stainless steel"]
[null,"RT24-11-11","MRI chair"]
[null,"RT24-11-12","Transport Chair"]
[null,"RT24-11-13"]
[]
["12. TROLLEYS"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-12-01","Trolley, emergency, crash cart, "]
[2,"RT24-12-02","Trolley, gas cylinder, 180mm"]
[3,"RT24-12-03","Trolley, Gas cylinder, 300mm"]
[4,"RT24-12-04","Trolley, gas cylinder, upright type"]
[5,"RT24-12-05","Trolley, anaesthetist. Type 3, size C. "]
[6,"RT24-12-06"," Trolley, Anaesthetist, ABS"]
[7,"RT24-12-07","Trolley, anaesthetist. Type 5, size B. "]
[8,"RT24-12-08","Trolley, medical dressing. Type 4, size A. "]
[9,"RT24-12-09","Trolley, medical dressing. Type 4, size C. "]
[10,"RT24-12-10","Trolley, medical dressing with bucket and bowl attachment. Type 6. "]
[11,"RT24-12-11","Trolley, medical instrument, Type 2, size A"]
[12,"RT24-12-12","Trolley, medical instrument, Type 2, Size B, No guard rails"]
[13,"RT24-12-13","Trolley, medical instrument, Type 2, Size B"]
[14,"RT24-12-14","Trolley, medical instrument, Type 2, size C,  No guard rail "]
[15,"RT24-12-15","Trolley, Utility"]
[18,"RT24-12-16","Trolley, Soiled Intrument & Linen \n","ME00.30.03 - Annexure L"]
[19,"RT24-12-17","Polyester Linen Receptacle, for Linen trolley"]
[20,"RT24-12-18","Carrier, soiled linen"]
[21,"RT24-12-19","Receptacle, polyester linen, for carrier"]
[22,"RT24-12-20","Carrier, soiled linen, plastic box"]
[23,"RT24-12-21","Carrier, for bin, "]
[24,"RT24-12-22","Bin, for soaking purposes"]
[25,"RT24-12-23","Bin, for soaking purposes, without drainage tap"]
[]
["13.  Mounted Items"]
["Item No.","Item Code","Description","Attached Reference"]
[1,"RT24-13-01","MRI Metal Detector"]
[2,"RT24-13-02","Burns Treatment Bath, Height-adjustable"]
[3,"RT24-13-03","Burns Treatment Bath, Stationary"]

{"sheet":"Category 1","index":1,"n_rows":188,"n_cols":4,"rows_kept":188,"merged":[[0,0,0,3],[2,0,2,3],[3,0,3,3],[87,0,87,3],[88,0,88,3],[124,0,124,3],[125,0,125,3]]}
["CATEGORY 1"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["MEDICAL BOWLS"]
["RT24-01-01","Medical Bowl, type A","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Bowl shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.3, type A, size 4"]
[1.3,"Rim to conform to fig.1(a) or fig.1(d) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Internal depth 45 - 50 mm"]
["1.5.2","Internal diameter at top 65 mm"]
["1.5.3","Internal diameter at the bottom of 26 mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-01-02","Medical Bowl, type B, 100mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Bowl shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.4, type B, size 2"]
[1.3,"Rim to conform to fig.1(a) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Internal depth 60 -65 mm"]
["1.5.2","Internal diameter at top 100 mm"]
["1.5.3","The sides must be straight and parallel"]
[1.6,"The base must be flat"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-01-03","Medical Bowl, type B, 150mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Bowl shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.4, type B, size 3"]
[1.3,"Rim to conform to fig.1(a) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Internal depth 70 -75 mm"]
["1.5.2","Internal diameter at top 150 mm"]
["1.5.3","The sides must be straight and parallel"]
[1.6,"The base must be flat"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-01-04","Medical Bowl, type B, 200mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Bowl shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.4, type B, size 4"]
[1.3,"Rim to conform to fig.1(a) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Internal depth 90 - 95mm"]
["1.5.2","Internal diameter at top 200 mm"]
["1.5.3","The sides must be straight and parallel"]
[1.6,"The base must be flat"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-01-05","Bowl Stand, type A","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest of CKS 157, type A Single"]
[1.2,"Stainless steel, to comply with SANS 417, subsection 4.1.2"]
[1.3,"Each leg of the stand must be fitted with a 75mm castor complying with the requirements of SANS 621"]
[1.4,"The method of joininig castors with stand legs must be good quality welded"]
[1.5,"Dimensions:"]
["1.5.1","The design and the dimensions must conform to CKS 157 to those shown in figure 1 for stainless steel with tolerance of + 10mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","SANS 621"]
["2.1.1","Please provide SANS 621 test Lab name and report number:"]
["2.3","CKS 157"]
["2.4","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.4.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["KIDNEY DISHES"]
["RT24-01-06","Kidney dish, 150mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Dish shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.2, type A, size 1"]
[1.3,"Rim to conform to fig.1(d) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Overall length: 150 mm (±3 mm)"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-01-07","Kidney dish, 195mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Dish shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.2, type A, size 2"]
[1.3,"Rim to conform to fig.1(d) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Overall length: 195 mm (±3 mm)"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-01-08","Kidney dish, 260mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Dish shall be made from stainless steel"]
[1.2,"To comply to the latest issue of SANS 417, subsection 4 and 5.2, type A, size 3"]
[1.3,"Rim to conform to fig.1(d) of SANS 417"]
[1.4,"Chemical composition of stainless steel shall comply with the requirements given in table 1 of SANS 417, SABS test report to be submitted and only Grade A will be acceptable"]
[1.5,"Dimensions:"]
["1.5.1","Overall length: 260 mm (±3 mm)"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
[]
["MEASURING JUGS"]
["RT24-01-09","Measuring Jug, Plastic, 500ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Material must be of autoclavable durable plastic"]
[1.2,"Graduation markings shall be on the outside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 500ml"]
[1.5,"The unit must be autoclable at 134oC - 250oC temperature"]
[1.6,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[1.7,"The markings must be etched or indillible for the life of the unit"]
[]
["RT24-01-10","Measuring Jug, Plastic, 1000ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Material must be of autoclavable durable plastic"]
[1.2,"Graduation markings shall be on the inside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 1000ml"]
[1.5,"The unit must be autoclable at 134oC - 250oC temperature"]
[1.6,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[1.7,"The markings must be etched or indillible for the life of the unit"]
[]
["RT24-01-11","Measuring Jug, Plastic, 2000ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Material must be of autoclavable durable plastic"]
[1.2,"Graduation markings shall be on the inside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 2000ml"]
[1.5,"The unit must be autoclable at 134oC - 250oC temperature"]
[1.6,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[1.7,"The markings must be etched or indillible for the life of the unit"]
[]
["RT24-01-12","Measuring Jug, Stainless steel, 500ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4 and 5.17"]
[1.2,"Graduation markings shall be on the inside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 500ml"]
[1.5,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-01-13","Measuring Jug, Stainless steel, 1000ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4 and 5.17"]
[1.2,"Graduation markings shall be on the inside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 1000ml"]
[1.5,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-01-14","Measuring Jug, Stainless steel, 2000ml","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4 and 5.17"]
[1.2,"Graduation markings shall be on the inside surface and shall be in millilitres"]
[1.3,"The markings shall be in 50 mL steps and every 100 mL shall be denominated"]
[1.4,"Jug capacity: 2000ml"]
[1.5,"Dimensions and graduation markings must be equivalent to the latest issue of SANS 417, subsection 5.17"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]

{"sheet":"Category 2","index":2,"n_rows":1601,"n_cols":4,"rows_kept":1601,"merged":[[0,0,0,3],[2,0,2,3],[5,1,5,3],[6,1,6,3],[7,1,7,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[77,1,77,3],[78,1,78,3],[79,1,79,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[165,1,165,3],[166,1,166,3],[167,1,167,3],[241,1,241,3],[242,1,242,3],[243,1,243,3],[292,1,292,3],[293,1,293,3],[294,1,294,3],[343,1,343,3],[344,1,344,3],[345,1,345,3],[434,1,434,3],[435,1,435,3],[436,1,436,3],[525,1,525,3],[526,1,526,3],[527,1,527,3],[589,1,589,3],[590,1,590,3],[591,1,591,3],[616,1,616,3],[617,1,617,3],[618,1,618,3],[647,1,647,3],[648,1,648,3],[649,1,649,3],[701,1,701,3],[702,1,702,3],[703,1,703,3],[760,1,760,3],[761,1,761,3],[762,1,762,3],[823,1,823,3],[824,1,824,3],[825,1,825,3],[895,1,895,3],[896,1,896,3],[897,1,897,3],[969,1,969,3],[970,1,970,3],[971,1,971,3],[1050,1,1050,3],[1051,1,1051,3],[1052,1,1052,3],[1170,1,1170,3],[1171,1,1171,3],[1172,1,1172,3],[1296,1,1296,3],[1297,1,1297,3],[1298,1,1298,3],[1370,1,1370,3],[1371,1,1371,3],[1372,1,1372,3],[1420,1,1420,3],[1421,1,1421,3],[1422,1,1422,3],[1460,1,1460,3],[1461,1,1461,3],[1462,1,1462,3],[1500,0,1500,3],[1502,1,1502,3],[1503,1,1503,3],[1504,1,1504,3],[1551,1,1551,3],[1552,1,1552,3],[1553,1,1553,3]]}
["CATEGORY 2"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-02-01","Bassinet, type A, with stand","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1," To comply with the latest issue of CKS 237, type A"]
[1.2,"The unit must be moulded from a durable translucent plastic material"]
[1.3,"The flange at each end shall be moulded in a way to ensure handgrip and facilitate handling"]
[1.4,"The designs and dimensions shall conform to those given in the latest issue of CKS 237, type A, figure 1"]
[1.5,"Tolerance for dimensions shall be +5mm"]
[1.6,"The unit must be supplied complete with stand and mattress"]
[1.7,"Stand:"]
["1.7.1","The frame of the stand shall be of Mild steel with epoxy/nylon powder-coated finish to comply with the SANS 778 requirements"]
["1.7.2","The frame shall have four equally spaced U-shaped supports to hold the bassinet"]
["1.7.3","The supports shall be of mild steel and welded to the undersides of the side rails"]
["1.7.4","The stand must have a mild steel tray welded to the legs"]
["1.7.5","The stand shall be mounted on four castros with diameter of 75mm"]
["1.7.6","The castors must comply with the requirements of SANS 621"]
["1.7.7","The stand must have incorporated cylinder holder"]
[1.8,"Mattress with cover:"]
["1.8.1","To comply with the latest issue of SANS 883 and 1291-1"]
["1.8.2","To be constructed of flexible polyurethane foam complying with SANS 883"]
["1.8.3","Thickness: 50 mm  (+ 5mm)"]
["1.8.4","Cover must be water-resistant, air permeable material and sealed"]
[2,"Standard Accessories: (This items comes standard with the unit and must priced individually as well)"]
["2.1","Stand"]
["2.2","Scoop"]
["2.3","Mattress"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 778 (subsection 5.2)"]
[3.2,"SANS 621"]
[3.3,"SANS 883"]
[3.4,"CKS 237"]
[null,"Type A Bassinet Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-01a","Bassinet/Scoop"]
["RT24-02-01b","Mattress"]
["RT24-02-01c","Bassinet stand"]
["RT24-02-02","Bassinet, Height-adjustable","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
["1.1","The unit must be of modern type offered in assorted colours"]
["1.2","All four sides of the matress platform must be fitted with transparent guards/panels."]
["1.3","The unit must be offered with collapsable side panels for smooth baby transfer to the mother's bed"]
["1.4","The unit must have height adjustable stand through hydraulic control to match mother's matress platform (Manual dial control will not be accepted)"]
["1.5","The dimensions of the platform shall be 720 x 450 mm"]
["1.6","Tolerance for dimensions shall be +20mm"]
["1.7","The frame of the stand shall be of Mild steel with epoxy/nylon powder-coated finish to comply with the SANS 778 requirements"]
["1.8","The frame shall be intergrated with the bassinet"]
["1.9","The supports shall be of mild steel and welded to the undersides of the side rails"]
["1.10","The unit must consist of at least 1 drawer/shelf for storage"]
["1.11","The unit must be easily moveable with lockable castors of 75mm in diameter."]
["1.12","The castors must comply with the requirements of SANS 621"]
["1.13","The stand must have incorporated cylinder holder"]
[1.8,"Mattress:"]
["1.8.1","Comply with the latest issue of SANS 883 and 1291-1"]
["1.8.2","To be constructed of flexible polyurethane foam complying with class 30, grade no. 12 of SANS 640"]
["1.8.3","Thickness: 50 mm  (+ 5mm)"]
["1.8.4","Cover must be water-resistant, air permeable material"]
[2,"Standard Accessories: (This items comes standard with the unit and must priced individually as well)"]
[2.1,"Stand"]
[2.2,"Mattress"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 778 (subsection 5.2)"]
[3.2,"SANS 621"]
[3.3,"SANS 883"]
[null,"Bassinet Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-02a","Bassinet/Scoop"]
["RT24-02-02b","Mattress"]
["RT24-02-03","Cot, Infant","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
["1","Technical Specification"]
["1.1","To comply with the latest issue SANS 521, subsection 5.5, fig. 6 "]
["1.2","Where the item offered differs from the specification in SANS 521, except for the items specified below, the supplier must indicate the deviation and supply relevant details"]
["1.3","Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
["1.4","Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: two-colour coded, end-user choice"]
["1.5","Dimension:"]
["1.5.5","Length: 980 mm (± 5 mm)"]
["1.5.2","Width: 560 mm (± 5 mm)"]
["1.6","Mattress support: mattress support other than weldmesh is required, provide details"]
["1.7","The unit must have hydraulic controlled rising backrest support, Trendelenberg and anti-Trendelenberg positions"]
["1.8","Mattress"]
["1.8.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["1.8.2","Must be flexible high-density foam with fully enclosing 2-way stretch sealed cover"]
["1.8.3","Density: 25 Kg/m3, Please state the density of the on offer"]
["1.8.4","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["1.8.5","Mattress must support a patient of at least 15 kg and return to original shape when not in use"]
["1.8.6","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["1.8.7","Overall dimensions:"]
["1.8.7.1","Length: 940 mm (+ 30 mm)"]
["1.8.7.2","Width: 540 mm (+ 20 mm)"]
["1.8.7.3","Thickness: 100 mm (+ 5 mm)"]
["1.8.8","Must be fully sealed 2-way stretch sealed cover;"]
["1.8.8.1","Vapour permeable"]
["1.8.8.2","Water resistant"]
["1.8.8.3","Interstitial anti-microbial agent"]
["1.8.8.4","Radiolucent"]
[2,"Warranty"]
["2.1","Mattress warranty of atleast 4 years"]
["2.2","Cover warranty of atleast 2 years"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","SANS 778 (subsection 5.2)"]
["3.2","SANS 521"]
["3.3","SANS 883"]
["3.4","IEC 60601-2-52"]
[null,"Infant Cot Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-03a","Infant Cot Mattress"]
["RT24-02-03b","Side panel"]
["RT24-02-03c","Castors"]
["RT24-02-04","Cot, Infant, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
["1","Technical Specification"]
["1.1","The unit must be of modern type offered in assorted colours"]
["1.2","The unit must have side panels that are collapsable, provide security and see-through visuals from at least 10m distance"]
["1.3","Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
["1.4","Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours"]
["1.5","The unit must have a panel to control height, backrest support, Trendelenberg and anti-Trendelenberg positions"]
["1.5.1","Height: 300 - 900mm"]
["1.5.2","Trendelenberg 0-12o"]
["1.5.3","Anti-trendelenberg 0- 12o"]
["1.6","Dimension:"]
["1.6.1","Length: 980 mm (+ 30 mm)"]
["1.6.2","Width: 560 mm (+ 20 mm)"]
["1.7","The following accessories must meet the above specification, be compatible and supplied with the main unit"]
["1.8","Mattress"]
["1.8.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["1.8.2","Must be flexible high-density foam with fully enclosing 2-way stretch cover"]
["1.8.3","Density: 25 Kg/m3, Please state the density of the on offer"]
["1.8.4","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["1.8.5","Mattress must support a patient of at least 15 kg and return to original shape when not in use"]
["1.8.6","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["1.8.7","Overall dimensions:"]
["1.8.7.1","Length: 940 mm (+ 30 mm)"]
["1.8.7.2","Width: 540 mm (+ 20 mm)"]
["1.8.7.3","Thickness: 100 mm (+ 5 mm)"]
["1.8.8","Must be fully sealed 2-way stretch cover;"]
["1.8.8.1","Vapour permeable"]
["1.8.8.2","Water resistant"]
["1.8.8.3","Interstitial anti-microbial agent"]
["1.8.8.4","Radiolucent"]
[2,"Warranty"]
["2.1","Mattress warranty of atleast 4 years"]
["2.2","Cover warranty of atleast 2 years"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","SANS 778 (subsection 5.2)"]
["3.2","SANS 521"]
["3.3","SANS 883"]
["3.4","IEC 60601-2-52"]
[null,"Infant Cot Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-04a","Infant Cot Mattress"]
["RT24-02-04b","Side panel"]
["RT24-02-05","Bed, Adolecent, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrical adjustment of height adjustment, backrest, reverse trendelenburg and trendelenburg must be possible"]
[1.3,"The height of the mattress support shall be adjustable in the range 380 – 800 mm (measured from the floor to the top of the mattress support), with tolerance of +40 mm"]
[1.4,"Backrest angle: 65o (+5o)"]
[1.5,"Trendelenburg angle: 15o (+3o)"]
[1.6,"Reverse trendelenburg angle: 15o (+3o)"]
[1.7,"The bed must be equiped with backrest angle indicator"]
[1.8,"The bed shall be clearly marked with the corresponding Maximum Patient Weight and Safe Working Load in kg."]
[1.9,"It must have a Maximum Patient Weight of at least 120kg"]
[{"v":1.1,"d":"1.10"},"Safe Working Load shall not be less than 180kg"]
[1.11,"The bed must have controls for all position"]
[1.12,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.13,"Collapsible safety sides must comply with IEC 60601-2-52 Annexure CC to prevent patient from falling off the bed"]
[1.14,"The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
[1.15,"The bed must be fitted with Oxygen cylinder holder"]
[1.16,"To be fitted with castors with a central castor locking system"]
[1.17,"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.18,"Removable head and foot ends (ABS material may be offered)"]
[1.19,"Mattress support: mattress support other than weldmesh is required, provide details"]
["1.6","Dimension:"]
["1.6.1","Length: 1700 mm (+ 20 mm)"]
["1.6.2","Width: 560 mm"]
[{"v":1.2,"d":"1.20"},"Extension of bed of at least 20cm must be possible and the additional mattress for the extension must be provided with the unit"]
[1.21,"The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price."]
["1.21.1","Driprod"]
["1.21.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.21.3","Traction pole with pulleys and weights"]
[1.22,"The bed dimensions must be compatible with the mattress dimensions"]
[1.23,"The bed must be equiped with CPR mechanism"]
[1.24,"The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Mattress"]
["1.24.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["1.24.3","Density: 32 - 38 Kg/m3, Please state the density of the on offer"]
["1.24.4","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["1.24.5","Mattress must support a patient of at least 150 kg and return to original shape when not in use"]
["1.24.6","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["1.24.7","Overall dimensions:"]
["1.24.7.1","Length: 1 700 mm  (+40mm)"]
["1.24.7.2","Width: 550 mm "]
["1.24.7.3","Thickness: 120 mm (+5mm)"]
["1.24.2","Must be flexible high-density foam with fully sealed 2-way stretch cover;"]
["1.25.2.1","Vapour permeable"]
["1.25.2.2","Water resistant"]
["1.25.2.3","Interstitial anti-microbial agent"]
["1.25.2.4","radiolucent"]
["1.25.1","To comply with the latest issue of SANS 1291-1, proof of compliance must be submitted"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) for the main unit should be as per the SCC document "]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
["3.2","Mattress warranty of atleast 4 years"]
["3.2","Cover warranty of atleast 2 years"]
[3.4,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.4.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[4.3,"SANS 778 (Subsection 5.2)"]
[4.4,"SANS 621"]
[null,"SANS 883"]
[null,"SANS 1291-1"]
[4.5,"IEC 60601-2-52"]
[4.6,"IEC 60601-1-2 "]
[null,"Adolecent Bed Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-05a","Adolecent Bed Mattress"]
["RT24-02-05b","Side panel"]
["RT24-02-05c","Driprod"]
["RT24-02-05d","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-05e","Traction pole with pulleys and weights"]
["RT24-02-06","Gynae Examination Chair, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[{"v":1,"d":"1.00"},"The chair must be designed specifically for the gynaecology examination according to the most advanced production criteria in the field of medical equipments aiming at the maximum functional use and comfort for both operator and patient."]
[1.1,"The frame shall of mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.2,"Solid construction in Mild steel with epoxy powder coated refined with elegant covers moulded in ABS at high resistance"]
[1.3,"Bed must support a patient mass up to a maximum of 250 kg"]
[1.4,"The upholstered parts of the chair must be  composed of high-density and undeformable foam pelted with bi-elastic, tear resistant, antimicrobial tissue, very easy to clean and disinfect."]
[1.5,"Trendelenburg inclination: 0 - 20°"]
[1.6,"Reverse trendelenburg position: 0 - 10°"]
[1.7,"It must be able to achieve backrest angle of 60°"]
[1.8,"Backrest, height and trendelenburg positions must be possible with electric motor using hand control"]
[1.9,"The height adjustment shall be by hand control and operated by means mains power "]
[{"v":1.1,"d":"1.10"},"Height adjustment shall be from atleast 700mm to 1100mm"]
[1.11,"Couple of arm rests in metal (removable) designed to grant a safe grip to patient (to be used as handles)"]
[1.12,"4 Stainless steel rails set on both sides of seat and back rest"]
[1.13,"Single-section leg rest electrically operated granting the chair to reach the bed position "]
[1.14,"Lumbar cushion for a comfortable back position of the patient when lying down"]
[1.15,"Couple of upholstered anatomical leg rests provided with stainless steel supports and manual adjustment in height and longitudinal direction"]
[1.16,"The chair should have following features:"]
["1.16.1","Footrest with arch-designed supports in stainless steel and with refined foot plates in supple foam and pelted with same sky as the rest of chair’s upholstery  – clamp fitting system in to the seat with manual adjustment in height and longitudinal direction "]
["1.16.2","Footrest must be detacheable"]
["1.16.3","Practical central cushion for filling the empy space between seat and single-leg rest to grant easy bed position"]
["1.16.4","Paper-roll holder fixed at the back rest of the chair"]
["1.16.5","Secretion basin in stainless steel provided with drainage system for waste liquids through a coiled tube "]
["1.16.6","Detachable head cushion"]
["1.16.7","Lithotomy poles that are attached to the framework underneath the seat section."]
["1.16.8","It must be possible to position the chair in a flat examination couch setup"]
["1.16.9","Compatable matching operator's chair"]
[2,"WARRANTY & MAINTENANCE "]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[2.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["2.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[3.3,"SANS 778 (Subsection 5.2)"]
[3.4,"IEC 60601-1-2 "]
[null,"Electric Gynae Chair Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-06a","Attacheable footrest"]
["RT24-02-06b","central cushion for filling the empy space between seat and single-leg rest"]
["RT24-02-06c","Paper-roll holder attacheable at the back rest of the chair"]
["RT24-02-06d","Secretion basin in stainless steel with drainage system"]
["RT24-02-06e","Lithotomy poles (pair)"]
["RT24-02-06f","Compatable matching operator's chair"]
["RT24-02-07","Gynae Examination Chair, Hydraulic","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[{"v":1,"d":"1.00"},"The chair must be designed specifically for the gynaecology examination according to the most advanced production criteria in the field of medical equipments aiming at the maximum functional use and comfort for both operator and patient."]
[1.1,"The frame shall of mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.2,"Solid construction in Mild steel with epoxy powder coated refined with elegant covers moulded in ABS at high resistance"]
[1.3,"Bed must support a patient mass up to a maximum of 250 kg"]
[1.4,"The upholstered parts of the chair must be  composed of high-density and undeformable foam pelted with bi-elastic, tear resistant, antimicrobial tissue, very easy to clean and disinfect."]
[1.5,"Trendelenburg inclination: 0 - 20°"]
[1.6,"Reverse trendelenburg position: 0 - 10°"]
[1.7,"It must be able to achieve backrest angle of 60°"]
[1.8,"Backrest, seat, height and trendelenburg positions must be possible using foot switch"]
[1.9,"All positions must be clearly marked and visible on the foot switch"]
[{"v":1.1,"d":"1.10"},"Height adjustment shall be from atleast 700mm to 1100mm"]
[1.11,"Couple of arm rests in metal (removable) designed to grant a safe grip to patient (to be used as handles)"]
[1.12,"4 Stainless steel rails set on both sides of seat and back rest"]
[1.13,"It must be possible to bring the chair to the bed position using a single push on the foot switch"]
[1.14,"Lumbar cushion for a comfortable back position of the patient when lying down"]
[1.15,"Couple of upholstered anatomical leg rests provided with stainless steel supports and manual adjustment in height and longitudinal direction"]
[1.16,"The chair should have following features:"]
["1.16.1","Footrest with arch-designed supports in stainless steel and with refined foot plates in supple foam and pelted with same sky as the rest of chair’s upholstery  – clamp fitting system in to the seat with manual adjustment in height and longitudinal direction "]
["1.16.2","Footrest must be detacheable"]
["1.16.3","Practical central cushion for filling the empy space between seat and single-leg rest to grant easy bed position"]
["1.16.4","Paper-roll holder fixed at the back rest of the chair"]
["1.16.5","Secretion basin in stainless steel provided with drainage system for waste liquids through a coiled tube "]
["1.16.6","Detachable head cushion"]
["1.16.7","Lithotomy poles that are attached to the framework underneath the seat section."]
["1.16.8","It must be possible to position the chair in a flat examination couch setup"]
["1.16.9","Compatable matching operator's chair"]
[2,"WARRANTY & MAINTENANCE "]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[2.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["2.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[3.3,"SANS 778 (Subsection 5.2)"]
[3.4,"IEC 60601-1-2 "]
[null,"Hydraulic Gynae Chair Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-07a","Attacheable footrest"]
["RT24-02-07b","central cushion for filling the empy space between seat and single-leg rest"]
["RT24-02-07c","Paper-roll holder attacheable at the back rest of the chair"]
["RT24-02-07d","Secretion basin in stainless steel with drainage system"]
["RT24-02-07e","Lithotomy poles pair"]
["RT24-02-07f","Compatable matching operator's chair"]
["RT24-02-08","Delivery Bed, Electric ","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"It must be possible to adjust trendelenburg, reverse trendelenburg, backrest and height of the bed"]
[1.2,"Safe workload up to at least 280kg"]
[1.3,"Structural metal parts shall be protected by a durable epoxy/nylon powder-coated finish to comply with SANS 778 which is resistant to chips and scratches"]
[1.4,"Electrically operated height adjustment, backrest, trendelenburg and reverse trendelenburg"]
[1.5,"The bed shall be able to deliver a highly versatile support surface which can be used for labour, delivery and recovery"]
[1.6,"The unit shall allow optimum access to the mother and baby through all stages of the birthing process"]
[1.7,"It shall be possible to convert quickly from a standard bed to a versatile delivery platform, and vice-versa."]
[1.8,"Manual  and electrical emergency CPR must be available"]
[1.9,"All controls shall be easily accessible. No controls shall be behind the headboard"]
[{"v":1.1,"d":"1.10"},"Compact size to fit into small delivery rooms"]
[1.11,"Retractable platform, optimizing access to perineal area, mother and baby during delivery procedures "]
[1.12,"Positions: The bed shall offer a choice of safe and comfortable positions that can be adopted during labour and delivery, minimum positions offered shall include:"]
["1.12.1","   Lithotomy position with leg rest and fluid collection bowl"]
["1.12.2","   Semi-chair with high foot support"]
["1.12.3","   Chair with high foot support and hand grips"]
["1.12.4","   Semi- chair with low foot support"]
["1.12.5","   Supported kneeling"]
["1.12.6","   Chair with handgrips and step"]
[1.13,"Removable 2-part mattress, with perineal cut-out seat section "]
[1.14,"Adjustable safety sides"]
[1.15,"Central brake on all four castors"]
[1.16,"Easy steer castor system for optimum mobility/stability "]
[1.17,"Removable, moulded head and foot panels "]
[1.18,"Easy to clean"]
[1.19,"Industrial antistatic, non marking, non staining , ± 125mm castors, with a sealed casing"]
[{"v":1.2,"d":"1.20"},"Built-in sockets for IV rod and Patient lifting pole, drop in accessories, no clamps shall be used."]
[1.21,"Revolving rubber buffer wheels fitted to the four corners of the bed"]
[1.22,"Removable fire retardant  head and foot ends"]
[1.23,"Counterbalanced base "]
[1.24,"Storage of accessories: convenient storage for accessories shall be available  and included in this offer"]
[1.25,"Complete with a comprehensive range of accessories storable away from the bed, the flexibility and ease-of-use offered"]
[1.26,"Sheet steel mattress platform for improved infection control. No protruding parts that can damage mattress or cover"]
[1.27,"Fire retardant,  ABS cover to the undercarriage"]
[1.28,"Battery back-up in the event of mains power failure "]
[1.29,"Dimensions:"]
["1.29.1","   Length:  ±2200mm , Width:     ± 900mm"]
["1.29.2","   Backrest Angle: 70o  +5o"]
["1.29.3","   Height adjustable: 260 – 600mm  +40mm"]
["1.29.4","   Trendelenburg angle: 15o  +2o"]
["1.29.5","   Reverse trendelenburg angle: 17o  +2o"]
[2,"Easy to fit accessories to be supplied as standard:"]
[2.1,"   Fixed, heavy duty safety sides"]
[2.2,"   Bed control unit / remote handset"]
[2.3,"   Electric motors 230V"]
[2.4,"   Accessories storage trolley / system"]
[2.5,"   Adjustable leg rests"]
[2.6,"   IV Rod –height adjustable"]
[2.7,"   Hand grips"]
[2.8,"   High foot supports"]
[2.9,"   Low foot supports"]
[{"v":2.1,"d":"2.10"},"   Removable step"]
[1.2,"Including mattress which adheres to the following specs: Description: "]
["1.2.1","  2 section / parts which merge into one unit when the retractable platform is joined with the upper section of the bed"]
["1.2.2","  It shall be able to retract the lower part of the mattress with the retractable platform to optimize  access to perineal area, mother and baby during delivery procedures "]
["1.2.3","  Flexible high density foam mattress with fully sealed 2 way stretch cover to comply with SANS 883"]
[1.3,"Mattress core data:"]
["1.3.1","  Mattress depth ±170mm profile cut and zoned melamine free  "]
["1.3.2","  Density:38 – 42 Kg/m3 "]
["1.3.3","  Hardness: 115 – 150 N"]
[1.4,"Cover data:"]
["1.4.1"," Fully enclosing 2 way stretch, Vapour permeable, Water resistant cover, with an Interstitial Anti-microbial agent and sealed, to prevent nosocomial and cross infections"]
["1.4.2"," Fire retardant "]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) for the main unit should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"Mattress warranty: At least 4 years"]
[3.3,"Cover warranty: At least 2 years"]
[3.4,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.4.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 883"]
["4.4","IEC 60601-1-2 "]
[null,"Electric Delivery Bed Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-08a","Mattress (complete 2-part)"]
["RT24-02-08b","Accessories storage trolley / system"]
["RT24-02-08c","Adjustable leg rests"]
["RT24-02-08d","IV Rod –height adjustable"]
["RT24-02-08e","Hand grips"]
["RT24-02-08f","High foot supports"]
["RT24-02-08g","Low foot supports"]
["RT24-02-08h","Removable step"]
["RT24-02-09","Delivery Bed, Hydraulic","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"It must be manually operated"]
[1.2,"Safe workload up to at least 280kg"]
[1.3,"Structural metal parts shall be protected by a durable epoxy/nylon powder-coated finish to comply with SANS 778 which is resistant to chips and scratches"]
[1.4,"Height adjustment by hydraulic foot switch from approximately 360 - 760mm"]
[1.5,"The bed shall be able to deliver a highly versatile support surface which can be used for labour, delivery and recovery (All phases of child birth)"]
[1.6,"The unit shall allow optimum access to the mother and baby through all stages of the birthing process"]
[1.7,"It shall be possible to convert quickly from a standard bed to a versatile delivery platform, and vice-versa."]
[1.8,"Dual side manual CPR levers"]
[1.9,"All controls shall be easily accessible. No controls shall be behind the headboard"]
[{"v":1.1,"d":"1.10"},"Compact size to fit into small delivery rooms"]
[1.11,"Retractable platform, optimizing access to perineal area, mother and baby during delivery procedures "]
[1.12,"Positions: The bed shall offer a choice of safe and comfortable positions that can be adopted during labour and delivery, minimum positions offered shall include:"]
["1.12.1","Lithotomy position with leg rest and fluid collection bowl"]
["1.12.2","Semi-chair with high foot support"]
["1.12.3","Chair with high foot support and hand grips"]
["1.12.4","Semi- chair with low foot support"]
["1.12.5","Supported kneeling"]
["1.12.6","Chair with handgrips and step"]
[1.13,"Removable 2-part mattress, with perineal cut-out seat section "]
[1.14,"Adjustable safety sides"]
[1.15,"Central brake on all four castors"]
[1.16,"Easy steer castor system for optimum mobility/stability "]
[1.17,"Removable, moulded head and foot panels "]
[1.18,"Easy to clean"]
[1.19,"Industrial antistatic, non marking, non staining , ± 125mm castors, with a sealed casing"]
[{"v":1.2,"d":"1.20"},"Built-in sockets for IV rod and Patient lifting pole, drop in accessories, no clamps shall be used."]
[1.21,"Revolving rubber buffer wheels fitted to the four corners of the bed"]
[1.22,"Removable fire retardant  head and foot ends"]
[1.23,"Counterbalanced base "]
[1.24,"Storage of accessories: convenient storage for accessories shall be available  and included in this offer"]
[1.25,"Complete with a comprehensive range of accessories storable away from the bed, the flexibility and ease-of-use offered"]
[1.26,"Sheet steel mattress platform for improved infection control. No protruding parts that can damage mattress or cover"]
[1.27,"Fire retardant,  ABS cover to the undercarriage"]
[1.28,"Battery back-up in the event of mains power failure "]
[1.29,"Dimensions:"]
["1.29.1","   Length:  ±2200mm , Width:     ± 900mm"]
["1.29.2","   Backrest Angle: 70o  +5o"]
["1.29.3","   Height adjustable: 260 – 600mm  +40mm"]
["1.29.4","   Trendelenburg angle: 15o  +2o"]
["1.29.5","   Reverse trendelenburg angle: 17o  +2o"]
[2,"Easy to fit accessories to be supplied as standard:"]
[2.1,"   Fixed, heavy duty safety sides"]
[2.2,"   Bed control unit / remote handset"]
[2.3,"   Electric motors 230V"]
[2.4,"   Accessories storage trolley / system"]
[2.5,"   Adjustable leg rests"]
[2.6,"   IV Rod –height adjustable"]
[2.7,"   Hand grips"]
[2.8,"   High foot supports"]
[2.9,"   Low foot supports"]
[{"v":2.1,"d":"2.10"},"   Removable step"]
[1.2,"Including mattress which adheres to the following specs: Description: "]
["1.2.1","  2 section / parts which merge into one unit when the retractable platform is joined with the upper section of the bed"]
["1.2.2","  It shall be able to retract the lower part of the mattress with the retractable platform to optimize  access to perineal area, mother and baby during delivery procedures "]
["1.2.3","  Flexible high density foam mattress with fully sealed 2 way stretch cover to comply with SANS 883"]
[1.3,"Mattress core data:"]
["1.3.1","  Mattress depth ±170mm profile cut and zoned melamine free  "]
["1.3.2","  Density:38 – 42 Kg/m3 "]
["1.3.3","  Hardness: 115 – 150 N"]
[1.4,"Cover data:"]
["1.4.1"," Fully enclosing 2 way stretch, Vapour permeable, Water resistant cover, with an Interstitial Anti-microbial agent and sealed, to prevent nosocomial and cross infections"]
["1.4.2"," Fire retardant "]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"Mattress warranty: At least 4 years"]
[3.3,"Cover warranty: At least 2 years"]
[3.4,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.4.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 883"]
["4.4","IEC 60601-1-2 "]
[null,"Hydraulic Delivery Bed Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-09a","Mattress (complete 2-part)"]
["RT24-02-09b","   Accessories storage trolley / system"]
["RT24-02-09c","   Adjustable leg rests"]
["RT24-02-09d","   IV Rod –height adjustable"]
["RT24-02-09e","   Hand grips"]
["RT24-02-09f","   High foot supports"]
["RT24-02-09g","   Low foot supports"]
["RT24-02-09h","   Removable step"]
["RT24-02-10","Chemotherapy and Dialysis Chair","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"The specification establishes the requirements for, supply, delivery, end user training, demonstration, commissioning and installation of a  fully automated mobile Chemotherapy and Dialysis chair."]
[1.2,"The chair must offer :"]
["1.2.1","High stability"]
["1.2.2","Safety against overturning."]
["1.2.3","Motorised position adjustment."]
[1.3,"High quality upholstery is a must for any good treatment couch being the interface between the couch and patient it must remain clean and resistant to damage."]
[1.4,"The exchangeable upholstery must designed such that it can be easily removed with few movement for cleaning or maintenance."]
[1.5,"Blood resistant artificial leather , which is resistant to disinfectants, blood and urine"]
[1.6,"The chair must have a rechargeable battery back-up operation in case of power failure."]
[1.7,"Length: 2000mm approx"]
[1.8,"Width: 1000mm including armrest approx"]
[1.9,"Height: 520mm – 1020mm approx (20” – 40”)approx"]
[{"v":1.1,"d":"1.10"},"Chair must offer maximum patient weight of atleast 200kg"]
[1.11,"The chair must be comfortable with soft armrests, which can be swivelled, folded upwards and adjusted in the height to offer perfect comfort for the patient."]
[1.12,"Motorized/electronic adjustment of:"]
["1.12.1","Backrest of 0 - 80°"]
["1.12.2","Footrest of 0 - 40°"]
["1.12.3","Height adjustment from 55cm (min) to 75cm (Max) "]
["1.12.4","Reverse trendelenburg function of 0 - 5°"]
["1.12.5","Trendelburg function of 0 - 15°"]
[1.13,"Foam armrests tiltable on both sides of the chair to allow the patient to easily enter or leave the chair"]
[1.14,"Antibacteria surface for upholstery with special soft back and seat part"]
[1.15,"Cleanable protective cover for foot part and all armrest"]
[1.16,"Electric height, tilt, foot & back operation"]
[1.17,"Safe working load 180kgs or above"]
[1.18,"Upholstery material"]
[1.19,"The material for Upholstery material should be either UV-proof, impermeable to moisture,able to check for biocompatinilty and toxicity , flame retardant. Please state the material used on the bidded chair."]
[{"v":1.2,"d":"1.20"},"Equipotential bonding cable(to be used when using intercardiac procedures)"]
[1.21,"Hand switch with buttons for basic settings"]
[1.22,"Relax pillow in upholstery colour"]
[1.23,"Elegant underframe- and side-part covers"]
[1.24,"Bed position"]
[2,"The chair must feature the following of which accessories must be included in the bid price:"]
[2.1,"Infusion bottle holder(IV pole) with height adjustment"]
["2.2","Two packets of these paper rolls must be supplied with chair and the price be included in the bid price."]
["2.3","Push bar made up of stainless steel."]
["2.4","Lumbar support"]
["2.5","Detachable table"]
["2.6","2 hook IV pole"]
["2.7","Hand remote control"]
[3,"WARRANTY & MAINTENANCE "]
["3.1","A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
["3.2","A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","IEC 60601-1-2 "]
[null,"Chemo-Dialysis Chair Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-10a","Infusion bottle holder(IV pole) with height adjustment"]
["RT24-02-10b","Push bar made up of stainless steel."]
["RT24-02-10c","Detachable table"]
["RT24-02-10d","2 hook IV pole"]
["RT24-02-10e","Hand remote control"]
["RT24-02-11","Examination couch, with Adjustable backrest","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of CKS 243"]
[1.2,"The design of the couch shall be generally in accordance with the typical design shown in figure 1."]
[1.3,"The dimensions shall conform to those given in figure 1 and in 3.4 and 3.5 with tolerance of + 5mm"]
[1.4,"The frame shall of mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.5,"The frame shall be made from mild steel tube of nominal outside diameter at least 32 mm and nominal wall thickness at least 1,60 mm."]
[1.6,"The floor ends of the legs shall be closed with mild steel plugs (as relevant), welded in position"]
[1.7,"The bearing edges of the plugs shall be rounded, and the plugs and part of the legs shall be covered with acceptable non-marking white or black rubber ferrules"]
[1.8,"The top shall be of mild steel and have a well constructed strong outer frame and a rigid seat (base)."]
[1.9,"The top shall be divided and suitably hinged at a distance of 560 ± 25 mm from the head end to allow a total elevation of the back rest through an angle of 60° to the horizontal."]
[{"v":1.1,"d":"1.10"},"Adjustment shall be by means of a notched prop that gives at least three angular positions through to 60° or by other acceptable adjustment means"]
[1.11,"The upper surface of the top shall be padded with comfortable high density foam  of thickness at least 50 mm."]
[1.12,"The upper surface and edges of the top shall be covered with waterproof vinyl or coated fabric for easy clening"]
[1.13,"Top cover to be available in a dark colour"]
[1.14,"All surfaces shall be clean, smooth, and free from sharp corners, edges, and other defects"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["2.2.1","Please provide unique ref number of the ceriticate:"]
["2.3","SANS 778 (subsection 5.2)"]
["2.4","CKS 243"]
["RT24-02-12","Examination couch, Electric Height Adjustable ","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of CKS 243"]
[1.2,"The design of the couch shall be generally in accordance with the typical design shown in figure 1."]
[1.3,"The dimensions shall conform to those given in figure 1 and in 3.4 and 3.5 with tolerance of + 5mm"]
[1.4,"Inclusion to the CKS 243:"]
["1.4.1","The height adjustment shall be by hand control and operated by means mains power "]
["1.4.2","Height adjustment shall be from atleast 500mm to 950mm"]
[1.5,"The frame shall of mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.6,"The frame shall be made from mild steel tube of nominal outside diameter at least 32 mm and nominal wall thickness at least 1,60 mm."]
[1.7,"The floor ends of the legs shall be closed with mild steel plugs (as relevant), welded in position"]
[1.8,"The bearing edges of the plugs shall be rounded, and the plugs and part of the legs shall be covered with acceptable non-marking white or black rubber ferrules"]
[1.9,"The top shall be of mild steel and have a well constructed strong outer frame and a rigid seat (base)."]
[{"v":1.1,"d":"1.10"},"The top shall be divided and suitably hinged at a distance of 560 ± 25 mm from the head end to allow a total elevation of the back rest through an angle of 60° to the horizontal."]
[1.11,"Backrest adjustment shall be by means of a gas-spring system through to 60° "]
[1.12,"The upper surface of the top shall be padded with comfortable high density foam  of thickness at least 50 mm."]
[1.13,"Surface should be tear proof covered with non pinching Rexine, seamless joint, washable and water-proof"]
[1.14,"The upper surface and edges of the top shall be covered with waterproof vinyl or coated fabric for easy clening"]
[1.15,"Top cover to be available in a dark colour"]
[1.16,"All surfaces shall be clean, smooth, and free from sharp corners, edges, and other defects"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["2.2.1","Please provide unique ref number of the ceriticate:"]
["2.3","SANS 778 (subsection 5.2)"]
["2.4","CKS 243"]
["RT24-02-13","Transport Stretcher","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specifications"]
["1.1","The trolley must have a hydraulic height adjustment with strong and stable structure"]
["1.2","It must be easy to activate central brake-and-go pedal"]
["1.3","Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.4","Trolley must be able to transport patient weight of minimum 180 kg"]
["1.5","Must have Rising backrest, gas spring assisted with range of 0o - 60o"]
["1.6","The trolley must be equiped with roller bumpers in all four corners"]
["1.7","Safety sides must be light weight and collapsible"]
["1.8","Must have Oxygen cylinder holder"]
["1.9","Must have Drip rod included"]
["1.10","Must have Castors of 150-200 mm diameter"]
["1.11","Castors must comply with the latest issue of SANS 621"]
["1.12","Castors must be easy to maneuver in all direction, please state how that maneuvering is achieved"]
["1.13","The trolley must have padded push handles in both sides"]
["1.14","X-ray cassette system (for full body length)"]
["1.15","The unit must have protection bumpers in all corners"]
["1.16","Dimension:"]
["1.16.1","Length: 2100 mm"]
["1.16.2","Width: 750 mm"]
["1.17","Height: Adjustable from 600 to 900 mm"]
[2,"Mattress:"]
["2.1","Mattress to be a good quality high density foam of no less than 32 Kg/m3"]
["2.2","Must be constructed of high resilience polyurethane foam, to comply with SANS 883"]
["2.3","Mattress must be radio translucent, waterproof, non-slip or with retaining straps/hooks"]
["2.3.1","Dimension:"]
["2.3.2","Length: 1 950 mm"]
["2.3.3","Width: 600 mm"]
["2.3.4","Thickness: minimum 80 mm"]
["2.4","Cover to comply with the latest issue of SANS 1291-1"]
["2.5","Must be removable and complying with the following characteristcs;"]
["2.5.1","Vapour permeable"]
["2.5.2","Water resistant"]
["2.5.3","Interstitial anti-microbial agent"]
["2.5.4","Radiolucent"]
["2.6","Cover must be non-slip and sealed"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
["3.3","SANS 621"]
["3.4","SANS 883"]
["3.5","SANS 778 (subsection 5.2)"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[]
["RT24-02-14","Emergency Patient Stretcher, Basic","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[null,"Technical Specifications"]
[1.1,"Adjustable height , hydraulic, with foot pedal"]
[1.2,"Rising back rest, gas spring assisted"]
[1.3,"X-ray cassette system (for full body length)"]
[1.4,"Must have Trendellenburg and Anti-Trendellenburg mechanism with no less than 12 degrees movement "]
[1.5,"Must be able support a patient of mass 180 kg"]
[1.6,"Must have Oxygen cylinder holder"]
[1.7,"Must be supplied with Utility tray"]
[1.8,"Telescopic/adjustable drip rod at head end of trolley"]
[1.9,"Side rails must be collapsable"]
[{"v":1.1,"d":"1.10"},"Dimensions (approximate):"]
["1.10.1","Length: 2 100 mm"]
["1.10.2","Width: 750 mm"]
["1.10.3","Height: Adjustable from 600 to 900 mm"]
[1.11,"Castors at least 200 mm diameter"]
[1.12,"Centralized braking system with directional lock"]
[1.13,"Castors must comply with the latest issue of SANS 621"]
[1.14,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods: "]
["1.14.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.14.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.14.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.15,"Trolley must be easy to maneuver and steer in all direction using retractable 5th wheel"]
[1.16,"The trolley must have padded push handles in both sides with option to store away and retract them"]
[1.17,"The trolley must be equiped with roller bumpers in all four corners"]
[1.18,"It must be easy to activate central brake-and-go pedal"]
[1.19,"Manual CPR lever must be accessible from both side of the trolley"]
[2,"Mattress:"]
["2.1","Mattress to be a good quality high density foam of no less than 32 Kg/m3"]
["2.2","Must be constructed of high resilience polyurethane foam, to comply with SANS 883"]
["2.3","Mattress must be radio translucent, waterproof, non-slip or with retaining straps/hooks"]
["2.3.1","Dimension:"]
["2.3.2","Length: 1 950 mm"]
["2.3.3","Width: 600 mm"]
["2.3.4","Thickness: minimum 80 mm"]
["2.4","Cover to comply with the latest issue of SANS 1291-1"]
["2.5","Must be removable and complying with the following characteristcs;"]
["2.5.1","Vapour permeable"]
["2.5.2","Water resistant"]
["2.5.3","Interstitial anti-microbial agent"]
["2.5.4","Radiolucent"]
["2.6","Cover must be non-slip"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
["3.3","SANS 621"]
["3.4","SANS 883"]
["3.5","SANS 1291-1"]
[4,"WARRANTY & MAINTENANCE "]
["4.1","A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["4.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
["4.2","A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["4.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["RT24-02-15","Emergency Patient Stretcher, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Adjustable height , electric, with controls accessible in both sides"]
[1.2,"Trolley structure must have shocks/springs to provide comfort ride for patient"]
[1.3,"Electric operated rising back rest from 0o - 90o"]
[1.4,"X-ray cassette system (for full body length)"]
[1.5,"Must have Trendelenburg and Anti-Trendelenburg mechanism also electric operated with no less than 18o movement "]
[1.6,"Must be able support a bariatric patient of mass atleast 300 kg"]
[1.7,"Must have Oxygen cylinder holder"]
[1.8,"Must be supplied with Utility tray"]
[1.9,"Telescopic/adjustable drip rod at head end of trolley"]
[{"v":1.1,"d":"1.10"},"Side rails must be collapsable"]
[1.11,"Dimensions (approximate):"]
["1.11.1","Length: 2 100 mm"]
["1.11.2","Width: 750 mm"]
["1.11.3","Height: Adjustable from 550 to 900 mm"]
[1.12,"Castors at least 150-200 mm diameter"]
[1.13,"Centralized braking system with directional lock"]
[1.14,"Castors must comply with the latest issue of SANS 621"]
[1.15,"Trolley must be easy to maneuver and steer in all direction using retractable 5th wheel"]
[1.16,"The trolley must have padded push handles in both sides with option to store away and retract them"]
[1.17,"The trolley must be equiped with roller bumpers in all four corners"]
[1.18,"It must be easy to activate brake-and-go pedal"]
[1.19,"Electrically powered by 220V using retractable power cord"]
[{"v":1.2,"d":"1.20"},"The unit must have a back-up battery"]
[2,"Mattress:"]
["2.1","Mattress to be a good quality high density foam of no less than 32 Kg/m3"]
["2.2","Must be constructed of high resilience polyurethane foam, to comply with SANS 883"]
["2.3","Mattress must be radio translucent, waterproof, non-slip or with retaining straps/hooks"]
["2.3.1","Dimension:"]
["2.3.2","Length: 1 950 mm"]
["2.3.3","Width: 600 mm"]
["2.3.4","Thickness: minimum 80 mm"]
["2.4","Cover to comply with the latest issue of SANS 1291-1"]
["2.5","Must be removable and complying with the following characteristcs;"]
["2.5.1","Vapour permeable"]
["2.5.2","Water resistant"]
["2.5.3","Interstitial anti-microbial agent"]
["2.5.4","Radiolucent"]
["2.6","Cover must be non-slip"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3.3,"Warranty of accessories:"]
["3.3.1","Mattress: At least 4 years"]
["3.3.2","Cover: At least 2 years"]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 883"]
["4.6","SANS 1291-1"]
["4.7","IEC 60601-1-2 "]
[]
["RT24-02-16","Hospital Bed, Hydraulic","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
["1","Technical Specification"]
[1.1,"To comply with the latest issue of CKS 447 Note: where the item offered differs from the specification in CKS 447, except for the items specified below, the supplier must indicate the deviation and supply relevant details"]
[1.2,"Exception of CKS 447:"]
["1.2.1","Mattress support: mattress support other than weldmesh is required, provide details"]
["1.2.2","The height of the mattress support shall be adjustable in the range 380 – 760 mm (measured from the floor to the top of the mattress support). Tolerance +40mm"]
[1.3,"The mattress platform shall be in 4 sections allowing for a profiling action"]
[1.4,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.5,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.6,"The bed shall have a 4 section platform. The knee-break section adjustable via a manual mechanism"]
[1.7,"The bed must have maximum patient weight of at least 250 kg"]
[1.8,"Hydraulically operated variable height operated by dual sided foot pedals"]
[1.9,"Adjustable backrest with gas spring assist"]
[{"v":1.1,"d":"1.10"},"To be fitted with castors with a central castor locking system"]
[1.11,"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.12,"Removable head and foot ends (ABS material may be offered)"]
[1.13,"Collapsible safety sides must comply with IEC 60601-2-52 Annexure CC to prevent patient from falling off the bed"]
[1.14,"Mattress support: mattress support other than weldmesh is required, provide details"]
[1.15,"Oxygen cylinder holder must be available"]
[1.16,"Extension of bed of at least 25cm must be possible and mattress piece of the extension must be provided with the unit"]
[1.17,"The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price."]
["1.17.1","Driprod"]
["1.17.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.17.3","Traction pole with pulleys and weights"]
["1.17.4","Urine bag holder"]
[1.18,"The bed must be equiped with CPR mechanism"]
[1.19,"The backrest of the bed must have X-ray cassette holder (Optional)"]
["1.20","Bed Dimensions:"]
["1.20.1","Length:2020 mm (tolerance + 20mm)"]
["1.20.2","Width:915 mm (tolerance + 15mm)"]
[2,"Mattress"]
["2.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["2.2","Density: 32 - 38 Kg/m3, Please state the density of the item on offer"]
["2.3","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["2.4","Mattress must support a patient of at least 250 kg and return to original shape when not in use"]
["2.5","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["2.6","Mattress dimensions:"]
["2.6.1","Length: 1 980 mm  (+40mm)"]
["2.6.2","Width: 860 mm  (+20mm)"]
["2.6.3","Thickness: 150 mm (+5mm)"]
["2.7","Cover to comply with the latest issue of SANS 1291-1, proof of compliance must be submitted"]
["2.8","Must be fully enclosing sealed 2-way stretch and avoiding wrinles;"]
["2.8.1","Vapour permeable"]
["2.8.2","Water resistant"]
["2.8.3","Interstitial anti-microbial agent"]
["2.8.4","radiolucent"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) for the main unit should be as per the SCC document "]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including hydralic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["3.3","Mattress warranty of atleast 4 years"]
["3.4","Cover warranty of atleast 2 years"]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 883"]
["4.6","IEC 60601-2-52"]
["4.7","CKS 447"]
[null,"Hydraulic hospital Bed Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-16a","Mattress with sealed cover"]
["RT24-02-16b","Driprod"]
["RT24-02-16c","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-16d","Traction pole with pulleys and weights"]
["RT24-02-17","Hospital bed, High low, Electric (3- Section)","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrically operated variable height adjustment, backrest, knee break, reverse trendelenburg and trendelenburg"]
[1.3,"The height of the mattress support shall be adjustable in the range 380 – 760 mm (measured from the floor to the top of the mattress support) Tolerance +40mm"]
[1.4,"Backrest angle: 65o (+5o)"]
[1.5,"Trendelenburg angle: 15o (+3o)"]
[1.6,"Reverse trendelenburg angle: 15o (+3o)"]
[null,"Knee-break angle: 35o (+5o)"]
[1.7,"Mattress support: mattress support other than weldmesh is required, provide details"]
[1.8,"Collapsible safety sides must comply with IEC 60601-2-52 Annexure CC to prevent patient from falling off the bed"]
[1.9,"The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
[{"v":1.1,"d":"1.10"},"It must be possible to access the central brake mechanism from all side of the bed"]
[1.11,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.12,"The bed must have maximum patient weight of at least 250 kg"]
[1.13,"The hand control must have graphical representation of all positions"]
[1.14,"A buffer wheel shall be fitted to each of the 4 corners of the bed"]
[1.15,"Electrically adjustable backrest."]
[1.16,"To be fitted with castors with a central castor locking system"]
[1.17,"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted."]
[1.18,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.19,"Removable head and foot ends (ABS material may be offered)"]
[1.23,"Extension of bed of at least 25cm must be possible and mattress piece of the extension must be provided with the unit"]
[{"v":1.2,"d":"1.20"},"The following accessories must be accommodated to fit on the bed. The price for these accessories must not be included on this item bid price. "]
["1.20.1","Driprod"]
["1.20.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.20.3","Traction pole with pulleys and weights"]
["1.20.4","The bed must be equiped with CPR mechanism"]
["1.20.5","Urine bag holder"]
["1.20.5","The bed dimensions must be compatible with the mattress dimensions"]
["1.21","The motor/actuator housing of the bed must be well sealed against any fluid spillage."]
[2,"Mattress"]
["2.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["2.2","Density: 32 - 38 Kg/m3, Please state the density of the item on offer"]
["2.3","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["2.4","Mattress must support a patient of at least 250 kg and return to original shape when not in use"]
["2.5","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["2.6","Overall dimensions:"]
["2.6.1","Length: 1 980 mm  (+40mm)"]
["2.6.2","Width: 860 mm  (+20mm)"]
["2.6.3","Thickness: 150 mm (+5mm)"]
["2.7","Cover to comply with the latest issue of SANS 1291-1, proof of compliance must be submitted"]
["2.8","Must be fully enclosing sealed 2-way stretch and avoiding wrinles;"]
["2.8.1","Vapour permeable"]
["2.8.2","Water resistant"]
["2.8.3","Interstitial anti-microbial agent"]
["2.8.4","radiolucent"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) for the main unit should be as per the SCC document "]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Motor, Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
["3.2","Mattress warranty of atleast 4 years"]
["3.2","Cover warranty of atleast 2 years"]
[3.4,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.4.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 883"]
["4.6","SANS 1291-1"]
["4.7","IEC 60601-2-52"]
["4.8","IEC 60601-1-2 "]
[null,"Electric hospital Bed, 3-section Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-17a","Mattress with sealed cover"]
["RT24-02-17b","Driprod"]
["RT24-02-17c","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-17d","Traction pole with pulleys and weights"]
["RT24-02-18"," ICU Bed, 4-sections, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrically operated variable height adjustment, backrest, knee-break, reverse trendelenburg and trendelenburg"]
[1.3,"The height of the mattress support shall be adjustable in the range 380 – 760 mm (measured from the floor to the top of the mattress support), with tolerance of +40 mm"]
[1.4,"Backrest angle: 65o (+5o)"]
[1.5,"Knee-break angle: 35o (+5o)"]
[1.6,"Trendelenburg angle: 15o (+3o)"]
[1.7,"Reverse trendelenburg angle: 15o (+3o)"]
[1.8,"The bed must be equiped with backrest angle indicator"]
[1.9,"The bed shall be clearly marked with the corresponding Maximum Patient Weight and Safe Working Load in kg."]
[{"v":1.1,"d":"1.10"},"Maximum Patient Weight shall not be less than 300kg"]
[1.12,"The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
[1.13,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.14,"Collapsible safety sides must comply with IEC 60601-2-52 Annexure CC to prevent patient from falling off the bed"]
[1.15,"The bed must be fitted with Oxygen cylinder holder"]
[1.16,"To be fitted with castors with a central castor locking system"]
[1.17,"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.18,"Removable head and foot ends (ABS material may be offered)"]
[1.19,"Mattress support: mattress support other than weldmesh is required, provide details"]
[{"v":1.2,"d":"1.20"},"Extension of bed of at least 25cm must be possible and mattress extension piece must be provided"]
[1.21,"The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price:"]
["1.21.1","Driprod"]
["1.21.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.21.3","Traction pole with pulleys and weights"]
["1.21.4","Urine bag holder"]
[1.22,"The bed must have a battery back-up in case of power failure"]
[1.23,"The capacity of battery when fully charged must last for no less than 4 hours"]
["1.24","The motor/actuator housing of the bed must be well sealed against any fluid spillage."]
[2,"Mattress"]
["2.1","It must be a two sided multi-zoned flexible high density foam mattress with fully enclosing 2 way stretch cover to comply SANS 883"]
["2.2","The mattress shall be able to turn in 4 different ways (4-way turn), bidder to describe it is achieved"]
["2.3","Must be a Pressure reducing mattress"]
["2.4","The mattresses’ cover shall be clearly marked with a turntable guide and washing instruction"]
["2.5","The foam core must be of very high density and quality"]
["2.6","Mattress core data required: Bidder to specify the core data of the mattress offered:"]
["2.6.1","Density:                 No less than 42 Kg/m3 ",null,"   "]
["2.6.2","Hardness:             115 – 150 N"]
["2.6.3","Mattress depth:    ±170mm profile cut and zoned melamine free  "]
["2.6.4","Classification:              V"]
["2.6.5","Size:  1980 x 860 x 170mm (78” x 33¾” x 6¾”). "]
["2.6.6","The mattress shall be fire retardant"]
["2.6.7","Patient SWL 250 kg"]
["2.6.8","Mattress shall be X-Ray translucency and shall be suitable for CPR"]
["2.6.9","The mattresses’ cover shall be clearly marked with a turntable guide and washing instruction"]
["2.7","Cover data: Fully enclosing 2 way stretch to comply with SANS 1291-1"]
["2.7.1","Must be high elongation in warp and welt cover"]
["2.7.2","Must have an Interstitial Anti-microbial agent to prevent nosocomial and cross infections"]
["2.7.3","To prevent patient injuries and cross contamination the cover must be sealed"]
["2.7.4","Water resistant and made of waterproof fabric",null,"  "]
["2.7.5","Vapour permeable and water vapour breathable of no less than 500 g/m2/24hrs"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Motor, Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Motor, Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3.3,"Warranty of accessories:"]
["3.3.1","Mattress: At least 4 years"]
["3.3.2","Cover: At least 2 years"]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 883"]
["4.6","SANS 1291-1"]
["4.7","IEC 60601-2-52"]
["4.8","IEC 60601-1-2 "]
[null,"Electric ICU Bed, 4-section Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-18a","Pressure Relief Mattress with sealed cover"]
["RT24-02-18b","Driprod"]
["RT24-02-18c","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-18d","Traction pole with pulleys and weights"]
["RT24-02-18e","Battery"]
["RT24-02-18f","Built-in electronic scale (Upgrade)"]
["RT24-02-19","Bed, ICU, Multi-Function, Electric, with Intergrated electronic weighting scale","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrically operated variable height adjustment, backrest, knee-break, reverse trendelenburg, trendelenburg and Cardiac chair position"]
[1.3,"The height of the mattress support shall be adjustable in the range 380 – 760 mm (measured from the floor to the top of the mattress support), with tolerance of +40 mm"]
[1.4,"Backrest angle: 65o (+5o)"]
[1.5,"Knee-break angle: 35o (+5o)"]
[1.6,"Trendelenburg angle: 15o (+3o)"]
[1.7,"Reverse trendelenburg angle: 15o (+3o)"]
[1.8,"The bed must have Emergency CPR function through one touch button and manually"]
[1.9,"The bed must be equiped with backrest angle indicator"]
[{"v":1.1,"d":"1.10"},"The bed shall be clearly marked with the corresponding Maximum Patient Weight and Safe Working Load in kg."]
[1.11,"The bed shall be equiped with a battery back-up in case of power failure"]
[1.12,"Maximum Patient Weight shall not be less than 250kg"]
[1.13,"Safe Working Load shall not be less than 280kg"]
[1.14,"The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
[1.15,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.16,"Safety sides must be collapsible and must fully conform to Annexure CC of IEC 60601-2-52"]
[1.17,"The bed must be fitted with Oxygen cylinder holder"]
[1.18,"The bed must have dual control unit for end-users in both side of safety sides with lock key and control with limited positions accessible by patient."]
[1.19,"To be fitted with castors with a central castor locking system"]
[{"v":1.2,"d":"1.20"},"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.21,"Removable head and foot ends (ABS material may be offered)"]
[1.22,"Foot end must also be used as footrest during chair position"]
[1.23,"Mattress support: mattress support other than weldmesh is required, provide details"]
[1.24,"Extension of bed of at least 25cm must be possible"]
[1.25,"The unit must have a battery back-up"]
[1.26,"The back-up must last for no less than 4 hours at least when fully charged"]
[1.27,"The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price."]
["1.27.1","Driprod"]
["1.27.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.27.3","Traction pole with pulleys and weights"]
["1.27.4","Urine bag holder"]
[1.28,"The bed must be equiped with bumper buffers in all corners"]
[1.29,"The bed must also have bed exit position with one button"]
[1.3,"The bed must have fullchair and chair egress position using one button"]
[{"v":1.3,"d":"1.30"},"Scale"]
["1.30.1","The bed must have an intergrated weight scale with auto compesation feature."]
["1.30.2","The scale must have weighting capacity of atleast 250kg"]
["1.30.3","The scale must automatic switch-off feature after few seconds of weight display"]
[1,"Air Mattress:"]
[1.1,"Mattress shall support patients up to 250 kg."]
[1.2,"Mattress cell configuration shall consist of:"]
[1.3,"One or more static head cells that must be replaceable"]
[1.4,"Alternating cells along the length of the mattress, that must be replaceable"]
[1.5,"The mattress shall provide a lift of approximately 135 mm"]
[1.6,"The mattress shall be of modular design allowing for easy and cost effective repairs"]
[1.7,"The mattress shall fit and be compatible to the bed"]
[1.8,"The alternating operating cycle shall be variable up to 10 minutes (approximately)"]
[1.9,"The mattress shall automatically adjust pressures to optimal level according to patient weight, build and position as set by dial on the bed"]
[{"v":1.1,"d":"1.10"},"The mattress shall have a single hand action, CPR release and deflate within 15 sec"]
[1.11,"Dimensions:"]
["1.11.1","Length: 2000mm"]
["1.11.2","Max height at edges: 135mm"]
["1.11.3","Width: 850mm"]
["1.11.4","Cell height inflated: 135mm"]
[2,"Cover:"]
[2.1,"The mattress cover shall be two way stretch and loose fitting to comply with SANS 1291-1"]
[2.2,"The cover shall be water resistant"]
[2.3,"The cover shall be vapour permeable"]
[2.4,"The cover shall be bacteriostatic, fungistatic and antimicrobial"]
[2.5,"The cover shall resist development of mould and mildew"]
[2.6,"The cover shall be completely removable"]
[2.7,"The cover shall be fire retardant"]
[3,"Pump:"]
[3.1,"The pump shall be ergonomically designed and integral part of the bed"]
[3.2,"The pump shall be whisper quiet and vibration free"]
[3.3,"The pump shall be able to redistribute pressure according to weight"]
[3.7,"Interface pressure measured shall be below 20 mmHg for 50% of the cycle time"]
[3.8,"Highest interface pressure shall be 45 mmHg reducing to 5 mmHg during cycle time"]
[3.9,"Pump shall be able to distinguish between genuine alarms and transitory patient movement"]
[{"v":3.1,"d":"3.10"},"Pump shall comply with internationally recognized safety standards"]
[3.11,"Operating cycle: variable, 0-10 minutes"]
[4,"Multiway Tube-set:"]
[4.1,"Connecting and disconnecting of tubing shall be a single handed operation"]
[4.2,"Tubing shall be anti-kinking preventing blockage"]
[4.3,"Tube-set shall be interchangeable thus eliminating incorrect connection"]
[5,"Alarms:"]
[5.1,"Alarm conditions to be recorded in memory for diagnostic purposes"]
[5.2,"Mute button to silence audible alarms"]
[5.3,"The following alarms must be available in both audible and visual:"]
[5.4,"Low pressure alarm"]
[5.5,"High pressure alarm"]
[5.6,"Power failure alarm"]
[5.7,"Pump fault alarm"]
[1.33,"The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
["2.1","Mattress"]
["2.2","Mattress Cover"]
["2.3","Pump"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3.3,"Warranty of accessories:"]
["3.3.1","Mattress: At least 4 years"]
["3.3.2","Cover: At least 2 years"]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 1291-1"]
["4.6","IEC 60601-2-52"]
["4.7","IEC 60601-1-2 "]
[null,"Electric ICU Bed, Multi-section Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-19a","Air Mattress"]
["RT24-02-19b","Driprod"]
["RT24-02-19c","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-19d","Traction pole with pulleys and weights"]
["RT24-02-19e","Battery"]
["RT24-02-19f","Mattress Cell"]
["RT24-02-19g","Pump"]
["RT24-02-20","Bed, ICU, Multi-Function, Electric, with lateral tilt","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrically operated variable height adjustment, backrest, knee-break, reverse trendelenburg, trendelenburg, lateral tilt and Cardiac chair position:"]
["1.2.1","The height of the mattress support shall be adjustable in the range 380 – 760 mm (measured from the floor to the top of the mattress support), with tolerance of +40 mm"]
["1.2.2","Backrest angle: 65o (+5o)"]
["1.2.3","Knee-break angle: 35o (+5o)"]
["1.2.4","Trendelenburg angle: 15o (+3o)"]
["1.2.5","Reverse trendelenburg angle: 15o (+3o)"]
["1.2.6","Lateral tilt on both sides: 25o (+5o)"]
["1.3","The bed must have Emergency CPR function through one touch button and manually"]
["1.4","The bed must be equiped with backrest angle indicator"]
["1.5","The bed shall be clearly marked with the corresponding Maximum Patient Weight and Safe Working Load in kg."]
["1.6","The bed shall be equiped with a battery back-up in case of power failure"]
["1.7","Maximum Patient Weight shall not be less than 250kg"]
["1.8","Safe Working Load shall not be less than 280kg"]
["1.9","The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
["1.10","Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
["1.11","Safety sides must be collapsible and must fully conform to Annexure CC of IEC 60601-2-52"]
["1.12","The bed must be fitted with Oxygen cylinder holder"]
["1.13","The bed must have dual control unit for end-users in both side of safety sides with lock key and control with limited positions accessible by patient."]
["1.14","To be fitted with castors with a central castor locking system"]
["1.15","Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
["1.16","Removable head and foot ends (ABS material may be offered)"]
["1.17","Foot end must also be used as footrest during chair position"]
["1.18","Mattress support: mattress support other than weldmesh is required, provide details"]
["1.19","Extension of bed of at least 25cm must be possible"]
["1.20","The unit must have a battery back-up"]
["1.21","The back-up must last for no less than 4 hours at least when fully charged"]
["1.22","The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price."]
["1.22.1","Driprod"]
["1.22.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.22.3","Traction pole with pulleys and weights"]
["1.22.4","Urine bag holder"]
["1.23","The bed must be equiped with bumper buffers in all corners"]
["1.24","The bed must also have bed exit position with one button"]
["1.25","The bed must have fullchair and chair egress position using one button"]
["1.26","The lateral tilt must be programmable to operate automatic at set intervals"]
[null,"Air Mattress:"]
["1.27","Mattress shall support patients up to 250 kg."]
["1.28","Mattress cell configuration shall consist of:"]
["1.29","One or more static head cells that must be replaceable"]
["1.30","Alternating cells along the length of the mattress, that must be replaceable"]
["1.31","The mattress shall provide a lift of approximately 135 mm"]
["1.32","The mattress shall be of modular design allowing for easy and cost effective repairs"]
["1.33","The mattress shall fit and be compatible to the bed"]
["1.34","The alternating operating cycle shall be variable up to 10 minutes (approximately)"]
["1.35","The mattress shall automatically adjust pressures to optimal level according to patient weight, build and position as set by dial on the bed"]
["1.36","The mattress shall have a single hand action, CPR release and deflate within 15 sec"]
["1.37","Dimensions:"]
["1.37.1","Length: 2000mm"]
["1.37.2","Max height at edges: 135mm"]
["1.37.3","Width: 850mm"]
["1.37.4","Cell height inflated: 135mm"]
[null,"Cover:"]
["1.38","The mattress cover shall be two way stretch and loose fitting to comply with SANS 1291-1"]
["1.39","The cover shall be water resistant"]
["1.40","The cover shall be vapour permeable"]
["1.41","The cover shall be bacteriostatic, fungistatic and antimicrobial"]
["1.42","The cover shall resist development of mould and mildew"]
["1.43","The cover shall be completely removable"]
["1.44","The cover shall be fire retardant"]
[null,"Pump:"]
["1.45","The pump shall be ergonomically designed and integral part of the bed"]
["1.46","The pump shall be whisper quiet and vibration free"]
["1.47","The pump shall be able to redistribute pressure according to weight"]
["1.48","Interface pressure measured shall be below 20 mmHg for 50% of the cycle time"]
["1.49","Highest interface pressure shall be 45 mmHg reducing to 5 mmHg during cycle time"]
["1.50","Pump shall be able to distinguish between genuine alarms and transitory patient movement"]
["1.51","Pump shall comply with internationally recognized safety standards"]
["1.52","Operating cycle: variable, 0-10 minutes"]
[null,"Multiway Tube-set:"]
[null,"Connecting and disconnecting of tubing shall be a single handed operation"]
["1.53","Tubing shall be anti-kinking preventing blockage"]
["1.54","Tube-set shall be interchangeable thus eliminating incorrect connection"]
[null,"Alarms:"]
["1.55","Alarm conditions to be recorded in memory for diagnostic purposes"]
["1.56","Mute button to silence audible alarms"]
["1.57","The following alarms must be available in both audible and visual:"]
["1.57.1","Low pressure alarm"]
["1.57.2","High pressure alarm"]
["1.57.3","Power failure alarm"]
["1.57.4","Pump fault alarm"]
["1.58","The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
["2.1","Mattress"]
["2.2","Mattress Cover"]
["2.3","Tilt side mattress (lower body) support"]
["2.4","Tilt side mattress (Upper body) support"]
["2.5","Tilt mattress (head) support"]
["2.6","Tilt mattress (between legs) support"]
["2.7","Pump"]
[3,"WARRANTY & MAINTENANCE "]
["3.1","A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
["3.2","A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["3.3","Mattress: At least 4 years"]
["3.4","Cover: At least 2 years"]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 1291-1"]
["4.6","IEC 60601-2-52"]
["4.7","IEC 60601-1-2 "]
[null,"Electric ICU Bed, Multi-section Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-20a","Air Mattress"]
["RT24-02-20b","Driprod"]
["RT24-02-20c","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-20d","Traction pole with pulleys and weights"]
["RT24-02-20e","Battery"]
["RT24-02-20f","Mattress Cell"]
["RT24-02-20g","Scale (upgrade option)"]
["RT24-02-20h","Tilt side mattress (lower body) support"]
["RT24-02-20i","Tilt side mattress (Upper body) support"]
["RT24-02-20j","Tilt mattress (head) support"]
["RT24-02-20k","Tilt mattress (between legs) support"]
["RT24-02-20L","Pump"]
["RT24-02-21","Bariatric Bed, ICU, Electric","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"Must comply with IEC 60601-2-52 (Particular requirements for basic safety and essential performance of medical beds) paragraphs: 201.1, 201.3, 201.7, 201.9, 201.13, 201.15, annex BB and annex CC"]
[1.2,"Electrically operated variable height adjustment, backrest, knee-break, reverse trendelenburg and trendelenburg"]
[1.3,"The height of the mattress support shall be adjustable in the range 260 – 600 mm (measured from the floor to the top of the mattress support), with tolerance of +40 mm"]
[1.4,"Backrest angle: 65o (+5o)"]
[1.5,"Knee-break angle: 35o (+5o)"]
[1.6,"Trendelenburg angle: 15o (+3o)"]
[1.7,"Reverse trendelenburg angle: 15o (+3o)"]
[1.8,"The bed must be equiped with backrest angle indicator"]
[1.9,"The bed shall be clearly marked with the corresponding Maximum Patient Weight and Safe Working Load in kg."]
[{"v":1.1,"d":"1.10"},"Maximum Patient Weight shall not be less than 450kg"]
[1.11,"Safe Working Load shall not be less than 500kg"]
[1.12,"The bed must have controls for both patient with limited positions and for endusers accessible in both sides with all positions including lock key"]
[1.13,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2, proof of compliance must be submitted.Epoxy/nylon powder coating colours: white, cream or grey"]
[1.14,"Collapsible safety sides must comply with IEC 60601-2-52 Annexure CC to prevent patient from falling off the bed"]
[1.15,"The bed must be fitted with Oxygen cylinder holder"]
[1.16,"To be fitted with castors with a central castor locking system"]
[1.17,"Castors must comply with the latest issue of SANS 621, proof of compliance must be submitted. Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm"]
[1.18,"Removable head and foot ends (ABS material may be offered)"]
[1.19,"Mattress support: mattress support other than weldmesh is required, provide details"]
[{"v":1.2,"d":"1.20"},"Extension of bed of at least 25cm must be possible and extension mattress piece must be provided"]
[1.21,"The following accessories MUST be offered to fit on the bed. The price for these accessories must not be included on this item bid price."]
["1.21.1","Driprod"]
["1.21.2","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["1.21.3","Traction pole with pulleys and weights"]
["1.21.4","Urine bag holder"]
[1.22,"The bed must have a battery back-up in case of power failure"]
[1.23,"The capacity of battery when fully charged must last for no less than 4 hours"]
[2,"Mattress"]
["2.1","To comply with the latest issue of SANS 883 AND 1291-1 (type 2), except for thickness indicated below. Proof of compliance must be submitted"]
["2.2","Density: No less than 42 Kg/m3, Please state the density of the item on offer"]
["2.3","The mattress with cover must be flexible to accommodate anatomical contouring of all the angles of the bed"]
["2.4","Mattress must support a patient of at least 450 kg and return to original shape when not in use"]
["2.5","Mattress must be radiolucent.  To be constructed of flexible polyurethane foam complying with SANS 883"]
["2.6","Overall dimensions:"]
["2.6.1","Length: 1 980 mm  (+40mm)"]
["2.6.2","Width: 900 mm  (+20mm)"]
["2.6.3","Thickness: 150 mm (+5mm)"]
["2.7","Cover to comply with the latest issue of SANS 1291-1, proof of compliance must be submitted"]
["2.8","Must be fully sealed 2-way stretch and avoiding wrinles;"]
["2.8.1","Vapour permeable"]
["2.8.2","Water resistant"]
["2.8.3","Interstitial anti-microbial agent"]
["2.8.4","radiolucent"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"Mattress warranty: At least 4 years"]
[3.3,"Cover warranty: At least 2 years"]
[3.4,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.4.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 778 (Subsection 5.2)"]
["4.4","SANS 621"]
["4.5","SANS 883"]
["4.6","SANS 1291-1"]
["4.7","IEC 60601-2-52"]
["4.8","IEC 60601-1-2 "]
[null,"Electric Bariatric Bed, Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-21a","Bariatric Mattress with sealed cover"]
["RT24-02-21b","Battery"]
["RT24-02-21c","Driprod"]
["RT24-02-21d","Patient lifting pole with chain or strap and handle, must support a mass of 75 kg"]
["RT24-02-21e","Traction pole with pulleys and weights"]
["RT24-02-21f","Scale (450kg) - Upgrade"]
["RT24-02-22","MRI Stretcher","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specifications"]
["1.1","The trolley must have a hydraulic height adjustment with strong and stable structure"]
["1.2","It must be easy to activate brake-and-go pedal"]
["1.3","The unit must be constructed from 304 or 316 stainless steel or other non magnetic quality structure up to 3 Tesla."]
[null,"The structure should have epoxy/nylon powder-coating to minimise the steel exposure."]
["1.4","Trolley must be able to transport patient weight of minimum 180 kg"]
["1.5","Must have Rising back rest, gas spring assisted with range of 0o - 60o"]
["1.6","The trolley must be equiped with roller bumpers in all four corners"]
["1.7","Safety sides must be light weight and collapsible"]
["1.10","Must have Castors of at least 120 mm diameter"]
["1.11","Castors must comply with the latest issue of SANS 621"]
["1.12","Castors must be easy to maneuver in all direction, please state how that maneuvering is achieved"]
["1.13","The trolley must have padded push handles in both sides"]
["1.15","The unit must have protection bumpers in all corners"]
["1.16","Dimension:"]
["1.16.1","Length: 2100 mm"]
["1.16.2","Width: 650 mm"]
["1.17","Height: Adjustable from 600 mm at minimum (lower is better) to 900 mm (higher is better)"]
[2,"Mattress:"]
["2.1","Mattress to be a good quality high density foam of no less than 32 Kg/m3"]
["2.2","Must be constructed of high resilience polyurethane foam, to comply with SANS 640, Grade no. 12, Class 30"]
["2.3","Mattress must be radio translucent, waterproof, non-slip or with retaining straps/hooks"]
["2.3.1","Dimension:"]
["2.3.2","Length: 1 950 mm"]
["2.3.3","Width: 600 mm"]
["2.3.4","Thickness: minimum 80 mm"]
["2.4","Cover to comply with the latest issue of SANS 1291-1"]
["2.5","Must be removable and complying with the following characteristcs;"]
["2.5.1","Vapour permeable"]
["2.5.2","Water resistant"]
["2.5.3","Interstitial anti-microbial agent"]
["2.5.4","Radiolucent"]
["2.6","Cover must be non-slip"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 621"]
["4.4","SANS 1291-1"]
["RT24-02-23","Mortuary Stretcher","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
["1","Technical Specification"]
[1.1,"Stainless steel body tray"]
[1.2,"The trolley must be fitted with at least nylon rollers on the body tray support frame to make it easy to slide the body tray"]
[1.3,"The top frame of the trolley must be fully attached to the main frame and providing sufficient space of at least 450mm between the body tray"]
[1.4,"The trolley must be fitted with temper proof body tray locking mechanism. It must not be possible for the body tray to accidentally slide out of the trolley. Bidder to demonstrate."]
["1.4.1","Canopy cover to be made of laminated PVC (not canvas)"]
[1.5,"Material: stainless steel, grade A or B"]
[1.6,"Materials which are easily cleaned and of lasting finish, and low noise generating nature"]
[1.7,"Dimensions:"]
["1.7.1","Length: 2000mm (Body tray support)"]
["1.7.2","Width: 630mm"]
["1.7.3","Height: 800mm"]
[1.8,"The dimensions shall be subject to a tolerance of ± 10 mm. Normal mill tolerances shall apply"]
[1.9,"Must be fitted with body straps"]
[{"v":1.1,"d":"1.10"},"The trolley must have Peripheral bumper guard and buffer wheels"]
["1.11","Trolley must be fitted with four lockable 125mm castors"]
[2,"Standard Accessories:"]
["2.1","Canopy cover"]
[2.2,"Body tray"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["4.3","SANS 621"]
[null,"Mortuary Stretcher Accessories replacements","Complies Yes/No","COMMENTS"]
["RT24-02-23a","Canopy cover (laminated PVC) H: 450mm , to fit L:2000 mm , W: 630 mm Mortuary stretcher"]
["RT24-02-23b","125mm Castor"]
["RT24-02-23c","Body tray support"]
["RT24-02-23d","Nylon roller "]
["RT24-02-24","Mortuary Hydraulic Elevation Trolley","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"The trolley must constructed from stainless steel frame"]
[1.2,"The trolley must be fitted with at least nylon rollers on the body tray support frame to make it easy to slide the body tray"]
[1.3,"Height adjustable using foot operated hydraulic pump"]
[1.4,"Lowering down the trolley must semi automatic"]
[1.5,"The trolley must be fitted with temper proof body tray locking mechanism. It must not be possible for the body tray to accidentally slide out of the trolley. Bidder to demonstrate."]
[1.6,"Standard size stainless steel body tray to fit the trolley"]
[1.7,"Material: stainless steel, grade A or B"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature"]
[1.9,"Dimensions:"]
["1.9.1","Length: 2000mm (Body tray support)"]
["1.9.2","Width: 630mm"]
["1.9.3","Height: 300mm - 1800mm"]
[{"v":1.1,"d":"1.10"},"The dimensions shall be subject to a tolerance of ± 10 mm. Normal mill tolerances shall apply"]
[1.11,"Must be fitted with body straps"]
[1.12,"The trolley must have Peripheral bumper guard and buffer wheels"]
[1.13,"Trolley must be fitted with four lockable 125mm castors"]
[1.14,"The trolley must support maximum lifting load of at least 250kg"]
[1.15,"The design must be of a modern type"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["2.2.1","Please provide unique ref number of the ceriticate:"]
["2.3","SANS 621"]
["2.4","SANS 417"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[null,"Mortuary Elevation Trolley replacements","Complies Yes/No","COMMENTS"]
["RT24-02-24a","125mm Castor"]
["RT24-02-24b","Body tray support"]
["RT24-02-24c","Nylon roller "]
["RT24-02-24d","Hydraulic Cylinder"]
["RT24-02-25","Patient Hoist, Electric, Mobile","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"The hoist frame must be made from durable steel material, please state the steel type"]
[1.2,"The hanger bar assembly must be constructed in stable and solid manner that will prevent patient from swinging"]
[1.3,"If the frame is made of  Mild steel with epoxy/nylon powder-coated finish, it must comply with SANS 778 paragraph 5.2"]
[1.4,"The unit must provide stable lifting of the stated Safe Working Load"]
[1.5,"The unit must be equiped with Emergency Quick Release system"]
[1.6,"Safe Working Load: 250kg"]
[1.7,"Minimum Lifting Height: 500mm"]
[1.8,"Maximum Lifting Height: 1800mm"]
[1.9,"Handset operated with spiral cable"]
[{"v":1.1,"d":"1.10"},"The unit must have non-slip handles to assist with easy manuevering"]
[1.11,"The unit must have battery back-up"]
[1.12,"A fully charged battery back-up must last no less than 5 hours"]
[1.13,"Both rear castors to be fitted with a locking device"]
[1.14,"Castors must comply to the latest issue of SANS 621"]
[1.15,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.16,"Provision shall be made on the underside of the seat to hold the slop bucket and to allow its easy insertion and withdrawal"]
[1.17,"The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
["2.1","Universal padded sling"]
["2.2","Sling with commode opening"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[4.3,"SANS 778 (Subsection 5.2)"]
[4.4,"SANS 621"]
[4.5,"IEC 60601-1-2 "]
[null,"Patient Hoist, Electric,  Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-25a","Scale (250kg)"]
["RT24-02-25b","Universal padded sling"]
["RT24-02-25c","Sling with commode opening"]
["RT24-02-25d","Castors (set of 4)"]
["RT24-02-25e","Battery"]
["RT24-02-25f","Battery charger"]
["RT24-02-26","Bariatric Patient Hoist, Electric, Mobile","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"The hoist frame must be made from durable steel material, please state the steel type"]
[1.2,"The hanger bar assembly must be constructed in stable and solid manner that will prevent patient from swinging"]
[1.3,"If the frame is made of  Mild steel with epoxy/nylon powder-coated finish, it must comply with SANS 778 paragraph 5.2"]
[1.4,"The unit must provide stable lifting of the stated Safe Working Load"]
[1.5,"The unit must be equiped with Emergency Quick Release system"]
[1.6,"Safe Working Load: 450kg"]
[1.7,"Minimum Lifting Height: 500mm"]
[1.8,"Maximum Lifting Height: 1800mm"]
[1.9,"Handset operated with spiral cable"]
[{"v":1.1,"d":"1.10"},"The unit must have non-slip handles to assist with easy manuevering"]
[1.11,"The unit must have battery back-up"]
[1.12,"A fully charged battery back-up must last no less than 5 hours"]
[1.13,"Both rear castors to be fitted with a locking device"]
[1.14,"Castors must comply to the latest issue of SANS 621"]
[1.15,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.16,"Provision shall be made on the underside of the seat to hold the slop bucket and to allow its easy insertion and withdrawal"]
[1.17,"The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
["2.1","Universal padded sling"]
["2.2","Sling with commode opening"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[4.3,"SANS 778 (Subsection 5.2)"]
[4.4,"SANS 621"]
[4.5,"IEC 60601-1-2 "]
[4.3,"SANS 778 (Subsection 5.2)"]
[4.4,"SANS 621"]
[4.5,"IEC 60601-1-2 "]
[null,"Bariatric Patient Hoist, Electric, Accessories","Complies Yes/No","COMMENTS"]
["RT24-02-26a","Scale (450kg)"]
["RT24-02-26b","Universal padded sling"]
["RT24-02-26c","Sling with commode opening"]
["RT24-02-26d","Castors (set of 4)"]
["RT24-02-26e","Battery"]
["RT24-02-26f","Battery charger"]

{"sheet":"Category 3","index":3,"n_rows":90,"n_cols":4,"rows_kept":90,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 3"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-03-01","Bedpan Slip-in, with handle (Re-usable)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Material: Autoclavable polypropelene"]
[1.2,"The finishing must be smooth"]
[1.3,"Size: Adult"]
[1.4,"Length: 250mm x 400mm"]
[1.5,"Height: 20mm (front) x 100mm (back)"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-03-02","Bedpan and Urinal Stand","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 417, subsection 4 and 5.8"]
[1.2,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.3,"The thickness of the material must be atleast 0.7mm"]
[1.4,"Size: Adult"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","SANS 417"]
["2.2.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-03-03","Bedpan Slip-in, with handle and Lid (Re-usable)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Material: Autoclavable polypropelene"]
[1.2,"The finishing must be smooth"]
[1.3,"Size: Adult"]
[1.4,"Length: 250mm x 400mm"]
[1.5,"Height: 20mm (front) x 100mm (back)"]
[]
["RT24-03-04","Bedpan, with Lid","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 417, subsection 4 and 5.8"]
[1.2,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.3,"The thickness of the material must be atleast 0.7mm"]
[1.4,"The unit must have a lid"]
[1.5,".Size: Adult"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","SANS 417"]
["2.2.1","Please provide SANS 417 test Lab name and report number:"]
[null,"Bedpan ","Complies Yes/No","COMMENTS"]
["RT24-03-04a","Bedpan lid (spec to comply with SANS 417 (5.8) opening)"]
[]
["RT24-03-05","Bedpan Slip-in, (Disposable)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1,"Material: To be constructed with flushable material"]
[3,"Size: Adult"]
[4,"Dimensions: 308mm x 76mm x 406mm"]
[5,"Minimum pack of 500 units"]
[]
["RT24-03-06","Urinal, Male, Plastic","Complies Yes/No","COMMENTS"]
["1","Technical Specification"]
[1.1,"The design and dimensions to conform to type A or B of the latest issue of SANS 417, subsection 5.9"]
[1.2,"Material: Autoclavable Polypropelene plastic"]
[1.3,"The urinal must have a lid"]
[1.4,"Capacity: 1000ml"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","SANS 417"]
["2.2.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-03-07","Urinal, Male, Stainless Steel","Complies Yes/No","COMMENTS"]
["1","Technical Specification"]
[1.1,"The design and dimensions to conform to type A or B of the latest issue of SANS 417, subsection 5.9"]
[1.2,"Material: Stainless steel, type A or B, to comply with subsection 4.1.2 of SANS 417"]
[1.3,"Capacity: 1000ml"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","SANS 417"]
["2.2.1","Please provide SANS 417 test Lab name and report number:"]
[]
["RT24-03-08","Urinal Rack, Wallmount","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To hold 5 urinals, conforming to Fig. 9(b) of SANS 417)"]
[1.2," Urinals must hang at an angle to allow liquid to drip out"]
[1.3,"NO TRAY BELOW URINALS "]
[1.4,"Material: Stainless steel, type A or B, to comply with subsection 4.1.2 of SANS 417"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.2","SANS 417"]
["2.2.1","Please provide SANS 417 test Lab name and report number:"]

{"sheet":"Category 4","index":4,"n_rows":276,"n_cols":4,"rows_kept":276,"merged":[[0,0,0,3],[2,0,2,3],[4,0,4,3],[48,0,48,3],[92,0,92,3],[136,0,136,3]]}
["CATEGORY 4"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-04-01","Hospital Food Trolley, Stainless steel, Large","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","The unit must be suitable for storage, transportation and distribution of hot, cold or neutral patients meals"]
["1.1.1","Capacity: minimum 30 trays"]
["1.2","Manufactured from 1.2 mm thickness AISI 304 or 316 stainless steel"]
["1.3","Configuration:"]
["1.3.1","Single or double door or multi-compartment design"]
["1.3.2","Flat, reinforced worktop for meal tray preparation"]
["1.3.3","The unit shall have adjustable stainless steel shelves or removable gastronorm tray racks"]
["1.3.4","The unit shall have double-hinged or sliding doors, insulated with magnetic sealing (for hot/cold trolleys)"]
["1.4","The unit must have high density polyurethane foam of 30-40mm for thermal retention"]
["1.5","The electric heating or cooling system shall utilize thermostat to regulate temp"]
["1.6","Temperature range:"]
["1.6.1","Hot: +60o C to +85o C"]
["1.6.2","Cold: +2o C to +8o C"]
["1.7","The unit shall have ergonomic push handles on both sides to enable easy steering and moving"]
["1.8","The unit must have protection bumpers in all corners"]
["1.9","The unit shall have at least 100kg loading capacity with design that ensure even weight distribution"]
["1.10","The design must incorporate a bottom drainage outlet on insulated trolleys"]
["1.11","Dimensions:"]
["1.11.1","Height: 1500 mm     (± 20mm)"]
["1.11.2","Width:  800 mm     (± 40mm)"]
["1.11.3","Depth: 1000 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, 2 fitted with brakes and 2 directional. "]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
["1.17","The unit shall be powered by 220 -240V AC, 50Hz and power cord will be axtractable or have coiled hooks for safe keeping during delivery"]
["1.18","Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
["2.2","SANS 417"]
[null,"Hospital Food Trolley, Stainless steel Replacements","Complies Yes/No","COMMENTS"]
["RT24-04-01a","Castors (set of 4)"]
["RT24-04-01b","Regular sized polycarbonate plastic tray with resessed areas (set of 10)"]
["RT24-04-01c","Polycarbonate plastic Bowls with lid (set of 10)"]
["RT24-04-01d","Polycarbonate plastic cups with lid (set of 10)"]
["RT24-04-01e","Polycarbonate plastic plates with lid (set of 10)"]
[]
["RT24-04-02","Hospital Food Trolley, ABS Polymer, Large","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","The unit must be suitable for storage, transportation and distribution of hot, cold or neutral patients meals"]
["1.1.1","Capacity: minimum 30 trays"]
["1.2","Manufactured from hybrid design with stainless steel frame and ABS/Polymer panels"]
["1.3","Configuration:"]
["1.3.1","Single or double door or multi-compartment design"]
["1.3.2","Flat, reinforced worktop for meal tray preparation"]
["1.3.3","The unit shall have adjustable stainless steel shelves or removable gastronorm tray racks"]
["1.3.4","The unit shall have double-hinged or sliding doors, insulated with magnetic sealing (for hot/cold trolleys)"]
["1.4","The unit must have high density polyurethane foam of 30-40mm for thermal retention"]
["1.5","The electric heating or cooling system shall utilize thermostat to regulate temp"]
["1.6","Temperature range:"]
["1.6.1","Hot: +60o C to +85o C"]
["1.6.2","Cold: +2o C to +8o C"]
["1.7","The unit shall have ergonomic push handles on both sides to enable easy steering and moving"]
["1.8","The unit must have protection bumpers in all corners"]
["1.9","The unit shall have at least 100kg loading capacity"]
["1.10","The design must incorporate a bottom drainage outlet on insulated trolleys"]
["1.11","Dimensions:"]
["1.11.1","Height: 1500 mm     (± 20mm)"]
["1.11.2","Width:  800 mm     (± 40mm)"]
["1.11.3","Depth: 1000 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, 2 fitted with brakes and 2 directional"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
["1.17","The unit shall be powered by 220 -240V AC, 50Hz and power cord will be axtractable or have coiled hooks for safe keeping during delivery"]
["1.18","Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
["2.2","SANS 417"]
[null,"Hospital Food Trolley, ABS Replacements","Complies Yes/No","COMMENTS"]
["RT24-04-02a","Castors (set of 4)"]
["RT24-04-02b","Regular sized polycarbonate plastic tray with resessed areas (set of 10)"]
["RT24-04-02c","Polycarbonate plastic Bowls with lid (set of 10)"]
["RT24-04-02d","Polycarbonate plastic cups with lid (set of 10)"]
["RT24-04-02e","Polycarbonate plastic plates with lid (set of 10)"]
[]
["RT24-04-03","Hospital Food Trolley, Stainless Steel, Medium","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","The unit must be suitable for storage, transportation and distribution of hot, cold or neutral patients meals"]
["1.1.1","Capacity: minimum 20 trays"]
["1.2","Manufactured from 1.2 mm thickness AISI 304 or 316 stainless steel"]
["1.3","Configuration:"]
["1.3.1","Single or double door or multi-compartment design"]
["1.3.2","Flat, reinforced worktop for meal tray preparation"]
["1.3.3","The unit shall have adjustable stainless steel shelves or removable gastronorm tray racks"]
["1.3.4","The unit shall have double-hinged or sliding doors, insulated with magnetic sealing (for hot/cold trolleys)"]
["1.4","The unit must have high density polyurethane foam of 30-40mm for thermal retention"]
["1.5","The electric heating or cooling system shall utilize thermostat to regulate temp"]
["1.6","Temperature range:"]
["1.6.1","Hot: +60o C to +85o C"]
["1.6.2","Cold: +2o C to +8o C"]
["1.7","The unit shall have ergonomic push handles on both sides to enable easy steering and moving"]
["1.8","The unit must have protection bumpers in all corners"]
["1.9","The unit shall have at least 100kg loading capacity"]
["1.10","The design must incorporate a bottom drainage outlet on insulated trolleys"]
["1.11","Dimensions:"]
["1.11.1","Height: 1200 mm     (± 20mm)"]
["1.11.2","Width:  700 mm     (± 40mm)"]
["1.11.3","Depth: 950 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, 2 fitted with brakes and 2 directional"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
["1.17","The unit shall be powered by 220 -240V AC, 50Hz and power cord will be axtractable or have coiled hooks for safe keeping during delivery"]
["1.18","Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
["2.2","SANS 417"]
[null,"Hospital Food Trolley, SS Replacements","Complies Yes/No","COMMENTS"]
["RT24-04-03a","Castors (set of 4)"]
["RT24-04-03b","Regular sized polycarbonate plastic tray with resessed areas (set of 10)"]
["RT24-04-03c","Polycarbonate plastic Bowls with lid (set of 10)"]
["RT24-04-03d","Polycarbonate plastic cups with lid (set of 10)"]
["RT24-04-03e","Polycarbonate plastic plates with lid (set of 10)"]
[]
["RT24-04-04","Hospital Food Trolley, ABS Polymer, Medium","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","The unit must be suitable for storage, transportation and distribution of hot, cold or neutral patients meals"]
["1.1.1","Capacity: minimum 20 trays"]
["1.2","Manufactured from hybrid design with stainless steel frame and ABS/Polymer panels"]
["1.3","Configuration:"]
["1.3.1","Single or double door or multi-compartment design"]
["1.3.2","Flat, reinforced worktop for meal tray preparation"]
["1.3.3","The unit shall have adjustable stainless steel shelves or removable gastronorm tray racks"]
["1.3.4","The unit shall have double-hinged or sliding doors, insulated with magnetic sealing (for hot/cold trolleys)"]
["1.4","The unit must have high density polyurethane foam of 30-40mm for thermal retention"]
["1.5","The electric heating or cooling system shall utilize thermostat to regulate temp"]
["1.6","Temperature range:"]
["1.6.1","Hot: +60o C to +85o C"]
["1.6.2","Cold: +2o C to +8o C"]
["1.7","The unit shall have ergonomic push handles on both sides to enable easy steering and moving"]
["1.8","The unit must have protection bumpers in all corners"]
["1.9","The unit shall have at least 100kg loading capacity"]
["1.10","The design must incorporate a bottom drainage outlet on insulated trolleys"]
["1.11","Dimensions:"]
["1.11.1","Height: 1200 mm     (± 20mm)"]
["1.11.2","Width:  700 mm     (± 40mm)"]
["1.11.3","Depth: 950 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, 2 fitted with brakes and 2 directional"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
["1.17","The unit shall be powered by 220 -240V AC, 50Hz and power cord will be axtractable or have coiled hooks for safe keeping during delivery"]
["1.18","Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
["2.2","SANS 417"]
[null,"Hospital Food Trolley, ABS Replacements","Complies Yes/No","COMMENTS"]
["RT24-04-04a","Castors (set of 4)"]
["RT24-04-04b","Regular sized polycarbonate plastic tray with resessed areas (set of 10)"]
["RT24-04-04c","Polycarbonate plastic Bowls with lid (set of 10)"]
["RT24-04-04d","Polycarbonate plastic cups with lid (set of 10)"]
[]
["RT24-04-05","Drug Cabinet, Wall-mount, small","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The design and dimensions to comply with the latest issue of CKS 181 (fig 2), type B"]
[1.2,"Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.3,"The mild steel plate shall have a nominal thickness of not less than 1,20 mm"]
[1.4,"The cabinet must not be marked \"Poison\""]
[1.5,"Size: small"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"CKS 181"]
[2.2,"SANS 778 (subsection 5.2)"]
[]
["RT24-04-06","Drug Cabinet, Wall-mount, large","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The design and dimensions to comply with the latest issue of CKS 181 (fig 4), type D"]
[1.2,"Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.3,"The mild steel plate shall have a nominal thickness of not less than 1,20 mm"]
[1.4,"The cabinet must not be marked \"Poison\""]
[1.5,"Size: Large"]
[1.6,"Cabinet must be a Double door type with internal cupboard"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"CKS 181"]
[2.2,"SANS 778 (subsection 5.2)"]
[]
["RT24-04-07","First-aid kit, Cabinet, Metal","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","Container:"]
["1.2","The entire contents to be contained in a metal box"]
["1.2.1","Dimension of the box must permit the adequate storing of the content, with all the bottles in an upright position"]
["1.2.2","Dimensions:"]
["1.2.2.1","450 x 350 x 120 mm"]
["1.2.3","Front of the box must be hinged at the bottom and securely supported by chains (of a type which do not become entangled) on both sides or similiar means to provide a platform to work on when in the horizontal fold down"]
["1.2.4","The box must be provided with a suitable devices for securing it to the wall"]
["1.2.5","The box must be fitted with a clasp and staple for locking purposes"]
["1.2.6","The box is to be finished according to the latest issue of SANS 1188-1"]
["2","First-aid Refill Consumables to be supplied on initial purchase and supplied as a set for refill purpose:"]
[2.1,"Wound cleaner (100 ml)"]
[2.2,"Swabs for cleaning wounds"]
[2.3,"Cotton wool for padding (100 g)"]
[2.4,"Sterile gauze (minimum qty 20)"]
[2.5,"Absorbent material (100g)"]
[2.6,"1 x Pair of forceps (for splinters)"]
[2.7,"1 x Pair of scissors (minimum size 100 mm)"]
[2.8,"1 x Card safety pins"]
[2.9,"4 x Triangular bandages"]
[{"v":2.1,"d":"2.10"},"4 x Roller bandages (75 mm x 5 m)"]
[2.11,"4 x Roller bandages (100 mm x 5 m)"]
[2.12,"1 x Roll elastic adhesive (25 mm x 3 m)"]
[2.13,"1 x Anti allergenic adhesive strip (25 mm x 3 m)"]
[2.14,"1 x Packet adhesive dressing strips (minimum quantity 10 assorted sizes)"]
[2.15,"4 x First aid dressings (75 mm x 100 mm)"]
[2.16,"4 x First aid dressings (150 mm x 200 mm)"]
[2.17,"2 x Straight splints"]
[2.18,"2 x Cardio Pulmonary resuscitation mouthpieces or similar device"]
[2.19,"Eye patch"]
[{"v":2.2,"d":"2.20"},"Space blanket"]
[2.21,"2 x Burn dressing 10 x 10 cm"]
[2.22,"2 x Burn dressing 20 x 20 cm"]
[2.23,"2 x Pairs latex-free gloves (medium)"]
[2.24,"2 x Pairs latex-free gloves (large)"]
[2.25,"Disposable, sealable plastic bag"]
[]
["RT24-04-08","First-aid kit, Cabinet, Plastic","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","Container:"]
["1.2","The entire contents to be contained in a metal box"]
["1.2.1","Dimension of the box must permit the adequate storing of the content, with all the bottles in an upright position"]
["1.2.2","Dimensions:"]
["1.2.2.1","450 x 350 x 120 mm"]
["1.2.3","Front of the box must be hinged at the bottom and securely supported by chains (of a type which do not become entangled) on both sides or similiar means to provide a platform to work on when in the horizontal fold down"]
["1.2.4","The box must be provided with a suitable devices for securing it to the wall"]
["1.2.5","The box must be fitted with a clasp and staple for locking purposes"]
["1.2.6","The box is to be finished according to the latest issue of SANS 1188-1"]
["2","First-aid Refill Consumables to be supplied on initial purchase and supplied as a set for refill purpose:"]
[2.1,"Wound cleaner (100 ml)"]
[2.2,"Swabs for cleaning wounds"]
[2.3,"Cotton wool for padding (100 g)"]
[2.4,"Sterile gauze (minimum qty 20)"]
[2.5,"Absorbent material (100g)"]
[2.6,"1 x Pair of forceps (for splinters)"]
[2.7,"1 x Pair of scissors (minimum size 100 mm)"]
[2.8,"1 x Card safety pins"]
[2.9,"4 x Triangular bandages"]
[{"v":2.1,"d":"2.10"},"4 x Roller bandages (75 mm x 5 m)"]
[2.11,"4 x Roller bandages (100 mm x 5 m)"]
[2.12,"1 x Roll elastic adhesive (25 mm x 3 m)"]
[2.13,"1 x Anti allergenic adhesive strip (25 mm x 3 m)"]
[2.14,"1 x Packet adhesive dressing strips (minimum quantity 10 assorted sizes)"]
[2.15,"4 x First aid dressings (75 mm x 100 mm)"]
[2.16,"4 x First aid dressings (150 mm x 200 mm)"]
[2.17,"2 x Straight splints"]
[2.18,"2 x Cardio Pulmonary resuscitation mouthpieces or similar device"]
[2.19,"Eye patch"]
[{"v":2.2,"d":"2.20"},"Space blanket"]
[2.21,"2 x Burn dressing 10 x 10 cm"]
[2.22,"2 x Burn dressing 20 x 20 cm"]
[2.23,"2 x Pairs latex-free gloves (medium)"]
[2.24,"2 x Pairs latex-free gloves (large)"]
[2.25,"Disposable, sealable plastic bag"]

{"sheet":"Category 5","index":5,"n_rows":166,"n_cols":4,"rows_kept":166,"merged":[[0,0,0,3],[1,0,1,3],[3,6,3,9],[6,1,6,3],[7,1,7,3],[8,1,8,3],[59,1,59,3],[65,1,65,3],[66,1,66,3],[67,1,67,3],[120,1,120,3],[127,2,127,3],[138,2,138,3],[147,2,147,3]]}
["CATEGORY 5"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-05-01","Theater Table, Standard","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
[1,"Description"]
[1.1,"Theatre table on which the patient lies during a surgical operation, universal electronically operated"]
[2,"Product Offered:"]
[2.1,"Make:"]
[2.2,"Model:"]
[2.3,"Initial Manufacturing year of Model:"]
[3,"Technical Specification"]
["3.1","The table must have a maximum load capacity of atleast 250kg"]
["3.2","Radiotranslucent table top for free C-arm access"]
["3.3","Decompression mattress with non-slip, antistatic, waterproof and seamless design"]
["3.4","Four section operation"]
["3.5","Trendelenberg and reverse trendelenberg function to at least 25o"]
["3.6","Lateral tilt of at least 18o"]
["3.7","Reflex position of at least 100o"]
["3.8","The maximum height of the table measured without mattress must be more than 1000mm from the floor and minimum height of the table must be less than 710mm from the floor"]
["3.9","Longitudinal shift of at least 25cm and still maintaining the balance and stability with maximum load capacity"]
["3.10","Table controls on remote handpiece as well as on the table column with positions clearly indicated."]
["3.11","Table column base covers must be at least 304 stainless steel grade"]
["3.12","The table base must have a clear and visible laminated label (\"Do not place any items here\") in yellow to deter user from placing accessories on the base"]
["3.13","The table base must be stable, mobile and lockable/brakes through both the hand remote piece and the coloumn panel and the unit must have manual override for the brakes should the electronic fails"]
["3.14","Separate 2 leg sections"]
["3.15","Battery backup of at least 2 hours operation when fully charded with internal battery charger"]
["3.16","The unit must be supplied complete with below standard accessories"]
[4,"Standard Accessories"]
["4.1","Anaesthetics arm board x 2"]
["4.2","Set of padded Lithotomy poles (manual) with their own universal clamps to allow resting of the calf"]
["4.3","2 sets of bedside rail clamps"]
["4.4","Anaesthetic screen"]
["4.5","Dedicated Accessory storage cart"]
["4.6","Horse-shoe Gel head support (neonatal), diameter between 8.3-9cm"]
["4.7","Horse-shoe Gel head support (Paeds), diameter between 14-16cm"]
["4.8","Horse-shoe Gel head support (Adult), diameter between 20-25cm"]
[5,"Conformity Compliance (Please attach certificate)"]
[5.1,"The unit must comply with an acceptable international electrical safety standard such as IEC 601-1 for medical equipment, attached certification"]
[5.2,"The unit must comply with electrical safety and performance standard such as IEC 60601-2-46, attached certification"]
["5.2.1","Please provide unique ref number of the IEC ceriticate:"]
["5.3","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["5.3.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["5.4","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["5.4.1","Please provide unique ref number of the ceriticate:"]
["5.5","The mains cable of the unit being quoted for must be 15 amp 3 prong hospital grade (rubber to with 2 screws) type and it must be a minimum length of three (3) meters. NB the mains cable of the unit tendered for must be SABS colour coded."]
["5.6","The equipment quoted for must be protected against electromagnetic interference IEC 60601-1-2"]
["5.6.1","Please provide unique ref number of the IEC ceriticate:"]
["5.7","Hazardous Substance Act:  If this type of equipment / apparatus appears on the schedule of Hazardous substances issued by the Directorate: Health Technology of the Department of Health, a license in terms of the Act on Hazardous Substances (Act 15/1973) must be submitted with the bid / quotation documents. The license must be registered under the bidders name or a letter of joint venture must be submitted by the license holder where the license is not in the name of the bidder. Bidders that neglect to submit a license will not be considered"]
["5.8","All electrical/electronic medical equipment must be licensed by Radiation Control, where applicable a copy of the license must be submitted The license must be registered under the bidders name or a letter of joint venture must be submitted by the license holder where the license is not in the name of the bidder. Bidders that neglect to submit a license will not be considered"]
["5.8.1","Radiation Control License number:"]
[6,"Comprehensive Maintenance"]
[6.1,"A 24 month warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["6.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[6.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["6.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["6.3","The bidder to provide the OEM recommended service interval of the unit:"]
["6.4","Bidder to provider details of technical work (Spare parts & Calibrations) involving the unit bidded for"]
["7","General  "]
["7.1","Has the product on offer being on safety recall by the Regulatory Authority in the last 5 years? If yes, please provide further details of the recall and how was it addressed"]
["7.2","The unit on offer must be the latest technology. "]
["7.2.1","Initial Manufacturing year of Model:"]
[]
["RT24-05-02","Theater Table, Bariatric","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
[1,"Description"]
[1.1,"Theatre table on which the patient lies during a surgical operation, universal electronically operated"]
[2,"Product Offered:"]
[1.1,"Make:"]
[1.2,"Model:"]
[1.3,"Initial Manufacturing year of Model:"]
[3,"Technical Specification"]
["3.1","The table must have a maximum load capacity of 450kg with extended sides and foot to accommodate Obese patient"]
["3.1.1","Table top width and foot width of 710mm"]
["3.2","Radiotranslucent table top for free C-arm access"]
["3.3","Decompression mattress with non-slip, antistatic, waterproof and seamless design"]
["3.4","Four section operation"]
["3.5","Trendelenberg and reverse trendelenberg function to at least 25o"]
["3.6","Lateral tilt of at least 18o"]
["3.7","Reflex position of at least 100o"]
["3.8","The maximum height of the table measured without mattress must be more than 1000mm from the floor and minimum height of the table must be less than 710mm from the floor"]
["3.9","Longitudinal shift of at least 25cm and still maintaining the balance and stability with maximum load capacity"]
["3.10","Table controls on remote handpiece as well as on the table column with positions clearly indicated."]
["3.11","Table column base covers must be at least 304 stainless steel grade"]
["3.12","The table base must have a clear and visible laminated label (\"Do not place any items here\") in yellow to deter user from placing accessories on the base"]
["3.13","The table base must be stable, mobile and lockable/brakes through both the hand remote piece and the coloumn panel and the unit must have manual override for the brakes should the electronic fails"]
["3.14","Separate 2 leg sections"]
["3.15","Battery backup of at least 2 hours operation when fully charded with internal battery charger"]
[4,"Standard Accessories"]
["4.1","Anaesthetics arm board x 2"]
["4.2","Set of padded Lithotomy poles (manual) with their own universal clamps to allow resting of the calf"]
["4.3","2 sets of bedside rail clamps"]
["4.4","Anaesthetic screen"]
["4.5","Dedicated Accessory storage cart"]
["4.6","Extensions (width & Foot)"]
["4.7","Horse-shoe Gel head support (Bariatric), Dia abobe 25cm"]
["4.8","Reverse trendelenburg straps"]
["4.9","Foot stop/board"]
[5,"Conformity Compliance (Please attach certificate)"]
[5.1,"The unit must comply with an acceptable international electrical safety standard such as IEC 601-1 for medical equipment, attached certification"]
[5.2,"The unit must comply with electrical safety and performance standard such as IEC 60601-2-46, attached certification"]
["5.2.1","Please provide unique ref number of the IEC ceriticate:"]
["5.3","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["5.3.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["5.4","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["5.4.1","Please provide unique ref number of the ceriticate:"]
["5.5","Hazardous Substance Act:  If this type of equipment / apparatus appears on the schedule of Hazardous substances issued by the Directorate: Health Technology of the Department of Health, a license in terms of the Act on Hazardous Substances (Act 15/1973) must be submitted with the bid / quotation documents. The license must be registered under the bidders name or a letter of joint venture must be submitted by the license holder where the license is not in the name of the bidder. Bidders that neglect to submit a license will not be considered"]
["5.6","All electrical/electronic medical equipment must be licensed by Radiation Control, where applicable a copy of the license must be submitted The license must be registered under the bidders name or a letter of joint venture must be submitted by the license holder where the license is not in the name of the bidder. Bidders that neglect to submit a license will not be considered"]
["5.6.1","Radiation Control License number:"]
["5.7","Must comply with 2.5 Occupational Health and Safety Act, Act no 85 of 1993 and Regulations"]
["5.8","The mains cable of the unit being quoted for must be 15 amp 3 prong hospital grade (rubber to with 2 screws) type and it must be a minimum length of three (3) meters. NB the mains cable of the unit tendered for must be SABS colour coded."]
["5.9","The equipment quoted for must be protected against electromagnetic interference IEC 60601-1-2"]
["5.9.1","Please provide unique ref number of the IEC ceriticate:"]
[6,"Comprehensive Maintenance"]
[6.1,"A 24 month warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["6.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[6.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["6.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["6.3","The bidder to provide the OEM recommended service interval of the unit:"]
["6.4","Bidder to provider details of technical work (Spare parts & Calibrations) involving the unit bidded for"]
["7","General  "]
["7.1","Has the product on offer being on safety recall by the Regulatory Authority in the last 5 years? If yes, please provide further details of the recall and how was it addressed"]
["7.2","The unit on offer must be the latest technology. "]
["7.2.1","Initial Manufacturing year of Model:"]
[null,"Bariatric Theater Table Accessories","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
["RT24-05-02a","Table extensions to 710mm"]
["RT24-05-02b","Reverse trendelenburg straps"]
["RT24-05-02c","Foot stop/board"]
["RT24-05-02d","710mm wide Foot extension"]
["RT24-05-03","Universal Orthopaedic Accessories","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
[null,"List of Models compatible with the set:\n(Bidder may be required to demo compatibility during Sample evaluation)"]
["RT24-05-03a","Neuro Head Support, Horseshoe Head Support (set of 3; Neo, Paeds & Adult)"]
["RT24-05-03b","Orthopaedic extension unit (complete to accommodate upper & lower limp surgery)"]
["RT24-05-03c","Back section extention"]
["RT24-05-03d","Arm hand table"]
["RT24-05-03e","Shoulder plate"]
["RT24-05-03f","Dedicated Orthopaedic Accessory cart"]
["RT24-05-03g","Patient strapping"]
["RT24-05-03h","Foot stop/board"]
[]
["RT24-05-04","Universal Neurosurgery Accessories","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
[null,"List of Models compatible with the set:\n(Bidder may be required to demo compatibility during Sample evaluation)"]
["RT24-05-04a","Neuro – Skull Clamp"]
["RT24-05-04b","Neuro – Horse Shoe"]
["RT24-05-04c","Neuro – Base Unit "]
["RT24-05-04d","Neuro – Swivel adaptor with clamps"]
["RT24-05-04e","Neuro – Crossbar Adaptor "]
["RT24-05-04f","Neuro – Dedicated Wall Storage Unit"]
["RT24-05-04g","Neuro – Head Rest adaptor"]
["RT24-05-05","Universal Spinal Accessories","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
[null,"List of Models compatible with the set:\n(Bidder may be required to demo compatibility during Sample evaluation)"]
[null,"Make and Model of Posterior attachment:"]
["RT24-05-05","Posterior spinal attachment consisting of a self-contained transport system, a completely radiolucent table top made up of a head support  system as well as an abdominal support system all of which must be able to move longitudinally to accommodate adult and pediatric size patients"]
[]
["RT24-05-06","Theater Table Replacement Accessories","Complies Yes/No","Provide your answers in this Column.  You are advised to be straight to the point."]
["RT24-05-06a","Anaesthetics arm board (Pair)"]
["RT24-05-06b","Padded Lithotomy poles (manual) with their own universal clamps to allow resting of the calf (Pair)"]
["RT24-05-06c","Bedside rail clamps (Pair)"]
["RT24-05-06d","Anaesthetic screen (Complete with clamps)"]
["RT24-05-06e","Dedicated Accessory storage cart"]
["RT24-05-06f","Disposable bin for Urology and Gynecology"]
["RT24-05-06g","urology adaptor"]
["RT24-05-06h","General purpose head support"]
["RT24-05-06i","Horse-shoe Gel head support (neonatal), diameter between 8.3-9cm"]
["RT24-05-06j","Horse-shoe Gel head support (Paeds), diameter between 14-16cm"]
["RT24-05-06k","Horse-shoe Gel head support (Adult), diameter between 20-25cm"]
["RT24-05-06L","Donut Gel head support (neonatal), diameter between 8.3-9cm"]
["RT24-05-06m","Donut Gel head support (Paeds), diameter between 14-16cm"]
["RT24-05-06n","Donut Gel head support (Adult), diameter between 20-25cm"]

{"sheet":"Category 6","index":6,"n_rows":155,"n_cols":4,"rows_kept":155,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 6"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-06-01","Wrist Restrain system, Small","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s hands to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe, and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both hands or a pair shall be supplied to restrain both hands"]
["1.10","Size:  Small ( dimensions: 120 - 190mm) +20mm tolerance"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)",null,"Replacements"]
[null,"Wrist Restrain system Replacements","Complies Yes/No","COMMENTS"]
["RT24-06-01a","Magnetic keys (Pk of 10)"]
[]
["RT24-06-02","Wrist Restrain system, Medium","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s hands to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both hands or a pair shall be supplied to restrain both hands"]
["1.10","Size:  Medium (Dimensions: 160 - 240mm) +20mm tolerance"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[]
["RT24-06-03","Wrist Restrain system, Large","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s hands to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both hands or a pair shall be supplied to restrain both hands"]
["1.10","Size:  Large (Dimesions: 220 - 290mm) +20mm tolerance"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[]
["RT24-06-04","Ankle Restrain system, Small","Complies Yes/No","COMMENTS"]
["1","Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s ankles to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both ankles "]
["1.10","Size:  Small"]
["1.11","Dimensions: 170 - 250mm (Tolerance +20mm)"]
["1.12","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[null,"Ankle Restrain system Replacements","Complies Yes/No","COMMENTS"]
["RT24-06-04a","Magnetic keys (Pk of 10)"]
[]
["RT24-06-05","Ankle Restrain system, Medium","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s ankles to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both ankles "]
["1.10","Size:  Medium"]
["1.11","Dimensions: 220 - 300mm (Tolerance +20mm)"]
["1.12","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[]
["RT24-06-06","Ankle Restrain system, Large","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient’s ankles to the bed frame"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism on the cuffs to prevent unauthorised opening"]
["1.5","The restrain bands must have a connecting strap"]
["1.6","The bidder must demonstrate the effectiveness of the system"]
["1.7","The unit to be supplied with magnetic keys"]
["1.8","Cuffs shall be adjustable to fit most limb sizes"]
["1.9","The restrain system must be a single unit for both ankles "]
["1.10","Size:  Large"]
["1.11","Dimensions: 270 - 330mm (Tolerance +20mm)"]
["1.12","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[]
["RT24-06-07","Waist Belt Restrain system, Small","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient from falling ",null,"Consider removal"]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism to prevent unauthorised opening"]
["1.5","The bidder must demonstrate the effectiveness of the system"]
["1.6","The unit to be supplied with magnetic keys"]
["1.7","System to prevent patient from getting out of bed"]
["1.8","The belt must allow patient to turn to either side and sit without the risk of falling"]
["1.9","Size:  Small"]
["1.10","Dimensions: 520 - 820mm (Tolerance +20mm)"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[null,"Waist Belt Restrain system Replacements","Complies Yes/No","COMMENTS"]
["RT24-06-07a","Magnetic keys (Pk of 10)"]
[]
["RT24-06-08","Waist Belt Restrain system, Medium","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient from falling "]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism to prevent unauthorised opening"]
["1.5","The bidder must demonstrate the effectiveness of the system"]
["1.6","The unit to be supplied with magnetic keys"]
["1.7","System to prevent patient from getting out of bed"]
["1.8","The belt must allow patient to turn to either side and sit without the risk of falling"]
["1.9","Size:  Medium"]
["1.10","Dimensions: 800 - 1200mm (Tolerance +20mm)"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]
[]
["RT24-06-09","Waist Belt Restrain system, Large","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The restrain bands must be well and smoothly padded to secure patient from falling "]
["1.2","Bands shall be made from good quality material. Bidder to specify material"]
["1.3","System to be secure, safe and tamperproof"]
["1.4","Bands must have locking mechanism to prevent unauthorised opening"]
["1.5","The bidder must demonstrate the effectiveness of the system"]
["1.6","The unit to be supplied with magnetic keys"]
["1.7","System to prevent patient from getting out of bed"]
["1.8","The belt must allow patient to turn to either side and sit without the risk of falling"]
["1.9","Size:  Large"]
["1.10","Dimensions: 1160 - 1560mm (Tolerance +20mm)"]
["1.11","The unit must be washable to prevent disinfection"]
[2,"Standard Accessories:"]
["2.1","Magnetic keys (Pk of 10)"]

{"sheet":"Category 7","index":7,"n_rows":213,"n_cols":4,"rows_kept":213,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 7"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-07-01","Bedside Locker, Mild steel","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 343, Type 1"]
[1.2,"Material: Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.3,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"Must have a rail on both sides and Pull-out drawer"]
[1.5,"Locker mounted on 4 castors.Castors must comply with the latest issue of SANS 621"]
[1.6,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.6.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.6.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.6.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.7,"Drawer must have a rust-free, heavy-duty sliding mechanism and stopper to prevent total extraction of drawer"]
["1.7.1","The drawer sliding mechanism must have a 4-year warranty cover"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 343"]
[2.3,"SANS 778 (subsection 5.2)"]
[2.4,"SANS 417"]
[null,"Bedside Locker, Mild steel","Complies Yes/No","COMMENTS"]
["RT24-07-01a","Dedicated castors, 50mm dia (set of 4)"]
[]
["RT24-07-02","Bedside Locker, ABS plastic","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 343, Type 1, with the following exception:"]
[1.2,"Material: Durable ABS"]
[1.3,"The ABS must be resistant to physical impact, chemical corrosion,  and high thermal stress."]
[1.4,"The unit must withstand heavy-use and adverse environmental condition"]
[1.5,"Must have a rail on both sides and Pull-out drawer"]
[1.6,"Locker mounted on 4 castors.Castors must comply with the latest issue of SANS 621"]
[1.7,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.7.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.7.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.7.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.8,"Drawer must have a durable sliding mechanism and stop to prevent total extraction of drawer"]
[1.9,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 343"]
[null,"Bedside Locker, ABS Plastic","Complies Yes/No","COMMENTS"]
["RT24-07-02a","Dedicated castors, 50mm dia (set of 4)"]
[]
["RT24-07-03","Bedside Locker, HPL","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 343, Type 1"]
[1.2,"Material: High-Pressure Laminate (HPL)"]
[1.3,"The unit must withstand heavy-use and adverse environmental condition"]
[1.4,"Must have a rail and Pull-out drawer"]
[1.5,"Locker mounted on 4 castors.Castors must comply with the latest issue of SANS 621"]
[1.6,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.6.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.6.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.6.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.7,"Drawer must have a rust-free, heavy-duty sliding mechanism and stopper to prevent total extraction of drawer"]
["1.7.1","The drawer sliding mechanism must have a 4-year warranty cover"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 343"]
[2.3,"SANS 778 (subsection 5.2)"]
[2.4,"SANS 417"]
[null,"Bedside Locker, HPL","Complies Yes/No","COMMENTS"]
["RT24-07-03a","Dedicated castors, 50mm dia (set of 4)"]
[]
["RT24-07-04","Overbed Table, Wood","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be Cantilever adjustable height"]
["1.1.1","Height adjustment from ± 740 mm to 1 080 mm"]
["1.2","To comply with the latest issue of SANS 777, Type B"]
["1.3","The ratio of table support frame and table top must be no less than 2:3 length coverage"]
["1.4","Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.5","Bonded wood melamine resin surface table-top with aluminium or similar edging"]
["1.6","It must be able to lock automatically"]
["1.7","The locking mechanism for the top must be of heavy-duty and able handle 25kg"]
["1.8","It must be possible for the patient to adjust the height themselves"]
["1.9","The top of the table must have a laminated warning sticker written \"Do not lean on the table\""]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[2.2,"SANS 777"]
[null,"Overbed Table, Wood Replacement Accessories/Parts","Complies Yes/No","COMMENTS"]
["RT24-07-04a","Castors, 50mm dia (set of 4)"]
["RT24-07-04b","Height Adjustment Spring mechanism"]
["RT24-07-04c","Height Adjustment Lever"]
[]
["RT24-07-05","Overbed Table, ABS Plastic","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be Cantilever adjustable height"]
["1,1,1","Height adjustment from ± 740 mm to 1 080 mm"]
["1.2","To comply with the latest issue of SANS 777, Type B"]
["1.3","The ratio of table support frame and table top must be no less than 2:3 length coverage"]
["1.4","Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2 OR Alternative frame material: ABS plastic"]
["1.5","It must be able to lock automatically"]
["1.6","The locking mechanism for the top must be of heavy-duty and able handle 25kg"]
["1.7","The top of the table must have a laminated warning sticker written \"Do not lean on the table\""]
["1.8","It must be possible for the patient to adjust the height"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[2.2,"SANS 777"]
[null,"Overbed Table, ABS Plastic Replacement Accessories/Parts","Complies Yes/No","COMMENTS"]
["RT24-07-05a","Castors, 50mm dia (set of 4)"]
["RT24-07-05b","Height Adjustment Spring mechanism"]
["RT24-07-05c","Height Adjustment Lever"]
[]
["RT24-07-06","Overbed Table, HPL","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be Cantilever adjustable height"]
["1.1.1","Height adjustment from ± 740 mm to 1 080 mm"]
["1.2","To comply with the latest issue of SANS 777, Type B"]
["1.3","The ratio of table support frame and table top must be no less than 2:3 length coverage"]
["1.4","Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.5","High pressure laminate table-top with smooth edging"]
["1.6","It must be able to lock automatically"]
["1.7","The locking mechanism for the top must be of heavy-duty and able handle 25kg"]
["1.8","It must be possible for the patient to adjust the height themselves"]
["1.9","The top of the table must have a laminated warning sticker written \"Do not lean on the table\""]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[2.2,"SANS 777"]
[null,"Overbed Table, HPL Replacement Accessories/Parts","Complies Yes/No","COMMENTS"]
["RT24-07-06a","Castors, 50mm dia (set of 4)"]
["RT24-07-06b","Height Adjustment Spring mechanism"]
["RT24-07-06c","Height Adjustment Lever"]
[]
["RT24-07-07","Overbed Table, HPL with tilting top","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be Cantilever adjustable height"]
["1.1.1","Height adjustment from ± 740 mm to 1 080 mm"]
["1.2","To comply with the latest issue of SANS 777, Type B"]
["1.3","Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.4","The ratio of table support frame and table top must be no less than 2:3 length coverage"]
["1.5","High pressure laminate table-top with smooth edging and top must tilt to provide reading & writing surface area"]
["1.6","It must be able to lock automatically"]
["1.7","The locking mechanism for the top must be of heavy-duty and able handle 25kg"]
["1.8","It must be possible for the patient to adjust the height themselves"]
["1.9","The top of the table must have a laminated warning sticker written \"Do not lean on the table\""]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[2.2,"SANS 777"]
[null,"Overbed Table, HPL Replacement Accessories/Parts","Complies Yes/No","COMMENTS"]
["RT24-07-07a","Castors, 50mm dia (set of 4)"]
["RT24-07-07b","Height Adjustment Spring mechanism"]
["RT24-07-07c","Height Adjustment Lever"]
[]
["RT24-07-08","Utility Table, 810mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications in Appendix P, Type B, see attached"]
[1.2,"Stainless steel table-top, without bottom shelf"]
[1.3,"Stainless steel must comply wit the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"The table must have rounded edges and corners"]
[1.5,"Size: ± 810 mm x  ±810 mm"]
[1.6,"Height: 900 mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
[null,"Utility Table Replacement Accessories","Complies Yes/No","COMMENTS"]
["RT24-07-08a","Adjustable Footpiece (set of 4)"]
["RT24-07-09","Utility Table, 1 720 mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications in Appendix P, Type B, see attached"]
[1.2,"Stainless steel table-top, without bottom shelf"]
[1.3,"Stainless steel must comply wit the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"The table must have rounded edges and corners"]
[1.5,"Size: ± 1 720 mm x  ±810 mm"]
[1.6,"Height: 900 mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
[null,"Utility Table Replacement Accessories","Complies Yes/No","COMMENTS"]
["RT24-07-09a","Adjustable Footpiece (set of 4)"]
[]
["RT24-07-10","Utility Table, with castors, 1 720 mm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications in Appendix P, Type B, see attached"]
[1.2,"Stainless steel table-top, without bottom shelf"]
[1.3,"Stainless steel must comply wit the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"The table must have rounded edges and corners"]
[1.5,"Size: ± 1 720 mm x  ±810 mm"]
[1.6,"Height: 900 mm"]
[1.7,"The unit must be supplied with heavy duty castors and at least two of them with brakes"]
[1.8,"Castors must comply to the latest issue of SANS 621"]
[1.9,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.9.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.9.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.9.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
[2.2,"SANS 621"]
[null,"Utility Table Replacement Accessories","Complies Yes/No","COMMENTS"]
["RT24-07-10a","Castors (set of 4)"]
["RT24-07-11","Mayo Table","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The table must have foot lever height adjustable table top using hydraulic pump"]
[1.2,"Constructed entirely of stainless steel"]
[1.3,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"Dimensions (Table top):"]
[null,"Length: 700mm +50mm"]
[null,"Width: 450mm +50mm"]
[null,"Dimensions (Height): 850mm - 1100mm (+50mm)"]
[null,"The table top must be capable of carrying a minimum load capacity of 20kg"]
[null,"The table must be fitted with four antistatic castors and at least 2 castors with brakes"]
[1.11,"Castors must comply to the latest issue of SANS 621"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.12.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.12.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 417"]
[2.2,"SANS 621"]
[null,"Mayo Table","Complies Yes/No","COMMENTS"]
["RT24-07-11a","Castors (set of 2)"]
["RT24-07-11b","Height Adjustment Foot lever "]
["RT24-07-11c","Hydraulic pump"]

{"sheet":"Category 8","index":8,"n_rows":403,"n_cols":4,"rows_kept":403,"merged":[[0,0,0,3],[2,0,2,3],[5,1,5,3],[6,1,6,3],[7,1,7,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[75,1,75,3],[76,1,76,3],[77,1,77,3],[99,1,99,3],[100,1,100,3],[101,1,101,3],[122,1,122,3],[123,1,123,3],[124,1,124,3],[152,1,152,3],[153,1,153,3],[154,1,154,3],[180,1,180,3],[181,1,181,3],[182,1,182,3],[218,1,218,3],[219,1,219,3],[220,1,220,3],[253,1,253,3],[254,1,254,3],[255,1,255,3],[286,1,286,3],[287,1,287,3],[288,1,288,3],[368,1,368,3],[369,1,369,3],[370,1,370,3],[387,1,387,3],[388,1,388,3],[389,1,389,3]]}
["CATEGORY 8"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-08-01","Scale, Electronic, Infant","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 3, see attached"]
[1.2,"The unit must be able to handle 1 month to 36 months"]
[1.3,"It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[1.4,"Automatic switch off when not in use"]
[1.5,"Weighing capacity of at least 35 kg"]
[1.6,"Increments: 10g up to 10kg, 20g > 10kg"]
[1.7,"LCD display: digits at least 20 mm high"]
[1.8,"Electronic damper"]
[1.9,"Hold feature to retain weight reading"]
[{"v":1.1,"d":"1.10"},"Function to display breast milk intake"]
[1.11,"Carry bag:"]
["1.11.1","Must be of durable nylon with zipper and carrying strap"]
["1.11.2","Must be compatible with the scale itself"]
[1.12,"The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
[2.1,"AC adapter with 3 pin plug compatibility"]
[2.2,"Rechargeable battery"]
[3,"Warranty & Maintenance"]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[5,"Optional Accessories:"]
[5.1,"Carry bag "]
[null,"Scale, Electronic, Infant Replacements","Complies Yes/No","COMMENTS"]
["RT24-08-01a","AC adapter with 3 pin plug compatibility"]
["RT24-08-01b","Rechargeable battery"]
["RT24-08-01c","Carry bag "]
[]
["RT24-08-02","Scale, Electronic, Neonatal","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 3, see attached"]
[1.2,"It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[1.3,"Automatic switch off when not in use"]
[1.4,"Weighing capacity up to 20 kg"]
[1.5,"Increments:1g up to 5kg,  5g > 5kg"]
[1.6,"Electronic damper"]
[1.7,"Hold feature to retain weight reading"]
[1.8,"Function to display breast milk intake"]
[2,"Standard Accessories:"]
[2.1,"AC adapter with 3 pin plug compatibility"]
[2.2,"Rechargeable battery"]
[3,"Warranty & Maintenance"]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[5,"Optional Accessories:"]
[5.1,"Carry bag "]
[null,"Scale, Electronic, Neonatal Replacements","Complies Yes/No","COMMENTS"]
["RT24-08-02a","AC adapter with 3 pin plug compatibility"]
["RT24-08-02b","Rechargeable battery"]
["RT24-08-02c","Carry bag "]
[]
["RT24-08-03","Scale, Analog, Neonatal","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 2, see attached"]
[1.2,"Weighing capacity: 20 kg"]
[1.3,"The unit must have visible dial display"]
[1.4,"Spring lever mechanism with vanadium steel spring"]
[1.5,"Heavy, hardened steel pivots and bearing"]
[1.6,"The unit to have zeroing or calibration dial"]
[1.7,"Scale must be of robust construnction"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be quoted for, as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[null,"Scale, Analog, Neonatal Replacement","Complies Yes/No","COMMENTS"]
["RT24-08-03a","Carry bag "]
[]
["RT24-08-04","Scale, Analog, Bathroom type","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 3, see attached"]
[1.2,"Weighing capacity: 150 kg at least"]
[1.3,"The unit must have Large dial display"]
[1.4,"Spring lever mechanism with vanadium steel spring"]
[1.5,"Heavy, hardened steel pivots and bearing"]
[1.6,"Scale must be of robust construnction"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[null,"Scale, Analog, Bathroom type Replacement ","Complies Yes/No","COMMENTS"]
["RT24-08-04a","Rubber Adjustable footpiece (set of 4)"]
[]
["RT24-08-05","Scale, Electronic, Bathroom type","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 3, see attached"]
[1.2,"It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[1.3,"Capacity: at least 150 kg"]
[1.4,"Battery operated and it must be rechargeable"]
[1.5,"Large LCD display with hold function"]
[1.6,"Automatic switch-off"]
[1.7,"Mother/child function to determine mass of a child held by an adult"]
[1.8,"Scale must be of robust construction"]
[2,"Standard Accessories:"]
[2.2,"AC adapter with 3 pin plug compatibility"]
[2.3,"Rechargeable battery"]
[3,"Warranty & Maintenance"]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
["RT24-08-05","Scale, Electronic, Bathroom type Replacements","Complies Yes/No","Comments"]
["RT24-08-05a","AC adapter with 3 pin plug compatibility"]
["RT24-08-05b","Rechargeable battery"]
["RT24-08-05c","Rubber Adjustable footpiece (set of 4)"]
[]
["RT24-08-06","Scale, Analog, with height rod","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
["1.1","To comply with the specifications on Appendix H, Type 2, see attached"]
["1.2","Capacity: at least 150 kg"]
["1.3","Dial to be at least 150 mm in diameter"]
["1.4","Must include height measuring rod"]
["1.5","The markings on the rod must be etched, permanent and long lasting for the life of the scale"]
["1.6","Scale to be able to tilt for moving"]
["1.6.1","Mounted on castors and activate when tilted, roller size: 30 - 50 mm"]
["1.7","Scale must be of robust construction"]
["1.8","Fixed direction rod for height measurements"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[null,"Scale, Analog, with height rod Replacements","Complies Yes/No","Comments"]
["RT24-08-06a","Rubber Adjustable footpiece (set of 4)"]
["RT24-08-06b","Height Measuring Rod"]
["RT24-08-06c","Castors, 30-50mm (set of 2)"]
[]
["RT24-08-07","Scale, Electronic, Height & Weight","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To comply with the specifications on Appendix H, Type 3, see attached"]
[1.2,"The unit must measure both height and weight electronically"]
[1.3,"Capacity: at least 150 kg"]
[1.4,"The height and weight values must be displayed in two different LCD"]
[1.5,"Must include height measuring rod with long lasting markings, etched"]
[1.6,"Height measuring range of 110 - 200cm"]
[1.7,"The following functions must be possible:"]
["1.7.1","Auto BMI"]
["1.7.2","TARE"]
["1.7.3","Hold"]
["1.8","Scale to be able to tilt for moving"]
["1.8.1","Mounted on castors, roller size: 30 - 50 mm"]
["1.9","Scale must be of robust construction"]
["1.10","Fixed direction for height rod"]
["1.11","It must automatically calculate BMI of the patient"]
["1.12","It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[2.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["2.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries, Flow sensors and Oxygen sensor), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[null,"Scale, Electroni, with height rod Replacements","Complies Yes/No","Comments"]
["RT24-08-07a","Rubber Adjustable footpiece (set of 4)"]
["RT24-08-07b","Height Measuring Rod"]
["RT24-08-07c","Castors, 30-50mm (set of 2)"]
["RT24-08-07d","Battery"]
[]
["RT24-08-08","Scale, Electronic, Mutifunctional Use","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
["1.1","The scale must serve as a multifunctional use allowing weighing in standing, seated and wheelchair platform"]
["1.2","The unit must have powder coated heavy-duty steel base frame"]
["1.3","The unit must have a seating platform that can be folded out of the away when not required"]
["1.4","Capacity: at least 300 kg"]
["1.5","The weight values must be displayed in LCD display"]
["1.6","Must include handrails on the sides and additional fron rail to ensure safety, stability and extra support"]
["1.7","The unit shall have ramp for wheelchair accessibility and weighing function that will take wheelchair weight into consideration. Bidder to demonstrate"]
["1.8","The following functions must be possible:"]
["1.8.1","BMI"]
["1.8.2","TARE"]
["1.8.3","Hold"]
["1.8.4","Pre-TARE"]
["1.8.5","Auto-Hold"]
["1.9","The wheelchair ramp shall form part of the base and both coated with non-slip rubber surface"]
["1.10","The unit shall have castors which will be activated when transported"]
["1.11","The unit must be wide enough to accommodate large size wheelchair without touching handrails"]
["1.11.1","No less than 900mm wide and 950mm depth"]
["1.12","It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[2.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["2.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries, Flow sensors and Oxygen sensor), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[]
["RT24-08-09"," Chair Scale, Electronic","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
["1.1","The scale must serve as weighing in seated position"]
["1.2","The unit must have powder coated heavy-duty steel base frame with hard plastic seat pan"]
["1.3","The unit must have rear lockable castor, front directional castors and adjustable foot support platform"]
["1.4","Capacity: at least 200 kg"]
["1.5","The weight values must be displayed in LCD display"]
["1.6","Must include foldable armrest on the sides and push handles "]
["1.8","The following functions must be possible:"]
["1.8.1","BMI"]
["1.8.2","TARE"]
["1.8.3","Hold"]
["1.8.4","Pre-TARE"]
["1.8.5","Auto-Hold"]
["1.9","Dimensions (WxDxH):"]
["1.9.1","Seating; 460 x 460 x 460mm"]
["1.9.2","Overall; 560 x 850 x 900"]
["1.10","It must be dual power unit; AC adapter or built-in power supply and battery operated"]
[2,"Warranty & Maintenance"]
[2.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["2.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[2.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["2.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Batteries, Flow sensors and Oxygen sensor), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["3.2.1","Please provide unique ref number of the ceriticate:"]
[]
["RT24-08-10","Scale, Pharmacy","Complies Yes/No","Comments"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
["1.1","The unit must be made from robust ABS housing or metal with removable stainless steel weighing pan for cleaning"]
["1.2","It must be dual power unit; AC adapter or built-in power supply and battery operated"]
["1.3","Capacity: at least 200g to 6 kg"]
["1.4","Battery operated and it must be rechargeable"]
["1.5","High-contrast LCD or LED digital display with backlight"]
["1.6","Display must have overload and underload indicators"]
["1.7","The unit must have the following weighing functions:"]
["1.7.1","Density determination"]
["1.7.2","Unit conversion; g, mg, oz, ct, dwt"]
["1.7.3","Standard weighing in grams and milligrams"]
["1.7.4","TARE"]
["1.7.5","Zeroing"]
["1.7.6","Perentage weighing"]
["1.7.7","check-weighing with high/low limits"]
["1.8","The unit must have anti-vibration mechanism and level indicator"]
["1.9","The unit must have printing capacity"]
["1.10","Must maintain the highest accuracy in pharmacy compounding environments"]
["1.11","The unit must automatically calibrate internally"]
[2,"Standard Accessories:"]
["2.1","AC adapter with 3 pin plug compatibility"]
["2.2","Rechargeable battery"]
["2.3","Dust cover"]
["2.4","Printing paper (pk of 5)"]
["2.5","Calibration weight set"]
[3,"Warranty & Maintenance"]
["3.1","A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Batteries), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[4,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["4.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["4.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["4.2","Model on offer must comply with EU Medical Device Regulation (EU) 2017/745 or equvalent from SAHPRA recognized jurisdictions . Attach a copy of certification"]
["4.2.1","Please provide unique ref number of the ceriticate:"]
[]
["RT24-08-11","Mid upper arm circumference (MUAC) tape, Child (Pack of 100)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Tape/armband to measure upper arm circumference of children"]
[1.2,"Threads into itself through a hole at one end Arrow marks to indicate the point of measurement"]
[1.3,"PVC, flexible, not stretchable"]
[1.4,"Must be washable"]
[1.5,"Thickness: 0,5 mm"]
[1.6,"Marked in cm, accurate to 0,1 mm per 10 cm"]
[1.7,"Graduations: 1 mm"]
[1.8,"Multicolored as follows:"]
["1.8.1","Red: 0 - 11,5 cm"]
["1.8.2","Yellow/Orange: 11,5 - 12,5 cm"]
["1.8.3","Green: 12,5 - 25 cm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-08-12","Weight Estimation Tape, Reusable","Complies Yes/No","Comments"]
[1,"Technical Specification"]
[1.1,"A  length-based paediatric weight estimation tape for use in emergencies. \n"]
[1.2,"It must be easy to use with clear markings "]
[1.3,"Minimally Flexible, non stretchable material"]
[1.4,"Must be available in reusable format"]
[1.5,"Drug doses and equipment sizes must be obtained based on the weight from the colour-coded accompanying card or on the tape itself. "]
[1.6,"Must accommodate for different body habituses"]
[1.7,"It must be compact and easy to store"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-08-13","Weight Estimation Tape, Single-use (Pk of 10","Complies Yes/No","Comments"]
[1,"Technical Specification"]
[1.1,"A  length-based paediatric weight estimation tape for use in emergencies. \n"]
[1.2,"It must be easy to use with clear markings "]
[1.3,"Minimally Flexible, non stretchable material"]
[1.4,"Must be available in single-use format"]
[1.5,"Drug doses and equipment sizes must be obtained based on the weight from the colour-coded accompanying card or on the tape itself. "]
[1.6,"Must accommodate for different body habituses"]
[1.7,"It must be compact and easy to store"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-08-14","Stadiometer (Height board)","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To measure height of children and adults while standing"]
[1.2,"Range: up to 2500 mm, graduated in m, cm and mm, with numbers at metre and cm positions"]
[1.3,"Measuring surface must be free of all moving parts that may affect the markings"]
[1.4,"Movable headboard must slide easily on the vertical section and lock in the measurement position"]
[1.5,"Headboard must lock at 90° to the vertical measuring section"]
[1.6,"Locking mechanism must not affect the measuring surface"]
[1.7,"Sturdy and stable footplate"]
[1.8,"Must allow the heels, buttocks and back of the head to make contact with the vertical surface during measurement"]
[1.9,"Must be made of durable, non-flexible, smooth material that is water resistant, easy to clean, with no sharp edges or unfinished parts"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[]
["RT24-08-15","Length board/Infantometer","Complies Yes/No","COMMENTS"]
[null,"Product Offered"]
[null,"Brand:"]
[null,"Model:"]
[null,"Initial Manufacturing year of Model:"]
[1,"Technical Specification"]
[1.1,"To measure length of children under 23 months, lying down"]
[1.2,"Range: up to 1000 mm, graduated in 1 mm, with numbers at mm and cm positions"]
[1.3,"Measuring surface must be free of all moving parts that may affect the markings"]
[1.4,"Fixed headboard, rigidly attached at 90° to horizontal surface"]
[1.5,"Movable footboard must slide easily on the horizontal section and lock in the measurement position"]
[1.6,"Headboard to be at least 15 cm wide and at least 15 cm high"]
[1.7,"Zero position at headboard, length reading made by movable footboard"]
[1.8,"Footboard must slide at 90° to the horizontal measuring section"]
[1.9,"Must be made of durable, non-flexible, smooth material that is water resistant, easy to clean, with no sharp edges or unfinished parts"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]

{"sheet":"Category 9","index":9,"n_rows":74,"n_cols":4,"rows_kept":74,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 9"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-09-01","Transfer board, 80 cm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be lightweight board for easy transportability"]
["1.2","It must be able to carry atleast patient weight of 150kg"]
["1.3","The material must be of composite/ high strength plastic for easy cleaning"]
["1.4","The surface must be smooth low friction for easy sliding, antimicrobial coating, non-slip pads and foldable design"]
["1.5","The unit must be comfortable with soft core"]
["1.6","The unit must not have hard metal rollers but must have similar transfer technique"]
["1.7","Size: 80 cm x  50 cm (± 20 cm)"]
["1.8","Radiotransluscent With handles"]
["1.9","Must have round smooth edges or beveled for comfort"]
["1.10","The starter pack on initial delivery must have both reusable and disposable cover"]
["1.11","All accessories and consumables listed must be compatible with main unit on offer"]
["1.12","The following accessories must meet the above specification, be compatible and supplied with the main unit"]
[2,"Standard Accessories and Consumables:"]
["2.1","Disposable plastic cover (Pk of 100)"]
["2.2","Reusable plastic cover (Pk of 10)"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[null,"80 cm Transfer board Accessories & Consumables","Complies Yes/No","COMMENTS"]
["RT24-09-01a","Disposable plastic cover (Pk of 100)"]
["RT24-09-01b","Reusable plastic cover (Pk of 10)"]
[]
["RT24-09-02","Transfer board, 180 cm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be lightweight board for easy transportability"]
["1.2","It must be able to carry atleast patient weight of 150kg"]
["1.3","The material must be of composite/ high strength plastic for easy cleaning"]
["1.4","The surface must be smooth low friction for easy sliding, antimicrobial coating, non-slip pads and foldable design"]
["1.5","The unit must be comfortable with soft core"]
["1.6","Must have round smooth edges or beveled for comfort"]
["1.7","The unit must not have hard metal rollers but must have similar transfer technique"]
["1.8","Size: 180 cm x  50 cm (± 20 cm)"]
["1.9","Radiotransluscent With handles"]
["1.10","The starter pack on initial delivery must have both reusable and disposable cover"]
["1.11","All accessories and consumables listed must be compatible with main unit on offer"]
[2,"Standard Accessories and Consumables:"]
["2.1","Disposable plastic cover (Pk of 100)"]
["2.2","Reusable plastic cover (Pk of 10)"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[null,"180 cm Transfer board Accessories & Consumables","Complies Yes/No","COMMENTS"]
["RT24-09-02a","Disposable plastic cover (Pk of 100)"]
["RT24-09-02b","Reusable plastic cover (Pk of 10)"]
[]
[]
["RT24-09-03","Transfer Board, 180 x 70 cm","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","It must be lightweight sheet for easy transportability"]
["1.2","It must be able to carry atleast patient weight of 150kg"]
["1.3","The material must be of composite/ high strength plastic for easy cleaning"]
["1.4","The surface must be smooth low friction for easy sliding, antimicrobial coating, non-slip pads and foldable design"]
["1.5","The unit must be comfortable with soft core"]
["1.6","Must have round smooth edges or beveled for comfort"]
["1.7","The unit must not have hard metal rollers but must have similar transfer technique"]
["1.8","Size: 180 cm x  70 cm (± 20 cm)"]
["1.9","Radiotransluscent With handles"]
["1.10","The starter pack on initial delivery must have both reusable and disposable cover"]
["1.11","With roll mat and folding"]
["1.12","All accessories and consumables listed must be compatible with main unit on offer"]
[2,"Standard Accessories and Consumables:"]
["2.1","Disposable plastic cover (Pk of 100)"]
["2.2","Reusable plastic cover (Pk of 10)"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.1.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[null,"180 x 70cm Transfer board Accessories & Consumables","Complies Yes/No","COMMENTS"]
["RT24-09-03a","Disposable plastic cover (Pk of 100)"]
["RT24-09-03b","Reusable plastic cover (Pk of 10)"]

{"sheet":"Category 10","index":10,"n_rows":161,"n_cols":4,"rows_kept":161,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 10"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-10-01","Drip stand, mobile (Mild Steel), 2 IV hooks","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of CKS 179, Type B"]
[1.2,"The design and dimensions must conform to the CKS 179, fig 1(a)"]
["1.2.1","Exception: Only extension rod clamping screw made from steel will be acceptable"]
[1.3,"Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.4,"Castors must comply with the latest issue of SANS 621"]
[1.5,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.5.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.5.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.5.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[2.3,"CKS 179"]
[null,"Drip stand, mobile (Mild steel), 2 IV hooks (Type B)","Complies Yes/No","COMMENTS"]
["RT24-10-01a","Castors, 75mm (set of 4)"]
["RT24-10-01b","Extension rod"]
["RT24-10-01c","Clamp screw"]
[]
["RT24-10-02","Drip stand, mobile (Mild steel), 2 IV hooks","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1,"To comply with the latest issue of CKS 179, Type C"]
[2,"The design and dimensions must conform to the CKS 179, fig 2"]
["1.2.1","Exception: Only extension rod clamping screw made from steel will be acceptable"]
[3,"Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[4,"Castors must comply with the latest issue of SANS 621"]
[5,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
[5.1,"Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
[5.2,"Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
[5.3,"Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[6,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[6.1,"SANS 621"]
[6.2,"SANS 778"]
[6.3,"CKS 179"]
[null,"Drip stand, mobile (Mild steel), 2 IV hooks (Type C)","Complies Yes/No","COMMENTS"]
["RT24-10-02a","Castors, 75mm (set of 4)"]
["RT24-10-02b","Extension rod"]
["RT24-10-02c","Clamp screw"]
[]
["RT24-10-03","Drip stand, (Mild steel), 4 IV hooks","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of CKS 179"]
[1.2,"The design and dimensions must conform to the CKS 179, fig 1(a)"]
["1.2.1","Exception: Only extension rod clamping screw made from steel will be acceptable"]
["1.2.2","The IV extension rod must consists of 4 or more hooks"]
["1.2.3","The unit will needed without base with castors but drip rod to fit any hospital bed or clamps on ward pendants"]
[1.3,"Mild steel frame with epoxy powder-coated or nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.2,"SANS 778 (subsection 5.2)"]
[2.3,"CKS 179"]
[]
["RT24-10-04","Drip stand, mobile (Stainless steel), 2 IV hooks","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of CKS 179, Type B"]
[1.2,"The design and dimensions must conform to the CKS 179, fig 1(a)"]
[1.3,"Stainless steel, to comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"Castors must comply with the latest issue of SANS 621"]
[1.5,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.5.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.5.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.5.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.3","SANS 621"]
["2.4","CKS 179"]
[null,"Drip stand, mobile (Stainless steel), 2 IV hooks (Type B)","Complies Yes/No","COMMENTS"]
["RT24-10-04a","Castors, 75mm (set of 4)"]
["RT24-10-04b","Extension rod"]
["RT24-10-04c","Clamp screw"]
[]
["RT24-10-05","Drip stand, mobile (Stainless steel), 2 IV hooks","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","To comply with the latest issue of CKS 179, Type C"]
["1.2","The design and dimensions must conform to the CKS 179, fig 2"]
["1.3","Stainless steel, to comply with the latest issue of SANS 417, subsection 4.1.2"]
["1.4","Castors must comply with the latest issue of SANS 621"]
["1.5","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.5.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.5.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.5.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["2.3","SANS 621"]
["2.4","CKS 179"]
[null,"Drip stand, mobile (Stainless steel), 2 IV hooks (Type C)","Complies Yes/No","COMMENTS"]
["RT24-10-05a","Castors, 75mm (set of 4)"]
["RT24-10-05b","Extension rod"]
["RT24-10-05c","Clamp screw"]
[]
["RT24-10-06","Kick-about for bucket","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specification on Appendix G,  Type A, see attached"]
[1.2,"Stainless steel, with medium directional satin finish"]
[1.3,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"Castors must comply with the latest issue of SANS 621"]
[1.5,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.5.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.5.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.5.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.6,"The horizontal braces to be arranged in a flat cross formation"]
[1.7,"Bucket"]
["1.7.1","To comply with the latest issue of SANS 417, subsection 4 and 5.18, Type A"]
["1.7.2","Material: stainless steel, to comply with the latest issue of 417, subsection 4.1.2"]
["1.7.3","Capacity: 14 litre"]
["1.7.4","Rim of the bucket must to comply with SANS 417, fig 1(a)"]
["1.7.5","With standing hoop"]
["1.7.6","The bucket must be compatible with the kick-about"]
[2,"Standard Accessories"]
["2.1","Bucket "]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","SANS 417"]
["3.1.1","Please provide SANS 417 test Lab name and report number:"]
["3.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.3","SANS 621"]
[null,"Kick-about, Bucket Replacements","Complies Yes/No","COMMENTS"]
["Rt24-10-06a","Bucket, 14L"]
["Rt24-10-06b","Castors (set of 4)"]
["Rt24-10-06c","Castor fitting mechanism (into a tube/leg)"]
[]
["RT24-10-07","Kick-about for basin","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specification on Appendix G,  Type B, see attached"]
[1.2,"Stainless steel, with medium directional satin finish"]
[1.3,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.4,"Castors must comply with the latest issue of SANS 621"]
[1.5,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.5.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.5.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.5.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.6,"The horizontal braces to be arranged in a flat cross formation"]
[1.7,"Basin"]
["1.7.1","To comply with the latest issue of SANS 417, subsection 4 and 5.19, Size 1"]
["1.7.2","Top inner diameter: 330 mm  (± 6 mm)"]
["1.7.3","Height: 150 mm  (± 6 mm)"]
["1.7.4","Bottom inner diameter: 220 mm (± 6 mm)"]
["1.7.5","Rim of the flange must conform with fig 1(d) of SANS 417"]
["1.7.6","Bottom of the basin must be slightly recessed upward to ensure stability and there must be a flat between the recess and sides of the basin"]
["1.7.7","The basin must be compatible with the kick-about"]
[2,"Standard Accessories"]
["2.1","Basin"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["3.1","SANS 417"]
["3.1.1","Please provide SANS 417 test Lab name and report number:"]
["3.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["3.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
["3.3","SANS 621"]
[null,"Kick-about, Basin Replacements","Complies Yes/No","COMMENTS"]
["Rt24-10-07a","Dedicated Basin"]
["Rt24-10-07b","Castors (set of 4)"]
["Rt24-10-07c","Castor fitting mechanism (into a tube/leg)"]

{"sheet":"Category 11","index":11,"n_rows":159,"n_cols":4,"rows_kept":159,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 11"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-11-01","Stool, anaesthetist, mobile with backrest","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The unit offered must be fitted with a +580mm alloy 5-star base with an adjustable foot ring"]
[1.2,"The vinyl upholstered parts of the chair (i.e. Seat pan and backrest) must be  composed of high-density and undeformable foam pelted with bi-elastic, tear resistant, antimicrobial tissue, very easy to clean and disinfect."]
[1.3,"The chair shall be height adjustable by means of a gas spring using hand lever under the seat pan or foot lever. Bidder to state if it uses hand or foot lever"]
[1.4,"Must have Height adjustments, floor to top of seat: 550 mm to 730 mm"]
[1.5,"The seat pan shall be 420mm in dimension with a tolerance of +20mm"]
[1.6,"The backrest height measured from the seat pan shall be at least 340mm"]
[1.7,"The chair shall have tilt facility for the backrest"]
[1.8,"It shall be possible to lock the seat and backrest in a free floating position when the users need to lean forward or backwards"]
[1.9,"Castors:"]
["1.9.1","Diameter of 75 mm"]
[{"v":1.1,"d":"1.10"}," Where castors are fitted into steel tubular legs, the tube must be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.10.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.10.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.10.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[]
["RT24-11-02","Foot Stool, Double, Aluminium top","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The unit offered to be of high quality in terms of workmanship with ability to withstand specified weight capacity over time"]
[1.2,"Aluminium chequered plate top of 2mm thickness"]
[1.3,"Stainless steel edging"]
[1.4,"Dimensions (Tolerance +10mm):"]
["1.4.1","Overall height: 340mm"]
["1.4.2","First step height: 170mm"]
["1.4.3","Width: 500mm"]
["1.4.4","Overall length: 530mm"]
["1.4.5","First step length: 225mm"]
[1.5,"Weight capacity: 200kg"]
[1.6,"Legs of the stool must be fitted with high quality rubber tips or equivalent to prevent slipping"]
[1.7,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.8,"The stool must be of heavy duty construction with steel band between steps for added strength"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-03","Foot Stool, Double, Rubber top","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The unit offered to be of high quality in terms of workmanship with ability to withstand specified weight capacity over time"]
[1.2,"Steel plate top with non-slip rubber sheeting of 4mm thickness"]
[1.3,"Stainless steel edging"]
[1.4,"Dimensions (Tolerance +10mm):"]
["1.4.1","Overall height: 340mm"]
["1.4.2","First step height: 170mm"]
["1.4.3","Width: 500mm"]
["1.4.4","Overall length: 530mm"]
["1.4.5","First step length: 225mm"]
[1.5,"Weight capacity: 200kg"]
[1.6,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.7,"Legs of the stool must be fitted with rubber tips or equivalent to prevent slipping"]
[1.8,"The stool must be of heavy duty construction with steel band between steps for added strength"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-04","Foot Stool, Single, Aluminium top","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The unit offered to be of high quality in terms of workmanship with ability to withstand specified weight capacity over time"]
[1.2,"Aluminium chequered plate top of 2mm thickness with Stainless steel edging"]
[1.3,"Legs of the stool must be fitted with rubber tips or equivalent to prevent slipping"]
[1.4,"Dimensions (Tolerance +10mm):"]
["1.4.1","Height: 170mm"]
["1.4.2","Width: 500mm"]
["1.4.3","Length: 310mm"]
[1.5,"Weight capacity: 200kg"]
[1.6,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.7,"The stool must be of heavy duty construction with steel band between legs for added strength"]
[1.8,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[1.9,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-05","Foot Stool, Single, Rubber top","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The unit offered to be of high quality in terms of workmanship with ability to withstand specified weight capacity over time"]
[1.2,"Steel plate top with non-slip rubber sheeting of 4mm thickness"]
[1.3,"Stainless steel edging"]
[1.4,"Dimensions (Tolerance +10mm):"]
["1.4.1","Height: 170mm"]
["1.4.2","Width: 500mm"]
["1.4.3","Length: 310mm"]
[1.5,"Weight capacity: 200kg"]
[1.6,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.7,"Weight capacity: 200kg"]
[1.8,"Legs of the stool must be fitted with rubber tips or equivalent to prevent slipping"]
[1.9,"The stool must be of heavy duty construction with steel band between legs for added strength"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-06","Visitor Chair, hospital, Sleigh base","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The chair must have full padding to the backrest and seat pan"]
[1.2,"The chair must have comfortable arm rests"]
[1.3,"The fabric upholstered padded section of the chair must be covered or laminated with long lasting plastic"]
[1.4,"The top plastic cover must be intact and professionally fitted"]
[1.5,"The chair must be easy to clean and disinfect "]
[1.6,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.7,"The chair must be fitted non-slip mechanism"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-07","Bathroom Stool, hospital","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"To comply with the specification in Appendix K, see attached"]
[1.2,"Dimensions:"]
["1.2.1","Seat length: 450mm"]
["1.2.2","Seat width: 305mm"]
[1.3,"Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
[1.4,"Hardwood top with natural finish"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-08","Waiting-area Chair, Stainless steel , 3-seater","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The chair must have hard PU padding on the backrest and seat pan"]
["1.2","The chair must have comfortable arm rests on both ends"]
["1.3","The chair must be of heavy duty to handle daily use by patients in waiting areas;"]
["1.3.1","The cross beam must be constructed from a 2.0mm thickness steel"]
["1.3.2","There must be armrest on each end of the chair with 1.5mm thickness steel"]
["1.3.3","The chair must have solid stable legs without slipping and provided with mounting option"]
["1.4","The chair must be easy to clean and disinfect "]
["1.5","Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
["1.6","The chair must be fitted non-slip mechanism"]
["1.7","Each seat of the 3-seater must be individually mounted on the beam"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-09","Waiting-area Chair, Stainless steel , 4-seater","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The chair must have hard PU padding on the backrest and seat pan"]
["1.2","The chair must have comfortable arm rests on both ends"]
["1.3","The chair must be of heavy duty to handle daily use by patients in waiting areas;"]
["1.3.1","The cross beam must be constructed from a 2.0mm thickness steel"]
["1.3.2","There must be armrest on each end of the chair with 1.5mm thickness steel"]
["1.3.4","There must be additional legs in the middle of the cross beam to provide support (between seat 2 and seat 3)"]
["1.3.3","The chair must have solid stable legs without slipping and provided with mounting option"]
["1.4","The chair must be easy to clean and disinfect "]
["1.5","Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
["1.6","The chair must be fitted non-slip mechanism"]
["1.7","Each seat of the 4-seater must be individually mounted on the beam"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]
[]
["RT24-11-10","Waiting-area Chair, Stainless steel , 5-seater","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The chair must have hard PU padding on the backrest and seat pan"]
["1.2","The chair must have comfortable arm rests on both ends"]
["1.3","The chair must be of heavy duty to handle daily use by patients in waiting areas;"]
["1.3.1","The cross beam must be constructed from a 2.0mm thickness steel"]
["1.3.2","There must be armrest on each end of the chair with 1.5mm thickness steel"]
["1.3.3","The chair must have solid stable legs without slipping and must be provided with mounting option"]
["1.3.4","There must be additional legs in the middle of the cross beam to provide support (on seat 3)"]
["1.4","The chair must be easy to clean and disinfect "]
["1.5","Mild steel frame and legs with epoxy/nylon powder-coated finish, to comply with SANS 778 paragraph 5.2"]
["1.6","The chair must be fitted non-slip mechanism"]
["1.7","Each seat of the 5-seater must be individually mounted on the beam"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 778 (subsection 5.2)"]

{"sheet":"Category 12","index":12,"n_rows":796,"n_cols":4,"rows_kept":796,"merged":[[0,0,0,3],[2,0,2,3],[227,0,227,3],[253,0,253,3],[282,0,282,3],[308,0,308,3],[331,0,331,3],[354,0,354,3],[385,0,385,3],[409,0,409,3],[433,0,433,3],[458,0,458,3],[482,0,482,3],[502,0,502,3],[535,0,535,3],[556,0,556,3],[577,0,577,3],[607,0,607,3],[638,0,638,3],[696,0,696,3],[729,0,729,3],[746,0,746,3],[764,0,764,3],[783,0,783,3]]}
["CATEGORY 12"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-12-01","Emergency Trolley/Crash cart","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The product required is a dedicated, mobile unit able to contain all equipment which is required for the resuscitation of a patient in emergencies"]
[1.2,"The unit shall contain at least three compartments (one top and two side compartments)"]
[1.3,"One side compartment shall incorporate at least two drawers:"]
["1.3.1","i) All drawers shall be provided with dividers to be customized by the end-user"]
["1.3.2","ii) Bottom drawer must be provided with the depth of at least 150mm"]
["1.3.3","iii) Drawers shall have a stopper to prevent complete extraction of drawer"]
[1.4,"Drawers must be equiped with heavy duty sliding mechanism and to be offered with 4-year warranty"]
[1.5,"Overhead tilt bins must have maximum height of 170mm to fit consumables"]
[1.6,"The second side compartment shall be fitted with at least two rows of long plastic bins for medicine storage"]
[1.7,"The top compartment shall be fitted with moulded plastic trays for the display of ampoules and vials. The door must serve as a working surface when opened and must be supported with rubber stoppers"]
[1.8,"A tamper evident locking system on drawers shall be available with instructions for use"]
[1.9,"Adequate work space should be available on the unit for performing the necessary procedures without the use of other working surfaces."]
[{"v":1.1,"d":"1.10"},"Provision for the administration of intravenous fluid shall be provided"]
[1.11,"Must have facilities for the administration of air or oxygen"]
[1.12,"Oxygen cylinder holder"]
[1.13,"Provision shall be made for housing any make of defibrillator in a position in which the defibrillator can be used immediately without obstructing the working surface"]
[1.14,"A cardio pulmonary resuscitation board, with a storage facility shall be provided"]
[1.15,"Facilities for the attachment of a sphygmomanometer shall be available"]
[1.16,"Provision shall be available for storage of an manual resuscitators"]
[1.17,"Must have handles for easy fast maneuvering"]
[1.18,"Materials which are easily cleaned, of lasting finish and low noise generating nature, shall be used."]
[1.19,"Security of contents is required in the design"]
[{"v":1.2,"d":"1.20"},"Castors 100 mm - 125 mm diameter (four swivel, two brakes). Castors, generating LOW noise levels, shall be in accordance with SANS 621, proof of compliance must be submitted"]
[1.21,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.21.1","a. solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.21.2","b. screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.21.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.22,"Emergency trolley must be able to be transported in an ordinary standard lift"]
[1.23,"Dimensions (Tolerance 50mm):"]
["1.23.1","Height: ± 950 mm"]
["1.23.2","Width: ± 550 mm"]
["1.23.3","Length: ± 850 mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[3,"Warranty"]
["3.1","Drawer sliding mechanism: 4-year warranty"]
[null,"Emergency Trolley/Crash cart Replacement ","Complies Yes/No","COMMENTS"]
["RT24-12-01a","Dedicated castor (set 4)"]
["RT24-12-01b","Resuscitation board"]
["RT24-12-01c","Drawer dividers (set per drawer)"]
["RT24-12-01d","Drawer sliding mechanism (set of 2)"]
["RT24-12-01e","Defib support tray"]
["RT24-12-01f","Dedicated Locking key (Set of 2)"]
[]
["RT24-12-02","Emergency Paediatric Trolley","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The product required is a dedicated, mobile unit able to contain all equipment which is required for paediatric emergencies"]
[1.2,"The unit must have nine (9) Broselow colour coded drawers with dividers"]
["1.2.1","Colour coded drawers as stipulated: Cream, Pink or Red, Purple, Yellow, White, Light blue, Orange, Green, Cream"]
["1.3","Drawers must be equiped with heavy duty sliding mechanism and to be offered with 4-year warranty"]
["1.4","Drawers must have a central locking mechanism for all drawers"]
["1.5","Drawers shall have a stopper to prevent complete extraction of drawer"]
["1.6","The unit must be lightweight and easy to steer"]
["1.7","The unit must have a recessed stainless steel handle on both sided to enable easy manouvering"]
["1.8","Dimensions :"]
["1.8.1","Height: 1080mm"]
["1.8.2","Width: 700 mm"]
["1.8.3","Depth: 500 mm"]
["1.9","Provision for the administration of intravenous fluid shall be provided"]
["1.10","Must have facilities for the administration of air or oxygen"]
["1.11","Oxygen cylinder holder"]
["1.12","Provision shall be made for housing any make of defibrillator in a position in which the defibrillator can be used immediately without obstructing the working surface"]
["1.13","A cardio pulmonary resuscitation board, with a storage facility shall be provided"]
["1.14","Provision shall be available for storage of an manual resuscitators"]
["1.15","Must have handles for easy fast maneuvering"]
["1.16","Materials which are easily cleaned, of lasting finish and low noise generating nature, shall be used."]
["1.17","Must include at least 4-way multiplug with surge protection"]
["1.18","Castors 100 mm - 125 mm diameter (four swivel, two brakes). Castors, generating LOW noise levels, shall be in accordance with SANS 621, proof of compliance must be submitted"]
["1.19","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.19.1","a. solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.19.2","b. screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.19.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[3,"Warranty"]
["3.1","Drawer sliding mechanism: 4-year warranty"]
[]
["RT24-12-03","Paediatric Cart, Mild Steel","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The cabinet must be made of mild steel with Epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2 throughout"]
["1.2","The unit must have five (5) drawers with top 4 having dividers:"]
["1.2.1","First 2 drawers of +75mm height"]
["1.2.2","Next 2 drawers of +150mm height"]
["1.2.3","Last large storage bottom drawers of +220mm height with no dividers"]
["1.3","The unit must feature child friendly sea stickers as appearance"]
["1.4","Drawers must have smooth, durable sliding mechanism with stop to prevent total extraction of drawer"]
["1.5","Dimensions:"]
["1.5.1","Height: 1000 mm  (+50mm)"]
["1.5.2","Width: 700 mm"]
["1.5.3","Depth: 500 mm"]
["1.6","Drawers must have central point of locking system"]
["1.7","Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel and two braking"]
["1.8","Castors must comply wih SANS 621"]
["1.9","Castors must be antistatic"]
["1.10","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.10.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.10.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.10.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.11","Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
["2.2","SANS 778"]
[]
["RT24-12-04","Anaesthetic Cart","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The cabinet must be made of mild steel with Epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2 throughout"]
[1.2,"Front of cabinet to be divided in 2 sections"]
[1.3,"One section with 6 drawers and other section with 3 open shelves"]
[1.4,"All drawers to have a durable sliding mechanism with stop to prevent total extraction of drawer."]
[1.5,"Two drawers to have partitions"]
[1.6,"Dimensions:"]
["1.6.1","Height: 1 100 mm (+50mm)"]
["1.6.2","Length: 1 000 mm  (+50mm)"]
["1.6.3","Width: 460 mm"]
[1.7,"Top cabinet surface: stainless steel"]
[1.8,"Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[1.9,"Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel two braking"]
[{"v":1.1,"d":"1.10"},"Castors shall be in accordance with SANS 621"]
[1.11,"Castors must be antistatic"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.12.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.12.3","Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.13,"All surfaces, including welds, to be free from pits, scratches, crimps, folds, buckles and other defects"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[2.3,"SANS 417"]
[]
["RT24-12-05","Medicine Cart, Mobile (Mild steel)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The design and dimensions must comply with the latest issue of CKS 556"]
[1.2,"Hinge other than \"piano hinge\" may be used"]
[1.3,"Folding or pull-out type writing shelf"]
[1.4,"The latter must have a stopper"]
[1.5,"Folding shelf (if supplied) to be on the left hand door"]
[1.6,"Cabinet must be lockable"]
[1.7,"For security reasons regarding unauthorized duplication of keys, Lock must not have an identification code displayed"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.9,"Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[{"v":1.1,"d":"1.10"},"Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel, two braking"]
[1.11,"Castors must be antistatic"]
[1.12,"Castors shall be in accordance with SANS 621"]
[1.13,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.13.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.13.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
[1.14,"All surfaces, including welds, to be free from pits, scratches, crimps, folds, buckles and other defects"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[2.3,"CKS 556"]
[]
["RT24-12-06","Medicine Cart, ABS","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"Top surface to be flat, suitable for writting and dispensing"]
[1.2,"The unit must have Six drawers with top 4 having dividers "]
[1.3,"Two large storage bottom drawers, no dividers"]
[1.4,"Drawers must have smooth, durable sliding mechanism with stop to prevent total extraction of drawer"]
[1.5,"Dimensions:"]
["1.5.1","Height: 950 mm  (+50mm)"]
["1.5.2","Width: 750 mm"]
["1.5.3","Depth: 500 mm"]
[1.6,"Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel and two braking"]
[1.7,"Castors must comply wih SANS 621"]
[1.8,"Castors must be antistatic"]
[1.9,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.9.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.9.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.9.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[{"v":1.1,"d":"1.10"},"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[]
["RT24-12-07","Utility Cabinet, Mobile (Mild steel)","Complies Yes/No","COMMENTS"]
["1","Technical Specification"]
[1.1,"To be in accordance with Annexure H, as per drawing ME00.30.35, see attached"]
[1.2,"Material: Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.3,"Shall be constructed of 1,2mm thick mild steel sheetThe cabinet must be fitted with two pull out or swivel drawers, one on either side which must comply with SANS 343, par. 3.3.4"]
[1.4,"All drawers must have a durable sliding mechanism with stop to prevent total extraction of drawer"]
[1.5,"The four doors of the top compartment must be fitted with a door stopper mechanism (hard rubber and sunk in screws)"]
[1.6,"The doors must be fitted with durable hinges"]
[1.7,"The retractable worktop shall be constructed of 1,2 mm thick stainless steel. Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.8,"The worktop must be of rigid construction and capable of being extended (not less than 300 mm) beyond the face of the cabinet without canting"]
[1.9,"Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel and two braking"]
[{"v":1.1,"d":"1.10"},"Castors: must comply with the latest issue SANS 621"]
[1.11,"Castors must be antistic"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.12.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.12.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.13,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[2.3,"SANS 343"]
[2.4,"SANS 417"]
[]
["RT24-12-08","ICU Chart Cart, (Mild steel)","Complies Yes/No","COMMENTS"]
["1","Technical Specification"]
["1.1","The unit will be used in front of the patient's bed in ICU and High Care areas"]
["1.2","Material: Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2 combined with corrosion proof ploymer that won't dent or rust"]
["1.3","The unit must be lockable"]
["1.4","All drawers must have a durable sliding mechanism with stop to prevent total extraction of drawer"]
["1.5","The unit shall contain two (2) compartments (left and right compartment)"]
["1.5.1","Left compartment must have four (4) polymer drawers"]
["1.5.2","Right compartment will contain one drawer and one polymer door with shelf divider"]
["1.6","The unit must come with a pull out shelf located on either side of the cart"]
["1.7","The top of the cart shall be a 20o chart writing sloping top with lip bottom to keep the chart in place"]
["1.8","The unit must have file pockets/slots on the side"]
["1.9","Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel and two braking"]
["1.10","Castors: must comply with the latest issue SANS 621"]
["1.11","Castors must be antistic"]
["1.12","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.12.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.12.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.13","Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[]
["RT24-12-09","Anaesthetist Trolley, Type 3 , size C","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726 (see fig 2 and table 2)"]
[1.2," Dimension:"]
["1.2.1","Length:  455 mm (± 5 mm)"]
["1.2.2","Width: 455 mm (± 5 mm)"]
[1.3,"The upper part is enclosed to contain a drawer (with no divisions) opening to the front"]
[1.4,"Drawer must have a stopper to prevent complete removal of drawer"]
[1.5,"Durable rubber plugs (or similar noise reducing material) must be inserted into rails below removable shelves"]
[1.6,"The top shelf has a rail along sides and back"]
[1.7,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.8,"Stainless steel throughout"]
[1.9,"Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[{"v":1.1,"d":"1.10"},"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[1.11,"Castors shall be in accordance with SANS 621"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or "]
["1.12.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[null,"Anaesthetist Trolley Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-09a","Dedicated castors 75mm (set of 4)"]
[]
["RT24-12-10","Anaesthetist Trolley, ABS","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"The product required is a dedicated, mobile unit able to contain all equipment which is required by Anaesthetist in Theater"]
[1.2," Dimension:"]
["1.2.1","Height:  1050 mm (± 20 mm)"]
["1.2.2","Width: 700 mm (± 20 mm)"]
[1.3,"Depth: 500 mm (+ 20mm)"]
[null,"The cart/trolley must have at least six drawers"]
[1.4,"All drawers shall be provided with dividers to be customized by the end-user"]
[1.5,"Bottom drawer must be provided with the depth of at least 150mm"]
[1.6,"Drawers shall have a stopper to prevent complete extraction of drawer"]
[1.7,"Drawers must be equiped with heavy duty sliding mechanism and to be offered with 4-year warranty"]
[1.8,"Overhead tilt bins must have maximum height of 170mm to fit consumables"]
[1.9,"The top compartment shall be fitted with moulded plastic trays for the display of ampoules and vials. The door must serve as a working surface when opened and must be supported with rubber stoppers"]
[{"v":1.1,"d":"1.10"},"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[1.11,"Castors shall be in accordance with SANS 621"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or "]
["1.12.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[3,"Warranty"]
["3.1","Drawer sliding mechanism: 4-year warranty"]
[null,"Anaesthetist Trolley, ABS","Complies Yes/No","COMMENTS"]
["RT24-12-10a","Dedicated castors 75mm (set of 4)"]
["RT24-12-10b","Drawer dividers (set per drawer)"]
["RT24-12-10c","Drawer sliding mechanism"]
[]
["RT24-12-11","Anaesthetist Trolley, Type 5 , size B","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["1","Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726, Size B, Type 5 (see fig. 5 and table 2)"]
[1.2," Dimension:"]
["1.2.1","Length:  610 mm (± 5 mm)"]
["1.2.2","Width: 455 mm (± 5 mm)"]
[1.3,"The upper part is enclosed to contain a drawer (with no divisions) opening to the front"]
[1.4,"Drawer must have a stopper to prevent complete removal of drawer"]
[1.5,"Durable rubber plugs (or similar noise reducing material) must be inserted into rails below removable shelves"]
[1.6,"The bottom shelf has a rail along sides and back"]
[1.7,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.8,"Stainless steel throughout"]
[1.9,"Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[{"v":1.1,"d":"1.10"},"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[1.11,"Castors shall be in accordance with SANS 621"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or "]
["1.12.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[null,"Anaesthetist Trolley Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-11a","Dedicated castors 75mm (set of 4)"]
[]
["RT24-12-12","Medical Dressing Trolley, Type 4 , size A","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["1","Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726 (see fig 4)"]
[1.2,"Dimensions:"]
["1.2.1","Length: 915 mm (± 5 mm)"]
["1.2.2","Width: 455 mm (± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"It has a continuous guard rail along the sides and back of the top shelf and a continuous rail fitted around the bottom, above the bottom shelf"]
[1.6,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.7,"Stainless steel throughout"]
[1.8,"Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[1.9,"Trolley must have Four swivel castors with a diameter of 100 mm each"]
[{"v":1.1,"d":"1.10"},"Castors shall be in accordance with SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner."]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-13","Medical Dressing Trolley, Type 4 , size C","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726 (see fig 4)"]
[1.2,"Dimensions:"]
["1.2.1","Length: 455 mm (± 5mm)"]
["1.2.2","Width: 455 mm (± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"It has a continuous guard rail along the sides and back of the top shelf and a continuous rail fitted around the bottom, above the bottom shelf"]
[1.6,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.7,"Stainless steel throughout"]
[1.8,"Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
[1.9,"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[{"v":1.1,"d":"1.10"},"Castors shall be in accordance with SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner."]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-14","Medical Dressing Trolley, Type 6 , with Bucket and Bowl","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[null,"Technical Specification"]
["1.1","To comply with the latest issue of SANS 726 (see fig 6)"]
["1.2","Bowl attachment (upper bracket) to accommodate a bowl  (size 3) as per paragraphs 4 and 5.21  of SANS 417"]
["1.3"," Bucket attachment (lower bracket) to accommodate a 14 litre bucket as per paragraphs 4 and 5.18 of SANS 417"]
["1.4","The trolley is open and has two removable stainless steel shelves"]
["1.5","Durable rubber plugs (or similar noise reducing material) must be inserted into rails below removable shelves"]
["1.6","It has a continuous guard rail along the sides and back of the top shelf and a continuous rail fitted around the bottom, above the bottom shelf"]
["1.7","Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
["1.8","Stainless steel throughout"]
["1.9","Shelves to be of stainless steel"]
["1.10","Stainless steel must comply with subsection 4.1.2 of the latest issue of SANS 417"]
["1.11","Trolley must have Four swivel castors with a diameter of 75 mm each"]
["1.12","Castors shall be in accordance with SANS 621"]
["1.13","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.13.1","i) Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.13.2","ii) Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner."]
[2,"Standard Accessories: (Must be compatible and supplied with main item)"]
[2.1,"Bucket"]
[2.2,"Bowl  "]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 621"]
[3.2,"SANS 726"]
[3.3,"SANS 417"]
[null,"Medical Dressing Trolley, Type 6 , with Bucket and Bowl Replacement","Complies Yes/No","COMMENTS"]
["RT24-12-14a","14L SS Bucket"]
["RT24-12-14b","SS Bowl"]
["RT24-12-14c","Dedicated castors (set of 4)"]
[]
[]
["RT24-12-15","Medical instrument Trolley, Type 2, Size A","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["1","Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726, Type 2, Size A"]
[1.2,"Dimension: "]
["1.2.1","Length: 915 mm (± 5 mm)"]
["1.2.2","Width: 455 mm ( ± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similiar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"Must not have guard rail around the top and no guard rail on bottom, above shelf"]
[1.6,"Stainless steel with medium directional satin finish"]
[1.7,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[1.9,"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[{"v":1.1,"d":"1.10"},"Castors must comply with the latest issue of SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","b. Screwed into 35 mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.11.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-16","Medical Instrument Trolley, Type 2, Size B, without Guard Rails","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726, Type 2, Size B"]
[1.2,"Dimension: "]
["1.2.1","Length: 610 mm (± 5 mm)"]
["1.2.2","Width: 455 mm ( ± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similiar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"Must not have guard rail around the top and no guard rail on bottom, above shelf"]
[1.6,"Stainless steel with medium directional satin finish"]
[1.7,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[1.9,"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[{"v":1.1,"d":"1.10"},"Castors must comply with the latest issue of SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","b. Screwed into 35 mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.11.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-17","Medical instrument Trolley, Type 2, Size B","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["1","Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726, Type 2, Size B"]
["1.1.1","Type 2 exception: continous guard rail fitted above bottom shelf"]
[1.2,"Dimension: "]
["1.2.1","Length: 610 mm (± 5 mm)"]
["1.2.2","Width: 455 mm ( ± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similiar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"No guard rail around the top but must have a continuous rail fitted around the bottom, above the shelf"]
[1.6,"Stainless steel with medium directional satin finish"]
[1.7,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[1.9,"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[{"v":1.1,"d":"1.10"},"Castors must comply with the latest issue of SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","b. Screwed into 35 mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.11.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-18","Medical instrument Trolley, Type 2, Size C, without guard rails","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 726, Type 2, Size C"]
[1.2,"Dimension: "]
["1.2.1","Length: 455 mm (± 5 mm)"]
["1.2.2","Width: 455 mm ( ± 5 mm)"]
[1.3,"The trolley is open and has two removable stainless steel shelves"]
[1.4,"Durable rubber plugs (or similiar noise reducing material) must be inserted into rails below removable shelves"]
[1.5,"Must not have guard rail around the top and no guard rail on bottom, above shelf"]
[1.6,"Stainless steel with medium directional satin finish"]
[1.7,"Stainless steel must comply with the latest issue of SANS 417, subsection 4.1.2"]
[1.8,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, must be used"]
[1.9,"Trolley must have Four swivel castors with a diameter of 75 mm each"]
[{"v":1.1,"d":"1.10"},"Castors must comply with the latest issue of SANS 621"]
[1.11,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.11.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","b. Screwed into 35 mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.11.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 726"]
[2.3,"SANS 417"]
[]
["RT24-12-19","Utility Trolley","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"The Trolley must comply with the latest issue of CKS 242, Type B (fig 2)"]
[1.2,"Material must be Stainless steel: To comply with the latest issue of SANS 417, subsecition 4.1.2"]
[1.3,"Exception: to be supplied With loop handles and not stick handles"]
[1.4,"The trolley must have a smooth directional satin finish"]
[1.5,"The trolley must be fitted with 100 mm diameter castors"]
[1.6,"Castors must comply with the latest issue of SANS 621"]
[1.7,"Where castors are fitted into steel tubular legs, the tube must be of wall thickness not less than 2,0mm and castors must be fixed to the tube by one of the following methods:"]
["1.7.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.7.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.7.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"CKS 242"]
[2.3,"SANS 417"]
[null,"Utility Trolley","Complies Yes/No","COMMENTS"]
["RT24-12-19a","Dedicated 100mm Castors (set of 4)"]
[]
["RT24-12-20","Soiled Instruments & Linen Trolley","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","The Trolley must supplied complete with polyester linen receptacle"]
["1.2","Must comply with specifications on Annexure L, drawing ME 00.30. 03, see attached"]
["1.3","Material must be a Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.4","The shelves must be constructed of 1,2 mm stainless steel sheeting"]
["1.5","The shelves must be shaped to fit neatly between the legs of the trolley and be supported on all sides by 15 mm OD tubular rails"]
["1.6","The shelves must be free of sharp edges and shall be attached to the rails in a manner to eliminate vibrations between the shelves and the rails"]
["1.7","The necessary fittings to achieve this must be concealed"]
["1.8","The bottom shelf must extend all the way to the fifth leg as indicated in drawing ME 00.30.03 of Annexure L and shall be braced by a 15 mm OD transverse member between the other two legs forming a triangle to support the weight of the canvas receptacle"]
["1.9","The trolley must be fitted with 75 mm diameter castors"]
["1.10","Castors must comply with the latest issue of SANS 621"]
["1.11","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors must be fixed to the tube by one of the following methods: "]
["1.11.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.11.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.11.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.12","Polyester linen receptacle:"]
["1.12.1","To comply with the latest issue of SANS 896, subsection 3.6"]
["1.12.2","Receptacle to have handles as specified in subsection 3.6.1"]
["1.12.3","The draw cord and eyelets to comply with paragraphs 3.1.6 and 3.1.8 of the latest issue of  SANS 896"]
["1.12.4","Diameter:    500 mm (± 10mm)"]
["1.12.5","Height: 800 mm (± 10 mm),  including 100 mm fold over lip"]
[2,"Standard Accessories:"]
["2.1","Polyester linen receptacle"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 621"]
[3.2,"SANS 778 (subsection 5.2)"]
[null,"Soiled Instruments & Linen Trolley Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-20a","Dedicated Polyester linen receptacle"]
["RT24-12-20b","Castors (set of 4)"]
[]
[]
["RT24-12-21","Soiled linen Carrier","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"To comply with the latest issue of SANS 896, Type A"]
[1.2,"The Carrier, soiled linen must have receptacle Polyester linen"]
[1.3,"Mild steel with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.4,"The following accessories must be compatible and supplied with the main unit"]
["1.12","Polyester linen receptacle:"]
["1.12.1","To comply with the latest issue of SANS 896, subsection 3.6"]
["1.12.2","Receptacle to have handles as specified in subsection 3.6.1"]
["1.12.3","The draw cord and eyelets to comply with paragraphs 3.1.6 and 3.1.8 of the latest issue of  SANS 896"]
[2,"Standard Accessories:"]
["2.1","Polyester linen receptacle"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 778"]
[3.2,"SANS 896"]
[null,"Soiled Linen Carrier Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-21a","Dedicated Polyester linen receptacle"]
["RT24-12-21b","Castors (set of 4)"]
[]
[]
["RT24-12-22","Soiled linen Carrier, Plastic Box","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"Moulded heavy duty plastic box type"]
[1.2,"Colour of box: WHITE"]
[1.3,"Lockable hinged top/lid"]
[1.4,"Durable nylon/rubber bumper strip around the base of frame "]
[1.5,"Frame with rounded corners"]
[1.6,"Size of Box:"]
["1.6.1","Height: 800 mm     (± 20mm)"]
["1.6.2","Width:  620 mm     (± 20mm)"]
["1.6.3","Length: 910 mm     (±20- mm)"]
[1.7,"Mounted on four heavy duty castors, 75 mm diameter,  two swivel and two fixed direction"]
[1.8,"Castors must comply with the latest issue of SANS 621"]
[1.9,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.9.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.9.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.9.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[]
["RT24-12-23","Storage Cart, Linen","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","Manufactured from high quality ABS and epoxy coated steel"]
["1.2","The unit shall have heavy duty epoxy or nylon coated wire mesh drawers"]
["1.3","The unit shall contain at least five (5) drawers"]
["1.4","The unit must have interior slots for height adjustment of drawers"]
["1.5","Drawers shall precisely fit the interior slots of the cart but still allow for easy height adjustment"]
["1.6","The design must allow air curculation for linen"]
["1.7","The unit shall have stainless steel handles on both lateral sides to enable easy steering and moving"]
["1.8","The unit must be lightweight and easy to steer"]
["1.9","The unit must be offered in shades of cream, white and grey colours"]
["1.10","The design must incorporate a full lockable roll front door"]
["1.11","Dimensions:"]
["1.11.1","Height: 1780 mm     (± 20mm)"]
["1.11.2","Width:  650 mm     (± 40mm)"]
["1.11.3","Depth: 630 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, fitted with braking system"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
[null,"Storage Cart, Linen Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-23a","Dedicated castors (set of 4)"]
[]
["RT24-12-24","Storage Cart, Consumables & Sterile supplies, Large","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","Manufactured from high quality ABS and epoxy coated steel"]
["1.2","The design of the unit must have impact resistant, clear see-through, heavy-duty and solid acrylic drawers"]
["1.3","The unit shall contain at least eight (8) drawers, each supplied with interchangeable dividers"]
["1.4","Drawers must be flat, smooth and easy to clean and disinfect surface. No mesh or holes will be considered"]
["1.5","Drawers shall precisely fit the interior slots of the cart but still allow for easy height adjustment"]
["1.6","The design must allow air curculation for linen"]
["1.7","The unit shall have stainless steel handles on both lateral sides to enable easy steering and moving"]
["1.8","The unit must be lightweight and easy to steer"]
["1.9","The unit ust be offered in shades of cream, white and grey colours"]
["1.10","The design must incorporate a full lockable roll front door"]
["1.11","Dimensions:"]
["1.11.1","Height: 1780 mm     (± 20mm)"]
["1.11.2","Width:  650 mm     (± 40mm)"]
["1.11.3","Depth: 630 mm     (±20 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, fitted with braking system"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
[null,"Storage Cart, Consumables & Sterile supplies Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-24a","Drawer dividers (set per drawer)"]
["RT24-12-24b","Castors (set of 4)"]
[]
["RT24-12-25","Storage Cart, Consumables & Sterile supplies, Small","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","Manufactured from high quality ABS and epoxy coated steel"]
["1.2","The design of the unit must have impact resistant, clear see-through, heavy-duty and solid acrylic drawers"]
["1.3","The unit shall contain at least four (4) drawers, each supplied with interchangeable dividers"]
["1.4","Drawers must be flat, smooth and easy to clean and disinfect surface. No mesh or holes will be considered"]
["1.5","Drawers shall precisely fit the interior slots of the cart but still allow for easy height adjustment"]
["1.6","The design must allow air curculation for linen"]
["1.7","The unit shall have stainless steel handles on both lateral sides to enable easy steering and moving"]
["1.8","The unit must be lightweight and easy to steer"]
["1.9","The unit ust be offered in shades of cream, white and grey colours"]
["1.10","The design must incorporate a full lockable roll front door"]
["1.11","Dimensions:"]
["1.11.1","Height: 900 mm     (± 40mm)"]
["1.11.2","Width:  650 mm     (± 50mm)"]
["1.11.3","Depth: 560 mm     (±40 mm)"]
["1.12","Durable nylon/rubber bumper strip around the base of frame "]
["1.13","Mounted on four heavy duty castors, 125 mm diameter, fitted with braking system"]
["1.14","Castors must comply with the latest issue of SANS 621"]
["1.15","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.15.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.15.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.15.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.16","Materials which are easily cleaned, disinfect, of lasting finish and low noise generating nature, shall be used."]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 621"]
[null,"Storage Cart, Consumables & Sterile supplies Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-25a","Drawer dividers (set per drawer)"]
["RT24-12-25b","Castors (set of 4)"]
[]
["RT24-12-26","Sterile Pack Cabinet","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The cabinet shall be constructed of 1,2 mm thick mild steel sheet and shall be mounted on, and attached to a 32 mm x 32 mm x 5 mm inverted angle iron base"]
[1.2,"Dimensions (Tolerance +20mm):"]
["1.2.1","Height: 1220 mm "]
["1.2.2","Length: 870 mm"]
["1.2.3","Width: 405 mm"]
[1.3,"The cabinet must have push handle on the side"]
[1.4,"The corners of the base shall be fitted with gussets to provide additional support for the mild steel tubular legs with 32 mm outside diameter x 1,6 mm thickness"]
[1.5,"The cabinet shall be provided with two adjustable mild steel shelves of rigid construction and glass doors"]
[1.6,"The doors shall be flush fitting, suspended on chromium-plated butt hinges and designed to open 180°"]
[1.7,"The doors shall be of rigid construction with modern locking mechanism"]
[1.8,"The locking mechanism must be supplied with 2 keys"]
[1.9,"The design of the doors shall be such that the door fitted with the locking bars shall also lock the adjacent door  Mounted on 4 heavy duty swivel castors 125 mm diameter, two swivel and two braking"]
[{"v":1.1,"d":"1.10"},"Castors must comply wih SANS 621"]
[1.11,"Castors must be antistatic"]
[1.12,"Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.12.1","Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.12.2","Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.12.3","Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
[1.13,"Materials which are easily cleaned and of lasting finish, and low noise generating nature, shall be used"]
[1.14,"Epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.15,"The cabinet must be fit for purpose"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[]
["RT24-12-27","Bin Carrier","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1","Bin for soaking purposes"]
["1.2","The frame must be designed to allow easy access to the tap, effective drainage and removal of the bin"]
["1.3","Foot pedal operated plastic lid secured to frame"]
["1.4","Tubular steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
["1.5","Size of Box:"]
["1.5.1","Height  : 960 mm (±10 mm)"]
["1.5.2","Width   : 400 mm (±10 mm)"]
["1.5.3","Length : 600 mm (±10 mm)"]
["1.6","Bin:"]
["1.6.1","Removable with drainage tap (to fit carrier)"]
["1.6.2","Made from heat resistant nylon/plastic"]
["1.6.3","Bin must have handles"]
["1.6.4","Capacity : ± 85 litre (tolerance of 5 litres)"]
["1.7","Mounted on four heavy duty castors, 75 mm diameter,  two swivel and two fixed direction"]
["1.8","Castors must comply with the latest issue of SANS 621"]
["1.9","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be fixed to the tube by one of the following methods:"]
["1.9.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.9.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.9.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.10","The following standard accessories must be compatible and supplied with the main unit"]
[2,"Standard Accessories:"]
["2.1","Bin, with a drainage tap"]
[3,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[3.1,"SANS 778 (subsection 5.2)"]
[null,"Bin Carrier","Complies Yes/No","COMMENTS"]
["RT24-12-27a","Dedicated Bin with drainage tap"]
["RT24-12-27b","Dedicated Bin without drainage tap"]
["RT24-12-27c","Castors (set of 4)"]
["RT24-12-27d","Bin lid"]
[]
["RT24-12-28","Gas cylinder Trolley, 180 mm","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"Must be able fit 180 mm diameter cylinder"]
[1.2,"To comply with the latest issue of SANS 895"]
[1.3,"The general design and overall dimensions shall be as shown in figure 1 of SANS 895"]
[1.4,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.5,"Castors must comply with the latest issue of SANS 621"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778"]
[2.3,"SANS 895"]
[null,"Gas cylinder Trolley Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-28a","Dedicated 150mm castors (set of 2)"]
["RT24-12-28b","Dedicated 75mm castors (set of 2)"]
["RT24-12-28c","Cylinder position locking mechanism"]
[]
["RT24-12-29","Gas cylinder Trolley, 300 mm","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1,"Must be able fit 300 mm diameter cylinder"]
[1.2,"To comply with the latest issue of SANS 895, with the following exception in dimensions:"]
[1.3,"To accommodate gas cylinder of 300 mm diameter and Length of 1 300 mm"]
[1.4,"The general design shall be as shown in figure 1 of SANS 895"]
[1.5,"Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.6,"Castors must comply with the latest issue of SANS 621"]
[7,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778"]
[2.3,"SANS 895"]
[null,"Gas cylinder Trolley Replacements","Complies Yes/No","COMMENTS"]
["RT24-12-29a","Dedicated 150mm castors (set of 2)"]
["RT24-12-29b","Dedicated 75mm castors (set of 2)"]
["RT24-12-29c","Cylider position locking mechanism"]
[]
["RT24-12-30","Gas cylinder Trolley, Upright Type","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
[1.1," Material: Mild steel frame with epoxy/nylon powder-coated finish to comply with SANS 778 paragraph 5.2"]
[1.2,"Dimensions:"]
["1.2.1","Base diameter must be 540 mm"]
["1.2.2","Overall height must be 670 mm"]
[1.3," Castors:"]
["1.3.1","Trolley must have 4  swivel castors with diameter of 75 mm"]
["1.3.2","Castors must comply with the latest issue of SANS 621"]
["1.4","Where castors are fitted into steel tubular legs, the tube shall be of wall thickness not less than 2,0mm and castors shall be welded to the tube by one of the following methods: "]
["1.4.1","a. Solid plug (long) complying with SANS 621 subsection 3.5.6 or"]
["1.4.2","b. Screwed into 35mm long sleeves welded into the tubular members and locked in an acceptable manner"]
["1.4.3","c. Rubber or plastic expanding sleeves for fitting castors are not acceptable"]
["1.5","The stand must fit cylinder diameter from 140mm up to 180mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 778 (subsection 5.2)"]
[]
["RT24-12-31","Folding Nose Trolley","Complies Yes/No","COMMENTS"]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
[1,"Technical Specification"]
["1.1"," Material: High quality steel frame with epoxy/nylon powder-coated finish or smooth polished"]
["1.2","Maximum loading capacity of atleast 200kg"]
["1.3","Handle must have angled designed for better handling"]
["1.4","Nose folds up for storage and unloaded transportation"]
["1.5","Dimensions:"]
["1.5.1","Nose Length must be 600mm"]
["1.5.2","Width of at least 600mm"]
["1.5.3","Overall height must be 1150 mm"]
["1.6","Trolley must have 2  heavy-duty rubber castors with diameter of 200mm"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 778 (subsection 5.2) if applicable"]

{"sheet":"Category 13","index":13,"n_rows":74,"n_cols":4,"rows_kept":74,"merged":[[0,0,0,3],[2,0,2,3]]}
["CATEGORY 13"]
[]
["All items being tendered for must comply with the following specification, failure to comply with any of the conditions set out below may result in immediate disqualification. Please note that where the specification calls for certification this certification must accompany the bid, failure to provide such certification will result in immediate disqualification. Bidders must give details of items being tendered for in the COMMENTS section where there are variation for further deliberation"]
["RT24-13-01","Ferrous Metal Detector (MRI Entrance)","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
["1.1","The must be mountable around the door entrance and plug-n-play on wall power socket"]
["1.2","The unit must have both audible and visual alarms when threat is detected"]
["1.3","The unit must be able to differentiate ferrous and non-ferrous metal;"]
["1.3.1","Alarm when metal is detected"]
["1.4","The unit must have separate screen to log and report incidents;"]
["1.4.1","Data storage for a lengthy period in order to generate weekly or monthly reports is a requirement"]
["1.5","The unit must have different sensors to locate the ferrous metal position and flashing of corresponding LED when detected"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
[2.1,"SANS 621"]
[2.2,"SANS 417"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["RT24-13-02","Burns Treatment Bath, Height-adjustable","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The bath tub must constructed with materials which are easily cleaned, disinfect and of lasting finish"]
[1.7,"Material: stainless steel 316 with high chemical-resistant properties"]
[1.2,"The unit must support a maximum patient weight of at least 180kg"]
[1.3,"Electrical height adjustable using a press-n-hold switch"]
[1.4,"The unit must be offered with temperature control and display"]
[1.5,"The unit must have a safe working load (SWL) of at least 500kg"]
[1.9,"Dimensions:"]
["1.9.1","Length: 2200mm "]
["1.9.2","Width: 800mm"]
["1.9.3","Height: 850 - 1300 mm"]
[{"v":1.1,"d":"1.10"},"The dimensions shall be subject to a tolerance of ± 50 mm. Normal mill tolerances shall apply"]
[1.11,"Must be fitted with flexible water spray arm long enough to reach the head of the bath"]
[1.12,"The unit must be fitted with mechanism to prevent overflow"]
[1.13,"The unit must be able to operate at minimum water pressure of 100kpa"]
[1.14,"The unit must be able to empty the water within 10 mins"]
[1.15,"The unit must remain stable when lifted at its maximum capacity"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]
["RT24-13-03","Burns Treatment Bath, Stationary","Complies Yes/No","COMMENTS"]
[1,"Technical Specification"]
[1.1,"The bath tub must constructed with materials which are easily cleaned, disinfect and of lasting finish"]
[1.7,"Material: stainless steel 316 with high chemical-resistant properties"]
[1.2,"The unit must support a maximum patient weight of at least 180kg"]
[1.4,"The unit must be offered with temperature control and display"]
[1.5,"The unit must have a safe working load (SWL) of at least 500kg"]
[1.9,"Dimensions:"]
["1.9.1","Length: 2200mm "]
["1.9.2","Width: 800mm"]
[{"v":1.1,"d":"1.10"},"The dimensions shall be subject to a tolerance of ± 50 mm. Normal mill tolerances shall apply"]
[1.11,"Must be fitted with flexible water spray arm long enough to reach the head of the bath"]
[null,"The unit must be fitted with mechanism to prevent overflow"]
[1.12,"The unit must be able to operate at minimum water pressure of 100kpa"]
[1.14,"The unit must be able to empty the water within 10 mins"]
[null,"The unit must remain stable when lifted at its maximum capacity"]
[2,"Conformity Compliance (Please attach proof of compliance/Certificate)"]
["2.1","SANS 417"]
["2.1.1","Please provide SANS 417 test Lab name and report number:"]
["2.2","OEM must comply and certified on ISO 13485  quality standards, attach proof of compliance"]
["2.2.1","Please provide unique ref number of the ISO 13485 ceriticate:"]
[3,"WARRANTY & MAINTENANCE "]
[3.1,"A 2-year warranty inclusive maintenance and service (Year 1 to Year 2) should be as per the SCC document"]
["3.1.1","THIS ENTAILS: A 2-year warranty against poor workmanship and latent defects and parts. This must be all inclusive and include, BUT NOT LIMITED TO, amongst others, ALL PARTS (including Hydraulic cylinder), Labour, Traveling and Accommodation. The 2-year warranty must also include all quality check, quality assurance requirements, Preventative Maintenance/Calibrations, Software updates and upgrades to be included.\nThis 2-year warranty will commence after formal Commissioning and handover of the equipment."]
[3.2,"A 5-year Comprehensive extended warranty (Year 3 to Year 7) must be quoted for, as per the SCC document"]
["3.2.1","THIS ENTAILS: A Fully Comprehensive 5-year Preventative Maintenance/Service and Corrective Maintenance/Repair contract covering all equipment, hardware and software. This contract would cover, but not be limited to the following: ALL PARTS (including Hydraulic cylinder), labour, travelling, accommodation, service and repair. The 5-year Maintenance Plan must also include all quality check, quality assurance requirements, calibrations , Software updates and upgrades.This contract will commence after the 2-year warranty period has expired."]