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	Requested by:
	Mmamoloto

	SARS BRANCH:
	Gauteng North & Head Office
	
	
	

	Address:
	Various Offices
	
	
	

	 
	PTA 
	
	
	 

	Contact Person:
	
	
	
	 

	Contact Number:
	
	
	
	 


Request for Service: Job scope and specifications: 
		Item
	Description
	Location
	QTY

	1.
	Remove existing blinds, Supply and Install new Vertical Blinds as per below spec:
	
HO & Gauteng North & offices 
	1

	1.1
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	2
	Remove existing blinds, Supply and Install new Roller Blinds as per below spec:
	HO & Gauteng North Offices
	1

	2.1
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	3
	Remove existing blinds, Supply and Install new Horizontal Wood Blinds as per below spec.
	
HO & Gauteng North Offices
	1

	3.1
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	4
	Remove existing blinds, Supply and Install new Horizontal Aluminium Blinds as per below spec.
	
HO & Gauteng North Offices
	1
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	5
	NB. IT’S THE SERVICE PROVIDERS RESPONSIBILITY TO MAKE SURE THEY CHECK WITH THEIR SUPPLIER & CLIENT PRIOR TO INSTALLATION THAT THEY HAVE THE CORRECT SPECIFICATION.
	
	

	6
	SERVICE PROVIDERS TO SUBMIT QUOTE PER WINDOW & QUOTATION TO BE APPROVED BY FM PRIOR TO INSTALLATION AS & WHEN REQUESTED
	
	





	




	Description of services	
	
	Price value

	Remove existing blind
	
	R

	Supply and Install vertical blind
	1
	R

	Supply and Install roller blind
	1
	R

	Supply and Install basswood venetian blind
	1
	R

	Supply and Install aluminium venetian blind
	1
	R

	Repair & Maintenance on each type of blind
	1
	R

	Labour rate/during office hours 07:00-16:00 (Skilled artisan)
	1
	R

	Labour rate/after-hours/ weekend/ holiday (Skilled artisan)
	1
	R

	Labour rate/during office hours 07:00-16:00 (Assistant Artisan)
	1
	R

	Labour rate/after-hours/ weekend/ holiday (Assistant artisan)
	1
	R

	Normal call out 
	1
	R

	
	
	

	Total Vat Excl  
	R

	VAT @15%
	R

	Grand Total Incl Vat @15%
	R


Pricing Template 



Applicable Mark-Ups

	Material, Equipment hire & Sub-contracting markups allowed
	Fixed Markup percentage 

	R0 – R4999.00
	12%

	R5000 – R19,999
	10%

	R20,000 – R100,000
	7 %

	R101,000 – R499,000
	5 %














image5.png
25mm ALUMINIUM VENETIAN BLINDS
SARS CODE: W-B-05

NOTE:
MAINTENANCE SPECIFICTION. TO REPLACE EXISTING DAMAGED BLINDS ONLY.

Similar or equal to picture.

TYPE: 25mm Aluminium Venetian Blinds

DESCRIPTION:  Stove enamelled head rail and fully closed bottom rail. Ladder tapes to be polyester with rungs
spaced at 20mm. Lift cord braided polyester with cord on each ladder tape. Tilt mechanism to
be equipped with self-lubricating gear controlled by clear synthetic wand. Aluminium slats to be
Stove enamelled with a nominal thickness of 0.2mm. All components to be colour coordinated
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BLINDS

VERTICAL BLINDS
SARS CODE: W-B-01

i

NOTE:
Normal Office Windows

ing equal)
TYPE: Vertical Blinds
| ‘ COLOUR: Driftwood (Block-out)
I Il

blind system. Slats 127mm, 90mm
and 63mm. 90mm is std

Standard rail is white powder
coated aluminium. SABS awarded
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ROLLER BLINDS
SARS CODE: W-B-02

NOTE:
Permission required before order

SUPPLIER:  BLINDSDIRECT (similar or
exceeding equal)

TYPE: Roller Blinds

COLOUR: Driftwood (Block-out)

DESCRIPTION: Nylon chain controlled system
that prevents the blinds from
automatically rolling down
Also has an aluminium head
rail system for strength and
stability.




image4.png
25mm BASSWOOD VENETIAN BLINDS
SARS CODE: W-B-03 SARS CODE: W-B-04

NOT!
ONLY for Executive Block A.

NOTE:
ONLY for Executive Block A.

Similar or equal to picture. Similar or equal to picture.

TYPE: 25mm Basswood Venetian Blinds TYPE: 25mm Basswood Venetian 8linds

coLou;  Natural COLOUR: Maple

DESCRIPTION:  wooden siats DESCRIPTION: Wooden slats
Head rail is made of matching powder coated Head rail is made of matching powder coated
aluminium, head-cover is the same waod colour to aluminium, head-cover is the same wood colour to
match the siats. the bottom rail Is selid matching match the slats. the bottom rail is solid matching

wood. wood.




