{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["275kV 400kV 550kV 765kV"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"275kV 400kV 550kV 765kV","index":0,"n_rows":75,"n_cols":7,"rows_kept":75,"merged":[[2,4,2,5]],"flags":["formulas_cached_only"]}
[{"$nulls":3},"HV AIS outdoor Live Tank Circuit Breakers for Eskom Transmission"]
[]
[{"$nulls":3},"Live Tank Circuit Breakers 275 kV up to 765 kV;including Livetank DCB's 400 kV to 550 kV; SF6 gas on cylinders; Electronic controllers and Online Condition Monitoring","Please indicated with \"X\""]
[null,"Item","Maerial SAP Numbers","        Description","Offered (X)","Not Offered (X)","Unit price"]
[null,1,null,"BKR 275kV 3150A 50kA 3P 31mm/kV 110V DC, (1050kV BIL) (candle-stick design)"]
[null,2,null,"BKR 275kV 3150A 50kA 3P 31mm/kV 220V DC, (1050kV BIL) (candle-stick design)"]
[]
[null,3,null,"BKR 275kV 3150A 50kA 1P 31mm/kV 110V DC, (1050kV BIL)"]
[null,4,null,"BKR 275kV 3150A 50kA 1P 31mm/kV 220V DC, (1050kV BIL) "]
[null,5,null,"BKR 275kV 3150A 50kA 1P 31mm/kV 110V DC, (1050 BIL) with Controlled Switching Device"]
[null,6,null,"BKR 275kV 3150A 50kA 1P 31mm/kV 220V DC, (1050 BIL) with Controlled Switching Device"]
[null,7,null,"Point on Wave (POW) relay for 275kV synchronous Controlled Switching Device 110V DC/ 220V DC"]
[]
[null,8,null,"BKR 400kV 3150A 50kA 1P 31mm/kV 110V DC, (1425kV BIL) "]
[null,9,null,"BKR 400kV 3150A 50kA 1P 31mm/kV 220V DC, (1425kV BIL) "]
[null,10,null,"BKR 400kV 3150A 50kA 1P 31mm/kV 110V DC, (1425kV BIL) with Controlled Switching device"]
[null,11,null,"BKR 400kV 3150A 50kA 1P 31mm/kV 220V DC, (1425kV BIL) with Controlled Switching Device"]
[null,12,null,"BKR:LT;400 KV;4000 A;50 KA;1;110 VDC"]
[null,13,null,"BKR:LT;400 KV;4000 A;50 KA;1;220 VDC"]
[]
[null,14,null,"BKR 400kV 3150A 63kA 1P 31mm/kV 110V DC, (1425kV BIL)"]
[null,15,null,"BKR 400kV 3150A 63kA 1P 31mm/kV 220V DC, (1425kV BIL)"]
[null,16,null,"BKR 400kV 3150A 63kA 1P 31mm/kV 110V DC, (1425kV BIL) with Controlled Switching Device"]
[null,17,null,"BKR 400kV 3150A 63kA 1P 31mm/kV 220V DC, (1425kV BIL) with Controlled Switching Device"]
[null,18,null,"BKR:LT;400 KV;4000 A;63 KA;1;110 VDC"]
[null,19,null,"BKR:LT;400 KV;4000 A;63 KA;1;220 VDC"]
[null,20,null,"Point on Wave (POW) relay for 400kV synchronous Controlled Switching Device 110V DC/ 220V DC"]
[]
[null,21,null,"DCB 400kV 3150A 50kA 1P 31mm/kV 110V DC, (1425kV BIL) "]
[null,22,null,"DCB 400kV 3150A 50kA 1P 31mm/kV 220V DC, (1425kV BIL) "]
[null,23,null,"DCB 400kV 3150A 50kA 1P 31mm/kV 110V DC, (1425kV BIL) with Controlled Switching device"]
[null,24,null,"DCB 400kV 3150A 50kA 1P 31mm/kV 220V DC, (1425kV BIL) with Controlled Switching Device"]
[null,25,null,"DCB 400kV 3150A 63kA 1P 31mm/kV 110V DC, (1425kV BIL)"]
[null,26,null,"DCB 400kV 3150A 63kA 1P 31mm/kV 220V DC, (1425kV BIL)"]
[null,27,null,"DCB 400kV 3150A 63kA 1P 31mm/kV 110V DC, (1425kV BIL) with Controlled Switching Device"]
[null,28,null,"DCB 400kV 3150A 63kA 1P 31mm/kV 220V DC, (1425kV BIL) with Controlled Switching Device"]
[null,29,null,"Point on Wave (POW) relay for 400kV synchronous Controlled Switching Device 110V DC/ 220V DC"]
[]
[null,30,null,"BKR 550kV 3150A 63kA 1P 31mm/kV 110V DC, (1550kV BIL)"]
[null,31,null,"BKR 550kV 3150A 63kA 1P 31mm/kV 220V DC, (1550kV BIL)"]
[null,32,null,"BKR 550kV 3150A 63kA 1P 31mm/kV 110V DC, (1550kV BIL) with Controlled Switching Device"]
[null,33,null,"BKR 550kV 3150A 63kA 1P 31mm/kV 220V DC, (1550kV BIL) with Controlled Switching Device"]
[null,34,null,"BKR LT 550kV 3150A 63kA 1P 31mm/kV 110V DC, (1550 BIL) Generator Synchronising"]
[null,35,null,"BKR LT 550kV 3150A 63kA 1P 31mm/kV 220V DC, (1550kV BIL) Generator Synchronising"]
[]
[null,36,null,"BKR 550kV 4000A 63kA 1P 31mm/kV 110V DC, (1550kV BIL)"]
[null,37,null,"BKR 550kV 4000A 63kA 1P 31mm/kV 220V DC, (1550kV BIL)"]
[null,38,null,"BKR 550kV 4000A 63kA 1P 31mm/kV 110V DC, (1550kV BIL) with Controlled Switching Device"]
[null,39,null,"BKR 550kV 4000A 63kA 1P 31mm/kV 220V DC, (1550kV BIL) with Controlled Switching Device"]
[null,40,null,"BKR LT 550kV 4000A 63kA 1P 31mm/kV 110V DC, (1550 BIL) Generator Synchronising"]
[null,41,null,"BKR LT 550kV 4000A 63kA 1P 31mm/kV 220V DC, (1550kV BIL) Generator Synchronising"]
[null,42,null,"Point on Wave (POW) relay for 550kV synchronous Controlled Switching Device 110V DC/ 220V DC"]
[]
[null,43,null,"DCB 550kV 4000A 63kA 1P 31mm/kV 110V DC, (1550kV BIL)"]
[null,44,null,"DCB 550kV 4000A 63kA 1P 31mm/kV 220V DC, (1550kV BIL)"]
[null,45,null,"DCB 550kV 4000A 63kA 1P 31mm/kV 110V DC, (1550kV BIL) with Controlled Switching Device"]
[null,46,null,"DCB 550kV 4000A 63kA 1P 31mm/kV 220V DC, (1550kV BIL) with Controlled Switching Device"]
[null,47,null,"Point on Wave (POW) relay for 550kV synchronous Controlled Switching Device 110V DC/ 220V DC"]
[]
[null,48,null,"BKR LT 765kV 3150A 50kA 1P 31mm/kV 220V DC, (2100kV BIL) Line + Tie"]
[null,49,null,"BKR LT 765kV 3150A 50kA 1P 31mm/kV 220V DC, (2100kV BIL) other"]
[null,50,null,"BKR LT 765kV 3150A 50kA 1P 31mm/kV 220V DC, (2100kV BIL) Reactor + synchronous Controlled Switching Device"]
[null,51,null,"BKR LT 765kV 4000A 50kA 1P 31mm/kV 220V DC, (2100kV BIL) Line + Tie"]
[null,52,null,"BKR LT 765kV 4000A 50kA 1P 31mm/kV 220V DC, (2100kV BIL) other"]
[null,53,null,"BKR LT 765kV 4000A 50kA 1P 31mm/kV 220V DC, ( 2100kV BIL) Reactor + synchronous Controlled Switching Device"]
[null,54,null,"Point on Wave (POW) relay for 765kV LT circuit-breaker synchronous Controlled Switching Device 220V DC"]
[]
[null,55,null,"Electronic Online Condition Monitoring and/or Integrated Diagnostic Devices"]
[null,56,null,"GAS:340415; SF6;99.9 PCT;CYL 9 KG"]
[null,57,null,"Gas, SF6, 9KG"]
[null,58,null,"GAS: TYPE: SF6; PURITY: 99.993 PCT; CONTAINER: CYL; 20KG"]
[null,59,null,"GAS:SF6;99.9 PCT;CYL 50 KG"]
[null,60,null,"GAS:SF6;99.9 PCT;CYL 63 KG"]
[]
[{"$nulls":3},"Total "]