CIVIL, MECHANICAL AND ELECTRICAL ENGINEERING
STRUCTURAL REMEDIATION WORKS AND CONCRETE/MASONRY DIAMOND CORE DRILLING WORKS AT SENTECH’S JOHANNESBURG T97 TRANSMITTER SITE
CONDITIONS OF CONTRACT

1.
DEFINITION OF TERMS
1.1
"Contract" means a bone fide quote for the works specified in the Contract, accepted by Sentech in writing.  This Quotation accepted by Sentech in writing constitutes a binding Contract between Sentech and the Quoter and shall be deemed for all purposes to be the Contract Agreement.

1.2
"Sentech" or "Employer" means Sentech.

1.3
"Quoter" means the person or persons, partnership, firm or company who/which submits a bone fide quote for the works specified in the Contract.

1.4
"Contract Works" means all the work contracted to be done by the Contractor in terms of the Contract.

1.5
"Contractor" means the Quoter whose Quote for the Contract Works has been accepted by Sentech and includes the Contractor's legal representative, successors and assigns.

1.6
"Quoted Price" means the amount stated in the Quotation for which the Quoter offers to complete and maintain the Contract Works.

1.7
"Letter of Acceptance" means the written advice from Sentech to the successful Quoter advising him that his quote had been accepted and stating the Contract Price for which his quote had been accepted.

1.8
"Site" means the road or ground or any other place on which or over which the Contract Works are to be executed and shall include any off-loading, storage and/or stacking sites.

1.9
"Specification" means the technical specification listed in the Project Specification and included in the Contract.

1.10
"Drawings" means and includes all working drawings and/or sketches relative to the Contract that may from time to time be issued by Sentech to the Contractor.

1.11
"Practical Completion" means the date stipulated in the Contract for completion of the Contract Works on which a list or remedial items will be compiled for completion by the Contractor within an agreed specified period.

1.12
"Final Completion" means the date on which the list of remedial items compiled at Practical Completion has been completed to the satisfaction of Sentech.

2.
PAYMENT
All payment claims will be verified by Sentech’s representative before payment is effected.

Sentech Finance Department will effect payment to the Contractor thirty (30) days after receiving a statement and tax invoice, from the Contractor.

3. RETENTION MONEY

N/A

4.
RESPONSIBILITY FOR CONTRACT WORKS
The Contractor shall be responsible for the proper protection of the Contract Works and shall make good all losses, damage or injuries thereto, howsoever caused, and shall re-instate the Contract Works in all respects at his own expense up to the time of Final Completion of the Contract Works.

5.
INJURY OR DAMAGE TO PERSONS OR PROPERTY
The Contractor shall take all precautions necessary for the protection of life and property

on or about or in connection with the Contract Works as well as anywhere upon Sentech's

property until the Final Completion of the Contract Works and the Contractor shall

handover the Contract Works in a safe condition.  

The Contractor shall be deemed to have indemnified Sentech as he hereby does indemnify

it against injury or damage to any person or to any property of Sentech or of others

occurring prior to the Final Completion of the Contract Works, or occurring owing to the

Contract Works being handed over in an unsafe condition.  The Contractor further

indemnifies Sentech against all actions, suits, demands costs or expenses arising in

connection with such injury or damage referred to above, either at common law or under

the Occupational Health and Safety Act.

The Contractor shall report any and every accident occurring on the site within twenty-four

(24) hours of its occurrence and shall furnish Sentech with a written report if required.

The Contractor shall at all times supervise and exercise control over all his employees and

shall be held responsible for any damage caused by his employees to private or public

property.

All work executed on site in terms of this contract shall, over and above compliance with

the OSH Act, comply with all relevant SANS Standards and be done in accordance with

accepted good engineering practice.

6.
NOTICES TO THE CONTRACTOR
All instructions, directions and notices from Sentech/Sentech’s Representative to the Contractor and vice versa concerning the Contract, as the case may be, shall be conveyed in writing by e-mail or by hand to the Contractor.

No oral instruction, objection, claim or notice by any party to others shall affect or modify any of the terms, conditions and obligations contained in the Contract document, and none of the specifications of the Contract document shall be held to be waived or modified by reason of any act whatsoever, other than by a definitely agreed waiver or modification thereof by Sentech in writing.

7.
CONTRACT WORKS AREA
The Contractor shall confine his activities to the Contract Works site and access route to the site. 

All equipment, materials, etc. is left on the premises at the Contractors own risk.

8.
UTILITIES ON SITE
Accommodation and shower facilities are not available in the Sentech building or on site. 
Toilet facilities and hand washing facilities are available in the Sentech building, for use by the Contractor. 

No site telephone nor any other form of communication is available on site.  Contractor to provide for these facilities where necessary.

15A Electricity for the contract works is available on site. Contractor to provide any plug adapters/extension leads required.

Potable water required for drinking and the execution of the contract works is available on site. It shall be the responsibility of the contractor to provide any hosepipes and adapters required.

9.
FIRES AND ACCESS GATES
No fires shall be made on Sentech or the adjacent landowners property.

All gates on access roads to Sentech transmitter buildings shall be kept closed at all times. The contractor shall be held liable for damage, loss or injury to persons or property, resulting from non-compliance with this condition.

10.
ENCLOSURE OF THE WORKS
The Contractor shall provide, erect, alter as necessary, maintain and remove and make good on completion suitable barriers as necessary for the enclosure of dangerous portions of the works and the protection of the workmen and the general public under this and other contracts being executed simultaneously on the site (only in so far as is necessary due to work executed under this contract).

11.
CONTRACTOR'S WORKING AREA, SECURITY AND SAFETY
The Contractor's working area will be demarcated on site by Sentech.  The Contractor will

be responsible in terms of the Occupational Health and Safety Act for this area for the full

duration of the Contract and shall appoint a "Responsible Person" accordingly.  The

Contractor will be "the Employer" as defined in the OHS Act, for his working area and shall

register with the divisional inspector accordingly.

The Contractor and his sub-contractors and all their personnel shall be subject to and shall

comply with all security and safety requirements of the Employer.

Security requirements for protection of the work and tools and equipment will be the sole

responsibility of the Contractor.

Sentech shall have the right to require compliance with any specific requirements of the

Act.

The Contractor shall supply Sentech with all safety information that he may require.

12.
INSPECTIONS

Sentech/Sentech’s Representative reserves the right to inspect the works at any stage and without prior notice of inspection.

13.
CLEANING

The Contractor shall be responsible for the cleaning of all areas which he occupies or works on under this contract and clearing and removal of all rubble from the site.
The Works is to be handed over in a clean and neat state and all damage is to be repaired before handing over.

14.
CONTRACT PRICE ADJUSTMENT

The contract price shall be fixed and no adjustment shall be made for the rise and fall of prices.

15.
ASSIGNMENT AND SUB-CONTRACTS

This Contract is personal to the Contractor and the Contractor shall not assign or sub-contract all or any portion of the Contract without the prior written approval of Sentech. Notwithstanding the approval of any sub-contractor, the Contractor shall remain entirely responsible for the performance and control of such sub-Contractor.  Any assignment or sub-contract by the Contractor without the prior written approval of Sentech shall be avoidable, at the sole option of Sentech.

16.
INSURANCE

The Contractor shall effect and maintain at a minimum during the entire performance of the Contract, all necessary insurance coverage and shall be responsible for the payment of all premiums and deductions associated therewith.

17.      DEMOLITION WORK

All coring, cutting of openings and breaking out of concrete or masonry is to be carried out as a completely dust free operation.

Openings/holes in concrete/brick walls and  concrete floor slabs are to be cut by diamond core drilling with cooling/lubricating water to prevent the generation of dust.

In areas where it is not possible to execute the work dust free or control the fumes, the work area must be sealed off completely with an airtight screen.

Equipment that cannot be screened off must be fully wrapped, in dust proof material, under the guidance of Sentech personnel.

Dust will damage the electronic equipment and the contractor will be held responsible for any damage to this equipment as a result of his /her failure to comply with the requirements of this condition.

All debris from demolition operations shall be prevented from falling uncontrolled and the Contractor shall take the necessary steps to control this and prevent damage to equipment and finishes in the building.

Lubricating water shall be controlled and prevented from coming into contact with any equipment or fittings where it could cause damage.

The Contractor shall remove all debris and rubble, generated as a result of this Contract, from site and shall include for such removal in his/her pricing

The sides of circular openings cut in concrete/brick walls or concrete floor slabs may be left as cut, but the sides of square openings formed in concrete/brick walls or concrete floor slabs by the (over) coring method must be made good with non-shrink grout  to form the final opening. Disturbed and damaged floor tiles along the edges must be repaired. Openings cut in masonry walls shall be made good with non-shrink grout, and painted with three coats of approved, colour matched PVA according to the manufacturer’s specifications.

18. TRANSPORTING AND HOISTING EQUIPMENT

Sentech’s transporting and hoisting equipment is not available to the Contractor. The Contractor shall be responsible for providing whatever equipment is required for off-loading, transporting and onsite hoisting.

19. ALL-INCLUSIVE QUOTATION

The quoted prices shall make provision for all overheads, labour, supply and delivery of materials, tools, equipment, transport, accommodation, water requirements, site establishment and disestablishment, chemical toilet hire, rubbish removal, storage, etc required to carry out all the work activities.
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