{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["GAS STERILIZER"],"not_rendered":{"images":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"GAS STERILIZER","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,5],[6,0,6,5],[7,0,7,5],[8,0,8,5],[9,0,9,5],[10,0,10,5],[11,0,11,5],[12,0,12,5],[13,0,13,5],[14,0,14,5]]}
["                             ANNEXURE-A TECHNICAL SPECIFICATION"]
["THE SUPPLY, DELIVERY, INSTALLATION, COMMISSIONING AND MAINTENANCE OF  GAS STERILISER UNIT 5XL OR EQUIVALENT FOR VARIOUS INSTITUTIONS OF GAUTENG HEALTH DEPARTMENT FOR A PERIOD OF THREE YEARS"]
["Note:                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   "]
["1. Technical Compliance"]
["All equipment tendered for must score a minimum score of 4 points or higher technically compliant to qualify for consideration for an award.                             (a) All Equipment tendered must comply with all the specifications with a # weight.\n"]
["2. Scoring of the bids"]
["2a. Weight: Each specification will have a weight of 1 or a hash (#), which indicates the level of importance, as follows:   "]
["1 -  A specification with a standard level of importance that must be complied with.,"]
["# -  Indicates a specification with a essential level of importance, where the bid offer will be disqualified, if the specification is not complied with."]
["2b. Score: The Bid Evaluation Committee will assign a score of 0 or1 for each specification, which indicates the level of compliance, as follows:"]
["0 -  The specification does not  comply.     1 -  The specification is fully compliant."]
["2c. Weighted and Total Score: The score will be multiplied by the weight to give the total score for each specification and be added up. "]
["2d. The bidders must comply as follows with the specification: "]
["i. The bidders must comply with all the specifications (line items) with a # weight. "]
["ii. The bidders must obtain a minimum score of 4 points or higher out of 6 points in respect of specifications (line) with a weight of 1."]
["A","B","C","D","E","F"]
["Item no.","Tender Specification","Weight","Comply (Yes/No)","Details of Product                                           (Provide your answers in this Colum. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification)"]
[1,"GENERAL DESCRIPTION (Free Standing Gas Steriliser)"]
["1.1","Must have a maximum chamber volume of at least 220 litres",1]
["1.2","Must come with loading baskets","#"]
["1.3","Cool cycles of 38 degrees Celsius","#"]
["1.4","Warm cycle of 55 degrees Celsius","#"]
["1.5","Thermal printer to print cycle report","#"]
["1.6","Touch screen",1]
["1.7","Must have an automatic error code notification","#"]
["1.8","Must have audible and visible alarm for cycle failure","#"]
["1.9","Must have USB drive ports to export","#"]
["1.10","Should be able to store at least details of the last 60 cycles",1]
["1.11","Must have a Software controlled door","#"]
["1.12","Ethylene Oxide gas cartridge barcode scanner","#"]
["1.13","Must be able to perform chamber leak test at the beginning of each cycle","#"]
["1.14","The door should not be open when the Ethylene oxide is in the chamber","#"]
["2.","Consumables"]
["2.1","Supply at least 5 Cartridges on delivery",1]
["2.2","Must supply with at least 10 biological indicators on delivery",1]
["2.3","at least 10 Rolls of Printer paper on delivery",1]
["2.4","TOTAL WEIGHTED SCORE",6]