{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Unpriced BoQ"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Unpriced BoQ","index":0,"n_rows":219,"n_cols":6,"rows_kept":219,"merged":[[1,0,1,2]],"flags":["formulas_cached_only"]}
[]
["REHABILITATION OF ROOF OF ROSHERVILLE ROOF STRUCTURES"]
["BILL OF QUANTITIES "]
[]
["ITEM NO ","DESCRIPTION OF WORK ","UNIT","QUANTITY ","RATE ","AMOUNT "]
[]
[1,"SECTION A "]
[null,"PRELIMINARY AND GENERAL "]
[]
[null,"PRELIMINARIES"]
[]
[null,"FIXED CHARGES ITEMS"]
[]
[null,"Establish Facilities on Site"]
[]
[null,"Contractual Requirements","SUM",{"v":1,"d":"1 "}]
[]
[null,"Site Offices and Storage Sheds including temporary fencing.\t","SUM",{"v":1,"d":"1 "}]
[]
[null,"Ablution and latrine facilities\t","SUM",{"v":1,"d":"1 "}]
[]
[null,"Tools and Equipment\t","SUM",{"v":1,"d":"1 "}]
[]
[null,"Establishment of Plant on Site\t","SUM",{"v":1,"d":"1 "}]
[]
[null,"Electrical power and communications","SUM",{"v":1,"d":"1 "}]
[]
[null,"OTHER FIXED CHARGES"]
[]
[null,"Remove contractor's site establishment on completion including making good and restoring the site to the satisfaction of the Client/Engineer.","SUM",{"v":1,"d":"1 "}]
[]
[null,"TIME RELATED ITEMS"]
[]
[null,"Operate and maintain facilities on site for the duration of construction facilities for contractor"]
[]
[null,"Site Offices and Storage Sheds\t","Month",{"v":9,"d":"9 "}]
[]
[null,"Ablution and latrine facilities\t","Month",9]
[]
[null,"Tools and Equipment\t","Month",9]
[]
[null,"Water Supply\t","Month",9]
[]
[null,"Electric power and communications / cell phones etc\t","Month",9]
[]
[null,"Company/head office overhead cost.\t","Month",9]
[]
[null,"Living accomodation","Month",9]
[]
[null,"Supervision","Month",9]
[]
[null,"Quality Manangement ","Month ",9]
[]
[null,"Environmental Management ","Month ",9]
[]
[]
[null,"HEALTH AND SAFETY"]
[]
[null,"Prepare, submit and obtain approval of safety plan/file and lodge same on site.","SUM",1]
[]
[null,"Personal Protective Equipment","SUM",1]
[]
[null,"Transportation of Employees","Month",9]
[]
[]
[null,"Carried to Summary Page",{"$nulls":3},0]
[]
[2,"SECTION B "]
[null,"BMS & CONSTRUCTION SERVICE  ROOF REHANILITATION "]
[]
[null,"Alterations and Demolitions "]
[null,"Remove extisting Concrete Tiles including insulation and timber trusses Cart away to a registered dump site. ","m2",{"v":2076,"d":"2,076"},null,0]
[]
[null,"Refurbishment"]
[]
[null,"Roof truss construction as per the appoved design  roof approximately 2076 m2 overall including wall plates, trusses, jack rafters, permanent bracing and pulirns/battens at required centres. ","m2",{"v":2076,"d":"2,076"},null,0]
[]
[null,"Supply and Installation of  \"Klip-Lok Light Industrial\" galvanised troughed sheet steel including  ridge, hip flashing and roof closures fixed to roof members as described complete under a five year guarantee by an approved firm of Specialists, all in accordance with the materials supplied ","m2",{"v":2076,"d":"2,076"},null,0]
[]
[null,"Supply and Installation of Insulation as per Manufacturers ","m2",{"v":2076,"d":"2,076"},null,0]
[]
[null,"Supply and installation of Waterproofing ","m2",{"v":2076,"d":"2,076"},null,0]
[]
[null,"Supply and installation of Rain water goods Downpipe, gutters and accessories) to be installed on a building appromatly  2076 m2","m",527,null,0]
[]
[]
[null,"Provisional Sum  of Five hundred thousand (R500 000.00)for making good after the roof rehabilitation","sum ",1]
[]
[null,"carried to summary page ",{"$nulls":3},0]
[]
[]
[3,"SECTION C "]
[null,"CANTEEN ROOF REHABILITATION "]
[]
[null,"Alterations and Demolitions "]
[]
[null,"Remove extisting IBR Sheets  including insulation and timber trusses Cart away to a registered dump site. ","m2",{"v":2113,"d":"2,113"}]
[]
[null,"Refurbishment"]
[]
[null,"Roof truss construction as per the appoved design  roof approximately 2113 m2 overall including wall plates, trusses, jack rafters, permanent bracing and pulirns/battens at required centres. ","m2",{"v":2113,"d":"2,113"}]
[]
[null,"Supply and Installation of  \"Klip-Lok Light Industrial\" galvanised troughed sheet steel including  ridge, hip flashing and roof closures fixed to roof members as described complete under a five year guarantee by an approved firm of Specialists, all in accordance with the materials supplied. ","m2",{"v":2113,"d":"2,113"}]
[]
[null,"Supply and application of gamazine on colums, upsatnd beams and soffits of slab","m2",{"v":1800,"d":"1,800"}]
[]
[null,"Supply and Installation of Insulation as per Manufacturers  specification ","m2",{"v":2133,"d":"2,133"}]
[]
[null,"Supply and installation of Waterproofing ","m2",{"v":2133,"d":"2,133"}]
[]
[null,"Supply and installation of Rain water goods Downpipe, gutters and accessories) to be installed on a building appromatly  2133 m2","m",182]
[]
[null,"Provisional Sum of Five Hundred Thousand Rands( R500 000) for making good after the roof rehabilitation","sum",1]
[]
[]
[]
[null,"Carried to summary page",{"$nulls":3},0]
[]
[]
[4,"SECTION D "]
[null,"REHABILITATION OF T&SS BUILDING "]
[]
[null,"Alterations and Demolitions "]
[]
[null,"Remove extisting Concrete Tiles including insulation and timber trusses Cart away to a registered dump site. ","m2",{"v":2043,"d":"2,043"}]
[]
[null,"Refurbishment"]
[]
[null,"Supply and Installation of  \"Klip-Lok Light Industrial\" galvanised troughed sheet steel including  ridge, hip flashing and roof closures fixed to roof members as described complete under a five year guarantee by an approved firm of Specialists, all in accordance with the materials supplied. ","m2",{"v":2043,"d":"2,043"}]
[]
[null,"Supply and Installation of Insulation as per Manufacturers  specification ","m2",{"v":2043,"d":"2,043"}]
[]
[null,"Supply and installation of Waterproofing ","m2",{"v":2043,"d":"2,043"}]
[]
[null,"Supply and installation of Rain water goods Downpipe, gutters and accessories) to be installed on a building appromatly  2043 m2","m2",{"v":204.3,"d":"204"}]
[]
[null,"Provisional of Five Hundred Thousand Rands (R500 000.00) Sum for making good after the roof rehabilitation","Sum",1]
[]
[null,"Provisional Sum of Eight Hundrend and Twenty Thousand Rands (R820 000.00) for Strenghning Steel Trusses","Sum",1]
[]
[null,"Carried to Summary Page",{"$nulls":3},0]
[]
[null,"SECTION E"]
[null,"REHABILITATION OF RMFW01"]
[]
[null,"Alterations and Demolitions "]
[]
[null,"Remove extisting IBR Sheets including insulation and timber trusses Cart away to a registered dump site. ","m2",361]
[]
[null,"Refurbishment"]
[]
[null,"Roof truss construction as per the appoved design area  approximately 361m2 overall including wall plates, trusses, jack rafters, permanent bracing and pulirns/battens at required centres. ","m2",361]
[]
[null,"Supply and Installation of  \"Klip-Lok Light Industrial\" galvanised troughed sheet steel including  ridge, hip flashing and roof closures fixed to roof members as described complete under a five year guarantee by an approved firm of Specialists, all in accordance with the materials supplied. ","m2",361]
[]
[null,"Supply and Installation of Insulation as per Manufacturers  specification ","m2",361]
[]
[null,"Supply and installation of Waterproofing ","m2",361]
[]
[null,"Supply and installation of Rain water goods Downpipe, gutters and accessories) to be installed on a building approximatly 8000m2","m2",396]
[]
[null,"Provisional Sum of  Five Hundred Thousand Rands(R500 000) Sum for making good after the roof rehabilition ","Sum",1]
[]
[null,"Provisional Sum of Three hundred Thousand Rands( R300 000) for Strenghning Steel trusses","sum",1]
[]
[]
[null,"Carried to Summary Page",{"$nulls":3},0]
[]
[]
[null,"SECTION F"]
[null,"REHABILITATION OF TRAINING CENTRE/ BICYCLE SHOP"]
[]
[null,"Alterations and Demolitions "]
[]
[null,"Remove extisting IBR Sheets including insulation and timber trusses Cart away to a registered dump site. ","m2",{"v":3189,"d":"3,189"}]
[]
[null,"Refurbishment"]
[]
[]
[null,"Supply and Installation of  \"Klip-Lok Light Industrial\" galvanised troughed sheet steel including  ridge, hip flashing and roof closures fixed to roof members as described complete under a five year guarantee by an approved firm of Specialists, all in accordance with the materials supplied. ","m2",{"v":3189,"d":"3,189"}]
[]
[null,"Supply and Installation of Insulation as per Manufacturers  specification ","m2",{"v":3189,"d":"3,189"}]
[]
[null,"Supply and installation of Waterproofing ","m2",{"v":3189,"d":"3,189"}]
[]
[null,"Supply and installation of Rain water goods Downpipe, gutters and accessories) to be installed on a building approximatly 3189m2","M",{"v":159.45000000000002,"d":"159"}]
[]
[null,"Provisional Sum for Five Hundred Thousand Rands(R500 000) for making good after the roof rehabilitation","Sum",1]
[]
[null,"Provisional Sum  of Seven Hundred Thousand Rands ( R700 000) for Strenghning Steel trusses","sum",1]
[]
[]
[null,"Carried to Summary Page",{"$nulls":3},0]
[]
[]
[null,"SUMMARY PAGE"]
[]
[null,"Section A -Preliminaries ",{"$nulls":3},0]
[]
[null,"Section B- BMS & Construction Service",{"$nulls":3},0]
[]
[null,"Section C- Canteen",{"$nulls":3},0]
[]
[null,"Section D- T&SS",{"$nulls":3},0]
[]
[null,"Section E- RMFW01",{"$nulls":3},0]
[]
[null,"Section F- Training Centre",{"$nulls":3},0]
[]
[]
[null,"Sub-Total",{"$nulls":3},0]
[]
[null,"Contigency ",{"v":0.05,"d":"5%"},null,null,0]
[]
[null,"Sub-Total B",{"$nulls":3},0]
[]
[null,"VAT",{"v":0.15,"d":"15%"},null,null,0]
[]
[null,"Proposed Estimate",{"$nulls":3},0]