{"text_format":"3","workbook":"xlsx","n_sheets":8,"sheets":["Schedule A-P&G","Schedule B-L&R","Schedule C-Enviromental","Schedule D-OH&S","Schedule E -QA-C","Schedule F-CP BOQ","Schedule G-SED","Schedule H-Summary of schedules"],"not_rendered":{"images":2,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Schedule A-P&G","index":0,"n_rows":140,"n_cols":7,"rows_kept":140,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,9],[8,0,8,7],[12,1,13,1]]}
[{"$nulls":6},"Form No: "]
["STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":6},"Rev No: xx"]
["SHEQ MANAGEMENT SYSTEM"]
[{"$nulls":6},"Effective Date: "]
["Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
["Project/Bid Number : RW 10408567/26"]
[]
["SCHEDULE A: PRELIMINARY AND GENERAL COSTS  PALMIET SYSTEM"]
[]
["Item No.","Payment Refers","Description","Unit","Qty","Rate","Amount"]
[null,null,"PRELIMINARY & GENERAL ( FIXED AND TIME RELATED)  RATES SHALL APPLY AFTER ACCEPTANCE OF THE DESIGNS BY THE EMPLOYER"]
[null,"SABS 1200A","PRELIMINARY & GENERAL "]
[null,null,"FIXED CHARGES"]
[1,"8.3.1","Contractual Requirements","Sum",1]
[]
[2,"8.3.2","Establishment of Facilities on Site","Sum",1]
[]
[3,"8.3.2.1","Facilities for Engineer  (SABS 1200AB)","Sum",1]
[]
[4,"8.3.2.1(a)","Provision of Office for the Engineer's Representative as per PSAB 3.2, including toilet facilities as per PSAB 5.2","Sum",1]
[]
[5,"8.3.2.1(c)","Name Board (Refer to RW Typical Name Board R028537)","No.",1]
[]
[6,"8.3.2.2","Facilities for Contractor"]
[]
[7,"8.3.2.2\n(a)(b)(c)","Offices, storage sheds, fencing, workshops, laboratories.","Sum",1]
[]
[8,"8.3.2.2(e)","Ablution and latrine facilities","Sum",1]
[]
[9,"8.3.2.2(f)","Tools and equipment","Sum",1]
[]
[10,"8.3.2.2(g)","Water supplies, electric power and communications","Sum",1]
[]
[11,"8.3.3","Other fixed charge obligations, including setting out of works, security of contractor's plant & personnel","Sum",1]
[]
[12,"8.3.4","Remove all site establishment on completion","Sum",1]
[null,8.8,"Temporary Works"]
[13]
[null,"8.8.1","Access to works including all temporary roads, excavations and ramps.","Sum",1]
[]
[]
[null,null,"Schedule A Carried Forward",{"$nulls":3},{"$f":"SUM(G42:G42)","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"Schedule A Brought Forward",{"$nulls":3},{"$f":"G43","v":{"v":0,"d":"0.00"}}]
[]
[null,"SABS 1200A","PRELIMINARY & GENERAL \nTIME RELATED ITEMS"]
[null,null,"Limited to the Project Duration. DATES FOR DELIVERY AND COMPLETION – FOR THE INDIVIDUAL PROJECT"]
[14,"8.4.1","Contractual Requirements","Sum",1]
[]
[15,"8.4.2","Operate and maintain facilities on Site","Sum",1]
[]
[16,"8.4.2.1","Facilities for Engineer for duration of contract (SABS 1200AB)","Sum",1]
[]
[17,"8.4.2.1(a)","Provision of office for the Engineer's representative, incl. toilet facilities as per PSAB 3.2 and PSAB 5.2","Sum",1]
[]
[18,"8.4.2.1(c)","Name Board (Refer to RW Typical Name Board R028537)","Sum",1]
[]
[19,"8.4.2.2","Facilities for Contractor"]
[]
[20,"8.4.2.2\n(a)(b)(c)","Offices, storage sheds, fencing, workshops, laboratories, etc.","Sum",1]
[]
[21,"8.4.2.2(e)","Ablution and latrine facilities","Sum",1]
[]
[22,"8.4.2.2(f)","Tools and equipment","Sum",1]
[]
[23,"8.4.2.2(g)","Water supplies, electric power and communications","Sum",1]
[]
[24,"8.4.3","Supervision for duration of construction including Project Management & Contract Administration ","Sum",1]
[]
[25,"8.4.4","Company and head office overhead costs","Sum",1]
[]
[26,"8.4.5","Other time related charges, including security of contractor's plant & personnel","Sum",1]
[]
[27,null,"Operating and Maintenance Manuals","Sum",1]
[28,null,"Data Books","Sum",1]
[29,null,"Training of Rand Water Personnel (inclusive of training manuals)","Sum",1]
[]
[null,null,"Schedule A Carried Forward",{"$nulls":3},{"$f":"SUM(G45:G78)","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"Schedule A Brought Forward",{"$nulls":3},{"$f":"G79","v":{"v":0,"d":"0.00"}}]
[]
[30,null,"As Builts"]
[]
[30.1,null,"The sum shall cover all items for providing detailed As Builts of the works completed ","Sum",1]
[]
[31,null,"Access to Spoil Sites"]
[]
[31.1,null,"Sum associated with identification, negotiations and access to designated spoil sites for disposal of surplus spoil material ","Sum",1]
[]
[32,null,"Temporary Works"]
[]
[32.1,"8.8.1","Access to works including all temporary roads, excavations and ramps, etc.","Sum",1]
[]
[32.2,"PSA 8.8.9","Protection of road surfaces","Sum",1]
[]
[33,null,"Relocation of existing services (water mains, electricity cables/poles, etc.) by Service Utility","Sum",1]
[]
[]
[34,null,"Local Municipality Electrical Permanent Grid connection ( Application to Munipality and installation)","Sum",1]
{"$rows_empty":8}
[null,null,"Schedule A Brought Forward to Summary"]
[]
[43,null,"Access to Spoil Sites"]
[]
[43.1,null,"Sum associated with identification, negotiations and access to designated spoil sites for disposal of surplus spoil material ","Sum",1]
[]
[44,null,"Temporary Works"]
[]
[44.1,"8.8.1","Access to works including all temporary roads, excavations and ramps, etc.","Sum",1]
[]
[44.2,"PSA 8.8.9","Protection of road surfaces","Sum",1]
[]
[45,null,"Relocation of existing services (water mains, electricity cables/poles, etc.) by Service Utility","Sum",1]
[]
[]
[]
[46,null,"Local Municipality Electrical Permanent Grid connection ( Application to Munipality and installation)","Sum",1]
{"$rows_empty":14}
[null,null,"Schedule A Brought Forward to Summary"]

{"sheet":"Schedule B-L&R","index":1,"n_rows":19,"n_cols":7,"rows_kept":19,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,9],[6,0,6,2],[8,0,8,6]]}
[{"$nulls":6},"Form No: "]
["STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":6},"Rev No: xx"]
["LAND SERVICES: LAND AND RIGHTS AND PIPELINE PROTECTION"]
[{"$nulls":6},"Effective Date: "]
["Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
["Project/Bid Number : RW 10408567/26"]
[]
["SCHEDULE A: PRELIMINARY AND GENERAL COSTS  PALMIET SYSTEM"]
[]
["Item No.","Payment Refers","Description","Unit","Qty","Rate","Amount"]
[1," ","Route Selection as per SAMLR00005F",1,"Sum"," "," "]
[2," ","Property Servitude Valuations as per SAMLR00013T",1,"Sum"," "," "]
[3," ","Land-Servitude negotiations as per L&R Procedure as per SAMLR00010Pr",1,"Sum"," "," "]
[4," ","Detail Survey as per SAMLR00012T",1,"Sum"," "," "]
[5," ","Service Detection as per SAMLR00011T",1,"Sum"," "," "]
[6," ","Setting Out Structures as per SAMLR00015T",1,"Sum"," "," "]
[7," ","As-built Survey as per SAMLR00010T",1,"Sum"," "," "]
[8," ","Wayleave Submission to Authorities, Approvals, Renewals of expired wayleaves and adhering to Stakeholder conditions",1,"Sum"," "," "]

{"sheet":"Schedule C-Enviromental","index":2,"n_rows":45,"n_cols":8,"rows_kept":45,"merged":[[1,2,1,4],[1,5,1,8],[2,1,3,1],[2,5,3,6],[2,7,3,8],[4,5,4,6],[4,7,4,8],[5,1,9,1],[5,5,5,6],[5,7,5,8],[6,5,6,6],[6,7,6,8],[7,5,7,6],[7,7,7,8],[8,5,8,6],[8,7,8,8],[9,5,9,6],[9,7,9,8],[10,1,11,1],[10,5,10,6],[10,7,10,8],[11,5,11,6],[11,7,11,8],[12,1,21,1],[12,5,12,6],[12,7,12,8],[13,5,13,6],[13,7,13,8],[14,3,17,3],[14,4,17,4],[14,5,17,6],[14,7,17,8],[18,5,18,6],[18,7,18,8],[19,5,19,6],[19,7,19,8],[20,5,20,6],[20,7,20,8],[21,5,21,6],[21,7,21,8],[22,1,25,1],[22,5,22,6],[22,7,22,8],[23,5,23,6],[23,7,23,8],[24,5,24,6],[24,7,24,8],[25,5,25,6],[25,7,25,8],[26,1,33,1],[26,5,26,6],[26,7,26,8],[27,5,27,6],[27,7,27,8],[28,5,28,6],[28,7,28,8],[29,5,29,6],[29,7,29,8],[30,5,30,6],[30,7,30,8],[31,5,31,6],[31,7,31,8],[32,5,32,6],[32,7,32,8],[33,5,33,6],[33,7,33,8],[34,5,34,6],[34,7,34,8],[35,5,35,6],[35,7,35,8],[36,5,36,6],[36,7,36,8],[37,5,37,6],[37,7,37,8],[38,5,38,6],[38,7,38,8],[39,5,39,6],[39,7,39,8],[40,5,40,6],[40,7,40,8],[41,5,41,6],[41,7,41,8],[42,5,42,6],[42,7,42,8],[44,1,44,8]]}
[]
[null,null,"     ENVIRONMENTAL AUTHORISATION AND COMPLIANCE                    ENVIRONMENTAL  BILL OF QUANITIES  (PALMIET SYSTEM)",null,null,"Form Number: SAM EAC 00019 F\n\nRev No.:              05\n\nEffective Date: April 2025"]
[null,"Item   No.","Description","Unit","Qty","Rate (B)",null,"Total A*B"]
[]
[null,1,"Administrative requirements as per the approved EMPr. Submission and Maintanance of the Contractors environmental file based on RW's environmental file approval checklist.","Sum",1]
[null,2,"Emergency preparedness funding"]
[null,null,"a)   Provision for spillage management and clean up","Sum",1]
[null,null,"b)  Equipment for fire fighting","Sum ",1]
[null,null,"d)    Call out of fire department","Prov Sum",1,{"v":100000,"d":"R100,000"},null,{"v":100000,"d":"R100,000"}]
[null,null,"  Contractor's mark up on item 2 (d)","%",{"v":100000,"d":"R100,000"}]
[null,3,"Environmental awareness "]
[null,null,"The rate for this item shall include costs for inductions and environmental awareness and training","Sum",1]
[null,4,"Establishment of site camp and works area."]
[null,null,"The rate for this item shall include costs for establishment of construction campsite and working areas"]
[null,null,"Signage The rate for this item must cover all expenses incurred in preparing signage at the entrance of the site offices indicating the following information ","Sum",1]
[null,null,"·        The contractor’s contact numbers"]
[null,null,"·        ECO details "]
[null,null,"·  Emergency numbers and provision for: – snake removal, bee removal, fire, large hydrocarbon spillages, sewerage spillages"]
[null,null,"speed limits signage as per the EMPr/EA/WUL","Sum",1]
[null,null,"environmental no go area signage","Sum",1]
[null,null,"Temporary fence for site camp for the duration of the construction period","Sum",1]
[null,null,"Provision of demarcated eating area ","Sum",1]
[null,5,"Barricading and demarcation"]
[null,null,"a)  Screening for unsightly works","Sum",1]
[null,null,"b)  Clear fencing and demarcating of the working foot print","Sum",1]
[null,null,"c) Barricading and fencing of sensitive no go areas","Sum",1]
[null,6,"Pollution prevention and preservation of environmental resources "]
[null,null,"The rate for this item shall include costs for  pollution prevention and preservation of environmental resources"]
[null,null,"a) Cleaning the site of litter ","Sum ",1]
[null,null,"d)  Provision and servicing of ablution facilities, includingsafe disposal at a registered waste facility. ","Sum ",1]
[null,null,"g) General waste Waste removal","Sum ",1]
[null,null,"j) Recycled waste management  Waste removal","Sum ",1]
[null,null,"k) Spillage kits to clean up spillages  ","Sum ",1]
[null,null,"n) Drip trays for all vehicles staying on site over night","Sum ",1]
[null,7,"Preservation of the environment: fauna ,flora, scenic value,  Archaeological artefacts"]
[null,7.1,"Rescue, relocation and reinstatement of flora  (including apllication for a permit and labour) ","Prov Sum",1,{"v":100000,"d":"R100,000"},null,{"v":100000,"d":"R100,000"}]
[null,7.2,"Contractors mark up on item 7.1","%",{"v":100000,"d":"R100,000"}]
[null,7.3,"Rescue, relocation and reinstatement of fauna (including apllication for a permit and labour)","Prov Sum",1,{"v":100000,"d":"R100,000"},null,{"v":100000,"d":"R100,000"}]
[null,7.4,"Contractors mark up on item 7.3","%",{"v":100000,"d":"R100,000"}]
[null,11,"Appointment of the qualified fulltime environmental officer for the duration of the  projects ","Sum",1]
[null,12,"Final clean up and rehabilitation of the construction camp to the state in which it was prior to comencement of work","Sum ",1]
[null,null,"Total amount carried forward"]
[]
[]
[null,"NB: All inputs in the form are dependant on the type of project that is being assessed"]

{"sheet":"Schedule D-OH&S","index":3,"n_rows":39,"n_cols":9,"rows_kept":39,"merged":[[0,1,0,7],[0,8,0,9],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,1,4,7],[4,8,4,9],[5,1,5,10],[8,1,8,8],[10,6,10,7],[10,8,10,9],[17,1,20,1],[17,2,20,2],[38,1,38,7]]}
[{"$nulls":8},"Form No: SAM SHE 81079 F"]
[null,"STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":8},"Rev No: 1"]
[null,"SHEQ MANAGEMENT SYSTEM"]
[{"$nulls":8},"Effective Date: August 2024"]
[null,"Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
[null,"Project/Bid Number : RW 10408567/26"]
[]
[null,"SCHEDULE C: OCCUPATIONAL HEALTH AND SAFETY PALMIET SYSTEM"]
[]
[null,"Item No.","Payment Refers","Description","Qty (A)","U O M","Rate (B)",null,"Total A*B"]
[null,null,"HS Spec.","OCCUPATIONAL HEALTH AND SAFETY "]
[null,1,null,"Preparation of the Contractor's site specific Health and Safety Plan"]
[null,1.1,"2.4, 31.1,  4.2 & 29","Principal Contractor's initial obligations in respect of the Occupational Health and Safety and Regulations (Act 85 of 1993)\n",1,"Sum"]
[null,2,"4.2 & 29","Principal Contractor's time related obligations in respect of the Occupational Health and Safety and Regulations (Act 85 of 1993)\n",1,"Sum"]
[null,3,"16 & 29","Provision of Personal Protective Equipment (PPE)",1,"Sum"]
[null,4,"4.2.1 & 29","Provision of a full-time professionally registered Construction Health and Safety Officer with SACPCMP including annual membership fees with SACPCMP",1,"Sum"]
[null,5,"17 & 29","Cost of medical certificates and medical surveillance",1]
[{"$nulls":3},"(a) Initial (baseline) medical examinations",1,"Sum"]
[{"$nulls":3},"(b) Periodic  examinations",1,"Sum"]
[{"$nulls":3},"(c) Exit examinations",1,"Sum"]
[null,6,"11 & 29","Induction training",1,"Sum"]
[null,7," 20 & 29","Provision of First Aid Boxes to GSR requirements and other emergency safety equipment such as fire extinguishers.",1,"Sum"]
[null,8,"14 & 29","Welfare Facilities",1,"Sum"]
[null,9,"17.3 & 29","Occupational Hygiene Surveys",1,"Sum"]
[null,10,"12 & 29","Health and Safety Training",1,"Sum"]
[null,11," 31.2 & 29","Security requirements including the security risk assessment (before site establishment)",1,"Sum"]
[null,12,"18 & 29","Alcohol Testing",1,"Sum"]
[null,13,"31.4 & 29","Barricading",1,"Sum"]
[null,14,"30 (a) & 29","Safety notices and signs",1,"Sum"]
[null,15.1,"2.8 & 29","Construction work permit application fee",1,"Prov. Sum","R     2,500.00",null,"R     2,500.00"]
[null,15.2,null,"Mark up on item 15.1 above",10,"%"]
[null,16,"30(v) & 29","Adequate ventilation and lighting during construction",1,"Sum"]
[null,17,"30 (h) & 29","Adequate fall prevention and protection procedures, methods, mechanisms and equipment",1,"Sum"]
[null,18,"2.10 & 29","Submission of the Health and Safety File (hard and soft copies)- after tender award and project completion.",1,"Sum"]
[null,19.1,29,"Provision of Client Pr.CHSA (Construction Health & Safety  Agent) registered with SACPCMP.",1,"Prov. Sum","R    6,000,000.00",null,"R    6,000,000.00"]
[null,19.2,null,"Mark up on item 19.1 above",10,"%"]
[]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to - Summary of Price Schedule "]

{"sheet":"Schedule E -QA-C","index":4,"n_rows":22,"n_cols":8,"rows_kept":22,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[5,1,5,10],[8,1,8,8],[10,5,10,6],[10,7,10,8],[21,1,21,6]]}
[{"$nulls":7},"Form No: "]
[null,"STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":7},"Rev No: xx"]
[null,"SHEQ MANAGEMENT SYSTEM"]
[{"$nulls":7},"Effective Date: "]
[null,"Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
[null,"Project/Bid Number : RW 10408567/26"]
[]
[null,"SCHEDULE E: QUALITY ASSURANCE AND CONTROL:PALMIET   SYSTEM "]
[]
[null,"Item No.","Description","Qty (A)","U O M","Rate (B)",null,"Total A*B"]
[null,null,"Quality Plans and Control"]
[null,1,"Quality control and all activities necessary to comply with all requirements of the specified quality control system as per PS 5."]
[null,1.1,"Inspection and Test Plans (ITPs): Detailing inspection and testing requirements for all  CP installation activities","Sum ",1]
[null,2,"The Contractor shall provide a full-time Quality Inspector for the duration of the contract to ensure compliance with project specifications, standards, and quality requirements","Sum ",1]
[null,3,"Maintenance of documents and final documentation for submission ","Sum ",1]
[null,4,"Provision of proper storage for Cathodic Protection units ","Sum ",1]
[null,5,"Testing Equipment calibration (The testing Equipments should be calibrated as per the manual) ","Sum ",1]
[null,6,"Provision of any other  testing and inspections requested by the Engineer","Prov Sum ",{"v":50000,"d":"50,000.00"}]
[null,6.1,"Contractor's mark up on item 9"]
[]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules"]

{"sheet":"Schedule F-CP BOQ","index":5,"n_rows":211,"n_cols":8,"rows_kept":211,"merged":[[6,1,6,10],[9,1,9,9],[14,1,14,7],[16,10,16,11],[33,1,33,7],[40,1,40,7],[50,1,50,7],[57,1,57,7],[65,1,65,7],[73,1,73,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[106,1,106,7],[116,1,116,7],[128,1,128,7],[136,1,136,7],[145,1,145,7],[154,1,154,7],[155,1,155,7],[167,1,167,7],[171,1,171,7],[178,1,178,7],[184,1,184,7],[189,1,189,7],[195,1,195,7],[200,1,200,7],[201,1,201,7],[209,1,209,6],[210,1,210,7]]}
[]
[{"$nulls":3},"STRATEGIC ASSET MANAGEMENT"]
[]
[{"$nulls":3},"SHEQ MANAGEMENT SYSTEM"]
[]
[]
[null,"Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
[null,"Project/Bid Number : RW 10408567/26"]
[]
[null,"SCHEDULE F: SUPPLY, DELIVERY AND INSTALLATION OF  CATHODIC PROTECTION RECTIFIERS INCLUDING DISPOSINGOF VANDALISED STRUCTURES IN MAPLETON  SYSTEM"]
[]
[null,"Tenderer to Take Note of Following: "]
[null,"1. Provide more details and Price under each heading in line with the applicable Scope of Work"]
[null,"2. Any item not applicable should be Marked as N/A  "]
[null,"CP System Repairs and Maintenance Palmiet System BOQ"]
[null,"Item","Payment","Description","Unit","Qty","Rate","Amount"]
[null,"No","Refers"]
[{"$nulls":3},"SECTION A :Supply Activities"]
[null,"1",null,"Supply Impressed Current Cathodic Protection System "]
[null,"1.1",null,"Transformer Rectifier Units"]
[null,"1.1.1","TS001","Supply 100V/100A Transformer Rectifier Unit (TRU) ","each",23]
[null,"1.1.2","TS021","Supply Ring main Positive Cable of single core red 35mm² double insulated PVC cable.(GB header and GB to TRU Header)","m",5520]
[null,"1.1.3","TS044","Supply concrete mass as per drawing 27645 for cable encasement ( Positive cable and supply cable).","m³",230]
[null,15,"TS049","Supply the TRU's steel housing structure","each",23]
[null,"1.1.5","TS021","Supply 25mm² four core aluminium supply cable  with 30m length each","m",690]
[null,"1.1.6","TS021","Supply PRE and coupon with enough tail cable to terminate inside the TRU - 3m ","each",23]
[null,"1.1.7","TS021","Supply 10mm² monitor cable with 3m length ","m",70]
[null,"1.1.8","TS021","Supply 2X35mm² pipe cable with 3m length ","m",140]
[null,"1.1.9","TS015","Supply coating make good material ,lugs and consumables, etc","sum",23]
[null,"1.1.10","TS 001","Supply 70mm² bare copper cable  for earthing ","m",580]
[null,"1.1.11","TS 001","Supply 1.2m earth rods with connecting clamps","each",230]
[null,"1.1.12","TS 001","Supply earthing and all consumables ","sum",23]
[null,"1.1.13","TS049","Supply  perimeter fence - clear view  type fence around the TRU housing as per RA 61412/001","each",23]
[]
[]
[null,"1.2",null," Horizontal Anode Groundbed  "]
[null,"1.2.1","TS002","Supply 2m canistor 33 MMO anodes X 200mm diameter with 2m tail cable and canisters are to be filled with Sasol calcined petroleum coke ","each",759]
[null,"1.2.2","Drg. RA-22675","Supply 1000mm length X 200mm diameter X 1mm thick galvanized steel canister spacer filled with Sasol calcined petroleum coke, installed before and in between the anodes as per drawing RA 22675.","each",782]
[null,"1.2.3","Drg. RA-22675","Supply  Sasol calcined petroleum coke breeze. ","m³",240]
[null,"1.2.4","TS046","Supply 'Y' splicing kit for anode tail connections to the ring main cable ","each",770]
[]
[]
[null,"1.3",null,"Supply Cross Bonding Facilities  to Foreing lines "]
[null,"1.3.1","TS013","Supply crossbond facility as per Third party specification","each",31]
[null,"1.3.2","TS013","Supply crossbond facility as per Rand Water specification","each",31]
[null,"1.3.3","TS014","Supply PRE and Coupon","sum",31]
[null,"1.3.4","TS013","Supply resistive bond as per Third Party Specification","each",62]
[null,"1.3.5","TS043","Supply black 2x35mm² cable for pipe connection on the Rand Water pipeline 6m length","m",372]
[null,"1.3.6","TS043","Supply red 2X35mm² cable for Third party pipe connection on the  pipeline 10m length in each ","m",610]
[null,"1.3.8","TS015","Supply cable lugs,  cable glands, coating make good materials and consumables  ","sum",124]
[]
[]
[null,"1.4",null,"Mushroom Monitoring Points"]
[null,"1.4.1","TS013","Supply Mushrooms Bonding Monitoring Points with link panel","each",50]
[null,"1.4.2","TS014","Supply PRE and coupon with the minimum tail cable of 3m ","each",50]
[null,"1.4.3","TS021","Supply 16mm² pipe cable with 2X3m length ","m",900]
[null,"1.4.4","TS019","Supply cable lugs,  and cable gland coating make good materials and consumables  ","sum",50]
[]
[]
[{"$nulls":3},"AK47 Anti-vandalism Monitoring Points"]
[null,"1.5.1","TS022","Supply AK47 CP Anti-vandalism Bunkers with the link panel","each",50]
[null,"1.5.2","TS014","Supply PRE and coupon with the minimum tail cable of 3m ","each",50]
[null,"1.5.3","TS021","Supply 35mm² pipe cable with 2X3m length ","m",600]
[null,"1.5.4","TS014","Supply AC and DC current density coupons","each",50]
[null,"1.5.5","TS015","Supply cable lugs,  cable glands coating make good materials and consumables  ","sum",50]
[]
[]
[null,"1.6",null,"Chamber Monitoring Points DUDC"]
[null,"1.6.1","TS022","Supply chamber monitoring bunkers with the link panel","each",125]
[null,"1.6.2","TS014","Supply PRE and coupon with the minimum tail cable of 3m ","each",125]
[null,"1.6.3","TS021","Supply 35mm² pipe cable with 2X6m length ","m",1500]
[null,"1.6.4","TS014","Supply AC and DC current density coupons","each",125]
[null,"1.6.5","TS015","Supply cable lugs,  cable glands coating make good materials and consumables  ","sum",125]
[]
[null,"1.7",null,"AC mitigation System"]
[null,"1.7.1","TS013","Supply earth mats around chamber as per drawing RA27375 ","each",5]
[null,"1.7.2","TS013","Supply Voltage Limiting Device (VLD) for earth mat termination ","each",5]
[null,"1.7.3","TS032","Supply single Zinc Ribbon","m",2000]
[null,"1.7.4","TS032","Supply DC decoupling devices (zinc ribbon) ","each",40]
[null,"1.7.5","TS032","Supply 35mm2 black pvc/pvc cables from Pipeline to the bunker","m",200]
[null,"1.7.6","TS032","Supply 35mm2 green/yellow pvc/pvc cables from each mitigation wires to the bunker","m",200]
[null,"1.7.7","TS032","Supply consumables for Zinc ribbon connection","sum",40]
[null,"1.7.8",null,"Supply Special bunkers - mega bunker","sum",40]
[]
[]
[]
[{"$nulls":3}," SECTION B: Installation Activities:6 months"]
[{"$nulls":3}," Impressed Current Cathodic Protection System "]
[null,2.1,null,"Transformer Rectifier Units"]
[null,"2.1.1",null,"Demolish damaged existing infrastructure and dispose at the nearest approved disposal site","each",23]
[null,"2.1.2","TS001","Install 100V/100A Transformer Rectifier Unit (TRU) ","each",23]
[null,"2.1.3","TS049","Install a vandal proof housing,  the steel structure","each",23]
[null,"2.1.4","TS049","Install perimeter fence - clear view  type fence around the TRU housing as per RA 61412/001","each",23]
[null,"2.1.5","TS021","Excavate a trench and install a supply cable of 25mm² four core aluminium cable of 1.5m deep X 0.5m width X 30m long ","m³",530]
[null,"2.1.6","TS021","Install PRE and coupon ","sum",23]
[null,"2.1.7","TS021","Install 10mm² monitor cable with 3m length ","sum",70]
[null,"2.1.8","TS021","Install 2X35mm² pipe cable with 3m length ","sum",140]
[null,"2.1.9","TS044","Incase the cable in a concrete mass as per drawing 27645.","m³",230]
[null,"2.1.10","TS015","Install cable lugs, consumables and repair coating  ","sum",23]
[null,"2.1.11","TS019","Service detection, backfilling and rehabilitation of the area","sum",23]
[null,"2.1.12","TS 001","Install 70mm² bare copper cable  for earthing ","sum",580]
[null,"2.1.13","TS 001","Install 1.2m earth rods with connecting clamps","sum",230]
[null,"2.1.14","TS 001","Install earthing and all consumables ","sum",23]
[null,"2.1.15",null,"WKS numbering on CP assets as per the  RW CP Asset register","sum",23]
[null,"2.1.16","TS036","Power application from the relevent power utility and installation  and issuing  COC ","each",23]
[null,"2.1.17","TS001","Install a free issued TRU Remote Monitoring  Unit","each",23]
[]
[]
[null,2.2,null,"Install Horizontal Anode Groundbed  "]
[null,"2.2.1","TS021","Excavate a trench of 2m deep X 0.5m width X 100m long to install the ring main positive cable of single core red 35mm² double insulated PVC cable and anodes.","m³",2300]
[null,"2.2.2","TS002","Excavate a trench of 2.5m deep X 0.5m width X 100m long for the ground bed installation. ","m³",2875]
[null,"2.2.3","Drg. RA-22675","Install 2m canistor 33 MMO anodes X 200mm diameter with 2m tail cable and canisters are to be filled with Sasol calcined petroleum coke ","Sum",760]
[null,"2.2.4","Drg. RA-22675","Install 1000mm length X 200mm diameter X 1mm thick galvanized steel canister spacer filled with Sasol calcined petroleum coke, installed before and in between the anodes as per drawing RA 22675.","Sum",782]
[null,"2.2.5","Drg. RA-22675","Backfill the anodes with Sasol calcined petroleum coke breeze. ","m³",240]
[null,"2.2.6","TS046","Connect the anodes tail cable to the ring main using the 'Y' splicing kit. ","Sum",770]
[null,"2.2.7","TS019","Service detection, backfilling and rehabilitation of the area","Sum",23]
[]
[null,"2.3",null,"Cross Bonding Facilities  to Foreing lines"]
[null,"2.3.1","TS013","Install Crossbond Facility as per Third party  specification","each",31]
[null,"2.3.2","TS013","Install  Crossbond Facility as per Rand Water specification","each",31]
[null,"2.3.3","TS014","Install  PRE and Coupon","each",31]
[null,"2.3.4","TS013","Install  resistive bond as per Air Product specification","each",62]
[null,"2.3.5","TS021","Install black 35mm² cable for pipe connection on the Rand Water pipeline 6m length in each","sum",372]
[null,"2.3.6","TS021","Install  red 35mm² cable for Air Product pipe connection on the  pipeline 10m length in each ","sum",610]
[null,"2.3.7","TS019","Service detection, excavation, trenching and backfilling","each",31]
[null,"2.3.8","TS015","Install cable lugs,  cable glands coating make good materials and consumables  ","each",124]
[null,"2.3.9",null,"Painting and  numbering on CP assets ","sum",31]
[null,"2.3.10","TS011","Perform CP Interference test between the foreign lines and Rand Water pipelines","sum",31]
[]
[null,2.4,null,"Mushroom Monitoring Point "]
[null,"2.4.1","TS013","Install Mushrooms Bonding Monitoring Points","each",50]
[null,"2.4.2","TS014","Install PRE and coupon with the minimum tail cable of 3m ","each",50]
[null,"2.4.3","TS021","Install 35mm² pipe cable with 2X3m length ","sum",900]
[null,"2.4.4","TS019","Service detection, excavation, trenching and backfilling","sum",50]
[null,"2.4.5","TS015","Install cable lugs, coating make good materials and consumables  ","sum",50]
[null,"2.4.6",null,"Painting and  numbering on CP assets ","sum",50]
[]
[null,2.5,null," AK 47 CP Anti Vandalism Monitoring Point"]
[null,"2.5.1","TS012","Install AK47 CP Anti-vandalism Bunkers","each",50]
[null,"2.5.2","TS014","Install PRE and coupon with the minimum tail cable of 3m ","each",50]
[null,"2.5.3","TS021","Install 35mm² pipe cable with 2X3m length ","sum",600]
[null,"2.5.4","TS014","Install AC and DC current density coupons","each",50]
[null,"2.5.5","TS019","Service detection, excavation, trenching and backfilling","sum",50]
[null,"2.5.6","TS019","Install  cable lugs,cable glands coating make good materials and consumables  ","sum",50]
[null,"2.5.7",null,"Painting and  numbering on CP assets ","sum",50]
[]
[null,2.6,null," Chamber Monitoring Point DUDC"]
[null,"2.6.1","TS012","Install chamber monitoring Bunker","each",125]
[null,"2.6.2","TS014","Install PRE and coupon with the minimum tail cable of 3m ","each",125]
[null,"2.6.3","TS021","Install 35mm² pipe cable with 2X3m length ","sum",1500]
[null,"2.6.4","TS014","Install AC and DC current density coupons","each",125]
[null,"2.6.5","TS019","Service detection, excavation, trenching and backfilling","sum",125]
[null,"2.6.6","TS015","Install  cable lugs,cable glands coating make good materials and consumables  ","sum",125]
[null,"2.6.7",null,"Painting and  numbering on CP assets ","sum",125]
[]
[]
[null,2.7,null," AC mitigation system "]
[null,"2.7.1","TS013","Install earth mat with Volatege Limiting Device (VLD's) around chambers as per drawing RA27375","sum",5]
[null,"2.7.2","TS013","Install Voltage Limiting Device (VLD) for earth mat termination ","sum",5]
[null,"2.7.3","TS032","Install Single Zinc Ribbon","each",40]
[null,"2.7.4","TS032","Install DC decoupling devices (zinc ribbon)","sum",40]
[null,"2.7.5","TS032","Install 35mm2 black pvc/pvc cables for pipe connection","sum",40]
[null,"2.7.6","TS032","Install 35mm2 green/yellow pvc/pvc cables from earth mat and zinc ribbon for termination","sum",40]
[null,"2.7.7","TS032","Service Detection, Excavation, Trenching and Backfilling","sum",40]
[null,"2.7.8",null,"Install Special bunkers - mega bunker","sum",40]
[null,"2.7.9",null,"Painting and  numbering on CP assets ","sum",40]
[]
[]
[null,3,null,"Commission and testing "]
[null,"3.1.1","TS023","Commissioning and interference testing ","sum",23]
[]
[]
[]
[{"$nulls":3},"SECTION C:Cathodic Protection System Monitoring  "]
[{"$nulls":3},"Cathodic Protection System Monitoring/Maintenance  Activities"]
[null,4.1,null,"Coating Survery "]
[null,"4.1.1","TS035/TS024","Provisional sum for conducting coating surveys along the pipeline network of a distance of 800Km at R2000 per Km = R1.6M.","prov",1,{"v":1600000,"d":"R1,600,000"},{"v":1600000,"d":"R1,600,000"}]
[null,"4.1.2",null,"Mark-up of the above","sum",1]
[]
[]
[null,4.2,null,"Cathodic Protection Monitoring Points and Cross Bond monitoring "]
[null,"4.2.1","TS023","Perform 24-hour recording using a logger for along the Rand Water pipeline network with a length of 800Km per system.","Km",800]
[null,"4.2.2","TS013","Perform 24 hours recordings for cross bonding facility with third party","sum",31]
[null,"4.2.3","TS023","Perform or collect spot potentials along the pipeline network with a length of 800Km per system and provide raw data report","sum",1]
[]
[]
[null,4.3,null,"Locate Possible Power Supply Points, 380V to 22kV 3 phase AC for CPS as and when required."]
[null,"4.3.1","TS036","Provisional sum for applying, deposit and installation of power supply (at R300 000 X 13 sites = R4 000 000) ","prov",1,{"v":4000000,"d":"R4,000,000"},{"v":4000000,"d":"R4,000,000"}]
[null,"4.3.2",null,"Mark-up of the above","sum",1]
[]
[null,4.4,null,"Rectifiers Inspections "]
[null,"4.4.1","TS001","Perform two weekly rectifier inspections and record the output voltage, output current, pipe-to-soil potentials ‘OFF’, pipe-to-soil potentials ‘ON’ and AC pipe potentials","sum",1]
[null,"4.4.2","TS001","Clean the rectifier and do visual inspection on all components and cables (report defects and repair).","sum",1]
[null,"4.4.3","TS001","Do fault finding on defective rectifiers and repair.","sum",1]
[null,"4.4.4","TS001","Compile the monthly inspection report and submit for approval","sum",1]
[]
[null,4.5,null,"Negotiate with Local Authorities"]
[null,"4.5.1","TS023","Negotiate with foreign pipe and / or railway line crossings authorities,","sum",1]
[null,"4.5.2","TS023","Conduct interference tests with third party or foreign pipelines","sum",1]
[null,"4.5.3","TS023","Provisional sum of servitude and wayleave applications (at R300 000 X 13 sites = R4 000 000) ","prov",1,{"v":4000000,"d":"R4,000,000"},{"v":4000000,"d":"R4,000,000"}]
[]
[]
[null,4.6,null,"Cathodic Protection Reports"]
[null,"4.6.1","TS030","Compile a commissioning report with recommendations","sum",1]
[null,"4.6.2","TS030","Compile interference test report with recommendations","sum",1]
[null,"4.6.3","TS030","Compile the maintenance monthly rectifiers report per system with findings and recommendations","sum",1]
[null,"4.6.4","TS030","Compile the quarterly 24-hour recordings report per system with findings and recommendations","sum",1]
[null,"4.6.5","TS030","Compile coating survey report with recommendations","sum",1]
[null,"4.6.6","TS030","Final documentation ,eletricity account documentation with account number and  handover  ","sum",1]
[null,"Sub-total "]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules  "]

{"sheet":"Schedule G-SED","index":6,"n_rows":54,"n_cols":7,"rows_kept":54,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,9],[9,0,10,0],[9,1,10,1],[9,2,10,4],[9,5,10,5],[9,6,10,6],[13,0,15,0],[13,1,15,1],[13,2,15,4],[13,5,15,5],[13,6,15,6],[21,0,23,0],[21,1,23,1],[21,2,23,4],[21,5,23,5],[21,6,23,6],[29,0,33,0],[29,1,33,1],[29,2,33,4],[29,5,33,5],[29,6,33,6],[39,0,40,0],[39,1,40,1],[39,2,40,4],[39,5,40,5],[39,6,40,6],[46,0,47,0],[46,1,47,1],[46,2,47,4],[46,5,47,5],[46,6,47,6]]}
["STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":6},"Rev No: xx"]
["SOCIO-ECONOMIC DEVELOPMENT"]
[{"$nulls":6},"Effective Date: "]
[{"$nulls":6},"Form No: "]
["Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
["Project/Bid Number : RW 10408567/26"]
[]
[" "," "," "," "," "," "," "]
["Item No","Payment","Description",null,null,"U O M","Qty (A)"]
[]
[1," ","Skills Development Program",null,null," "," "]
[" "," "," ",null," "," "," "]
[1.1," ","Accredited training programmes are targeted which will provide the beneficiaries with significant and recongnised credit value in accordance with the National Qualification Framework (NQF). ( minimum 2.5% of the Project value)",null,null,"sum",{"v":0.025,"d":"2.50%"}]
[]
[]
[" "," "," ",null," "," "," "]
[1.2," ","Contractors Mark-up on the items 1.1 above",null,null,"%"," "]
[" "," "," ",null," "," "," "]
[2," ","Corparate social resposibiliy program",null,null," "," "]
[" "," "," ",null," "," "," "]
[2.1," ","Corparate social resposibility programs aimed at Improving the livelihood of the communit ( Minimum 1% of Project Value)",null,null,"sum",{"v":0.01,"d":"1.00%"}]
[]
[]
[" "," "," ",null," "," "," "]
[2.2," ","Contractors mark-up on item 2.1 above",null,null,"%"," "]
[" "," "," ",null," "," "," "]
[3," ","Community Liason Officer",null,null," "," "]
[" "," "," ",null," "," "," "]
[3.1," ","Community liason officer. A key component in aiding the realisation of the SED objectives is effective community liason with all the relevant role-players, structured, civil organisation and the community at large. (minimum 0.5% of the project value)",null,null,"sum",{"v":0.005,"d":"0.50%"}]
[]
[]
[]
[]
[" "," "," ",null," "," "," "]
[3.2," ","Contractors mark-up on the item 3.1 above",null,null,"%"," "]
[" "," "," ",null," "," "," "]
[4," ","SED Administration",null," "," "," "]
[" "," "," ",null," "," "," "]
[4.1," ","Labour management services ( minimum 1% of the project value)",null,null,"sum",{"v":0.01,"d":"1.00%"}]
[]
[" "," "," ",null," "," "," "]
[4.2," ","Contractor mark-up on the items 4.1 above",null,null,"%"," "]
[" "," "," ",null," "," "," "]
[5," ","Participation of local enterprices",null,null," "," "]
[" "," "," ",null," "," "," "]
[5.1," ","work allocated to local enterprises ( Inclusive of the P&G's and SHEQ) ( Minimum 5% of the project)",null,null,"sum",{"v":0.05,"d":"5.00%"}]
[]
[" "," "," "," "," "," "," "]
[5.2," ","Contracotors mark-up on item 5.1 above",null,null,"%",{"v":0.015,"d":"1.50%"}]
[" "," "," "," "," "," "," "]
[" "," "," ",null," "," "," "]
[" "," "," ",null," "," "," "]
[" "," "," "," "," "," "," "]

{"sheet":"Schedule H-Summary of schedules","index":7,"n_rows":32,"n_cols":4,"rows_kept":32,"merged":[[0,1,0,2],[1,1,1,2],[2,1,2,2],[3,1,3,2],[4,1,4,2],[9,1,9,4],[11,1,12,2],[11,3,11,4],[12,3,12,4],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[26,3,28,3],[26,4,28,4],[27,1,27,2],[28,1,28,2],[29,1,29,2],[31,1,31,3]]}
[{"$nulls":3},"Form No: "]
[null,"STRATEGIC ASSET MANAGEMENT"]
[{"$nulls":3},"Rev No: xx"]
[null,"SHEQ MANAGEMENT SYSTEM"]
[{"$nulls":3},"Effective Date: "]
[null,"Description of the Project: The Appointment of Service Providers to Supply, Deliver and Installation of Cathodic Protection Rectifiers and Monitoring Points and Maintenance of Cathodic Protection Systems Along The Rand Water Pipeline Network Over A Period of 3 Years "]
[]
[null,"Project/Bid Number : RW 10408567/26"]
[]
[null,"SCHEDULE H:  SUMMARY OF PRICE SCHEDULES"]
[]
[null,"PRICE SCHEDULES",null,"TOTAL AMOUNT"]
[{"$nulls":3},"                 R                        c"]
[null,"ALL PLANT BUILDINGS AND ASSOCIATED STRUCTURES"]
[null,"Total brought forward from SCHEDULE A: PRELIMINARY AND GENERAL COSTS"]
[null,"Total brought forward from SCHEDULE B: LAND AND RIGHTS "]
[null,"Total brought forward from SCHEDULE C: ENVIRONMENTAL "]
[null,"Total brought forward from SCHEDULE D: OCCUPATIONAL HEALTH AND SAFETY "]
[null,"Total brought forward from SCHEDULE E: QUALITY ASSURANCE AND CONTROL "]
[null,"Total brought forward from SCHEDULE F: CP WORK"]
[]
[]
[null,"SUBTOTAL A ……………………………………..……………………………………………"]
[null,"Total brought forward from SCHEDULE G:  SOCIO-ECONOMIC DEVELOPMENT"]
[]
[null,"SUBTOTAL B ……………………………………..……………………………………………"]
[null,"VALUE ADDED TAX"]
[null,"Add 15% of Subtotal B ………..…….……………………..………...……..………………"]
[null,"(Provisional sum based on current rate of VAT)"]
[null,"TOTAL CARRIED TO SUB-PACKAGE SUMMARY"]
[]
[null,"SIGNED ON BEHALF OF TENDERER: ……………………………………………..……………………………………………."]