400m - 1.8m Hinge Joint Fence – project ISC01240500026
Site: Troya Village, Dr JS Moroka, Nkangala District Municipality, Mpumalanga,
	Description 
	Quantity 
	Unit

	POSTS - 2.450M X 114MM
H/DUTY 2 x GATE POSTS
	6.000 
	 each

	STAYS - 2.450M X 50MM H/D 
	10.000 
	each

	Y-STANDARDS – MITTAL 2450MM
	36
	 each

	DROPPERS - CAPE GATE - 1850MM
	120
	 each

	HINGE JOINT GAMEFENCE 13-
1830-150*4/4/4
	4
	100M

	B/WIRE HANDYPACK -
1.60MM - 317M - 5KG
	2
	each

	BOLT & NUT ELECTRO PLD
M12 X 140 GR 4.8
	6
	each

	GATE D/MESH - 4.200M X
1.800M
	1
	each

	CEMENT
	
	

	Sand 
	
	Sand 

	Aggregates
	
	Aggregates

	Compulsory Site inspection
	Troya, Dr JS Moroka, Nkangala District Municipality, Mpumalanga, South Africa

	Delivery to 
	Troya, Dr JS Moroka, Nkangala District Municipality, Mpumalanga, South Africa



