{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["PRICING SCHEDULE MASTER OF THE "],"not_rendered":{"images":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"PRICING SCHEDULE MASTER OF THE ","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"merged":[[2,1,2,2],[3,1,3,2],[4,1,4,2],[13,4,13,6],[16,0,17,0],[29,2,32,2],[29,3,29,4],[29,5,29,6],[30,3,30,4],[30,5,30,6],[31,3,31,4],[31,5,31,6],[32,3,32,4],[32,5,32,6]]}
[null,null,"          SUPPLY CHAIN MANAGEMENT"]
[null,null,"              Pricing schedule"]
["RFx No","RFB 06 2025"]
["RFB Title"," APPOINTMENT OF A SERVICE PROVIDER FOR THE MANUFACTURING, SUPPLY, DELIVERY AND INSTALLATION OF OFFICE FURNITURE: MASTER OF HIGH COURT, PRETORIA"]
["Bidder Name "]
[]
["1. INSTRUCTION FOR COMPLETING THE PRICING SCHEDULE"]
["(a)  THIS PRICING SCHEDULE MUST BE SUBMITTED SEPARATELY FROM THE TECHNICAL RESPONSE, failing which the BID may be DISQUALIFIED."]
["(b)  Bidder must complete/enter YELLOW cells only"]
["(c)  Unit and Line prices must be VAT EXCLUSIVE and in South African Rand (ZAR) currency."]
["(d) The price must include all cost to deliver the goods or render the service, including all applicable taxes, duty fees, logistics/delivery, storage, labour, overtime and subsistance and travel"]
["(e) Bidders must attached a separate bill of quantities linked to the statement of work totaling to their bid price in the letterhead of the bidder"]
[]
[{"$nulls":7},"TOTAL"]
["Office NO ","Item No","Goods/Service description","Unit of measure","Qty ","Unit Price \n(Excl VAT)","Line Price","Line Price Term \n(Excl VAT)"]
[1234,null,"MANUFACTURE, SUPPLY, DELIVER & INSTALLATION"]
["3rd Floor","1.","3rd floor Boardroom: Chairs: Mid Back Heavy duty chairs with arms, 650mm wide, full shell ply wood with 18ply. High density foam on seat VP70.Medium density foam on back VP30(170kg Max Weight) (Blue Colour).","Each",18,null,{"$f":"E17*F17","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(G17)","v":{"v":0,"d":"R0.00"}}]
[null,2,"3rd floor Boardroom: 18-seater Boardroom table in Mahogany veneer 2,2m (L) X 5 m (W) x 780 mm (H) with 38mm top). U shape of the table. ","Each",1,null,{"$f":"E18*F18","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(G18)","v":{"v":0,"d":"R0.00"}}]
["3rd Floor","3.","Admin Clerks and other: 2 Officials  (3rd floor):  Open Plan 2-way cluster consists of:\n2 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge. -  1 X 1584mmW x 864mmH X 32mmD Panel with double sided pinboard upholstered in WW”Mirage 8668”                                                                              CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.\n","Each",1,null,"R0.00","R0.00"]
["3rd Floor",4,"Admin Clerks and other: 12 Officials  (3rd floor):  Open Plan 4-way cluster consists of:\n4 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge. -  2 X 1584mmW x 864mmH X 32mmD Panel with double sided pinboard upholstered in WW”Mirage 8668”                                                                           CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.\n","Each",3,null,"R0.00","R0.00"]
["2nd Floor","5.","Admin Clerks and other: 64 Officials  (2nd floor):  Open 4-way cluster consists of:\n4 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge.-  2 X 1584mmw x 864mmH X 32mmD PANEL WITH DOUBLE SIDED PINBOARD UPHOLSTERED IN WW”MIRAGE 8668”                                                                               CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.\n","Each",16,null,{"$f":"E21*F21","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(G21)","v":{"v":0,"d":"R0.00"}}]
["1st Floor","6.","Admin Clerks and other: 82 officials (1st floor): Open 4-way cluster consists of:                              44 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge. -  2 X 1584mmW x 864mmH X 32mmD Panel with double sided pinboard upholstered in WW”Mirage 8668”                                                                           CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.","Each",21,null,{"v":0,"d":"R0.00"},{"$f":"SUM(G22)","v":{"v":0,"d":"R0.00"}}]
["Ground Floor","7.","Registry Clerks x 12 Officials (ground floor):   \n4 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge. -  2 X 1584mmW x 864mmH X 32mmD Panel with double sided pinboard upholstered in WW”Mirage 8668”                                                                           CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.","Each",3,null,{"v":0,"d":"R0.00"},{"$f":"SUM(G23)","v":{"v":0,"d":"R0.00"}}]
["Ground Floor","8.","Registry Offices x 2 Officials (ground floor):   \n2 x 2000mm x 800mm desk tops in 32mm melawood “summer oak” with 2mm matching pvc edge with 2 x 75mm cut-outs per desk for cabling, including covers for cut-outs to match “summer oak”  4 x 416mmw x 575mmd x 718mmh 3-drawer desk high pedestals with 2 x standard drawers with pen and pencil tray insert in the top drawer and 1 x deep filer. Fitted with silver bow handles and central locking mechanism. Outer edge or drawer unit in 16mm summer oak” with 2mm matching pvc edging. Inner pedestal, drawer units and drawer fronts are to be in melawood “super white” with 2mm matching pvc edge. -  1 X 1584mmW x 864mmH X 32mmD Panel with double sided pinboard upholstered in WW”Mirage 8668”                                                                              CPU holder under table in black.\n4 x 3500mmw x 100mmh x 40mmd 2-tier cable channels in 1mm mild steel powder coated silver fitted under desks. Top channel for data, bottom channel for power. “Corporate connections” (or similar) per desk – 2 x red dedicated plugs, 1 x white normal power, 1 x 2-pin plug. Units to daisy chain under the desks in the cable channels. Maximum of 3 3 desks to be connected together in one run. Unit closest to wall will connect to plugs in the power skirting or dry wall.\nFurniture contractor will supply, install and connect the “corporate connections” under the desks and will connect the units to the electrical point provided in the power skirting or dry wall.\n","Each",1,null,"R0.00","R0.00"]
[null,null,"TOTAL BID PRICE  (EXCL VAT)",{"$nulls":3},{"$f":"SUBTOTAL(9,G16:G24)","v":{"v":0,"d":"R0.00"}},{"$f":"SUBTOTAL(9,H16:H24)","v":{"v":0,"d":"R0.00"}}]
[null,null,"VAT (@15%)",{"$nulls":3},{"$f":"G25*0.15","v":{"v":0,"d":"R0.00"}},{"$f":"H25*0.15","v":{"v":0,"d":"R0.00"}}]
[null,null,"TOTAL  BID PRICE (INCL VAT)",{"$nulls":3},{"$f":"G25+G26","v":{"v":0,"d":"R0.00"}},{"$f":"H25+H26","v":{"v":0,"d":"R0.00"}}]
[]
[]
[null,null,"I, the bidder, confirm that the price(s) and rate(s) quoted cover all the goods and/or works specified in the bidding documents; that the price(s) or rate(s) cover all my obligations and I accept that any mistakes regarding price(s), rate(s) or calculations will be at my own risk.\n[Note: First convert to PDF, then add signature]"]
[{"$nulls":3},"Name (above)",null,"Capacity"]
[]
[{"$nulls":3},"Signature (above)",null,"Date"]