{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":59,"n_cols":7,"rows_kept":59,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,0,4,6],[6,4,6,5],[7,4,7,5],[9,1,9,6],[10,1,10,6],[13,2,13,3],[14,2,14,3],[15,3,15,4],[21,3,21,4],[32,3,32,4],[36,2,36,4],[37,2,37,5],[38,3,38,4],[40,3,40,4],[42,3,42,4],[47,0,47,6],[48,1,49,6],[51,0,51,6],[53,0,53,1],[58,2,58,3]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," DDT-3098 - NON-TENSION JOINT"]
[null,"NB. UNIQUE SCHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW "]
["NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[]
[{"$nulls":3},"SAP Number","Technical Description "]
[{"$nulls":3},214100,"JOINT,NON-TEN CHIC AL-OAK/HAR AL I/CD3098","JOINT,NON-TEN CHIC AL-OAK/HAR AL I/CD3098"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No","SAP 0214100","xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier, product code, conductor name/code and knurl marks indelibly marked on product body","Specify markings","xxxxxxxxxx"]
[null,"1.1.6","·","Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.1.6.1",null,"NON TENSION JOINT SET\n\n- Compression indent crimps "," Eskom DDT-3098","YES"]
[null,"1.1.6.2",null,"NON TENSION JOINT SET\n\n- Tubular"," Eskom DDT-3098","YES"]
[null,"1.1.6.3",null,"NON TENSION JOINT SET\n\n- Bi-metal or aluminium as per SAP number"," Eskom DDT-3098","YES"]
[null,"1.1.6.4",null,"NON TENSION JOINT SET\n\n- Conductor application as per SAP number"," Eskom DDT-3098","YES"]
[null,"1.1.6.5",null,"NON TENSION JOINT SET\n\n- Colour code as per SAP number "," Eskom DDT-3098","YES"]
[null,"1.1.6.6",null,"NON TENSION JOINT SET\n\n- Barrel equiped with centre plug"," Eskom DDT-3098","YES"]
[null,"1.1.6.7",null,"NON TENSION JOINT SET\n\n- Filled with jointing compound and capped"," Eskom DDT-3098","YES"]
[null,"1.1.6.8",null,"NON TENSION JOINT SET\n\n- Individually packed in sealed plastic bag"," Eskom DDT-3098","YES"]
[null,"1.1.6.9",null,"NON TENSION JOINT SET\n\n- For use with crimping tool as per SAP number"," Eskom DDT-3098","YES"]
[null,"1.1.7",null,"Item sample required, upon request from Eskom  (As per the Technical Criteria Document)",null,"YES"]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Material Grade - Bi-metal or Aluminium as per clause 3.1.9 of 240-75883110",null,"YES"]
[null,"1.2.2",null,"Material - Bi-metal fitting as per clause 3.1.10 of 240-75883110",null,"YES"]
[null,"1.2.3",null,"Material compound -  Electrical jointing compound as per clause 3.2 of 240-75883110",null,"YES"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,3,null,"Packaging"]
[null,3.1,null,"Packaging material, method and maximum quantity, not exceeding 30kg.",null,"Supplier to provide details"]
[null,3.2,null,"Markings to be stipulated.",null,"Supplier to provide details"]
[null,3.3,null,"Installation instructions provided in packaging.",null,"YES"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,2,41,3],[45,2,45,3]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" DDT-3098 - NON-TENSION JOINT"]
["SAP No: 0214100"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":25,"n_cols":5,"rows_kept":25,"merged":[[0,0,0,5],[1,0,1,6],[2,0,2,6],[3,1,3,4],[4,0,4,6],[16,1,16,7],[17,1,17,7],[20,1,20,2],[24,1,24,2]]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
["DDT-3098 - NON-TENSION JOINT"]
[null,"The test reports are required for the selected SAP number listed on this sheet."]
["SAP No: 0214100"]
[]
[null,1,2,3,4]
[null,"Item ","Description","Standard","Report No."]
[null,"2.2.1","Tensile load for phase & neutral","SANS 50483"]
[null,"2.2.2","Dielectrical voltage test ","SANS 50483"]
[null,"2.2.3","Water tightening test ","SANS 50483"]
[null,"2.2.4","Low temperature assembly test ","SANS 50483"]
[null,"2.2.5","Corrosion ageing test ","SANS 50483"]
[null,"2.2.6","Climatic ageing test ","SANS 50483"]
[null,"2.2.7","Electrical ageing test ","SANS 50483"]
[null,"2.2.8","Endurance test ","SANS 50483"]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,"Sign",null,null,"Date"]