{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["TEC Development Guidelines ","Response Guidelines","TEC","Definitions and Abbreviations"],"not_rendered":{"images":1,"external_links":2,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"TEC Development Guidelines ","index":0,"n_rows":11,"n_cols":2,"rows_kept":11,"merged":[[1,1,1,9],[2,0,2,9],[3,1,3,9],[5,0,5,9],[6,1,6,9],[9,0,9,9],[10,1,10,9]]}
[]
[null,"This Tab provides guidance to the TET on how the evaluation criteria must be structured and where information can be sourced.\nDelete this tab before the TEC is published with the RFP."]
["Response Guidelines"]
[null,"Once all criteria questions are complete revise the response guidelines tab, the information provided is for vendors to understand what is required of them. \nYou may need to rename or remove the demo tab if it is not applicable.\nRead through all the information removing what is not applicable and adding important information you want vendors to be aware of.\nThe template has one reference sheet (Definitions and Abbreviations) it may be necessary to provide vendors with more reference information, which can be listed here."]
[]
["TEC Tab"]
[null,"Gatekeepers are captured here - Gatekeepers are limited to legislative and compliance related criteria only.\nIf a vendor fails any of the gatekeepers it is not necessary to evaluate the vendor further.\nDesktop evaluations and demonstrations are separate evaluation stages and the scores may not be added together.\nEnsure each stage has a defined threshold\nEnsure the weight of each questions adds to 100%\nThe category column may be removed or edited as required\nThe EL must check the formulas to ensure all are working correctly before evaluations begin."]
[]
[]
["Demonstration tab"]
[null,"The demonstration tab has important notes to vendors in rows 10 to 13, read these and edit as required by your criteria and evaluation plan. After editing, there must not be any blue text remaining.\nIf a requirement was evaluated during the desktop evaluation, it may be evaluated again at the demo if there is a need to see/verify the information. \nThe demonstration duration agreed to must be strictly adhered to for all vendors for fairness. "]

{"sheet":"Response Guidelines","index":1,"n_rows":181,"n_cols":4,"rows_kept":181,"merged":[[1,1,1,10],[2,2,2,3],[3,1,3,2],[4,1,4,10],[6,1,6,2],[7,2,7,10],[8,1,8,2],[9,1,9,2],[11,1,11,10],[13,3,13,10],[66,1,67,1]]}
[]
[null,"Tenderer to take note of the following key instructions:"]
[]
[]
[null,"Technical Evaluation Guidelines"]
[]
[]
[null,"*"," "]
[]
[]
[]
[null,"Reference Information"]
[]
[null,"*","Definitions and Abbreviations\n","Provides information on the definitions and abbreviations used in the Evaluation workbook."]
{"$rows_empty":46}
[null,null,"Data Ranges"]
[null,null,"Gatekeeper drop down"]
[null,null,"Pass"]
[null,null,"Fail"]
[]
[null,null,"Summary highlight based on GK response"]
[null,null,{"$f":"IF(AND('[2]Scoring Summary'!F10=\"Pass\",'[2]Scoring Summary'!F11=\"Pass\"),\"Pass\",\"\")","v":""}]
[null,null,{"$f":"IF(OR('[2]Scoring Summary'!F10=\"Fail\",'[2]Scoring Summary'!F11=\"Fail\"),\"Fail\",\"\")","v":""}]
[]
[null,null,"Priority Rating"]
[null,null,0,"No interest"]
[null,null,1,"Nice to have"]
[null,null,2,"Useful"]
[null,null,3,"Important"]
[null,null,4,"Very important"]
[null,null,5,"Critical"]
[null,null,6,"Show stopper"]
[]
[]
[null,null,"Weight calculation formula"]
[null,null,"Divide by","category weight"]
[null,null,1,{"v":1,"d":"100%"}]
[null,null,1.0101010101010102,{"v":0.99,"d":"99%"}]
[null,null,1.0204081632653061,{"v":0.98,"d":"98%"}]
[null,null,1.0309278350515465,{"v":0.97,"d":"97%"}]
[null,null,1.0416666666666667,{"v":0.96,"d":"96%"}]
[null,null,1.0526315789473684,{"v":0.95,"d":"95%"}]
[null,null,1.0638297872340425,{"v":0.94,"d":"94%"}]
[null,null,1.075268817204301,{"v":0.93,"d":"93%"}]
[null,null,1.0869565217391304,{"v":0.92,"d":"92%"}]
[null,null,1.0989010989010988,{"v":0.91,"d":"91%"}]
[null,null,1.1111111111111112,{"v":0.9,"d":"90%"}]
[null,null,1.1235955056179776,{"v":0.89,"d":"89%"}]
[null,null,1.1363636363636365,{"v":0.88,"d":"88%"}]
[null,null,1.1494252873563218,{"v":0.87,"d":"87%"}]
[null,null,1.1627906976744187,{"v":0.86,"d":"86%"}]
[null,null,1.1764705882352942,{"v":0.85,"d":"85%"}]
[null,null,1.1904761904761905,{"v":0.84,"d":"84%"}]
[null,null,1.2048192771084338,{"v":0.83,"d":"83%"}]
[null,null,1.2195121951219512,{"v":0.82,"d":"82%"}]
[null,null,1.2345679012345678,{"v":0.81,"d":"81%"}]
[null,null,1.25,{"v":0.8,"d":"80%"}]
[null,null,1.2658227848101264,{"v":0.79,"d":"79%"}]
[null,null,1.282051282051282,{"v":0.78,"d":"78%"}]
[null,null,1.2987012987012987,{"v":0.77,"d":"77%"}]
[null,null,1.3157894736842106,{"v":0.76,"d":"76%"}]
[null,null,1.3333333333333333,{"v":0.75,"d":"75%"}]
[null,null,1.3513513513513513,{"v":0.74,"d":"74%"}]
[null,null,1.36986301369863,{"v":0.73,"d":"73%"}]
[null,null,1.3888888888888888,{"v":0.72,"d":"72%"}]
[null,null,1.4084507042253522,{"v":0.71,"d":"71%"}]
[null,null,1.4285714285714286,{"v":0.7,"d":"70%"}]
[null,null,1.4492753623188408,{"v":0.69,"d":"69%"}]
[null,null,1.4705882352941175,{"v":0.68,"d":"68%"}]
[null,null,1.4925373134328357,{"v":0.67,"d":"67%"}]
[null,null,1.5151515151515151,{"v":0.66,"d":"66%"}]
[null,null,1.5384615384615383,{"v":0.65,"d":"65%"}]
[null,null,1.5625,{"v":0.64,"d":"64%"}]
[null,null,1.5873015873015872,{"v":0.63,"d":"63%"}]
[null,null,1.6129032258064517,{"v":0.62,"d":"62%"}]
[null,null,1.639344262295082,{"v":0.61,"d":"61%"}]
[null,null,1.6666666666666667,{"v":0.6,"d":"60%"}]
[null,null,1.6949152542372883,{"v":0.59,"d":"59%"}]
[null,null,1.7241379310344829,{"v":0.58,"d":"58%"}]
[null,null,1.7543859649122808,{"v":0.57,"d":"57%"}]
[null,null,1.7857142857142856,{"v":0.56,"d":"56%"}]
[null,null,1.8181818181818181,{"v":0.55,"d":"55%"}]
[null,null,1.8518518518518516,{"v":0.54,"d":"54%"}]
[null,null,1.8867924528301885,{"v":0.53,"d":"53%"}]
[null,null,1.923076923076923,{"v":0.52,"d":"52%"}]
[null,null,1.9607843137254901,{"v":0.51,"d":"51%"}]
[null,null,2,{"v":0.5,"d":"50%"}]
[null,null,2.0408163265306123,{"v":0.49,"d":"49%"}]
[null,null,2.0833333333333335,{"v":0.48,"d":"48%"}]
[null,null,2.127659574468085,{"v":0.47,"d":"47%"}]
[null,null,2.1739130434782608,{"v":0.46,"d":"46%"}]
[null,null,2.2222222222222223,{"v":0.45,"d":"45%"}]
[null,null,2.272727272727273,{"v":0.44,"d":"44%"}]
[null,null,2.3255813953488427,{"v":0.43,"d":"43%"}]
[null,null,2.3809523809523867,{"v":0.42,"d":"42%"}]
[null,null,2.4390243902439086,{"v":0.41,"d":"41%"}]
[null,null,2.500000000000006,{"v":0.4,"d":"40%"}]
[null,null,2.5641025641025705,{"v":0.39,"d":"39%"}]
[null,null,2.631578947368428,{"v":0.38,"d":"38%"}]
[null,null,2.70270270270271,{"v":0.37,"d":"37%"}]
[null,null,2.7777777777777857,{"v":0.36,"d":"36%"}]
[null,null,2.85714285714287,{"v":0.35,"d":"35%"}]
[null,null,2.941176470588244,{"v":0.34,"d":"34%"}]
[null,null,3.030303030303039,{"v":0.33,"d":"33%"}]
[null,null,3.1250000000000098,{"v":0.32,"d":"32%"}]
[null,null,3.2258064516129137,{"v":0.31,"d":"31%"}]
[null,null,3.3333333333333446,{"v":0.3,"d":"30%"}]
[null,null,3.4482758620689777,{"v":0.29,"d":"29%"}]
[null,null,3.571428571428584,{"v":0.28,"d":"28%"}]
[null,null,3.703703703703717,{"v":0.27,"d":"27%"}]
[null,null,3.846153846153861,{"v":0.26,"d":"26%"}]
[null,null,4.000000000000016,{"v":0.25,"d":"25%"}]
[null,null,4.166666666666684,{"v":0.24,"d":"24%"}]
[null,null,4.34782608695654,{"v":0.23,"d":"23%"}]
[null,null,4.545454545454566,{"v":0.22,"d":"22%"}]
[null,null,4.761904761904785,{"v":0.21,"d":"21%"}]
[null,null,5.000000000000025,{"v":0.2,"d":"20%"}]
[null,null,5.26315789473687,{"v":0.19,"d":"19%"}]
[null,null,5.5555555555555864,{"v":0.18,"d":"18%"}]
[null,null,5.882352941176505,{"v":0.17,"d":"17%"}]
[null,null,6.250000000000039,{"v":0.16,"d":"16%"}]
[null,null,6.666666666666711,{"v":0.15,"d":"15%"}]
[null,null,7.142857142857195,{"v":0.14,"d":"14%"}]
[null,null,7.692307692307751,{"v":0.13,"d":"13%"}]
[null,null,8.333333333333403,{"v":0.12,"d":"12%"}]
[null,null,9.090909090909173,{"v":0.11,"d":"11%"}]
[null,null,10.0000000000001,{"v":0.1,"d":"10%"}]
[null,null,11.111111111111235,{"v":0.09,"d":"9%"}]
[null,null,12.500000000000156,{"v":0.08,"d":"8%"}]
[null,null,14.28571428571449,{"v":0.07,"d":"7%"}]
[null,null,16.666666666666917,{"v":0.06,"d":"6%"}]
[null,null,20.0000000000004,{"v":0.05,"d":"5%"}]
[null,null,25.000000000000625,{"v":0.04,"d":"4%"}]
[null,null,33.333333333334444,{"v":0.03,"d":"3%"}]
[null,null,50.000000000002494,{"v":0.02,"d":"2%"}]
[null,null,100.0000000000099,{"v":0.01,"d":"1%"}]

{"sheet":"TEC","index":2,"n_rows":117,"n_cols":12,"rows_kept":117,"merged":[[1,3,1,11],[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,14,4],[14,5,14,6],[16,0,30,0],[16,1,30,1],[16,2,20,2],[16,3,20,3],[16,4,20,4],[16,5,20,5],[16,6,20,6],[16,7,20,7],[16,8,18,8],[16,9,18,9],[16,10,20,10],[16,11,20,11],[19,8,20,8],[19,9,20,9],[21,2,25,2],[21,3,25,3],[21,4,25,4],[21,5,25,5],[21,6,25,6],[21,7,25,7],[21,8,23,8],[21,9,23,9],[21,10,25,10],[21,11,25,11],[24,8,25,8],[24,9,25,9],[26,2,30,2],[26,3,30,3],[26,4,30,4],[26,5,30,5],[26,6,30,6],[26,7,30,7],[26,8,28,8],[26,9,28,9],[26,10,30,10],[26,11,30,11],[29,8,30,8],[29,9,30,9],[31,0,45,0],[31,1,45,1],[31,2,35,2],[31,3,35,3],[31,4,35,4],[31,5,35,5],[31,6,35,6],[31,7,35,7],[31,8,33,8],[31,9,33,9],[31,10,35,10],[31,11,35,11],[34,8,35,8],[34,9,35,9],[36,2,40,2],[36,3,40,3],[36,4,40,4],[36,5,40,5],[36,6,40,6],[36,7,40,7],[36,8,38,8],[36,9,38,9],[36,10,40,10],[36,11,40,11],[39,8,40,8],[39,9,40,9],[41,2,45,2],[41,3,45,3],[41,4,45,4],[41,5,45,5],[41,6,45,6],[41,7,45,7],[41,8,43,8],[41,9,43,9],[41,10,45,10],[41,11,45,11],[44,8,45,8],[44,9,45,9],[46,0,65,0],[46,1,65,1],[46,2,50,2],[46,3,50,3],[46,4,50,4],[46,5,50,5],[46,6,50,6],[46,7,50,7],[46,8,48,8],[46,9,48,9],[46,10,50,10],[46,11,50,11],[49,8,50,8],[49,9,50,9],[51,2,55,2],[51,3,55,3],[51,4,55,4],[51,5,55,5],[51,6,55,6],[51,7,55,7],[51,8,53,8],[51,9,53,9],[51,10,55,10],[51,11,55,11],[54,8,55,8],[54,9,55,9],[56,2,60,2],[56,3,60,3],[56,4,60,4],[56,5,60,5],[56,6,60,6],[56,7,60,7],[56,8,58,8],[56,9,58,9],[56,10,60,10],[56,11,60,11],[59,8,60,8],[59,9,60,9],[61,2,65,2],[61,3,65,3],[61,4,65,4],[61,5,65,5],[61,6,65,6],[61,7,65,7],[61,8,63,8],[61,9,63,9],[61,10,65,10],[61,11,65,11],[64,8,65,8],[64,9,65,9],[66,0,75,0],[66,1,75,1],[66,2,70,2],[66,3,70,3],[66,4,70,4],[66,5,70,5],[66,6,70,6],[66,7,70,7],[66,8,68,8],[66,9,68,9],[66,10,70,10],[66,11,70,11],[69,8,70,8],[69,9,70,9],[71,2,75,2],[71,3,75,3],[71,4,75,4],[71,5,75,5],[71,6,75,6],[71,7,75,7],[71,8,73,8],[71,9,73,9],[71,10,75,10],[71,11,75,11],[74,8,75,8],[74,9,75,9],[76,0,95,0],[76,1,95,1],[76,2,80,2],[76,3,80,3],[76,4,80,4],[76,5,80,5],[76,6,80,6],[76,7,80,7],[76,8,78,8],[76,9,78,9],[76,10,80,10],[76,11,80,11],[79,8,80,8],[79,9,80,9],[81,2,85,2],[81,3,85,3],[81,4,85,4],[81,5,85,5],[81,6,85,6],[81,7,85,7],[81,8,83,8],[81,9,83,9],[81,10,85,10],[81,11,85,11],[84,8,85,8],[84,9,85,9],[86,2,90,2],[86,3,90,3],[86,4,90,4],[86,5,90,5],[86,6,90,6],[86,7,90,7],[86,8,88,8],[86,9,88,9],[86,10,90,10],[86,11,90,11],[89,8,90,8],[89,9,90,9],[91,2,95,2],[91,3,95,3],[91,4,95,4],[91,5,95,5],[91,6,95,6],[91,7,95,7],[91,8,93,8],[91,9,93,9],[91,10,95,10],[91,11,95,11],[94,8,95,8],[94,9,95,9],[96,0,105,0],[96,1,105,1],[96,2,100,2],[96,3,100,3],[96,4,100,4],[96,5,100,5],[96,6,100,6],[96,7,100,7],[96,8,98,8],[96,9,98,9],[96,10,100,10],[96,11,100,11],[99,8,100,8],[99,9,100,9],[101,2,105,2],[101,3,105,3],[101,4,105,4],[101,5,105,5],[101,6,105,6],[101,7,105,7],[101,8,103,8],[101,9,103,9],[101,10,105,10],[101,11,105,11],[104,8,105,8],[104,9,105,9],[106,0,115,0],[106,1,115,1],[106,2,110,2],[106,3,110,3],[106,4,110,4],[106,5,110,5],[106,6,110,6],[106,7,110,7],[106,8,108,8],[106,9,108,9],[106,10,110,10],[106,11,110,11],[109,8,110,8],[109,9,110,9],[111,2,115,2],[111,3,115,3],[111,4,115,4],[111,5,115,5],[111,6,115,6],[111,7,115,7],[111,8,113,8],[111,9,113,9],[111,10,115,10],[111,11,115,11],[114,8,115,8],[114,9,115,9],[116,8,116,9]]}
[]
[{"$nulls":3},"Eskom Group IT:  Technical Evaluation Criteria"]
[]
[{"$nulls":3},"Tender Number:"]
[{"$nulls":3},"Transaction Description:","Network time Protocol Server device for supply, maintenance and support for period of five (5) years."]
[{"$nulls":3},"Technical Threshold:",{"v":0.8,"d":"80%"}]
[{"$nulls":3},"Tenderer Registered Name:"]
[{"$nulls":3},"Evaluator Name and Surname:"]
[{"$nulls":3},"Date of Evaluation"]
[{"$nulls":3},"Evaluator Signature"]
[]
[]
[]
[]
["Categories","Category Weight","Item #","Technical Requirements",null,"Vendor Responses",null,"Evaluator Scores"]
[{"$nulls":3},"Business requirements ","Mandatory Returnables - Evidence below to be provided in the technical file and numbered to align with each criteria question. ","Vendor Response: Vendor to provide answer the questions below and provide detail in their tender submission","Vendor Evidence: Location of Supporting Document/detailed response in your tender submission (state the file number, section & page number)","Weight / Max score","Scoring guideline","Selection Options","Evaluators Response","Evaluator comments"]
["Time Accuracy & Hardware",{"$f":"SUM(H17:H31)","v":{"v":0.15000000000000002,"d":"15.0%"}},1,"Reference Clock Technology","Must utilize multiple atomic references (cesium/rubidium) with GPS/GNSS synchronization capability 25. Device must maintain stratum 1 operation with ≤100 nanoseconds RMS accuracy to UTC.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E17","v":"Must utilize multiple atomic references (cesium/rubidium) with GPS/GNSS synchronization capability 25. Device must maintain stratum 1 operation with ≤100 nanoseconds RMS accuracy to UTC."},{"$f":"H17","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[]
[null,null,2,"Holdover Stability","Must feature OCXO oscillator with holdover stability of ≤250ms/year or rubidium atomic clock with ≤1ms/year stability during reference signal loss.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E22","v":"Must feature OCXO oscillator with holdover stability of ≤250ms/year or rubidium atomic clock with ≤1ms/year stability during reference signal loss."},{"v":0.05,"d":"5.00%"}]
[{"$nulls":8},"6-7 c",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"4-5 c",{"v":0.06,"d":"6.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,3,"Timestamping Precision","Must implement hardware-based timestamping on all network interfaces with precision ≤15 nanoseconds.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E27","v":"Must implement hardware-based timestamping on all network interfaces with precision ≤15 nanoseconds."},{"$f":"H27","v":{"v":0.05,"d":"5.00%"}}]
[]
[{"$nulls":8},"5 - 10 c",{"v":0.1,"d":"10.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0.05,"d":"5.00%"}]
["Security Capabilities",{"$f":"SUM(H32:H46)","v":{"v":0.15000000000000002,"d":"15.0%"}},4,"Authentication & Encryption","Must support NTP authentication with SHA-256 or better, TACACS+/RADIUS integration, and encrypted communications (IPsec/TLS).",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E32","v":"Must support NTP authentication with SHA-256 or better, TACACS+/RADIUS integration, and encrypted communications (IPsec/TLS)."},{"v":0.05,"d":"5.00%"}]
[{"$nulls":8},"6-7 provinces",{"v":0.1,"d":"10.00%"}]
[{"$nulls":8},"4-5 provinces",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,5,"Threat Protection","Must include DoS detection/protection, NTP reflector hardening, and GPS spoofing/jamming detection (BlueSky technology or equivalent).",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E37","v":"Must include DoS detection/protection, NTP reflector hardening, and GPS spoofing/jamming detection (BlueSky technology or equivalent)."},{"$f":"H37","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,6,"Access Controls","Must implement role-based access control, secure management interfaces (SSH/TLS), and ability to disable insecure protocols (telnet/FTP).",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E42","v":"Must implement role-based access control, secure management interfaces (SSH/TLS), and ability to disable insecure protocols (telnet/FTP)."},{"$f":"H42","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
["Management & Monitoring",{"$f":"SUM(H47:H66)","v":{"v":0.2,"d":"20.0%"}},7,"Power & Hardware Redundancy","Must include dual power supplies, hot-swappable components, and modular design for failure isolation.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E47","v":"Must include dual power supplies, hot-swappable components, and modular design for failure isolation."},{"$f":"H47","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6 functions",{"v":0.18,"d":"18.00%"}]
[{"$nulls":8},"5 functions",{"v":0.15,"d":"15.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0.03,"d":"3.00%"}]
[null,null,8,"Industry Certifications","Must support multiple simultaneous time sources (GNSS, PTP, external clocks) with automatic failover capability.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E52","v":"Must support multiple simultaneous time sources (GNSS, PTP, external clocks) with automatic failover capability."},{"$f":"H52","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,9,"Management Interface","Web-based management with high-security cipher suite and extensive REST API following OpenAPI specification 3.0 for automation integration ",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E57","v":"Web-based management with high-security cipher suite and extensive REST API following OpenAPI specification 3.0 for automation integration "},{"$f":"H57","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,10,"Integration Options","Support for enterprise monitoring systems via SNMP, syslog, and API integrations for unified network management.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E62","v":"Support for enterprise monitoring systems via SNMP, syslog, and API integrations for unified network management."},{"$f":"H62","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
["Reliability & Redundancy",{"$f":"SUM(H67:H76)","v":{"v":0.1,"d":"10.0%"}},11,"Power & Hardware Redundancy","Must include dual power supplies, hot-swappable components, and modular design for failure isolation.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E67","v":"Must include dual power supplies, hot-swappable components, and modular design for failure isolation."},{"$f":"H67","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6 functions",{"v":0.18,"d":"18.00%"}]
[{"$nulls":8},"5 functions",{"v":0.15,"d":"15.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0.03,"d":"3.00%"}]
[null,null,12,"Industry Certifications","Must support multiple simultaneous time sources (GNSS, PTP, external clocks) with automatic failover capability.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E72","v":"Must support multiple simultaneous time sources (GNSS, PTP, external clocks) with automatic failover capability."},{"$f":"H72","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,{"v":0.2,"d":"20%"},13,"Industry Certifications","Should comply with the South African National Cybersecurity Policy Framework (NCPF) and Critical Infrastructure Protection Act (CIPA) requirements for government deployments",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E77","v":"Should comply with the South African National Cybersecurity Policy Framework (NCPF) and Critical Infrastructure Protection Act (CIPA) requirements for government deployments"},{"$f":"H77","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6-7 c",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"4-5 c",{"v":0.06,"d":"6.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,14,"Industry Compliance","Must function as IEEE 1588 PTP grandmaster with multiple port/profile output options for precision timing applications ",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E82","v":"Must function as IEEE 1588 PTP grandmaster with multiple port/profile output options for precision timing applications "},{"$f":"H82","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6-7 c",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"4-5 c",{"v":0.06,"d":"6.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,15,"Network Architecture","the device must comply with IEC 61850 standards for utility substations and support for PRP/HSR lossless network architectures",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E87","v":"the device must comply with IEC 61850 standards for utility substations and support for PRP/HSR lossless network architectures"},{"$f":"H87","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6-7 c",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"4-5 c",{"v":0.06,"d":"6.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,16,"Multi-Protocol \nOperation","Device must concurrency support for NTP, PTP, SyncE, IRIG-B, 1PPS, ToD and other timing protocols to meet diverse infrastructure needs",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E92","v":"Device must concurrency support for NTP, PTP, SyncE, IRIG-B, 1PPS, ToD and other timing protocols to meet diverse infrastructure needs"},{"$f":"H92","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6-7 c",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"4-5 c",{"v":0.06,"d":"6.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
["Scalability & Performance",{"$f":"SUM(H97:H106)","v":{"v":0.1,"d":"10.0%"}},17,"Network Capacity","Must support ≥10 GbE interfaces with capability to handle ≥500,000 NTP requests/second 10.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E97","v":"Must support ≥10 GbE interfaces with capability to handle ≥500,000 NTP requests/second 10."},{"$f":"H97","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6-7 provinces",{"v":0.1,"d":"10.00%"}]
[{"$nulls":8},"4-5 provinces",{"v":0.08,"d":"8.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[null,null,18,"Protocol Support","Must simultaneously support NTP, SNTP, PTP with IPv4/IPv6 compatibility and multicast/broadcast modes 58.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E102","v":"Must simultaneously support NTP, SNTP, PTP with IPv4/IPv6 compatibility and multicast/broadcast modes 58."},{"$f":"H102","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
["Provider Expertise",{"$f":"SUM(H107:H116)","v":{"v":0.1,"d":"10.0%"}},19,"Implementation Services","The tender must provide in the submission a list of the functions available with the system with a screenshot as evidence that the function is available.",null,null,{"v":0.05,"d":"5.00%"},"Screenshots provided",{"$f":"H107","v":{"v":0.05,"d":"5.00%"}}]
[{"$nulls":8},"6 functions",{"v":0.18,"d":"18.00%"}]
[{"$nulls":8},"5 functions",{"v":0.15,"d":"15.00%"}]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0.03,"d":"3.00%"}]
[null,null,20,"Support & Maintenance","Must include 24/7 monitoring, ≤1-hour response time for critical issues, and firmware/security updates.",null,null,{"v":0.05,"d":"5.00%"},{"$f":"E112","v":"Must include 24/7 monitoring, ≤1-hour response time for critical issues, and firmware/security updates."},{"$f":"H112","v":{"v":0.05,"d":"5.00%"}}]
[]
[]
[{"$nulls":8},"Does not comply to mandatory returnable system requirements",{"v":0,"d":"0.00%"}]
[{"$nulls":9},{"v":0,"d":"0.00%"}]
[{"$nulls":3},"Total",{"$nulls":3},{"$f":"SUM(H17:H116)","v":{"v":1.0000000000000002,"d":"100%"}},"Final Score",null,{"$f":"SUM(K77:K116)","v":{"v":0,"d":"0%"}}]

{"sheet":"Definitions and Abbreviations","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"merged":[[1,1,1,2],[16,1,16,2]]}
[]
[null,"Abbreviations"]
{"$rows_empty":14}
[null,"Definitions"]