{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["Rietvlei (HO)","Central Depot (BWD)","Zwartkopies","Zuikerbosch","Vereeniging","Analytical Services","Distribution Sites"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Rietvlei (HO)","index":0,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[null,"C2.2. PRICING SCHEDULES / BILLS OF QUANTITIES (BoQ)"]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure"]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Central Depot (BWD)","index":1,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Zwartkopies","index":2,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Zuikerbosch","index":3,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Vereeniging","index":4,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Analytical Services","index":5,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT 6 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category 6 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP Cat6 Fly lead 10m",null,1]
[6,"UTP Cat6 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]

{"sheet":"Distribution Sites","index":6,"n_rows":261,"n_cols":5,"rows_kept":261,"merged":[[0,1,0,4],[19,0,19,4],[27,0,27,4],[61,0,61,4],[116,0,116,4],[140,0,140,4],[198,0,198,4],[226,0,226,4],[230,0,230,4],[258,2,258,7],[259,2,259,7],[260,2,260,7]]}
[null,"RAND WATER"]
[]
[null,null,"UNIT PRICE","QUANTITY","TOTAL PRICE"]
["A","SERVER ROOM"]
[1,"Environmental Enclosure",null,1]
[null,"Suppply abd install 43 U IP 55 rated weatherproof enclosure 360 access Dimensions H: 2200mm, W 850mm, L1000,Glass front door, with PDU , Surge & Lightning protected unit, Acess Conroll 3 point Pin locking system with remote management with internal Air-contitioning unit, and with Dual detector operationg sysytem, aerosol Fire Extinguisher.",null,1]
[null,"Internal Air-contitioning unit 2KW",null,1]
[null,"Internal Air-contitioning unit 4KW",null,1]
[null,"Internal Air-contitioning unit 6KW",null,1]
[null,"UPS and rail kit 2kVA",null,1]
[null,"UPS and rail kit 5kVA",null,1]
[null,"UPS and rail kit 10kVA",null,1]
[null,"UPS and rail kit 15kVA",null,1]
[null,"On-site support at sites",null,1]
[null,"Labour - Normal Hours",null,1]
[null,"Labour - After Hours",null,1]
[null,"Travelling",null,1]
[null,"Accommodation",null,1]
[null,"Meals and Out of town Allowances ",null,1]
[]
[2,"DATA CABLING"]
[1,"Complete UTP CAT-8 Data Point flush mount with twin insert, blank cover, 3m Fly Lead, 2m Patch Lead, Labelling & Testing (average of 70m per point)",null,1]
[2,"50 x 50 Punch out plate",null,1]
[3,"24 Port Category-8 patch panel",null,1]
[4,"I U brush panel (2 rings)",null,1]
[5,"UTP CAT-8 Fly lead 10m",null,1]
[6,"UTP CAT-8 Fly lead 5m",null,1]
[]
[3,"ENCLOSURES"]
[1,"9U  Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[2,"12U x 650 mm Swing Frame 450mm + 200mm Collar (with steel perforated door)",null,1]
[null,"2 Way Fan  Units Wired Complete With Sponge Filters",null,1]
[null,"6 Way Metal  ",null,1]
[3,"25U x 800 x 800 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 800 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[4,"25U x 800 x 1000 Cabinet,  Perforated Front & Split Perfotated Rear Doors, (Black)",null,1]
[null,"Gland Plates, Front & Rear Punch Profiles, 4 x Adjustable Feet ",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"10 Way Power (1,8m Cord)",null,1]
[null,"300mm Cable Tray",null,1]
[null,"Plinth 800 x 1000 x 150",null,1]
[null,"Base Entry Panel (Left & Right)",null,1]
[5,"42U x 600 x 800 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[6,"42U x 600 x 1000 Cabinet, Perforateds Front & Double Perforated Rear Doors, (Black)",null,1]
[null,"10 Way Power",null,1]
[null,"4 Way Fan Unit",null,1]
[null,"800 x 600 x 150mm Plinth",null,1]
[null,"Brush Panel Bottom Entry (2Left + 2 Right)",null,1]
[null,"300mm Cable Tray",null,1]
[]
[4,"FIBRE"]
[1,"Singlemode HDD 8 Core ",null,1]
[{"$f":"A64+1","v":2},"Singlemode HDD 12 Core ",null,1]
[{"$f":"A65+1","v":3},"Singlemode HDD 24 Core ",null,1]
[4,"Multimode HDD 8 Core ",null,1]
[5,"Multimode HDD 12 Core ",null,1]
[6,"Multimode HDD 24 Core ",null,1]
[7,"Splice Tray front plate and box, entry gland, splice cassette, blanks back and front",null,1]
[8,"Splice Cassette",null,1]
[9,"ST Multimode 1m Unjacketed Pigtail",null,1]
[10,"ST Single mode 1m Unjacketed Pigtail",null,1]
[11,"SC  - (10/125) 1m SC Unjacketed Pigtail",null,1]
[12,"SC  - (50/125) 1m SC Unjacketed Pigtail",null,1]
[13,"LC Multimode 1m Unjacketed Pigtail",null,1]
[14,"LC Single mode 1m Unjacketed Pigtail",null,1]
[15,"Midcouplers - Multimode SC Midcoupler Duplex",null,1]
[16,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[17,"Midcouplers - Multimode LC Midcoupler Duplex",null,1]
[18,"Midcouplers - Single mode SC Midcoupler Duplex",null,1]
[19,"Midcouplers - Single mode ST Midcoupler Duplex",null,1]
[20,"Midcouplers - Single mode LC Midcoupler Duplex",null,1]
[21,"Midcouplers - Multimode ST Midcoupler Duplex",null,1]
[22,"Fibre Labelling",null,1]
[23,"Fibre OTDR Testing",null,1]
[24,"Fibre Splicing",null,1]
[25,"Splice Protectors",null,1]
[26,"2 Way  Dome Joint",null,1]
[27,"3 Way  Dome Joint",null,1]
[28,"4 Way  Dome Joint",null,1]
[29,"Termination Box - J2",null,1]
[30,"Fibre patch cord duplex multimode 1m LC-LC  ",null,1]
[31,"Fibre patch cord duplex multimode 1m SC-LC",null,1]
[32,"Fibre patch cord duplex multimode 1m SC-SC",null,1]
[33,"Fibre patch cord duplex multimode 3m LC-LC  ",null,1]
[34,"Fibre patch cord duplex multimode 3m SC-LC  ",null,1]
[35,"Fibre patch cord duplex multimode 3m SC-SC  ",null,1]
[36,"Fibre patch cord duplex single mode 1m LC-LC  ",null,1]
[37,"Fibre patch cord duplex single mode 1m SC-LC",null,1]
[38,"Fibre patch cord duplex single mode 1m SC-SC",null,1]
[39,"Fibre patch cord duplex single mode 3m LC-LC  ",null,1]
[40,"Fibre patch cord duplex single mode 3m SC-LC",null,1]
[41,"Fibre patch cord duplex single mode 3m SC-SC  ",null,1]
[42,"Compression GLAND  Size 1  pvc black  - Fibre",null,1]
[43,"Compression GLAND  Size 2  pvc black - Fibre",null,1]
[44,"Dead End Clamp Fig 8 Cable - Catenary Wire",null,1]
[45,"Heat shrink Fibre 6.4mm clear",null,1]
[46,"Fibre Optic \"Warning\"/\"Caution\" Tag",null,1]
[47,"Pigtail Bolt & Socket M12/340MM",null,1]
[48,"S-Hook Welded",null,1]
[49,"S-Hook Double",null,1]
[50,"Thimble Dead Ends 9,2 - 9.4 MM",null,1]
[51,"Thimble Dead Ends 11.8MM",null,1]
[52,"Thimble Dead Ends 13.5",null,1]
[53,"Thimble Dead Ends 7.7 MM",null,1]
[]
[5,"POWER"]
[1,"Electrical normal power point",null,1]
[{"$f":"A119+1","v":2},"Electrical dedicated power point",null,1]
[{"$f":"A120+1","v":3},"Draw box 50mm",null,1]
[4,"16mm Feeder Cable",null,1]
[5,"Cable Surfex 2.5 x 2 core + Earth",null,1]
[6,"Cable Surfex 4 x 2 core + Earth",null,1]
[7,"Circuit Breaker 20 Amp, 5KA",null,1]
[8,"Circuit Breaker 30 Amp, 5KA",null,1]
[9,"Circuit Breaker 20 Amp, 6KA",null,1]
[10,"Circuit Breaker 32 Amp, 6KA",null,1]
[11,"Distribution Board, Surface Mountable 8 Way mounted",null,1]
[12,"Distribution Board, Surface Mountable 12 Way mounted",null,1]
[13,"Distribution Board, Surface Mountable 16 Way mounted",null,1]
[14,"Distribution Board, Surface Mountable 24 Way mounted",null,1]
[15,"Earth Leakage 60 Amp",null,1]
[16,"Earth Leakage 80 Amp",null,1]
[17,"Earth Rods (1.5m)",null,1]
[18,"Hubble Plug 32 Amp female switched Plug 3 PIN",null,1]
[19,"Hubble Plug 32 Amp Male Plug 3 PIN",null,1]
[20,"Isolator 60a new DB",null,1]
[21,"Isolator 80a new DB",null,1]
[22,"MCB Copper Bridge Bar in DB",null,1]
[]
[6,"INFRASTRUCTURE"]
[1,"Bosal Pipe 50mm (4m length)",null,1]
[{"$f":"A143+1","v":2},"50mm Bosal Pipe Hospital Saddles",null,1]
[{"$f":"A144+1","v":3},"50mm Bosal Pipe Couplings",null,1]
[4,"50mm Bosal Pipe Bend",null,1]
[5,"Bosal Pipe 32mm (4m length)",null,1]
[6,"32mm Bosal Pipe Hospital Saddles",null,1]
[7,"32mm Bosal Pipe Couplings",null,1]
[8,"32mm Bosal Pipe Bend",null,1]
[9,"Bosal Pipe 25mm (4m length)",null,1]
[10,"25mm Bosal Pipe Hospital Saddles",null,1]
[11,"25mm Bosal Pipe Couplings",null,1]
[12,"25mm Bosal Pipe Bend",null,1]
[13,"Core drilling 110mm /per hole",null,1]
[14,"Core drilling 200mm / per hole",null,1]
[15,"Core drilling 25mm / per hole",null,1]
[16,"Core drilling 50mm / per hole",null,1]
[17,"P801 Power Skirting X2.438m  Straight Channel Wire 1 Cover & Splices, anchors and washers",null,1]
[18,"P801 Power Skirting  45' Horizontal Elbow",null,1]
[19,"P801 Power Skirting  90' Horizontal Elbow",null,1]
[20,"P801 Power Skirting  90' Vertical Elbow ",null,1]
[21,"P801 Power Skirting  Divider Only PG",null,1]
[22,"P801 Power Skirting  End Cap",null,1]
[23,"P801 Power Skirting  Horizontal Tee Piece",null,1]
[24,"P801 Power Skirting  Vertical tee Piece ",null,1]
[25,"P802 Power Skirting X2.438m  Straight C/W 2 Cover & Splices,  anchors and washers",null,1]
[26,"P802 Power Skirting  45' Horizontal Elbow",null,1]
[27,"P802 Power Skirting  90' Horizontal Elbow",null,1]
[28,"P802 Power Skirting  90' Vertical Elbow (Flat)",null,1]
[29,"P802 Power Skirting  End Cap",null,1]
[30,"P802 Power Skirting  Horizontal Tee Piece",null,1]
[31,"P802 Power Skirting  Vertical tee Piece (Flat)",null,1]
[32,"16 X 25 Ega Pvc Length",null,1]
[33,"25 X 40 Ega Pvc Length",null,1]
[34,"40 X 40 Ega Pvc Length",null,1]
[35,"50 X 50 Ega Pvc Length",null,1]
[36,"100 X 40 Ega Pvc Length",null,1]
[37,"100 X 100 Ega Pvc Length",null,1]
[38,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[39,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[40,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[41,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[42,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[43,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[44,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[45,"Wire Mesh Cable Trays TEE 150 SPLICE CLAMP SET",null,1]
[46,"Wire Mesh Cable Trays TEE 200 SPLICE CLAMP SET",null,1]
[47,"Wire Mesh Cable Trays TEE 300 SPLICE CLAMP SET",null,1]
[48,"Wire Mesh Cable Trays 150MM 3M 50 X 50 SPLICE CLAMP SET",null,1]
[49,"Wire Mesh Cable Trays HQR BEND 150 SPLICE CLAMP SET",null,1]
[50,"Wire Mesh Cable Trays HQR BEND 200 SPLICE CLAMP SET",null,1]
[51,"Wire Mesh Cable Trays HQR BEND 300 SPLICE CLAMP SET",null,1]
[52,"Wire Mesh Cable Trays INT/EXT BEND 150 SPLICE CLAMP SET",null,1]
[53,"Wire Mesh Cable Trays INT/EXT BEND 200 SPLICE CLAMP SET",null,1]
[54,"Wire Mesh Cable Trays INT/EXT BEND 300 SPLICE CLAMP SET",null,1]
[55,"Ripple Draw Box Large",null,1]
[56,"Ripple Draw Box Small",null,1]
[]
[7,"CIVIL WORKS"]
[1,"Bedding - River sand when existing bedding cannot be utilized p/cubic metre",null,1]
[{"$f":"A201+1","v":2},"Break into existing manhole",null,1]
[{"$f":"A202+1","v":3},"Building Entry Double Pipe",null,1]
[4,"Building Entry Single Pipe",null,1]
[5,"Butt Welding E Dolomite sites",null,1]
[6,"Danger tape (skull & bone) p/m",null,1]
[7,"Flexi Pipe 110mm including 7mm nylon draw rope",null,1]
[8,"Nylon Draw Wire 7mm",null,1]
[9,"Heavy Duty Round Man-Hole 1200mm X 1200mm Construction & Building Material with Frame and lid including T-labelling",null,1]
[10,"Heavy Duty square Man-Hole 800mm X 800mm Construction & Building Material with round frame and lid including T-labelling sealing",null,1]
[11,"Imported backfill when trenching in rock ground p/cubic metre",null,1]
[12,"Medium Duty Man-Hole 450mm X 600mm X 68kg Construction & Building Material with frame and lid including T-labelling",null,1]
[13,"Pole Treated Wooden 10m",null,1]
[14,"Pole Treated Wooden 6m",null,1]
[15,"Reinforcing for casting of manhole 800mm x 800mm for heavy vehicle movement",null,1]
[16,"Reinstatement of Surfaces: Cement p/running metre",null,1]
[17,"Reinstatement of Surfaces: Gravel or paving or grass p/running metre",null,1]
[18,"Removal of surfaces road, tar & cement - Cutting ",null,1]
[19,"S Cantilever Brackets Single Standard 850 X 300",null,1]
[20,"Trenching Hard Rock 800(d) X 300(w) p/m including bedding, backfill, padding and compacting including warning and danger tape",null,1]
[21,"Trenching Hard Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[22,"Trenching Soft Gravel 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[23,"Trenching Soft Gravel 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[24,"Trenching Soft Rock 850 X 300 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[25,"Trenching Soft Rock 850 X 450 X p/m including bedding, backfill and compacting including warning and danger tape",null,1]
[26,"Warning Tape (barricading tape) p/m",null,1]
[]
[8,"UPS"]
[null,"2KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[null,"5KVA Rack Mountable True Online Double Conversion UPS with 10 – 15 min backup at 70% load",null,1]
[]
[9,"SERVICES"]
[1,"COC - Electrical Certification",null,1]
[{"$f":"A233+1","v":2},"Dismantling and Recovery of Infrastructure, cabinets and cables",null,1]
[{"$f":"A234+1","v":3},"Labour - 2 man team",null,1]
[4,"Labour - 3 man team",null,1]
[5,"Labour - 3 man team - Test and Repair data point",null,1]
[6,"Labour - 4 man team",null,1]
[7,"Labour - 2 man team After Hours",null,1]
[8,"Labour - 3 man team After Hours",null,1]
[9,"Labour - 4 man team After Hours",null,1]
[10,"Labour - Project Manager",null,1]
[11,"Removal of Debris from site",null,1]
[12,"Schematic Layout of Site",null,1]
[13,"Site Visit - Call Out Fee",null,1]
[14,"Site Visit for pre-installation",null,1]
[15,"Site Visit Sign Cabling Sign Off",null,1]
[16,"Travelling",null,1]
[17,"Accommodation",null,1]
[18,"Contengencies 15%",null,1]
[{"$f":"A250+1","v":19},"Site Establishment",null,1]
[{"$f":"A251+1","v":20},"Quote and Design",null,1]
[21,"Testing of Data points",null,1]
[null,"TOTAL EXCLUDING VAT"]
[null,"VAT * 15%"]
[null,"TOTAL INCLUDING VAT"]
[]
[]
[null,"BIDDER:"]
[null,"SIGNATURE:"]
[null,"DATE:"]