{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["A320"],"read":"whole","date_system":"1900"}

{"sheet":"A320","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"merged":[[18,0,18,5],[19,0,19,5]]}
[null,null,"Annexure A"]
["Critical Requirement","YES","NO"]
["A320-232 aircraft should be 2011 model or younger OR A320 NEO -2013 or younger"]
["A320-232 ETOPS (EASA/JAA 120 min) - IAE V2527-A5 OR A320 NEO - Pratt & Whitney GTF or CFM LEAP"]
["APS 3200 APU"]
["Compliance status with EU-OPS 1 - subpart K plus L requirements"]
["A320-232 increased design weights - MTOW to 77 t, MLW to 66 t, MZFW to 62.5 t (wv 012) or A320 Neo - MTOW to 79 t, MLW to 67.40 t, MZFW to 64.30 t and capability to increase max takeoff weight  "]
["Ventilation system for complete aft cargo hold"]
["Heating system for complete aft cargo hold"]
["Satcom plus minimum of 1 HF"]
["ENTERTAINMENT SYSTEM Dropdown Monitors and Audio"]
["Cockpit Door Survey System"]
["2 x Galleys and galley catering definition. Galley must be heated and cold similar to the LOPA"]
["Medical outlets in aft LH dado panel (230V/50Hz & 115V/60Hz)"]
["Medical outlets in fwd LH dado panel (230V/50hz and 115V/60Hz)"]
["Cargo holds fire extinguishers extended duration for ETOPS 120 min (A320)"]
["3 x Lavatories similar to the LOPA"]
[]
["Critical Requirement"]
["Avionic systems Equipment"]
["SYSTEM","VENDOR                ","PART NUMBER ","QUANTITY","YES","NO"]
["ELAC    ","THALES                           ","B372BBM",2]
["SEC                         ","THALES ","B372CAM0100        ",3]
["EADL     ","TELEDYNE ","2235300-21    ",1]
["SSFDR     ","HONEYWELL ","980-4700-042         ",1]
["DISPLAY-FULL COLOUR","THALES   ","C19366AF05    ",6]
["PRINTER MULTI-USE","THALES","8055515-4501   ",1]
["FDIMU               ","TELEDYNE "," 2234320-01-01    ",1]
["MMR                          ","COLLINS","822-1821-430",2]
["ATC – MODE S TRANSPONDER ","HONEYWELL ","066-01127-1402     ",2]
["MCDU             ","HONEYWELL                       ","4089740-961                   ",2]
["ISIS              ","THALES","C16786EA01   ",1]
["ADF RECEIVER         ","COLLINS     ","822-0299-020         ",2]
["ADIRU                         ","HONEYWELL  ","HG2030BE03   ",3]
["DME INTERROGATOR    ","COLLINS                ","822-2325-020            ",2]
["RADIO ALT. TRANSCEIVER ","COLLINS                ","822-0334-020       ",2]
["TCAS II COMPUTER","HONEYWELL  ","940-0351-005",1]
["VOR RECEIVER   ","COLLINS                ","822-0297-020      ",2]
["WEATHER RADAR TXRX ","COLLINS                ","822-1710-213  ",1]
["FMGC             ","THALES   ","C13042BA08",2]
["FCU                ","THALES   ","C12850AC03      ",1]
["HF TRANSCEIVER         ","COLLINS                ","822-0990-003  ",1]
["VHF TRANSCEIVER","COLLINS                ","822-1287-121   ",3]
["CIDS DIRECTOR           ","AIRBUS ","Z014H000333B       ",2]
["FAP                            ","AIRBUS ","Z133H052751D    ",1]
["ATSU                  ","AIRBUS ","LA2T0G20705C070  ",1]
["ELT                                ","ELTA ","01N65900    ",1]
["VOICE RECORDER           ","HONEYWELL  ","980-6022-001 ",1]
[]
["Must Have - Negotiable item. Functional Requirement","YES","NO"]
["Wheels and brakes GOODRICH"]
["Installation of universal brake cooling fans on BF-GOODRICH wheels and brakes"]