{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["BoQ"],"read":"whole","date_system":"1900"}

{"sheet":"BoQ","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"merged":[[1,4,1,6],[1,7,1,8],[1,9,1,10],[1,11,1,12],[2,4,2,6],[2,7,2,8],[2,9,2,10],[2,11,2,12],[3,4,3,6],[3,7,3,8],[3,9,3,10],[3,11,3,12]]}
[]
[null,null,"System Parameter",null,"5kW",null,null,"8kW",null,"10kW",null,"12kW"]
[null,null,"Minimum PV (Wp)",null,{"$f":"8*550","v":4400},null,null,{"$f":"14*550","v":7700},null,{"$f":"16*550","v":8800},null,{"$f":"18*550","v":9900}]
[null,null,"Minimum BESS (kWh)",null,5,null,null,8,null,10,null,12]
[{"$nulls":3},"Unit of measure","Unit","QTY","Unit Price","Unit","Unit Price","Unit","Unit Price","Unit","Unit Price"]
[null,"Line Item","Notes / Description"]
[1,"Site Assessment","Initial site visit: roof structural capacity, shading analysis, rooftop layout, safety assessment. ","Sum",1,null,null,1,null,1,null,1]
[2,"Feasibility Study","Evaluate if the system is viable: generation estimates, ROI, structural modifications, grid export potential, interconnection constraints.","Sum",1,null,null,1,null,1,null,1]
[3,"System Detailed Engineering & Design","Electrical single-line diagrams, string design, mounting layout, earthing, switchgear design, protection. Comply with NRS / SANS standards. ","Sum",1,null,null,1,null,1,null,1]
[4,"SSEG Application / Registration","Prepare and submit the SSEG application to Eskom or municipal utility. Required parts include SLD, CoC, inverter spec, EGI report, etc.","Sum",1,null,null,1,null,1,null,1]
[5,"PV Modules","Supply of PV solar modules (panels) - number and power depending on system size.(miniumum 550W)","Each",8,null,null,14,null,16,null,18]
[6,"PV Mount System","Roof-mounted racking, rails, brackets, supports; structural components for mounting.","Each",1,null,null,1,null,1,null,1]
[7,"Hybrid Inverters","Inverters capable of handling both PV and battery. Must comply with NRS-097-2-1 ","Each",1,null,null,1,null,1,null,1]
[8,"Batteries (LFP, installed)","Supply & installation of lithium-iron phosphate (LFP) batteries.","Each",1,null,null,1,null,1,null,1]
[9,"Battery BoS (Cabinets, Cables, Protection)","Battery enclosures, interconnect cabling, safety disconnects, fuses, battery management system wiring.","Each",1,null,null,1,null,1,null,1]
[10,"PV BoS (AC/DC, cables, DBs, protection, combiner box)","DC cabling, AC cabling, combiner / junction boxes, protection devices (fuses, surge arrestors), distribution boards. Appropriate sizes and standards upto 20m from customer DB","Each",1,null,null,1,null,1,null,1]
[11,"Installation, Testing, Commissioning & CoC","Functional tests, safety checks, inverter commissioning, Certificate of Compliance (CoC) by a registered electrician per SANS 10142-1 / SANS 10142-1-2. (SAPVIA PV GreenCard compliance or equivalent.","Each",1,null,null,1,null,1,null,1]
[12,"After Sales Installation Support services (up to 12 months)","Warranty support, remote monitoring, performance checks and installation corrective maintenance for first year.","Month",1,null,null,1,null,1,null,1]
[13,"Add on service:Installation Support & Maintenance service (Months 13-36)","Extended O&M: periodic maintenance, cleaning, performance review, preventive checks.","Month",1,null,null,1,null,1,null,1]
[14,"Add on service: Training: Installation and Maintenance","Training for installers / maintenance staff; could be via PV GreenCard course or equivalent. The SAPVIA PV GreenCard installer course (5-day) gives both theoretical and practical training. \nAssessment: PV GreenCard assessment or quivalent as required","Month",1,null,null,1,null,1,null,1]
[15,"Add on service: Internet Access / Connectivity for Inverter/Remote monitoring - Where no internet available.","Required minimum for remote inverter / system monitoring in sites where no fixed-line broadband is available. Could include 4G router, SIM-slot, external antenna (if needed), installation and configuration. Could also include a data-subscription option.","Sum",1,null,null,1,null,1,null,1]
[16,"Travelling","During project execution","Rate/KM",1,null,null,1,null,1,null,1]
[17,"Accommodation ","if customer location is  >200km from City/Town centre","Per night",1,null,null,1,null,1,null,1]
[18,"Establishment, De-establishment & rehabilitation of Site","Site camp","Sum",1,null,null,1,null,1,null,1]